{"text_format":"1","workbook":"xlsx","n_sheets":10,"sheets":["Input Form","Run Selections","Estimation Schedule","Building Summary","Notes","Active Throw","Performance Schedule","Active Configure & Quote","ListSheet","Lookup Tables"],"not_rendered":{"charts":1,"images":14,"macros":1,"external_links":0,"defined_names":1051,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Input Form","index":0,"n_rows":313,"n_cols":21,"rows_kept":313,"cut":false,"hidden":false,"merged":[[5,13,6,20],[10,18,10,20],[7,20,9,20],[5,5,6,12],[8,17,9,17],[7,5,10,5],[7,6,10,6],[7,7,9,7],[7,8,9,8],[7,9,9,9],[7,10,9,10],[7,11,10,11],[7,12,10,12],[7,13,10,13],[7,15,7,16],[7,18,9,18],[7,19,9,19],[8,14,9,14],[8,15,9,15],[8,16,9,16],[11,0,11,1],[12,0,12,1],[27,0,27,1],[25,0,26,3],[18,0,19,3],[20,0,20,1],[21,0,21,1],[23,0,24,0],[14,0,15,0],[16,0,17,1],[16,2,17,2],[16,3,17,3],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[9,0,10,1],[9,2,10,2],[9,3,10,3]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Basic"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Advanced"]
[]
[null,null,"Basic"]
[]
["Date","Project Name","Owner","Project Elevation\n(ft)",null,"Input Design Zone Requirements",null,null,null,null,null,null,null,"Selection Parameters per Active Beam"]
[]
[{"$f":"TODAY()","v":"2023-09-06"},"Project Name","Name",0,null,"Room or Zone Number/Name","Room or Zone Area/ft^2","Sensible Load","Latent Load","Heating Load","Min Primary Air","Number of Beams in Zone","Model","2 or 4 Pipe Coil","Beam","Primary Air",null,"Air Inlet","Chilled Water","Hot Water","Fin Tube Hot Water"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Length","Flow","Target Pressure","Size"]
["Room Conditions",null,"Cooling","Heating"]
[null,null,null,null,null,null,null,"BTUH","BTUH","BTUH","CFM",null,null,null,"ft (nom)","CFM","in W.G.","in","GPM"]
["Dry Bulb ⁰F",null,75,72]
["Relative Humidity % RH",null,50,50,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
["Wet Bulb","⁰F",{"$f":"getWetBulbFromRH(C13,C12,$D$8)","v":62.682799999999958},{"$f":"getWetBulbFromRH(D13,D12,$D$8)","v":60.211399999999927},null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
["Dew Point","⁰F",{"$f":"getDewPointFromRH(C13,C12,$D$8)","v":55.181526218884954},{"$f":"getDewPointFromRH(D13,D12,$D$8)","v":52.428836553616385},null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,"gr/lb",{"$f":"getgrainperpound(C13,C12,$D$8)","v":64.649670871442396},{"$f":"getgrainperpound(D13,D12,$D$8)","v":58.364961883371663},null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
["On-Coil Temperature ⁰F\n(if different to Room Dry Bulb)",null,{"$f":"InputCRoomTemp","v":75},{"$f":"D12","v":72},null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
["Primary Air Conditions (ducted to room)",null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
["Dry Bulb ⁰F",null,55,55,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
["Relative Humidity % RH",null,80,80,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
["Wet Bulb","⁰F",{"$f":"getWetBulbFromRH(C22,C21,$D$8)","v":51.64519999999996},{"$f":"getWetBulbFromRH(D22,D21,$D$8)","v":51.64519999999996},null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
["Dew Point","⁰F",{"$f":"getDewPointFromRH(C22,C21,$D$8)","v":49.014353359704707},{"$f":"getDewPointFromRH(D22,D21,$D$8)","v":49.014353359704707},null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,"gr/lb",{"$f":"getgrainperpound(C22,C21,$D$8)","v":51.339360278659356},{"$f":"getgrainperpound(D22,D21,$D$8)","v":51.339360278659356},null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
["Entering Water Conditions",null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
["Temperature ⁰F",null,57,120,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"Select Model",2,4,50,0.75,5,1.5,0.5,0]

{"sheet":"Run Selections","index":1,"n_rows":315,"n_cols":56,"rows_kept":315,"cut":false,"hidden":true,"merged":[[43,2,43,3],[36,0,36,1],[36,2,36,3],[37,2,37,3],[38,2,38,3],[39,2,39,3],[40,2,40,3],[35,0,35,1],[21,2,22,2],[21,3,22,3],[32,0,32,1],[40,0,40,1],[39,0,39,1],[38,0,38,1],[33,0,34,3],[27,0,27,1],[30,0,31,0],[28,0,28,1],[25,0,26,3],[23,0,23,1],[23,2,23,3],[50,0,51,3],[9,36,11,36],[9,41,11,42],[9,39,10,40],[10,24,11,24],[10,26,11,26],[10,27,11,27],[12,39,12,40],[10,31,11,31],[10,32,11,32],[10,33,11,33],[12,31,12,33],[9,37,9,38],[12,25,12,26],[10,38,11,38],[9,29,11,29],[19,0,20,0],[21,0,22,1],[32,2,32,3],[24,0,24,1],[9,34,12,34],[37,0,37,1],[41,0,42,3],[43,0,43,1],[7,31,8,42],[10,13,11,13],[9,14,11,14],[9,15,11,15],[10,46,11,46],[10,47,11,47],[10,50,11,50],[10,51,11,51],[10,44,11,44],[10,45,11,45],[9,49,9,51],[10,49,11,49],[10,37,11,37],[9,31,9,33],[9,35,12,35],[12,37,12,38],[9,46,9,48],[12,43,12,45],[9,43,9,45],[10,43,11,43],[7,18,8,30],[9,30,11,30],[9,21,12,21],[7,44,8,54],[12,16,12,17],[16,0,16,1],[17,0,17,1],[10,12,11,12],[24,2,24,3],[11,0,11,2],[12,0,12,2],[7,5,12,5],[7,0,7,2],[8,0,10,2],[7,6,12,6],[7,12,8,17],[7,7,8,11],[9,7,11,7],[9,8,11,8],[9,9,11,9],[9,16,11,16],[9,17,11,17],[9,55,12,55],[10,48,11,48],[9,11,12,11],[12,12,12,14],[12,28,12,30],[9,10,11,10],[14,0,15,1],[14,2,15,2],[14,3,15,3],[9,52,9,54],[10,54,11,54],[10,53,11,53],[10,52,11,52],[9,22,9,23],[9,24,9,26],[9,28,11,28],[9,12,9,13],[10,22,11,22],[10,23,11,23],[9,20,12,20],[10,25,11,25],[9,18,12,18],[9,19,12,19],[12,49,12,51]]}
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUMIF(P15:P315,\">0\")-SUMIF(T15:T315,\"=Select Model\",P15:P315)","v":0},null,null,{"$f":"SUMIF(L15:L315,\">0\")-SUMIF(T15:T315,\"=Select Model\",L15:L315)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUMIF(Q15:Q315,\">0\")-SUMIF(T15:T315,\"=Select Model\",Q15:Q315)","v":0},null,null,{"$f":"SUMPRODUCT(--NOT(T15:T315=\"Select Model\"),L15:L315,W15:W315)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUMIFS(R15:R315,T15:T315, \"<>Select Model\", U15:U315, \"=4\") + SUMIFS(R15:R315,T15:T315, \"<>Select Model\", U15:U315, \"=2\", J15:J315, \">=1\")","v":0},null,null,{"$f":"COUNTIF(T15:T315,\"<>Select Model\")","v":0}]
[]
[]
["Project Name",null,null,"Owner",null,"Room or Zone Number/Name","Room or Zone Area/Square Footage","Input Design Zone Requirements",null,null,null,null,"Total Outputs for Zone (not per beam)",null,null,null,null,null,"Selection Parameters per Active Beam",null,null,null,null,null,null,null,null,null,null,null,null,"Airside Data per Active Beam",null,null,null,null,null,null,null,null,null,null,null,null,"Waterside Data per Active Beam"]
["Project Name",null,null,"Name"]
[null,null,null,"Revision",null,null,null,"Sensible Load","Latent Load","Heating Load","Min Primary Air","Number of Beams in Zone","Cooling",null,"Heating","Primary Air Flow","Chilled Water","Hot Water","Zone/Room Selection Options","Model","2 or 4 Pipe Coil","Coil Circuit","Beam",null,"Primary Air",null,null,"Air Inlet","Chilled Water","Hot Water","Fin Tube Hot Water","Primary Air",null,null,"Nozzle Code","Induction\nRatio","Transfer Effectiveness","Air Flow",null,"Discharge Air Temp",null,"Sound Level",null,"Cooling",null,null,"Chilled Water",null,null,"Heating",null,null,"Hot Water",null,null,"Nozzle Size"]
[null,null,null,"001",null,null,null,null,null,null,null,null,"Sensible","Latent",null,null,null,null,null,null,null,null,"Length","Width","Flow","Target Pressure","Exact Pressure","Size",null,null,null,"Airside Capacity (in Cooling)","Latent    (in Cooling)","Airside Capacity (in Heating)",null,null,null,"Total Discharge","VAV - Min Primary Air",null,null,null,null,"LatentCoil Capacity","Coil Capacity","Total Sensible","Pressure Drop","Leaving Temp","Delta T","Fin Tube Capacity","Coil Capacity","Total Sensible","Pressure Drop","Leaving Temp","Delta T"]
["Project Elevation (ft)",null,null,"Date",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cooling","Heating"]
[0,null,null,{"$f":"TODAY()","v":"2023-09-06"},null,null,null,"BTUH","BTUH","BTUH","CFM",null,"BTUH",null,null,"CFM","GPM",null,null,null,null,null,"ft (nom)","in (nom)","CFM","in W.G.",null,"in","GPM",null,null,"BTUH",null,null,null,null,"BTUH/CFM","CFM",null,"⁰F",null,"dB(A)","NC","BTUH",null,null,"ft W.G.","⁰F","⁰F","BTUH",null,null,"ft W.G.","⁰F","⁰F"]
[]
["Room Conditions",null,"Cooling","Heating",null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I15)),I15<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I15, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H15)),H15<0),\"\",intlEstQuantity(T15, W15*12, H15)),1)","v":""},{"$f":"IF(LEFT(T15, 4)=\"ACBC\",IF(AND(ISNUMBER(L15),ISNUMBER(AT15)),IF(AA15=-1,\"LOW CFM\",L15*AT15),\"\"),IF(AND(ISNUMBER(L15),ISNUMBER(AT15)),IF(AA15=-1,\"N/A CFM\",L15*AT15),\"\"))","v":""},{"$f":"IF(LEFT(T15,4)=\"ACBC\",IF(AND(ISNUMBER(L15),ISNUMBER(AG15)),IF(AA15=-1,\"LOW CFM\",L15*AG15),\"\"),IF(AND(ISNUMBER(L15),ISNUMBER(AG15)),IF(AA15=-1,\"N/A CFM\",L15*AG15),\"\"))","v":""},{"$f":"IF(LEFT(T15,4)=\"ACBC\",IF(AND(ISNUMBER(L15),ISNUMBER(AZ15)),IF(AA15=-1,\"LOW CFM\",L15*AZ15),\"\"),IF(AND(ISNUMBER(L15),ISNUMBER(AZ15)),IF(AA15=-1,\"N/A CFM\",L15*AZ15),\"\"))","v":""},{"$f":"IF(AND(ISNUMBER(L15),ISNUMBER(Y15)),L15*Y15,\"\")","v":""},{"$f":"IF(AND(ISNUMBER(L15),ISNUMBER(AC15)),L15*AC15,\"\")","v":""},{"$f":"IF(AND(ISNUMBER(L15),ISNUMBER(AD15)),IF(AND(T15=\"ACBC_1W\",AD15=0),AE15*L15,L15*AD15))","v":false},"Default","Select Model",2,{"$f":"IF(T15=\"Select Model\",\"\",coilCircuitChange(W15, U15, AC15, T15,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T15=\"Select Model\",\"\",beamWidth(T15))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T15=\"Select Model\",T15=\"PCBL\"), 0,getSPIP(T15, W15, Y15, BD15, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T15=\"Select Model\", \"\",IF(T15=\"PCBL\",0,primaryAirSensibleCapacityIP($T15,$W15,activeRoomTempCooling,activePriAirTempCooling,$Y15,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T15=\"Select Model\",\"\",IF($T15=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y15,activeElevation)))","v":""},{"$f":"IF(OR(T15=\"Select Model\",T15=\"PCBL\"), 0,IF(AD15=0,0,-primaryAirSensibleCapacityIP($T15,$W15,activeRoomTempHeating,activePriAirTempHeating,$Y15,activeElevation,\"heating\")))","v":0},{"$f":"getCurrentNozzleCode(T15, W15, Y15, Z15, activeElevation, TRUE)","v":""},{"$f":"IFERROR(IF(T15=\"Select Model\", \"\", InductionRatio($T15,BD15,$W15,$Y15)),\"N/A\")","v":""},{"$f":"IFERROR(AT15/Y15,\"\")","v":""},{"$f":"IFERROR(IF(T15=\"Select Model\", \"\",(1+AJ15)*Y15),\"N/A\")","v":""},{"$f":"IFERROR(IF(T15=\"Select Model\", \"\",IF($T15=\"PCBL\",\"N/A\",minVAVSetBack(AA15, Y15))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T15=\"Select Model\", \"\",IF($T15= \"PCBL\",\"N/A\",getDischargeAirTemp($T15,$V15,$AC15,$W15,BD15,$AL15, $Y15, $AS15, \"cooling\",activeElevation,$AB15,$AJ15,$AV15,$BB15))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T15=\"Select Model\",$T15=\"PCBL\"), \"\",getDischargeAirTemp($T15,$V15,$AD15,$W15,BD15,$AL15, $Y15, $AY15, \"heating\",activeElevation,$AB15,$AJ15,$AV15,$BB15)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T15=\"Select Model\", \"\",IF(OR($T15=\"ACBC_1W\",$T15=\"ACBC_2W\",LEFT($T15,4)=\"ACBR\",$T15 = \"LIU24_2W\",LEFT($T15,3)=\"RIU\",LEFT($T15,6)=\"ACBL12\"), IF((soundLevel($T15, $AB15, BD15, $Y15, $W15,$AJ15,$AA15,\"dba\"))<15,\"<15\",soundLevel($T15, $AB15, BD15, $Y15, $W15,$AJ15,$AA15,\"dba\")+0.4),IF((soundLevel($T15, $AB15, BD15, $Y15, $W15,$AJ15,$AA15,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T15, $AB15, BD15, $Y15, $W15,$AJ15,$AA15,\"dba\")+5)<15, \"<15\", soundLevel($T15, $AB15, BD15,$Y15, $W15,$AJ15,$AA15,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T15=\"Select Model\", \"\",IF(OR($T15=\"ACBC_1W\",$T15=\"ACBC_2W\",LEFT($T15,4)=\"ACBR\",$T15=\"LIU24_2W\",LEFT($T15,3)=\"RIU\",LEFT($T15,6)=\"ACBL12\"), IF((soundLevel($T15, $AB15, BD15, $Y15, $W15,$AJ15,$AA15,\"NC\"))<15,\"<15\",soundLevel($T15, $AB15, BD15, $Y15, $W15,$AJ15,$AA15,\"NC\")+0.4),IF((soundLevel($T15, $AB15, BD15, $Y15, $W15,$AJ15,$AA15,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T15, $AB15, BD15, $Y15, $W15,$AJ15,$AA15,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T15, $AB15, BD15, $Y15, $W15,$AJ15,$AA15,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T15=\"Select Model\", \"\",IF(OR($T15=\"ACBC_1W\",$T15=\"ACBC_2W\",LEFT($T15,4)=\"ACBR\",$T15=\"LIU24_2W\",LEFT($T15,3)=\"RIU\",LEFT($T15,6)=\"ACBL12\"), IF((soundLevel($T15, $AB15, BE15, $Y15, $W15,$AJ15,$AA15,\"NC\"))<15,\"<15\",soundLevel($T15, $AB15, BE15, $Y15, $W15,$AJ15,$AA15,\"NC\")+0.4),IF((soundLevel($T15, $AB15, BE15, $Y15, $W15,$AJ15,$AA15,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T15, $AB15, BE15, $Y15, $W15,$AJ15,$AA15,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T15, $AB15, BE15, $Y15, $W15,$AJ15,$AA15,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T15=\"Select Model\",\"\",IF($T15=\"ACBC_1W\",calcQwIP($Y15,$W15,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC15,BD15,\"capacity\",$U15&\"P\"&IF($V15=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T15,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y15,$W15,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC15,BD15,\"capacity\",$U15&\"P\"&IF($V15=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T15,activeElevation)))","v":""},{"$f":"IF(T15=\"Select Model\", \"\",IF(T15 = \"LIU24_2W\", AS15+AF15+AR15, AS15+AF15))","v":""},{"$f":"IF(T15=\"Select Model\", 0,waterPressureDrop(W15, U15 & \"P\" & IF(V15=\"Dual\",2,1) &\"C\", AC15, \"cooling\", T15))","v":0},{"$f":"IF(T15=\"Select Model\", \"\",getReturnWaterTemp(T15,AC15, activeEWTCooling, AS15, \"cooling\"))","v":""},{"$f":"IF(T15=\"Select Model\", \"\",$AV15-activeEWTCooling)","v":""},{"$f":"IF($T15<>\"ACBC_1W\",\"\",IF($J15=\"\",\"\",FintubeCapacity($T15,$W15,$AE15,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T15=\"Select Model\",T15=\"PCBL\"),\"\",calcQwIP(Y15,W15,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD15,BD15,\"capacity\",U15&\"P\"&IF(V15=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T15,activeElevation))","v":""},{"$f":"IF(OR(T15=\"Select Model\",T15=\"PCBL\"),\"\",IF(AND(AD15=0,T15=\"ACBC_1W\"),AX15+AH15,AY15+AH15))","v":""},{"$f":"IF(OR(T15=\"Select Model\",T15=\"PCBL\"), \"\",IF(AY15=0,\"N/A\",waterPressureDrop(W15, U15 & \"P\" & IF(V15=\"Dual\",2,1) &\"C\", AD15, \"heating\", T15)))","v":""},{"$f":"IF(OR(T15=\"Select Model\",T15=\"PCBL\"), \"\",IF(AY15=0,getReturnWaterTemp(T15,AE15, activeEWTHeating, AX15, \"heating\"),getReturnWaterTemp(T15,AD15, activeEWTHeating, AY15, \"heating\")))","v":""},{"$f":"IF(OR($T15=\"Select Model\",$J15=\"\",T15=\"PCBL\"), \"\",activeEWTHeating-$BB15)","v":""},{"$f":" getNozzle(T15, W15, Y15, Z15, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I16)),I16<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I16, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H16)),H16<0),\"\",intlEstQuantity(T16, W16*12, H16)),1)","v":""},{"$f":"IF(LEFT(T16, 4)=\"ACBC\",IF(AND(ISNUMBER(L16),ISNUMBER(AT16)),IF(AA16=-1,\"LOW CFM\",L16*AT16),\"\"),IF(AND(ISNUMBER(L16),ISNUMBER(AT16)),IF(AA16=-1,\"N/A CFM\",L16*AT16),\"\"))","v":""},{"$f":"IF(LEFT(T16,4)=\"ACBC\",IF(AND(ISNUMBER(L16),ISNUMBER(AG16)),IF(AA16=-1,\"LOW CFM\",L16*AG16),\"\"),IF(AND(ISNUMBER(L16),ISNUMBER(AG16)),IF(AA16=-1,\"N/A CFM\",L16*AG16),\"\"))","v":""},{"$f":"IF(LEFT(T16,4)=\"ACBC\",IF(AND(ISNUMBER(L16),ISNUMBER(AZ16)),IF(AA16=-1,\"LOW CFM\",L16*AZ16),\"\"),IF(AND(ISNUMBER(L16),ISNUMBER(AZ16)),IF(AA16=-1,\"N/A CFM\",L16*AZ16),\"\"))","v":""},{"$f":"IF(AND(ISNUMBER(L16),ISNUMBER(Y16)),L16*Y16,\"\")","v":""},{"$f":"IF(AND(ISNUMBER(L16),ISNUMBER(AC16)),L16*AC16,\"\")","v":""},{"$f":"IF(AND(ISNUMBER(L16),ISNUMBER(AD16)),IF(AND(T16=\"ACBC_1W\",AD16=0),AE16*L16,L16*AD16))","v":false},"Default","Select Model",2,{"$f":"IF(T16=\"Select Model\",\"\",coilCircuitChange(W16, U16, AC16, T16,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T16=\"Select Model\",\"\",beamWidth(T16))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T16=\"Select Model\",T16=\"PCBL\"), 0,getSPIP(T16, W16, Y16, BD16, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T16=\"Select Model\", \"\",IF(T16=\"PCBL\",0,primaryAirSensibleCapacityIP($T16,$W16,activeRoomTempCooling,activePriAirTempCooling,$Y16,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T16=\"Select Model\",\"\",IF($T16=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y16,activeElevation)))","v":""},{"$f":"IF(OR(T16=\"Select Model\",T16=\"PCBL\"), 0,IF(AD16=0,0,-primaryAirSensibleCapacityIP($T16,$W16,activeRoomTempHeating,activePriAirTempHeating,$Y16,activeElevation,\"heating\")))","v":0},{"$f":"getCurrentNozzleCode(T16, W16, Y16, Z16, activeElevation, TRUE)","v":""},{"$f":"IFERROR(IF(T16=\"Select Model\", \"\", InductionRatio($T16,BD16,$W16,$Y16)),\"N/A\")","v":""},{"$f":"IFERROR(AT16/Y16,\"\")","v":""},{"$f":"IFERROR(IF(T16=\"Select Model\", \"\",(1+AJ16)*Y16),\"N/A\")","v":""},{"$f":"IFERROR(IF(T16=\"Select Model\", \"\",IF($T16=\"PCBL\",\"N/A\",minVAVSetBack(AA16, Y16))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T16=\"Select Model\", \"\",IF($T16= \"PCBL\",\"N/A\",getDischargeAirTemp($T16,$V16,$AC16,$W16,BD16,$AL16, $Y16, $AS16, \"cooling\",activeElevation,$AB16,$AJ16,$AV16,$BB16))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T16=\"Select Model\",$T16=\"PCBL\"), \"\",getDischargeAirTemp($T16,$V16,$AD16,$W16,BD16,$AL16, $Y16, $AY16, \"heating\",activeElevation,$AB16,$AJ16,$AV16,$BB16)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T16=\"Select Model\", \"\",IF(OR($T16=\"ACBC_1W\",$T16=\"ACBC_2W\",LEFT($T16,4)=\"ACBR\",$T16 = \"LIU24_2W\",LEFT($T16,3)=\"RIU\",LEFT($T16,6)=\"ACBL12\"), IF((soundLevel($T16, $AB16, BD16, $Y16, $W16,$AJ16,$AA16,\"dba\"))<15,\"<15\",soundLevel($T16, $AB16, BD16, $Y16, $W16,$AJ16,$AA16,\"dba\")+0.4),IF((soundLevel($T16, $AB16, BD16, $Y16, $W16,$AJ16,$AA16,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T16, $AB16, BD16, $Y16, $W16,$AJ16,$AA16,\"dba\")+5)<15, \"<15\", soundLevel($T16, $AB16, BD16,$Y16, $W16,$AJ16,$AA16,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T16=\"Select Model\", \"\",IF(OR($T16=\"ACBC_1W\",$T16=\"ACBC_2W\",LEFT($T16,4)=\"ACBR\",$T16=\"LIU24_2W\",LEFT($T16,3)=\"RIU\",LEFT($T16,6)=\"ACBL12\"), IF((soundLevel($T16, $AB16, BD16, $Y16, $W16,$AJ16,$AA16,\"NC\"))<15,\"<15\",soundLevel($T16, $AB16, BD16, $Y16, $W16,$AJ16,$AA16,\"NC\")+0.4),IF((soundLevel($T16, $AB16, BD16, $Y16, $W16,$AJ16,$AA16,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T16, $AB16, BD16, $Y16, $W16,$AJ16,$AA16,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T16, $AB16, BD16, $Y16, $W16,$AJ16,$AA16,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T16=\"Select Model\",\"\",IF($T16=\"LIU24_2W\",calcQwIP($Y16,$W16,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC16,$AI16,\"latent\",$U16&\"P\"&IF($V16=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T16,activeElevation),\"\"))","v":""},{"$f":"IF($T16=\"Select Model\",\"\",IF($T16=\"ACBC_1W\",calcQwIP($Y16,$W16,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC16,BD16,\"capacity\",$U16&\"P\"&IF($V16=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T16,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y16,$W16,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC16,BD16,\"capacity\",$U16&\"P\"&IF($V16=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T16,activeElevation)))","v":""},{"$f":"IF(T16=\"Select Model\", \"\",IF(T16 = \"LIU24_2W\", AS16+AF16+AR16, AS16+AF16))","v":""},{"$f":"IF(T16=\"Select Model\", 0,waterPressureDrop(W16, U16 & \"P\" & IF(V16=\"Dual\",2,1) &\"C\", AC16, \"cooling\", T16))","v":0},{"$f":"IF(T16=\"Select Model\", \"\",getReturnWaterTemp(T16,AC16, activeEWTCooling, AS16, \"cooling\"))","v":""},{"$f":"IF(T16=\"Select Model\", \"\",$AV16-activeEWTCooling)","v":""},{"$f":"IF($T16<>\"ACBC_1W\",\"\",IF($J16=\"\",\"\",FintubeCapacity($T16,$W16,$AE16,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T16=\"Select Model\",T16=\"PCBL\"),\"\",calcQwIP(Y16,W16,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD16,BD16,\"capacity\",U16&\"P\"&IF(V16=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T16,activeElevation))","v":""},{"$f":"IF(OR(T16=\"Select Model\",T16=\"PCBL\"),\"\",IF(AND(AD16=0,T16=\"ACBC_1W\"),AX16+AH16,AY16+AH16))","v":""},{"$f":"IF(OR(T16=\"Select Model\",T16=\"PCBL\"), \"\",IF(AY16=0,\"N/A\",waterPressureDrop(W16, U16 & \"P\" & IF(V16=\"Dual\",2,1) &\"C\", AD16, \"heating\", T16)))","v":""},{"$f":"IF(OR(T16=\"Select Model\",T16=\"PCBL\"), \"\",IF(AY16=0,getReturnWaterTemp(T16,AE16, activeEWTHeating, AX16, \"heating\"),getReturnWaterTemp(T16,AD16, activeEWTHeating, AY16, \"heating\")))","v":""},{"$f":"IF(OR($T16=\"Select Model\",$J16=\"\",T16=\"PCBL\"), \"\",activeEWTHeating-$BB16)","v":""},{"$f":" getNozzle(T16, W16, Y16, Z16, activeElevation, TRUE)","v":0}]
["Dry Bulb ⁰F",null,75,72,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I17)),I17<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I17, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H17)),H17<0),\"\",intlEstQuantity(T17, W17*12, H17)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T17=\"Select Model\",\"\",coilCircuitChange(W17, U17, AC17, T17,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T17=\"Select Model\",\"\",beamWidth(T17))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T17=\"Select Model\",T17=\"PCBL\"), 0,getSPIP(T17, W17, Y17, BD17, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T17=\"Select Model\", \"\",IF(T17=\"PCBL\",0,primaryAirSensibleCapacityIP($T17,$W17,activeRoomTempCooling,activePriAirTempCooling,$Y17,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T17=\"Select Model\",\"\",IF($T17=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y17,activeElevation)))","v":""},{"$f":"IF(OR(T17=\"Select Model\",T17=\"PCBL\"), 0,IF(AD17=0,0,-primaryAirSensibleCapacityIP($T17,$W17,activeRoomTempHeating,activePriAirTempHeating,$Y17,activeElevation,\"heating\")))","v":0},{"$f":"getCurrentNozzleCode(T17, W17, Y17, Z17, activeElevation, TRUE)","v":""},{"$f":"IFERROR(IF(T17=\"Select Model\", \"\", InductionRatio($T17,BD17,$W17,$Y17)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T17=\"Select Model\", \"\",IF($T17=\"PCBL\",\"N/A\",minVAVSetBack(AA17, Y17))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T17=\"Select Model\", \"\",IF($T17= \"PCBL\",\"N/A\",getDischargeAirTemp($T17,$V17,$AC17,$W17,BD17,$AL17, $Y17, $AS17, \"cooling\",activeElevation,$AB17,$AJ17,$AV17,$BB17))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T17=\"Select Model\",$T17=\"PCBL\"), \"\",getDischargeAirTemp($T17,$V17,$AD17,$W17,BD17,$AL17, $Y17, $AY17, \"heating\",activeElevation,$AB17,$AJ17,$AV17,$BB17)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T17=\"Select Model\", \"\",IF(OR($T17=\"ACBC_1W\",$T17=\"ACBC_2W\",LEFT($T17,4)=\"ACBR\",$T17 = \"LIU24_2W\",LEFT($T17,3)=\"RIU\",LEFT($T17,6)=\"ACBL12\"), IF((soundLevel($T17, $AB17, BD17, $Y17, $W17,$AJ17,$AA17,\"dba\"))<15,\"<15\",soundLevel($T17, $AB17, BD17, $Y17, $W17,$AJ17,$AA17,\"dba\")+0.4),IF((soundLevel($T17, $AB17, BD17, $Y17, $W17,$AJ17,$AA17,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T17, $AB17, BD17, $Y17, $W17,$AJ17,$AA17,\"dba\")+5)<15, \"<15\", soundLevel($T17, $AB17, BD17,$Y17, $W17,$AJ17,$AA17,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T17=\"Select Model\", \"\",IF(OR($T17=\"ACBC_1W\",$T17=\"ACBC_2W\",LEFT($T17,4)=\"ACBR\",$T17=\"LIU24_2W\",LEFT($T17,3)=\"RIU\",LEFT($T17,6)=\"ACBL12\"), IF((soundLevel($T17, $AB17, BD17, $Y17, $W17,$AJ17,$AA17,\"NC\"))<15,\"<15\",soundLevel($T17, $AB17, BD17, $Y17, $W17,$AJ17,$AA17,\"NC\")+0.4),IF((soundLevel($T17, $AB17, BD17, $Y17, $W17,$AJ17,$AA17,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T17, $AB17, BD17, $Y17, $W17,$AJ17,$AA17,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T17, $AB17, BD17, $Y17, $W17,$AJ17,$AA17,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T17=\"Select Model\",\"\",IF($T17=\"LIU24_2W\",calcQwIP($Y17,$W17,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC17,$AI17,\"latent\",$U17&\"P\"&IF($V17=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T17,activeElevation),\"\"))","v":""},{"$f":"IF($T17=\"Select Model\",\"\",IF($T17=\"ACBC_1W\",calcQwIP($Y17,$W17,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC17,BD17,\"capacity\",$U17&\"P\"&IF($V17=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T17,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y17,$W17,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC17,BD17,\"capacity\",$U17&\"P\"&IF($V17=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T17,activeElevation)))","v":""},"",{"$f":"IF(T17=\"Select Model\", 0,waterPressureDrop(W17, U17 & \"P\" & IF(V17=\"Dual\",2,1) &\"C\", AC17, \"cooling\", T17))","v":0},{"$f":"IF(T17=\"Select Model\", \"\",getReturnWaterTemp(T17,AC17, activeEWTCooling, AS17, \"cooling\"))","v":""},"",{"$f":"IF($T17<>\"ACBC_1W\",\"\",IF($J17=\"\",\"\",FintubeCapacity($T17,$W17,$AE17,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T17=\"Select Model\",T17=\"PCBL\"),\"\",calcQwIP(Y17,W17,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD17,BD17,\"capacity\",U17&\"P\"&IF(V17=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T17,activeElevation))","v":""},"",{"$f":"IF(OR(T17=\"Select Model\",T17=\"PCBL\"), \"\",IF(AY17=0,\"N/A\",waterPressureDrop(W17, U17 & \"P\" & IF(V17=\"Dual\",2,1) &\"C\", AD17, \"heating\", T17)))","v":""},{"$f":"IF(OR(T17=\"Select Model\",T17=\"PCBL\"), \"\",IF(AY17=0,getReturnWaterTemp(T17,AE17, activeEWTHeating, AX17, \"heating\"),getReturnWaterTemp(T17,AD17, activeEWTHeating, AY17, \"heating\")))","v":""},"",{"$f":" getNozzle(T17, W17, Y17, Z17, activeElevation, TRUE)","v":0}]
["Relative Humidity % RH",null,50,50,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I18)),I18<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I18, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H18)),H18<0),\"\",intlEstQuantity(T18, W18*12, H18)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T18=\"Select Model\",\"\",coilCircuitChange(W18, U18, AC18, T18,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T18=\"Select Model\",\"\",beamWidth(T18))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T18=\"Select Model\",T18=\"PCBL\"), 0,getSPIP(T18, W18, Y18, BD18, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T18=\"Select Model\", \"\",IF(T18=\"PCBL\",0,primaryAirSensibleCapacityIP($T18,$W18,activeRoomTempCooling,activePriAirTempCooling,$Y18,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T18=\"Select Model\",\"\",IF($T18=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y18,activeElevation)))","v":""},{"$f":"IF(OR(T18=\"Select Model\",T18=\"PCBL\"), 0,IF(AD18=0,0,-primaryAirSensibleCapacityIP($T18,$W18,activeRoomTempHeating,activePriAirTempHeating,$Y18,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T18=\"Select Model\", \"\", InductionRatio($T18,BD18,$W18,$Y18)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T18=\"Select Model\", \"\",IF($T18=\"PCBL\",\"N/A\",minVAVSetBack(AA18, Y18))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T18=\"Select Model\", \"\",IF($T18= \"PCBL\",\"N/A\",getDischargeAirTemp($T18,$V18,$AC18,$W18,BD18,$AL18, $Y18, $AS18, \"cooling\",activeElevation,$AB18,$AJ18,$AV18,$BB18))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T18=\"Select Model\",$T18=\"PCBL\"), \"\",getDischargeAirTemp($T18,$V18,$AD18,$W18,BD18,$AL18, $Y18, $AY18, \"heating\",activeElevation,$AB18,$AJ18,$AV18,$BB18)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T18=\"Select Model\", \"\",IF(OR($T18=\"ACBC_1W\",$T18=\"ACBC_2W\",LEFT($T18,4)=\"ACBR\",$T18 = \"LIU24_2W\",LEFT($T18,3)=\"RIU\",LEFT($T18,6)=\"ACBL12\"), IF((soundLevel($T18, $AB18, BD18, $Y18, $W18,$AJ18,$AA18,\"dba\"))<15,\"<15\",soundLevel($T18, $AB18, BD18, $Y18, $W18,$AJ18,$AA18,\"dba\")+0.4),IF((soundLevel($T18, $AB18, BD18, $Y18, $W18,$AJ18,$AA18,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T18, $AB18, BD18, $Y18, $W18,$AJ18,$AA18,\"dba\")+5)<15, \"<15\", soundLevel($T18, $AB18, BD18,$Y18, $W18,$AJ18,$AA18,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T18=\"Select Model\", \"\",IF(OR($T18=\"ACBC_1W\",$T18=\"ACBC_2W\",LEFT($T18,4)=\"ACBR\",$T18=\"LIU24_2W\",LEFT($T18,3)=\"RIU\",LEFT($T18,6)=\"ACBL12\"), IF((soundLevel($T18, $AB18, BD18, $Y18, $W18,$AJ18,$AA18,\"NC\"))<15,\"<15\",soundLevel($T18, $AB18, BD18, $Y18, $W18,$AJ18,$AA18,\"NC\")+0.4),IF((soundLevel($T18, $AB18, BD18, $Y18, $W18,$AJ18,$AA18,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T18, $AB18, BD18, $Y18, $W18,$AJ18,$AA18,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T18, $AB18, BD18, $Y18, $W18,$AJ18,$AA18,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T18=\"Select Model\",\"\",IF($T18=\"LIU24_2W\",calcQwIP($Y18,$W18,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC18,$AI18,\"latent\",$U18&\"P\"&IF($V18=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T18,activeElevation),\"\"))","v":""},{"$f":"IF($T18=\"Select Model\",\"\",IF($T18=\"ACBC_1W\",calcQwIP($Y18,$W18,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC18,BD18,\"capacity\",$U18&\"P\"&IF($V18=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T18,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y18,$W18,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC18,BD18,\"capacity\",$U18&\"P\"&IF($V18=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T18,activeElevation)))","v":""},"",{"$f":"IF(T18=\"Select Model\", 0,waterPressureDrop(W18, U18 & \"P\" & IF(V18=\"Dual\",2,1) &\"C\", AC18, \"cooling\", T18))","v":0},{"$f":"IF(T18=\"Select Model\", \"\",getReturnWaterTemp(T18,AC18, activeEWTCooling, AS18, \"cooling\"))","v":""},"",{"$f":"IF($T18<>\"ACBC_1W\",\"\",IF($J18=\"\",\"\",FintubeCapacity($T18,$W18,$AE18,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T18=\"Select Model\",T18=\"PCBL\"),\"\",calcQwIP(Y18,W18,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD18,BD18,\"capacity\",U18&\"P\"&IF(V18=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T18,activeElevation))","v":""},"",{"$f":"IF(OR(T18=\"Select Model\",T18=\"PCBL\"), \"\",IF(AY18=0,\"N/A\",waterPressureDrop(W18, U18 & \"P\" & IF(V18=\"Dual\",2,1) &\"C\", AD18, \"heating\", T18)))","v":""},{"$f":"IF(OR(T18=\"Select Model\",T18=\"PCBL\"), \"\",IF(AY18=0,getReturnWaterTemp(T18,AE18, activeEWTHeating, AX18, \"heating\"),getReturnWaterTemp(T18,AD18, activeEWTHeating, AY18, \"heating\")))","v":""},"",{"$f":" getNozzle(T18, W18, Y18, Z18, activeElevation, TRUE)","v":0}]
["Wet Bulb","⁰F",{"$f":"getWetBulbFromRH(C18,C17,$A$13)","v":62.682799999999958},{"$f":"getWetBulbFromRH(D18,D17,$A$13)","v":60.211399999999927},null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I19)),I19<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I19, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H19)),H19<0),\"\",intlEstQuantity(T19, W19*12, H19)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T19=\"Select Model\",\"\",coilCircuitChange(W19, U19, AC19, T19,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T19=\"Select Model\",\"\",beamWidth(T19))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T19=\"Select Model\",T19=\"PCBL\"), 0,getSPIP(T19, W19, Y19, BD19, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T19=\"Select Model\", \"\",IF(T19=\"PCBL\",0,primaryAirSensibleCapacityIP($T19,$W19,activeRoomTempCooling,activePriAirTempCooling,$Y19,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T19=\"Select Model\",\"\",IF($T19=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y19,activeElevation)))","v":""},{"$f":"IF(OR(T19=\"Select Model\",T19=\"PCBL\"), 0,IF(AD19=0,0,-primaryAirSensibleCapacityIP($T19,$W19,activeRoomTempHeating,activePriAirTempHeating,$Y19,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T19=\"Select Model\", \"\", InductionRatio($T19,BD19,$W19,$Y19)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T19=\"Select Model\", \"\",IF($T19=\"PCBL\",\"N/A\",minVAVSetBack(AA19, Y19))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T19=\"Select Model\", \"\",IF($T19= \"PCBL\",\"N/A\",getDischargeAirTemp($T19,$V19,$AC19,$W19,BD19,$AL19, $Y19, $AS19, \"cooling\",activeElevation,$AB19,$AJ19,$AV19,$BB19))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T19=\"Select Model\",$T19=\"PCBL\"), \"\",getDischargeAirTemp($T19,$V19,$AD19,$W19,BD19,$AL19, $Y19, $AY19, \"heating\",activeElevation,$AB19,$AJ19,$AV19,$BB19)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T19=\"Select Model\", \"\",IF(OR($T19=\"ACBC_1W\",$T19=\"ACBC_2W\",LEFT($T19,4)=\"ACBR\",$T19 = \"LIU24_2W\",LEFT($T19,3)=\"RIU\",LEFT($T19,6)=\"ACBL12\"), IF((soundLevel($T19, $AB19, BD19, $Y19, $W19,$AJ19,$AA19,\"dba\"))<15,\"<15\",soundLevel($T19, $AB19, BD19, $Y19, $W19,$AJ19,$AA19,\"dba\")+0.4),IF((soundLevel($T19, $AB19, BD19, $Y19, $W19,$AJ19,$AA19,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T19, $AB19, BD19, $Y19, $W19,$AJ19,$AA19,\"dba\")+5)<15, \"<15\", soundLevel($T19, $AB19, BD19,$Y19, $W19,$AJ19,$AA19,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T19=\"Select Model\", \"\",IF(OR($T19=\"ACBC_1W\",$T19=\"ACBC_2W\",LEFT($T19,4)=\"ACBR\",$T19=\"LIU24_2W\",LEFT($T19,3)=\"RIU\",LEFT($T19,6)=\"ACBL12\"), IF((soundLevel($T19, $AB19, BD19, $Y19, $W19,$AJ19,$AA19,\"NC\"))<15,\"<15\",soundLevel($T19, $AB19, BD19, $Y19, $W19,$AJ19,$AA19,\"NC\")+0.4),IF((soundLevel($T19, $AB19, BD19, $Y19, $W19,$AJ19,$AA19,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T19, $AB19, BD19, $Y19, $W19,$AJ19,$AA19,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T19, $AB19, BD19, $Y19, $W19,$AJ19,$AA19,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T19=\"Select Model\",\"\",IF($T19=\"LIU24_2W\",calcQwIP($Y19,$W19,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC19,$AI19,\"latent\",$U19&\"P\"&IF($V19=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T19,activeElevation),\"\"))","v":""},{"$f":"IF($T19=\"Select Model\",\"\",IF($T19=\"ACBC_1W\",calcQwIP($Y19,$W19,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC19,BD19,\"capacity\",$U19&\"P\"&IF($V19=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T19,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y19,$W19,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC19,BD19,\"capacity\",$U19&\"P\"&IF($V19=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T19,activeElevation)))","v":""},"",{"$f":"IF(T19=\"Select Model\", 0,waterPressureDrop(W19, U19 & \"P\" & IF(V19=\"Dual\",2,1) &\"C\", AC19, \"cooling\", T19))","v":0},{"$f":"IF(T19=\"Select Model\", \"\",getReturnWaterTemp(T19,AC19, activeEWTCooling, AS19, \"cooling\"))","v":""},"",{"$f":"IF($T19<>\"ACBC_1W\",\"\",IF($J19=\"\",\"\",FintubeCapacity($T19,$W19,$AE19,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T19=\"Select Model\",T19=\"PCBL\"),\"\",calcQwIP(Y19,W19,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD19,BD19,\"capacity\",U19&\"P\"&IF(V19=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T19,activeElevation))","v":""},"",{"$f":"IF(OR(T19=\"Select Model\",T19=\"PCBL\"), \"\",IF(AY19=0,\"N/A\",waterPressureDrop(W19, U19 & \"P\" & IF(V19=\"Dual\",2,1) &\"C\", AD19, \"heating\", T19)))","v":""},{"$f":"IF(OR(T19=\"Select Model\",T19=\"PCBL\"), \"\",IF(AY19=0,getReturnWaterTemp(T19,AE19, activeEWTHeating, AX19, \"heating\"),getReturnWaterTemp(T19,AD19, activeEWTHeating, AY19, \"heating\")))","v":""},"",{"$f":" getNozzle(T19, W19, Y19, Z19, activeElevation, TRUE)","v":0}]
["Dew Point","⁰F",{"$f":"getDewPointFromRH(C18,C17,$A$13)","v":55.181526218884954},{"$f":"getDewPointFromRH(D18,D17,$A$13)","v":52.428836553616385},null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I20)),I20<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I20, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H20)),H20<0),\"\",intlEstQuantity(T20, W20*12, H20)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T20=\"Select Model\",\"\",coilCircuitChange(W20, U20, AC20, T20,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T20=\"Select Model\",\"\",beamWidth(T20))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T20=\"Select Model\",T20=\"PCBL\"), 0,getSPIP(T20, W20, Y20, BD20, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T20=\"Select Model\", \"\",IF(T20=\"PCBL\",0,primaryAirSensibleCapacityIP($T20,$W20,activeRoomTempCooling,activePriAirTempCooling,$Y20,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T20=\"Select Model\",\"\",IF($T20=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y20,activeElevation)))","v":""},{"$f":"IF(OR(T20=\"Select Model\",T20=\"PCBL\"), 0,IF(AD20=0,0,-primaryAirSensibleCapacityIP($T20,$W20,activeRoomTempHeating,activePriAirTempHeating,$Y20,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T20=\"Select Model\", \"\", InductionRatio($T20,BD20,$W20,$Y20)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T20=\"Select Model\", \"\",IF($T20=\"PCBL\",\"N/A\",minVAVSetBack(AA20, Y20))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T20=\"Select Model\", \"\",IF($T20= \"PCBL\",\"N/A\",getDischargeAirTemp($T20,$V20,$AC20,$W20,BD20,$AL20, $Y20, $AS20, \"cooling\",activeElevation,$AB20,$AJ20,$AV20,$BB20))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T20=\"Select Model\",$T20=\"PCBL\"), \"\",getDischargeAirTemp($T20,$V20,$AD20,$W20,BD20,$AL20, $Y20, $AY20, \"heating\",activeElevation,$AB20,$AJ20,$AV20,$BB20)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T20=\"Select Model\", \"\",IF(OR($T20=\"ACBC_1W\",$T20=\"ACBC_2W\",LEFT($T20,4)=\"ACBR\",$T20 = \"LIU24_2W\",LEFT($T20,3)=\"RIU\",LEFT($T20,6)=\"ACBL12\"), IF((soundLevel($T20, $AB20, BD20, $Y20, $W20,$AJ20,$AA20,\"dba\"))<15,\"<15\",soundLevel($T20, $AB20, BD20, $Y20, $W20,$AJ20,$AA20,\"dba\")+0.4),IF((soundLevel($T20, $AB20, BD20, $Y20, $W20,$AJ20,$AA20,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T20, $AB20, BD20, $Y20, $W20,$AJ20,$AA20,\"dba\")+5)<15, \"<15\", soundLevel($T20, $AB20, BD20,$Y20, $W20,$AJ20,$AA20,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T20=\"Select Model\", \"\",IF(OR($T20=\"ACBC_1W\",$T20=\"ACBC_2W\",LEFT($T20,4)=\"ACBR\",$T20=\"LIU24_2W\",LEFT($T20,3)=\"RIU\",LEFT($T20,6)=\"ACBL12\"), IF((soundLevel($T20, $AB20, BD20, $Y20, $W20,$AJ20,$AA20,\"NC\"))<15,\"<15\",soundLevel($T20, $AB20, BD20, $Y20, $W20,$AJ20,$AA20,\"NC\")+0.4),IF((soundLevel($T20, $AB20, BD20, $Y20, $W20,$AJ20,$AA20,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T20, $AB20, BD20, $Y20, $W20,$AJ20,$AA20,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T20, $AB20, BD20, $Y20, $W20,$AJ20,$AA20,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T20=\"Select Model\",\"\",IF($T20=\"LIU24_2W\",calcQwIP($Y20,$W20,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC20,$AI20,\"latent\",$U20&\"P\"&IF($V20=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T20,activeElevation),\"\"))","v":""},{"$f":"IF($T20=\"Select Model\",\"\",IF($T20=\"ACBC_1W\",calcQwIP($Y20,$W20,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC20,BD20,\"capacity\",$U20&\"P\"&IF($V20=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T20,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y20,$W20,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC20,BD20,\"capacity\",$U20&\"P\"&IF($V20=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T20,activeElevation)))","v":""},"",{"$f":"IF(T20=\"Select Model\", 0,waterPressureDrop(W20, U20 & \"P\" & IF(V20=\"Dual\",2,1) &\"C\", AC20, \"cooling\", T20))","v":0},{"$f":"IF(T20=\"Select Model\", \"\",getReturnWaterTemp(T20,AC20, activeEWTCooling, AS20, \"cooling\"))","v":""},"",{"$f":"IF($T20<>\"ACBC_1W\",\"\",IF($J20=\"\",\"\",FintubeCapacity($T20,$W20,$AE20,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T20=\"Select Model\",T20=\"PCBL\"),\"\",calcQwIP(Y20,W20,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD20,BD20,\"capacity\",U20&\"P\"&IF(V20=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T20,activeElevation))","v":""},"",{"$f":"IF(OR(T20=\"Select Model\",T20=\"PCBL\"), \"\",IF(AY20=0,\"N/A\",waterPressureDrop(W20, U20 & \"P\" & IF(V20=\"Dual\",2,1) &\"C\", AD20, \"heating\", T20)))","v":""},{"$f":"IF(OR(T20=\"Select Model\",T20=\"PCBL\"), \"\",IF(AY20=0,getReturnWaterTemp(T20,AE20, activeEWTHeating, AX20, \"heating\"),getReturnWaterTemp(T20,AD20, activeEWTHeating, AY20, \"heating\")))","v":""},"",{"$f":" getNozzle(T20, W20, Y20, Z20, activeElevation, TRUE)","v":0}]
[null,"gr/lb",{"$f":"getgrainperpound(C18,C17,$A$13)","v":64.649670871442396},{"$f":"getgrainperpound(D18,D17,$A$13)","v":58.364961883371663},null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I21)),I21<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I21, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H21)),H21<0),\"\",intlEstQuantity(T21, W21*12, H21)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T21=\"Select Model\",\"\",coilCircuitChange(W21, U21, AC21, T21,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T21=\"Select Model\",\"\",beamWidth(T21))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T21=\"Select Model\",T21=\"PCBL\"), 0,getSPIP(T21, W21, Y21, BD21, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T21=\"Select Model\", \"\",IF(T21=\"PCBL\",0,primaryAirSensibleCapacityIP($T21,$W21,activeRoomTempCooling,activePriAirTempCooling,$Y21,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T21=\"Select Model\",\"\",IF($T21=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y21,activeElevation)))","v":""},{"$f":"IF(OR(T21=\"Select Model\",T21=\"PCBL\"), 0,IF(AD21=0,0,-primaryAirSensibleCapacityIP($T21,$W21,activeRoomTempHeating,activePriAirTempHeating,$Y21,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T21=\"Select Model\", \"\", InductionRatio($T21,BD21,$W21,$Y21)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T21=\"Select Model\", \"\",IF($T21=\"PCBL\",\"N/A\",minVAVSetBack(AA21, Y21))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T21=\"Select Model\", \"\",IF($T21= \"PCBL\",\"N/A\",getDischargeAirTemp($T21,$V21,$AC21,$W21,BD21,$AL21, $Y21, $AS21, \"cooling\",activeElevation,$AB21,$AJ21,$AV21,$BB21))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T21=\"Select Model\",$T21=\"PCBL\"), \"\",getDischargeAirTemp($T21,$V21,$AD21,$W21,BD21,$AL21, $Y21, $AY21, \"heating\",activeElevation,$AB21,$AJ21,$AV21,$BB21)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T21=\"Select Model\", \"\",IF(OR($T21=\"ACBC_1W\",$T21=\"ACBC_2W\",LEFT($T21,4)=\"ACBR\",$T21 = \"LIU24_2W\",LEFT($T21,3)=\"RIU\",LEFT($T21,6)=\"ACBL12\"), IF((soundLevel($T21, $AB21, BD21, $Y21, $W21,$AJ21,$AA21,\"dba\"))<15,\"<15\",soundLevel($T21, $AB21, BD21, $Y21, $W21,$AJ21,$AA21,\"dba\")+0.4),IF((soundLevel($T21, $AB21, BD21, $Y21, $W21,$AJ21,$AA21,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T21, $AB21, BD21, $Y21, $W21,$AJ21,$AA21,\"dba\")+5)<15, \"<15\", soundLevel($T21, $AB21, BD21,$Y21, $W21,$AJ21,$AA21,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T21=\"Select Model\", \"\",IF(OR($T21=\"ACBC_1W\",$T21=\"ACBC_2W\",LEFT($T21,4)=\"ACBR\",$T21=\"LIU24_2W\",LEFT($T21,3)=\"RIU\",LEFT($T21,6)=\"ACBL12\"), IF((soundLevel($T21, $AB21, BD21, $Y21, $W21,$AJ21,$AA21,\"NC\"))<15,\"<15\",soundLevel($T21, $AB21, BD21, $Y21, $W21,$AJ21,$AA21,\"NC\")+0.4),IF((soundLevel($T21, $AB21, BD21, $Y21, $W21,$AJ21,$AA21,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T21, $AB21, BD21, $Y21, $W21,$AJ21,$AA21,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T21, $AB21, BD21, $Y21, $W21,$AJ21,$AA21,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T21=\"Select Model\",\"\",IF($T21=\"LIU24_2W\",calcQwIP($Y21,$W21,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC21,$AI21,\"latent\",$U21&\"P\"&IF($V21=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T21,activeElevation),\"\"))","v":""},{"$f":"IF($T21=\"Select Model\",\"\",IF($T21=\"ACBC_1W\",calcQwIP($Y21,$W21,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC21,BD21,\"capacity\",$U21&\"P\"&IF($V21=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T21,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y21,$W21,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC21,BD21,\"capacity\",$U21&\"P\"&IF($V21=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T21,activeElevation)))","v":""},"",{"$f":"IF(T21=\"Select Model\", 0,waterPressureDrop(W21, U21 & \"P\" & IF(V21=\"Dual\",2,1) &\"C\", AC21, \"cooling\", T21))","v":0},{"$f":"IF(T21=\"Select Model\", \"\",getReturnWaterTemp(T21,AC21, activeEWTCooling, AS21, \"cooling\"))","v":""},"",{"$f":"IF($T21<>\"ACBC_1W\",\"\",IF($J21=\"\",\"\",FintubeCapacity($T21,$W21,$AE21,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T21=\"Select Model\",T21=\"PCBL\"),\"\",calcQwIP(Y21,W21,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD21,BD21,\"capacity\",U21&\"P\"&IF(V21=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T21,activeElevation))","v":""},"",{"$f":"IF(OR(T21=\"Select Model\",T21=\"PCBL\"), \"\",IF(AY21=0,\"N/A\",waterPressureDrop(W21, U21 & \"P\" & IF(V21=\"Dual\",2,1) &\"C\", AD21, \"heating\", T21)))","v":""},{"$f":"IF(OR(T21=\"Select Model\",T21=\"PCBL\"), \"\",IF(AY21=0,getReturnWaterTemp(T21,AE21, activeEWTHeating, AX21, \"heating\"),getReturnWaterTemp(T21,AD21, activeEWTHeating, AY21, \"heating\")))","v":""},"",{"$f":" getNozzle(T21, W21, Y21, Z21, activeElevation, TRUE)","v":0}]
["On-Coil Temperature ⁰F\n(if different to Room Dry Bulb)",null,{"$f":"activeRoomTempCooling","v":75},{"$f":"D17","v":72},null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I22)),I22<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I22, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H22)),H22<0),\"\",intlEstQuantity(T22, W22*12, H22)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T22=\"Select Model\",\"\",coilCircuitChange(W22, U22, AC22, T22,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T22=\"Select Model\",\"\",beamWidth(T22))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T22=\"Select Model\",T22=\"PCBL\"), 0,getSPIP(T22, W22, Y22, BD22, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T22=\"Select Model\", \"\",IF(T22=\"PCBL\",0,primaryAirSensibleCapacityIP($T22,$W22,activeRoomTempCooling,activePriAirTempCooling,$Y22,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T22=\"Select Model\",\"\",IF($T22=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y22,activeElevation)))","v":""},{"$f":"IF(OR(T22=\"Select Model\",T22=\"PCBL\"), 0,IF(AD22=0,0,-primaryAirSensibleCapacityIP($T22,$W22,activeRoomTempHeating,activePriAirTempHeating,$Y22,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T22=\"Select Model\", \"\", InductionRatio($T22,BD22,$W22,$Y22)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T22=\"Select Model\", \"\",IF($T22=\"PCBL\",\"N/A\",minVAVSetBack(AA22, Y22))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T22=\"Select Model\", \"\",IF($T22= \"PCBL\",\"N/A\",getDischargeAirTemp($T22,$V22,$AC22,$W22,BD22,$AL22, $Y22, $AS22, \"cooling\",activeElevation,$AB22,$AJ22,$AV22,$BB22))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T22=\"Select Model\",$T22=\"PCBL\"), \"\",getDischargeAirTemp($T22,$V22,$AD22,$W22,BD22,$AL22, $Y22, $AY22, \"heating\",activeElevation,$AB22,$AJ22,$AV22,$BB22)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T22=\"Select Model\", \"\",IF(OR($T22=\"ACBC_1W\",$T22=\"ACBC_2W\",LEFT($T22,4)=\"ACBR\",$T22 = \"LIU24_2W\",LEFT($T22,3)=\"RIU\",LEFT($T22,6)=\"ACBL12\"), IF((soundLevel($T22, $AB22, BD22, $Y22, $W22,$AJ22,$AA22,\"dba\"))<15,\"<15\",soundLevel($T22, $AB22, BD22, $Y22, $W22,$AJ22,$AA22,\"dba\")+0.4),IF((soundLevel($T22, $AB22, BD22, $Y22, $W22,$AJ22,$AA22,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T22, $AB22, BD22, $Y22, $W22,$AJ22,$AA22,\"dba\")+5)<15, \"<15\", soundLevel($T22, $AB22, BD22,$Y22, $W22,$AJ22,$AA22,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T22=\"Select Model\", \"\",IF(OR($T22=\"ACBC_1W\",$T22=\"ACBC_2W\",LEFT($T22,4)=\"ACBR\",$T22=\"LIU24_2W\",LEFT($T22,3)=\"RIU\",LEFT($T22,6)=\"ACBL12\"), IF((soundLevel($T22, $AB22, BD22, $Y22, $W22,$AJ22,$AA22,\"NC\"))<15,\"<15\",soundLevel($T22, $AB22, BD22, $Y22, $W22,$AJ22,$AA22,\"NC\")+0.4),IF((soundLevel($T22, $AB22, BD22, $Y22, $W22,$AJ22,$AA22,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T22, $AB22, BD22, $Y22, $W22,$AJ22,$AA22,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T22, $AB22, BD22, $Y22, $W22,$AJ22,$AA22,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T22=\"Select Model\",\"\",IF($T22=\"LIU24_2W\",calcQwIP($Y22,$W22,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC22,$AI22,\"latent\",$U22&\"P\"&IF($V22=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T22,activeElevation),\"\"))","v":""},{"$f":"IF($T22=\"Select Model\",\"\",IF($T22=\"ACBC_1W\",calcQwIP($Y22,$W22,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC22,BD22,\"capacity\",$U22&\"P\"&IF($V22=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T22,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y22,$W22,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC22,BD22,\"capacity\",$U22&\"P\"&IF($V22=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T22,activeElevation)))","v":""},"",{"$f":"IF(T22=\"Select Model\", 0,waterPressureDrop(W22, U22 & \"P\" & IF(V22=\"Dual\",2,1) &\"C\", AC22, \"cooling\", T22))","v":0},{"$f":"IF(T22=\"Select Model\", \"\",getReturnWaterTemp(T22,AC22, activeEWTCooling, AS22, \"cooling\"))","v":""},"",{"$f":"IF($T22<>\"ACBC_1W\",\"\",IF($J22=\"\",\"\",FintubeCapacity($T22,$W22,$AE22,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T22=\"Select Model\",T22=\"PCBL\"),\"\",calcQwIP(Y22,W22,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD22,BD22,\"capacity\",U22&\"P\"&IF(V22=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T22,activeElevation))","v":""},"",{"$f":"IF(OR(T22=\"Select Model\",T22=\"PCBL\"), \"\",IF(AY22=0,\"N/A\",waterPressureDrop(W22, U22 & \"P\" & IF(V22=\"Dual\",2,1) &\"C\", AD22, \"heating\", T22)))","v":""},{"$f":"IF(OR(T22=\"Select Model\",T22=\"PCBL\"), \"\",IF(AY22=0,getReturnWaterTemp(T22,AE22, activeEWTHeating, AX22, \"heating\"),getReturnWaterTemp(T22,AD22, activeEWTHeating, AY22, \"heating\")))","v":""},"",{"$f":" getNozzle(T22, W22, Y22, Z22, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I23)),I23<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I23, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H23)),H23<0),\"\",intlEstQuantity(T23, W23*12, H23)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T23=\"Select Model\",\"\",coilCircuitChange(W23, U23, AC23, T23,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T23=\"Select Model\",\"\",beamWidth(T23))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T23=\"Select Model\",T23=\"PCBL\"), 0,getSPIP(T23, W23, Y23, BD23, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T23=\"Select Model\", \"\",IF(T23=\"PCBL\",0,primaryAirSensibleCapacityIP($T23,$W23,activeRoomTempCooling,activePriAirTempCooling,$Y23,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T23=\"Select Model\",\"\",IF($T23=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y23,activeElevation)))","v":""},{"$f":"IF(OR(T23=\"Select Model\",T23=\"PCBL\"), 0,IF(AD23=0,0,-primaryAirSensibleCapacityIP($T23,$W23,activeRoomTempHeating,activePriAirTempHeating,$Y23,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T23=\"Select Model\", \"\", InductionRatio($T23,BD23,$W23,$Y23)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T23=\"Select Model\", \"\",IF($T23=\"PCBL\",\"N/A\",minVAVSetBack(AA23, Y23))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T23=\"Select Model\", \"\",IF($T23= \"PCBL\",\"N/A\",getDischargeAirTemp($T23,$V23,$AC23,$W23,BD23,$AL23, $Y23, $AS23, \"cooling\",activeElevation,$AB23,$AJ23,$AV23,$BB23))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T23=\"Select Model\",$T23=\"PCBL\"), \"\",getDischargeAirTemp($T23,$V23,$AD23,$W23,BD23,$AL23, $Y23, $AY23, \"heating\",activeElevation,$AB23,$AJ23,$AV23,$BB23)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T23=\"Select Model\", \"\",IF(OR($T23=\"ACBC_1W\",$T23=\"ACBC_2W\",LEFT($T23,4)=\"ACBR\",$T23 = \"LIU24_2W\",LEFT($T23,3)=\"RIU\",LEFT($T23,6)=\"ACBL12\"), IF((soundLevel($T23, $AB23, BD23, $Y23, $W23,$AJ23,$AA23,\"dba\"))<15,\"<15\",soundLevel($T23, $AB23, BD23, $Y23, $W23,$AJ23,$AA23,\"dba\")+0.4),IF((soundLevel($T23, $AB23, BD23, $Y23, $W23,$AJ23,$AA23,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T23, $AB23, BD23, $Y23, $W23,$AJ23,$AA23,\"dba\")+5)<15, \"<15\", soundLevel($T23, $AB23, BD23,$Y23, $W23,$AJ23,$AA23,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T23=\"Select Model\", \"\",IF(OR($T23=\"ACBC_1W\",$T23=\"ACBC_2W\",LEFT($T23,4)=\"ACBR\",$T23=\"LIU24_2W\",LEFT($T23,3)=\"RIU\",LEFT($T23,6)=\"ACBL12\"), IF((soundLevel($T23, $AB23, BD23, $Y23, $W23,$AJ23,$AA23,\"NC\"))<15,\"<15\",soundLevel($T23, $AB23, BD23, $Y23, $W23,$AJ23,$AA23,\"NC\")+0.4),IF((soundLevel($T23, $AB23, BD23, $Y23, $W23,$AJ23,$AA23,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T23, $AB23, BD23, $Y23, $W23,$AJ23,$AA23,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T23, $AB23, BD23, $Y23, $W23,$AJ23,$AA23,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T23=\"Select Model\",\"\",IF($T23=\"LIU24_2W\",calcQwIP($Y23,$W23,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC23,$AI23,\"latent\",$U23&\"P\"&IF($V23=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T23,activeElevation),\"\"))","v":""},{"$f":"IF($T23=\"Select Model\",\"\",IF($T23=\"ACBC_1W\",calcQwIP($Y23,$W23,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC23,BD23,\"capacity\",$U23&\"P\"&IF($V23=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T23,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y23,$W23,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC23,BD23,\"capacity\",$U23&\"P\"&IF($V23=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T23,activeElevation)))","v":""},"",{"$f":"IF(T23=\"Select Model\", 0,waterPressureDrop(W23, U23 & \"P\" & IF(V23=\"Dual\",2,1) &\"C\", AC23, \"cooling\", T23))","v":0},{"$f":"IF(T23=\"Select Model\", \"\",getReturnWaterTemp(T23,AC23, activeEWTCooling, AS23, \"cooling\"))","v":""},"",{"$f":"IF($T23<>\"ACBC_1W\",\"\",IF($J23=\"\",\"\",FintubeCapacity($T23,$W23,$AE23,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T23=\"Select Model\",T23=\"PCBL\"),\"\",calcQwIP(Y23,W23,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD23,BD23,\"capacity\",U23&\"P\"&IF(V23=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T23,activeElevation))","v":""},"",{"$f":"IF(OR(T23=\"Select Model\",T23=\"PCBL\"), \"\",IF(AY23=0,\"N/A\",waterPressureDrop(W23, U23 & \"P\" & IF(V23=\"Dual\",2,1) &\"C\", AD23, \"heating\", T23)))","v":""},{"$f":"IF(OR(T23=\"Select Model\",T23=\"PCBL\"), \"\",IF(AY23=0,getReturnWaterTemp(T23,AE23, activeEWTHeating, AX23, \"heating\"),getReturnWaterTemp(T23,AD23, activeEWTHeating, AY23, \"heating\")))","v":""},"",{"$f":" getNozzle(T23, W23, Y23, Z23, activeElevation, TRUE)","v":0}]
["Noise NC",null,30,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I24)),I24<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I24, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H24)),H24<0),\"\",intlEstQuantity(T24, W24*12, H24)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T24=\"Select Model\",\"\",coilCircuitChange(W24, U24, AC24, T24,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T24=\"Select Model\",\"\",beamWidth(T24))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T24=\"Select Model\",T24=\"PCBL\"), 0,getSPIP(T24, W24, Y24, BD24, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T24=\"Select Model\", \"\",IF(T24=\"PCBL\",0,primaryAirSensibleCapacityIP($T24,$W24,activeRoomTempCooling,activePriAirTempCooling,$Y24,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T24=\"Select Model\",\"\",IF($T24=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y24,activeElevation)))","v":""},{"$f":"IF(OR(T24=\"Select Model\",T24=\"PCBL\"), 0,IF(AD24=0,0,-primaryAirSensibleCapacityIP($T24,$W24,activeRoomTempHeating,activePriAirTempHeating,$Y24,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T24=\"Select Model\", \"\", InductionRatio($T24,BD24,$W24,$Y24)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T24=\"Select Model\", \"\",IF($T24=\"PCBL\",\"N/A\",minVAVSetBack(AA24, Y24))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T24=\"Select Model\", \"\",IF($T24= \"PCBL\",\"N/A\",getDischargeAirTemp($T24,$V24,$AC24,$W24,BD24,$AL24, $Y24, $AS24, \"cooling\",activeElevation,$AB24,$AJ24,$AV24,$BB24))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T24=\"Select Model\",$T24=\"PCBL\"), \"\",getDischargeAirTemp($T24,$V24,$AD24,$W24,BD24,$AL24, $Y24, $AY24, \"heating\",activeElevation,$AB24,$AJ24,$AV24,$BB24)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T24=\"Select Model\", \"\",IF(OR($T24=\"ACBC_1W\",$T24=\"ACBC_2W\",LEFT($T24,4)=\"ACBR\",$T24 = \"LIU24_2W\",LEFT($T24,3)=\"RIU\",LEFT($T24,6)=\"ACBL12\"), IF((soundLevel($T24, $AB24, BD24, $Y24, $W24,$AJ24,$AA24,\"dba\"))<15,\"<15\",soundLevel($T24, $AB24, BD24, $Y24, $W24,$AJ24,$AA24,\"dba\")+0.4),IF((soundLevel($T24, $AB24, BD24, $Y24, $W24,$AJ24,$AA24,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T24, $AB24, BD24, $Y24, $W24,$AJ24,$AA24,\"dba\")+5)<15, \"<15\", soundLevel($T24, $AB24, BD24,$Y24, $W24,$AJ24,$AA24,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T24=\"Select Model\", \"\",IF(OR($T24=\"ACBC_1W\",$T24=\"ACBC_2W\",LEFT($T24,4)=\"ACBR\",$T24=\"LIU24_2W\",LEFT($T24,3)=\"RIU\",LEFT($T24,6)=\"ACBL12\"), IF((soundLevel($T24, $AB24, BD24, $Y24, $W24,$AJ24,$AA24,\"NC\"))<15,\"<15\",soundLevel($T24, $AB24, BD24, $Y24, $W24,$AJ24,$AA24,\"NC\")+0.4),IF((soundLevel($T24, $AB24, BD24, $Y24, $W24,$AJ24,$AA24,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T24, $AB24, BD24, $Y24, $W24,$AJ24,$AA24,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T24, $AB24, BD24, $Y24, $W24,$AJ24,$AA24,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T24=\"Select Model\",\"\",IF($T24=\"LIU24_2W\",calcQwIP($Y24,$W24,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC24,$AI24,\"latent\",$U24&\"P\"&IF($V24=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T24,activeElevation),\"\"))","v":""},{"$f":"IF($T24=\"Select Model\",\"\",IF($T24=\"ACBC_1W\",calcQwIP($Y24,$W24,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC24,BD24,\"capacity\",$U24&\"P\"&IF($V24=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T24,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y24,$W24,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC24,BD24,\"capacity\",$U24&\"P\"&IF($V24=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T24,activeElevation)))","v":""},"",{"$f":"IF(T24=\"Select Model\", 0,waterPressureDrop(W24, U24 & \"P\" & IF(V24=\"Dual\",2,1) &\"C\", AC24, \"cooling\", T24))","v":0},{"$f":"IF(T24=\"Select Model\", \"\",getReturnWaterTemp(T24,AC24, activeEWTCooling, AS24, \"cooling\"))","v":""},"",{"$f":"IF($T24<>\"ACBC_1W\",\"\",IF($J24=\"\",\"\",FintubeCapacity($T24,$W24,$AE24,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T24=\"Select Model\",T24=\"PCBL\"),\"\",calcQwIP(Y24,W24,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD24,BD24,\"capacity\",U24&\"P\"&IF(V24=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T24,activeElevation))","v":""},"",{"$f":"IF(OR(T24=\"Select Model\",T24=\"PCBL\"), \"\",IF(AY24=0,\"N/A\",waterPressureDrop(W24, U24 & \"P\" & IF(V24=\"Dual\",2,1) &\"C\", AD24, \"heating\", T24)))","v":""},{"$f":"IF(OR(T24=\"Select Model\",T24=\"PCBL\"), \"\",IF(AY24=0,getReturnWaterTemp(T24,AE24, activeEWTHeating, AX24, \"heating\"),getReturnWaterTemp(T24,AD24, activeEWTHeating, AY24, \"heating\")))","v":""},"",{"$f":" getNozzle(T24, W24, Y24, Z24, activeElevation, TRUE)","v":0}]
["Room Attenuation (dB)",null,10,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I25)),I25<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I25, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H25)),H25<0),\"\",intlEstQuantity(T25, W25*12, H25)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T25=\"Select Model\",\"\",coilCircuitChange(W25, U25, AC25, T25,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T25=\"Select Model\",\"\",beamWidth(T25))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T25=\"Select Model\",T25=\"PCBL\"), 0,getSPIP(T25, W25, Y25, BD25, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T25=\"Select Model\", \"\",IF(T25=\"PCBL\",0,primaryAirSensibleCapacityIP($T25,$W25,activeRoomTempCooling,activePriAirTempCooling,$Y25,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T25=\"Select Model\",\"\",IF($T25=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y25,activeElevation)))","v":""},{"$f":"IF(OR(T25=\"Select Model\",T25=\"PCBL\"), 0,IF(AD25=0,0,-primaryAirSensibleCapacityIP($T25,$W25,activeRoomTempHeating,activePriAirTempHeating,$Y25,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T25=\"Select Model\", \"\", InductionRatio($T25,BD25,$W25,$Y25)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T25=\"Select Model\", \"\",IF($T25=\"PCBL\",\"N/A\",minVAVSetBack(AA25, Y25))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T25=\"Select Model\", \"\",IF($T25= \"PCBL\",\"N/A\",getDischargeAirTemp($T25,$V25,$AC25,$W25,BD25,$AL25, $Y25, $AS25, \"cooling\",activeElevation,$AB25,$AJ25,$AV25,$BB25))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T25=\"Select Model\",$T25=\"PCBL\"), \"\",getDischargeAirTemp($T25,$V25,$AD25,$W25,BD25,$AL25, $Y25, $AY25, \"heating\",activeElevation,$AB25,$AJ25,$AV25,$BB25)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T25=\"Select Model\", \"\",IF(OR($T25=\"ACBC_1W\",$T25=\"ACBC_2W\",LEFT($T25,4)=\"ACBR\",$T25 = \"LIU24_2W\",LEFT($T25,3)=\"RIU\",LEFT($T25,6)=\"ACBL12\"), IF((soundLevel($T25, $AB25, BD25, $Y25, $W25,$AJ25,$AA25,\"dba\"))<15,\"<15\",soundLevel($T25, $AB25, BD25, $Y25, $W25,$AJ25,$AA25,\"dba\")+0.4),IF((soundLevel($T25, $AB25, BD25, $Y25, $W25,$AJ25,$AA25,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T25, $AB25, BD25, $Y25, $W25,$AJ25,$AA25,\"dba\")+5)<15, \"<15\", soundLevel($T25, $AB25, BD25,$Y25, $W25,$AJ25,$AA25,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T25=\"Select Model\", \"\",IF(OR($T25=\"ACBC_1W\",$T25=\"ACBC_2W\",LEFT($T25,4)=\"ACBR\",$T25=\"LIU24_2W\",LEFT($T25,3)=\"RIU\",LEFT($T25,6)=\"ACBL12\"), IF((soundLevel($T25, $AB25, BD25, $Y25, $W25,$AJ25,$AA25,\"NC\"))<15,\"<15\",soundLevel($T25, $AB25, BD25, $Y25, $W25,$AJ25,$AA25,\"NC\")+0.4),IF((soundLevel($T25, $AB25, BD25, $Y25, $W25,$AJ25,$AA25,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T25, $AB25, BD25, $Y25, $W25,$AJ25,$AA25,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T25, $AB25, BD25, $Y25, $W25,$AJ25,$AA25,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T25=\"Select Model\",\"\",IF($T25=\"LIU24_2W\",calcQwIP($Y25,$W25,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC25,$AI25,\"latent\",$U25&\"P\"&IF($V25=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T25,activeElevation),\"\"))","v":""},{"$f":"IF($T25=\"Select Model\",\"\",IF($T25=\"ACBC_1W\",calcQwIP($Y25,$W25,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC25,BD25,\"capacity\",$U25&\"P\"&IF($V25=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T25,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y25,$W25,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC25,BD25,\"capacity\",$U25&\"P\"&IF($V25=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T25,activeElevation)))","v":""},"",{"$f":"IF(T25=\"Select Model\", 0,waterPressureDrop(W25, U25 & \"P\" & IF(V25=\"Dual\",2,1) &\"C\", AC25, \"cooling\", T25))","v":0},{"$f":"IF(T25=\"Select Model\", \"\",getReturnWaterTemp(T25,AC25, activeEWTCooling, AS25, \"cooling\"))","v":""},"",{"$f":"IF($T25<>\"ACBC_1W\",\"\",IF($J25=\"\",\"\",FintubeCapacity($T25,$W25,$AE25,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T25=\"Select Model\",T25=\"PCBL\"),\"\",calcQwIP(Y25,W25,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD25,BD25,\"capacity\",U25&\"P\"&IF(V25=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T25,activeElevation))","v":""},"",{"$f":"IF(OR(T25=\"Select Model\",T25=\"PCBL\"), \"\",IF(AY25=0,\"N/A\",waterPressureDrop(W25, U25 & \"P\" & IF(V25=\"Dual\",2,1) &\"C\", AD25, \"heating\", T25)))","v":""},{"$f":"IF(OR(T25=\"Select Model\",T25=\"PCBL\"), \"\",IF(AY25=0,getReturnWaterTemp(T25,AE25, activeEWTHeating, AX25, \"heating\"),getReturnWaterTemp(T25,AD25, activeEWTHeating, AY25, \"heating\")))","v":""},"",{"$f":" getNozzle(T25, W25, Y25, Z25, activeElevation, TRUE)","v":0}]
["Primary Air Conditions (ducted to room)",null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I26)),I26<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I26, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H26)),H26<0),\"\",intlEstQuantity(T26, W26*12, H26)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T26=\"Select Model\",\"\",coilCircuitChange(W26, U26, AC26, T26,activeMaxWaterPressureDrop))","v":""},4.33,{"$f":"IF(T26=\"Select Model\",\"\",beamWidth(T26))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T26=\"Select Model\",T26=\"PCBL\"), 0,getSPIP(T26, W26, Y26, BD26, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T26=\"Select Model\", \"\",IF(T26=\"PCBL\",0,primaryAirSensibleCapacityIP($T26,$W26,activeRoomTempCooling,activePriAirTempCooling,$Y26,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T26=\"Select Model\",\"\",IF($T26=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y26,activeElevation)))","v":""},{"$f":"IF(OR(T26=\"Select Model\",T26=\"PCBL\"), 0,IF(AD26=0,0,-primaryAirSensibleCapacityIP($T26,$W26,activeRoomTempHeating,activePriAirTempHeating,$Y26,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T26=\"Select Model\", \"\", InductionRatio($T26,BD26,$W26,$Y26)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T26=\"Select Model\", \"\",IF($T26=\"PCBL\",\"N/A\",minVAVSetBack(AA26, Y26))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T26=\"Select Model\", \"\",IF($T26= \"PCBL\",\"N/A\",getDischargeAirTemp($T26,$V26,$AC26,$W26,BD26,$AL26, $Y26, $AS26, \"cooling\",activeElevation,$AB26,$AJ26,$AV26,$BB26))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T26=\"Select Model\",$T26=\"PCBL\"), \"\",getDischargeAirTemp($T26,$V26,$AD26,$W26,BD26,$AL26, $Y26, $AY26, \"heating\",activeElevation,$AB26,$AJ26,$AV26,$BB26)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T26=\"Select Model\", \"\",IF(OR($T26=\"ACBC_1W\",$T26=\"ACBC_2W\",LEFT($T26,4)=\"ACBR\",$T26 = \"LIU24_2W\",LEFT($T26,3)=\"RIU\",LEFT($T26,6)=\"ACBL12\"), IF((soundLevel($T26, $AB26, BD26, $Y26, $W26,$AJ26,$AA26,\"dba\"))<15,\"<15\",soundLevel($T26, $AB26, BD26, $Y26, $W26,$AJ26,$AA26,\"dba\")+0.4),IF((soundLevel($T26, $AB26, BD26, $Y26, $W26,$AJ26,$AA26,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T26, $AB26, BD26, $Y26, $W26,$AJ26,$AA26,\"dba\")+5)<15, \"<15\", soundLevel($T26, $AB26, BD26,$Y26, $W26,$AJ26,$AA26,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T26=\"Select Model\", \"\",IF(OR($T26=\"ACBC_1W\",$T26=\"ACBC_2W\",LEFT($T26,4)=\"ACBR\",$T26=\"LIU24_2W\",LEFT($T26,3)=\"RIU\",LEFT($T26,6)=\"ACBL12\"), IF((soundLevel($T26, $AB26, BD26, $Y26, $W26,$AJ26,$AA26,\"NC\"))<15,\"<15\",soundLevel($T26, $AB26, BD26, $Y26, $W26,$AJ26,$AA26,\"NC\")+0.4),IF((soundLevel($T26, $AB26, BD26, $Y26, $W26,$AJ26,$AA26,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T26, $AB26, BD26, $Y26, $W26,$AJ26,$AA26,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T26, $AB26, BD26, $Y26, $W26,$AJ26,$AA26,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T26=\"Select Model\",\"\",IF($T26=\"LIU24_2W\",calcQwIP($Y26,$W26,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC26,$AI26,\"latent\",$U26&\"P\"&IF($V26=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T26,activeElevation),\"\"))","v":""},{"$f":"IF($T26=\"Select Model\",\"\",IF($T26=\"ACBC_1W\",calcQwIP($Y26,$W26,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC26,BD26,\"capacity\",$U26&\"P\"&IF($V26=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T26,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y26,$W26,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC26,BD26,\"capacity\",$U26&\"P\"&IF($V26=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T26,activeElevation)))","v":""},"",{"$f":"IF(T26=\"Select Model\", 0,waterPressureDrop(W26, U26 & \"P\" & IF(V26=\"Dual\",2,1) &\"C\", AC26, \"cooling\", T26))","v":0},{"$f":"IF(T26=\"Select Model\", \"\",getReturnWaterTemp(T26,AC26, activeEWTCooling, AS26, \"cooling\"))","v":""},"",{"$f":"IF($T26<>\"ACBC_1W\",\"\",IF($J26=\"\",\"\",FintubeCapacity($T26,$W26,$AE26,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T26=\"Select Model\",T26=\"PCBL\"),\"\",calcQwIP(Y26,W26,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD26,BD26,\"capacity\",U26&\"P\"&IF(V26=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T26,activeElevation))","v":""},"",{"$f":"IF(OR(T26=\"Select Model\",T26=\"PCBL\"), \"\",IF(AY26=0,\"N/A\",waterPressureDrop(W26, U26 & \"P\" & IF(V26=\"Dual\",2,1) &\"C\", AD26, \"heating\", T26)))","v":""},{"$f":"IF(OR(T26=\"Select Model\",T26=\"PCBL\"), \"\",IF(AY26=0,getReturnWaterTemp(T26,AE26, activeEWTHeating, AX26, \"heating\"),getReturnWaterTemp(T26,AD26, activeEWTHeating, AY26, \"heating\")))","v":""},"",{"$f":" getNozzle(T26, W26, Y26, Z26, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I27)),I27<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I27, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H27)),H27<0),\"\",intlEstQuantity(T27, W27*12, H27)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T27=\"Select Model\",\"\",coilCircuitChange(W27, U27, AC27, T27,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T27=\"Select Model\",\"\",beamWidth(T27))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T27=\"Select Model\",T27=\"PCBL\"), 0,getSPIP(T27, W27, Y27, BD27, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T27=\"Select Model\", \"\",IF(T27=\"PCBL\",0,primaryAirSensibleCapacityIP($T27,$W27,activeRoomTempCooling,activePriAirTempCooling,$Y27,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T27=\"Select Model\",\"\",IF($T27=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y27,activeElevation)))","v":""},{"$f":"IF(OR(T27=\"Select Model\",T27=\"PCBL\"), 0,IF(AD27=0,0,-primaryAirSensibleCapacityIP($T27,$W27,activeRoomTempHeating,activePriAirTempHeating,$Y27,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T27=\"Select Model\", \"\", InductionRatio($T27,BD27,$W27,$Y27)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T27=\"Select Model\", \"\",IF($T27=\"PCBL\",\"N/A\",minVAVSetBack(AA27, Y27))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T27=\"Select Model\", \"\",IF($T27= \"PCBL\",\"N/A\",getDischargeAirTemp($T27,$V27,$AC27,$W27,BD27,$AL27, $Y27, $AS27, \"cooling\",activeElevation,$AB27,$AJ27,$AV27,$BB27))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T27=\"Select Model\",$T27=\"PCBL\"), \"\",getDischargeAirTemp($T27,$V27,$AD27,$W27,BD27,$AL27, $Y27, $AY27, \"heating\",activeElevation,$AB27,$AJ27,$AV27,$BB27)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T27=\"Select Model\", \"\",IF(OR($T27=\"ACBC_1W\",$T27=\"ACBC_2W\",LEFT($T27,4)=\"ACBR\",$T27 = \"LIU24_2W\",LEFT($T27,3)=\"RIU\",LEFT($T27,6)=\"ACBL12\"), IF((soundLevel($T27, $AB27, BD27, $Y27, $W27,$AJ27,$AA27,\"dba\"))<15,\"<15\",soundLevel($T27, $AB27, BD27, $Y27, $W27,$AJ27,$AA27,\"dba\")+0.4),IF((soundLevel($T27, $AB27, BD27, $Y27, $W27,$AJ27,$AA27,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T27, $AB27, BD27, $Y27, $W27,$AJ27,$AA27,\"dba\")+5)<15, \"<15\", soundLevel($T27, $AB27, BD27,$Y27, $W27,$AJ27,$AA27,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T27=\"Select Model\", \"\",IF(OR($T27=\"ACBC_1W\",$T27=\"ACBC_2W\",LEFT($T27,4)=\"ACBR\",$T27=\"LIU24_2W\",LEFT($T27,3)=\"RIU\",LEFT($T27,6)=\"ACBL12\"), IF((soundLevel($T27, $AB27, BD27, $Y27, $W27,$AJ27,$AA27,\"NC\"))<15,\"<15\",soundLevel($T27, $AB27, BD27, $Y27, $W27,$AJ27,$AA27,\"NC\")+0.4),IF((soundLevel($T27, $AB27, BD27, $Y27, $W27,$AJ27,$AA27,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T27, $AB27, BD27, $Y27, $W27,$AJ27,$AA27,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T27, $AB27, BD27, $Y27, $W27,$AJ27,$AA27,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T27=\"Select Model\",\"\",IF($T27=\"LIU24_2W\",calcQwIP($Y27,$W27,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC27,$AI27,\"latent\",$U27&\"P\"&IF($V27=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T27,activeElevation),\"\"))","v":""},{"$f":"IF($T27=\"Select Model\",\"\",IF($T27=\"ACBC_1W\",calcQwIP($Y27,$W27,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC27,BD27,\"capacity\",$U27&\"P\"&IF($V27=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T27,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y27,$W27,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC27,BD27,\"capacity\",$U27&\"P\"&IF($V27=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T27,activeElevation)))","v":""},"",{"$f":"IF(T27=\"Select Model\", 0,waterPressureDrop(W27, U27 & \"P\" & IF(V27=\"Dual\",2,1) &\"C\", AC27, \"cooling\", T27))","v":0},{"$f":"IF(T27=\"Select Model\", \"\",getReturnWaterTemp(T27,AC27, activeEWTCooling, AS27, \"cooling\"))","v":""},"",{"$f":"IF($T27<>\"ACBC_1W\",\"\",IF($J27=\"\",\"\",FintubeCapacity($T27,$W27,$AE27,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T27=\"Select Model\",T27=\"PCBL\"),\"\",calcQwIP(Y27,W27,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD27,BD27,\"capacity\",U27&\"P\"&IF(V27=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T27,activeElevation))","v":""},"",{"$f":"IF(OR(T27=\"Select Model\",T27=\"PCBL\"), \"\",IF(AY27=0,\"N/A\",waterPressureDrop(W27, U27 & \"P\" & IF(V27=\"Dual\",2,1) &\"C\", AD27, \"heating\", T27)))","v":""},{"$f":"IF(OR(T27=\"Select Model\",T27=\"PCBL\"), \"\",IF(AY27=0,getReturnWaterTemp(T27,AE27, activeEWTHeating, AX27, \"heating\"),getReturnWaterTemp(T27,AD27, activeEWTHeating, AY27, \"heating\")))","v":""},"",{"$f":" getNozzle(T27, W27, Y27, Z27, activeElevation, TRUE)","v":0}]
["Dry Bulb ⁰F",null,55,55,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I28)),I28<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I28, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H28)),H28<0),\"\",intlEstQuantity(T28, W28*12, H28)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T28=\"Select Model\",\"\",coilCircuitChange(W28, U28, AC28, T28,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T28=\"Select Model\",\"\",beamWidth(T28))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T28=\"Select Model\",T28=\"PCBL\"), 0,getSPIP(T28, W28, Y28, BD28, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T28=\"Select Model\", \"\",IF(T28=\"PCBL\",0,primaryAirSensibleCapacityIP($T28,$W28,activeRoomTempCooling,activePriAirTempCooling,$Y28,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T28=\"Select Model\",\"\",IF($T28=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y28,activeElevation)))","v":""},{"$f":"IF(OR(T28=\"Select Model\",T28=\"PCBL\"), 0,IF(AD28=0,0,-primaryAirSensibleCapacityIP($T28,$W28,activeRoomTempHeating,activePriAirTempHeating,$Y28,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T28=\"Select Model\", \"\", InductionRatio($T28,BD28,$W28,$Y28)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T28=\"Select Model\", \"\",IF($T28=\"PCBL\",\"N/A\",minVAVSetBack(AA28, Y28))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T28=\"Select Model\", \"\",IF($T28= \"PCBL\",\"N/A\",getDischargeAirTemp($T28,$V28,$AC28,$W28,BD28,$AL28, $Y28, $AS28, \"cooling\",activeElevation,$AB28,$AJ28,$AV28,$BB28))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T28=\"Select Model\",$T28=\"PCBL\"), \"\",getDischargeAirTemp($T28,$V28,$AD28,$W28,BD28,$AL28, $Y28, $AY28, \"heating\",activeElevation,$AB28,$AJ28,$AV28,$BB28)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T28=\"Select Model\", \"\",IF(OR($T28=\"ACBC_1W\",$T28=\"ACBC_2W\",LEFT($T28,4)=\"ACBR\",$T28 = \"LIU24_2W\",LEFT($T28,3)=\"RIU\",LEFT($T28,6)=\"ACBL12\"), IF((soundLevel($T28, $AB28, BD28, $Y28, $W28,$AJ28,$AA28,\"dba\"))<15,\"<15\",soundLevel($T28, $AB28, BD28, $Y28, $W28,$AJ28,$AA28,\"dba\")+0.4),IF((soundLevel($T28, $AB28, BD28, $Y28, $W28,$AJ28,$AA28,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T28, $AB28, BD28, $Y28, $W28,$AJ28,$AA28,\"dba\")+5)<15, \"<15\", soundLevel($T28, $AB28, BD28,$Y28, $W28,$AJ28,$AA28,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T28=\"Select Model\", \"\",IF(OR($T28=\"ACBC_1W\",$T28=\"ACBC_2W\",LEFT($T28,4)=\"ACBR\",$T28=\"LIU24_2W\",LEFT($T28,3)=\"RIU\",LEFT($T28,6)=\"ACBL12\"), IF((soundLevel($T28, $AB28, BD28, $Y28, $W28,$AJ28,$AA28,\"NC\"))<15,\"<15\",soundLevel($T28, $AB28, BD28, $Y28, $W28,$AJ28,$AA28,\"NC\")+0.4),IF((soundLevel($T28, $AB28, BD28, $Y28, $W28,$AJ28,$AA28,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T28, $AB28, BD28, $Y28, $W28,$AJ28,$AA28,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T28, $AB28, BD28, $Y28, $W28,$AJ28,$AA28,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T28=\"Select Model\",\"\",IF($T28=\"LIU24_2W\",calcQwIP($Y28,$W28,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC28,$AI28,\"latent\",$U28&\"P\"&IF($V28=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T28,activeElevation),\"\"))","v":""},{"$f":"IF($T28=\"Select Model\",\"\",IF($T28=\"ACBC_1W\",calcQwIP($Y28,$W28,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC28,BD28,\"capacity\",$U28&\"P\"&IF($V28=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T28,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y28,$W28,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC28,BD28,\"capacity\",$U28&\"P\"&IF($V28=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T28,activeElevation)))","v":""},"",{"$f":"IF(T28=\"Select Model\", 0,waterPressureDrop(W28, U28 & \"P\" & IF(V28=\"Dual\",2,1) &\"C\", AC28, \"cooling\", T28))","v":0},{"$f":"IF(T28=\"Select Model\", \"\",getReturnWaterTemp(T28,AC28, activeEWTCooling, AS28, \"cooling\"))","v":""},"",{"$f":"IF($T28<>\"ACBC_1W\",\"\",IF($J28=\"\",\"\",FintubeCapacity($T28,$W28,$AE28,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T28=\"Select Model\",T28=\"PCBL\"),\"\",calcQwIP(Y28,W28,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD28,BD28,\"capacity\",U28&\"P\"&IF(V28=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T28,activeElevation))","v":""},"",{"$f":"IF(OR(T28=\"Select Model\",T28=\"PCBL\"), \"\",IF(AY28=0,\"N/A\",waterPressureDrop(W28, U28 & \"P\" & IF(V28=\"Dual\",2,1) &\"C\", AD28, \"heating\", T28)))","v":""},{"$f":"IF(OR(T28=\"Select Model\",T28=\"PCBL\"), \"\",IF(AY28=0,getReturnWaterTemp(T28,AE28, activeEWTHeating, AX28, \"heating\"),getReturnWaterTemp(T28,AD28, activeEWTHeating, AY28, \"heating\")))","v":""},"",{"$f":" getNozzle(T28, W28, Y28, Z28, activeElevation, TRUE)","v":0}]
["Relative Humidity % RH",null,80,80,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I29)),I29<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I29, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H29)),H29<0),\"\",intlEstQuantity(T29, W29*12, H29)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T29=\"Select Model\",\"\",coilCircuitChange(W29, U29, AC29, T29,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T29=\"Select Model\",\"\",beamWidth(T29))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T29=\"Select Model\",T29=\"PCBL\"), 0,getSPIP(T29, W29, Y29, BD29, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T29=\"Select Model\", \"\",IF(T29=\"PCBL\",0,primaryAirSensibleCapacityIP($T29,$W29,activeRoomTempCooling,activePriAirTempCooling,$Y29,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T29=\"Select Model\",\"\",IF($T29=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y29,activeElevation)))","v":""},{"$f":"IF(OR(T29=\"Select Model\",T29=\"PCBL\"), 0,IF(AD29=0,0,-primaryAirSensibleCapacityIP($T29,$W29,activeRoomTempHeating,activePriAirTempHeating,$Y29,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T29=\"Select Model\", \"\", InductionRatio($T29,BD29,$W29,$Y29)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T29=\"Select Model\", \"\",IF($T29=\"PCBL\",\"N/A\",minVAVSetBack(AA29, Y29))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T29=\"Select Model\", \"\",IF($T29= \"PCBL\",\"N/A\",getDischargeAirTemp($T29,$V29,$AC29,$W29,BD29,$AL29, $Y29, $AS29, \"cooling\",activeElevation,$AB29,$AJ29,$AV29,$BB29))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T29=\"Select Model\",$T29=\"PCBL\"), \"\",getDischargeAirTemp($T29,$V29,$AD29,$W29,BD29,$AL29, $Y29, $AY29, \"heating\",activeElevation,$AB29,$AJ29,$AV29,$BB29)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T29=\"Select Model\", \"\",IF(OR($T29=\"ACBC_1W\",$T29=\"ACBC_2W\",LEFT($T29,4)=\"ACBR\",$T29 = \"LIU24_2W\",LEFT($T29,3)=\"RIU\",LEFT($T29,6)=\"ACBL12\"), IF((soundLevel($T29, $AB29, BD29, $Y29, $W29,$AJ29,$AA29,\"dba\"))<15,\"<15\",soundLevel($T29, $AB29, BD29, $Y29, $W29,$AJ29,$AA29,\"dba\")+0.4),IF((soundLevel($T29, $AB29, BD29, $Y29, $W29,$AJ29,$AA29,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T29, $AB29, BD29, $Y29, $W29,$AJ29,$AA29,\"dba\")+5)<15, \"<15\", soundLevel($T29, $AB29, BD29,$Y29, $W29,$AJ29,$AA29,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T29=\"Select Model\", \"\",IF(OR($T29=\"ACBC_1W\",$T29=\"ACBC_2W\",LEFT($T29,4)=\"ACBR\",$T29=\"LIU24_2W\",LEFT($T29,3)=\"RIU\",LEFT($T29,6)=\"ACBL12\"), IF((soundLevel($T29, $AB29, BD29, $Y29, $W29,$AJ29,$AA29,\"NC\"))<15,\"<15\",soundLevel($T29, $AB29, BD29, $Y29, $W29,$AJ29,$AA29,\"NC\")+0.4),IF((soundLevel($T29, $AB29, BD29, $Y29, $W29,$AJ29,$AA29,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T29, $AB29, BD29, $Y29, $W29,$AJ29,$AA29,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T29, $AB29, BD29, $Y29, $W29,$AJ29,$AA29,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T29=\"Select Model\",\"\",IF($T29=\"LIU24_2W\",calcQwIP($Y29,$W29,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC29,$AI29,\"latent\",$U29&\"P\"&IF($V29=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T29,activeElevation),\"\"))","v":""},{"$f":"IF($T29=\"Select Model\",\"\",IF($T29=\"ACBC_1W\",calcQwIP($Y29,$W29,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC29,BD29,\"capacity\",$U29&\"P\"&IF($V29=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T29,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y29,$W29,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC29,BD29,\"capacity\",$U29&\"P\"&IF($V29=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T29,activeElevation)))","v":""},"",{"$f":"IF(T29=\"Select Model\", 0,waterPressureDrop(W29, U29 & \"P\" & IF(V29=\"Dual\",2,1) &\"C\", AC29, \"cooling\", T29))","v":0},{"$f":"IF(T29=\"Select Model\", \"\",getReturnWaterTemp(T29,AC29, activeEWTCooling, AS29, \"cooling\"))","v":""},"",{"$f":"IF($T29<>\"ACBC_1W\",\"\",IF($J29=\"\",\"\",FintubeCapacity($T29,$W29,$AE29,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T29=\"Select Model\",T29=\"PCBL\"),\"\",calcQwIP(Y29,W29,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD29,BD29,\"capacity\",U29&\"P\"&IF(V29=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T29,activeElevation))","v":""},"",{"$f":"IF(OR(T29=\"Select Model\",T29=\"PCBL\"), \"\",IF(AY29=0,\"N/A\",waterPressureDrop(W29, U29 & \"P\" & IF(V29=\"Dual\",2,1) &\"C\", AD29, \"heating\", T29)))","v":""},{"$f":"IF(OR(T29=\"Select Model\",T29=\"PCBL\"), \"\",IF(AY29=0,getReturnWaterTemp(T29,AE29, activeEWTHeating, AX29, \"heating\"),getReturnWaterTemp(T29,AD29, activeEWTHeating, AY29, \"heating\")))","v":""},"",{"$f":" getNozzle(T29, W29, Y29, Z29, activeElevation, TRUE)","v":0}]
["Wet Bulb","⁰F",{"$f":"getWetBulbFromRH(C29,C28,$A$13)","v":51.64519999999996},{"$f":"getWetBulbFromRH(D29,D28,$A$13)","v":51.64519999999996},null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I30)),I30<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I30, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H30)),H30<0),\"\",intlEstQuantity(T30, W30*12, H30)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T30=\"Select Model\",\"\",coilCircuitChange(W30, U30, AC30, T30,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T30=\"Select Model\",\"\",beamWidth(T30))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T30=\"Select Model\",T30=\"PCBL\"), 0,getSPIP(T30, W30, Y30, BD30, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T30=\"Select Model\", \"\",IF(T30=\"PCBL\",0,primaryAirSensibleCapacityIP($T30,$W30,activeRoomTempCooling,activePriAirTempCooling,$Y30,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T30=\"Select Model\",\"\",IF($T30=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y30,activeElevation)))","v":""},{"$f":"IF(OR(T30=\"Select Model\",T30=\"PCBL\"), 0,IF(AD30=0,0,-primaryAirSensibleCapacityIP($T30,$W30,activeRoomTempHeating,activePriAirTempHeating,$Y30,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T30=\"Select Model\", \"\", InductionRatio($T30,BD30,$W30,$Y30)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T30=\"Select Model\", \"\",IF($T30=\"PCBL\",\"N/A\",minVAVSetBack(AA30, Y30))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T30=\"Select Model\", \"\",IF($T30= \"PCBL\",\"N/A\",getDischargeAirTemp($T30,$V30,$AC30,$W30,BD30,$AL30, $Y30, $AS30, \"cooling\",activeElevation,$AB30,$AJ30,$AV30,$BB30))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T30=\"Select Model\",$T30=\"PCBL\"), \"\",getDischargeAirTemp($T30,$V30,$AD30,$W30,BD30,$AL30, $Y30, $AY30, \"heating\",activeElevation,$AB30,$AJ30,$AV30,$BB30)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T30=\"Select Model\", \"\",IF(OR($T30=\"ACBC_1W\",$T30=\"ACBC_2W\",LEFT($T30,4)=\"ACBR\",$T30 = \"LIU24_2W\",LEFT($T30,3)=\"RIU\",LEFT($T30,6)=\"ACBL12\"), IF((soundLevel($T30, $AB30, BD30, $Y30, $W30,$AJ30,$AA30,\"dba\"))<15,\"<15\",soundLevel($T30, $AB30, BD30, $Y30, $W30,$AJ30,$AA30,\"dba\")+0.4),IF((soundLevel($T30, $AB30, BD30, $Y30, $W30,$AJ30,$AA30,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T30, $AB30, BD30, $Y30, $W30,$AJ30,$AA30,\"dba\")+5)<15, \"<15\", soundLevel($T30, $AB30, BD30,$Y30, $W30,$AJ30,$AA30,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T30=\"Select Model\", \"\",IF(OR($T30=\"ACBC_1W\",$T30=\"ACBC_2W\",LEFT($T30,4)=\"ACBR\",$T30=\"LIU24_2W\",LEFT($T30,3)=\"RIU\",LEFT($T30,6)=\"ACBL12\"), IF((soundLevel($T30, $AB30, BD30, $Y30, $W30,$AJ30,$AA30,\"NC\"))<15,\"<15\",soundLevel($T30, $AB30, BD30, $Y30, $W30,$AJ30,$AA30,\"NC\")+0.4),IF((soundLevel($T30, $AB30, BD30, $Y30, $W30,$AJ30,$AA30,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T30, $AB30, BD30, $Y30, $W30,$AJ30,$AA30,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T30, $AB30, BD30, $Y30, $W30,$AJ30,$AA30,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T30=\"Select Model\",\"\",IF($T30=\"LIU24_2W\",calcQwIP($Y30,$W30,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC30,$AI30,\"latent\",$U30&\"P\"&IF($V30=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T30,activeElevation),\"\"))","v":""},{"$f":"IF($T30=\"Select Model\",\"\",IF($T30=\"ACBC_1W\",calcQwIP($Y30,$W30,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC30,BD30,\"capacity\",$U30&\"P\"&IF($V30=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T30,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y30,$W30,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC30,BD30,\"capacity\",$U30&\"P\"&IF($V30=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T30,activeElevation)))","v":""},"",{"$f":"IF(T30=\"Select Model\", 0,waterPressureDrop(W30, U30 & \"P\" & IF(V30=\"Dual\",2,1) &\"C\", AC30, \"cooling\", T30))","v":0},{"$f":"IF(T30=\"Select Model\", \"\",getReturnWaterTemp(T30,AC30, activeEWTCooling, AS30, \"cooling\"))","v":""},"",{"$f":"IF($T30<>\"ACBC_1W\",\"\",IF($J30=\"\",\"\",FintubeCapacity($T30,$W30,$AE30,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T30=\"Select Model\",T30=\"PCBL\"),\"\",calcQwIP(Y30,W30,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD30,BD30,\"capacity\",U30&\"P\"&IF(V30=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T30,activeElevation))","v":""},"",{"$f":"IF(OR(T30=\"Select Model\",T30=\"PCBL\"), \"\",IF(AY30=0,\"N/A\",waterPressureDrop(W30, U30 & \"P\" & IF(V30=\"Dual\",2,1) &\"C\", AD30, \"heating\", T30)))","v":""},{"$f":"IF(OR(T30=\"Select Model\",T30=\"PCBL\"), \"\",IF(AY30=0,getReturnWaterTemp(T30,AE30, activeEWTHeating, AX30, \"heating\"),getReturnWaterTemp(T30,AD30, activeEWTHeating, AY30, \"heating\")))","v":""},"",{"$f":" getNozzle(T30, W30, Y30, Z30, activeElevation, TRUE)","v":0}]
["Dew Point","⁰F",{"$f":"getDewPointFromRH(C29,C28,$A$13)","v":49.014353359704707},{"$f":"getDewPointFromRH(D29,D28,$A$13)","v":49.014353359704707},null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I31)),I31<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I31, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H31)),H31<0),\"\",intlEstQuantity(T31, W31*12, H31)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T31=\"Select Model\",\"\",coilCircuitChange(W31, U31, AC31, T31,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T31=\"Select Model\",\"\",beamWidth(T31))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T31=\"Select Model\",T31=\"PCBL\"), 0,getSPIP(T31, W31, Y31, BD31, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T31=\"Select Model\", \"\",IF(T31=\"PCBL\",0,primaryAirSensibleCapacityIP($T31,$W31,activeRoomTempCooling,activePriAirTempCooling,$Y31,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T31=\"Select Model\",\"\",IF($T31=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y31,activeElevation)))","v":""},{"$f":"IF(OR(T31=\"Select Model\",T31=\"PCBL\"), 0,IF(AD31=0,0,-primaryAirSensibleCapacityIP($T31,$W31,activeRoomTempHeating,activePriAirTempHeating,$Y31,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T31=\"Select Model\", \"\", InductionRatio($T31,BD31,$W31,$Y31)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T31=\"Select Model\", \"\",IF($T31=\"PCBL\",\"N/A\",minVAVSetBack(AA31, Y31))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T31=\"Select Model\", \"\",IF($T31= \"PCBL\",\"N/A\",getDischargeAirTemp($T31,$V31,$AC31,$W31,BD31,$AL31, $Y31, $AS31, \"cooling\",activeElevation,$AB31,$AJ31,$AV31,$BB31))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T31=\"Select Model\",$T31=\"PCBL\"), \"\",getDischargeAirTemp($T31,$V31,$AD31,$W31,BD31,$AL31, $Y31, $AY31, \"heating\",activeElevation,$AB31,$AJ31,$AV31,$BB31)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T31=\"Select Model\", \"\",IF(OR($T31=\"ACBC_1W\",$T31=\"ACBC_2W\",LEFT($T31,4)=\"ACBR\",$T31 = \"LIU24_2W\",LEFT($T31,3)=\"RIU\",LEFT($T31,6)=\"ACBL12\"), IF((soundLevel($T31, $AB31, BD31, $Y31, $W31,$AJ31,$AA31,\"dba\"))<15,\"<15\",soundLevel($T31, $AB31, BD31, $Y31, $W31,$AJ31,$AA31,\"dba\")+0.4),IF((soundLevel($T31, $AB31, BD31, $Y31, $W31,$AJ31,$AA31,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T31, $AB31, BD31, $Y31, $W31,$AJ31,$AA31,\"dba\")+5)<15, \"<15\", soundLevel($T31, $AB31, BD31,$Y31, $W31,$AJ31,$AA31,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T31=\"Select Model\", \"\",IF(OR($T31=\"ACBC_1W\",$T31=\"ACBC_2W\",LEFT($T31,4)=\"ACBR\",$T31=\"LIU24_2W\",LEFT($T31,3)=\"RIU\",LEFT($T31,6)=\"ACBL12\"), IF((soundLevel($T31, $AB31, BD31, $Y31, $W31,$AJ31,$AA31,\"NC\"))<15,\"<15\",soundLevel($T31, $AB31, BD31, $Y31, $W31,$AJ31,$AA31,\"NC\")+0.4),IF((soundLevel($T31, $AB31, BD31, $Y31, $W31,$AJ31,$AA31,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T31, $AB31, BD31, $Y31, $W31,$AJ31,$AA31,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T31, $AB31, BD31, $Y31, $W31,$AJ31,$AA31,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T31=\"Select Model\",\"\",IF($T31=\"LIU24_2W\",calcQwIP($Y31,$W31,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC31,$AI31,\"latent\",$U31&\"P\"&IF($V31=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T31,activeElevation),\"\"))","v":""},{"$f":"IF($T31=\"Select Model\",\"\",IF($T31=\"ACBC_1W\",calcQwIP($Y31,$W31,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC31,BD31,\"capacity\",$U31&\"P\"&IF($V31=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T31,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y31,$W31,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC31,BD31,\"capacity\",$U31&\"P\"&IF($V31=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T31,activeElevation)))","v":""},"",{"$f":"IF(T31=\"Select Model\", 0,waterPressureDrop(W31, U31 & \"P\" & IF(V31=\"Dual\",2,1) &\"C\", AC31, \"cooling\", T31))","v":0},{"$f":"IF(T31=\"Select Model\", \"\",getReturnWaterTemp(T31,AC31, activeEWTCooling, AS31, \"cooling\"))","v":""},"",{"$f":"IF($T31<>\"ACBC_1W\",\"\",IF($J31=\"\",\"\",FintubeCapacity($T31,$W31,$AE31,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T31=\"Select Model\",T31=\"PCBL\"),\"\",calcQwIP(Y31,W31,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD31,BD31,\"capacity\",U31&\"P\"&IF(V31=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T31,activeElevation))","v":""},"",{"$f":"IF(OR(T31=\"Select Model\",T31=\"PCBL\"), \"\",IF(AY31=0,\"N/A\",waterPressureDrop(W31, U31 & \"P\" & IF(V31=\"Dual\",2,1) &\"C\", AD31, \"heating\", T31)))","v":""},{"$f":"IF(OR(T31=\"Select Model\",T31=\"PCBL\"), \"\",IF(AY31=0,getReturnWaterTemp(T31,AE31, activeEWTHeating, AX31, \"heating\"),getReturnWaterTemp(T31,AD31, activeEWTHeating, AY31, \"heating\")))","v":""},"",{"$f":" getNozzle(T31, W31, Y31, Z31, activeElevation, TRUE)","v":0}]
[null,"gr/lb",{"$f":"getgrainperpound(C29,C28,$A$13)","v":51.339360278659356},{"$f":"getgrainperpound(D29,D28,$A$13)","v":51.339360278659356},null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I32)),I32<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I32, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H32)),H32<0),\"\",intlEstQuantity(T32, W32*12, H32)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T32=\"Select Model\",\"\",coilCircuitChange(W32, U32, AC32, T32,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T32=\"Select Model\",\"\",beamWidth(T32))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T32=\"Select Model\",T32=\"PCBL\"), 0,getSPIP(T32, W32, Y32, BD32, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T32=\"Select Model\", \"\",IF(T32=\"PCBL\",0,primaryAirSensibleCapacityIP($T32,$W32,activeRoomTempCooling,activePriAirTempCooling,$Y32,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T32=\"Select Model\",\"\",IF($T32=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y32,activeElevation)))","v":""},{"$f":"IF(OR(T32=\"Select Model\",T32=\"PCBL\"), 0,IF(AD32=0,0,-primaryAirSensibleCapacityIP($T32,$W32,activeRoomTempHeating,activePriAirTempHeating,$Y32,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T32=\"Select Model\", \"\", InductionRatio($T32,BD32,$W32,$Y32)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T32=\"Select Model\", \"\",IF($T32=\"PCBL\",\"N/A\",minVAVSetBack(AA32, Y32))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T32=\"Select Model\", \"\",IF($T32= \"PCBL\",\"N/A\",getDischargeAirTemp($T32,$V32,$AC32,$W32,BD32,$AL32, $Y32, $AS32, \"cooling\",activeElevation,$AB32,$AJ32,$AV32,$BB32))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T32=\"Select Model\",$T32=\"PCBL\"), \"\",getDischargeAirTemp($T32,$V32,$AD32,$W32,BD32,$AL32, $Y32, $AY32, \"heating\",activeElevation,$AB32,$AJ32,$AV32,$BB32)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T32=\"Select Model\", \"\",IF(OR($T32=\"ACBC_1W\",$T32=\"ACBC_2W\",LEFT($T32,4)=\"ACBR\",$T32 = \"LIU24_2W\",LEFT($T32,3)=\"RIU\",LEFT($T32,6)=\"ACBL12\"), IF((soundLevel($T32, $AB32, BD32, $Y32, $W32,$AJ32,$AA32,\"dba\"))<15,\"<15\",soundLevel($T32, $AB32, BD32, $Y32, $W32,$AJ32,$AA32,\"dba\")+0.4),IF((soundLevel($T32, $AB32, BD32, $Y32, $W32,$AJ32,$AA32,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T32, $AB32, BD32, $Y32, $W32,$AJ32,$AA32,\"dba\")+5)<15, \"<15\", soundLevel($T32, $AB32, BD32,$Y32, $W32,$AJ32,$AA32,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T32=\"Select Model\", \"\",IF(OR($T32=\"ACBC_1W\",$T32=\"ACBC_2W\",LEFT($T32,4)=\"ACBR\",$T32=\"LIU24_2W\",LEFT($T32,3)=\"RIU\",LEFT($T32,6)=\"ACBL12\"), IF((soundLevel($T32, $AB32, BD32, $Y32, $W32,$AJ32,$AA32,\"NC\"))<15,\"<15\",soundLevel($T32, $AB32, BD32, $Y32, $W32,$AJ32,$AA32,\"NC\")+0.4),IF((soundLevel($T32, $AB32, BD32, $Y32, $W32,$AJ32,$AA32,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T32, $AB32, BD32, $Y32, $W32,$AJ32,$AA32,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T32, $AB32, BD32, $Y32, $W32,$AJ32,$AA32,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T32=\"Select Model\",\"\",IF($T32=\"LIU24_2W\",calcQwIP($Y32,$W32,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC32,$AI32,\"latent\",$U32&\"P\"&IF($V32=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T32,activeElevation),\"\"))","v":""},{"$f":"IF($T32=\"Select Model\",\"\",IF($T32=\"ACBC_1W\",calcQwIP($Y32,$W32,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC32,BD32,\"capacity\",$U32&\"P\"&IF($V32=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T32,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y32,$W32,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC32,BD32,\"capacity\",$U32&\"P\"&IF($V32=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T32,activeElevation)))","v":""},"",{"$f":"IF(T32=\"Select Model\", 0,waterPressureDrop(W32, U32 & \"P\" & IF(V32=\"Dual\",2,1) &\"C\", AC32, \"cooling\", T32))","v":0},{"$f":"IF(T32=\"Select Model\", \"\",getReturnWaterTemp(T32,AC32, activeEWTCooling, AS32, \"cooling\"))","v":""},"",{"$f":"IF($T32<>\"ACBC_1W\",\"\",IF($J32=\"\",\"\",FintubeCapacity($T32,$W32,$AE32,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T32=\"Select Model\",T32=\"PCBL\"),\"\",calcQwIP(Y32,W32,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD32,BD32,\"capacity\",U32&\"P\"&IF(V32=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T32,activeElevation))","v":""},"",{"$f":"IF(OR(T32=\"Select Model\",T32=\"PCBL\"), \"\",IF(AY32=0,\"N/A\",waterPressureDrop(W32, U32 & \"P\" & IF(V32=\"Dual\",2,1) &\"C\", AD32, \"heating\", T32)))","v":""},{"$f":"IF(OR(T32=\"Select Model\",T32=\"PCBL\"), \"\",IF(AY32=0,getReturnWaterTemp(T32,AE32, activeEWTHeating, AX32, \"heating\"),getReturnWaterTemp(T32,AD32, activeEWTHeating, AY32, \"heating\")))","v":""},"",{"$f":" getNozzle(T32, W32, Y32, Z32, activeElevation, TRUE)","v":0}]
["Max Airside ∆P in w.g.",null,0.75,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I33)),I33<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I33, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H33)),H33<0),\"\",intlEstQuantity(T33, W33*12, H33)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T33=\"Select Model\",\"\",coilCircuitChange(W33, U33, AC33, T33,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T33=\"Select Model\",\"\",beamWidth(T33))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T33=\"Select Model\",T33=\"PCBL\"), 0,getSPIP(T33, W33, Y33, BD33, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T33=\"Select Model\", \"\",IF(T33=\"PCBL\",0,primaryAirSensibleCapacityIP($T33,$W33,activeRoomTempCooling,activePriAirTempCooling,$Y33,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T33=\"Select Model\",\"\",IF($T33=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y33,activeElevation)))","v":""},{"$f":"IF(OR(T33=\"Select Model\",T33=\"PCBL\"), 0,IF(AD33=0,0,-primaryAirSensibleCapacityIP($T33,$W33,activeRoomTempHeating,activePriAirTempHeating,$Y33,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T33=\"Select Model\", \"\", InductionRatio($T33,BD33,$W33,$Y33)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T33=\"Select Model\", \"\",IF($T33=\"PCBL\",\"N/A\",minVAVSetBack(AA33, Y33))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T33=\"Select Model\", \"\",IF($T33= \"PCBL\",\"N/A\",getDischargeAirTemp($T33,$V33,$AC33,$W33,BD33,$AL33, $Y33, $AS33, \"cooling\",activeElevation,$AB33,$AJ33,$AV33,$BB33))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T33=\"Select Model\",$T33=\"PCBL\"), \"\",getDischargeAirTemp($T33,$V33,$AD33,$W33,BD33,$AL33, $Y33, $AY33, \"heating\",activeElevation,$AB33,$AJ33,$AV33,$BB33)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T33=\"Select Model\", \"\",IF(OR($T33=\"ACBC_1W\",$T33=\"ACBC_2W\",LEFT($T33,4)=\"ACBR\",$T33 = \"LIU24_2W\",LEFT($T33,3)=\"RIU\",LEFT($T33,6)=\"ACBL12\"), IF((soundLevel($T33, $AB33, BD33, $Y33, $W33,$AJ33,$AA33,\"dba\"))<15,\"<15\",soundLevel($T33, $AB33, BD33, $Y33, $W33,$AJ33,$AA33,\"dba\")+0.4),IF((soundLevel($T33, $AB33, BD33, $Y33, $W33,$AJ33,$AA33,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T33, $AB33, BD33, $Y33, $W33,$AJ33,$AA33,\"dba\")+5)<15, \"<15\", soundLevel($T33, $AB33, BD33,$Y33, $W33,$AJ33,$AA33,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T33=\"Select Model\", \"\",IF(OR($T33=\"ACBC_1W\",$T33=\"ACBC_2W\",LEFT($T33,4)=\"ACBR\",$T33=\"LIU24_2W\",LEFT($T33,3)=\"RIU\",LEFT($T33,6)=\"ACBL12\"), IF((soundLevel($T33, $AB33, BD33, $Y33, $W33,$AJ33,$AA33,\"NC\"))<15,\"<15\",soundLevel($T33, $AB33, BD33, $Y33, $W33,$AJ33,$AA33,\"NC\")+0.4),IF((soundLevel($T33, $AB33, BD33, $Y33, $W33,$AJ33,$AA33,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T33, $AB33, BD33, $Y33, $W33,$AJ33,$AA33,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T33, $AB33, BD33, $Y33, $W33,$AJ33,$AA33,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T33=\"Select Model\",\"\",IF($T33=\"LIU24_2W\",calcQwIP($Y33,$W33,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC33,$AI33,\"latent\",$U33&\"P\"&IF($V33=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T33,activeElevation),\"\"))","v":""},{"$f":"IF($T33=\"Select Model\",\"\",IF($T33=\"ACBC_1W\",calcQwIP($Y33,$W33,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC33,BD33,\"capacity\",$U33&\"P\"&IF($V33=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T33,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y33,$W33,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC33,BD33,\"capacity\",$U33&\"P\"&IF($V33=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T33,activeElevation)))","v":""},"",{"$f":"IF(T33=\"Select Model\", 0,waterPressureDrop(W33, U33 & \"P\" & IF(V33=\"Dual\",2,1) &\"C\", AC33, \"cooling\", T33))","v":0},{"$f":"IF(T33=\"Select Model\", \"\",getReturnWaterTemp(T33,AC33, activeEWTCooling, AS33, \"cooling\"))","v":""},"",{"$f":"IF($T33<>\"ACBC_1W\",\"\",IF($J33=\"\",\"\",FintubeCapacity($T33,$W33,$AE33,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T33=\"Select Model\",T33=\"PCBL\"),\"\",calcQwIP(Y33,W33,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD33,BD33,\"capacity\",U33&\"P\"&IF(V33=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T33,activeElevation))","v":""},"",{"$f":"IF(OR(T33=\"Select Model\",T33=\"PCBL\"), \"\",IF(AY33=0,\"N/A\",waterPressureDrop(W33, U33 & \"P\" & IF(V33=\"Dual\",2,1) &\"C\", AD33, \"heating\", T33)))","v":""},{"$f":"IF(OR(T33=\"Select Model\",T33=\"PCBL\"), \"\",IF(AY33=0,getReturnWaterTemp(T33,AE33, activeEWTHeating, AX33, \"heating\"),getReturnWaterTemp(T33,AD33, activeEWTHeating, AY33, \"heating\")))","v":""},"",{"$f":" getNozzle(T33, W33, Y33, Z33, activeElevation, TRUE)","v":0}]
["Entering Water Conditions",null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I34)),I34<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I34, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H34)),H34<0),\"\",intlEstQuantity(T34, W34*12, H34)),1)","v":""},"","","",{"$f":"IF(AND(ISNUMBER(L34),ISNUMBER(Y34)),L34*Y34,\"\")","v":""},{"$f":"IF(AND(ISNUMBER(L34),ISNUMBER(AC34)),L34*AC34,\"\")","v":""},{"$f":"IF(AND(ISNUMBER(L34),ISNUMBER(AD34)),IF(AND(T34=\"ACBC_1W\",AD34=0),AE34*L34,L34*AD34))","v":false},"Default","Select Model",2,{"$f":"IF(T34=\"Select Model\",\"\",coilCircuitChange(W34, U34, AC34, T34,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T34=\"Select Model\",\"\",beamWidth(T34))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T34=\"Select Model\",T34=\"PCBL\"), 0,getSPIP(T34, W34, Y34, BD34, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T34=\"Select Model\", \"\",IF(T34=\"PCBL\",0,primaryAirSensibleCapacityIP($T34,$W34,activeRoomTempCooling,activePriAirTempCooling,$Y34,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T34=\"Select Model\",\"\",IF($T34=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y34,activeElevation)))","v":""},{"$f":"IF(OR(T34=\"Select Model\",T34=\"PCBL\"), 0,IF(AD34=0,0,-primaryAirSensibleCapacityIP($T34,$W34,activeRoomTempHeating,activePriAirTempHeating,$Y34,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T34=\"Select Model\", \"\", InductionRatio($T34,BD34,$W34,$Y34)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T34=\"Select Model\", \"\",IF($T34=\"PCBL\",\"N/A\",minVAVSetBack(AA34, Y34))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T34=\"Select Model\", \"\",IF($T34= \"PCBL\",\"N/A\",getDischargeAirTemp($T34,$V34,$AC34,$W34,BD34,$AL34, $Y34, $AS34, \"cooling\",activeElevation,$AB34,$AJ34,$AV34,$BB34))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T34=\"Select Model\",$T34=\"PCBL\"), \"\",getDischargeAirTemp($T34,$V34,$AD34,$W34,BD34,$AL34, $Y34, $AY34, \"heating\",activeElevation,$AB34,$AJ34,$AV34,$BB34)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T34=\"Select Model\", \"\",IF(OR($T34=\"ACBC_1W\",$T34=\"ACBC_2W\",LEFT($T34,4)=\"ACBR\",$T34 = \"LIU24_2W\",LEFT($T34,3)=\"RIU\",LEFT($T34,6)=\"ACBL12\"), IF((soundLevel($T34, $AB34, BD34, $Y34, $W34,$AJ34,$AA34,\"dba\"))<15,\"<15\",soundLevel($T34, $AB34, BD34, $Y34, $W34,$AJ34,$AA34,\"dba\")+0.4),IF((soundLevel($T34, $AB34, BD34, $Y34, $W34,$AJ34,$AA34,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T34, $AB34, BD34, $Y34, $W34,$AJ34,$AA34,\"dba\")+5)<15, \"<15\", soundLevel($T34, $AB34, BD34,$Y34, $W34,$AJ34,$AA34,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T34=\"Select Model\", \"\",IF(OR($T34=\"ACBC_1W\",$T34=\"ACBC_2W\",LEFT($T34,4)=\"ACBR\",$T34=\"LIU24_2W\",LEFT($T34,3)=\"RIU\",LEFT($T34,6)=\"ACBL12\"), IF((soundLevel($T34, $AB34, BD34, $Y34, $W34,$AJ34,$AA34,\"NC\"))<15,\"<15\",soundLevel($T34, $AB34, BD34, $Y34, $W34,$AJ34,$AA34,\"NC\")+0.4),IF((soundLevel($T34, $AB34, BD34, $Y34, $W34,$AJ34,$AA34,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T34, $AB34, BD34, $Y34, $W34,$AJ34,$AA34,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T34, $AB34, BD34, $Y34, $W34,$AJ34,$AA34,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T34=\"Select Model\",\"\",IF($T34=\"LIU24_2W\",calcQwIP($Y34,$W34,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC34,$AI34,\"latent\",$U34&\"P\"&IF($V34=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T34,activeElevation),\"\"))","v":""},{"$f":"IF($T34=\"Select Model\",\"\",IF($T34=\"ACBC_1W\",calcQwIP($Y34,$W34,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC34,BD34,\"capacity\",$U34&\"P\"&IF($V34=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T34,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y34,$W34,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC34,BD34,\"capacity\",$U34&\"P\"&IF($V34=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T34,activeElevation)))","v":""},"",{"$f":"IF(T34=\"Select Model\", 0,waterPressureDrop(W34, U34 & \"P\" & IF(V34=\"Dual\",2,1) &\"C\", AC34, \"cooling\", T34))","v":0},{"$f":"IF(T34=\"Select Model\", \"\",getReturnWaterTemp(T34,AC34, activeEWTCooling, AS34, \"cooling\"))","v":""},"",{"$f":"IF($T34<>\"ACBC_1W\",\"\",IF($J34=\"\",\"\",FintubeCapacity($T34,$W34,$AE34,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T34=\"Select Model\",T34=\"PCBL\"),\"\",calcQwIP(Y34,W34,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD34,BD34,\"capacity\",U34&\"P\"&IF(V34=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T34,activeElevation))","v":""},"",{"$f":"IF(OR(T34=\"Select Model\",T34=\"PCBL\"), \"\",IF(AY34=0,\"N/A\",waterPressureDrop(W34, U34 & \"P\" & IF(V34=\"Dual\",2,1) &\"C\", AD34, \"heating\", T34)))","v":""},{"$f":"IF(OR(T34=\"Select Model\",T34=\"PCBL\"), \"\",IF(AY34=0,getReturnWaterTemp(T34,AE34, activeEWTHeating, AX34, \"heating\"),getReturnWaterTemp(T34,AD34, activeEWTHeating, AY34, \"heating\")))","v":""},"",{"$f":" getNozzle(T34, W34, Y34, Z34, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I35)),I35<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I35, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H35)),H35<0),\"\",intlEstQuantity(T35, W35*12, H35)),1)","v":""},"","","",{"$f":"IF(AND(ISNUMBER(L35),ISNUMBER(Y35)),L35*Y35,\"\")","v":""},"",false,"Default","Select Model",2,{"$f":"IF(T35=\"Select Model\",\"\",coilCircuitChange(W35, U35, AC35, T35,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T35=\"Select Model\",\"\",beamWidth(T35))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T35=\"Select Model\",T35=\"PCBL\"), 0,getSPIP(T35, W35, Y35, BD35, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T35=\"Select Model\", \"\",IF(T35=\"PCBL\",0,primaryAirSensibleCapacityIP($T35,$W35,activeRoomTempCooling,activePriAirTempCooling,$Y35,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T35=\"Select Model\",\"\",IF($T35=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y35,activeElevation)))","v":""},{"$f":"IF(OR(T35=\"Select Model\",T35=\"PCBL\"), 0,IF(AD35=0,0,-primaryAirSensibleCapacityIP($T35,$W35,activeRoomTempHeating,activePriAirTempHeating,$Y35,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T35=\"Select Model\", \"\", InductionRatio($T35,BD35,$W35,$Y35)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T35=\"Select Model\", \"\",IF($T35=\"PCBL\",\"N/A\",minVAVSetBack(AA35, Y35))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T35=\"Select Model\", \"\",IF($T35= \"PCBL\",\"N/A\",getDischargeAirTemp($T35,$V35,$AC35,$W35,BD35,$AL35, $Y35, $AS35, \"cooling\",activeElevation,$AB35,$AJ35,$AV35,$BB35))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T35=\"Select Model\",$T35=\"PCBL\"), \"\",getDischargeAirTemp($T35,$V35,$AD35,$W35,BD35,$AL35, $Y35, $AY35, \"heating\",activeElevation,$AB35,$AJ35,$AV35,$BB35)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T35=\"Select Model\", \"\",IF(OR($T35=\"ACBC_1W\",$T35=\"ACBC_2W\",LEFT($T35,4)=\"ACBR\",$T35 = \"LIU24_2W\",LEFT($T35,3)=\"RIU\",LEFT($T35,6)=\"ACBL12\"), IF((soundLevel($T35, $AB35, BD35, $Y35, $W35,$AJ35,$AA35,\"dba\"))<15,\"<15\",soundLevel($T35, $AB35, BD35, $Y35, $W35,$AJ35,$AA35,\"dba\")+0.4),IF((soundLevel($T35, $AB35, BD35, $Y35, $W35,$AJ35,$AA35,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T35, $AB35, BD35, $Y35, $W35,$AJ35,$AA35,\"dba\")+5)<15, \"<15\", soundLevel($T35, $AB35, BD35,$Y35, $W35,$AJ35,$AA35,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T35=\"Select Model\", \"\",IF(OR($T35=\"ACBC_1W\",$T35=\"ACBC_2W\",LEFT($T35,4)=\"ACBR\",$T35=\"LIU24_2W\",LEFT($T35,3)=\"RIU\",LEFT($T35,6)=\"ACBL12\"), IF((soundLevel($T35, $AB35, BD35, $Y35, $W35,$AJ35,$AA35,\"NC\"))<15,\"<15\",soundLevel($T35, $AB35, BD35, $Y35, $W35,$AJ35,$AA35,\"NC\")+0.4),IF((soundLevel($T35, $AB35, BD35, $Y35, $W35,$AJ35,$AA35,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T35, $AB35, BD35, $Y35, $W35,$AJ35,$AA35,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T35, $AB35, BD35, $Y35, $W35,$AJ35,$AA35,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T35=\"Select Model\",\"\",IF($T35=\"LIU24_2W\",calcQwIP($Y35,$W35,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC35,$AI35,\"latent\",$U35&\"P\"&IF($V35=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T35,activeElevation),\"\"))","v":""},{"$f":"IF($T35=\"Select Model\",\"\",IF($T35=\"ACBC_1W\",calcQwIP($Y35,$W35,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC35,BD35,\"capacity\",$U35&\"P\"&IF($V35=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T35,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y35,$W35,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC35,BD35,\"capacity\",$U35&\"P\"&IF($V35=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T35,activeElevation)))","v":""},"",{"$f":"IF(T35=\"Select Model\", 0,waterPressureDrop(W35, U35 & \"P\" & IF(V35=\"Dual\",2,1) &\"C\", AC35, \"cooling\", T35))","v":0},{"$f":"IF(T35=\"Select Model\", \"\",getReturnWaterTemp(T35,AC35, activeEWTCooling, AS35, \"cooling\"))","v":""},"",{"$f":"IF($T35<>\"ACBC_1W\",\"\",IF($J35=\"\",\"\",FintubeCapacity($T35,$W35,$AE35,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T35=\"Select Model\",T35=\"PCBL\"),\"\",calcQwIP(Y35,W35,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD35,BD35,\"capacity\",U35&\"P\"&IF(V35=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T35,activeElevation))","v":""},"",{"$f":"IF(OR(T35=\"Select Model\",T35=\"PCBL\"), \"\",IF(AY35=0,\"N/A\",waterPressureDrop(W35, U35 & \"P\" & IF(V35=\"Dual\",2,1) &\"C\", AD35, \"heating\", T35)))","v":""},{"$f":"IF(OR(T35=\"Select Model\",T35=\"PCBL\"), \"\",IF(AY35=0,getReturnWaterTemp(T35,AE35, activeEWTHeating, AX35, \"heating\"),getReturnWaterTemp(T35,AD35, activeEWTHeating, AY35, \"heating\")))","v":""},"",{"$f":" getNozzle(T35, W35, Y35, Z35, activeElevation, TRUE)","v":0}]
["Temperature ⁰F",null,57,120,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I36)),I36<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I36, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H36)),H36<0),\"\",intlEstQuantity(T36, W36*12, H36)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T36=\"Select Model\",\"\",coilCircuitChange(W36, U36, AC36, T36,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T36=\"Select Model\",\"\",beamWidth(T36))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T36=\"Select Model\",T36=\"PCBL\"), 0,getSPIP(T36, W36, Y36, BD36, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T36=\"Select Model\", \"\",IF(T36=\"PCBL\",0,primaryAirSensibleCapacityIP($T36,$W36,activeRoomTempCooling,activePriAirTempCooling,$Y36,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T36=\"Select Model\",\"\",IF($T36=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y36,activeElevation)))","v":""},{"$f":"IF(OR(T36=\"Select Model\",T36=\"PCBL\"), 0,IF(AD36=0,0,-primaryAirSensibleCapacityIP($T36,$W36,activeRoomTempHeating,activePriAirTempHeating,$Y36,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T36=\"Select Model\", \"\", InductionRatio($T36,BD36,$W36,$Y36)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T36=\"Select Model\", \"\",IF($T36=\"PCBL\",\"N/A\",minVAVSetBack(AA36, Y36))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T36=\"Select Model\", \"\",IF($T36= \"PCBL\",\"N/A\",getDischargeAirTemp($T36,$V36,$AC36,$W36,BD36,$AL36, $Y36, $AS36, \"cooling\",activeElevation,$AB36,$AJ36,$AV36,$BB36))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T36=\"Select Model\",$T36=\"PCBL\"), \"\",getDischargeAirTemp($T36,$V36,$AD36,$W36,BD36,$AL36, $Y36, $AY36, \"heating\",activeElevation,$AB36,$AJ36,$AV36,$BB36)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T36=\"Select Model\", \"\",IF(OR($T36=\"ACBC_1W\",$T36=\"ACBC_2W\",LEFT($T36,4)=\"ACBR\",$T36 = \"LIU24_2W\",LEFT($T36,3)=\"RIU\",LEFT($T36,6)=\"ACBL12\"), IF((soundLevel($T36, $AB36, BD36, $Y36, $W36,$AJ36,$AA36,\"dba\"))<15,\"<15\",soundLevel($T36, $AB36, BD36, $Y36, $W36,$AJ36,$AA36,\"dba\")+0.4),IF((soundLevel($T36, $AB36, BD36, $Y36, $W36,$AJ36,$AA36,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T36, $AB36, BD36, $Y36, $W36,$AJ36,$AA36,\"dba\")+5)<15, \"<15\", soundLevel($T36, $AB36, BD36,$Y36, $W36,$AJ36,$AA36,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T36=\"Select Model\", \"\",IF(OR($T36=\"ACBC_1W\",$T36=\"ACBC_2W\",LEFT($T36,4)=\"ACBR\",$T36=\"LIU24_2W\",LEFT($T36,3)=\"RIU\",LEFT($T36,6)=\"ACBL12\"), IF((soundLevel($T36, $AB36, BD36, $Y36, $W36,$AJ36,$AA36,\"NC\"))<15,\"<15\",soundLevel($T36, $AB36, BD36, $Y36, $W36,$AJ36,$AA36,\"NC\")+0.4),IF((soundLevel($T36, $AB36, BD36, $Y36, $W36,$AJ36,$AA36,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T36, $AB36, BD36, $Y36, $W36,$AJ36,$AA36,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T36, $AB36, BD36, $Y36, $W36,$AJ36,$AA36,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T36=\"Select Model\",\"\",IF($T36=\"LIU24_2W\",calcQwIP($Y36,$W36,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC36,$AI36,\"latent\",$U36&\"P\"&IF($V36=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T36,activeElevation),\"\"))","v":""},{"$f":"IF($T36=\"Select Model\",\"\",IF($T36=\"ACBC_1W\",calcQwIP($Y36,$W36,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC36,BD36,\"capacity\",$U36&\"P\"&IF($V36=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T36,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y36,$W36,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC36,BD36,\"capacity\",$U36&\"P\"&IF($V36=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T36,activeElevation)))","v":""},"",{"$f":"IF(T36=\"Select Model\", 0,waterPressureDrop(W36, U36 & \"P\" & IF(V36=\"Dual\",2,1) &\"C\", AC36, \"cooling\", T36))","v":0},{"$f":"IF(T36=\"Select Model\", \"\",getReturnWaterTemp(T36,AC36, activeEWTCooling, AS36, \"cooling\"))","v":""},"",{"$f":"IF($T36<>\"ACBC_1W\",\"\",IF($J36=\"\",\"\",FintubeCapacity($T36,$W36,$AE36,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T36=\"Select Model\",T36=\"PCBL\"),\"\",calcQwIP(Y36,W36,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD36,BD36,\"capacity\",U36&\"P\"&IF(V36=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T36,activeElevation))","v":""},"",{"$f":"IF(OR(T36=\"Select Model\",T36=\"PCBL\"), \"\",IF(AY36=0,\"N/A\",waterPressureDrop(W36, U36 & \"P\" & IF(V36=\"Dual\",2,1) &\"C\", AD36, \"heating\", T36)))","v":""},{"$f":"IF(OR(T36=\"Select Model\",T36=\"PCBL\"), \"\",IF(AY36=0,getReturnWaterTemp(T36,AE36, activeEWTHeating, AX36, \"heating\"),getReturnWaterTemp(T36,AD36, activeEWTHeating, AY36, \"heating\")))","v":""},"",{"$f":" getNozzle(T36, W36, Y36, Z36, activeElevation, TRUE)","v":0}]
["Fluid Type (Cooling)",null,"Water",null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I37)),I37<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I37, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H37)),H37<0),\"\",intlEstQuantity(T37, W37*12, H37)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T37=\"Select Model\",\"\",coilCircuitChange(W37, U37, AC37, T37,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T37=\"Select Model\",\"\",beamWidth(T37))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T37=\"Select Model\",T37=\"PCBL\"), 0,getSPIP(T37, W37, Y37, BD37, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T37=\"Select Model\", \"\",IF(T37=\"PCBL\",0,primaryAirSensibleCapacityIP($T37,$W37,activeRoomTempCooling,activePriAirTempCooling,$Y37,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T37=\"Select Model\",\"\",IF($T37=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y37,activeElevation)))","v":""},{"$f":"IF(OR(T37=\"Select Model\",T37=\"PCBL\"), 0,IF(AD37=0,0,-primaryAirSensibleCapacityIP($T37,$W37,activeRoomTempHeating,activePriAirTempHeating,$Y37,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T37=\"Select Model\", \"\", InductionRatio($T37,BD37,$W37,$Y37)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T37=\"Select Model\", \"\",IF($T37=\"PCBL\",\"N/A\",minVAVSetBack(AA37, Y37))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T37=\"Select Model\", \"\",IF($T37= \"PCBL\",\"N/A\",getDischargeAirTemp($T37,$V37,$AC37,$W37,BD37,$AL37, $Y37, $AS37, \"cooling\",activeElevation,$AB37,$AJ37,$AV37,$BB37))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T37=\"Select Model\",$T37=\"PCBL\"), \"\",getDischargeAirTemp($T37,$V37,$AD37,$W37,BD37,$AL37, $Y37, $AY37, \"heating\",activeElevation,$AB37,$AJ37,$AV37,$BB37)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T37=\"Select Model\", \"\",IF(OR($T37=\"ACBC_1W\",$T37=\"ACBC_2W\",LEFT($T37,4)=\"ACBR\",$T37 = \"LIU24_2W\",LEFT($T37,3)=\"RIU\",LEFT($T37,6)=\"ACBL12\"), IF((soundLevel($T37, $AB37, BD37, $Y37, $W37,$AJ37,$AA37,\"dba\"))<15,\"<15\",soundLevel($T37, $AB37, BD37, $Y37, $W37,$AJ37,$AA37,\"dba\")+0.4),IF((soundLevel($T37, $AB37, BD37, $Y37, $W37,$AJ37,$AA37,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T37, $AB37, BD37, $Y37, $W37,$AJ37,$AA37,\"dba\")+5)<15, \"<15\", soundLevel($T37, $AB37, BD37,$Y37, $W37,$AJ37,$AA37,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T37=\"Select Model\", \"\",IF(OR($T37=\"ACBC_1W\",$T37=\"ACBC_2W\",LEFT($T37,4)=\"ACBR\",$T37=\"LIU24_2W\",LEFT($T37,3)=\"RIU\",LEFT($T37,6)=\"ACBL12\"), IF((soundLevel($T37, $AB37, BD37, $Y37, $W37,$AJ37,$AA37,\"NC\"))<15,\"<15\",soundLevel($T37, $AB37, BD37, $Y37, $W37,$AJ37,$AA37,\"NC\")+0.4),IF((soundLevel($T37, $AB37, BD37, $Y37, $W37,$AJ37,$AA37,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T37, $AB37, BD37, $Y37, $W37,$AJ37,$AA37,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T37, $AB37, BD37, $Y37, $W37,$AJ37,$AA37,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T37=\"Select Model\",\"\",IF($T37=\"LIU24_2W\",calcQwIP($Y37,$W37,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC37,$AI37,\"latent\",$U37&\"P\"&IF($V37=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T37,activeElevation),\"\"))","v":""},{"$f":"IF($T37=\"Select Model\",\"\",IF($T37=\"ACBC_1W\",calcQwIP($Y37,$W37,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC37,BD37,\"capacity\",$U37&\"P\"&IF($V37=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T37,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y37,$W37,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC37,BD37,\"capacity\",$U37&\"P\"&IF($V37=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T37,activeElevation)))","v":""},"",{"$f":"IF(T37=\"Select Model\", 0,waterPressureDrop(W37, U37 & \"P\" & IF(V37=\"Dual\",2,1) &\"C\", AC37, \"cooling\", T37))","v":0},{"$f":"IF(T37=\"Select Model\", \"\",getReturnWaterTemp(T37,AC37, activeEWTCooling, AS37, \"cooling\"))","v":""},"",{"$f":"IF($T37<>\"ACBC_1W\",\"\",IF($J37=\"\",\"\",FintubeCapacity($T37,$W37,$AE37,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T37=\"Select Model\",T37=\"PCBL\"),\"\",calcQwIP(Y37,W37,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD37,BD37,\"capacity\",U37&\"P\"&IF(V37=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T37,activeElevation))","v":""},"",{"$f":"IF(OR(T37=\"Select Model\",T37=\"PCBL\"), \"\",IF(AY37=0,\"N/A\",waterPressureDrop(W37, U37 & \"P\" & IF(V37=\"Dual\",2,1) &\"C\", AD37, \"heating\", T37)))","v":""},{"$f":"IF(OR(T37=\"Select Model\",T37=\"PCBL\"), \"\",IF(AY37=0,getReturnWaterTemp(T37,AE37, activeEWTHeating, AX37, \"heating\"),getReturnWaterTemp(T37,AD37, activeEWTHeating, AY37, \"heating\")))","v":""},"",{"$f":" getNozzle(T37, W37, Y37, Z37, activeElevation, TRUE)","v":0}]
["Glycol Concentration %",null,0,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I38)),I38<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I38, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H38)),H38<0),\"\",intlEstQuantity(T38, W38*12, H38)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T38=\"Select Model\",\"\",coilCircuitChange(W38, U38, AC38, T38,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T38=\"Select Model\",\"\",beamWidth(T38))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T38=\"Select Model\",T38=\"PCBL\"), 0,getSPIP(T38, W38, Y38, BD38, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T38=\"Select Model\", \"\",IF(T38=\"PCBL\",0,primaryAirSensibleCapacityIP($T38,$W38,activeRoomTempCooling,activePriAirTempCooling,$Y38,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T38=\"Select Model\",\"\",IF($T38=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y38,activeElevation)))","v":""},{"$f":"IF(OR(T38=\"Select Model\",T38=\"PCBL\"), 0,IF(AD38=0,0,-primaryAirSensibleCapacityIP($T38,$W38,activeRoomTempHeating,activePriAirTempHeating,$Y38,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T38=\"Select Model\", \"\", InductionRatio($T38,BD38,$W38,$Y38)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T38=\"Select Model\", \"\",IF($T38=\"PCBL\",\"N/A\",minVAVSetBack(AA38, Y38))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T38=\"Select Model\", \"\",IF($T38= \"PCBL\",\"N/A\",getDischargeAirTemp($T38,$V38,$AC38,$W38,BD38,$AL38, $Y38, $AS38, \"cooling\",activeElevation,$AB38,$AJ38,$AV38,$BB38))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T38=\"Select Model\",$T38=\"PCBL\"), \"\",getDischargeAirTemp($T38,$V38,$AD38,$W38,BD38,$AL38, $Y38, $AY38, \"heating\",activeElevation,$AB38,$AJ38,$AV38,$BB38)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T38=\"Select Model\", \"\",IF(OR($T38=\"ACBC_1W\",$T38=\"ACBC_2W\",LEFT($T38,4)=\"ACBR\",$T38 = \"LIU24_2W\",LEFT($T38,3)=\"RIU\",LEFT($T38,6)=\"ACBL12\"), IF((soundLevel($T38, $AB38, BD38, $Y38, $W38,$AJ38,$AA38,\"dba\"))<15,\"<15\",soundLevel($T38, $AB38, BD38, $Y38, $W38,$AJ38,$AA38,\"dba\")+0.4),IF((soundLevel($T38, $AB38, BD38, $Y38, $W38,$AJ38,$AA38,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T38, $AB38, BD38, $Y38, $W38,$AJ38,$AA38,\"dba\")+5)<15, \"<15\", soundLevel($T38, $AB38, BD38,$Y38, $W38,$AJ38,$AA38,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T38=\"Select Model\", \"\",IF(OR($T38=\"ACBC_1W\",$T38=\"ACBC_2W\",LEFT($T38,4)=\"ACBR\",$T38=\"LIU24_2W\",LEFT($T38,3)=\"RIU\",LEFT($T38,6)=\"ACBL12\"), IF((soundLevel($T38, $AB38, BD38, $Y38, $W38,$AJ38,$AA38,\"NC\"))<15,\"<15\",soundLevel($T38, $AB38, BD38, $Y38, $W38,$AJ38,$AA38,\"NC\")+0.4),IF((soundLevel($T38, $AB38, BD38, $Y38, $W38,$AJ38,$AA38,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T38, $AB38, BD38, $Y38, $W38,$AJ38,$AA38,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T38, $AB38, BD38, $Y38, $W38,$AJ38,$AA38,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T38=\"Select Model\",\"\",IF($T38=\"LIU24_2W\",calcQwIP($Y38,$W38,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC38,$AI38,\"latent\",$U38&\"P\"&IF($V38=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T38,activeElevation),\"\"))","v":""},{"$f":"IF($T38=\"Select Model\",\"\",IF($T38=\"ACBC_1W\",calcQwIP($Y38,$W38,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC38,BD38,\"capacity\",$U38&\"P\"&IF($V38=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T38,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y38,$W38,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC38,BD38,\"capacity\",$U38&\"P\"&IF($V38=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T38,activeElevation)))","v":""},"",{"$f":"IF(T38=\"Select Model\", 0,waterPressureDrop(W38, U38 & \"P\" & IF(V38=\"Dual\",2,1) &\"C\", AC38, \"cooling\", T38))","v":0},{"$f":"IF(T38=\"Select Model\", \"\",getReturnWaterTemp(T38,AC38, activeEWTCooling, AS38, \"cooling\"))","v":""},"",{"$f":"IF($T38<>\"ACBC_1W\",\"\",IF($J38=\"\",\"\",FintubeCapacity($T38,$W38,$AE38,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T38=\"Select Model\",T38=\"PCBL\"),\"\",calcQwIP(Y38,W38,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD38,BD38,\"capacity\",U38&\"P\"&IF(V38=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T38,activeElevation))","v":""},"",{"$f":"IF(OR(T38=\"Select Model\",T38=\"PCBL\"), \"\",IF(AY38=0,\"N/A\",waterPressureDrop(W38, U38 & \"P\" & IF(V38=\"Dual\",2,1) &\"C\", AD38, \"heating\", T38)))","v":""},{"$f":"IF(OR(T38=\"Select Model\",T38=\"PCBL\"), \"\",IF(AY38=0,getReturnWaterTemp(T38,AE38, activeEWTHeating, AX38, \"heating\"),getReturnWaterTemp(T38,AD38, activeEWTHeating, AY38, \"heating\")))","v":""},"",{"$f":" getNozzle(T38, W38, Y38, Z38, activeElevation, TRUE)","v":0}]
["Fluid Type (Heating)",null,"Water",null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I39)),I39<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I39, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H39)),H39<0),\"\",intlEstQuantity(T39, W39*12, H39)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T39=\"Select Model\",\"\",coilCircuitChange(W39, U39, AC39, T39,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T39=\"Select Model\",\"\",beamWidth(T39))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T39=\"Select Model\",T39=\"PCBL\"), 0,getSPIP(T39, W39, Y39, BD39, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T39=\"Select Model\", \"\",IF(T39=\"PCBL\",0,primaryAirSensibleCapacityIP($T39,$W39,activeRoomTempCooling,activePriAirTempCooling,$Y39,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T39=\"Select Model\",\"\",IF($T39=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y39,activeElevation)))","v":""},{"$f":"IF(OR(T39=\"Select Model\",T39=\"PCBL\"), 0,IF(AD39=0,0,-primaryAirSensibleCapacityIP($T39,$W39,activeRoomTempHeating,activePriAirTempHeating,$Y39,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T39=\"Select Model\", \"\", InductionRatio($T39,BD39,$W39,$Y39)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T39=\"Select Model\", \"\",IF($T39=\"PCBL\",\"N/A\",minVAVSetBack(AA39, Y39))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T39=\"Select Model\", \"\",IF($T39= \"PCBL\",\"N/A\",getDischargeAirTemp($T39,$V39,$AC39,$W39,BD39,$AL39, $Y39, $AS39, \"cooling\",activeElevation,$AB39,$AJ39,$AV39,$BB39))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T39=\"Select Model\",$T39=\"PCBL\"), \"\",getDischargeAirTemp($T39,$V39,$AD39,$W39,BD39,$AL39, $Y39, $AY39, \"heating\",activeElevation,$AB39,$AJ39,$AV39,$BB39)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T39=\"Select Model\", \"\",IF(OR($T39=\"ACBC_1W\",$T39=\"ACBC_2W\",LEFT($T39,4)=\"ACBR\",$T39 = \"LIU24_2W\",LEFT($T39,3)=\"RIU\",LEFT($T39,6)=\"ACBL12\"), IF((soundLevel($T39, $AB39, BD39, $Y39, $W39,$AJ39,$AA39,\"dba\"))<15,\"<15\",soundLevel($T39, $AB39, BD39, $Y39, $W39,$AJ39,$AA39,\"dba\")+0.4),IF((soundLevel($T39, $AB39, BD39, $Y39, $W39,$AJ39,$AA39,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T39, $AB39, BD39, $Y39, $W39,$AJ39,$AA39,\"dba\")+5)<15, \"<15\", soundLevel($T39, $AB39, BD39,$Y39, $W39,$AJ39,$AA39,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T39=\"Select Model\", \"\",IF(OR($T39=\"ACBC_1W\",$T39=\"ACBC_2W\",LEFT($T39,4)=\"ACBR\",$T39=\"LIU24_2W\",LEFT($T39,3)=\"RIU\",LEFT($T39,6)=\"ACBL12\"), IF((soundLevel($T39, $AB39, BD39, $Y39, $W39,$AJ39,$AA39,\"NC\"))<15,\"<15\",soundLevel($T39, $AB39, BD39, $Y39, $W39,$AJ39,$AA39,\"NC\")+0.4),IF((soundLevel($T39, $AB39, BD39, $Y39, $W39,$AJ39,$AA39,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T39, $AB39, BD39, $Y39, $W39,$AJ39,$AA39,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T39, $AB39, BD39, $Y39, $W39,$AJ39,$AA39,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T39=\"Select Model\",\"\",IF($T39=\"LIU24_2W\",calcQwIP($Y39,$W39,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC39,$AI39,\"latent\",$U39&\"P\"&IF($V39=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T39,activeElevation),\"\"))","v":""},{"$f":"IF($T39=\"Select Model\",\"\",IF($T39=\"ACBC_1W\",calcQwIP($Y39,$W39,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC39,BD39,\"capacity\",$U39&\"P\"&IF($V39=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T39,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y39,$W39,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC39,BD39,\"capacity\",$U39&\"P\"&IF($V39=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T39,activeElevation)))","v":""},"",{"$f":"IF(T39=\"Select Model\", 0,waterPressureDrop(W39, U39 & \"P\" & IF(V39=\"Dual\",2,1) &\"C\", AC39, \"cooling\", T39))","v":0},{"$f":"IF(T39=\"Select Model\", \"\",getReturnWaterTemp(T39,AC39, activeEWTCooling, AS39, \"cooling\"))","v":""},"",{"$f":"IF($T39<>\"ACBC_1W\",\"\",IF($J39=\"\",\"\",FintubeCapacity($T39,$W39,$AE39,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T39=\"Select Model\",T39=\"PCBL\"),\"\",calcQwIP(Y39,W39,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD39,BD39,\"capacity\",U39&\"P\"&IF(V39=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T39,activeElevation))","v":""},"",{"$f":"IF(OR(T39=\"Select Model\",T39=\"PCBL\"), \"\",IF(AY39=0,\"N/A\",waterPressureDrop(W39, U39 & \"P\" & IF(V39=\"Dual\",2,1) &\"C\", AD39, \"heating\", T39)))","v":""},{"$f":"IF(OR(T39=\"Select Model\",T39=\"PCBL\"), \"\",IF(AY39=0,getReturnWaterTemp(T39,AE39, activeEWTHeating, AX39, \"heating\"),getReturnWaterTemp(T39,AD39, activeEWTHeating, AY39, \"heating\")))","v":""},"",{"$f":" getNozzle(T39, W39, Y39, Z39, activeElevation, TRUE)","v":0}]
["Glycol Concentration %",null,0,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I40)),I40<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I40, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H40)),H40<0),\"\",intlEstQuantity(T40, W40*12, H40)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T40=\"Select Model\",\"\",coilCircuitChange(W40, U40, AC40, T40,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T40=\"Select Model\",\"\",beamWidth(T40))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T40=\"Select Model\",T40=\"PCBL\"), 0,getSPIP(T40, W40, Y40, BD40, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T40=\"Select Model\", \"\",IF(T40=\"PCBL\",0,primaryAirSensibleCapacityIP($T40,$W40,activeRoomTempCooling,activePriAirTempCooling,$Y40,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T40=\"Select Model\",\"\",IF($T40=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y40,activeElevation)))","v":""},{"$f":"IF(OR(T40=\"Select Model\",T40=\"PCBL\"), 0,IF(AD40=0,0,-primaryAirSensibleCapacityIP($T40,$W40,activeRoomTempHeating,activePriAirTempHeating,$Y40,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T40=\"Select Model\", \"\", InductionRatio($T40,BD40,$W40,$Y40)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T40=\"Select Model\", \"\",IF($T40=\"PCBL\",\"N/A\",minVAVSetBack(AA40, Y40))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T40=\"Select Model\", \"\",IF($T40= \"PCBL\",\"N/A\",getDischargeAirTemp($T40,$V40,$AC40,$W40,BD40,$AL40, $Y40, $AS40, \"cooling\",activeElevation,$AB40,$AJ40,$AV40,$BB40))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T40=\"Select Model\",$T40=\"PCBL\"), \"\",getDischargeAirTemp($T40,$V40,$AD40,$W40,BD40,$AL40, $Y40, $AY40, \"heating\",activeElevation,$AB40,$AJ40,$AV40,$BB40)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T40=\"Select Model\", \"\",IF(OR($T40=\"ACBC_1W\",$T40=\"ACBC_2W\",LEFT($T40,4)=\"ACBR\",$T40 = \"LIU24_2W\",LEFT($T40,3)=\"RIU\",LEFT($T40,6)=\"ACBL12\"), IF((soundLevel($T40, $AB40, BD40, $Y40, $W40,$AJ40,$AA40,\"dba\"))<15,\"<15\",soundLevel($T40, $AB40, BD40, $Y40, $W40,$AJ40,$AA40,\"dba\")+0.4),IF((soundLevel($T40, $AB40, BD40, $Y40, $W40,$AJ40,$AA40,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T40, $AB40, BD40, $Y40, $W40,$AJ40,$AA40,\"dba\")+5)<15, \"<15\", soundLevel($T40, $AB40, BD40,$Y40, $W40,$AJ40,$AA40,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T40=\"Select Model\", \"\",IF(OR($T40=\"ACBC_1W\",$T40=\"ACBC_2W\",LEFT($T40,4)=\"ACBR\",$T40=\"LIU24_2W\",LEFT($T40,3)=\"RIU\",LEFT($T40,6)=\"ACBL12\"), IF((soundLevel($T40, $AB40, BD40, $Y40, $W40,$AJ40,$AA40,\"NC\"))<15,\"<15\",soundLevel($T40, $AB40, BD40, $Y40, $W40,$AJ40,$AA40,\"NC\")+0.4),IF((soundLevel($T40, $AB40, BD40, $Y40, $W40,$AJ40,$AA40,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T40, $AB40, BD40, $Y40, $W40,$AJ40,$AA40,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T40, $AB40, BD40, $Y40, $W40,$AJ40,$AA40,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T40=\"Select Model\",\"\",IF($T40=\"LIU24_2W\",calcQwIP($Y40,$W40,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC40,$AI40,\"latent\",$U40&\"P\"&IF($V40=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T40,activeElevation),\"\"))","v":""},{"$f":"IF($T40=\"Select Model\",\"\",IF($T40=\"ACBC_1W\",calcQwIP($Y40,$W40,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC40,BD40,\"capacity\",$U40&\"P\"&IF($V40=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T40,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y40,$W40,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC40,BD40,\"capacity\",$U40&\"P\"&IF($V40=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T40,activeElevation)))","v":""},"",{"$f":"IF(T40=\"Select Model\", 0,waterPressureDrop(W40, U40 & \"P\" & IF(V40=\"Dual\",2,1) &\"C\", AC40, \"cooling\", T40))","v":0},{"$f":"IF(T40=\"Select Model\", \"\",getReturnWaterTemp(T40,AC40, activeEWTCooling, AS40, \"cooling\"))","v":""},"",{"$f":"IF($T40<>\"ACBC_1W\",\"\",IF($J40=\"\",\"\",FintubeCapacity($T40,$W40,$AE40,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T40=\"Select Model\",T40=\"PCBL\"),\"\",calcQwIP(Y40,W40,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD40,BD40,\"capacity\",U40&\"P\"&IF(V40=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T40,activeElevation))","v":""},"",{"$f":"IF(OR(T40=\"Select Model\",T40=\"PCBL\"), \"\",IF(AY40=0,\"N/A\",waterPressureDrop(W40, U40 & \"P\" & IF(V40=\"Dual\",2,1) &\"C\", AD40, \"heating\", T40)))","v":""},{"$f":"IF(OR(T40=\"Select Model\",T40=\"PCBL\"), \"\",IF(AY40=0,getReturnWaterTemp(T40,AE40, activeEWTHeating, AX40, \"heating\"),getReturnWaterTemp(T40,AD40, activeEWTHeating, AY40, \"heating\")))","v":""},"",{"$f":" getNozzle(T40, W40, Y40, Z40, activeElevation, TRUE)","v":0}]
["Max Waterside ∆P ft w.g.",null,10,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I41)),I41<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I41, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H41)),H41<0),\"\",intlEstQuantity(T41, W41*12, H41)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T41=\"Select Model\",\"\",coilCircuitChange(W41, U41, AC41, T41,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T41=\"Select Model\",\"\",beamWidth(T41))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T41=\"Select Model\",T41=\"PCBL\"), 0,getSPIP(T41, W41, Y41, BD41, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T41=\"Select Model\", \"\",IF(T41=\"PCBL\",0,primaryAirSensibleCapacityIP($T41,$W41,activeRoomTempCooling,activePriAirTempCooling,$Y41,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T41=\"Select Model\",\"\",IF($T41=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y41,activeElevation)))","v":""},{"$f":"IF(OR(T41=\"Select Model\",T41=\"PCBL\"), 0,IF(AD41=0,0,-primaryAirSensibleCapacityIP($T41,$W41,activeRoomTempHeating,activePriAirTempHeating,$Y41,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T41=\"Select Model\", \"\", InductionRatio($T41,BD41,$W41,$Y41)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T41=\"Select Model\", \"\",IF($T41=\"PCBL\",\"N/A\",minVAVSetBack(AA41, Y41))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T41=\"Select Model\", \"\",IF($T41= \"PCBL\",\"N/A\",getDischargeAirTemp($T41,$V41,$AC41,$W41,BD41,$AL41, $Y41, $AS41, \"cooling\",activeElevation,$AB41,$AJ41,$AV41,$BB41))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T41=\"Select Model\",$T41=\"PCBL\"), \"\",getDischargeAirTemp($T41,$V41,$AD41,$W41,BD41,$AL41, $Y41, $AY41, \"heating\",activeElevation,$AB41,$AJ41,$AV41,$BB41)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T41=\"Select Model\", \"\",IF(OR($T41=\"ACBC_1W\",$T41=\"ACBC_2W\",LEFT($T41,4)=\"ACBR\",$T41 = \"LIU24_2W\",LEFT($T41,3)=\"RIU\",LEFT($T41,6)=\"ACBL12\"), IF((soundLevel($T41, $AB41, BD41, $Y41, $W41,$AJ41,$AA41,\"dba\"))<15,\"<15\",soundLevel($T41, $AB41, BD41, $Y41, $W41,$AJ41,$AA41,\"dba\")+0.4),IF((soundLevel($T41, $AB41, BD41, $Y41, $W41,$AJ41,$AA41,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T41, $AB41, BD41, $Y41, $W41,$AJ41,$AA41,\"dba\")+5)<15, \"<15\", soundLevel($T41, $AB41, BD41,$Y41, $W41,$AJ41,$AA41,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T41=\"Select Model\", \"\",IF(OR($T41=\"ACBC_1W\",$T41=\"ACBC_2W\",LEFT($T41,4)=\"ACBR\",$T41=\"LIU24_2W\",LEFT($T41,3)=\"RIU\",LEFT($T41,6)=\"ACBL12\"), IF((soundLevel($T41, $AB41, BD41, $Y41, $W41,$AJ41,$AA41,\"NC\"))<15,\"<15\",soundLevel($T41, $AB41, BD41, $Y41, $W41,$AJ41,$AA41,\"NC\")+0.4),IF((soundLevel($T41, $AB41, BD41, $Y41, $W41,$AJ41,$AA41,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T41, $AB41, BD41, $Y41, $W41,$AJ41,$AA41,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T41, $AB41, BD41, $Y41, $W41,$AJ41,$AA41,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T41=\"Select Model\",\"\",IF($T41=\"LIU24_2W\",calcQwIP($Y41,$W41,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC41,$AI41,\"latent\",$U41&\"P\"&IF($V41=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T41,activeElevation),\"\"))","v":""},{"$f":"IF($T41=\"Select Model\",\"\",IF($T41=\"ACBC_1W\",calcQwIP($Y41,$W41,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC41,BD41,\"capacity\",$U41&\"P\"&IF($V41=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T41,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y41,$W41,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC41,BD41,\"capacity\",$U41&\"P\"&IF($V41=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T41,activeElevation)))","v":""},"",{"$f":"IF(T41=\"Select Model\", 0,waterPressureDrop(W41, U41 & \"P\" & IF(V41=\"Dual\",2,1) &\"C\", AC41, \"cooling\", T41))","v":0},{"$f":"IF(T41=\"Select Model\", \"\",getReturnWaterTemp(T41,AC41, activeEWTCooling, AS41, \"cooling\"))","v":""},"",{"$f":"IF($T41<>\"ACBC_1W\",\"\",IF($J41=\"\",\"\",FintubeCapacity($T41,$W41,$AE41,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T41=\"Select Model\",T41=\"PCBL\"),\"\",calcQwIP(Y41,W41,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD41,BD41,\"capacity\",U41&\"P\"&IF(V41=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T41,activeElevation))","v":""},"",{"$f":"IF(OR(T41=\"Select Model\",T41=\"PCBL\"), \"\",IF(AY41=0,\"N/A\",waterPressureDrop(W41, U41 & \"P\" & IF(V41=\"Dual\",2,1) &\"C\", AD41, \"heating\", T41)))","v":""},{"$f":"IF(OR(T41=\"Select Model\",T41=\"PCBL\"), \"\",IF(AY41=0,getReturnWaterTemp(T41,AE41, activeEWTHeating, AX41, \"heating\"),getReturnWaterTemp(T41,AD41, activeEWTHeating, AY41, \"heating\")))","v":""},"",{"$f":" getNozzle(T41, W41, Y41, Z41, activeElevation, TRUE)","v":0}]
["Stratification Credit",null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I42)),I42<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I42, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H42)),H42<0),\"\",intlEstQuantity(T42, W42*12, H42)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T42=\"Select Model\",\"\",coilCircuitChange(W42, U42, AC42, T42,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T42=\"Select Model\",\"\",beamWidth(T42))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T42=\"Select Model\",T42=\"PCBL\"), 0,getSPIP(T42, W42, Y42, BD42, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T42=\"Select Model\", \"\",IF(T42=\"PCBL\",0,primaryAirSensibleCapacityIP($T42,$W42,activeRoomTempCooling,activePriAirTempCooling,$Y42,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T42=\"Select Model\",\"\",IF($T42=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y42,activeElevation)))","v":""},{"$f":"IF(OR(T42=\"Select Model\",T42=\"PCBL\"), 0,IF(AD42=0,0,-primaryAirSensibleCapacityIP($T42,$W42,activeRoomTempHeating,activePriAirTempHeating,$Y42,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T42=\"Select Model\", \"\", InductionRatio($T42,BD42,$W42,$Y42)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T42=\"Select Model\", \"\",IF($T42=\"PCBL\",\"N/A\",minVAVSetBack(AA42, Y42))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T42=\"Select Model\", \"\",IF($T42= \"PCBL\",\"N/A\",getDischargeAirTemp($T42,$V42,$AC42,$W42,BD42,$AL42, $Y42, $AS42, \"cooling\",activeElevation,$AB42,$AJ42,$AV42,$BB42))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T42=\"Select Model\",$T42=\"PCBL\"), \"\",getDischargeAirTemp($T42,$V42,$AD42,$W42,BD42,$AL42, $Y42, $AY42, \"heating\",activeElevation,$AB42,$AJ42,$AV42,$BB42)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T42=\"Select Model\", \"\",IF(OR($T42=\"ACBC_1W\",$T42=\"ACBC_2W\",LEFT($T42,4)=\"ACBR\",$T42 = \"LIU24_2W\",LEFT($T42,3)=\"RIU\",LEFT($T42,6)=\"ACBL12\"), IF((soundLevel($T42, $AB42, BD42, $Y42, $W42,$AJ42,$AA42,\"dba\"))<15,\"<15\",soundLevel($T42, $AB42, BD42, $Y42, $W42,$AJ42,$AA42,\"dba\")+0.4),IF((soundLevel($T42, $AB42, BD42, $Y42, $W42,$AJ42,$AA42,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T42, $AB42, BD42, $Y42, $W42,$AJ42,$AA42,\"dba\")+5)<15, \"<15\", soundLevel($T42, $AB42, BD42,$Y42, $W42,$AJ42,$AA42,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T42=\"Select Model\", \"\",IF(OR($T42=\"ACBC_1W\",$T42=\"ACBC_2W\",LEFT($T42,4)=\"ACBR\",$T42=\"LIU24_2W\",LEFT($T42,3)=\"RIU\",LEFT($T42,6)=\"ACBL12\"), IF((soundLevel($T42, $AB42, BD42, $Y42, $W42,$AJ42,$AA42,\"NC\"))<15,\"<15\",soundLevel($T42, $AB42, BD42, $Y42, $W42,$AJ42,$AA42,\"NC\")+0.4),IF((soundLevel($T42, $AB42, BD42, $Y42, $W42,$AJ42,$AA42,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T42, $AB42, BD42, $Y42, $W42,$AJ42,$AA42,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T42, $AB42, BD42, $Y42, $W42,$AJ42,$AA42,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T42=\"Select Model\",\"\",IF($T42=\"LIU24_2W\",calcQwIP($Y42,$W42,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC42,$AI42,\"latent\",$U42&\"P\"&IF($V42=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T42,activeElevation),\"\"))","v":""},{"$f":"IF($T42=\"Select Model\",\"\",IF($T42=\"ACBC_1W\",calcQwIP($Y42,$W42,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC42,BD42,\"capacity\",$U42&\"P\"&IF($V42=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T42,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y42,$W42,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC42,BD42,\"capacity\",$U42&\"P\"&IF($V42=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T42,activeElevation)))","v":""},"",{"$f":"IF(T42=\"Select Model\", 0,waterPressureDrop(W42, U42 & \"P\" & IF(V42=\"Dual\",2,1) &\"C\", AC42, \"cooling\", T42))","v":0},{"$f":"IF(T42=\"Select Model\", \"\",getReturnWaterTemp(T42,AC42, activeEWTCooling, AS42, \"cooling\"))","v":""},"",{"$f":"IF($T42<>\"ACBC_1W\",\"\",IF($J42=\"\",\"\",FintubeCapacity($T42,$W42,$AE42,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T42=\"Select Model\",T42=\"PCBL\"),\"\",calcQwIP(Y42,W42,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD42,BD42,\"capacity\",U42&\"P\"&IF(V42=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T42,activeElevation))","v":""},"",{"$f":"IF(OR(T42=\"Select Model\",T42=\"PCBL\"), \"\",IF(AY42=0,\"N/A\",waterPressureDrop(W42, U42 & \"P\" & IF(V42=\"Dual\",2,1) &\"C\", AD42, \"heating\", T42)))","v":""},{"$f":"IF(OR(T42=\"Select Model\",T42=\"PCBL\"), \"\",IF(AY42=0,getReturnWaterTemp(T42,AE42, activeEWTHeating, AX42, \"heating\"),getReturnWaterTemp(T42,AD42, activeEWTHeating, AY42, \"heating\")))","v":""},"",{"$f":" getNozzle(T42, W42, Y42, Z42, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I43)),I43<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I43, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H43)),H43<0),\"\",intlEstQuantity(T43, W43*12, H43)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T43=\"Select Model\",\"\",coilCircuitChange(W43, U43, AC43, T43,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T43=\"Select Model\",\"\",beamWidth(T43))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T43=\"Select Model\",T43=\"PCBL\"), 0,getSPIP(T43, W43, Y43, BD43, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T43=\"Select Model\", \"\",IF(T43=\"PCBL\",0,primaryAirSensibleCapacityIP($T43,$W43,activeRoomTempCooling,activePriAirTempCooling,$Y43,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T43=\"Select Model\",\"\",IF($T43=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y43,activeElevation)))","v":""},{"$f":"IF(OR(T43=\"Select Model\",T43=\"PCBL\"), 0,IF(AD43=0,0,-primaryAirSensibleCapacityIP($T43,$W43,activeRoomTempHeating,activePriAirTempHeating,$Y43,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T43=\"Select Model\", \"\", InductionRatio($T43,BD43,$W43,$Y43)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T43=\"Select Model\", \"\",IF($T43=\"PCBL\",\"N/A\",minVAVSetBack(AA43, Y43))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T43=\"Select Model\", \"\",IF($T43= \"PCBL\",\"N/A\",getDischargeAirTemp($T43,$V43,$AC43,$W43,BD43,$AL43, $Y43, $AS43, \"cooling\",activeElevation,$AB43,$AJ43,$AV43,$BB43))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T43=\"Select Model\",$T43=\"PCBL\"), \"\",getDischargeAirTemp($T43,$V43,$AD43,$W43,BD43,$AL43, $Y43, $AY43, \"heating\",activeElevation,$AB43,$AJ43,$AV43,$BB43)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T43=\"Select Model\", \"\",IF(OR($T43=\"ACBC_1W\",$T43=\"ACBC_2W\",LEFT($T43,4)=\"ACBR\",$T43 = \"LIU24_2W\",LEFT($T43,3)=\"RIU\",LEFT($T43,6)=\"ACBL12\"), IF((soundLevel($T43, $AB43, BD43, $Y43, $W43,$AJ43,$AA43,\"dba\"))<15,\"<15\",soundLevel($T43, $AB43, BD43, $Y43, $W43,$AJ43,$AA43,\"dba\")+0.4),IF((soundLevel($T43, $AB43, BD43, $Y43, $W43,$AJ43,$AA43,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T43, $AB43, BD43, $Y43, $W43,$AJ43,$AA43,\"dba\")+5)<15, \"<15\", soundLevel($T43, $AB43, BD43,$Y43, $W43,$AJ43,$AA43,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T43=\"Select Model\", \"\",IF(OR($T43=\"ACBC_1W\",$T43=\"ACBC_2W\",LEFT($T43,4)=\"ACBR\",$T43=\"LIU24_2W\",LEFT($T43,3)=\"RIU\",LEFT($T43,6)=\"ACBL12\"), IF((soundLevel($T43, $AB43, BD43, $Y43, $W43,$AJ43,$AA43,\"NC\"))<15,\"<15\",soundLevel($T43, $AB43, BD43, $Y43, $W43,$AJ43,$AA43,\"NC\")+0.4),IF((soundLevel($T43, $AB43, BD43, $Y43, $W43,$AJ43,$AA43,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T43, $AB43, BD43, $Y43, $W43,$AJ43,$AA43,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T43, $AB43, BD43, $Y43, $W43,$AJ43,$AA43,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T43=\"Select Model\",\"\",IF($T43=\"LIU24_2W\",calcQwIP($Y43,$W43,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC43,$AI43,\"latent\",$U43&\"P\"&IF($V43=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T43,activeElevation),\"\"))","v":""},{"$f":"IF($T43=\"Select Model\",\"\",IF($T43=\"ACBC_1W\",calcQwIP($Y43,$W43,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC43,BD43,\"capacity\",$U43&\"P\"&IF($V43=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T43,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y43,$W43,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC43,BD43,\"capacity\",$U43&\"P\"&IF($V43=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T43,activeElevation)))","v":""},"",{"$f":"IF(T43=\"Select Model\", 0,waterPressureDrop(W43, U43 & \"P\" & IF(V43=\"Dual\",2,1) &\"C\", AC43, \"cooling\", T43))","v":0},{"$f":"IF(T43=\"Select Model\", \"\",getReturnWaterTemp(T43,AC43, activeEWTCooling, AS43, \"cooling\"))","v":""},"",{"$f":"IF($T43<>\"ACBC_1W\",\"\",IF($J43=\"\",\"\",FintubeCapacity($T43,$W43,$AE43,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T43=\"Select Model\",T43=\"PCBL\"),\"\",calcQwIP(Y43,W43,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD43,BD43,\"capacity\",U43&\"P\"&IF(V43=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T43,activeElevation))","v":""},"",{"$f":"IF(OR(T43=\"Select Model\",T43=\"PCBL\"), \"\",IF(AY43=0,\"N/A\",waterPressureDrop(W43, U43 & \"P\" & IF(V43=\"Dual\",2,1) &\"C\", AD43, \"heating\", T43)))","v":""},{"$f":"IF(OR(T43=\"Select Model\",T43=\"PCBL\"), \"\",IF(AY43=0,getReturnWaterTemp(T43,AE43, activeEWTHeating, AX43, \"heating\"),getReturnWaterTemp(T43,AD43, activeEWTHeating, AY43, \"heating\")))","v":""},"",{"$f":" getNozzle(T43, W43, Y43, Z43, activeElevation, TRUE)","v":0}]
["Credit Percentage %",null,0.33,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I44)),I44<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I44, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H44)),H44<0),\"\",intlEstQuantity(T44, W44*12, H44)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T44=\"Select Model\",\"\",coilCircuitChange(W44, U44, AC44, T44,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T44=\"Select Model\",\"\",beamWidth(T44))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T44=\"Select Model\",T44=\"PCBL\"), 0,getSPIP(T44, W44, Y44, BD44, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T44=\"Select Model\", \"\",IF(T44=\"PCBL\",0,primaryAirSensibleCapacityIP($T44,$W44,activeRoomTempCooling,activePriAirTempCooling,$Y44,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T44=\"Select Model\",\"\",IF($T44=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y44,activeElevation)))","v":""},{"$f":"IF(OR(T44=\"Select Model\",T44=\"PCBL\"), 0,IF(AD44=0,0,-primaryAirSensibleCapacityIP($T44,$W44,activeRoomTempHeating,activePriAirTempHeating,$Y44,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T44=\"Select Model\", \"\", InductionRatio($T44,BD44,$W44,$Y44)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T44=\"Select Model\", \"\",IF($T44=\"PCBL\",\"N/A\",minVAVSetBack(AA44, Y44))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T44=\"Select Model\", \"\",IF($T44= \"PCBL\",\"N/A\",getDischargeAirTemp($T44,$V44,$AC44,$W44,BD44,$AL44, $Y44, $AS44, \"cooling\",activeElevation,$AB44,$AJ44,$AV44,$BB44))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T44=\"Select Model\",$T44=\"PCBL\"), \"\",getDischargeAirTemp($T44,$V44,$AD44,$W44,BD44,$AL44, $Y44, $AY44, \"heating\",activeElevation,$AB44,$AJ44,$AV44,$BB44)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T44=\"Select Model\", \"\",IF(OR($T44=\"ACBC_1W\",$T44=\"ACBC_2W\",LEFT($T44,4)=\"ACBR\",$T44 = \"LIU24_2W\",LEFT($T44,3)=\"RIU\",LEFT($T44,6)=\"ACBL12\"), IF((soundLevel($T44, $AB44, BD44, $Y44, $W44,$AJ44,$AA44,\"dba\"))<15,\"<15\",soundLevel($T44, $AB44, BD44, $Y44, $W44,$AJ44,$AA44,\"dba\")+0.4),IF((soundLevel($T44, $AB44, BD44, $Y44, $W44,$AJ44,$AA44,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T44, $AB44, BD44, $Y44, $W44,$AJ44,$AA44,\"dba\")+5)<15, \"<15\", soundLevel($T44, $AB44, BD44,$Y44, $W44,$AJ44,$AA44,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T44=\"Select Model\", \"\",IF(OR($T44=\"ACBC_1W\",$T44=\"ACBC_2W\",LEFT($T44,4)=\"ACBR\",$T44=\"LIU24_2W\",LEFT($T44,3)=\"RIU\",LEFT($T44,6)=\"ACBL12\"), IF((soundLevel($T44, $AB44, BD44, $Y44, $W44,$AJ44,$AA44,\"NC\"))<15,\"<15\",soundLevel($T44, $AB44, BD44, $Y44, $W44,$AJ44,$AA44,\"NC\")+0.4),IF((soundLevel($T44, $AB44, BD44, $Y44, $W44,$AJ44,$AA44,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T44, $AB44, BD44, $Y44, $W44,$AJ44,$AA44,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T44, $AB44, BD44, $Y44, $W44,$AJ44,$AA44,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T44=\"Select Model\",\"\",IF($T44=\"LIU24_2W\",calcQwIP($Y44,$W44,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC44,$AI44,\"latent\",$U44&\"P\"&IF($V44=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T44,activeElevation),\"\"))","v":""},{"$f":"IF($T44=\"Select Model\",\"\",IF($T44=\"ACBC_1W\",calcQwIP($Y44,$W44,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC44,BD44,\"capacity\",$U44&\"P\"&IF($V44=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T44,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y44,$W44,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC44,BD44,\"capacity\",$U44&\"P\"&IF($V44=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T44,activeElevation)))","v":""},"",{"$f":"IF(T44=\"Select Model\", 0,waterPressureDrop(W44, U44 & \"P\" & IF(V44=\"Dual\",2,1) &\"C\", AC44, \"cooling\", T44))","v":0},{"$f":"IF(T44=\"Select Model\", \"\",getReturnWaterTemp(T44,AC44, activeEWTCooling, AS44, \"cooling\"))","v":""},"",{"$f":"IF($T44<>\"ACBC_1W\",\"\",IF($J44=\"\",\"\",FintubeCapacity($T44,$W44,$AE44,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T44=\"Select Model\",T44=\"PCBL\"),\"\",calcQwIP(Y44,W44,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD44,BD44,\"capacity\",U44&\"P\"&IF(V44=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T44,activeElevation))","v":""},"",{"$f":"IF(OR(T44=\"Select Model\",T44=\"PCBL\"), \"\",IF(AY44=0,\"N/A\",waterPressureDrop(W44, U44 & \"P\" & IF(V44=\"Dual\",2,1) &\"C\", AD44, \"heating\", T44)))","v":""},{"$f":"IF(OR(T44=\"Select Model\",T44=\"PCBL\"), \"\",IF(AY44=0,getReturnWaterTemp(T44,AE44, activeEWTHeating, AX44, \"heating\"),getReturnWaterTemp(T44,AD44, activeEWTHeating, AY44, \"heating\")))","v":""},"",{"$f":" getNozzle(T44, W44, Y44, Z44, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I45)),I45<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I45, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H45)),H45<0),\"\",intlEstQuantity(T45, W45*12, H45)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T45=\"Select Model\",\"\",coilCircuitChange(W45, U45, AC45, T45,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T45=\"Select Model\",\"\",beamWidth(T45))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T45=\"Select Model\",T45=\"PCBL\"), 0,getSPIP(T45, W45, Y45, BD45, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T45=\"Select Model\", \"\",IF(T45=\"PCBL\",0,primaryAirSensibleCapacityIP($T45,$W45,activeRoomTempCooling,activePriAirTempCooling,$Y45,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T45=\"Select Model\",\"\",IF($T45=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y45,activeElevation)))","v":""},{"$f":"IF(OR(T45=\"Select Model\",T45=\"PCBL\"), 0,IF(AD45=0,0,-primaryAirSensibleCapacityIP($T45,$W45,activeRoomTempHeating,activePriAirTempHeating,$Y45,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T45=\"Select Model\", \"\", InductionRatio($T45,BD45,$W45,$Y45)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T45=\"Select Model\", \"\",IF($T45=\"PCBL\",\"N/A\",minVAVSetBack(AA45, Y45))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T45=\"Select Model\", \"\",IF($T45= \"PCBL\",\"N/A\",getDischargeAirTemp($T45,$V45,$AC45,$W45,BD45,$AL45, $Y45, $AS45, \"cooling\",activeElevation,$AB45,$AJ45,$AV45,$BB45))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T45=\"Select Model\",$T45=\"PCBL\"), \"\",getDischargeAirTemp($T45,$V45,$AD45,$W45,BD45,$AL45, $Y45, $AY45, \"heating\",activeElevation,$AB45,$AJ45,$AV45,$BB45)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T45=\"Select Model\", \"\",IF(OR($T45=\"ACBC_1W\",$T45=\"ACBC_2W\",LEFT($T45,4)=\"ACBR\",$T45 = \"LIU24_2W\",LEFT($T45,3)=\"RIU\",LEFT($T45,6)=\"ACBL12\"), IF((soundLevel($T45, $AB45, BD45, $Y45, $W45,$AJ45,$AA45,\"dba\"))<15,\"<15\",soundLevel($T45, $AB45, BD45, $Y45, $W45,$AJ45,$AA45,\"dba\")+0.4),IF((soundLevel($T45, $AB45, BD45, $Y45, $W45,$AJ45,$AA45,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T45, $AB45, BD45, $Y45, $W45,$AJ45,$AA45,\"dba\")+5)<15, \"<15\", soundLevel($T45, $AB45, BD45,$Y45, $W45,$AJ45,$AA45,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T45=\"Select Model\", \"\",IF(OR($T45=\"ACBC_1W\",$T45=\"ACBC_2W\",LEFT($T45,4)=\"ACBR\",$T45=\"LIU24_2W\",LEFT($T45,3)=\"RIU\",LEFT($T45,6)=\"ACBL12\"), IF((soundLevel($T45, $AB45, BD45, $Y45, $W45,$AJ45,$AA45,\"NC\"))<15,\"<15\",soundLevel($T45, $AB45, BD45, $Y45, $W45,$AJ45,$AA45,\"NC\")+0.4),IF((soundLevel($T45, $AB45, BD45, $Y45, $W45,$AJ45,$AA45,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T45, $AB45, BD45, $Y45, $W45,$AJ45,$AA45,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T45, $AB45, BD45, $Y45, $W45,$AJ45,$AA45,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T45=\"Select Model\",\"\",IF($T45=\"LIU24_2W\",calcQwIP($Y45,$W45,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC45,$AI45,\"latent\",$U45&\"P\"&IF($V45=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T45,activeElevation),\"\"))","v":""},{"$f":"IF($T45=\"Select Model\",\"\",IF($T45=\"ACBC_1W\",calcQwIP($Y45,$W45,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC45,BD45,\"capacity\",$U45&\"P\"&IF($V45=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T45,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y45,$W45,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC45,BD45,\"capacity\",$U45&\"P\"&IF($V45=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T45,activeElevation)))","v":""},"",{"$f":"IF(T45=\"Select Model\", 0,waterPressureDrop(W45, U45 & \"P\" & IF(V45=\"Dual\",2,1) &\"C\", AC45, \"cooling\", T45))","v":0},{"$f":"IF(T45=\"Select Model\", \"\",getReturnWaterTemp(T45,AC45, activeEWTCooling, AS45, \"cooling\"))","v":""},"",{"$f":"IF($T45<>\"ACBC_1W\",\"\",IF($J45=\"\",\"\",FintubeCapacity($T45,$W45,$AE45,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T45=\"Select Model\",T45=\"PCBL\"),\"\",calcQwIP(Y45,W45,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD45,BD45,\"capacity\",U45&\"P\"&IF(V45=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T45,activeElevation))","v":""},"",{"$f":"IF(OR(T45=\"Select Model\",T45=\"PCBL\"), \"\",IF(AY45=0,\"N/A\",waterPressureDrop(W45, U45 & \"P\" & IF(V45=\"Dual\",2,1) &\"C\", AD45, \"heating\", T45)))","v":""},{"$f":"IF(OR(T45=\"Select Model\",T45=\"PCBL\"), \"\",IF(AY45=0,getReturnWaterTemp(T45,AE45, activeEWTHeating, AX45, \"heating\"),getReturnWaterTemp(T45,AD45, activeEWTHeating, AY45, \"heating\")))","v":""},"",{"$f":" getNozzle(T45, W45, Y45, Z45, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I46)),I46<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I46, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H46)),H46<0),\"\",intlEstQuantity(T46, W46*12, H46)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T46=\"Select Model\",\"\",coilCircuitChange(W46, U46, AC46, T46,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T46=\"Select Model\",\"\",beamWidth(T46))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T46=\"Select Model\",T46=\"PCBL\"), 0,getSPIP(T46, W46, Y46, BD46, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T46=\"Select Model\", \"\",IF(T46=\"PCBL\",0,primaryAirSensibleCapacityIP($T46,$W46,activeRoomTempCooling,activePriAirTempCooling,$Y46,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T46=\"Select Model\",\"\",IF($T46=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y46,activeElevation)))","v":""},{"$f":"IF(OR(T46=\"Select Model\",T46=\"PCBL\"), 0,IF(AD46=0,0,-primaryAirSensibleCapacityIP($T46,$W46,activeRoomTempHeating,activePriAirTempHeating,$Y46,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T46=\"Select Model\", \"\", InductionRatio($T46,BD46,$W46,$Y46)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T46=\"Select Model\", \"\",IF($T46=\"PCBL\",\"N/A\",minVAVSetBack(AA46, Y46))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T46=\"Select Model\", \"\",IF($T46= \"PCBL\",\"N/A\",getDischargeAirTemp($T46,$V46,$AC46,$W46,BD46,$AL46, $Y46, $AS46, \"cooling\",activeElevation,$AB46,$AJ46,$AV46,$BB46))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T46=\"Select Model\",$T46=\"PCBL\"), \"\",getDischargeAirTemp($T46,$V46,$AD46,$W46,BD46,$AL46, $Y46, $AY46, \"heating\",activeElevation,$AB46,$AJ46,$AV46,$BB46)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T46=\"Select Model\", \"\",IF(OR($T46=\"ACBC_1W\",$T46=\"ACBC_2W\",LEFT($T46,4)=\"ACBR\",$T46 = \"LIU24_2W\",LEFT($T46,3)=\"RIU\",LEFT($T46,6)=\"ACBL12\"), IF((soundLevel($T46, $AB46, BD46, $Y46, $W46,$AJ46,$AA46,\"dba\"))<15,\"<15\",soundLevel($T46, $AB46, BD46, $Y46, $W46,$AJ46,$AA46,\"dba\")+0.4),IF((soundLevel($T46, $AB46, BD46, $Y46, $W46,$AJ46,$AA46,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T46, $AB46, BD46, $Y46, $W46,$AJ46,$AA46,\"dba\")+5)<15, \"<15\", soundLevel($T46, $AB46, BD46,$Y46, $W46,$AJ46,$AA46,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T46=\"Select Model\", \"\",IF(OR($T46=\"ACBC_1W\",$T46=\"ACBC_2W\",LEFT($T46,4)=\"ACBR\",$T46=\"LIU24_2W\",LEFT($T46,3)=\"RIU\",LEFT($T46,6)=\"ACBL12\"), IF((soundLevel($T46, $AB46, BD46, $Y46, $W46,$AJ46,$AA46,\"NC\"))<15,\"<15\",soundLevel($T46, $AB46, BD46, $Y46, $W46,$AJ46,$AA46,\"NC\")+0.4),IF((soundLevel($T46, $AB46, BD46, $Y46, $W46,$AJ46,$AA46,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T46, $AB46, BD46, $Y46, $W46,$AJ46,$AA46,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T46, $AB46, BD46, $Y46, $W46,$AJ46,$AA46,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T46=\"Select Model\",\"\",IF($T46=\"LIU24_2W\",calcQwIP($Y46,$W46,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC46,$AI46,\"latent\",$U46&\"P\"&IF($V46=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T46,activeElevation),\"\"))","v":""},{"$f":"IF($T46=\"Select Model\",\"\",IF($T46=\"ACBC_1W\",calcQwIP($Y46,$W46,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC46,BD46,\"capacity\",$U46&\"P\"&IF($V46=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T46,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y46,$W46,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC46,BD46,\"capacity\",$U46&\"P\"&IF($V46=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T46,activeElevation)))","v":""},"",{"$f":"IF(T46=\"Select Model\", 0,waterPressureDrop(W46, U46 & \"P\" & IF(V46=\"Dual\",2,1) &\"C\", AC46, \"cooling\", T46))","v":0},{"$f":"IF(T46=\"Select Model\", \"\",getReturnWaterTemp(T46,AC46, activeEWTCooling, AS46, \"cooling\"))","v":""},"",{"$f":"IF($T46<>\"ACBC_1W\",\"\",IF($J46=\"\",\"\",FintubeCapacity($T46,$W46,$AE46,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T46=\"Select Model\",T46=\"PCBL\"),\"\",calcQwIP(Y46,W46,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD46,BD46,\"capacity\",U46&\"P\"&IF(V46=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T46,activeElevation))","v":""},"",{"$f":"IF(OR(T46=\"Select Model\",T46=\"PCBL\"), \"\",IF(AY46=0,\"N/A\",waterPressureDrop(W46, U46 & \"P\" & IF(V46=\"Dual\",2,1) &\"C\", AD46, \"heating\", T46)))","v":""},{"$f":"IF(OR(T46=\"Select Model\",T46=\"PCBL\"), \"\",IF(AY46=0,getReturnWaterTemp(T46,AE46, activeEWTHeating, AX46, \"heating\"),getReturnWaterTemp(T46,AD46, activeEWTHeating, AY46, \"heating\")))","v":""},"",{"$f":" getNozzle(T46, W46, Y46, Z46, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I47)),I47<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I47, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H47)),H47<0),\"\",intlEstQuantity(T47, W47*12, H47)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T47=\"Select Model\",\"\",coilCircuitChange(W47, U47, AC47, T47,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T47=\"Select Model\",\"\",beamWidth(T47))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T47=\"Select Model\",T47=\"PCBL\"), 0,getSPIP(T47, W47, Y47, BD47, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T47=\"Select Model\", \"\",IF(T47=\"PCBL\",0,primaryAirSensibleCapacityIP($T47,$W47,activeRoomTempCooling,activePriAirTempCooling,$Y47,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T47=\"Select Model\",\"\",IF($T47=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y47,activeElevation)))","v":""},{"$f":"IF(OR(T47=\"Select Model\",T47=\"PCBL\"), 0,IF(AD47=0,0,-primaryAirSensibleCapacityIP($T47,$W47,activeRoomTempHeating,activePriAirTempHeating,$Y47,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T47=\"Select Model\", \"\", InductionRatio($T47,BD47,$W47,$Y47)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T47=\"Select Model\", \"\",IF($T47=\"PCBL\",\"N/A\",minVAVSetBack(AA47, Y47))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T47=\"Select Model\", \"\",IF($T47= \"PCBL\",\"N/A\",getDischargeAirTemp($T47,$V47,$AC47,$W47,BD47,$AL47, $Y47, $AS47, \"cooling\",activeElevation,$AB47,$AJ47,$AV47,$BB47))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T47=\"Select Model\",$T47=\"PCBL\"), \"\",getDischargeAirTemp($T47,$V47,$AD47,$W47,BD47,$AL47, $Y47, $AY47, \"heating\",activeElevation,$AB47,$AJ47,$AV47,$BB47)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T47=\"Select Model\", \"\",IF(OR($T47=\"ACBC_1W\",$T47=\"ACBC_2W\",LEFT($T47,4)=\"ACBR\",$T47 = \"LIU24_2W\",LEFT($T47,3)=\"RIU\",LEFT($T47,6)=\"ACBL12\"), IF((soundLevel($T47, $AB47, BD47, $Y47, $W47,$AJ47,$AA47,\"dba\"))<15,\"<15\",soundLevel($T47, $AB47, BD47, $Y47, $W47,$AJ47,$AA47,\"dba\")+0.4),IF((soundLevel($T47, $AB47, BD47, $Y47, $W47,$AJ47,$AA47,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T47, $AB47, BD47, $Y47, $W47,$AJ47,$AA47,\"dba\")+5)<15, \"<15\", soundLevel($T47, $AB47, BD47,$Y47, $W47,$AJ47,$AA47,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T47=\"Select Model\", \"\",IF(OR($T47=\"ACBC_1W\",$T47=\"ACBC_2W\",LEFT($T47,4)=\"ACBR\",$T47=\"LIU24_2W\",LEFT($T47,3)=\"RIU\",LEFT($T47,6)=\"ACBL12\"), IF((soundLevel($T47, $AB47, BD47, $Y47, $W47,$AJ47,$AA47,\"NC\"))<15,\"<15\",soundLevel($T47, $AB47, BD47, $Y47, $W47,$AJ47,$AA47,\"NC\")+0.4),IF((soundLevel($T47, $AB47, BD47, $Y47, $W47,$AJ47,$AA47,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T47, $AB47, BD47, $Y47, $W47,$AJ47,$AA47,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T47, $AB47, BD47, $Y47, $W47,$AJ47,$AA47,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T47=\"Select Model\",\"\",IF($T47=\"LIU24_2W\",calcQwIP($Y47,$W47,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC47,$AI47,\"latent\",$U47&\"P\"&IF($V47=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T47,activeElevation),\"\"))","v":""},{"$f":"IF($T47=\"Select Model\",\"\",IF($T47=\"ACBC_1W\",calcQwIP($Y47,$W47,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC47,BD47,\"capacity\",$U47&\"P\"&IF($V47=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T47,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y47,$W47,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC47,BD47,\"capacity\",$U47&\"P\"&IF($V47=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T47,activeElevation)))","v":""},"",{"$f":"IF(T47=\"Select Model\", 0,waterPressureDrop(W47, U47 & \"P\" & IF(V47=\"Dual\",2,1) &\"C\", AC47, \"cooling\", T47))","v":0},{"$f":"IF(T47=\"Select Model\", \"\",getReturnWaterTemp(T47,AC47, activeEWTCooling, AS47, \"cooling\"))","v":""},"",{"$f":"IF($T47<>\"ACBC_1W\",\"\",IF($J47=\"\",\"\",FintubeCapacity($T47,$W47,$AE47,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T47=\"Select Model\",T47=\"PCBL\"),\"\",calcQwIP(Y47,W47,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD47,BD47,\"capacity\",U47&\"P\"&IF(V47=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T47,activeElevation))","v":""},"",{"$f":"IF(OR(T47=\"Select Model\",T47=\"PCBL\"), \"\",IF(AY47=0,\"N/A\",waterPressureDrop(W47, U47 & \"P\" & IF(V47=\"Dual\",2,1) &\"C\", AD47, \"heating\", T47)))","v":""},{"$f":"IF(OR(T47=\"Select Model\",T47=\"PCBL\"), \"\",IF(AY47=0,getReturnWaterTemp(T47,AE47, activeEWTHeating, AX47, \"heating\"),getReturnWaterTemp(T47,AD47, activeEWTHeating, AY47, \"heating\")))","v":""},"",{"$f":" getNozzle(T47, W47, Y47, Z47, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I48)),I48<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I48, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H48)),H48<0),\"\",intlEstQuantity(T48, W48*12, H48)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T48=\"Select Model\",\"\",coilCircuitChange(W48, U48, AC48, T48,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T48=\"Select Model\",\"\",beamWidth(T48))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T48=\"Select Model\",T48=\"PCBL\"), 0,getSPIP(T48, W48, Y48, BD48, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T48=\"Select Model\", \"\",IF(T48=\"PCBL\",0,primaryAirSensibleCapacityIP($T48,$W48,activeRoomTempCooling,activePriAirTempCooling,$Y48,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T48=\"Select Model\",\"\",IF($T48=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y48,activeElevation)))","v":""},{"$f":"IF(OR(T48=\"Select Model\",T48=\"PCBL\"), 0,IF(AD48=0,0,-primaryAirSensibleCapacityIP($T48,$W48,activeRoomTempHeating,activePriAirTempHeating,$Y48,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T48=\"Select Model\", \"\", InductionRatio($T48,BD48,$W48,$Y48)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T48=\"Select Model\", \"\",IF($T48=\"PCBL\",\"N/A\",minVAVSetBack(AA48, Y48))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T48=\"Select Model\", \"\",IF($T48= \"PCBL\",\"N/A\",getDischargeAirTemp($T48,$V48,$AC48,$W48,BD48,$AL48, $Y48, $AS48, \"cooling\",activeElevation,$AB48,$AJ48,$AV48,$BB48))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T48=\"Select Model\",$T48=\"PCBL\"), \"\",getDischargeAirTemp($T48,$V48,$AD48,$W48,BD48,$AL48, $Y48, $AY48, \"heating\",activeElevation,$AB48,$AJ48,$AV48,$BB48)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T48=\"Select Model\", \"\",IF(OR($T48=\"ACBC_1W\",$T48=\"ACBC_2W\",LEFT($T48,4)=\"ACBR\",$T48 = \"LIU24_2W\",LEFT($T48,3)=\"RIU\",LEFT($T48,6)=\"ACBL12\"), IF((soundLevel($T48, $AB48, BD48, $Y48, $W48,$AJ48,$AA48,\"dba\"))<15,\"<15\",soundLevel($T48, $AB48, BD48, $Y48, $W48,$AJ48,$AA48,\"dba\")+0.4),IF((soundLevel($T48, $AB48, BD48, $Y48, $W48,$AJ48,$AA48,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T48, $AB48, BD48, $Y48, $W48,$AJ48,$AA48,\"dba\")+5)<15, \"<15\", soundLevel($T48, $AB48, BD48,$Y48, $W48,$AJ48,$AA48,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T48=\"Select Model\", \"\",IF(OR($T48=\"ACBC_1W\",$T48=\"ACBC_2W\",LEFT($T48,4)=\"ACBR\",$T48=\"LIU24_2W\",LEFT($T48,3)=\"RIU\",LEFT($T48,6)=\"ACBL12\"), IF((soundLevel($T48, $AB48, BD48, $Y48, $W48,$AJ48,$AA48,\"NC\"))<15,\"<15\",soundLevel($T48, $AB48, BD48, $Y48, $W48,$AJ48,$AA48,\"NC\")+0.4),IF((soundLevel($T48, $AB48, BD48, $Y48, $W48,$AJ48,$AA48,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T48, $AB48, BD48, $Y48, $W48,$AJ48,$AA48,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T48, $AB48, BD48, $Y48, $W48,$AJ48,$AA48,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T48=\"Select Model\",\"\",IF($T48=\"LIU24_2W\",calcQwIP($Y48,$W48,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC48,$AI48,\"latent\",$U48&\"P\"&IF($V48=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T48,activeElevation),\"\"))","v":""},{"$f":"IF($T48=\"Select Model\",\"\",IF($T48=\"ACBC_1W\",calcQwIP($Y48,$W48,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC48,BD48,\"capacity\",$U48&\"P\"&IF($V48=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T48,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y48,$W48,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC48,BD48,\"capacity\",$U48&\"P\"&IF($V48=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T48,activeElevation)))","v":""},"",{"$f":"IF(T48=\"Select Model\", 0,waterPressureDrop(W48, U48 & \"P\" & IF(V48=\"Dual\",2,1) &\"C\", AC48, \"cooling\", T48))","v":0},{"$f":"IF(T48=\"Select Model\", \"\",getReturnWaterTemp(T48,AC48, activeEWTCooling, AS48, \"cooling\"))","v":""},"",{"$f":"IF($T48<>\"ACBC_1W\",\"\",IF($J48=\"\",\"\",FintubeCapacity($T48,$W48,$AE48,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T48=\"Select Model\",T48=\"PCBL\"),\"\",calcQwIP(Y48,W48,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD48,BD48,\"capacity\",U48&\"P\"&IF(V48=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T48,activeElevation))","v":""},"",{"$f":"IF(OR(T48=\"Select Model\",T48=\"PCBL\"), \"\",IF(AY48=0,\"N/A\",waterPressureDrop(W48, U48 & \"P\" & IF(V48=\"Dual\",2,1) &\"C\", AD48, \"heating\", T48)))","v":""},{"$f":"IF(OR(T48=\"Select Model\",T48=\"PCBL\"), \"\",IF(AY48=0,getReturnWaterTemp(T48,AE48, activeEWTHeating, AX48, \"heating\"),getReturnWaterTemp(T48,AD48, activeEWTHeating, AY48, \"heating\")))","v":""},"",{"$f":" getNozzle(T48, W48, Y48, Z48, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I49)),I49<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I49, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H49)),H49<0),\"\",intlEstQuantity(T49, W49*12, H49)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T49=\"Select Model\",\"\",coilCircuitChange(W49, U49, AC49, T49,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T49=\"Select Model\",\"\",beamWidth(T49))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T49=\"Select Model\",T49=\"PCBL\"), 0,getSPIP(T49, W49, Y49, BD49, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T49=\"Select Model\", \"\",IF(T49=\"PCBL\",0,primaryAirSensibleCapacityIP($T49,$W49,activeRoomTempCooling,activePriAirTempCooling,$Y49,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T49=\"Select Model\",\"\",IF($T49=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y49,activeElevation)))","v":""},{"$f":"IF(OR(T49=\"Select Model\",T49=\"PCBL\"), 0,IF(AD49=0,0,-primaryAirSensibleCapacityIP($T49,$W49,activeRoomTempHeating,activePriAirTempHeating,$Y49,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T49=\"Select Model\", \"\", InductionRatio($T49,BD49,$W49,$Y49)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T49=\"Select Model\", \"\",IF($T49=\"PCBL\",\"N/A\",minVAVSetBack(AA49, Y49))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T49=\"Select Model\", \"\",IF($T49= \"PCBL\",\"N/A\",getDischargeAirTemp($T49,$V49,$AC49,$W49,BD49,$AL49, $Y49, $AS49, \"cooling\",activeElevation,$AB49,$AJ49,$AV49,$BB49))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T49=\"Select Model\",$T49=\"PCBL\"), \"\",getDischargeAirTemp($T49,$V49,$AD49,$W49,BD49,$AL49, $Y49, $AY49, \"heating\",activeElevation,$AB49,$AJ49,$AV49,$BB49)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T49=\"Select Model\", \"\",IF(OR($T49=\"ACBC_1W\",$T49=\"ACBC_2W\",LEFT($T49,4)=\"ACBR\",$T49 = \"LIU24_2W\",LEFT($T49,3)=\"RIU\",LEFT($T49,6)=\"ACBL12\"), IF((soundLevel($T49, $AB49, BD49, $Y49, $W49,$AJ49,$AA49,\"dba\"))<15,\"<15\",soundLevel($T49, $AB49, BD49, $Y49, $W49,$AJ49,$AA49,\"dba\")+0.4),IF((soundLevel($T49, $AB49, BD49, $Y49, $W49,$AJ49,$AA49,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T49, $AB49, BD49, $Y49, $W49,$AJ49,$AA49,\"dba\")+5)<15, \"<15\", soundLevel($T49, $AB49, BD49,$Y49, $W49,$AJ49,$AA49,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T49=\"Select Model\", \"\",IF(OR($T49=\"ACBC_1W\",$T49=\"ACBC_2W\",LEFT($T49,4)=\"ACBR\",$T49=\"LIU24_2W\",LEFT($T49,3)=\"RIU\",LEFT($T49,6)=\"ACBL12\"), IF((soundLevel($T49, $AB49, BD49, $Y49, $W49,$AJ49,$AA49,\"NC\"))<15,\"<15\",soundLevel($T49, $AB49, BD49, $Y49, $W49,$AJ49,$AA49,\"NC\")+0.4),IF((soundLevel($T49, $AB49, BD49, $Y49, $W49,$AJ49,$AA49,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T49, $AB49, BD49, $Y49, $W49,$AJ49,$AA49,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T49, $AB49, BD49, $Y49, $W49,$AJ49,$AA49,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T49=\"Select Model\",\"\",IF($T49=\"LIU24_2W\",calcQwIP($Y49,$W49,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC49,$AI49,\"latent\",$U49&\"P\"&IF($V49=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T49,activeElevation),\"\"))","v":""},{"$f":"IF($T49=\"Select Model\",\"\",IF($T49=\"ACBC_1W\",calcQwIP($Y49,$W49,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC49,BD49,\"capacity\",$U49&\"P\"&IF($V49=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T49,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y49,$W49,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC49,BD49,\"capacity\",$U49&\"P\"&IF($V49=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T49,activeElevation)))","v":""},"",{"$f":"IF(T49=\"Select Model\", 0,waterPressureDrop(W49, U49 & \"P\" & IF(V49=\"Dual\",2,1) &\"C\", AC49, \"cooling\", T49))","v":0},{"$f":"IF(T49=\"Select Model\", \"\",getReturnWaterTemp(T49,AC49, activeEWTCooling, AS49, \"cooling\"))","v":""},"",{"$f":"IF($T49<>\"ACBC_1W\",\"\",IF($J49=\"\",\"\",FintubeCapacity($T49,$W49,$AE49,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T49=\"Select Model\",T49=\"PCBL\"),\"\",calcQwIP(Y49,W49,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD49,BD49,\"capacity\",U49&\"P\"&IF(V49=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T49,activeElevation))","v":""},"",{"$f":"IF(OR(T49=\"Select Model\",T49=\"PCBL\"), \"\",IF(AY49=0,\"N/A\",waterPressureDrop(W49, U49 & \"P\" & IF(V49=\"Dual\",2,1) &\"C\", AD49, \"heating\", T49)))","v":""},{"$f":"IF(OR(T49=\"Select Model\",T49=\"PCBL\"), \"\",IF(AY49=0,getReturnWaterTemp(T49,AE49, activeEWTHeating, AX49, \"heating\"),getReturnWaterTemp(T49,AD49, activeEWTHeating, AY49, \"heating\")))","v":""},"",{"$f":" getNozzle(T49, W49, Y49, Z49, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I50)),I50<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I50, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H50)),H50<0),\"\",intlEstQuantity(T50, W50*12, H50)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T50=\"Select Model\",\"\",coilCircuitChange(W50, U50, AC50, T50,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T50=\"Select Model\",\"\",beamWidth(T50))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T50=\"Select Model\",T50=\"PCBL\"), 0,getSPIP(T50, W50, Y50, BD50, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T50=\"Select Model\", \"\",IF(T50=\"PCBL\",0,primaryAirSensibleCapacityIP($T50,$W50,activeRoomTempCooling,activePriAirTempCooling,$Y50,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T50=\"Select Model\",\"\",IF($T50=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y50,activeElevation)))","v":""},{"$f":"IF(OR(T50=\"Select Model\",T50=\"PCBL\"), 0,IF(AD50=0,0,-primaryAirSensibleCapacityIP($T50,$W50,activeRoomTempHeating,activePriAirTempHeating,$Y50,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T50=\"Select Model\", \"\", InductionRatio($T50,BD50,$W50,$Y50)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T50=\"Select Model\", \"\",IF($T50=\"PCBL\",\"N/A\",minVAVSetBack(AA50, Y50))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T50=\"Select Model\", \"\",IF($T50= \"PCBL\",\"N/A\",getDischargeAirTemp($T50,$V50,$AC50,$W50,BD50,$AL50, $Y50, $AS50, \"cooling\",activeElevation,$AB50,$AJ50,$AV50,$BB50))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T50=\"Select Model\",$T50=\"PCBL\"), \"\",getDischargeAirTemp($T50,$V50,$AD50,$W50,BD50,$AL50, $Y50, $AY50, \"heating\",activeElevation,$AB50,$AJ50,$AV50,$BB50)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T50=\"Select Model\", \"\",IF(OR($T50=\"ACBC_1W\",$T50=\"ACBC_2W\",LEFT($T50,4)=\"ACBR\",$T50 = \"LIU24_2W\",LEFT($T50,3)=\"RIU\",LEFT($T50,6)=\"ACBL12\"), IF((soundLevel($T50, $AB50, BD50, $Y50, $W50,$AJ50,$AA50,\"dba\"))<15,\"<15\",soundLevel($T50, $AB50, BD50, $Y50, $W50,$AJ50,$AA50,\"dba\")+0.4),IF((soundLevel($T50, $AB50, BD50, $Y50, $W50,$AJ50,$AA50,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T50, $AB50, BD50, $Y50, $W50,$AJ50,$AA50,\"dba\")+5)<15, \"<15\", soundLevel($T50, $AB50, BD50,$Y50, $W50,$AJ50,$AA50,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T50=\"Select Model\", \"\",IF(OR($T50=\"ACBC_1W\",$T50=\"ACBC_2W\",LEFT($T50,4)=\"ACBR\",$T50=\"LIU24_2W\",LEFT($T50,3)=\"RIU\",LEFT($T50,6)=\"ACBL12\"), IF((soundLevel($T50, $AB50, BD50, $Y50, $W50,$AJ50,$AA50,\"NC\"))<15,\"<15\",soundLevel($T50, $AB50, BD50, $Y50, $W50,$AJ50,$AA50,\"NC\")+0.4),IF((soundLevel($T50, $AB50, BD50, $Y50, $W50,$AJ50,$AA50,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T50, $AB50, BD50, $Y50, $W50,$AJ50,$AA50,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T50, $AB50, BD50, $Y50, $W50,$AJ50,$AA50,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T50=\"Select Model\",\"\",IF($T50=\"LIU24_2W\",calcQwIP($Y50,$W50,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC50,$AI50,\"latent\",$U50&\"P\"&IF($V50=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T50,activeElevation),\"\"))","v":""},{"$f":"IF($T50=\"Select Model\",\"\",IF($T50=\"ACBC_1W\",calcQwIP($Y50,$W50,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC50,BD50,\"capacity\",$U50&\"P\"&IF($V50=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T50,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y50,$W50,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC50,BD50,\"capacity\",$U50&\"P\"&IF($V50=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T50,activeElevation)))","v":""},"",{"$f":"IF(T50=\"Select Model\", 0,waterPressureDrop(W50, U50 & \"P\" & IF(V50=\"Dual\",2,1) &\"C\", AC50, \"cooling\", T50))","v":0},{"$f":"IF(T50=\"Select Model\", \"\",getReturnWaterTemp(T50,AC50, activeEWTCooling, AS50, \"cooling\"))","v":""},"",{"$f":"IF($T50<>\"ACBC_1W\",\"\",IF($J50=\"\",\"\",FintubeCapacity($T50,$W50,$AE50,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T50=\"Select Model\",T50=\"PCBL\"),\"\",calcQwIP(Y50,W50,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD50,BD50,\"capacity\",U50&\"P\"&IF(V50=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T50,activeElevation))","v":""},"",{"$f":"IF(OR(T50=\"Select Model\",T50=\"PCBL\"), \"\",IF(AY50=0,\"N/A\",waterPressureDrop(W50, U50 & \"P\" & IF(V50=\"Dual\",2,1) &\"C\", AD50, \"heating\", T50)))","v":""},{"$f":"IF(OR(T50=\"Select Model\",T50=\"PCBL\"), \"\",IF(AY50=0,getReturnWaterTemp(T50,AE50, activeEWTHeating, AX50, \"heating\"),getReturnWaterTemp(T50,AD50, activeEWTHeating, AY50, \"heating\")))","v":""},"",{"$f":" getNozzle(T50, W50, Y50, Z50, activeElevation, TRUE)","v":0}]
["Notes:",null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I51)),I51<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I51, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H51)),H51<0),\"\",intlEstQuantity(T51, W51*12, H51)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T51=\"Select Model\",\"\",coilCircuitChange(W51, U51, AC51, T51,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T51=\"Select Model\",\"\",beamWidth(T51))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T51=\"Select Model\",T51=\"PCBL\"), 0,getSPIP(T51, W51, Y51, BD51, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T51=\"Select Model\", \"\",IF(T51=\"PCBL\",0,primaryAirSensibleCapacityIP($T51,$W51,activeRoomTempCooling,activePriAirTempCooling,$Y51,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T51=\"Select Model\",\"\",IF($T51=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y51,activeElevation)))","v":""},{"$f":"IF(OR(T51=\"Select Model\",T51=\"PCBL\"), 0,IF(AD51=0,0,-primaryAirSensibleCapacityIP($T51,$W51,activeRoomTempHeating,activePriAirTempHeating,$Y51,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T51=\"Select Model\", \"\", InductionRatio($T51,BD51,$W51,$Y51)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T51=\"Select Model\", \"\",IF($T51=\"PCBL\",\"N/A\",minVAVSetBack(AA51, Y51))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T51=\"Select Model\", \"\",IF($T51= \"PCBL\",\"N/A\",getDischargeAirTemp($T51,$V51,$AC51,$W51,BD51,$AL51, $Y51, $AS51, \"cooling\",activeElevation,$AB51,$AJ51,$AV51,$BB51))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T51=\"Select Model\",$T51=\"PCBL\"), \"\",getDischargeAirTemp($T51,$V51,$AD51,$W51,BD51,$AL51, $Y51, $AY51, \"heating\",activeElevation,$AB51,$AJ51,$AV51,$BB51)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T51=\"Select Model\", \"\",IF(OR($T51=\"ACBC_1W\",$T51=\"ACBC_2W\",LEFT($T51,4)=\"ACBR\",$T51 = \"LIU24_2W\",LEFT($T51,3)=\"RIU\",LEFT($T51,6)=\"ACBL12\"), IF((soundLevel($T51, $AB51, BD51, $Y51, $W51,$AJ51,$AA51,\"dba\"))<15,\"<15\",soundLevel($T51, $AB51, BD51, $Y51, $W51,$AJ51,$AA51,\"dba\")+0.4),IF((soundLevel($T51, $AB51, BD51, $Y51, $W51,$AJ51,$AA51,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T51, $AB51, BD51, $Y51, $W51,$AJ51,$AA51,\"dba\")+5)<15, \"<15\", soundLevel($T51, $AB51, BD51,$Y51, $W51,$AJ51,$AA51,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T51=\"Select Model\", \"\",IF(OR($T51=\"ACBC_1W\",$T51=\"ACBC_2W\",LEFT($T51,4)=\"ACBR\",$T51=\"LIU24_2W\",LEFT($T51,3)=\"RIU\",LEFT($T51,6)=\"ACBL12\"), IF((soundLevel($T51, $AB51, BD51, $Y51, $W51,$AJ51,$AA51,\"NC\"))<15,\"<15\",soundLevel($T51, $AB51, BD51, $Y51, $W51,$AJ51,$AA51,\"NC\")+0.4),IF((soundLevel($T51, $AB51, BD51, $Y51, $W51,$AJ51,$AA51,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T51, $AB51, BD51, $Y51, $W51,$AJ51,$AA51,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T51, $AB51, BD51, $Y51, $W51,$AJ51,$AA51,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T51=\"Select Model\",\"\",IF($T51=\"LIU24_2W\",calcQwIP($Y51,$W51,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC51,$AI51,\"latent\",$U51&\"P\"&IF($V51=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T51,activeElevation),\"\"))","v":""},{"$f":"IF($T51=\"Select Model\",\"\",IF($T51=\"ACBC_1W\",calcQwIP($Y51,$W51,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC51,BD51,\"capacity\",$U51&\"P\"&IF($V51=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T51,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y51,$W51,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC51,BD51,\"capacity\",$U51&\"P\"&IF($V51=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T51,activeElevation)))","v":""},"",{"$f":"IF(T51=\"Select Model\", 0,waterPressureDrop(W51, U51 & \"P\" & IF(V51=\"Dual\",2,1) &\"C\", AC51, \"cooling\", T51))","v":0},{"$f":"IF(T51=\"Select Model\", \"\",getReturnWaterTemp(T51,AC51, activeEWTCooling, AS51, \"cooling\"))","v":""},"",{"$f":"IF($T51<>\"ACBC_1W\",\"\",IF($J51=\"\",\"\",FintubeCapacity($T51,$W51,$AE51,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T51=\"Select Model\",T51=\"PCBL\"),\"\",calcQwIP(Y51,W51,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD51,BD51,\"capacity\",U51&\"P\"&IF(V51=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T51,activeElevation))","v":""},"",{"$f":"IF(OR(T51=\"Select Model\",T51=\"PCBL\"), \"\",IF(AY51=0,\"N/A\",waterPressureDrop(W51, U51 & \"P\" & IF(V51=\"Dual\",2,1) &\"C\", AD51, \"heating\", T51)))","v":""},{"$f":"IF(OR(T51=\"Select Model\",T51=\"PCBL\"), \"\",IF(AY51=0,getReturnWaterTemp(T51,AE51, activeEWTHeating, AX51, \"heating\"),getReturnWaterTemp(T51,AD51, activeEWTHeating, AY51, \"heating\")))","v":""},"",{"$f":" getNozzle(T51, W51, Y51, Z51, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I52)),I52<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I52, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H52)),H52<0),\"\",intlEstQuantity(T52, W52*12, H52)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T52=\"Select Model\",\"\",coilCircuitChange(W52, U52, AC52, T52,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T52=\"Select Model\",\"\",beamWidth(T52))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T52=\"Select Model\",T52=\"PCBL\"), 0,getSPIP(T52, W52, Y52, BD52, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T52=\"Select Model\", \"\",IF(T52=\"PCBL\",0,primaryAirSensibleCapacityIP($T52,$W52,activeRoomTempCooling,activePriAirTempCooling,$Y52,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T52=\"Select Model\",\"\",IF($T52=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y52,activeElevation)))","v":""},{"$f":"IF(OR(T52=\"Select Model\",T52=\"PCBL\"), 0,IF(AD52=0,0,-primaryAirSensibleCapacityIP($T52,$W52,activeRoomTempHeating,activePriAirTempHeating,$Y52,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T52=\"Select Model\", \"\", InductionRatio($T52,BD52,$W52,$Y52)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T52=\"Select Model\", \"\",IF($T52=\"PCBL\",\"N/A\",minVAVSetBack(AA52, Y52))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T52=\"Select Model\", \"\",IF($T52= \"PCBL\",\"N/A\",getDischargeAirTemp($T52,$V52,$AC52,$W52,BD52,$AL52, $Y52, $AS52, \"cooling\",activeElevation,$AB52,$AJ52,$AV52,$BB52))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T52=\"Select Model\",$T52=\"PCBL\"), \"\",getDischargeAirTemp($T52,$V52,$AD52,$W52,BD52,$AL52, $Y52, $AY52, \"heating\",activeElevation,$AB52,$AJ52,$AV52,$BB52)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T52=\"Select Model\", \"\",IF(OR($T52=\"ACBC_1W\",$T52=\"ACBC_2W\",LEFT($T52,4)=\"ACBR\",$T52 = \"LIU24_2W\",LEFT($T52,3)=\"RIU\",LEFT($T52,6)=\"ACBL12\"), IF((soundLevel($T52, $AB52, BD52, $Y52, $W52,$AJ52,$AA52,\"dba\"))<15,\"<15\",soundLevel($T52, $AB52, BD52, $Y52, $W52,$AJ52,$AA52,\"dba\")+0.4),IF((soundLevel($T52, $AB52, BD52, $Y52, $W52,$AJ52,$AA52,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T52, $AB52, BD52, $Y52, $W52,$AJ52,$AA52,\"dba\")+5)<15, \"<15\", soundLevel($T52, $AB52, BD52,$Y52, $W52,$AJ52,$AA52,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T52=\"Select Model\", \"\",IF(OR($T52=\"ACBC_1W\",$T52=\"ACBC_2W\",LEFT($T52,4)=\"ACBR\",$T52=\"LIU24_2W\",LEFT($T52,3)=\"RIU\",LEFT($T52,6)=\"ACBL12\"), IF((soundLevel($T52, $AB52, BD52, $Y52, $W52,$AJ52,$AA52,\"NC\"))<15,\"<15\",soundLevel($T52, $AB52, BD52, $Y52, $W52,$AJ52,$AA52,\"NC\")+0.4),IF((soundLevel($T52, $AB52, BD52, $Y52, $W52,$AJ52,$AA52,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T52, $AB52, BD52, $Y52, $W52,$AJ52,$AA52,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T52, $AB52, BD52, $Y52, $W52,$AJ52,$AA52,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T52=\"Select Model\",\"\",IF($T52=\"LIU24_2W\",calcQwIP($Y52,$W52,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC52,$AI52,\"latent\",$U52&\"P\"&IF($V52=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T52,activeElevation),\"\"))","v":""},{"$f":"IF($T52=\"Select Model\",\"\",IF($T52=\"ACBC_1W\",calcQwIP($Y52,$W52,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC52,BD52,\"capacity\",$U52&\"P\"&IF($V52=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T52,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y52,$W52,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC52,BD52,\"capacity\",$U52&\"P\"&IF($V52=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T52,activeElevation)))","v":""},"",{"$f":"IF(T52=\"Select Model\", 0,waterPressureDrop(W52, U52 & \"P\" & IF(V52=\"Dual\",2,1) &\"C\", AC52, \"cooling\", T52))","v":0},{"$f":"IF(T52=\"Select Model\", \"\",getReturnWaterTemp(T52,AC52, activeEWTCooling, AS52, \"cooling\"))","v":""},"",{"$f":"IF($T52<>\"ACBC_1W\",\"\",IF($J52=\"\",\"\",FintubeCapacity($T52,$W52,$AE52,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T52=\"Select Model\",T52=\"PCBL\"),\"\",calcQwIP(Y52,W52,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD52,BD52,\"capacity\",U52&\"P\"&IF(V52=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T52,activeElevation))","v":""},"",{"$f":"IF(OR(T52=\"Select Model\",T52=\"PCBL\"), \"\",IF(AY52=0,\"N/A\",waterPressureDrop(W52, U52 & \"P\" & IF(V52=\"Dual\",2,1) &\"C\", AD52, \"heating\", T52)))","v":""},{"$f":"IF(OR(T52=\"Select Model\",T52=\"PCBL\"), \"\",IF(AY52=0,getReturnWaterTemp(T52,AE52, activeEWTHeating, AX52, \"heating\"),getReturnWaterTemp(T52,AD52, activeEWTHeating, AY52, \"heating\")))","v":""},"",{"$f":" getNozzle(T52, W52, Y52, Z52, activeElevation, TRUE)","v":0}]
[{"$f":"\"- Green cells are inputs\"","v":"- Green cells are inputs"},null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I53)),I53<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I53, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H53)),H53<0),\"\",intlEstQuantity(T53, W53*12, H53)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T53=\"Select Model\",\"\",coilCircuitChange(W53, U53, AC53, T53,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T53=\"Select Model\",\"\",beamWidth(T53))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T53=\"Select Model\",T53=\"PCBL\"), 0,getSPIP(T53, W53, Y53, BD53, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T53=\"Select Model\", \"\",IF(T53=\"PCBL\",0,primaryAirSensibleCapacityIP($T53,$W53,activeRoomTempCooling,activePriAirTempCooling,$Y53,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T53=\"Select Model\",\"\",IF($T53=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y53,activeElevation)))","v":""},{"$f":"IF(OR(T53=\"Select Model\",T53=\"PCBL\"), 0,IF(AD53=0,0,-primaryAirSensibleCapacityIP($T53,$W53,activeRoomTempHeating,activePriAirTempHeating,$Y53,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T53=\"Select Model\", \"\", InductionRatio($T53,BD53,$W53,$Y53)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T53=\"Select Model\", \"\",IF($T53=\"PCBL\",\"N/A\",minVAVSetBack(AA53, Y53))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T53=\"Select Model\", \"\",IF($T53= \"PCBL\",\"N/A\",getDischargeAirTemp($T53,$V53,$AC53,$W53,BD53,$AL53, $Y53, $AS53, \"cooling\",activeElevation,$AB53,$AJ53,$AV53,$BB53))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T53=\"Select Model\",$T53=\"PCBL\"), \"\",getDischargeAirTemp($T53,$V53,$AD53,$W53,BD53,$AL53, $Y53, $AY53, \"heating\",activeElevation,$AB53,$AJ53,$AV53,$BB53)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T53=\"Select Model\", \"\",IF(OR($T53=\"ACBC_1W\",$T53=\"ACBC_2W\",LEFT($T53,4)=\"ACBR\",$T53 = \"LIU24_2W\",LEFT($T53,3)=\"RIU\",LEFT($T53,6)=\"ACBL12\"), IF((soundLevel($T53, $AB53, BD53, $Y53, $W53,$AJ53,$AA53,\"dba\"))<15,\"<15\",soundLevel($T53, $AB53, BD53, $Y53, $W53,$AJ53,$AA53,\"dba\")+0.4),IF((soundLevel($T53, $AB53, BD53, $Y53, $W53,$AJ53,$AA53,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T53, $AB53, BD53, $Y53, $W53,$AJ53,$AA53,\"dba\")+5)<15, \"<15\", soundLevel($T53, $AB53, BD53,$Y53, $W53,$AJ53,$AA53,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T53=\"Select Model\", \"\",IF(OR($T53=\"ACBC_1W\",$T53=\"ACBC_2W\",LEFT($T53,4)=\"ACBR\",$T53=\"LIU24_2W\",LEFT($T53,3)=\"RIU\",LEFT($T53,6)=\"ACBL12\"), IF((soundLevel($T53, $AB53, BD53, $Y53, $W53,$AJ53,$AA53,\"NC\"))<15,\"<15\",soundLevel($T53, $AB53, BD53, $Y53, $W53,$AJ53,$AA53,\"NC\")+0.4),IF((soundLevel($T53, $AB53, BD53, $Y53, $W53,$AJ53,$AA53,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T53, $AB53, BD53, $Y53, $W53,$AJ53,$AA53,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T53, $AB53, BD53, $Y53, $W53,$AJ53,$AA53,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T53=\"Select Model\",\"\",IF($T53=\"LIU24_2W\",calcQwIP($Y53,$W53,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC53,$AI53,\"latent\",$U53&\"P\"&IF($V53=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T53,activeElevation),\"\"))","v":""},{"$f":"IF($T53=\"Select Model\",\"\",IF($T53=\"ACBC_1W\",calcQwIP($Y53,$W53,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC53,BD53,\"capacity\",$U53&\"P\"&IF($V53=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T53,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y53,$W53,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC53,BD53,\"capacity\",$U53&\"P\"&IF($V53=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T53,activeElevation)))","v":""},"",{"$f":"IF(T53=\"Select Model\", 0,waterPressureDrop(W53, U53 & \"P\" & IF(V53=\"Dual\",2,1) &\"C\", AC53, \"cooling\", T53))","v":0},{"$f":"IF(T53=\"Select Model\", \"\",getReturnWaterTemp(T53,AC53, activeEWTCooling, AS53, \"cooling\"))","v":""},"",{"$f":"IF($T53<>\"ACBC_1W\",\"\",IF($J53=\"\",\"\",FintubeCapacity($T53,$W53,$AE53,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T53=\"Select Model\",T53=\"PCBL\"),\"\",calcQwIP(Y53,W53,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD53,BD53,\"capacity\",U53&\"P\"&IF(V53=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T53,activeElevation))","v":""},"",{"$f":"IF(OR(T53=\"Select Model\",T53=\"PCBL\"), \"\",IF(AY53=0,\"N/A\",waterPressureDrop(W53, U53 & \"P\" & IF(V53=\"Dual\",2,1) &\"C\", AD53, \"heating\", T53)))","v":""},{"$f":"IF(OR(T53=\"Select Model\",T53=\"PCBL\"), \"\",IF(AY53=0,getReturnWaterTemp(T53,AE53, activeEWTHeating, AX53, \"heating\"),getReturnWaterTemp(T53,AD53, activeEWTHeating, AY53, \"heating\")))","v":""},"",{"$f":" getNozzle(T53, W53, Y53, Z53, activeElevation, TRUE)","v":0}]
[{"$f":"\"- White cells are outputs\"","v":"- White cells are outputs"},null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I54)),I54<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I54, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H54)),H54<0),\"\",intlEstQuantity(T54, W54*12, H54)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T54=\"Select Model\",\"\",coilCircuitChange(W54, U54, AC54, T54,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T54=\"Select Model\",\"\",beamWidth(T54))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T54=\"Select Model\",T54=\"PCBL\"), 0,getSPIP(T54, W54, Y54, BD54, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T54=\"Select Model\", \"\",IF(T54=\"PCBL\",0,primaryAirSensibleCapacityIP($T54,$W54,activeRoomTempCooling,activePriAirTempCooling,$Y54,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T54=\"Select Model\",\"\",IF($T54=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y54,activeElevation)))","v":""},{"$f":"IF(OR(T54=\"Select Model\",T54=\"PCBL\"), 0,IF(AD54=0,0,-primaryAirSensibleCapacityIP($T54,$W54,activeRoomTempHeating,activePriAirTempHeating,$Y54,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T54=\"Select Model\", \"\", InductionRatio($T54,BD54,$W54,$Y54)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T54=\"Select Model\", \"\",IF($T54=\"PCBL\",\"N/A\",minVAVSetBack(AA54, Y54))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T54=\"Select Model\", \"\",IF($T54= \"PCBL\",\"N/A\",getDischargeAirTemp($T54,$V54,$AC54,$W54,BD54,$AL54, $Y54, $AS54, \"cooling\",activeElevation,$AB54,$AJ54,$AV54,$BB54))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T54=\"Select Model\",$T54=\"PCBL\"), \"\",getDischargeAirTemp($T54,$V54,$AD54,$W54,BD54,$AL54, $Y54, $AY54, \"heating\",activeElevation,$AB54,$AJ54,$AV54,$BB54)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T54=\"Select Model\", \"\",IF(OR($T54=\"ACBC_1W\",$T54=\"ACBC_2W\",LEFT($T54,4)=\"ACBR\",$T54 = \"LIU24_2W\",LEFT($T54,3)=\"RIU\",LEFT($T54,6)=\"ACBL12\"), IF((soundLevel($T54, $AB54, BD54, $Y54, $W54,$AJ54,$AA54,\"dba\"))<15,\"<15\",soundLevel($T54, $AB54, BD54, $Y54, $W54,$AJ54,$AA54,\"dba\")+0.4),IF((soundLevel($T54, $AB54, BD54, $Y54, $W54,$AJ54,$AA54,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T54, $AB54, BD54, $Y54, $W54,$AJ54,$AA54,\"dba\")+5)<15, \"<15\", soundLevel($T54, $AB54, BD54,$Y54, $W54,$AJ54,$AA54,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T54=\"Select Model\", \"\",IF(OR($T54=\"ACBC_1W\",$T54=\"ACBC_2W\",LEFT($T54,4)=\"ACBR\",$T54=\"LIU24_2W\",LEFT($T54,3)=\"RIU\",LEFT($T54,6)=\"ACBL12\"), IF((soundLevel($T54, $AB54, BD54, $Y54, $W54,$AJ54,$AA54,\"NC\"))<15,\"<15\",soundLevel($T54, $AB54, BD54, $Y54, $W54,$AJ54,$AA54,\"NC\")+0.4),IF((soundLevel($T54, $AB54, BD54, $Y54, $W54,$AJ54,$AA54,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T54, $AB54, BD54, $Y54, $W54,$AJ54,$AA54,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T54, $AB54, BD54, $Y54, $W54,$AJ54,$AA54,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T54=\"Select Model\",\"\",IF($T54=\"LIU24_2W\",calcQwIP($Y54,$W54,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC54,$AI54,\"latent\",$U54&\"P\"&IF($V54=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T54,activeElevation),\"\"))","v":""},{"$f":"IF($T54=\"Select Model\",\"\",IF($T54=\"ACBC_1W\",calcQwIP($Y54,$W54,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC54,BD54,\"capacity\",$U54&\"P\"&IF($V54=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T54,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y54,$W54,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC54,BD54,\"capacity\",$U54&\"P\"&IF($V54=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T54,activeElevation)))","v":""},"",{"$f":"IF(T54=\"Select Model\", 0,waterPressureDrop(W54, U54 & \"P\" & IF(V54=\"Dual\",2,1) &\"C\", AC54, \"cooling\", T54))","v":0},{"$f":"IF(T54=\"Select Model\", \"\",getReturnWaterTemp(T54,AC54, activeEWTCooling, AS54, \"cooling\"))","v":""},"",{"$f":"IF($T54<>\"ACBC_1W\",\"\",IF($J54=\"\",\"\",FintubeCapacity($T54,$W54,$AE54,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T54=\"Select Model\",T54=\"PCBL\"),\"\",calcQwIP(Y54,W54,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD54,BD54,\"capacity\",U54&\"P\"&IF(V54=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T54,activeElevation))","v":""},"",{"$f":"IF(OR(T54=\"Select Model\",T54=\"PCBL\"), \"\",IF(AY54=0,\"N/A\",waterPressureDrop(W54, U54 & \"P\" & IF(V54=\"Dual\",2,1) &\"C\", AD54, \"heating\", T54)))","v":""},{"$f":"IF(OR(T54=\"Select Model\",T54=\"PCBL\"), \"\",IF(AY54=0,getReturnWaterTemp(T54,AE54, activeEWTHeating, AX54, \"heating\"),getReturnWaterTemp(T54,AD54, activeEWTHeating, AY54, \"heating\")))","v":""},"",{"$f":" getNozzle(T54, W54, Y54, Z54, activeElevation, TRUE)","v":0}]
[{"$f":"\"- Values that turn blue are manual inputs\"","v":"- Values that turn blue are manual inputs"},null,null,1,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I55)),I55<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I55, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H55)),H55<0),\"\",intlEstQuantity(T55, W55*12, H55)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T55=\"Select Model\",\"\",coilCircuitChange(W55, U55, AC55, T55,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T55=\"Select Model\",\"\",beamWidth(T55))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T55=\"Select Model\",T55=\"PCBL\"), 0,getSPIP(T55, W55, Y55, BD55, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T55=\"Select Model\", \"\",IF(T55=\"PCBL\",0,primaryAirSensibleCapacityIP($T55,$W55,activeRoomTempCooling,activePriAirTempCooling,$Y55,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T55=\"Select Model\",\"\",IF($T55=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y55,activeElevation)))","v":""},{"$f":"IF(OR(T55=\"Select Model\",T55=\"PCBL\"), 0,IF(AD55=0,0,-primaryAirSensibleCapacityIP($T55,$W55,activeRoomTempHeating,activePriAirTempHeating,$Y55,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T55=\"Select Model\", \"\", InductionRatio($T55,BD55,$W55,$Y55)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T55=\"Select Model\", \"\",IF($T55=\"PCBL\",\"N/A\",minVAVSetBack(AA55, Y55))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T55=\"Select Model\", \"\",IF($T55= \"PCBL\",\"N/A\",getDischargeAirTemp($T55,$V55,$AC55,$W55,BD55,$AL55, $Y55, $AS55, \"cooling\",activeElevation,$AB55,$AJ55,$AV55,$BB55))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T55=\"Select Model\",$T55=\"PCBL\"), \"\",getDischargeAirTemp($T55,$V55,$AD55,$W55,BD55,$AL55, $Y55, $AY55, \"heating\",activeElevation,$AB55,$AJ55,$AV55,$BB55)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T55=\"Select Model\", \"\",IF(OR($T55=\"ACBC_1W\",$T55=\"ACBC_2W\",LEFT($T55,4)=\"ACBR\",$T55 = \"LIU24_2W\",LEFT($T55,3)=\"RIU\",LEFT($T55,6)=\"ACBL12\"), IF((soundLevel($T55, $AB55, BD55, $Y55, $W55,$AJ55,$AA55,\"dba\"))<15,\"<15\",soundLevel($T55, $AB55, BD55, $Y55, $W55,$AJ55,$AA55,\"dba\")+0.4),IF((soundLevel($T55, $AB55, BD55, $Y55, $W55,$AJ55,$AA55,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T55, $AB55, BD55, $Y55, $W55,$AJ55,$AA55,\"dba\")+5)<15, \"<15\", soundLevel($T55, $AB55, BD55,$Y55, $W55,$AJ55,$AA55,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T55=\"Select Model\", \"\",IF(OR($T55=\"ACBC_1W\",$T55=\"ACBC_2W\",LEFT($T55,4)=\"ACBR\",$T55=\"LIU24_2W\",LEFT($T55,3)=\"RIU\",LEFT($T55,6)=\"ACBL12\"), IF((soundLevel($T55, $AB55, BD55, $Y55, $W55,$AJ55,$AA55,\"NC\"))<15,\"<15\",soundLevel($T55, $AB55, BD55, $Y55, $W55,$AJ55,$AA55,\"NC\")+0.4),IF((soundLevel($T55, $AB55, BD55, $Y55, $W55,$AJ55,$AA55,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T55, $AB55, BD55, $Y55, $W55,$AJ55,$AA55,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T55, $AB55, BD55, $Y55, $W55,$AJ55,$AA55,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T55=\"Select Model\",\"\",IF($T55=\"LIU24_2W\",calcQwIP($Y55,$W55,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC55,$AI55,\"latent\",$U55&\"P\"&IF($V55=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T55,activeElevation),\"\"))","v":""},{"$f":"IF($T55=\"Select Model\",\"\",IF($T55=\"ACBC_1W\",calcQwIP($Y55,$W55,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC55,BD55,\"capacity\",$U55&\"P\"&IF($V55=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T55,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y55,$W55,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC55,BD55,\"capacity\",$U55&\"P\"&IF($V55=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T55,activeElevation)))","v":""},"",{"$f":"IF(T55=\"Select Model\", 0,waterPressureDrop(W55, U55 & \"P\" & IF(V55=\"Dual\",2,1) &\"C\", AC55, \"cooling\", T55))","v":0},{"$f":"IF(T55=\"Select Model\", \"\",getReturnWaterTemp(T55,AC55, activeEWTCooling, AS55, \"cooling\"))","v":""},"",{"$f":"IF($T55<>\"ACBC_1W\",\"\",IF($J55=\"\",\"\",FintubeCapacity($T55,$W55,$AE55,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T55=\"Select Model\",T55=\"PCBL\"),\"\",calcQwIP(Y55,W55,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD55,BD55,\"capacity\",U55&\"P\"&IF(V55=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T55,activeElevation))","v":""},"",{"$f":"IF(OR(T55=\"Select Model\",T55=\"PCBL\"), \"\",IF(AY55=0,\"N/A\",waterPressureDrop(W55, U55 & \"P\" & IF(V55=\"Dual\",2,1) &\"C\", AD55, \"heating\", T55)))","v":""},{"$f":"IF(OR(T55=\"Select Model\",T55=\"PCBL\"), \"\",IF(AY55=0,getReturnWaterTemp(T55,AE55, activeEWTHeating, AX55, \"heating\"),getReturnWaterTemp(T55,AD55, activeEWTHeating, AY55, \"heating\")))","v":""},"",{"$f":" getNozzle(T55, W55, Y55, Z55, activeElevation, TRUE)","v":0}]
[{"$f":"\"- Stratification credit is applied to ACBC_1W only\"","v":"- Stratification credit is applied to ACBC_1W only"},null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I56)),I56<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I56, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H56)),H56<0),\"\",intlEstQuantity(T56, W56*12, H56)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T56=\"Select Model\",\"\",coilCircuitChange(W56, U56, AC56, T56,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T56=\"Select Model\",\"\",beamWidth(T56))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T56=\"Select Model\",T56=\"PCBL\"), 0,getSPIP(T56, W56, Y56, BD56, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T56=\"Select Model\", \"\",IF(T56=\"PCBL\",0,primaryAirSensibleCapacityIP($T56,$W56,activeRoomTempCooling,activePriAirTempCooling,$Y56,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T56=\"Select Model\",\"\",IF($T56=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y56,activeElevation)))","v":""},{"$f":"IF(OR(T56=\"Select Model\",T56=\"PCBL\"), 0,IF(AD56=0,0,-primaryAirSensibleCapacityIP($T56,$W56,activeRoomTempHeating,activePriAirTempHeating,$Y56,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T56=\"Select Model\", \"\", InductionRatio($T56,BD56,$W56,$Y56)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T56=\"Select Model\", \"\",IF($T56=\"PCBL\",\"N/A\",minVAVSetBack(AA56, Y56))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T56=\"Select Model\", \"\",IF($T56= \"PCBL\",\"N/A\",getDischargeAirTemp($T56,$V56,$AC56,$W56,BD56,$AL56, $Y56, $AS56, \"cooling\",activeElevation,$AB56,$AJ56,$AV56,$BB56))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T56=\"Select Model\",$T56=\"PCBL\"), \"\",getDischargeAirTemp($T56,$V56,$AD56,$W56,BD56,$AL56, $Y56, $AY56, \"heating\",activeElevation,$AB56,$AJ56,$AV56,$BB56)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T56=\"Select Model\", \"\",IF(OR($T56=\"ACBC_1W\",$T56=\"ACBC_2W\",LEFT($T56,4)=\"ACBR\",$T56 = \"LIU24_2W\",LEFT($T56,3)=\"RIU\",LEFT($T56,6)=\"ACBL12\"), IF((soundLevel($T56, $AB56, BD56, $Y56, $W56,$AJ56,$AA56,\"dba\"))<15,\"<15\",soundLevel($T56, $AB56, BD56, $Y56, $W56,$AJ56,$AA56,\"dba\")+0.4),IF((soundLevel($T56, $AB56, BD56, $Y56, $W56,$AJ56,$AA56,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T56, $AB56, BD56, $Y56, $W56,$AJ56,$AA56,\"dba\")+5)<15, \"<15\", soundLevel($T56, $AB56, BD56,$Y56, $W56,$AJ56,$AA56,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T56=\"Select Model\", \"\",IF(OR($T56=\"ACBC_1W\",$T56=\"ACBC_2W\",LEFT($T56,4)=\"ACBR\",$T56=\"LIU24_2W\",LEFT($T56,3)=\"RIU\",LEFT($T56,6)=\"ACBL12\"), IF((soundLevel($T56, $AB56, BD56, $Y56, $W56,$AJ56,$AA56,\"NC\"))<15,\"<15\",soundLevel($T56, $AB56, BD56, $Y56, $W56,$AJ56,$AA56,\"NC\")+0.4),IF((soundLevel($T56, $AB56, BD56, $Y56, $W56,$AJ56,$AA56,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T56, $AB56, BD56, $Y56, $W56,$AJ56,$AA56,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T56, $AB56, BD56, $Y56, $W56,$AJ56,$AA56,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T56=\"Select Model\",\"\",IF($T56=\"LIU24_2W\",calcQwIP($Y56,$W56,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC56,$AI56,\"latent\",$U56&\"P\"&IF($V56=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T56,activeElevation),\"\"))","v":""},{"$f":"IF($T56=\"Select Model\",\"\",IF($T56=\"ACBC_1W\",calcQwIP($Y56,$W56,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC56,BD56,\"capacity\",$U56&\"P\"&IF($V56=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T56,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y56,$W56,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC56,BD56,\"capacity\",$U56&\"P\"&IF($V56=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T56,activeElevation)))","v":""},"",{"$f":"IF(T56=\"Select Model\", 0,waterPressureDrop(W56, U56 & \"P\" & IF(V56=\"Dual\",2,1) &\"C\", AC56, \"cooling\", T56))","v":0},{"$f":"IF(T56=\"Select Model\", \"\",getReturnWaterTemp(T56,AC56, activeEWTCooling, AS56, \"cooling\"))","v":""},"",{"$f":"IF($T56<>\"ACBC_1W\",\"\",IF($J56=\"\",\"\",FintubeCapacity($T56,$W56,$AE56,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T56=\"Select Model\",T56=\"PCBL\"),\"\",calcQwIP(Y56,W56,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD56,BD56,\"capacity\",U56&\"P\"&IF(V56=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T56,activeElevation))","v":""},"",{"$f":"IF(OR(T56=\"Select Model\",T56=\"PCBL\"), \"\",IF(AY56=0,\"N/A\",waterPressureDrop(W56, U56 & \"P\" & IF(V56=\"Dual\",2,1) &\"C\", AD56, \"heating\", T56)))","v":""},{"$f":"IF(OR(T56=\"Select Model\",T56=\"PCBL\"), \"\",IF(AY56=0,getReturnWaterTemp(T56,AE56, activeEWTHeating, AX56, \"heating\"),getReturnWaterTemp(T56,AD56, activeEWTHeating, AY56, \"heating\")))","v":""},"",{"$f":" getNozzle(T56, W56, Y56, Z56, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I57)),I57<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I57, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H57)),H57<0),\"\",intlEstQuantity(T57, W57*12, H57)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T57=\"Select Model\",\"\",coilCircuitChange(W57, U57, AC57, T57,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T57=\"Select Model\",\"\",beamWidth(T57))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T57=\"Select Model\",T57=\"PCBL\"), 0,getSPIP(T57, W57, Y57, BD57, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T57=\"Select Model\", \"\",IF(T57=\"PCBL\",0,primaryAirSensibleCapacityIP($T57,$W57,activeRoomTempCooling,activePriAirTempCooling,$Y57,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T57=\"Select Model\",\"\",IF($T57=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y57,activeElevation)))","v":""},{"$f":"IF(OR(T57=\"Select Model\",T57=\"PCBL\"), 0,IF(AD57=0,0,-primaryAirSensibleCapacityIP($T57,$W57,activeRoomTempHeating,activePriAirTempHeating,$Y57,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T57=\"Select Model\", \"\", InductionRatio($T57,BD57,$W57,$Y57)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T57=\"Select Model\", \"\",IF($T57=\"PCBL\",\"N/A\",minVAVSetBack(AA57, Y57))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T57=\"Select Model\", \"\",IF($T57= \"PCBL\",\"N/A\",getDischargeAirTemp($T57,$V57,$AC57,$W57,BD57,$AL57, $Y57, $AS57, \"cooling\",activeElevation,$AB57,$AJ57,$AV57,$BB57))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T57=\"Select Model\",$T57=\"PCBL\"), \"\",getDischargeAirTemp($T57,$V57,$AD57,$W57,BD57,$AL57, $Y57, $AY57, \"heating\",activeElevation,$AB57,$AJ57,$AV57,$BB57)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T57=\"Select Model\", \"\",IF(OR($T57=\"ACBC_1W\",$T57=\"ACBC_2W\",LEFT($T57,4)=\"ACBR\",$T57 = \"LIU24_2W\",LEFT($T57,3)=\"RIU\",LEFT($T57,6)=\"ACBL12\"), IF((soundLevel($T57, $AB57, BD57, $Y57, $W57,$AJ57,$AA57,\"dba\"))<15,\"<15\",soundLevel($T57, $AB57, BD57, $Y57, $W57,$AJ57,$AA57,\"dba\")+0.4),IF((soundLevel($T57, $AB57, BD57, $Y57, $W57,$AJ57,$AA57,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T57, $AB57, BD57, $Y57, $W57,$AJ57,$AA57,\"dba\")+5)<15, \"<15\", soundLevel($T57, $AB57, BD57,$Y57, $W57,$AJ57,$AA57,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T57=\"Select Model\", \"\",IF(OR($T57=\"ACBC_1W\",$T57=\"ACBC_2W\",LEFT($T57,4)=\"ACBR\",$T57=\"LIU24_2W\",LEFT($T57,3)=\"RIU\",LEFT($T57,6)=\"ACBL12\"), IF((soundLevel($T57, $AB57, BD57, $Y57, $W57,$AJ57,$AA57,\"NC\"))<15,\"<15\",soundLevel($T57, $AB57, BD57, $Y57, $W57,$AJ57,$AA57,\"NC\")+0.4),IF((soundLevel($T57, $AB57, BD57, $Y57, $W57,$AJ57,$AA57,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T57, $AB57, BD57, $Y57, $W57,$AJ57,$AA57,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T57, $AB57, BD57, $Y57, $W57,$AJ57,$AA57,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T57=\"Select Model\",\"\",IF($T57=\"LIU24_2W\",calcQwIP($Y57,$W57,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC57,$AI57,\"latent\",$U57&\"P\"&IF($V57=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T57,activeElevation),\"\"))","v":""},{"$f":"IF($T57=\"Select Model\",\"\",IF($T57=\"ACBC_1W\",calcQwIP($Y57,$W57,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC57,BD57,\"capacity\",$U57&\"P\"&IF($V57=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T57,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y57,$W57,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC57,BD57,\"capacity\",$U57&\"P\"&IF($V57=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T57,activeElevation)))","v":""},"",{"$f":"IF(T57=\"Select Model\", 0,waterPressureDrop(W57, U57 & \"P\" & IF(V57=\"Dual\",2,1) &\"C\", AC57, \"cooling\", T57))","v":0},{"$f":"IF(T57=\"Select Model\", \"\",getReturnWaterTemp(T57,AC57, activeEWTCooling, AS57, \"cooling\"))","v":""},"",{"$f":"IF($T57<>\"ACBC_1W\",\"\",IF($J57=\"\",\"\",FintubeCapacity($T57,$W57,$AE57,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T57=\"Select Model\",T57=\"PCBL\"),\"\",calcQwIP(Y57,W57,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD57,BD57,\"capacity\",U57&\"P\"&IF(V57=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T57,activeElevation))","v":""},"",{"$f":"IF(OR(T57=\"Select Model\",T57=\"PCBL\"), \"\",IF(AY57=0,\"N/A\",waterPressureDrop(W57, U57 & \"P\" & IF(V57=\"Dual\",2,1) &\"C\", AD57, \"heating\", T57)))","v":""},{"$f":"IF(OR(T57=\"Select Model\",T57=\"PCBL\"), \"\",IF(AY57=0,getReturnWaterTemp(T57,AE57, activeEWTHeating, AX57, \"heating\"),getReturnWaterTemp(T57,AD57, activeEWTHeating, AY57, \"heating\")))","v":""},"",{"$f":" getNozzle(T57, W57, Y57, Z57, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I58)),I58<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I58, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H58)),H58<0),\"\",intlEstQuantity(T58, W58*12, H58)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T58=\"Select Model\",\"\",coilCircuitChange(W58, U58, AC58, T58,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T58=\"Select Model\",\"\",beamWidth(T58))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T58=\"Select Model\",T58=\"PCBL\"), 0,getSPIP(T58, W58, Y58, BD58, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T58=\"Select Model\", \"\",IF(T58=\"PCBL\",0,primaryAirSensibleCapacityIP($T58,$W58,activeRoomTempCooling,activePriAirTempCooling,$Y58,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T58=\"Select Model\",\"\",IF($T58=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y58,activeElevation)))","v":""},{"$f":"IF(OR(T58=\"Select Model\",T58=\"PCBL\"), 0,IF(AD58=0,0,-primaryAirSensibleCapacityIP($T58,$W58,activeRoomTempHeating,activePriAirTempHeating,$Y58,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T58=\"Select Model\", \"\", InductionRatio($T58,BD58,$W58,$Y58)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T58=\"Select Model\", \"\",IF($T58=\"PCBL\",\"N/A\",minVAVSetBack(AA58, Y58))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T58=\"Select Model\", \"\",IF($T58= \"PCBL\",\"N/A\",getDischargeAirTemp($T58,$V58,$AC58,$W58,BD58,$AL58, $Y58, $AS58, \"cooling\",activeElevation,$AB58,$AJ58,$AV58,$BB58))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T58=\"Select Model\",$T58=\"PCBL\"), \"\",getDischargeAirTemp($T58,$V58,$AD58,$W58,BD58,$AL58, $Y58, $AY58, \"heating\",activeElevation,$AB58,$AJ58,$AV58,$BB58)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T58=\"Select Model\", \"\",IF(OR($T58=\"ACBC_1W\",$T58=\"ACBC_2W\",LEFT($T58,4)=\"ACBR\",$T58 = \"LIU24_2W\",LEFT($T58,3)=\"RIU\",LEFT($T58,6)=\"ACBL12\"), IF((soundLevel($T58, $AB58, BD58, $Y58, $W58,$AJ58,$AA58,\"dba\"))<15,\"<15\",soundLevel($T58, $AB58, BD58, $Y58, $W58,$AJ58,$AA58,\"dba\")+0.4),IF((soundLevel($T58, $AB58, BD58, $Y58, $W58,$AJ58,$AA58,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T58, $AB58, BD58, $Y58, $W58,$AJ58,$AA58,\"dba\")+5)<15, \"<15\", soundLevel($T58, $AB58, BD58,$Y58, $W58,$AJ58,$AA58,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T58=\"Select Model\", \"\",IF(OR($T58=\"ACBC_1W\",$T58=\"ACBC_2W\",LEFT($T58,4)=\"ACBR\",$T58=\"LIU24_2W\",LEFT($T58,3)=\"RIU\",LEFT($T58,6)=\"ACBL12\"), IF((soundLevel($T58, $AB58, BD58, $Y58, $W58,$AJ58,$AA58,\"NC\"))<15,\"<15\",soundLevel($T58, $AB58, BD58, $Y58, $W58,$AJ58,$AA58,\"NC\")+0.4),IF((soundLevel($T58, $AB58, BD58, $Y58, $W58,$AJ58,$AA58,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T58, $AB58, BD58, $Y58, $W58,$AJ58,$AA58,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T58, $AB58, BD58, $Y58, $W58,$AJ58,$AA58,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T58=\"Select Model\",\"\",IF($T58=\"LIU24_2W\",calcQwIP($Y58,$W58,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC58,$AI58,\"latent\",$U58&\"P\"&IF($V58=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T58,activeElevation),\"\"))","v":""},{"$f":"IF($T58=\"Select Model\",\"\",IF($T58=\"ACBC_1W\",calcQwIP($Y58,$W58,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC58,BD58,\"capacity\",$U58&\"P\"&IF($V58=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T58,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y58,$W58,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC58,BD58,\"capacity\",$U58&\"P\"&IF($V58=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T58,activeElevation)))","v":""},"",{"$f":"IF(T58=\"Select Model\", 0,waterPressureDrop(W58, U58 & \"P\" & IF(V58=\"Dual\",2,1) &\"C\", AC58, \"cooling\", T58))","v":0},{"$f":"IF(T58=\"Select Model\", \"\",getReturnWaterTemp(T58,AC58, activeEWTCooling, AS58, \"cooling\"))","v":""},"",{"$f":"IF($T58<>\"ACBC_1W\",\"\",IF($J58=\"\",\"\",FintubeCapacity($T58,$W58,$AE58,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T58=\"Select Model\",T58=\"PCBL\"),\"\",calcQwIP(Y58,W58,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD58,BD58,\"capacity\",U58&\"P\"&IF(V58=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T58,activeElevation))","v":""},"",{"$f":"IF(OR(T58=\"Select Model\",T58=\"PCBL\"), \"\",IF(AY58=0,\"N/A\",waterPressureDrop(W58, U58 & \"P\" & IF(V58=\"Dual\",2,1) &\"C\", AD58, \"heating\", T58)))","v":""},{"$f":"IF(OR(T58=\"Select Model\",T58=\"PCBL\"), \"\",IF(AY58=0,getReturnWaterTemp(T58,AE58, activeEWTHeating, AX58, \"heating\"),getReturnWaterTemp(T58,AD58, activeEWTHeating, AY58, \"heating\")))","v":""},"",{"$f":" getNozzle(T58, W58, Y58, Z58, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I59)),I59<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I59, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H59)),H59<0),\"\",intlEstQuantity(T59, W59*12, H59)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T59=\"Select Model\",\"\",coilCircuitChange(W59, U59, AC59, T59,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T59=\"Select Model\",\"\",beamWidth(T59))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T59=\"Select Model\",T59=\"PCBL\"), 0,getSPIP(T59, W59, Y59, BD59, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T59=\"Select Model\", \"\",IF(T59=\"PCBL\",0,primaryAirSensibleCapacityIP($T59,$W59,activeRoomTempCooling,activePriAirTempCooling,$Y59,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T59=\"Select Model\",\"\",IF($T59=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y59,activeElevation)))","v":""},{"$f":"IF(OR(T59=\"Select Model\",T59=\"PCBL\"), 0,IF(AD59=0,0,-primaryAirSensibleCapacityIP($T59,$W59,activeRoomTempHeating,activePriAirTempHeating,$Y59,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T59=\"Select Model\", \"\", InductionRatio($T59,BD59,$W59,$Y59)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T59=\"Select Model\", \"\",IF($T59=\"PCBL\",\"N/A\",minVAVSetBack(AA59, Y59))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T59=\"Select Model\", \"\",IF($T59= \"PCBL\",\"N/A\",getDischargeAirTemp($T59,$V59,$AC59,$W59,BD59,$AL59, $Y59, $AS59, \"cooling\",activeElevation,$AB59,$AJ59,$AV59,$BB59))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T59=\"Select Model\",$T59=\"PCBL\"), \"\",getDischargeAirTemp($T59,$V59,$AD59,$W59,BD59,$AL59, $Y59, $AY59, \"heating\",activeElevation,$AB59,$AJ59,$AV59,$BB59)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T59=\"Select Model\", \"\",IF(OR($T59=\"ACBC_1W\",$T59=\"ACBC_2W\",LEFT($T59,4)=\"ACBR\",$T59 = \"LIU24_2W\",LEFT($T59,3)=\"RIU\",LEFT($T59,6)=\"ACBL12\"), IF((soundLevel($T59, $AB59, BD59, $Y59, $W59,$AJ59,$AA59,\"dba\"))<15,\"<15\",soundLevel($T59, $AB59, BD59, $Y59, $W59,$AJ59,$AA59,\"dba\")+0.4),IF((soundLevel($T59, $AB59, BD59, $Y59, $W59,$AJ59,$AA59,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T59, $AB59, BD59, $Y59, $W59,$AJ59,$AA59,\"dba\")+5)<15, \"<15\", soundLevel($T59, $AB59, BD59,$Y59, $W59,$AJ59,$AA59,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T59=\"Select Model\", \"\",IF(OR($T59=\"ACBC_1W\",$T59=\"ACBC_2W\",LEFT($T59,4)=\"ACBR\",$T59=\"LIU24_2W\",LEFT($T59,3)=\"RIU\",LEFT($T59,6)=\"ACBL12\"), IF((soundLevel($T59, $AB59, BD59, $Y59, $W59,$AJ59,$AA59,\"NC\"))<15,\"<15\",soundLevel($T59, $AB59, BD59, $Y59, $W59,$AJ59,$AA59,\"NC\")+0.4),IF((soundLevel($T59, $AB59, BD59, $Y59, $W59,$AJ59,$AA59,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T59, $AB59, BD59, $Y59, $W59,$AJ59,$AA59,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T59, $AB59, BD59, $Y59, $W59,$AJ59,$AA59,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T59=\"Select Model\",\"\",IF($T59=\"LIU24_2W\",calcQwIP($Y59,$W59,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC59,$AI59,\"latent\",$U59&\"P\"&IF($V59=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T59,activeElevation),\"\"))","v":""},{"$f":"IF($T59=\"Select Model\",\"\",IF($T59=\"ACBC_1W\",calcQwIP($Y59,$W59,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC59,BD59,\"capacity\",$U59&\"P\"&IF($V59=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T59,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y59,$W59,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC59,BD59,\"capacity\",$U59&\"P\"&IF($V59=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T59,activeElevation)))","v":""},"",{"$f":"IF(T59=\"Select Model\", 0,waterPressureDrop(W59, U59 & \"P\" & IF(V59=\"Dual\",2,1) &\"C\", AC59, \"cooling\", T59))","v":0},{"$f":"IF(T59=\"Select Model\", \"\",getReturnWaterTemp(T59,AC59, activeEWTCooling, AS59, \"cooling\"))","v":""},"",{"$f":"IF($T59<>\"ACBC_1W\",\"\",IF($J59=\"\",\"\",FintubeCapacity($T59,$W59,$AE59,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T59=\"Select Model\",T59=\"PCBL\"),\"\",calcQwIP(Y59,W59,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD59,BD59,\"capacity\",U59&\"P\"&IF(V59=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T59,activeElevation))","v":""},"",{"$f":"IF(OR(T59=\"Select Model\",T59=\"PCBL\"), \"\",IF(AY59=0,\"N/A\",waterPressureDrop(W59, U59 & \"P\" & IF(V59=\"Dual\",2,1) &\"C\", AD59, \"heating\", T59)))","v":""},{"$f":"IF(OR(T59=\"Select Model\",T59=\"PCBL\"), \"\",IF(AY59=0,getReturnWaterTemp(T59,AE59, activeEWTHeating, AX59, \"heating\"),getReturnWaterTemp(T59,AD59, activeEWTHeating, AY59, \"heating\")))","v":""},"",{"$f":" getNozzle(T59, W59, Y59, Z59, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I60)),I60<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I60, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H60)),H60<0),\"\",intlEstQuantity(T60, W60*12, H60)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T60=\"Select Model\",\"\",coilCircuitChange(W60, U60, AC60, T60,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T60=\"Select Model\",\"\",beamWidth(T60))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T60=\"Select Model\",T60=\"PCBL\"), 0,getSPIP(T60, W60, Y60, BD60, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T60=\"Select Model\", \"\",IF(T60=\"PCBL\",0,primaryAirSensibleCapacityIP($T60,$W60,activeRoomTempCooling,activePriAirTempCooling,$Y60,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T60=\"Select Model\",\"\",IF($T60=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y60,activeElevation)))","v":""},{"$f":"IF(OR(T60=\"Select Model\",T60=\"PCBL\"), 0,IF(AD60=0,0,-primaryAirSensibleCapacityIP($T60,$W60,activeRoomTempHeating,activePriAirTempHeating,$Y60,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T60=\"Select Model\", \"\", InductionRatio($T60,BD60,$W60,$Y60)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T60=\"Select Model\", \"\",IF($T60=\"PCBL\",\"N/A\",minVAVSetBack(AA60, Y60))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T60=\"Select Model\", \"\",IF($T60= \"PCBL\",\"N/A\",getDischargeAirTemp($T60,$V60,$AC60,$W60,BD60,$AL60, $Y60, $AS60, \"cooling\",activeElevation,$AB60,$AJ60,$AV60,$BB60))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T60=\"Select Model\",$T60=\"PCBL\"), \"\",getDischargeAirTemp($T60,$V60,$AD60,$W60,BD60,$AL60, $Y60, $AY60, \"heating\",activeElevation,$AB60,$AJ60,$AV60,$BB60)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T60=\"Select Model\", \"\",IF(OR($T60=\"ACBC_1W\",$T60=\"ACBC_2W\",LEFT($T60,4)=\"ACBR\",$T60 = \"LIU24_2W\",LEFT($T60,3)=\"RIU\",LEFT($T60,6)=\"ACBL12\"), IF((soundLevel($T60, $AB60, BD60, $Y60, $W60,$AJ60,$AA60,\"dba\"))<15,\"<15\",soundLevel($T60, $AB60, BD60, $Y60, $W60,$AJ60,$AA60,\"dba\")+0.4),IF((soundLevel($T60, $AB60, BD60, $Y60, $W60,$AJ60,$AA60,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T60, $AB60, BD60, $Y60, $W60,$AJ60,$AA60,\"dba\")+5)<15, \"<15\", soundLevel($T60, $AB60, BD60,$Y60, $W60,$AJ60,$AA60,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T60=\"Select Model\", \"\",IF(OR($T60=\"ACBC_1W\",$T60=\"ACBC_2W\",LEFT($T60,4)=\"ACBR\",$T60=\"LIU24_2W\",LEFT($T60,3)=\"RIU\",LEFT($T60,6)=\"ACBL12\"), IF((soundLevel($T60, $AB60, BD60, $Y60, $W60,$AJ60,$AA60,\"NC\"))<15,\"<15\",soundLevel($T60, $AB60, BD60, $Y60, $W60,$AJ60,$AA60,\"NC\")+0.4),IF((soundLevel($T60, $AB60, BD60, $Y60, $W60,$AJ60,$AA60,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T60, $AB60, BD60, $Y60, $W60,$AJ60,$AA60,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T60, $AB60, BD60, $Y60, $W60,$AJ60,$AA60,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T60=\"Select Model\",\"\",IF($T60=\"LIU24_2W\",calcQwIP($Y60,$W60,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC60,$AI60,\"latent\",$U60&\"P\"&IF($V60=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T60,activeElevation),\"\"))","v":""},{"$f":"IF($T60=\"Select Model\",\"\",IF($T60=\"ACBC_1W\",calcQwIP($Y60,$W60,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC60,BD60,\"capacity\",$U60&\"P\"&IF($V60=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T60,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y60,$W60,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC60,BD60,\"capacity\",$U60&\"P\"&IF($V60=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T60,activeElevation)))","v":""},"",{"$f":"IF(T60=\"Select Model\", 0,waterPressureDrop(W60, U60 & \"P\" & IF(V60=\"Dual\",2,1) &\"C\", AC60, \"cooling\", T60))","v":0},{"$f":"IF(T60=\"Select Model\", \"\",getReturnWaterTemp(T60,AC60, activeEWTCooling, AS60, \"cooling\"))","v":""},"",{"$f":"IF($T60<>\"ACBC_1W\",\"\",IF($J60=\"\",\"\",FintubeCapacity($T60,$W60,$AE60,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T60=\"Select Model\",T60=\"PCBL\"),\"\",calcQwIP(Y60,W60,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD60,BD60,\"capacity\",U60&\"P\"&IF(V60=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T60,activeElevation))","v":""},"",{"$f":"IF(OR(T60=\"Select Model\",T60=\"PCBL\"), \"\",IF(AY60=0,\"N/A\",waterPressureDrop(W60, U60 & \"P\" & IF(V60=\"Dual\",2,1) &\"C\", AD60, \"heating\", T60)))","v":""},{"$f":"IF(OR(T60=\"Select Model\",T60=\"PCBL\"), \"\",IF(AY60=0,getReturnWaterTemp(T60,AE60, activeEWTHeating, AX60, \"heating\"),getReturnWaterTemp(T60,AD60, activeEWTHeating, AY60, \"heating\")))","v":""},"",{"$f":" getNozzle(T60, W60, Y60, Z60, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I61)),I61<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I61, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H61)),H61<0),\"\",intlEstQuantity(T61, W61*12, H61)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T61=\"Select Model\",\"\",coilCircuitChange(W61, U61, AC61, T61,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T61=\"Select Model\",\"\",beamWidth(T61))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T61=\"Select Model\",T61=\"PCBL\"), 0,getSPIP(T61, W61, Y61, BD61, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T61=\"Select Model\", \"\",IF(T61=\"PCBL\",0,primaryAirSensibleCapacityIP($T61,$W61,activeRoomTempCooling,activePriAirTempCooling,$Y61,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T61=\"Select Model\",\"\",IF($T61=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y61,activeElevation)))","v":""},{"$f":"IF(OR(T61=\"Select Model\",T61=\"PCBL\"), 0,IF(AD61=0,0,-primaryAirSensibleCapacityIP($T61,$W61,activeRoomTempHeating,activePriAirTempHeating,$Y61,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T61=\"Select Model\", \"\", InductionRatio($T61,BD61,$W61,$Y61)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T61=\"Select Model\", \"\",IF($T61=\"PCBL\",\"N/A\",minVAVSetBack(AA61, Y61))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T61=\"Select Model\", \"\",IF($T61= \"PCBL\",\"N/A\",getDischargeAirTemp($T61,$V61,$AC61,$W61,BD61,$AL61, $Y61, $AS61, \"cooling\",activeElevation,$AB61,$AJ61,$AV61,$BB61))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T61=\"Select Model\",$T61=\"PCBL\"), \"\",getDischargeAirTemp($T61,$V61,$AD61,$W61,BD61,$AL61, $Y61, $AY61, \"heating\",activeElevation,$AB61,$AJ61,$AV61,$BB61)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T61=\"Select Model\", \"\",IF(OR($T61=\"ACBC_1W\",$T61=\"ACBC_2W\",LEFT($T61,4)=\"ACBR\",$T61 = \"LIU24_2W\",LEFT($T61,3)=\"RIU\",LEFT($T61,6)=\"ACBL12\"), IF((soundLevel($T61, $AB61, BD61, $Y61, $W61,$AJ61,$AA61,\"dba\"))<15,\"<15\",soundLevel($T61, $AB61, BD61, $Y61, $W61,$AJ61,$AA61,\"dba\")+0.4),IF((soundLevel($T61, $AB61, BD61, $Y61, $W61,$AJ61,$AA61,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T61, $AB61, BD61, $Y61, $W61,$AJ61,$AA61,\"dba\")+5)<15, \"<15\", soundLevel($T61, $AB61, BD61,$Y61, $W61,$AJ61,$AA61,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T61=\"Select Model\", \"\",IF(OR($T61=\"ACBC_1W\",$T61=\"ACBC_2W\",LEFT($T61,4)=\"ACBR\",$T61=\"LIU24_2W\",LEFT($T61,3)=\"RIU\",LEFT($T61,6)=\"ACBL12\"), IF((soundLevel($T61, $AB61, BD61, $Y61, $W61,$AJ61,$AA61,\"NC\"))<15,\"<15\",soundLevel($T61, $AB61, BD61, $Y61, $W61,$AJ61,$AA61,\"NC\")+0.4),IF((soundLevel($T61, $AB61, BD61, $Y61, $W61,$AJ61,$AA61,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T61, $AB61, BD61, $Y61, $W61,$AJ61,$AA61,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T61, $AB61, BD61, $Y61, $W61,$AJ61,$AA61,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T61=\"Select Model\",\"\",IF($T61=\"LIU24_2W\",calcQwIP($Y61,$W61,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC61,$AI61,\"latent\",$U61&\"P\"&IF($V61=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T61,activeElevation),\"\"))","v":""},{"$f":"IF($T61=\"Select Model\",\"\",IF($T61=\"ACBC_1W\",calcQwIP($Y61,$W61,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC61,BD61,\"capacity\",$U61&\"P\"&IF($V61=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T61,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y61,$W61,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC61,BD61,\"capacity\",$U61&\"P\"&IF($V61=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T61,activeElevation)))","v":""},"",{"$f":"IF(T61=\"Select Model\", 0,waterPressureDrop(W61, U61 & \"P\" & IF(V61=\"Dual\",2,1) &\"C\", AC61, \"cooling\", T61))","v":0},{"$f":"IF(T61=\"Select Model\", \"\",getReturnWaterTemp(T61,AC61, activeEWTCooling, AS61, \"cooling\"))","v":""},"",{"$f":"IF($T61<>\"ACBC_1W\",\"\",IF($J61=\"\",\"\",FintubeCapacity($T61,$W61,$AE61,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T61=\"Select Model\",T61=\"PCBL\"),\"\",calcQwIP(Y61,W61,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD61,BD61,\"capacity\",U61&\"P\"&IF(V61=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T61,activeElevation))","v":""},"",{"$f":"IF(OR(T61=\"Select Model\",T61=\"PCBL\"), \"\",IF(AY61=0,\"N/A\",waterPressureDrop(W61, U61 & \"P\" & IF(V61=\"Dual\",2,1) &\"C\", AD61, \"heating\", T61)))","v":""},{"$f":"IF(OR(T61=\"Select Model\",T61=\"PCBL\"), \"\",IF(AY61=0,getReturnWaterTemp(T61,AE61, activeEWTHeating, AX61, \"heating\"),getReturnWaterTemp(T61,AD61, activeEWTHeating, AY61, \"heating\")))","v":""},"",{"$f":" getNozzle(T61, W61, Y61, Z61, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I62)),I62<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I62, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H62)),H62<0),\"\",intlEstQuantity(T62, W62*12, H62)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T62=\"Select Model\",\"\",coilCircuitChange(W62, U62, AC62, T62,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T62=\"Select Model\",\"\",beamWidth(T62))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T62=\"Select Model\",T62=\"PCBL\"), 0,getSPIP(T62, W62, Y62, BD62, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T62=\"Select Model\", \"\",IF(T62=\"PCBL\",0,primaryAirSensibleCapacityIP($T62,$W62,activeRoomTempCooling,activePriAirTempCooling,$Y62,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T62=\"Select Model\",\"\",IF($T62=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y62,activeElevation)))","v":""},{"$f":"IF(OR(T62=\"Select Model\",T62=\"PCBL\"), 0,IF(AD62=0,0,-primaryAirSensibleCapacityIP($T62,$W62,activeRoomTempHeating,activePriAirTempHeating,$Y62,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T62=\"Select Model\", \"\", InductionRatio($T62,BD62,$W62,$Y62)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T62=\"Select Model\", \"\",IF($T62=\"PCBL\",\"N/A\",minVAVSetBack(AA62, Y62))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T62=\"Select Model\", \"\",IF($T62= \"PCBL\",\"N/A\",getDischargeAirTemp($T62,$V62,$AC62,$W62,BD62,$AL62, $Y62, $AS62, \"cooling\",activeElevation,$AB62,$AJ62,$AV62,$BB62))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T62=\"Select Model\",$T62=\"PCBL\"), \"\",getDischargeAirTemp($T62,$V62,$AD62,$W62,BD62,$AL62, $Y62, $AY62, \"heating\",activeElevation,$AB62,$AJ62,$AV62,$BB62)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T62=\"Select Model\", \"\",IF(OR($T62=\"ACBC_1W\",$T62=\"ACBC_2W\",LEFT($T62,4)=\"ACBR\",$T62 = \"LIU24_2W\",LEFT($T62,3)=\"RIU\",LEFT($T62,6)=\"ACBL12\"), IF((soundLevel($T62, $AB62, BD62, $Y62, $W62,$AJ62,$AA62,\"dba\"))<15,\"<15\",soundLevel($T62, $AB62, BD62, $Y62, $W62,$AJ62,$AA62,\"dba\")+0.4),IF((soundLevel($T62, $AB62, BD62, $Y62, $W62,$AJ62,$AA62,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T62, $AB62, BD62, $Y62, $W62,$AJ62,$AA62,\"dba\")+5)<15, \"<15\", soundLevel($T62, $AB62, BD62,$Y62, $W62,$AJ62,$AA62,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T62=\"Select Model\", \"\",IF(OR($T62=\"ACBC_1W\",$T62=\"ACBC_2W\",LEFT($T62,4)=\"ACBR\",$T62=\"LIU24_2W\",LEFT($T62,3)=\"RIU\",LEFT($T62,6)=\"ACBL12\"), IF((soundLevel($T62, $AB62, BD62, $Y62, $W62,$AJ62,$AA62,\"NC\"))<15,\"<15\",soundLevel($T62, $AB62, BD62, $Y62, $W62,$AJ62,$AA62,\"NC\")+0.4),IF((soundLevel($T62, $AB62, BD62, $Y62, $W62,$AJ62,$AA62,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T62, $AB62, BD62, $Y62, $W62,$AJ62,$AA62,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T62, $AB62, BD62, $Y62, $W62,$AJ62,$AA62,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T62=\"Select Model\",\"\",IF($T62=\"LIU24_2W\",calcQwIP($Y62,$W62,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC62,$AI62,\"latent\",$U62&\"P\"&IF($V62=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T62,activeElevation),\"\"))","v":""},{"$f":"IF($T62=\"Select Model\",\"\",IF($T62=\"ACBC_1W\",calcQwIP($Y62,$W62,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC62,BD62,\"capacity\",$U62&\"P\"&IF($V62=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T62,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y62,$W62,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC62,BD62,\"capacity\",$U62&\"P\"&IF($V62=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T62,activeElevation)))","v":""},"",{"$f":"IF(T62=\"Select Model\", 0,waterPressureDrop(W62, U62 & \"P\" & IF(V62=\"Dual\",2,1) &\"C\", AC62, \"cooling\", T62))","v":0},{"$f":"IF(T62=\"Select Model\", \"\",getReturnWaterTemp(T62,AC62, activeEWTCooling, AS62, \"cooling\"))","v":""},"",{"$f":"IF($T62<>\"ACBC_1W\",\"\",IF($J62=\"\",\"\",FintubeCapacity($T62,$W62,$AE62,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T62=\"Select Model\",T62=\"PCBL\"),\"\",calcQwIP(Y62,W62,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD62,BD62,\"capacity\",U62&\"P\"&IF(V62=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T62,activeElevation))","v":""},"",{"$f":"IF(OR(T62=\"Select Model\",T62=\"PCBL\"), \"\",IF(AY62=0,\"N/A\",waterPressureDrop(W62, U62 & \"P\" & IF(V62=\"Dual\",2,1) &\"C\", AD62, \"heating\", T62)))","v":""},{"$f":"IF(OR(T62=\"Select Model\",T62=\"PCBL\"), \"\",IF(AY62=0,getReturnWaterTemp(T62,AE62, activeEWTHeating, AX62, \"heating\"),getReturnWaterTemp(T62,AD62, activeEWTHeating, AY62, \"heating\")))","v":""},"",{"$f":" getNozzle(T62, W62, Y62, Z62, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I63)),I63<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I63, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H63)),H63<0),\"\",intlEstQuantity(T63, W63*12, H63)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T63=\"Select Model\",\"\",coilCircuitChange(W63, U63, AC63, T63,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T63=\"Select Model\",\"\",beamWidth(T63))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T63=\"Select Model\",T63=\"PCBL\"), 0,getSPIP(T63, W63, Y63, BD63, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T63=\"Select Model\", \"\",IF(T63=\"PCBL\",0,primaryAirSensibleCapacityIP($T63,$W63,activeRoomTempCooling,activePriAirTempCooling,$Y63,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T63=\"Select Model\",\"\",IF($T63=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y63,activeElevation)))","v":""},{"$f":"IF(OR(T63=\"Select Model\",T63=\"PCBL\"), 0,IF(AD63=0,0,-primaryAirSensibleCapacityIP($T63,$W63,activeRoomTempHeating,activePriAirTempHeating,$Y63,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T63=\"Select Model\", \"\", InductionRatio($T63,BD63,$W63,$Y63)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T63=\"Select Model\", \"\",IF($T63=\"PCBL\",\"N/A\",minVAVSetBack(AA63, Y63))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T63=\"Select Model\", \"\",IF($T63= \"PCBL\",\"N/A\",getDischargeAirTemp($T63,$V63,$AC63,$W63,BD63,$AL63, $Y63, $AS63, \"cooling\",activeElevation,$AB63,$AJ63,$AV63,$BB63))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T63=\"Select Model\",$T63=\"PCBL\"), \"\",getDischargeAirTemp($T63,$V63,$AD63,$W63,BD63,$AL63, $Y63, $AY63, \"heating\",activeElevation,$AB63,$AJ63,$AV63,$BB63)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T63=\"Select Model\", \"\",IF(OR($T63=\"ACBC_1W\",$T63=\"ACBC_2W\",LEFT($T63,4)=\"ACBR\",$T63 = \"LIU24_2W\",LEFT($T63,3)=\"RIU\",LEFT($T63,6)=\"ACBL12\"), IF((soundLevel($T63, $AB63, BD63, $Y63, $W63,$AJ63,$AA63,\"dba\"))<15,\"<15\",soundLevel($T63, $AB63, BD63, $Y63, $W63,$AJ63,$AA63,\"dba\")+0.4),IF((soundLevel($T63, $AB63, BD63, $Y63, $W63,$AJ63,$AA63,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T63, $AB63, BD63, $Y63, $W63,$AJ63,$AA63,\"dba\")+5)<15, \"<15\", soundLevel($T63, $AB63, BD63,$Y63, $W63,$AJ63,$AA63,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T63=\"Select Model\", \"\",IF(OR($T63=\"ACBC_1W\",$T63=\"ACBC_2W\",LEFT($T63,4)=\"ACBR\",$T63=\"LIU24_2W\",LEFT($T63,3)=\"RIU\",LEFT($T63,6)=\"ACBL12\"), IF((soundLevel($T63, $AB63, BD63, $Y63, $W63,$AJ63,$AA63,\"NC\"))<15,\"<15\",soundLevel($T63, $AB63, BD63, $Y63, $W63,$AJ63,$AA63,\"NC\")+0.4),IF((soundLevel($T63, $AB63, BD63, $Y63, $W63,$AJ63,$AA63,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T63, $AB63, BD63, $Y63, $W63,$AJ63,$AA63,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T63, $AB63, BD63, $Y63, $W63,$AJ63,$AA63,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T63=\"Select Model\",\"\",IF($T63=\"LIU24_2W\",calcQwIP($Y63,$W63,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC63,$AI63,\"latent\",$U63&\"P\"&IF($V63=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T63,activeElevation),\"\"))","v":""},{"$f":"IF($T63=\"Select Model\",\"\",IF($T63=\"ACBC_1W\",calcQwIP($Y63,$W63,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC63,BD63,\"capacity\",$U63&\"P\"&IF($V63=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T63,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y63,$W63,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC63,BD63,\"capacity\",$U63&\"P\"&IF($V63=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T63,activeElevation)))","v":""},"",{"$f":"IF(T63=\"Select Model\", 0,waterPressureDrop(W63, U63 & \"P\" & IF(V63=\"Dual\",2,1) &\"C\", AC63, \"cooling\", T63))","v":0},{"$f":"IF(T63=\"Select Model\", \"\",getReturnWaterTemp(T63,AC63, activeEWTCooling, AS63, \"cooling\"))","v":""},"",{"$f":"IF($T63<>\"ACBC_1W\",\"\",IF($J63=\"\",\"\",FintubeCapacity($T63,$W63,$AE63,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T63=\"Select Model\",T63=\"PCBL\"),\"\",calcQwIP(Y63,W63,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD63,BD63,\"capacity\",U63&\"P\"&IF(V63=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T63,activeElevation))","v":""},"",{"$f":"IF(OR(T63=\"Select Model\",T63=\"PCBL\"), \"\",IF(AY63=0,\"N/A\",waterPressureDrop(W63, U63 & \"P\" & IF(V63=\"Dual\",2,1) &\"C\", AD63, \"heating\", T63)))","v":""},{"$f":"IF(OR(T63=\"Select Model\",T63=\"PCBL\"), \"\",IF(AY63=0,getReturnWaterTemp(T63,AE63, activeEWTHeating, AX63, \"heating\"),getReturnWaterTemp(T63,AD63, activeEWTHeating, AY63, \"heating\")))","v":""},"",{"$f":" getNozzle(T63, W63, Y63, Z63, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I64)),I64<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I64, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H64)),H64<0),\"\",intlEstQuantity(T64, W64*12, H64)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T64=\"Select Model\",\"\",coilCircuitChange(W64, U64, AC64, T64,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T64=\"Select Model\",\"\",beamWidth(T64))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T64=\"Select Model\",T64=\"PCBL\"), 0,getSPIP(T64, W64, Y64, BD64, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T64=\"Select Model\", \"\",IF(T64=\"PCBL\",0,primaryAirSensibleCapacityIP($T64,$W64,activeRoomTempCooling,activePriAirTempCooling,$Y64,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T64=\"Select Model\",\"\",IF($T64=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y64,activeElevation)))","v":""},{"$f":"IF(OR(T64=\"Select Model\",T64=\"PCBL\"), 0,IF(AD64=0,0,-primaryAirSensibleCapacityIP($T64,$W64,activeRoomTempHeating,activePriAirTempHeating,$Y64,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T64=\"Select Model\", \"\", InductionRatio($T64,BD64,$W64,$Y64)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T64=\"Select Model\", \"\",IF($T64=\"PCBL\",\"N/A\",minVAVSetBack(AA64, Y64))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T64=\"Select Model\", \"\",IF($T64= \"PCBL\",\"N/A\",getDischargeAirTemp($T64,$V64,$AC64,$W64,BD64,$AL64, $Y64, $AS64, \"cooling\",activeElevation,$AB64,$AJ64,$AV64,$BB64))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T64=\"Select Model\",$T64=\"PCBL\"), \"\",getDischargeAirTemp($T64,$V64,$AD64,$W64,BD64,$AL64, $Y64, $AY64, \"heating\",activeElevation,$AB64,$AJ64,$AV64,$BB64)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T64=\"Select Model\", \"\",IF(OR($T64=\"ACBC_1W\",$T64=\"ACBC_2W\",LEFT($T64,4)=\"ACBR\",$T64 = \"LIU24_2W\",LEFT($T64,3)=\"RIU\",LEFT($T64,6)=\"ACBL12\"), IF((soundLevel($T64, $AB64, BD64, $Y64, $W64,$AJ64,$AA64,\"dba\"))<15,\"<15\",soundLevel($T64, $AB64, BD64, $Y64, $W64,$AJ64,$AA64,\"dba\")+0.4),IF((soundLevel($T64, $AB64, BD64, $Y64, $W64,$AJ64,$AA64,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T64, $AB64, BD64, $Y64, $W64,$AJ64,$AA64,\"dba\")+5)<15, \"<15\", soundLevel($T64, $AB64, BD64,$Y64, $W64,$AJ64,$AA64,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T64=\"Select Model\", \"\",IF(OR($T64=\"ACBC_1W\",$T64=\"ACBC_2W\",LEFT($T64,4)=\"ACBR\",$T64=\"LIU24_2W\",LEFT($T64,3)=\"RIU\",LEFT($T64,6)=\"ACBL12\"), IF((soundLevel($T64, $AB64, BD64, $Y64, $W64,$AJ64,$AA64,\"NC\"))<15,\"<15\",soundLevel($T64, $AB64, BD64, $Y64, $W64,$AJ64,$AA64,\"NC\")+0.4),IF((soundLevel($T64, $AB64, BD64, $Y64, $W64,$AJ64,$AA64,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T64, $AB64, BD64, $Y64, $W64,$AJ64,$AA64,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T64, $AB64, BD64, $Y64, $W64,$AJ64,$AA64,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T64=\"Select Model\",\"\",IF($T64=\"LIU24_2W\",calcQwIP($Y64,$W64,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC64,$AI64,\"latent\",$U64&\"P\"&IF($V64=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T64,activeElevation),\"\"))","v":""},{"$f":"IF($T64=\"Select Model\",\"\",IF($T64=\"ACBC_1W\",calcQwIP($Y64,$W64,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC64,BD64,\"capacity\",$U64&\"P\"&IF($V64=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T64,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y64,$W64,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC64,BD64,\"capacity\",$U64&\"P\"&IF($V64=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T64,activeElevation)))","v":""},"",{"$f":"IF(T64=\"Select Model\", 0,waterPressureDrop(W64, U64 & \"P\" & IF(V64=\"Dual\",2,1) &\"C\", AC64, \"cooling\", T64))","v":0},{"$f":"IF(T64=\"Select Model\", \"\",getReturnWaterTemp(T64,AC64, activeEWTCooling, AS64, \"cooling\"))","v":""},"",{"$f":"IF($T64<>\"ACBC_1W\",\"\",IF($J64=\"\",\"\",FintubeCapacity($T64,$W64,$AE64,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T64=\"Select Model\",T64=\"PCBL\"),\"\",calcQwIP(Y64,W64,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD64,BD64,\"capacity\",U64&\"P\"&IF(V64=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T64,activeElevation))","v":""},"",{"$f":"IF(OR(T64=\"Select Model\",T64=\"PCBL\"), \"\",IF(AY64=0,\"N/A\",waterPressureDrop(W64, U64 & \"P\" & IF(V64=\"Dual\",2,1) &\"C\", AD64, \"heating\", T64)))","v":""},{"$f":"IF(OR(T64=\"Select Model\",T64=\"PCBL\"), \"\",IF(AY64=0,getReturnWaterTemp(T64,AE64, activeEWTHeating, AX64, \"heating\"),getReturnWaterTemp(T64,AD64, activeEWTHeating, AY64, \"heating\")))","v":""},"",{"$f":" getNozzle(T64, W64, Y64, Z64, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I65)),I65<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I65, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H65)),H65<0),\"\",intlEstQuantity(T65, W65*12, H65)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T65=\"Select Model\",\"\",coilCircuitChange(W65, U65, AC65, T65,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T65=\"Select Model\",\"\",beamWidth(T65))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T65=\"Select Model\",T65=\"PCBL\"), 0,getSPIP(T65, W65, Y65, BD65, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T65=\"Select Model\", \"\",IF(T65=\"PCBL\",0,primaryAirSensibleCapacityIP($T65,$W65,activeRoomTempCooling,activePriAirTempCooling,$Y65,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T65=\"Select Model\",\"\",IF($T65=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y65,activeElevation)))","v":""},{"$f":"IF(OR(T65=\"Select Model\",T65=\"PCBL\"), 0,IF(AD65=0,0,-primaryAirSensibleCapacityIP($T65,$W65,activeRoomTempHeating,activePriAirTempHeating,$Y65,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T65=\"Select Model\", \"\", InductionRatio($T65,BD65,$W65,$Y65)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T65=\"Select Model\", \"\",IF($T65=\"PCBL\",\"N/A\",minVAVSetBack(AA65, Y65))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T65=\"Select Model\", \"\",IF($T65= \"PCBL\",\"N/A\",getDischargeAirTemp($T65,$V65,$AC65,$W65,BD65,$AL65, $Y65, $AS65, \"cooling\",activeElevation,$AB65,$AJ65,$AV65,$BB65))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T65=\"Select Model\",$T65=\"PCBL\"), \"\",getDischargeAirTemp($T65,$V65,$AD65,$W65,BD65,$AL65, $Y65, $AY65, \"heating\",activeElevation,$AB65,$AJ65,$AV65,$BB65)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T65=\"Select Model\", \"\",IF(OR($T65=\"ACBC_1W\",$T65=\"ACBC_2W\",LEFT($T65,4)=\"ACBR\",$T65 = \"LIU24_2W\",LEFT($T65,3)=\"RIU\",LEFT($T65,6)=\"ACBL12\"), IF((soundLevel($T65, $AB65, BD65, $Y65, $W65,$AJ65,$AA65,\"dba\"))<15,\"<15\",soundLevel($T65, $AB65, BD65, $Y65, $W65,$AJ65,$AA65,\"dba\")+0.4),IF((soundLevel($T65, $AB65, BD65, $Y65, $W65,$AJ65,$AA65,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T65, $AB65, BD65, $Y65, $W65,$AJ65,$AA65,\"dba\")+5)<15, \"<15\", soundLevel($T65, $AB65, BD65,$Y65, $W65,$AJ65,$AA65,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T65=\"Select Model\", \"\",IF(OR($T65=\"ACBC_1W\",$T65=\"ACBC_2W\",LEFT($T65,4)=\"ACBR\",$T65=\"LIU24_2W\",LEFT($T65,3)=\"RIU\",LEFT($T65,6)=\"ACBL12\"), IF((soundLevel($T65, $AB65, BD65, $Y65, $W65,$AJ65,$AA65,\"NC\"))<15,\"<15\",soundLevel($T65, $AB65, BD65, $Y65, $W65,$AJ65,$AA65,\"NC\")+0.4),IF((soundLevel($T65, $AB65, BD65, $Y65, $W65,$AJ65,$AA65,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T65, $AB65, BD65, $Y65, $W65,$AJ65,$AA65,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T65, $AB65, BD65, $Y65, $W65,$AJ65,$AA65,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T65=\"Select Model\",\"\",IF($T65=\"LIU24_2W\",calcQwIP($Y65,$W65,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC65,$AI65,\"latent\",$U65&\"P\"&IF($V65=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T65,activeElevation),\"\"))","v":""},{"$f":"IF($T65=\"Select Model\",\"\",IF($T65=\"ACBC_1W\",calcQwIP($Y65,$W65,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC65,BD65,\"capacity\",$U65&\"P\"&IF($V65=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T65,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y65,$W65,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC65,BD65,\"capacity\",$U65&\"P\"&IF($V65=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T65,activeElevation)))","v":""},"",{"$f":"IF(T65=\"Select Model\", 0,waterPressureDrop(W65, U65 & \"P\" & IF(V65=\"Dual\",2,1) &\"C\", AC65, \"cooling\", T65))","v":0},{"$f":"IF(T65=\"Select Model\", \"\",getReturnWaterTemp(T65,AC65, activeEWTCooling, AS65, \"cooling\"))","v":""},"",{"$f":"IF($T65<>\"ACBC_1W\",\"\",IF($J65=\"\",\"\",FintubeCapacity($T65,$W65,$AE65,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T65=\"Select Model\",T65=\"PCBL\"),\"\",calcQwIP(Y65,W65,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD65,BD65,\"capacity\",U65&\"P\"&IF(V65=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T65,activeElevation))","v":""},"",{"$f":"IF(OR(T65=\"Select Model\",T65=\"PCBL\"), \"\",IF(AY65=0,\"N/A\",waterPressureDrop(W65, U65 & \"P\" & IF(V65=\"Dual\",2,1) &\"C\", AD65, \"heating\", T65)))","v":""},{"$f":"IF(OR(T65=\"Select Model\",T65=\"PCBL\"), \"\",IF(AY65=0,getReturnWaterTemp(T65,AE65, activeEWTHeating, AX65, \"heating\"),getReturnWaterTemp(T65,AD65, activeEWTHeating, AY65, \"heating\")))","v":""},"",{"$f":" getNozzle(T65, W65, Y65, Z65, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I66)),I66<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I66, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H66)),H66<0),\"\",intlEstQuantity(T66, W66*12, H66)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T66=\"Select Model\",\"\",coilCircuitChange(W66, U66, AC66, T66,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T66=\"Select Model\",\"\",beamWidth(T66))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T66=\"Select Model\",T66=\"PCBL\"), 0,getSPIP(T66, W66, Y66, BD66, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T66=\"Select Model\", \"\",IF(T66=\"PCBL\",0,primaryAirSensibleCapacityIP($T66,$W66,activeRoomTempCooling,activePriAirTempCooling,$Y66,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T66=\"Select Model\",\"\",IF($T66=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y66,activeElevation)))","v":""},{"$f":"IF(OR(T66=\"Select Model\",T66=\"PCBL\"), 0,IF(AD66=0,0,-primaryAirSensibleCapacityIP($T66,$W66,activeRoomTempHeating,activePriAirTempHeating,$Y66,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T66=\"Select Model\", \"\", InductionRatio($T66,BD66,$W66,$Y66)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T66=\"Select Model\", \"\",IF($T66=\"PCBL\",\"N/A\",minVAVSetBack(AA66, Y66))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T66=\"Select Model\", \"\",IF($T66= \"PCBL\",\"N/A\",getDischargeAirTemp($T66,$V66,$AC66,$W66,BD66,$AL66, $Y66, $AS66, \"cooling\",activeElevation,$AB66,$AJ66,$AV66,$BB66))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T66=\"Select Model\",$T66=\"PCBL\"), \"\",getDischargeAirTemp($T66,$V66,$AD66,$W66,BD66,$AL66, $Y66, $AY66, \"heating\",activeElevation,$AB66,$AJ66,$AV66,$BB66)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T66=\"Select Model\", \"\",IF(OR($T66=\"ACBC_1W\",$T66=\"ACBC_2W\",LEFT($T66,4)=\"ACBR\",$T66 = \"LIU24_2W\",LEFT($T66,3)=\"RIU\",LEFT($T66,6)=\"ACBL12\"), IF((soundLevel($T66, $AB66, BD66, $Y66, $W66,$AJ66,$AA66,\"dba\"))<15,\"<15\",soundLevel($T66, $AB66, BD66, $Y66, $W66,$AJ66,$AA66,\"dba\")+0.4),IF((soundLevel($T66, $AB66, BD66, $Y66, $W66,$AJ66,$AA66,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T66, $AB66, BD66, $Y66, $W66,$AJ66,$AA66,\"dba\")+5)<15, \"<15\", soundLevel($T66, $AB66, BD66,$Y66, $W66,$AJ66,$AA66,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T66=\"Select Model\", \"\",IF(OR($T66=\"ACBC_1W\",$T66=\"ACBC_2W\",LEFT($T66,4)=\"ACBR\",$T66=\"LIU24_2W\",LEFT($T66,3)=\"RIU\",LEFT($T66,6)=\"ACBL12\"), IF((soundLevel($T66, $AB66, BD66, $Y66, $W66,$AJ66,$AA66,\"NC\"))<15,\"<15\",soundLevel($T66, $AB66, BD66, $Y66, $W66,$AJ66,$AA66,\"NC\")+0.4),IF((soundLevel($T66, $AB66, BD66, $Y66, $W66,$AJ66,$AA66,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T66, $AB66, BD66, $Y66, $W66,$AJ66,$AA66,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T66, $AB66, BD66, $Y66, $W66,$AJ66,$AA66,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T66=\"Select Model\",\"\",IF($T66=\"LIU24_2W\",calcQwIP($Y66,$W66,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC66,$AI66,\"latent\",$U66&\"P\"&IF($V66=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T66,activeElevation),\"\"))","v":""},{"$f":"IF($T66=\"Select Model\",\"\",IF($T66=\"ACBC_1W\",calcQwIP($Y66,$W66,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC66,BD66,\"capacity\",$U66&\"P\"&IF($V66=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T66,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y66,$W66,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC66,BD66,\"capacity\",$U66&\"P\"&IF($V66=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T66,activeElevation)))","v":""},"",{"$f":"IF(T66=\"Select Model\", 0,waterPressureDrop(W66, U66 & \"P\" & IF(V66=\"Dual\",2,1) &\"C\", AC66, \"cooling\", T66))","v":0},{"$f":"IF(T66=\"Select Model\", \"\",getReturnWaterTemp(T66,AC66, activeEWTCooling, AS66, \"cooling\"))","v":""},"",{"$f":"IF($T66<>\"ACBC_1W\",\"\",IF($J66=\"\",\"\",FintubeCapacity($T66,$W66,$AE66,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T66=\"Select Model\",T66=\"PCBL\"),\"\",calcQwIP(Y66,W66,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD66,BD66,\"capacity\",U66&\"P\"&IF(V66=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T66,activeElevation))","v":""},"",{"$f":"IF(OR(T66=\"Select Model\",T66=\"PCBL\"), \"\",IF(AY66=0,\"N/A\",waterPressureDrop(W66, U66 & \"P\" & IF(V66=\"Dual\",2,1) &\"C\", AD66, \"heating\", T66)))","v":""},{"$f":"IF(OR(T66=\"Select Model\",T66=\"PCBL\"), \"\",IF(AY66=0,getReturnWaterTemp(T66,AE66, activeEWTHeating, AX66, \"heating\"),getReturnWaterTemp(T66,AD66, activeEWTHeating, AY66, \"heating\")))","v":""},"",{"$f":" getNozzle(T66, W66, Y66, Z66, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I67)),I67<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I67, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H67)),H67<0),\"\",intlEstQuantity(T67, W67*12, H67)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T67=\"Select Model\",\"\",coilCircuitChange(W67, U67, AC67, T67,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T67=\"Select Model\",\"\",beamWidth(T67))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T67=\"Select Model\",T67=\"PCBL\"), 0,getSPIP(T67, W67, Y67, BD67, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T67=\"Select Model\", \"\",IF(T67=\"PCBL\",0,primaryAirSensibleCapacityIP($T67,$W67,activeRoomTempCooling,activePriAirTempCooling,$Y67,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T67=\"Select Model\",\"\",IF($T67=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y67,activeElevation)))","v":""},{"$f":"IF(OR(T67=\"Select Model\",T67=\"PCBL\"), 0,IF(AD67=0,0,-primaryAirSensibleCapacityIP($T67,$W67,activeRoomTempHeating,activePriAirTempHeating,$Y67,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T67=\"Select Model\", \"\", InductionRatio($T67,BD67,$W67,$Y67)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T67=\"Select Model\", \"\",IF($T67=\"PCBL\",\"N/A\",minVAVSetBack(AA67, Y67))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T67=\"Select Model\", \"\",IF($T67= \"PCBL\",\"N/A\",getDischargeAirTemp($T67,$V67,$AC67,$W67,BD67,$AL67, $Y67, $AS67, \"cooling\",activeElevation,$AB67,$AJ67,$AV67,$BB67))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T67=\"Select Model\",$T67=\"PCBL\"), \"\",getDischargeAirTemp($T67,$V67,$AD67,$W67,BD67,$AL67, $Y67, $AY67, \"heating\",activeElevation,$AB67,$AJ67,$AV67,$BB67)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T67=\"Select Model\", \"\",IF(OR($T67=\"ACBC_1W\",$T67=\"ACBC_2W\",LEFT($T67,4)=\"ACBR\",$T67 = \"LIU24_2W\",LEFT($T67,3)=\"RIU\",LEFT($T67,6)=\"ACBL12\"), IF((soundLevel($T67, $AB67, BD67, $Y67, $W67,$AJ67,$AA67,\"dba\"))<15,\"<15\",soundLevel($T67, $AB67, BD67, $Y67, $W67,$AJ67,$AA67,\"dba\")+0.4),IF((soundLevel($T67, $AB67, BD67, $Y67, $W67,$AJ67,$AA67,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T67, $AB67, BD67, $Y67, $W67,$AJ67,$AA67,\"dba\")+5)<15, \"<15\", soundLevel($T67, $AB67, BD67,$Y67, $W67,$AJ67,$AA67,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T67=\"Select Model\", \"\",IF(OR($T67=\"ACBC_1W\",$T67=\"ACBC_2W\",LEFT($T67,4)=\"ACBR\",$T67=\"LIU24_2W\",LEFT($T67,3)=\"RIU\",LEFT($T67,6)=\"ACBL12\"), IF((soundLevel($T67, $AB67, BD67, $Y67, $W67,$AJ67,$AA67,\"NC\"))<15,\"<15\",soundLevel($T67, $AB67, BD67, $Y67, $W67,$AJ67,$AA67,\"NC\")+0.4),IF((soundLevel($T67, $AB67, BD67, $Y67, $W67,$AJ67,$AA67,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T67, $AB67, BD67, $Y67, $W67,$AJ67,$AA67,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T67, $AB67, BD67, $Y67, $W67,$AJ67,$AA67,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T67=\"Select Model\",\"\",IF($T67=\"LIU24_2W\",calcQwIP($Y67,$W67,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC67,$AI67,\"latent\",$U67&\"P\"&IF($V67=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T67,activeElevation),\"\"))","v":""},{"$f":"IF($T67=\"Select Model\",\"\",IF($T67=\"ACBC_1W\",calcQwIP($Y67,$W67,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC67,BD67,\"capacity\",$U67&\"P\"&IF($V67=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T67,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y67,$W67,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC67,BD67,\"capacity\",$U67&\"P\"&IF($V67=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T67,activeElevation)))","v":""},"",{"$f":"IF(T67=\"Select Model\", 0,waterPressureDrop(W67, U67 & \"P\" & IF(V67=\"Dual\",2,1) &\"C\", AC67, \"cooling\", T67))","v":0},{"$f":"IF(T67=\"Select Model\", \"\",getReturnWaterTemp(T67,AC67, activeEWTCooling, AS67, \"cooling\"))","v":""},"",{"$f":"IF($T67<>\"ACBC_1W\",\"\",IF($J67=\"\",\"\",FintubeCapacity($T67,$W67,$AE67,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T67=\"Select Model\",T67=\"PCBL\"),\"\",calcQwIP(Y67,W67,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD67,BD67,\"capacity\",U67&\"P\"&IF(V67=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T67,activeElevation))","v":""},"",{"$f":"IF(OR(T67=\"Select Model\",T67=\"PCBL\"), \"\",IF(AY67=0,\"N/A\",waterPressureDrop(W67, U67 & \"P\" & IF(V67=\"Dual\",2,1) &\"C\", AD67, \"heating\", T67)))","v":""},{"$f":"IF(OR(T67=\"Select Model\",T67=\"PCBL\"), \"\",IF(AY67=0,getReturnWaterTemp(T67,AE67, activeEWTHeating, AX67, \"heating\"),getReturnWaterTemp(T67,AD67, activeEWTHeating, AY67, \"heating\")))","v":""},"",{"$f":" getNozzle(T67, W67, Y67, Z67, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I68)),I68<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I68, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H68)),H68<0),\"\",intlEstQuantity(T68, W68*12, H68)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T68=\"Select Model\",\"\",coilCircuitChange(W68, U68, AC68, T68,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T68=\"Select Model\",\"\",beamWidth(T68))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T68=\"Select Model\",T68=\"PCBL\"), 0,getSPIP(T68, W68, Y68, BD68, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T68=\"Select Model\", \"\",IF(T68=\"PCBL\",0,primaryAirSensibleCapacityIP($T68,$W68,activeRoomTempCooling,activePriAirTempCooling,$Y68,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T68=\"Select Model\",\"\",IF($T68=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y68,activeElevation)))","v":""},{"$f":"IF(OR(T68=\"Select Model\",T68=\"PCBL\"), 0,IF(AD68=0,0,-primaryAirSensibleCapacityIP($T68,$W68,activeRoomTempHeating,activePriAirTempHeating,$Y68,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T68=\"Select Model\", \"\", InductionRatio($T68,BD68,$W68,$Y68)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T68=\"Select Model\", \"\",IF($T68=\"PCBL\",\"N/A\",minVAVSetBack(AA68, Y68))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T68=\"Select Model\", \"\",IF($T68= \"PCBL\",\"N/A\",getDischargeAirTemp($T68,$V68,$AC68,$W68,BD68,$AL68, $Y68, $AS68, \"cooling\",activeElevation,$AB68,$AJ68,$AV68,$BB68))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T68=\"Select Model\",$T68=\"PCBL\"), \"\",getDischargeAirTemp($T68,$V68,$AD68,$W68,BD68,$AL68, $Y68, $AY68, \"heating\",activeElevation,$AB68,$AJ68,$AV68,$BB68)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T68=\"Select Model\", \"\",IF(OR($T68=\"ACBC_1W\",$T68=\"ACBC_2W\",LEFT($T68,4)=\"ACBR\",$T68 = \"LIU24_2W\",LEFT($T68,3)=\"RIU\",LEFT($T68,6)=\"ACBL12\"), IF((soundLevel($T68, $AB68, BD68, $Y68, $W68,$AJ68,$AA68,\"dba\"))<15,\"<15\",soundLevel($T68, $AB68, BD68, $Y68, $W68,$AJ68,$AA68,\"dba\")+0.4),IF((soundLevel($T68, $AB68, BD68, $Y68, $W68,$AJ68,$AA68,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T68, $AB68, BD68, $Y68, $W68,$AJ68,$AA68,\"dba\")+5)<15, \"<15\", soundLevel($T68, $AB68, BD68,$Y68, $W68,$AJ68,$AA68,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T68=\"Select Model\", \"\",IF(OR($T68=\"ACBC_1W\",$T68=\"ACBC_2W\",LEFT($T68,4)=\"ACBR\",$T68=\"LIU24_2W\",LEFT($T68,3)=\"RIU\",LEFT($T68,6)=\"ACBL12\"), IF((soundLevel($T68, $AB68, BD68, $Y68, $W68,$AJ68,$AA68,\"NC\"))<15,\"<15\",soundLevel($T68, $AB68, BD68, $Y68, $W68,$AJ68,$AA68,\"NC\")+0.4),IF((soundLevel($T68, $AB68, BD68, $Y68, $W68,$AJ68,$AA68,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T68, $AB68, BD68, $Y68, $W68,$AJ68,$AA68,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T68, $AB68, BD68, $Y68, $W68,$AJ68,$AA68,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T68=\"Select Model\",\"\",IF($T68=\"LIU24_2W\",calcQwIP($Y68,$W68,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC68,$AI68,\"latent\",$U68&\"P\"&IF($V68=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T68,activeElevation),\"\"))","v":""},{"$f":"IF($T68=\"Select Model\",\"\",IF($T68=\"ACBC_1W\",calcQwIP($Y68,$W68,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC68,BD68,\"capacity\",$U68&\"P\"&IF($V68=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T68,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y68,$W68,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC68,BD68,\"capacity\",$U68&\"P\"&IF($V68=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T68,activeElevation)))","v":""},"",{"$f":"IF(T68=\"Select Model\", 0,waterPressureDrop(W68, U68 & \"P\" & IF(V68=\"Dual\",2,1) &\"C\", AC68, \"cooling\", T68))","v":0},{"$f":"IF(T68=\"Select Model\", \"\",getReturnWaterTemp(T68,AC68, activeEWTCooling, AS68, \"cooling\"))","v":""},"",{"$f":"IF($T68<>\"ACBC_1W\",\"\",IF($J68=\"\",\"\",FintubeCapacity($T68,$W68,$AE68,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T68=\"Select Model\",T68=\"PCBL\"),\"\",calcQwIP(Y68,W68,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD68,BD68,\"capacity\",U68&\"P\"&IF(V68=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T68,activeElevation))","v":""},"",{"$f":"IF(OR(T68=\"Select Model\",T68=\"PCBL\"), \"\",IF(AY68=0,\"N/A\",waterPressureDrop(W68, U68 & \"P\" & IF(V68=\"Dual\",2,1) &\"C\", AD68, \"heating\", T68)))","v":""},{"$f":"IF(OR(T68=\"Select Model\",T68=\"PCBL\"), \"\",IF(AY68=0,getReturnWaterTemp(T68,AE68, activeEWTHeating, AX68, \"heating\"),getReturnWaterTemp(T68,AD68, activeEWTHeating, AY68, \"heating\")))","v":""},"",{"$f":" getNozzle(T68, W68, Y68, Z68, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I69)),I69<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I69, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H69)),H69<0),\"\",intlEstQuantity(T69, W69*12, H69)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T69=\"Select Model\",\"\",coilCircuitChange(W69, U69, AC69, T69,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T69=\"Select Model\",\"\",beamWidth(T69))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T69=\"Select Model\",T69=\"PCBL\"), 0,getSPIP(T69, W69, Y69, BD69, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T69=\"Select Model\", \"\",IF(T69=\"PCBL\",0,primaryAirSensibleCapacityIP($T69,$W69,activeRoomTempCooling,activePriAirTempCooling,$Y69,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T69=\"Select Model\",\"\",IF($T69=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y69,activeElevation)))","v":""},{"$f":"IF(OR(T69=\"Select Model\",T69=\"PCBL\"), 0,IF(AD69=0,0,-primaryAirSensibleCapacityIP($T69,$W69,activeRoomTempHeating,activePriAirTempHeating,$Y69,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T69=\"Select Model\", \"\", InductionRatio($T69,BD69,$W69,$Y69)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T69=\"Select Model\", \"\",IF($T69=\"PCBL\",\"N/A\",minVAVSetBack(AA69, Y69))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T69=\"Select Model\", \"\",IF($T69= \"PCBL\",\"N/A\",getDischargeAirTemp($T69,$V69,$AC69,$W69,BD69,$AL69, $Y69, $AS69, \"cooling\",activeElevation,$AB69,$AJ69,$AV69,$BB69))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T69=\"Select Model\",$T69=\"PCBL\"), \"\",getDischargeAirTemp($T69,$V69,$AD69,$W69,BD69,$AL69, $Y69, $AY69, \"heating\",activeElevation,$AB69,$AJ69,$AV69,$BB69)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T69=\"Select Model\", \"\",IF(OR($T69=\"ACBC_1W\",$T69=\"ACBC_2W\",LEFT($T69,4)=\"ACBR\",$T69 = \"LIU24_2W\",LEFT($T69,3)=\"RIU\",LEFT($T69,6)=\"ACBL12\"), IF((soundLevel($T69, $AB69, BD69, $Y69, $W69,$AJ69,$AA69,\"dba\"))<15,\"<15\",soundLevel($T69, $AB69, BD69, $Y69, $W69,$AJ69,$AA69,\"dba\")+0.4),IF((soundLevel($T69, $AB69, BD69, $Y69, $W69,$AJ69,$AA69,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T69, $AB69, BD69, $Y69, $W69,$AJ69,$AA69,\"dba\")+5)<15, \"<15\", soundLevel($T69, $AB69, BD69,$Y69, $W69,$AJ69,$AA69,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T69=\"Select Model\", \"\",IF(OR($T69=\"ACBC_1W\",$T69=\"ACBC_2W\",LEFT($T69,4)=\"ACBR\",$T69=\"LIU24_2W\",LEFT($T69,3)=\"RIU\",LEFT($T69,6)=\"ACBL12\"), IF((soundLevel($T69, $AB69, BD69, $Y69, $W69,$AJ69,$AA69,\"NC\"))<15,\"<15\",soundLevel($T69, $AB69, BD69, $Y69, $W69,$AJ69,$AA69,\"NC\")+0.4),IF((soundLevel($T69, $AB69, BD69, $Y69, $W69,$AJ69,$AA69,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T69, $AB69, BD69, $Y69, $W69,$AJ69,$AA69,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T69, $AB69, BD69, $Y69, $W69,$AJ69,$AA69,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T69=\"Select Model\",\"\",IF($T69=\"LIU24_2W\",calcQwIP($Y69,$W69,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC69,$AI69,\"latent\",$U69&\"P\"&IF($V69=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T69,activeElevation),\"\"))","v":""},{"$f":"IF($T69=\"Select Model\",\"\",IF($T69=\"ACBC_1W\",calcQwIP($Y69,$W69,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC69,BD69,\"capacity\",$U69&\"P\"&IF($V69=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T69,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y69,$W69,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC69,BD69,\"capacity\",$U69&\"P\"&IF($V69=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T69,activeElevation)))","v":""},"",{"$f":"IF(T69=\"Select Model\", 0,waterPressureDrop(W69, U69 & \"P\" & IF(V69=\"Dual\",2,1) &\"C\", AC69, \"cooling\", T69))","v":0},{"$f":"IF(T69=\"Select Model\", \"\",getReturnWaterTemp(T69,AC69, activeEWTCooling, AS69, \"cooling\"))","v":""},"",{"$f":"IF($T69<>\"ACBC_1W\",\"\",IF($J69=\"\",\"\",FintubeCapacity($T69,$W69,$AE69,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T69=\"Select Model\",T69=\"PCBL\"),\"\",calcQwIP(Y69,W69,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD69,BD69,\"capacity\",U69&\"P\"&IF(V69=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T69,activeElevation))","v":""},"",{"$f":"IF(OR(T69=\"Select Model\",T69=\"PCBL\"), \"\",IF(AY69=0,\"N/A\",waterPressureDrop(W69, U69 & \"P\" & IF(V69=\"Dual\",2,1) &\"C\", AD69, \"heating\", T69)))","v":""},{"$f":"IF(OR(T69=\"Select Model\",T69=\"PCBL\"), \"\",IF(AY69=0,getReturnWaterTemp(T69,AE69, activeEWTHeating, AX69, \"heating\"),getReturnWaterTemp(T69,AD69, activeEWTHeating, AY69, \"heating\")))","v":""},"",{"$f":" getNozzle(T69, W69, Y69, Z69, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I70)),I70<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I70, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H70)),H70<0),\"\",intlEstQuantity(T70, W70*12, H70)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T70=\"Select Model\",\"\",coilCircuitChange(W70, U70, AC70, T70,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T70=\"Select Model\",\"\",beamWidth(T70))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T70=\"Select Model\",T70=\"PCBL\"), 0,getSPIP(T70, W70, Y70, BD70, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T70=\"Select Model\", \"\",IF(T70=\"PCBL\",0,primaryAirSensibleCapacityIP($T70,$W70,activeRoomTempCooling,activePriAirTempCooling,$Y70,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T70=\"Select Model\",\"\",IF($T70=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y70,activeElevation)))","v":""},{"$f":"IF(OR(T70=\"Select Model\",T70=\"PCBL\"), 0,IF(AD70=0,0,-primaryAirSensibleCapacityIP($T70,$W70,activeRoomTempHeating,activePriAirTempHeating,$Y70,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T70=\"Select Model\", \"\", InductionRatio($T70,BD70,$W70,$Y70)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T70=\"Select Model\", \"\",IF($T70=\"PCBL\",\"N/A\",minVAVSetBack(AA70, Y70))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T70=\"Select Model\", \"\",IF($T70= \"PCBL\",\"N/A\",getDischargeAirTemp($T70,$V70,$AC70,$W70,BD70,$AL70, $Y70, $AS70, \"cooling\",activeElevation,$AB70,$AJ70,$AV70,$BB70))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T70=\"Select Model\",$T70=\"PCBL\"), \"\",getDischargeAirTemp($T70,$V70,$AD70,$W70,BD70,$AL70, $Y70, $AY70, \"heating\",activeElevation,$AB70,$AJ70,$AV70,$BB70)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T70=\"Select Model\", \"\",IF(OR($T70=\"ACBC_1W\",$T70=\"ACBC_2W\",LEFT($T70,4)=\"ACBR\",$T70 = \"LIU24_2W\",LEFT($T70,3)=\"RIU\",LEFT($T70,6)=\"ACBL12\"), IF((soundLevel($T70, $AB70, BD70, $Y70, $W70,$AJ70,$AA70,\"dba\"))<15,\"<15\",soundLevel($T70, $AB70, BD70, $Y70, $W70,$AJ70,$AA70,\"dba\")+0.4),IF((soundLevel($T70, $AB70, BD70, $Y70, $W70,$AJ70,$AA70,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T70, $AB70, BD70, $Y70, $W70,$AJ70,$AA70,\"dba\")+5)<15, \"<15\", soundLevel($T70, $AB70, BD70,$Y70, $W70,$AJ70,$AA70,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T70=\"Select Model\", \"\",IF(OR($T70=\"ACBC_1W\",$T70=\"ACBC_2W\",LEFT($T70,4)=\"ACBR\",$T70=\"LIU24_2W\",LEFT($T70,3)=\"RIU\",LEFT($T70,6)=\"ACBL12\"), IF((soundLevel($T70, $AB70, BD70, $Y70, $W70,$AJ70,$AA70,\"NC\"))<15,\"<15\",soundLevel($T70, $AB70, BD70, $Y70, $W70,$AJ70,$AA70,\"NC\")+0.4),IF((soundLevel($T70, $AB70, BD70, $Y70, $W70,$AJ70,$AA70,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T70, $AB70, BD70, $Y70, $W70,$AJ70,$AA70,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T70, $AB70, BD70, $Y70, $W70,$AJ70,$AA70,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T70=\"Select Model\",\"\",IF($T70=\"LIU24_2W\",calcQwIP($Y70,$W70,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC70,$AI70,\"latent\",$U70&\"P\"&IF($V70=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T70,activeElevation),\"\"))","v":""},{"$f":"IF($T70=\"Select Model\",\"\",IF($T70=\"ACBC_1W\",calcQwIP($Y70,$W70,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC70,BD70,\"capacity\",$U70&\"P\"&IF($V70=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T70,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y70,$W70,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC70,BD70,\"capacity\",$U70&\"P\"&IF($V70=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T70,activeElevation)))","v":""},"",{"$f":"IF(T70=\"Select Model\", 0,waterPressureDrop(W70, U70 & \"P\" & IF(V70=\"Dual\",2,1) &\"C\", AC70, \"cooling\", T70))","v":0},{"$f":"IF(T70=\"Select Model\", \"\",getReturnWaterTemp(T70,AC70, activeEWTCooling, AS70, \"cooling\"))","v":""},"",{"$f":"IF($T70<>\"ACBC_1W\",\"\",IF($J70=\"\",\"\",FintubeCapacity($T70,$W70,$AE70,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T70=\"Select Model\",T70=\"PCBL\"),\"\",calcQwIP(Y70,W70,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD70,BD70,\"capacity\",U70&\"P\"&IF(V70=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T70,activeElevation))","v":""},"",{"$f":"IF(OR(T70=\"Select Model\",T70=\"PCBL\"), \"\",IF(AY70=0,\"N/A\",waterPressureDrop(W70, U70 & \"P\" & IF(V70=\"Dual\",2,1) &\"C\", AD70, \"heating\", T70)))","v":""},{"$f":"IF(OR(T70=\"Select Model\",T70=\"PCBL\"), \"\",IF(AY70=0,getReturnWaterTemp(T70,AE70, activeEWTHeating, AX70, \"heating\"),getReturnWaterTemp(T70,AD70, activeEWTHeating, AY70, \"heating\")))","v":""},"",{"$f":" getNozzle(T70, W70, Y70, Z70, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I71)),I71<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I71, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H71)),H71<0),\"\",intlEstQuantity(T71, W71*12, H71)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T71=\"Select Model\",\"\",coilCircuitChange(W71, U71, AC71, T71,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T71=\"Select Model\",\"\",beamWidth(T71))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T71=\"Select Model\",T71=\"PCBL\"), 0,getSPIP(T71, W71, Y71, BD71, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T71=\"Select Model\", \"\",IF(T71=\"PCBL\",0,primaryAirSensibleCapacityIP($T71,$W71,activeRoomTempCooling,activePriAirTempCooling,$Y71,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T71=\"Select Model\",\"\",IF($T71=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y71,activeElevation)))","v":""},{"$f":"IF(OR(T71=\"Select Model\",T71=\"PCBL\"), 0,IF(AD71=0,0,-primaryAirSensibleCapacityIP($T71,$W71,activeRoomTempHeating,activePriAirTempHeating,$Y71,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T71=\"Select Model\", \"\", InductionRatio($T71,BD71,$W71,$Y71)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T71=\"Select Model\", \"\",IF($T71=\"PCBL\",\"N/A\",minVAVSetBack(AA71, Y71))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T71=\"Select Model\", \"\",IF($T71= \"PCBL\",\"N/A\",getDischargeAirTemp($T71,$V71,$AC71,$W71,BD71,$AL71, $Y71, $AS71, \"cooling\",activeElevation,$AB71,$AJ71,$AV71,$BB71))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T71=\"Select Model\",$T71=\"PCBL\"), \"\",getDischargeAirTemp($T71,$V71,$AD71,$W71,BD71,$AL71, $Y71, $AY71, \"heating\",activeElevation,$AB71,$AJ71,$AV71,$BB71)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T71=\"Select Model\", \"\",IF(OR($T71=\"ACBC_1W\",$T71=\"ACBC_2W\",LEFT($T71,4)=\"ACBR\",$T71 = \"LIU24_2W\",LEFT($T71,3)=\"RIU\",LEFT($T71,6)=\"ACBL12\"), IF((soundLevel($T71, $AB71, BD71, $Y71, $W71,$AJ71,$AA71,\"dba\"))<15,\"<15\",soundLevel($T71, $AB71, BD71, $Y71, $W71,$AJ71,$AA71,\"dba\")+0.4),IF((soundLevel($T71, $AB71, BD71, $Y71, $W71,$AJ71,$AA71,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T71, $AB71, BD71, $Y71, $W71,$AJ71,$AA71,\"dba\")+5)<15, \"<15\", soundLevel($T71, $AB71, BD71,$Y71, $W71,$AJ71,$AA71,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T71=\"Select Model\", \"\",IF(OR($T71=\"ACBC_1W\",$T71=\"ACBC_2W\",LEFT($T71,4)=\"ACBR\",$T71=\"LIU24_2W\",LEFT($T71,3)=\"RIU\",LEFT($T71,6)=\"ACBL12\"), IF((soundLevel($T71, $AB71, BD71, $Y71, $W71,$AJ71,$AA71,\"NC\"))<15,\"<15\",soundLevel($T71, $AB71, BD71, $Y71, $W71,$AJ71,$AA71,\"NC\")+0.4),IF((soundLevel($T71, $AB71, BD71, $Y71, $W71,$AJ71,$AA71,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T71, $AB71, BD71, $Y71, $W71,$AJ71,$AA71,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T71, $AB71, BD71, $Y71, $W71,$AJ71,$AA71,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T71=\"Select Model\",\"\",IF($T71=\"LIU24_2W\",calcQwIP($Y71,$W71,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC71,$AI71,\"latent\",$U71&\"P\"&IF($V71=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T71,activeElevation),\"\"))","v":""},{"$f":"IF($T71=\"Select Model\",\"\",IF($T71=\"ACBC_1W\",calcQwIP($Y71,$W71,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC71,BD71,\"capacity\",$U71&\"P\"&IF($V71=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T71,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y71,$W71,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC71,BD71,\"capacity\",$U71&\"P\"&IF($V71=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T71,activeElevation)))","v":""},"",{"$f":"IF(T71=\"Select Model\", 0,waterPressureDrop(W71, U71 & \"P\" & IF(V71=\"Dual\",2,1) &\"C\", AC71, \"cooling\", T71))","v":0},{"$f":"IF(T71=\"Select Model\", \"\",getReturnWaterTemp(T71,AC71, activeEWTCooling, AS71, \"cooling\"))","v":""},"",{"$f":"IF($T71<>\"ACBC_1W\",\"\",IF($J71=\"\",\"\",FintubeCapacity($T71,$W71,$AE71,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T71=\"Select Model\",T71=\"PCBL\"),\"\",calcQwIP(Y71,W71,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD71,BD71,\"capacity\",U71&\"P\"&IF(V71=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T71,activeElevation))","v":""},"",{"$f":"IF(OR(T71=\"Select Model\",T71=\"PCBL\"), \"\",IF(AY71=0,\"N/A\",waterPressureDrop(W71, U71 & \"P\" & IF(V71=\"Dual\",2,1) &\"C\", AD71, \"heating\", T71)))","v":""},{"$f":"IF(OR(T71=\"Select Model\",T71=\"PCBL\"), \"\",IF(AY71=0,getReturnWaterTemp(T71,AE71, activeEWTHeating, AX71, \"heating\"),getReturnWaterTemp(T71,AD71, activeEWTHeating, AY71, \"heating\")))","v":""},"",{"$f":" getNozzle(T71, W71, Y71, Z71, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I72)),I72<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I72, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H72)),H72<0),\"\",intlEstQuantity(T72, W72*12, H72)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T72=\"Select Model\",\"\",coilCircuitChange(W72, U72, AC72, T72,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T72=\"Select Model\",\"\",beamWidth(T72))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T72=\"Select Model\",T72=\"PCBL\"), 0,getSPIP(T72, W72, Y72, BD72, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T72=\"Select Model\", \"\",IF(T72=\"PCBL\",0,primaryAirSensibleCapacityIP($T72,$W72,activeRoomTempCooling,activePriAirTempCooling,$Y72,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T72=\"Select Model\",\"\",IF($T72=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y72,activeElevation)))","v":""},{"$f":"IF(OR(T72=\"Select Model\",T72=\"PCBL\"), 0,IF(AD72=0,0,-primaryAirSensibleCapacityIP($T72,$W72,activeRoomTempHeating,activePriAirTempHeating,$Y72,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T72=\"Select Model\", \"\", InductionRatio($T72,BD72,$W72,$Y72)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T72=\"Select Model\", \"\",IF($T72=\"PCBL\",\"N/A\",minVAVSetBack(AA72, Y72))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T72=\"Select Model\", \"\",IF($T72= \"PCBL\",\"N/A\",getDischargeAirTemp($T72,$V72,$AC72,$W72,BD72,$AL72, $Y72, $AS72, \"cooling\",activeElevation,$AB72,$AJ72,$AV72,$BB72))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T72=\"Select Model\",$T72=\"PCBL\"), \"\",getDischargeAirTemp($T72,$V72,$AD72,$W72,BD72,$AL72, $Y72, $AY72, \"heating\",activeElevation,$AB72,$AJ72,$AV72,$BB72)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T72=\"Select Model\", \"\",IF(OR($T72=\"ACBC_1W\",$T72=\"ACBC_2W\",LEFT($T72,4)=\"ACBR\",$T72 = \"LIU24_2W\",LEFT($T72,3)=\"RIU\",LEFT($T72,6)=\"ACBL12\"), IF((soundLevel($T72, $AB72, BD72, $Y72, $W72,$AJ72,$AA72,\"dba\"))<15,\"<15\",soundLevel($T72, $AB72, BD72, $Y72, $W72,$AJ72,$AA72,\"dba\")+0.4),IF((soundLevel($T72, $AB72, BD72, $Y72, $W72,$AJ72,$AA72,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T72, $AB72, BD72, $Y72, $W72,$AJ72,$AA72,\"dba\")+5)<15, \"<15\", soundLevel($T72, $AB72, BD72,$Y72, $W72,$AJ72,$AA72,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T72=\"Select Model\", \"\",IF(OR($T72=\"ACBC_1W\",$T72=\"ACBC_2W\",LEFT($T72,4)=\"ACBR\",$T72=\"LIU24_2W\",LEFT($T72,3)=\"RIU\",LEFT($T72,6)=\"ACBL12\"), IF((soundLevel($T72, $AB72, BD72, $Y72, $W72,$AJ72,$AA72,\"NC\"))<15,\"<15\",soundLevel($T72, $AB72, BD72, $Y72, $W72,$AJ72,$AA72,\"NC\")+0.4),IF((soundLevel($T72, $AB72, BD72, $Y72, $W72,$AJ72,$AA72,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T72, $AB72, BD72, $Y72, $W72,$AJ72,$AA72,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T72, $AB72, BD72, $Y72, $W72,$AJ72,$AA72,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T72=\"Select Model\",\"\",IF($T72=\"LIU24_2W\",calcQwIP($Y72,$W72,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC72,$AI72,\"latent\",$U72&\"P\"&IF($V72=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T72,activeElevation),\"\"))","v":""},{"$f":"IF($T72=\"Select Model\",\"\",IF($T72=\"ACBC_1W\",calcQwIP($Y72,$W72,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC72,BD72,\"capacity\",$U72&\"P\"&IF($V72=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T72,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y72,$W72,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC72,BD72,\"capacity\",$U72&\"P\"&IF($V72=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T72,activeElevation)))","v":""},"",{"$f":"IF(T72=\"Select Model\", 0,waterPressureDrop(W72, U72 & \"P\" & IF(V72=\"Dual\",2,1) &\"C\", AC72, \"cooling\", T72))","v":0},{"$f":"IF(T72=\"Select Model\", \"\",getReturnWaterTemp(T72,AC72, activeEWTCooling, AS72, \"cooling\"))","v":""},"",{"$f":"IF($T72<>\"ACBC_1W\",\"\",IF($J72=\"\",\"\",FintubeCapacity($T72,$W72,$AE72,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T72=\"Select Model\",T72=\"PCBL\"),\"\",calcQwIP(Y72,W72,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD72,BD72,\"capacity\",U72&\"P\"&IF(V72=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T72,activeElevation))","v":""},"",{"$f":"IF(OR(T72=\"Select Model\",T72=\"PCBL\"), \"\",IF(AY72=0,\"N/A\",waterPressureDrop(W72, U72 & \"P\" & IF(V72=\"Dual\",2,1) &\"C\", AD72, \"heating\", T72)))","v":""},{"$f":"IF(OR(T72=\"Select Model\",T72=\"PCBL\"), \"\",IF(AY72=0,getReturnWaterTemp(T72,AE72, activeEWTHeating, AX72, \"heating\"),getReturnWaterTemp(T72,AD72, activeEWTHeating, AY72, \"heating\")))","v":""},"",{"$f":" getNozzle(T72, W72, Y72, Z72, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I73)),I73<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I73, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H73)),H73<0),\"\",intlEstQuantity(T73, W73*12, H73)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T73=\"Select Model\",\"\",coilCircuitChange(W73, U73, AC73, T73,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T73=\"Select Model\",\"\",beamWidth(T73))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T73=\"Select Model\",T73=\"PCBL\"), 0,getSPIP(T73, W73, Y73, BD73, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T73=\"Select Model\", \"\",IF(T73=\"PCBL\",0,primaryAirSensibleCapacityIP($T73,$W73,activeRoomTempCooling,activePriAirTempCooling,$Y73,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T73=\"Select Model\",\"\",IF($T73=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y73,activeElevation)))","v":""},{"$f":"IF(OR(T73=\"Select Model\",T73=\"PCBL\"), 0,IF(AD73=0,0,-primaryAirSensibleCapacityIP($T73,$W73,activeRoomTempHeating,activePriAirTempHeating,$Y73,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T73=\"Select Model\", \"\", InductionRatio($T73,BD73,$W73,$Y73)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T73=\"Select Model\", \"\",IF($T73=\"PCBL\",\"N/A\",minVAVSetBack(AA73, Y73))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T73=\"Select Model\", \"\",IF($T73= \"PCBL\",\"N/A\",getDischargeAirTemp($T73,$V73,$AC73,$W73,BD73,$AL73, $Y73, $AS73, \"cooling\",activeElevation,$AB73,$AJ73,$AV73,$BB73))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T73=\"Select Model\",$T73=\"PCBL\"), \"\",getDischargeAirTemp($T73,$V73,$AD73,$W73,BD73,$AL73, $Y73, $AY73, \"heating\",activeElevation,$AB73,$AJ73,$AV73,$BB73)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T73=\"Select Model\", \"\",IF(OR($T73=\"ACBC_1W\",$T73=\"ACBC_2W\",LEFT($T73,4)=\"ACBR\",$T73 = \"LIU24_2W\",LEFT($T73,3)=\"RIU\",LEFT($T73,6)=\"ACBL12\"), IF((soundLevel($T73, $AB73, BD73, $Y73, $W73,$AJ73,$AA73,\"dba\"))<15,\"<15\",soundLevel($T73, $AB73, BD73, $Y73, $W73,$AJ73,$AA73,\"dba\")+0.4),IF((soundLevel($T73, $AB73, BD73, $Y73, $W73,$AJ73,$AA73,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T73, $AB73, BD73, $Y73, $W73,$AJ73,$AA73,\"dba\")+5)<15, \"<15\", soundLevel($T73, $AB73, BD73,$Y73, $W73,$AJ73,$AA73,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T73=\"Select Model\", \"\",IF(OR($T73=\"ACBC_1W\",$T73=\"ACBC_2W\",LEFT($T73,4)=\"ACBR\",$T73=\"LIU24_2W\",LEFT($T73,3)=\"RIU\",LEFT($T73,6)=\"ACBL12\"), IF((soundLevel($T73, $AB73, BD73, $Y73, $W73,$AJ73,$AA73,\"NC\"))<15,\"<15\",soundLevel($T73, $AB73, BD73, $Y73, $W73,$AJ73,$AA73,\"NC\")+0.4),IF((soundLevel($T73, $AB73, BD73, $Y73, $W73,$AJ73,$AA73,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T73, $AB73, BD73, $Y73, $W73,$AJ73,$AA73,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T73, $AB73, BD73, $Y73, $W73,$AJ73,$AA73,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T73=\"Select Model\",\"\",IF($T73=\"LIU24_2W\",calcQwIP($Y73,$W73,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC73,$AI73,\"latent\",$U73&\"P\"&IF($V73=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T73,activeElevation),\"\"))","v":""},{"$f":"IF($T73=\"Select Model\",\"\",IF($T73=\"ACBC_1W\",calcQwIP($Y73,$W73,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC73,BD73,\"capacity\",$U73&\"P\"&IF($V73=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T73,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y73,$W73,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC73,BD73,\"capacity\",$U73&\"P\"&IF($V73=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T73,activeElevation)))","v":""},"",{"$f":"IF(T73=\"Select Model\", 0,waterPressureDrop(W73, U73 & \"P\" & IF(V73=\"Dual\",2,1) &\"C\", AC73, \"cooling\", T73))","v":0},{"$f":"IF(T73=\"Select Model\", \"\",getReturnWaterTemp(T73,AC73, activeEWTCooling, AS73, \"cooling\"))","v":""},"",{"$f":"IF($T73<>\"ACBC_1W\",\"\",IF($J73=\"\",\"\",FintubeCapacity($T73,$W73,$AE73,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T73=\"Select Model\",T73=\"PCBL\"),\"\",calcQwIP(Y73,W73,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD73,BD73,\"capacity\",U73&\"P\"&IF(V73=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T73,activeElevation))","v":""},"",{"$f":"IF(OR(T73=\"Select Model\",T73=\"PCBL\"), \"\",IF(AY73=0,\"N/A\",waterPressureDrop(W73, U73 & \"P\" & IF(V73=\"Dual\",2,1) &\"C\", AD73, \"heating\", T73)))","v":""},{"$f":"IF(OR(T73=\"Select Model\",T73=\"PCBL\"), \"\",IF(AY73=0,getReturnWaterTemp(T73,AE73, activeEWTHeating, AX73, \"heating\"),getReturnWaterTemp(T73,AD73, activeEWTHeating, AY73, \"heating\")))","v":""},"",{"$f":" getNozzle(T73, W73, Y73, Z73, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I74)),I74<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I74, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H74)),H74<0),\"\",intlEstQuantity(T74, W74*12, H74)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T74=\"Select Model\",\"\",coilCircuitChange(W74, U74, AC74, T74,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T74=\"Select Model\",\"\",beamWidth(T74))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T74=\"Select Model\",T74=\"PCBL\"), 0,getSPIP(T74, W74, Y74, BD74, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T74=\"Select Model\", \"\",IF(T74=\"PCBL\",0,primaryAirSensibleCapacityIP($T74,$W74,activeRoomTempCooling,activePriAirTempCooling,$Y74,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T74=\"Select Model\",\"\",IF($T74=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y74,activeElevation)))","v":""},{"$f":"IF(OR(T74=\"Select Model\",T74=\"PCBL\"), 0,IF(AD74=0,0,-primaryAirSensibleCapacityIP($T74,$W74,activeRoomTempHeating,activePriAirTempHeating,$Y74,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T74=\"Select Model\", \"\", InductionRatio($T74,BD74,$W74,$Y74)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T74=\"Select Model\", \"\",IF($T74=\"PCBL\",\"N/A\",minVAVSetBack(AA74, Y74))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T74=\"Select Model\", \"\",IF($T74= \"PCBL\",\"N/A\",getDischargeAirTemp($T74,$V74,$AC74,$W74,BD74,$AL74, $Y74, $AS74, \"cooling\",activeElevation,$AB74,$AJ74,$AV74,$BB74))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T74=\"Select Model\",$T74=\"PCBL\"), \"\",getDischargeAirTemp($T74,$V74,$AD74,$W74,BD74,$AL74, $Y74, $AY74, \"heating\",activeElevation,$AB74,$AJ74,$AV74,$BB74)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T74=\"Select Model\", \"\",IF(OR($T74=\"ACBC_1W\",$T74=\"ACBC_2W\",LEFT($T74,4)=\"ACBR\",$T74 = \"LIU24_2W\",LEFT($T74,3)=\"RIU\",LEFT($T74,6)=\"ACBL12\"), IF((soundLevel($T74, $AB74, BD74, $Y74, $W74,$AJ74,$AA74,\"dba\"))<15,\"<15\",soundLevel($T74, $AB74, BD74, $Y74, $W74,$AJ74,$AA74,\"dba\")+0.4),IF((soundLevel($T74, $AB74, BD74, $Y74, $W74,$AJ74,$AA74,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T74, $AB74, BD74, $Y74, $W74,$AJ74,$AA74,\"dba\")+5)<15, \"<15\", soundLevel($T74, $AB74, BD74,$Y74, $W74,$AJ74,$AA74,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T74=\"Select Model\", \"\",IF(OR($T74=\"ACBC_1W\",$T74=\"ACBC_2W\",LEFT($T74,4)=\"ACBR\",$T74=\"LIU24_2W\",LEFT($T74,3)=\"RIU\",LEFT($T74,6)=\"ACBL12\"), IF((soundLevel($T74, $AB74, BD74, $Y74, $W74,$AJ74,$AA74,\"NC\"))<15,\"<15\",soundLevel($T74, $AB74, BD74, $Y74, $W74,$AJ74,$AA74,\"NC\")+0.4),IF((soundLevel($T74, $AB74, BD74, $Y74, $W74,$AJ74,$AA74,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T74, $AB74, BD74, $Y74, $W74,$AJ74,$AA74,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T74, $AB74, BD74, $Y74, $W74,$AJ74,$AA74,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T74=\"Select Model\",\"\",IF($T74=\"LIU24_2W\",calcQwIP($Y74,$W74,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC74,$AI74,\"latent\",$U74&\"P\"&IF($V74=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T74,activeElevation),\"\"))","v":""},{"$f":"IF($T74=\"Select Model\",\"\",IF($T74=\"ACBC_1W\",calcQwIP($Y74,$W74,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC74,BD74,\"capacity\",$U74&\"P\"&IF($V74=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T74,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y74,$W74,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC74,BD74,\"capacity\",$U74&\"P\"&IF($V74=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T74,activeElevation)))","v":""},"",{"$f":"IF(T74=\"Select Model\", 0,waterPressureDrop(W74, U74 & \"P\" & IF(V74=\"Dual\",2,1) &\"C\", AC74, \"cooling\", T74))","v":0},{"$f":"IF(T74=\"Select Model\", \"\",getReturnWaterTemp(T74,AC74, activeEWTCooling, AS74, \"cooling\"))","v":""},"",{"$f":"IF($T74<>\"ACBC_1W\",\"\",IF($J74=\"\",\"\",FintubeCapacity($T74,$W74,$AE74,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T74=\"Select Model\",T74=\"PCBL\"),\"\",calcQwIP(Y74,W74,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD74,BD74,\"capacity\",U74&\"P\"&IF(V74=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T74,activeElevation))","v":""},"",{"$f":"IF(OR(T74=\"Select Model\",T74=\"PCBL\"), \"\",IF(AY74=0,\"N/A\",waterPressureDrop(W74, U74 & \"P\" & IF(V74=\"Dual\",2,1) &\"C\", AD74, \"heating\", T74)))","v":""},{"$f":"IF(OR(T74=\"Select Model\",T74=\"PCBL\"), \"\",IF(AY74=0,getReturnWaterTemp(T74,AE74, activeEWTHeating, AX74, \"heating\"),getReturnWaterTemp(T74,AD74, activeEWTHeating, AY74, \"heating\")))","v":""},"",{"$f":" getNozzle(T74, W74, Y74, Z74, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I75)),I75<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I75, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H75)),H75<0),\"\",intlEstQuantity(T75, W75*12, H75)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T75=\"Select Model\",\"\",coilCircuitChange(W75, U75, AC75, T75,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T75=\"Select Model\",\"\",beamWidth(T75))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T75=\"Select Model\",T75=\"PCBL\"), 0,getSPIP(T75, W75, Y75, BD75, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T75=\"Select Model\", \"\",IF(T75=\"PCBL\",0,primaryAirSensibleCapacityIP($T75,$W75,activeRoomTempCooling,activePriAirTempCooling,$Y75,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T75=\"Select Model\",\"\",IF($T75=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y75,activeElevation)))","v":""},{"$f":"IF(OR(T75=\"Select Model\",T75=\"PCBL\"), 0,IF(AD75=0,0,-primaryAirSensibleCapacityIP($T75,$W75,activeRoomTempHeating,activePriAirTempHeating,$Y75,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T75=\"Select Model\", \"\", InductionRatio($T75,BD75,$W75,$Y75)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T75=\"Select Model\", \"\",IF($T75=\"PCBL\",\"N/A\",minVAVSetBack(AA75, Y75))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T75=\"Select Model\", \"\",IF($T75= \"PCBL\",\"N/A\",getDischargeAirTemp($T75,$V75,$AC75,$W75,BD75,$AL75, $Y75, $AS75, \"cooling\",activeElevation,$AB75,$AJ75,$AV75,$BB75))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T75=\"Select Model\",$T75=\"PCBL\"), \"\",getDischargeAirTemp($T75,$V75,$AD75,$W75,BD75,$AL75, $Y75, $AY75, \"heating\",activeElevation,$AB75,$AJ75,$AV75,$BB75)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T75=\"Select Model\", \"\",IF(OR($T75=\"ACBC_1W\",$T75=\"ACBC_2W\",LEFT($T75,4)=\"ACBR\",$T75 = \"LIU24_2W\",LEFT($T75,3)=\"RIU\",LEFT($T75,6)=\"ACBL12\"), IF((soundLevel($T75, $AB75, BD75, $Y75, $W75,$AJ75,$AA75,\"dba\"))<15,\"<15\",soundLevel($T75, $AB75, BD75, $Y75, $W75,$AJ75,$AA75,\"dba\")+0.4),IF((soundLevel($T75, $AB75, BD75, $Y75, $W75,$AJ75,$AA75,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T75, $AB75, BD75, $Y75, $W75,$AJ75,$AA75,\"dba\")+5)<15, \"<15\", soundLevel($T75, $AB75, BD75,$Y75, $W75,$AJ75,$AA75,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T75=\"Select Model\", \"\",IF(OR($T75=\"ACBC_1W\",$T75=\"ACBC_2W\",LEFT($T75,4)=\"ACBR\",$T75=\"LIU24_2W\",LEFT($T75,3)=\"RIU\",LEFT($T75,6)=\"ACBL12\"), IF((soundLevel($T75, $AB75, BD75, $Y75, $W75,$AJ75,$AA75,\"NC\"))<15,\"<15\",soundLevel($T75, $AB75, BD75, $Y75, $W75,$AJ75,$AA75,\"NC\")+0.4),IF((soundLevel($T75, $AB75, BD75, $Y75, $W75,$AJ75,$AA75,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T75, $AB75, BD75, $Y75, $W75,$AJ75,$AA75,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T75, $AB75, BD75, $Y75, $W75,$AJ75,$AA75,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T75=\"Select Model\",\"\",IF($T75=\"LIU24_2W\",calcQwIP($Y75,$W75,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC75,$AI75,\"latent\",$U75&\"P\"&IF($V75=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T75,activeElevation),\"\"))","v":""},{"$f":"IF($T75=\"Select Model\",\"\",IF($T75=\"ACBC_1W\",calcQwIP($Y75,$W75,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC75,BD75,\"capacity\",$U75&\"P\"&IF($V75=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T75,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y75,$W75,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC75,BD75,\"capacity\",$U75&\"P\"&IF($V75=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T75,activeElevation)))","v":""},"",{"$f":"IF(T75=\"Select Model\", 0,waterPressureDrop(W75, U75 & \"P\" & IF(V75=\"Dual\",2,1) &\"C\", AC75, \"cooling\", T75))","v":0},{"$f":"IF(T75=\"Select Model\", \"\",getReturnWaterTemp(T75,AC75, activeEWTCooling, AS75, \"cooling\"))","v":""},"",{"$f":"IF($T75<>\"ACBC_1W\",\"\",IF($J75=\"\",\"\",FintubeCapacity($T75,$W75,$AE75,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T75=\"Select Model\",T75=\"PCBL\"),\"\",calcQwIP(Y75,W75,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD75,BD75,\"capacity\",U75&\"P\"&IF(V75=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T75,activeElevation))","v":""},"",{"$f":"IF(OR(T75=\"Select Model\",T75=\"PCBL\"), \"\",IF(AY75=0,\"N/A\",waterPressureDrop(W75, U75 & \"P\" & IF(V75=\"Dual\",2,1) &\"C\", AD75, \"heating\", T75)))","v":""},{"$f":"IF(OR(T75=\"Select Model\",T75=\"PCBL\"), \"\",IF(AY75=0,getReturnWaterTemp(T75,AE75, activeEWTHeating, AX75, \"heating\"),getReturnWaterTemp(T75,AD75, activeEWTHeating, AY75, \"heating\")))","v":""},"",{"$f":" getNozzle(T75, W75, Y75, Z75, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I76)),I76<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I76, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H76)),H76<0),\"\",intlEstQuantity(T76, W76*12, H76)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T76=\"Select Model\",\"\",coilCircuitChange(W76, U76, AC76, T76,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T76=\"Select Model\",\"\",beamWidth(T76))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T76=\"Select Model\",T76=\"PCBL\"), 0,getSPIP(T76, W76, Y76, BD76, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T76=\"Select Model\", \"\",IF(T76=\"PCBL\",0,primaryAirSensibleCapacityIP($T76,$W76,activeRoomTempCooling,activePriAirTempCooling,$Y76,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T76=\"Select Model\",\"\",IF($T76=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y76,activeElevation)))","v":""},{"$f":"IF(OR(T76=\"Select Model\",T76=\"PCBL\"), 0,IF(AD76=0,0,-primaryAirSensibleCapacityIP($T76,$W76,activeRoomTempHeating,activePriAirTempHeating,$Y76,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T76=\"Select Model\", \"\", InductionRatio($T76,BD76,$W76,$Y76)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T76=\"Select Model\", \"\",IF($T76=\"PCBL\",\"N/A\",minVAVSetBack(AA76, Y76))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T76=\"Select Model\", \"\",IF($T76= \"PCBL\",\"N/A\",getDischargeAirTemp($T76,$V76,$AC76,$W76,BD76,$AL76, $Y76, $AS76, \"cooling\",activeElevation,$AB76,$AJ76,$AV76,$BB76))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T76=\"Select Model\",$T76=\"PCBL\"), \"\",getDischargeAirTemp($T76,$V76,$AD76,$W76,BD76,$AL76, $Y76, $AY76, \"heating\",activeElevation,$AB76,$AJ76,$AV76,$BB76)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T76=\"Select Model\", \"\",IF(OR($T76=\"ACBC_1W\",$T76=\"ACBC_2W\",LEFT($T76,4)=\"ACBR\",$T76 = \"LIU24_2W\",LEFT($T76,3)=\"RIU\",LEFT($T76,6)=\"ACBL12\"), IF((soundLevel($T76, $AB76, BD76, $Y76, $W76,$AJ76,$AA76,\"dba\"))<15,\"<15\",soundLevel($T76, $AB76, BD76, $Y76, $W76,$AJ76,$AA76,\"dba\")+0.4),IF((soundLevel($T76, $AB76, BD76, $Y76, $W76,$AJ76,$AA76,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T76, $AB76, BD76, $Y76, $W76,$AJ76,$AA76,\"dba\")+5)<15, \"<15\", soundLevel($T76, $AB76, BD76,$Y76, $W76,$AJ76,$AA76,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T76=\"Select Model\", \"\",IF(OR($T76=\"ACBC_1W\",$T76=\"ACBC_2W\",LEFT($T76,4)=\"ACBR\",$T76=\"LIU24_2W\",LEFT($T76,3)=\"RIU\",LEFT($T76,6)=\"ACBL12\"), IF((soundLevel($T76, $AB76, BD76, $Y76, $W76,$AJ76,$AA76,\"NC\"))<15,\"<15\",soundLevel($T76, $AB76, BD76, $Y76, $W76,$AJ76,$AA76,\"NC\")+0.4),IF((soundLevel($T76, $AB76, BD76, $Y76, $W76,$AJ76,$AA76,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T76, $AB76, BD76, $Y76, $W76,$AJ76,$AA76,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T76, $AB76, BD76, $Y76, $W76,$AJ76,$AA76,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T76=\"Select Model\",\"\",IF($T76=\"LIU24_2W\",calcQwIP($Y76,$W76,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC76,$AI76,\"latent\",$U76&\"P\"&IF($V76=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T76,activeElevation),\"\"))","v":""},{"$f":"IF($T76=\"Select Model\",\"\",IF($T76=\"ACBC_1W\",calcQwIP($Y76,$W76,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC76,BD76,\"capacity\",$U76&\"P\"&IF($V76=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T76,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y76,$W76,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC76,BD76,\"capacity\",$U76&\"P\"&IF($V76=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T76,activeElevation)))","v":""},"",{"$f":"IF(T76=\"Select Model\", 0,waterPressureDrop(W76, U76 & \"P\" & IF(V76=\"Dual\",2,1) &\"C\", AC76, \"cooling\", T76))","v":0},{"$f":"IF(T76=\"Select Model\", \"\",getReturnWaterTemp(T76,AC76, activeEWTCooling, AS76, \"cooling\"))","v":""},"",{"$f":"IF($T76<>\"ACBC_1W\",\"\",IF($J76=\"\",\"\",FintubeCapacity($T76,$W76,$AE76,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T76=\"Select Model\",T76=\"PCBL\"),\"\",calcQwIP(Y76,W76,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD76,BD76,\"capacity\",U76&\"P\"&IF(V76=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T76,activeElevation))","v":""},"",{"$f":"IF(OR(T76=\"Select Model\",T76=\"PCBL\"), \"\",IF(AY76=0,\"N/A\",waterPressureDrop(W76, U76 & \"P\" & IF(V76=\"Dual\",2,1) &\"C\", AD76, \"heating\", T76)))","v":""},{"$f":"IF(OR(T76=\"Select Model\",T76=\"PCBL\"), \"\",IF(AY76=0,getReturnWaterTemp(T76,AE76, activeEWTHeating, AX76, \"heating\"),getReturnWaterTemp(T76,AD76, activeEWTHeating, AY76, \"heating\")))","v":""},"",{"$f":" getNozzle(T76, W76, Y76, Z76, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I77)),I77<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I77, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H77)),H77<0),\"\",intlEstQuantity(T77, W77*12, H77)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T77=\"Select Model\",\"\",coilCircuitChange(W77, U77, AC77, T77,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T77=\"Select Model\",\"\",beamWidth(T77))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T77=\"Select Model\",T77=\"PCBL\"), 0,getSPIP(T77, W77, Y77, BD77, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T77=\"Select Model\", \"\",IF(T77=\"PCBL\",0,primaryAirSensibleCapacityIP($T77,$W77,activeRoomTempCooling,activePriAirTempCooling,$Y77,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T77=\"Select Model\",\"\",IF($T77=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y77,activeElevation)))","v":""},{"$f":"IF(OR(T77=\"Select Model\",T77=\"PCBL\"), 0,IF(AD77=0,0,-primaryAirSensibleCapacityIP($T77,$W77,activeRoomTempHeating,activePriAirTempHeating,$Y77,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T77=\"Select Model\", \"\", InductionRatio($T77,BD77,$W77,$Y77)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T77=\"Select Model\", \"\",IF($T77=\"PCBL\",\"N/A\",minVAVSetBack(AA77, Y77))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T77=\"Select Model\", \"\",IF($T77= \"PCBL\",\"N/A\",getDischargeAirTemp($T77,$V77,$AC77,$W77,BD77,$AL77, $Y77, $AS77, \"cooling\",activeElevation,$AB77,$AJ77,$AV77,$BB77))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T77=\"Select Model\",$T77=\"PCBL\"), \"\",getDischargeAirTemp($T77,$V77,$AD77,$W77,BD77,$AL77, $Y77, $AY77, \"heating\",activeElevation,$AB77,$AJ77,$AV77,$BB77)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T77=\"Select Model\", \"\",IF(OR($T77=\"ACBC_1W\",$T77=\"ACBC_2W\",LEFT($T77,4)=\"ACBR\",$T77 = \"LIU24_2W\",LEFT($T77,3)=\"RIU\",LEFT($T77,6)=\"ACBL12\"), IF((soundLevel($T77, $AB77, BD77, $Y77, $W77,$AJ77,$AA77,\"dba\"))<15,\"<15\",soundLevel($T77, $AB77, BD77, $Y77, $W77,$AJ77,$AA77,\"dba\")+0.4),IF((soundLevel($T77, $AB77, BD77, $Y77, $W77,$AJ77,$AA77,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T77, $AB77, BD77, $Y77, $W77,$AJ77,$AA77,\"dba\")+5)<15, \"<15\", soundLevel($T77, $AB77, BD77,$Y77, $W77,$AJ77,$AA77,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T77=\"Select Model\", \"\",IF(OR($T77=\"ACBC_1W\",$T77=\"ACBC_2W\",LEFT($T77,4)=\"ACBR\",$T77=\"LIU24_2W\",LEFT($T77,3)=\"RIU\",LEFT($T77,6)=\"ACBL12\"), IF((soundLevel($T77, $AB77, BD77, $Y77, $W77,$AJ77,$AA77,\"NC\"))<15,\"<15\",soundLevel($T77, $AB77, BD77, $Y77, $W77,$AJ77,$AA77,\"NC\")+0.4),IF((soundLevel($T77, $AB77, BD77, $Y77, $W77,$AJ77,$AA77,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T77, $AB77, BD77, $Y77, $W77,$AJ77,$AA77,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T77, $AB77, BD77, $Y77, $W77,$AJ77,$AA77,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T77=\"Select Model\",\"\",IF($T77=\"LIU24_2W\",calcQwIP($Y77,$W77,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC77,$AI77,\"latent\",$U77&\"P\"&IF($V77=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T77,activeElevation),\"\"))","v":""},{"$f":"IF($T77=\"Select Model\",\"\",IF($T77=\"ACBC_1W\",calcQwIP($Y77,$W77,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC77,BD77,\"capacity\",$U77&\"P\"&IF($V77=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T77,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y77,$W77,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC77,BD77,\"capacity\",$U77&\"P\"&IF($V77=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T77,activeElevation)))","v":""},"",{"$f":"IF(T77=\"Select Model\", 0,waterPressureDrop(W77, U77 & \"P\" & IF(V77=\"Dual\",2,1) &\"C\", AC77, \"cooling\", T77))","v":0},{"$f":"IF(T77=\"Select Model\", \"\",getReturnWaterTemp(T77,AC77, activeEWTCooling, AS77, \"cooling\"))","v":""},"",{"$f":"IF($T77<>\"ACBC_1W\",\"\",IF($J77=\"\",\"\",FintubeCapacity($T77,$W77,$AE77,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T77=\"Select Model\",T77=\"PCBL\"),\"\",calcQwIP(Y77,W77,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD77,BD77,\"capacity\",U77&\"P\"&IF(V77=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T77,activeElevation))","v":""},"",{"$f":"IF(OR(T77=\"Select Model\",T77=\"PCBL\"), \"\",IF(AY77=0,\"N/A\",waterPressureDrop(W77, U77 & \"P\" & IF(V77=\"Dual\",2,1) &\"C\", AD77, \"heating\", T77)))","v":""},{"$f":"IF(OR(T77=\"Select Model\",T77=\"PCBL\"), \"\",IF(AY77=0,getReturnWaterTemp(T77,AE77, activeEWTHeating, AX77, \"heating\"),getReturnWaterTemp(T77,AD77, activeEWTHeating, AY77, \"heating\")))","v":""},"",{"$f":" getNozzle(T77, W77, Y77, Z77, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I78)),I78<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I78, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H78)),H78<0),\"\",intlEstQuantity(T78, W78*12, H78)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T78=\"Select Model\",\"\",coilCircuitChange(W78, U78, AC78, T78,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T78=\"Select Model\",\"\",beamWidth(T78))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T78=\"Select Model\",T78=\"PCBL\"), 0,getSPIP(T78, W78, Y78, BD78, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T78=\"Select Model\", \"\",IF(T78=\"PCBL\",0,primaryAirSensibleCapacityIP($T78,$W78,activeRoomTempCooling,activePriAirTempCooling,$Y78,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T78=\"Select Model\",\"\",IF($T78=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y78,activeElevation)))","v":""},{"$f":"IF(OR(T78=\"Select Model\",T78=\"PCBL\"), 0,IF(AD78=0,0,-primaryAirSensibleCapacityIP($T78,$W78,activeRoomTempHeating,activePriAirTempHeating,$Y78,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T78=\"Select Model\", \"\", InductionRatio($T78,BD78,$W78,$Y78)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T78=\"Select Model\", \"\",IF($T78=\"PCBL\",\"N/A\",minVAVSetBack(AA78, Y78))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T78=\"Select Model\", \"\",IF($T78= \"PCBL\",\"N/A\",getDischargeAirTemp($T78,$V78,$AC78,$W78,BD78,$AL78, $Y78, $AS78, \"cooling\",activeElevation,$AB78,$AJ78,$AV78,$BB78))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T78=\"Select Model\",$T78=\"PCBL\"), \"\",getDischargeAirTemp($T78,$V78,$AD78,$W78,BD78,$AL78, $Y78, $AY78, \"heating\",activeElevation,$AB78,$AJ78,$AV78,$BB78)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T78=\"Select Model\", \"\",IF(OR($T78=\"ACBC_1W\",$T78=\"ACBC_2W\",LEFT($T78,4)=\"ACBR\",$T78 = \"LIU24_2W\",LEFT($T78,3)=\"RIU\",LEFT($T78,6)=\"ACBL12\"), IF((soundLevel($T78, $AB78, BD78, $Y78, $W78,$AJ78,$AA78,\"dba\"))<15,\"<15\",soundLevel($T78, $AB78, BD78, $Y78, $W78,$AJ78,$AA78,\"dba\")+0.4),IF((soundLevel($T78, $AB78, BD78, $Y78, $W78,$AJ78,$AA78,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T78, $AB78, BD78, $Y78, $W78,$AJ78,$AA78,\"dba\")+5)<15, \"<15\", soundLevel($T78, $AB78, BD78,$Y78, $W78,$AJ78,$AA78,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T78=\"Select Model\", \"\",IF(OR($T78=\"ACBC_1W\",$T78=\"ACBC_2W\",LEFT($T78,4)=\"ACBR\",$T78=\"LIU24_2W\",LEFT($T78,3)=\"RIU\",LEFT($T78,6)=\"ACBL12\"), IF((soundLevel($T78, $AB78, BD78, $Y78, $W78,$AJ78,$AA78,\"NC\"))<15,\"<15\",soundLevel($T78, $AB78, BD78, $Y78, $W78,$AJ78,$AA78,\"NC\")+0.4),IF((soundLevel($T78, $AB78, BD78, $Y78, $W78,$AJ78,$AA78,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T78, $AB78, BD78, $Y78, $W78,$AJ78,$AA78,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T78, $AB78, BD78, $Y78, $W78,$AJ78,$AA78,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T78=\"Select Model\",\"\",IF($T78=\"LIU24_2W\",calcQwIP($Y78,$W78,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC78,$AI78,\"latent\",$U78&\"P\"&IF($V78=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T78,activeElevation),\"\"))","v":""},{"$f":"IF($T78=\"Select Model\",\"\",IF($T78=\"ACBC_1W\",calcQwIP($Y78,$W78,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC78,BD78,\"capacity\",$U78&\"P\"&IF($V78=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T78,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y78,$W78,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC78,BD78,\"capacity\",$U78&\"P\"&IF($V78=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T78,activeElevation)))","v":""},"",{"$f":"IF(T78=\"Select Model\", 0,waterPressureDrop(W78, U78 & \"P\" & IF(V78=\"Dual\",2,1) &\"C\", AC78, \"cooling\", T78))","v":0},{"$f":"IF(T78=\"Select Model\", \"\",getReturnWaterTemp(T78,AC78, activeEWTCooling, AS78, \"cooling\"))","v":""},"",{"$f":"IF($T78<>\"ACBC_1W\",\"\",IF($J78=\"\",\"\",FintubeCapacity($T78,$W78,$AE78,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T78=\"Select Model\",T78=\"PCBL\"),\"\",calcQwIP(Y78,W78,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD78,BD78,\"capacity\",U78&\"P\"&IF(V78=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T78,activeElevation))","v":""},"",{"$f":"IF(OR(T78=\"Select Model\",T78=\"PCBL\"), \"\",IF(AY78=0,\"N/A\",waterPressureDrop(W78, U78 & \"P\" & IF(V78=\"Dual\",2,1) &\"C\", AD78, \"heating\", T78)))","v":""},{"$f":"IF(OR(T78=\"Select Model\",T78=\"PCBL\"), \"\",IF(AY78=0,getReturnWaterTemp(T78,AE78, activeEWTHeating, AX78, \"heating\"),getReturnWaterTemp(T78,AD78, activeEWTHeating, AY78, \"heating\")))","v":""},"",{"$f":" getNozzle(T78, W78, Y78, Z78, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I79)),I79<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I79, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H79)),H79<0),\"\",intlEstQuantity(T79, W79*12, H79)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T79=\"Select Model\",\"\",coilCircuitChange(W79, U79, AC79, T79,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T79=\"Select Model\",\"\",beamWidth(T79))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T79=\"Select Model\",T79=\"PCBL\"), 0,getSPIP(T79, W79, Y79, BD79, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T79=\"Select Model\", \"\",IF(T79=\"PCBL\",0,primaryAirSensibleCapacityIP($T79,$W79,activeRoomTempCooling,activePriAirTempCooling,$Y79,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T79=\"Select Model\",\"\",IF($T79=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y79,activeElevation)))","v":""},{"$f":"IF(OR(T79=\"Select Model\",T79=\"PCBL\"), 0,IF(AD79=0,0,-primaryAirSensibleCapacityIP($T79,$W79,activeRoomTempHeating,activePriAirTempHeating,$Y79,activeElevation,\"heating\")))","v":0},{"$f":"getCurrentNozzleCode(T79, W79, Y79, Z79, activeElevation, TRUE)","v":""},{"$f":"IFERROR(IF(T79=\"Select Model\", \"\", InductionRatio($T79,BD79,$W79,$Y79)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T79=\"Select Model\", \"\",IF($T79=\"PCBL\",\"N/A\",minVAVSetBack(AA79, Y79))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T79=\"Select Model\", \"\",IF($T79= \"PCBL\",\"N/A\",getDischargeAirTemp($T79,$V79,$AC79,$W79,BD79,$AL79, $Y79, $AS79, \"cooling\",activeElevation,$AB79,$AJ79,$AV79,$BB79))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T79=\"Select Model\",$T79=\"PCBL\"), \"\",getDischargeAirTemp($T79,$V79,$AD79,$W79,BD79,$AL79, $Y79, $AY79, \"heating\",activeElevation,$AB79,$AJ79,$AV79,$BB79)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T79=\"Select Model\", \"\",IF(OR($T79=\"ACBC_1W\",$T79=\"ACBC_2W\",LEFT($T79,4)=\"ACBR\",$T79 = \"LIU24_2W\",LEFT($T79,3)=\"RIU\",LEFT($T79,6)=\"ACBL12\"), IF((soundLevel($T79, $AB79, BD79, $Y79, $W79,$AJ79,$AA79,\"dba\"))<15,\"<15\",soundLevel($T79, $AB79, BD79, $Y79, $W79,$AJ79,$AA79,\"dba\")+0.4),IF((soundLevel($T79, $AB79, BD79, $Y79, $W79,$AJ79,$AA79,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T79, $AB79, BD79, $Y79, $W79,$AJ79,$AA79,\"dba\")+5)<15, \"<15\", soundLevel($T79, $AB79, BD79,$Y79, $W79,$AJ79,$AA79,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T79=\"Select Model\", \"\",IF(OR($T79=\"ACBC_1W\",$T79=\"ACBC_2W\",LEFT($T79,4)=\"ACBR\",$T79=\"LIU24_2W\",LEFT($T79,3)=\"RIU\",LEFT($T79,6)=\"ACBL12\"), IF((soundLevel($T79, $AB79, BD79, $Y79, $W79,$AJ79,$AA79,\"NC\"))<15,\"<15\",soundLevel($T79, $AB79, BD79, $Y79, $W79,$AJ79,$AA79,\"NC\")+0.4),IF((soundLevel($T79, $AB79, BD79, $Y79, $W79,$AJ79,$AA79,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T79, $AB79, BD79, $Y79, $W79,$AJ79,$AA79,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T79, $AB79, BD79, $Y79, $W79,$AJ79,$AA79,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T79=\"Select Model\",\"\",IF($T79=\"LIU24_2W\",calcQwIP($Y79,$W79,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC79,$AI79,\"latent\",$U79&\"P\"&IF($V79=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T79,activeElevation),\"\"))","v":""},{"$f":"IF($T79=\"Select Model\",\"\",IF($T79=\"ACBC_1W\",calcQwIP($Y79,$W79,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC79,BD79,\"capacity\",$U79&\"P\"&IF($V79=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T79,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y79,$W79,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC79,BD79,\"capacity\",$U79&\"P\"&IF($V79=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T79,activeElevation)))","v":""},"",{"$f":"IF(T79=\"Select Model\", 0,waterPressureDrop(W79, U79 & \"P\" & IF(V79=\"Dual\",2,1) &\"C\", AC79, \"cooling\", T79))","v":0},{"$f":"IF(T79=\"Select Model\", \"\",getReturnWaterTemp(T79,AC79, activeEWTCooling, AS79, \"cooling\"))","v":""},"",{"$f":"IF($T79<>\"ACBC_1W\",\"\",IF($J79=\"\",\"\",FintubeCapacity($T79,$W79,$AE79,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T79=\"Select Model\",T79=\"PCBL\"),\"\",calcQwIP(Y79,W79,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD79,BD79,\"capacity\",U79&\"P\"&IF(V79=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T79,activeElevation))","v":""},"",{"$f":"IF(OR(T79=\"Select Model\",T79=\"PCBL\"), \"\",IF(AY79=0,\"N/A\",waterPressureDrop(W79, U79 & \"P\" & IF(V79=\"Dual\",2,1) &\"C\", AD79, \"heating\", T79)))","v":""},{"$f":"IF(OR(T79=\"Select Model\",T79=\"PCBL\"), \"\",IF(AY79=0,getReturnWaterTemp(T79,AE79, activeEWTHeating, AX79, \"heating\"),getReturnWaterTemp(T79,AD79, activeEWTHeating, AY79, \"heating\")))","v":""},"",{"$f":" getNozzle(T79, W79, Y79, Z79, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I80)),I80<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I80, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H80)),H80<0),\"\",intlEstQuantity(T80, W80*12, H80)),1)","v":""},{"$f":"IF(LEFT(T80, 4)=\"ACBC\",IF(AND(ISNUMBER(L80),ISNUMBER(AT80)),IF(AA80=-1,\"LOW CFM\",L80*AT80),\"\"),IF(AND(ISNUMBER(L80),ISNUMBER(AT80)),IF(AA80=-1,\"N/A CFM\",L80*AT80),\"\"))","v":""},{"$f":"IF(LEFT(T80,4)=\"ACBC\",IF(AND(ISNUMBER(L80),ISNUMBER(AG80)),IF(AA80=-1,\"LOW CFM\",L80*AG80),\"\"),IF(AND(ISNUMBER(L80),ISNUMBER(AG80)),IF(AA80=-1,\"N/A CFM\",L80*AG80),\"\"))","v":""},{"$f":"IF(LEFT(T80,4)=\"ACBC\",IF(AND(ISNUMBER(L80),ISNUMBER(AZ80)),IF(AA80=-1,\"LOW CFM\",L80*AZ80),\"\"),IF(AND(ISNUMBER(L80),ISNUMBER(AZ80)),IF(AA80=-1,\"N/A CFM\",L80*AZ80),\"\"))","v":""},{"$f":"IF(AND(ISNUMBER(L80),ISNUMBER(Y80)),L80*Y80,\"\")","v":""},{"$f":"IF(AND(ISNUMBER(L80),ISNUMBER(AC80)),L80*AC80,\"\")","v":""},{"$f":"IF(AND(ISNUMBER(L80),ISNUMBER(AD80)),IF(AND(T80=\"ACBC_1W\",AD80=0),AE80*L80,L80*AD80))","v":false},"Default","Select Model",2,{"$f":"IF(T80=\"Select Model\",\"\",coilCircuitChange(W80, U80, AC80, T80,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T80=\"Select Model\",\"\",beamWidth(T80))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T80=\"Select Model\",T80=\"PCBL\"), 0,getSPIP(T80, W80, Y80, BD80, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T80=\"Select Model\", \"\",IF(T80=\"PCBL\",0,primaryAirSensibleCapacityIP($T80,$W80,activeRoomTempCooling,activePriAirTempCooling,$Y80,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T80=\"Select Model\",\"\",IF($T80=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y80,activeElevation)))","v":""},{"$f":"IF(OR(T80=\"Select Model\",T80=\"PCBL\"), 0,IF(AD80=0,0,-primaryAirSensibleCapacityIP($T80,$W80,activeRoomTempHeating,activePriAirTempHeating,$Y80,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T80=\"Select Model\", \"\", InductionRatio($T80,BD80,$W80,$Y80)),\"N/A\")","v":""},{"$f":"IFERROR(AT80/Y80,\"\")","v":""},{"$f":"IFERROR(IF(T80=\"Select Model\", \"\",(1+AJ80)*Y80),\"N/A\")","v":""},{"$f":"IFERROR(IF(T80=\"Select Model\", \"\",IF($T80=\"PCBL\",\"N/A\",minVAVSetBack(AA80, Y80))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T80=\"Select Model\", \"\",IF($T80= \"PCBL\",\"N/A\",getDischargeAirTemp($T80,$V80,$AC80,$W80,BD80,$AL80, $Y80, $AS80, \"cooling\",activeElevation,$AB80,$AJ80,$AV80,$BB80))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T80=\"Select Model\",$T80=\"PCBL\"), \"\",getDischargeAirTemp($T80,$V80,$AD80,$W80,BD80,$AL80, $Y80, $AY80, \"heating\",activeElevation,$AB80,$AJ80,$AV80,$BB80)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T80=\"Select Model\", \"\",IF(OR($T80=\"ACBC_1W\",$T80=\"ACBC_2W\",LEFT($T80,4)=\"ACBR\",$T80 = \"LIU24_2W\",LEFT($T80,3)=\"RIU\",LEFT($T80,6)=\"ACBL12\"), IF((soundLevel($T80, $AB80, BD80, $Y80, $W80,$AJ80,$AA80,\"dba\"))<15,\"<15\",soundLevel($T80, $AB80, BD80, $Y80, $W80,$AJ80,$AA80,\"dba\")+0.4),IF((soundLevel($T80, $AB80, BD80, $Y80, $W80,$AJ80,$AA80,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T80, $AB80, BD80, $Y80, $W80,$AJ80,$AA80,\"dba\")+5)<15, \"<15\", soundLevel($T80, $AB80, BD80,$Y80, $W80,$AJ80,$AA80,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T80=\"Select Model\", \"\",IF(OR($T80=\"ACBC_1W\",$T80=\"ACBC_2W\",LEFT($T80,4)=\"ACBR\",$T80=\"LIU24_2W\",LEFT($T80,3)=\"RIU\",LEFT($T80,6)=\"ACBL12\"), IF((soundLevel($T80, $AB80, BD80, $Y80, $W80,$AJ80,$AA80,\"NC\"))<15,\"<15\",soundLevel($T80, $AB80, BD80, $Y80, $W80,$AJ80,$AA80,\"NC\")+0.4),IF((soundLevel($T80, $AB80, BD80, $Y80, $W80,$AJ80,$AA80,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T80, $AB80, BD80, $Y80, $W80,$AJ80,$AA80,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T80, $AB80, BD80, $Y80, $W80,$AJ80,$AA80,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T80=\"Select Model\",\"\",IF($T80=\"LIU24_2W\",calcQwIP($Y80,$W80,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC80,$AI80,\"latent\",$U80&\"P\"&IF($V80=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T80,activeElevation),\"\"))","v":""},{"$f":"IF($T80=\"Select Model\",\"\",IF($T80=\"ACBC_1W\",calcQwIP($Y80,$W80,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC80,BD80,\"capacity\",$U80&\"P\"&IF($V80=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T80,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y80,$W80,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC80,BD80,\"capacity\",$U80&\"P\"&IF($V80=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T80,activeElevation)))","v":""},{"$f":"IF(T80=\"Select Model\", \"\",IF(T80 = \"LIU24_2W\", AS80+AF80+AR80, AS80+AF80))","v":""},{"$f":"IF(T80=\"Select Model\", 0,waterPressureDrop(W80, U80 & \"P\" & IF(V80=\"Dual\",2,1) &\"C\", AC80, \"cooling\", T80))","v":0},{"$f":"IF(T80=\"Select Model\", \"\",getReturnWaterTemp(T80,AC80, activeEWTCooling, AS80, \"cooling\"))","v":""},{"$f":"IF(T80=\"Select Model\", \"\",$AV80-activeEWTCooling)","v":""},{"$f":"IF($T80<>\"ACBC_1W\",\"\",IF($J80=\"\",\"\",FintubeCapacity($T80,$W80,$AE80,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T80=\"Select Model\",T80=\"PCBL\"),\"\",calcQwIP(Y80,W80,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD80,BD80,\"capacity\",U80&\"P\"&IF(V80=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T80,activeElevation))","v":""},{"$f":"IF(OR(T80=\"Select Model\",T80=\"PCBL\"),\"\",IF(AND(AD80=0,T80=\"ACBC_1W\"),AX80+AH80,AY80+AH80))","v":""},{"$f":"IF(OR(T80=\"Select Model\",T80=\"PCBL\"), \"\",IF(AY80=0,\"N/A\",waterPressureDrop(W80, U80 & \"P\" & IF(V80=\"Dual\",2,1) &\"C\", AD80, \"heating\", T80)))","v":""},{"$f":"IF(OR(T80=\"Select Model\",T80=\"PCBL\"), \"\",IF(AY80=0,getReturnWaterTemp(T80,AE80, activeEWTHeating, AX80, \"heating\"),getReturnWaterTemp(T80,AD80, activeEWTHeating, AY80, \"heating\")))","v":""},{"$f":"IF(OR($T80=\"Select Model\",$J80=\"\",T80=\"PCBL\"), \"\",activeEWTHeating-$BB80)","v":""},{"$f":" getNozzle(T80, W80, Y80, Z80, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I81)),I81<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I81, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H81)),H81<0),\"\",intlEstQuantity(T81, W81*12, H81)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T81=\"Select Model\",\"\",coilCircuitChange(W81, U81, AC81, T81,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T81=\"Select Model\",\"\",beamWidth(T81))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T81=\"Select Model\",T81=\"PCBL\"), 0,getSPIP(T81, W81, Y81, BD81, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T81=\"Select Model\", \"\",IF(T81=\"PCBL\",0,primaryAirSensibleCapacityIP($T81,$W81,activeRoomTempCooling,activePriAirTempCooling,$Y81,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T81=\"Select Model\",\"\",IF($T81=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y81,activeElevation)))","v":""},{"$f":"IF(OR(T81=\"Select Model\",T81=\"PCBL\"), 0,IF(AD81=0,0,-primaryAirSensibleCapacityIP($T81,$W81,activeRoomTempHeating,activePriAirTempHeating,$Y81,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T81=\"Select Model\", \"\", InductionRatio($T81,BD81,$W81,$Y81)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T81=\"Select Model\", \"\",IF($T81=\"PCBL\",\"N/A\",minVAVSetBack(AA81, Y81))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T81=\"Select Model\", \"\",IF($T81= \"PCBL\",\"N/A\",getDischargeAirTemp($T81,$V81,$AC81,$W81,BD81,$AL81, $Y81, $AS81, \"cooling\",activeElevation,$AB81,$AJ81,$AV81,$BB81))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T81=\"Select Model\",$T81=\"PCBL\"), \"\",getDischargeAirTemp($T81,$V81,$AD81,$W81,BD81,$AL81, $Y81, $AY81, \"heating\",activeElevation,$AB81,$AJ81,$AV81,$BB81)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T81=\"Select Model\", \"\",IF(OR($T81=\"ACBC_1W\",$T81=\"ACBC_2W\",LEFT($T81,4)=\"ACBR\",$T81 = \"LIU24_2W\",LEFT($T81,3)=\"RIU\",LEFT($T81,6)=\"ACBL12\"), IF((soundLevel($T81, $AB81, BD81, $Y81, $W81,$AJ81,$AA81,\"dba\"))<15,\"<15\",soundLevel($T81, $AB81, BD81, $Y81, $W81,$AJ81,$AA81,\"dba\")+0.4),IF((soundLevel($T81, $AB81, BD81, $Y81, $W81,$AJ81,$AA81,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T81, $AB81, BD81, $Y81, $W81,$AJ81,$AA81,\"dba\")+5)<15, \"<15\", soundLevel($T81, $AB81, BD81,$Y81, $W81,$AJ81,$AA81,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T81=\"Select Model\", \"\",IF(OR($T81=\"ACBC_1W\",$T81=\"ACBC_2W\",LEFT($T81,4)=\"ACBR\",$T81=\"LIU24_2W\",LEFT($T81,3)=\"RIU\",LEFT($T81,6)=\"ACBL12\"), IF((soundLevel($T81, $AB81, BD81, $Y81, $W81,$AJ81,$AA81,\"NC\"))<15,\"<15\",soundLevel($T81, $AB81, BD81, $Y81, $W81,$AJ81,$AA81,\"NC\")+0.4),IF((soundLevel($T81, $AB81, BD81, $Y81, $W81,$AJ81,$AA81,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T81, $AB81, BD81, $Y81, $W81,$AJ81,$AA81,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T81, $AB81, BD81, $Y81, $W81,$AJ81,$AA81,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T81=\"Select Model\",\"\",IF($T81=\"LIU24_2W\",calcQwIP($Y81,$W81,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC81,$AI81,\"latent\",$U81&\"P\"&IF($V81=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T81,activeElevation),\"\"))","v":""},{"$f":"IF($T81=\"Select Model\",\"\",IF($T81=\"ACBC_1W\",calcQwIP($Y81,$W81,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC81,BD81,\"capacity\",$U81&\"P\"&IF($V81=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T81,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y81,$W81,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC81,BD81,\"capacity\",$U81&\"P\"&IF($V81=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T81,activeElevation)))","v":""},"",{"$f":"IF(T81=\"Select Model\", 0,waterPressureDrop(W81, U81 & \"P\" & IF(V81=\"Dual\",2,1) &\"C\", AC81, \"cooling\", T81))","v":0},{"$f":"IF(T81=\"Select Model\", \"\",getReturnWaterTemp(T81,AC81, activeEWTCooling, AS81, \"cooling\"))","v":""},"",{"$f":"IF($T81<>\"ACBC_1W\",\"\",IF($J81=\"\",\"\",FintubeCapacity($T81,$W81,$AE81,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T81=\"Select Model\",T81=\"PCBL\"),\"\",calcQwIP(Y81,W81,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD81,BD81,\"capacity\",U81&\"P\"&IF(V81=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T81,activeElevation))","v":""},"",{"$f":"IF(OR(T81=\"Select Model\",T81=\"PCBL\"), \"\",IF(AY81=0,\"N/A\",waterPressureDrop(W81, U81 & \"P\" & IF(V81=\"Dual\",2,1) &\"C\", AD81, \"heating\", T81)))","v":""},{"$f":"IF(OR(T81=\"Select Model\",T81=\"PCBL\"), \"\",IF(AY81=0,getReturnWaterTemp(T81,AE81, activeEWTHeating, AX81, \"heating\"),getReturnWaterTemp(T81,AD81, activeEWTHeating, AY81, \"heating\")))","v":""},"",{"$f":" getNozzle(T81, W81, Y81, Z81, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I82)),I82<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I82, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H82)),H82<0),\"\",intlEstQuantity(T82, W82*12, H82)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T82=\"Select Model\",\"\",coilCircuitChange(W82, U82, AC82, T82,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T82=\"Select Model\",\"\",beamWidth(T82))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T82=\"Select Model\",T82=\"PCBL\"), 0,getSPIP(T82, W82, Y82, BD82, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T82=\"Select Model\", \"\",IF(T82=\"PCBL\",0,primaryAirSensibleCapacityIP($T82,$W82,activeRoomTempCooling,activePriAirTempCooling,$Y82,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T82=\"Select Model\",\"\",IF($T82=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y82,activeElevation)))","v":""},{"$f":"IF(OR(T82=\"Select Model\",T82=\"PCBL\"), 0,IF(AD82=0,0,-primaryAirSensibleCapacityIP($T82,$W82,activeRoomTempHeating,activePriAirTempHeating,$Y82,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T82=\"Select Model\", \"\", InductionRatio($T82,BD82,$W82,$Y82)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T82=\"Select Model\", \"\",IF($T82=\"PCBL\",\"N/A\",minVAVSetBack(AA82, Y82))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T82=\"Select Model\", \"\",IF($T82= \"PCBL\",\"N/A\",getDischargeAirTemp($T82,$V82,$AC82,$W82,BD82,$AL82, $Y82, $AS82, \"cooling\",activeElevation,$AB82,$AJ82,$AV82,$BB82))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T82=\"Select Model\",$T82=\"PCBL\"), \"\",getDischargeAirTemp($T82,$V82,$AD82,$W82,BD82,$AL82, $Y82, $AY82, \"heating\",activeElevation,$AB82,$AJ82,$AV82,$BB82)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T82=\"Select Model\", \"\",IF(OR($T82=\"ACBC_1W\",$T82=\"ACBC_2W\",LEFT($T82,4)=\"ACBR\",$T82 = \"LIU24_2W\",LEFT($T82,3)=\"RIU\",LEFT($T82,6)=\"ACBL12\"), IF((soundLevel($T82, $AB82, BD82, $Y82, $W82,$AJ82,$AA82,\"dba\"))<15,\"<15\",soundLevel($T82, $AB82, BD82, $Y82, $W82,$AJ82,$AA82,\"dba\")+0.4),IF((soundLevel($T82, $AB82, BD82, $Y82, $W82,$AJ82,$AA82,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T82, $AB82, BD82, $Y82, $W82,$AJ82,$AA82,\"dba\")+5)<15, \"<15\", soundLevel($T82, $AB82, BD82,$Y82, $W82,$AJ82,$AA82,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T82=\"Select Model\", \"\",IF(OR($T82=\"ACBC_1W\",$T82=\"ACBC_2W\",LEFT($T82,4)=\"ACBR\",$T82=\"LIU24_2W\",LEFT($T82,3)=\"RIU\",LEFT($T82,6)=\"ACBL12\"), IF((soundLevel($T82, $AB82, BD82, $Y82, $W82,$AJ82,$AA82,\"NC\"))<15,\"<15\",soundLevel($T82, $AB82, BD82, $Y82, $W82,$AJ82,$AA82,\"NC\")+0.4),IF((soundLevel($T82, $AB82, BD82, $Y82, $W82,$AJ82,$AA82,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T82, $AB82, BD82, $Y82, $W82,$AJ82,$AA82,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T82, $AB82, BD82, $Y82, $W82,$AJ82,$AA82,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T82=\"Select Model\",\"\",IF($T82=\"LIU24_2W\",calcQwIP($Y82,$W82,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC82,$AI82,\"latent\",$U82&\"P\"&IF($V82=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T82,activeElevation),\"\"))","v":""},{"$f":"IF($T82=\"Select Model\",\"\",IF($T82=\"ACBC_1W\",calcQwIP($Y82,$W82,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC82,BD82,\"capacity\",$U82&\"P\"&IF($V82=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T82,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y82,$W82,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC82,BD82,\"capacity\",$U82&\"P\"&IF($V82=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T82,activeElevation)))","v":""},"",{"$f":"IF(T82=\"Select Model\", 0,waterPressureDrop(W82, U82 & \"P\" & IF(V82=\"Dual\",2,1) &\"C\", AC82, \"cooling\", T82))","v":0},{"$f":"IF(T82=\"Select Model\", \"\",getReturnWaterTemp(T82,AC82, activeEWTCooling, AS82, \"cooling\"))","v":""},"",{"$f":"IF($T82<>\"ACBC_1W\",\"\",IF($J82=\"\",\"\",FintubeCapacity($T82,$W82,$AE82,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T82=\"Select Model\",T82=\"PCBL\"),\"\",calcQwIP(Y82,W82,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD82,BD82,\"capacity\",U82&\"P\"&IF(V82=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T82,activeElevation))","v":""},"",{"$f":"IF(OR(T82=\"Select Model\",T82=\"PCBL\"), \"\",IF(AY82=0,\"N/A\",waterPressureDrop(W82, U82 & \"P\" & IF(V82=\"Dual\",2,1) &\"C\", AD82, \"heating\", T82)))","v":""},{"$f":"IF(OR(T82=\"Select Model\",T82=\"PCBL\"), \"\",IF(AY82=0,getReturnWaterTemp(T82,AE82, activeEWTHeating, AX82, \"heating\"),getReturnWaterTemp(T82,AD82, activeEWTHeating, AY82, \"heating\")))","v":""},"",{"$f":" getNozzle(T82, W82, Y82, Z82, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I83)),I83<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I83, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H83)),H83<0),\"\",intlEstQuantity(T83, W83*12, H83)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T83=\"Select Model\",\"\",coilCircuitChange(W83, U83, AC83, T83,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T83=\"Select Model\",\"\",beamWidth(T83))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T83=\"Select Model\",T83=\"PCBL\"), 0,getSPIP(T83, W83, Y83, BD83, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T83=\"Select Model\", \"\",IF(T83=\"PCBL\",0,primaryAirSensibleCapacityIP($T83,$W83,activeRoomTempCooling,activePriAirTempCooling,$Y83,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T83=\"Select Model\",\"\",IF($T83=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y83,activeElevation)))","v":""},{"$f":"IF(OR(T83=\"Select Model\",T83=\"PCBL\"), 0,IF(AD83=0,0,-primaryAirSensibleCapacityIP($T83,$W83,activeRoomTempHeating,activePriAirTempHeating,$Y83,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T83=\"Select Model\", \"\", InductionRatio($T83,BD83,$W83,$Y83)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T83=\"Select Model\", \"\",IF($T83=\"PCBL\",\"N/A\",minVAVSetBack(AA83, Y83))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T83=\"Select Model\", \"\",IF($T83= \"PCBL\",\"N/A\",getDischargeAirTemp($T83,$V83,$AC83,$W83,BD83,$AL83, $Y83, $AS83, \"cooling\",activeElevation,$AB83,$AJ83,$AV83,$BB83))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T83=\"Select Model\",$T83=\"PCBL\"), \"\",getDischargeAirTemp($T83,$V83,$AD83,$W83,BD83,$AL83, $Y83, $AY83, \"heating\",activeElevation,$AB83,$AJ83,$AV83,$BB83)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T83=\"Select Model\", \"\",IF(OR($T83=\"ACBC_1W\",$T83=\"ACBC_2W\",LEFT($T83,4)=\"ACBR\",$T83 = \"LIU24_2W\",LEFT($T83,3)=\"RIU\",LEFT($T83,6)=\"ACBL12\"), IF((soundLevel($T83, $AB83, BD83, $Y83, $W83,$AJ83,$AA83,\"dba\"))<15,\"<15\",soundLevel($T83, $AB83, BD83, $Y83, $W83,$AJ83,$AA83,\"dba\")+0.4),IF((soundLevel($T83, $AB83, BD83, $Y83, $W83,$AJ83,$AA83,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T83, $AB83, BD83, $Y83, $W83,$AJ83,$AA83,\"dba\")+5)<15, \"<15\", soundLevel($T83, $AB83, BD83,$Y83, $W83,$AJ83,$AA83,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T83=\"Select Model\", \"\",IF(OR($T83=\"ACBC_1W\",$T83=\"ACBC_2W\",LEFT($T83,4)=\"ACBR\",$T83=\"LIU24_2W\",LEFT($T83,3)=\"RIU\",LEFT($T83,6)=\"ACBL12\"), IF((soundLevel($T83, $AB83, BD83, $Y83, $W83,$AJ83,$AA83,\"NC\"))<15,\"<15\",soundLevel($T83, $AB83, BD83, $Y83, $W83,$AJ83,$AA83,\"NC\")+0.4),IF((soundLevel($T83, $AB83, BD83, $Y83, $W83,$AJ83,$AA83,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T83, $AB83, BD83, $Y83, $W83,$AJ83,$AA83,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T83, $AB83, BD83, $Y83, $W83,$AJ83,$AA83,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T83=\"Select Model\",\"\",IF($T83=\"LIU24_2W\",calcQwIP($Y83,$W83,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC83,$AI83,\"latent\",$U83&\"P\"&IF($V83=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T83,activeElevation),\"\"))","v":""},{"$f":"IF($T83=\"Select Model\",\"\",IF($T83=\"ACBC_1W\",calcQwIP($Y83,$W83,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC83,BD83,\"capacity\",$U83&\"P\"&IF($V83=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T83,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y83,$W83,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC83,BD83,\"capacity\",$U83&\"P\"&IF($V83=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T83,activeElevation)))","v":""},"",{"$f":"IF(T83=\"Select Model\", 0,waterPressureDrop(W83, U83 & \"P\" & IF(V83=\"Dual\",2,1) &\"C\", AC83, \"cooling\", T83))","v":0},{"$f":"IF(T83=\"Select Model\", \"\",getReturnWaterTemp(T83,AC83, activeEWTCooling, AS83, \"cooling\"))","v":""},"",{"$f":"IF($T83<>\"ACBC_1W\",\"\",IF($J83=\"\",\"\",FintubeCapacity($T83,$W83,$AE83,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T83=\"Select Model\",T83=\"PCBL\"),\"\",calcQwIP(Y83,W83,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD83,BD83,\"capacity\",U83&\"P\"&IF(V83=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T83,activeElevation))","v":""},"",{"$f":"IF(OR(T83=\"Select Model\",T83=\"PCBL\"), \"\",IF(AY83=0,\"N/A\",waterPressureDrop(W83, U83 & \"P\" & IF(V83=\"Dual\",2,1) &\"C\", AD83, \"heating\", T83)))","v":""},{"$f":"IF(OR(T83=\"Select Model\",T83=\"PCBL\"), \"\",IF(AY83=0,getReturnWaterTemp(T83,AE83, activeEWTHeating, AX83, \"heating\"),getReturnWaterTemp(T83,AD83, activeEWTHeating, AY83, \"heating\")))","v":""},"",{"$f":" getNozzle(T83, W83, Y83, Z83, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I84)),I84<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I84, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H84)),H84<0),\"\",intlEstQuantity(T84, W84*12, H84)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T84=\"Select Model\",\"\",coilCircuitChange(W84, U84, AC84, T84,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T84=\"Select Model\",\"\",beamWidth(T84))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T84=\"Select Model\",T84=\"PCBL\"), 0,getSPIP(T84, W84, Y84, BD84, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T84=\"Select Model\", \"\",IF(T84=\"PCBL\",0,primaryAirSensibleCapacityIP($T84,$W84,activeRoomTempCooling,activePriAirTempCooling,$Y84,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T84=\"Select Model\",\"\",IF($T84=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y84,activeElevation)))","v":""},{"$f":"IF(OR(T84=\"Select Model\",T84=\"PCBL\"), 0,IF(AD84=0,0,-primaryAirSensibleCapacityIP($T84,$W84,activeRoomTempHeating,activePriAirTempHeating,$Y84,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T84=\"Select Model\", \"\", InductionRatio($T84,BD84,$W84,$Y84)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T84=\"Select Model\", \"\",IF($T84=\"PCBL\",\"N/A\",minVAVSetBack(AA84, Y84))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T84=\"Select Model\", \"\",IF($T84= \"PCBL\",\"N/A\",getDischargeAirTemp($T84,$V84,$AC84,$W84,BD84,$AL84, $Y84, $AS84, \"cooling\",activeElevation,$AB84,$AJ84,$AV84,$BB84))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T84=\"Select Model\",$T84=\"PCBL\"), \"\",getDischargeAirTemp($T84,$V84,$AD84,$W84,BD84,$AL84, $Y84, $AY84, \"heating\",activeElevation,$AB84,$AJ84,$AV84,$BB84)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T84=\"Select Model\", \"\",IF(OR($T84=\"ACBC_1W\",$T84=\"ACBC_2W\",LEFT($T84,4)=\"ACBR\",$T84 = \"LIU24_2W\",LEFT($T84,3)=\"RIU\",LEFT($T84,6)=\"ACBL12\"), IF((soundLevel($T84, $AB84, BD84, $Y84, $W84,$AJ84,$AA84,\"dba\"))<15,\"<15\",soundLevel($T84, $AB84, BD84, $Y84, $W84,$AJ84,$AA84,\"dba\")+0.4),IF((soundLevel($T84, $AB84, BD84, $Y84, $W84,$AJ84,$AA84,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T84, $AB84, BD84, $Y84, $W84,$AJ84,$AA84,\"dba\")+5)<15, \"<15\", soundLevel($T84, $AB84, BD84,$Y84, $W84,$AJ84,$AA84,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T84=\"Select Model\", \"\",IF(OR($T84=\"ACBC_1W\",$T84=\"ACBC_2W\",LEFT($T84,4)=\"ACBR\",$T84=\"LIU24_2W\",LEFT($T84,3)=\"RIU\",LEFT($T84,6)=\"ACBL12\"), IF((soundLevel($T84, $AB84, BD84, $Y84, $W84,$AJ84,$AA84,\"NC\"))<15,\"<15\",soundLevel($T84, $AB84, BD84, $Y84, $W84,$AJ84,$AA84,\"NC\")+0.4),IF((soundLevel($T84, $AB84, BD84, $Y84, $W84,$AJ84,$AA84,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T84, $AB84, BD84, $Y84, $W84,$AJ84,$AA84,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T84, $AB84, BD84, $Y84, $W84,$AJ84,$AA84,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T84=\"Select Model\",\"\",IF($T84=\"LIU24_2W\",calcQwIP($Y84,$W84,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC84,$AI84,\"latent\",$U84&\"P\"&IF($V84=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T84,activeElevation),\"\"))","v":""},{"$f":"IF($T84=\"Select Model\",\"\",IF($T84=\"ACBC_1W\",calcQwIP($Y84,$W84,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC84,BD84,\"capacity\",$U84&\"P\"&IF($V84=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T84,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y84,$W84,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC84,BD84,\"capacity\",$U84&\"P\"&IF($V84=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T84,activeElevation)))","v":""},"",{"$f":"IF(T84=\"Select Model\", 0,waterPressureDrop(W84, U84 & \"P\" & IF(V84=\"Dual\",2,1) &\"C\", AC84, \"cooling\", T84))","v":0},{"$f":"IF(T84=\"Select Model\", \"\",getReturnWaterTemp(T84,AC84, activeEWTCooling, AS84, \"cooling\"))","v":""},"",{"$f":"IF($T84<>\"ACBC_1W\",\"\",IF($J84=\"\",\"\",FintubeCapacity($T84,$W84,$AE84,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T84=\"Select Model\",T84=\"PCBL\"),\"\",calcQwIP(Y84,W84,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD84,BD84,\"capacity\",U84&\"P\"&IF(V84=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T84,activeElevation))","v":""},"",{"$f":"IF(OR(T84=\"Select Model\",T84=\"PCBL\"), \"\",IF(AY84=0,\"N/A\",waterPressureDrop(W84, U84 & \"P\" & IF(V84=\"Dual\",2,1) &\"C\", AD84, \"heating\", T84)))","v":""},{"$f":"IF(OR(T84=\"Select Model\",T84=\"PCBL\"), \"\",IF(AY84=0,getReturnWaterTemp(T84,AE84, activeEWTHeating, AX84, \"heating\"),getReturnWaterTemp(T84,AD84, activeEWTHeating, AY84, \"heating\")))","v":""},"",{"$f":" getNozzle(T84, W84, Y84, Z84, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I85)),I85<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I85, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H85)),H85<0),\"\",intlEstQuantity(T85, W85*12, H85)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T85=\"Select Model\",\"\",coilCircuitChange(W85, U85, AC85, T85,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T85=\"Select Model\",\"\",beamWidth(T85))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T85=\"Select Model\",T85=\"PCBL\"), 0,getSPIP(T85, W85, Y85, BD85, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T85=\"Select Model\", \"\",IF(T85=\"PCBL\",0,primaryAirSensibleCapacityIP($T85,$W85,activeRoomTempCooling,activePriAirTempCooling,$Y85,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T85=\"Select Model\",\"\",IF($T85=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y85,activeElevation)))","v":""},{"$f":"IF(OR(T85=\"Select Model\",T85=\"PCBL\"), 0,IF(AD85=0,0,-primaryAirSensibleCapacityIP($T85,$W85,activeRoomTempHeating,activePriAirTempHeating,$Y85,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T85=\"Select Model\", \"\", InductionRatio($T85,BD85,$W85,$Y85)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T85=\"Select Model\", \"\",IF($T85=\"PCBL\",\"N/A\",minVAVSetBack(AA85, Y85))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T85=\"Select Model\", \"\",IF($T85= \"PCBL\",\"N/A\",getDischargeAirTemp($T85,$V85,$AC85,$W85,BD85,$AL85, $Y85, $AS85, \"cooling\",activeElevation,$AB85,$AJ85,$AV85,$BB85))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T85=\"Select Model\",$T85=\"PCBL\"), \"\",getDischargeAirTemp($T85,$V85,$AD85,$W85,BD85,$AL85, $Y85, $AY85, \"heating\",activeElevation,$AB85,$AJ85,$AV85,$BB85)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T85=\"Select Model\", \"\",IF(OR($T85=\"ACBC_1W\",$T85=\"ACBC_2W\",LEFT($T85,4)=\"ACBR\",$T85 = \"LIU24_2W\",LEFT($T85,3)=\"RIU\",LEFT($T85,6)=\"ACBL12\"), IF((soundLevel($T85, $AB85, BD85, $Y85, $W85,$AJ85,$AA85,\"dba\"))<15,\"<15\",soundLevel($T85, $AB85, BD85, $Y85, $W85,$AJ85,$AA85,\"dba\")+0.4),IF((soundLevel($T85, $AB85, BD85, $Y85, $W85,$AJ85,$AA85,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T85, $AB85, BD85, $Y85, $W85,$AJ85,$AA85,\"dba\")+5)<15, \"<15\", soundLevel($T85, $AB85, BD85,$Y85, $W85,$AJ85,$AA85,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T85=\"Select Model\", \"\",IF(OR($T85=\"ACBC_1W\",$T85=\"ACBC_2W\",LEFT($T85,4)=\"ACBR\",$T85=\"LIU24_2W\",LEFT($T85,3)=\"RIU\",LEFT($T85,6)=\"ACBL12\"), IF((soundLevel($T85, $AB85, BD85, $Y85, $W85,$AJ85,$AA85,\"NC\"))<15,\"<15\",soundLevel($T85, $AB85, BD85, $Y85, $W85,$AJ85,$AA85,\"NC\")+0.4),IF((soundLevel($T85, $AB85, BD85, $Y85, $W85,$AJ85,$AA85,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T85, $AB85, BD85, $Y85, $W85,$AJ85,$AA85,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T85, $AB85, BD85, $Y85, $W85,$AJ85,$AA85,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T85=\"Select Model\",\"\",IF($T85=\"LIU24_2W\",calcQwIP($Y85,$W85,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC85,$AI85,\"latent\",$U85&\"P\"&IF($V85=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T85,activeElevation),\"\"))","v":""},{"$f":"IF($T85=\"Select Model\",\"\",IF($T85=\"ACBC_1W\",calcQwIP($Y85,$W85,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC85,BD85,\"capacity\",$U85&\"P\"&IF($V85=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T85,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y85,$W85,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC85,BD85,\"capacity\",$U85&\"P\"&IF($V85=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T85,activeElevation)))","v":""},"",{"$f":"IF(T85=\"Select Model\", 0,waterPressureDrop(W85, U85 & \"P\" & IF(V85=\"Dual\",2,1) &\"C\", AC85, \"cooling\", T85))","v":0},{"$f":"IF(T85=\"Select Model\", \"\",getReturnWaterTemp(T85,AC85, activeEWTCooling, AS85, \"cooling\"))","v":""},"",{"$f":"IF($T85<>\"ACBC_1W\",\"\",IF($J85=\"\",\"\",FintubeCapacity($T85,$W85,$AE85,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T85=\"Select Model\",T85=\"PCBL\"),\"\",calcQwIP(Y85,W85,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD85,BD85,\"capacity\",U85&\"P\"&IF(V85=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T85,activeElevation))","v":""},"",{"$f":"IF(OR(T85=\"Select Model\",T85=\"PCBL\"), \"\",IF(AY85=0,\"N/A\",waterPressureDrop(W85, U85 & \"P\" & IF(V85=\"Dual\",2,1) &\"C\", AD85, \"heating\", T85)))","v":""},{"$f":"IF(OR(T85=\"Select Model\",T85=\"PCBL\"), \"\",IF(AY85=0,getReturnWaterTemp(T85,AE85, activeEWTHeating, AX85, \"heating\"),getReturnWaterTemp(T85,AD85, activeEWTHeating, AY85, \"heating\")))","v":""},"",{"$f":" getNozzle(T85, W85, Y85, Z85, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I86)),I86<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I86, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H86)),H86<0),\"\",intlEstQuantity(T86, W86*12, H86)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T86=\"Select Model\",\"\",coilCircuitChange(W86, U86, AC86, T86,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T86=\"Select Model\",\"\",beamWidth(T86))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T86=\"Select Model\",T86=\"PCBL\"), 0,getSPIP(T86, W86, Y86, BD86, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T86=\"Select Model\", \"\",IF(T86=\"PCBL\",0,primaryAirSensibleCapacityIP($T86,$W86,activeRoomTempCooling,activePriAirTempCooling,$Y86,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T86=\"Select Model\",\"\",IF($T86=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y86,activeElevation)))","v":""},{"$f":"IF(OR(T86=\"Select Model\",T86=\"PCBL\"), 0,IF(AD86=0,0,-primaryAirSensibleCapacityIP($T86,$W86,activeRoomTempHeating,activePriAirTempHeating,$Y86,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T86=\"Select Model\", \"\", InductionRatio($T86,BD86,$W86,$Y86)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T86=\"Select Model\", \"\",IF($T86=\"PCBL\",\"N/A\",minVAVSetBack(AA86, Y86))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T86=\"Select Model\", \"\",IF($T86= \"PCBL\",\"N/A\",getDischargeAirTemp($T86,$V86,$AC86,$W86,BD86,$AL86, $Y86, $AS86, \"cooling\",activeElevation,$AB86,$AJ86,$AV86,$BB86))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T86=\"Select Model\",$T86=\"PCBL\"), \"\",getDischargeAirTemp($T86,$V86,$AD86,$W86,BD86,$AL86, $Y86, $AY86, \"heating\",activeElevation,$AB86,$AJ86,$AV86,$BB86)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T86=\"Select Model\", \"\",IF(OR($T86=\"ACBC_1W\",$T86=\"ACBC_2W\",LEFT($T86,4)=\"ACBR\",$T86 = \"LIU24_2W\",LEFT($T86,3)=\"RIU\",LEFT($T86,6)=\"ACBL12\"), IF((soundLevel($T86, $AB86, BD86, $Y86, $W86,$AJ86,$AA86,\"dba\"))<15,\"<15\",soundLevel($T86, $AB86, BD86, $Y86, $W86,$AJ86,$AA86,\"dba\")+0.4),IF((soundLevel($T86, $AB86, BD86, $Y86, $W86,$AJ86,$AA86,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T86, $AB86, BD86, $Y86, $W86,$AJ86,$AA86,\"dba\")+5)<15, \"<15\", soundLevel($T86, $AB86, BD86,$Y86, $W86,$AJ86,$AA86,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T86=\"Select Model\", \"\",IF(OR($T86=\"ACBC_1W\",$T86=\"ACBC_2W\",LEFT($T86,4)=\"ACBR\",$T86=\"LIU24_2W\",LEFT($T86,3)=\"RIU\",LEFT($T86,6)=\"ACBL12\"), IF((soundLevel($T86, $AB86, BD86, $Y86, $W86,$AJ86,$AA86,\"NC\"))<15,\"<15\",soundLevel($T86, $AB86, BD86, $Y86, $W86,$AJ86,$AA86,\"NC\")+0.4),IF((soundLevel($T86, $AB86, BD86, $Y86, $W86,$AJ86,$AA86,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T86, $AB86, BD86, $Y86, $W86,$AJ86,$AA86,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T86, $AB86, BD86, $Y86, $W86,$AJ86,$AA86,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T86=\"Select Model\",\"\",IF($T86=\"LIU24_2W\",calcQwIP($Y86,$W86,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC86,$AI86,\"latent\",$U86&\"P\"&IF($V86=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T86,activeElevation),\"\"))","v":""},{"$f":"IF($T86=\"Select Model\",\"\",IF($T86=\"ACBC_1W\",calcQwIP($Y86,$W86,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC86,BD86,\"capacity\",$U86&\"P\"&IF($V86=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T86,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y86,$W86,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC86,BD86,\"capacity\",$U86&\"P\"&IF($V86=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T86,activeElevation)))","v":""},"",{"$f":"IF(T86=\"Select Model\", 0,waterPressureDrop(W86, U86 & \"P\" & IF(V86=\"Dual\",2,1) &\"C\", AC86, \"cooling\", T86))","v":0},{"$f":"IF(T86=\"Select Model\", \"\",getReturnWaterTemp(T86,AC86, activeEWTCooling, AS86, \"cooling\"))","v":""},"",{"$f":"IF($T86<>\"ACBC_1W\",\"\",IF($J86=\"\",\"\",FintubeCapacity($T86,$W86,$AE86,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T86=\"Select Model\",T86=\"PCBL\"),\"\",calcQwIP(Y86,W86,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD86,BD86,\"capacity\",U86&\"P\"&IF(V86=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T86,activeElevation))","v":""},"",{"$f":"IF(OR(T86=\"Select Model\",T86=\"PCBL\"), \"\",IF(AY86=0,\"N/A\",waterPressureDrop(W86, U86 & \"P\" & IF(V86=\"Dual\",2,1) &\"C\", AD86, \"heating\", T86)))","v":""},{"$f":"IF(OR(T86=\"Select Model\",T86=\"PCBL\"), \"\",IF(AY86=0,getReturnWaterTemp(T86,AE86, activeEWTHeating, AX86, \"heating\"),getReturnWaterTemp(T86,AD86, activeEWTHeating, AY86, \"heating\")))","v":""},"",{"$f":" getNozzle(T86, W86, Y86, Z86, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I87)),I87<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I87, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H87)),H87<0),\"\",intlEstQuantity(T87, W87*12, H87)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T87=\"Select Model\",\"\",coilCircuitChange(W87, U87, AC87, T87,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T87=\"Select Model\",\"\",beamWidth(T87))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T87=\"Select Model\",T87=\"PCBL\"), 0,getSPIP(T87, W87, Y87, BD87, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T87=\"Select Model\", \"\",IF(T87=\"PCBL\",0,primaryAirSensibleCapacityIP($T87,$W87,activeRoomTempCooling,activePriAirTempCooling,$Y87,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T87=\"Select Model\",\"\",IF($T87=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y87,activeElevation)))","v":""},{"$f":"IF(OR(T87=\"Select Model\",T87=\"PCBL\"), 0,IF(AD87=0,0,-primaryAirSensibleCapacityIP($T87,$W87,activeRoomTempHeating,activePriAirTempHeating,$Y87,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T87=\"Select Model\", \"\", InductionRatio($T87,BD87,$W87,$Y87)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T87=\"Select Model\", \"\",IF($T87=\"PCBL\",\"N/A\",minVAVSetBack(AA87, Y87))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T87=\"Select Model\", \"\",IF($T87= \"PCBL\",\"N/A\",getDischargeAirTemp($T87,$V87,$AC87,$W87,BD87,$AL87, $Y87, $AS87, \"cooling\",activeElevation,$AB87,$AJ87,$AV87,$BB87))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T87=\"Select Model\",$T87=\"PCBL\"), \"\",getDischargeAirTemp($T87,$V87,$AD87,$W87,BD87,$AL87, $Y87, $AY87, \"heating\",activeElevation,$AB87,$AJ87,$AV87,$BB87)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T87=\"Select Model\", \"\",IF(OR($T87=\"ACBC_1W\",$T87=\"ACBC_2W\",LEFT($T87,4)=\"ACBR\",$T87 = \"LIU24_2W\",LEFT($T87,3)=\"RIU\",LEFT($T87,6)=\"ACBL12\"), IF((soundLevel($T87, $AB87, BD87, $Y87, $W87,$AJ87,$AA87,\"dba\"))<15,\"<15\",soundLevel($T87, $AB87, BD87, $Y87, $W87,$AJ87,$AA87,\"dba\")+0.4),IF((soundLevel($T87, $AB87, BD87, $Y87, $W87,$AJ87,$AA87,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T87, $AB87, BD87, $Y87, $W87,$AJ87,$AA87,\"dba\")+5)<15, \"<15\", soundLevel($T87, $AB87, BD87,$Y87, $W87,$AJ87,$AA87,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T87=\"Select Model\", \"\",IF(OR($T87=\"ACBC_1W\",$T87=\"ACBC_2W\",LEFT($T87,4)=\"ACBR\",$T87=\"LIU24_2W\",LEFT($T87,3)=\"RIU\",LEFT($T87,6)=\"ACBL12\"), IF((soundLevel($T87, $AB87, BD87, $Y87, $W87,$AJ87,$AA87,\"NC\"))<15,\"<15\",soundLevel($T87, $AB87, BD87, $Y87, $W87,$AJ87,$AA87,\"NC\")+0.4),IF((soundLevel($T87, $AB87, BD87, $Y87, $W87,$AJ87,$AA87,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T87, $AB87, BD87, $Y87, $W87,$AJ87,$AA87,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T87, $AB87, BD87, $Y87, $W87,$AJ87,$AA87,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T87=\"Select Model\",\"\",IF($T87=\"LIU24_2W\",calcQwIP($Y87,$W87,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC87,$AI87,\"latent\",$U87&\"P\"&IF($V87=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T87,activeElevation),\"\"))","v":""},{"$f":"IF($T87=\"Select Model\",\"\",IF($T87=\"ACBC_1W\",calcQwIP($Y87,$W87,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC87,BD87,\"capacity\",$U87&\"P\"&IF($V87=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T87,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y87,$W87,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC87,BD87,\"capacity\",$U87&\"P\"&IF($V87=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T87,activeElevation)))","v":""},"",{"$f":"IF(T87=\"Select Model\", 0,waterPressureDrop(W87, U87 & \"P\" & IF(V87=\"Dual\",2,1) &\"C\", AC87, \"cooling\", T87))","v":0},{"$f":"IF(T87=\"Select Model\", \"\",getReturnWaterTemp(T87,AC87, activeEWTCooling, AS87, \"cooling\"))","v":""},"",{"$f":"IF($T87<>\"ACBC_1W\",\"\",IF($J87=\"\",\"\",FintubeCapacity($T87,$W87,$AE87,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T87=\"Select Model\",T87=\"PCBL\"),\"\",calcQwIP(Y87,W87,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD87,BD87,\"capacity\",U87&\"P\"&IF(V87=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T87,activeElevation))","v":""},"",{"$f":"IF(OR(T87=\"Select Model\",T87=\"PCBL\"), \"\",IF(AY87=0,\"N/A\",waterPressureDrop(W87, U87 & \"P\" & IF(V87=\"Dual\",2,1) &\"C\", AD87, \"heating\", T87)))","v":""},{"$f":"IF(OR(T87=\"Select Model\",T87=\"PCBL\"), \"\",IF(AY87=0,getReturnWaterTemp(T87,AE87, activeEWTHeating, AX87, \"heating\"),getReturnWaterTemp(T87,AD87, activeEWTHeating, AY87, \"heating\")))","v":""},"",{"$f":" getNozzle(T87, W87, Y87, Z87, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I88)),I88<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I88, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H88)),H88<0),\"\",intlEstQuantity(T88, W88*12, H88)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T88=\"Select Model\",\"\",coilCircuitChange(W88, U88, AC88, T88,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T88=\"Select Model\",\"\",beamWidth(T88))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T88=\"Select Model\",T88=\"PCBL\"), 0,getSPIP(T88, W88, Y88, BD88, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T88=\"Select Model\", \"\",IF(T88=\"PCBL\",0,primaryAirSensibleCapacityIP($T88,$W88,activeRoomTempCooling,activePriAirTempCooling,$Y88,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T88=\"Select Model\",\"\",IF($T88=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y88,activeElevation)))","v":""},{"$f":"IF(OR(T88=\"Select Model\",T88=\"PCBL\"), 0,IF(AD88=0,0,-primaryAirSensibleCapacityIP($T88,$W88,activeRoomTempHeating,activePriAirTempHeating,$Y88,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T88=\"Select Model\", \"\", InductionRatio($T88,BD88,$W88,$Y88)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T88=\"Select Model\", \"\",IF($T88=\"PCBL\",\"N/A\",minVAVSetBack(AA88, Y88))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T88=\"Select Model\", \"\",IF($T88= \"PCBL\",\"N/A\",getDischargeAirTemp($T88,$V88,$AC88,$W88,BD88,$AL88, $Y88, $AS88, \"cooling\",activeElevation,$AB88,$AJ88,$AV88,$BB88))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T88=\"Select Model\",$T88=\"PCBL\"), \"\",getDischargeAirTemp($T88,$V88,$AD88,$W88,BD88,$AL88, $Y88, $AY88, \"heating\",activeElevation,$AB88,$AJ88,$AV88,$BB88)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T88=\"Select Model\", \"\",IF(OR($T88=\"ACBC_1W\",$T88=\"ACBC_2W\",LEFT($T88,4)=\"ACBR\",$T88 = \"LIU24_2W\",LEFT($T88,3)=\"RIU\",LEFT($T88,6)=\"ACBL12\"), IF((soundLevel($T88, $AB88, BD88, $Y88, $W88,$AJ88,$AA88,\"dba\"))<15,\"<15\",soundLevel($T88, $AB88, BD88, $Y88, $W88,$AJ88,$AA88,\"dba\")+0.4),IF((soundLevel($T88, $AB88, BD88, $Y88, $W88,$AJ88,$AA88,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T88, $AB88, BD88, $Y88, $W88,$AJ88,$AA88,\"dba\")+5)<15, \"<15\", soundLevel($T88, $AB88, BD88,$Y88, $W88,$AJ88,$AA88,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T88=\"Select Model\", \"\",IF(OR($T88=\"ACBC_1W\",$T88=\"ACBC_2W\",LEFT($T88,4)=\"ACBR\",$T88=\"LIU24_2W\",LEFT($T88,3)=\"RIU\",LEFT($T88,6)=\"ACBL12\"), IF((soundLevel($T88, $AB88, BD88, $Y88, $W88,$AJ88,$AA88,\"NC\"))<15,\"<15\",soundLevel($T88, $AB88, BD88, $Y88, $W88,$AJ88,$AA88,\"NC\")+0.4),IF((soundLevel($T88, $AB88, BD88, $Y88, $W88,$AJ88,$AA88,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T88, $AB88, BD88, $Y88, $W88,$AJ88,$AA88,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T88, $AB88, BD88, $Y88, $W88,$AJ88,$AA88,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T88=\"Select Model\",\"\",IF($T88=\"LIU24_2W\",calcQwIP($Y88,$W88,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC88,$AI88,\"latent\",$U88&\"P\"&IF($V88=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T88,activeElevation),\"\"))","v":""},{"$f":"IF($T88=\"Select Model\",\"\",IF($T88=\"ACBC_1W\",calcQwIP($Y88,$W88,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC88,BD88,\"capacity\",$U88&\"P\"&IF($V88=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T88,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y88,$W88,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC88,BD88,\"capacity\",$U88&\"P\"&IF($V88=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T88,activeElevation)))","v":""},"",{"$f":"IF(T88=\"Select Model\", 0,waterPressureDrop(W88, U88 & \"P\" & IF(V88=\"Dual\",2,1) &\"C\", AC88, \"cooling\", T88))","v":0},{"$f":"IF(T88=\"Select Model\", \"\",getReturnWaterTemp(T88,AC88, activeEWTCooling, AS88, \"cooling\"))","v":""},"",{"$f":"IF($T88<>\"ACBC_1W\",\"\",IF($J88=\"\",\"\",FintubeCapacity($T88,$W88,$AE88,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T88=\"Select Model\",T88=\"PCBL\"),\"\",calcQwIP(Y88,W88,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD88,BD88,\"capacity\",U88&\"P\"&IF(V88=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T88,activeElevation))","v":""},"",{"$f":"IF(OR(T88=\"Select Model\",T88=\"PCBL\"), \"\",IF(AY88=0,\"N/A\",waterPressureDrop(W88, U88 & \"P\" & IF(V88=\"Dual\",2,1) &\"C\", AD88, \"heating\", T88)))","v":""},{"$f":"IF(OR(T88=\"Select Model\",T88=\"PCBL\"), \"\",IF(AY88=0,getReturnWaterTemp(T88,AE88, activeEWTHeating, AX88, \"heating\"),getReturnWaterTemp(T88,AD88, activeEWTHeating, AY88, \"heating\")))","v":""},"",{"$f":" getNozzle(T88, W88, Y88, Z88, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I89)),I89<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I89, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H89)),H89<0),\"\",intlEstQuantity(T89, W89*12, H89)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T89=\"Select Model\",\"\",coilCircuitChange(W89, U89, AC89, T89,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T89=\"Select Model\",\"\",beamWidth(T89))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T89=\"Select Model\",T89=\"PCBL\"), 0,getSPIP(T89, W89, Y89, BD89, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T89=\"Select Model\", \"\",IF(T89=\"PCBL\",0,primaryAirSensibleCapacityIP($T89,$W89,activeRoomTempCooling,activePriAirTempCooling,$Y89,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T89=\"Select Model\",\"\",IF($T89=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y89,activeElevation)))","v":""},{"$f":"IF(OR(T89=\"Select Model\",T89=\"PCBL\"), 0,IF(AD89=0,0,-primaryAirSensibleCapacityIP($T89,$W89,activeRoomTempHeating,activePriAirTempHeating,$Y89,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T89=\"Select Model\", \"\", InductionRatio($T89,BD89,$W89,$Y89)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T89=\"Select Model\", \"\",IF($T89=\"PCBL\",\"N/A\",minVAVSetBack(AA89, Y89))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T89=\"Select Model\", \"\",IF($T89= \"PCBL\",\"N/A\",getDischargeAirTemp($T89,$V89,$AC89,$W89,BD89,$AL89, $Y89, $AS89, \"cooling\",activeElevation,$AB89,$AJ89,$AV89,$BB89))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T89=\"Select Model\",$T89=\"PCBL\"), \"\",getDischargeAirTemp($T89,$V89,$AD89,$W89,BD89,$AL89, $Y89, $AY89, \"heating\",activeElevation,$AB89,$AJ89,$AV89,$BB89)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T89=\"Select Model\", \"\",IF(OR($T89=\"ACBC_1W\",$T89=\"ACBC_2W\",LEFT($T89,4)=\"ACBR\",$T89 = \"LIU24_2W\",LEFT($T89,3)=\"RIU\",LEFT($T89,6)=\"ACBL12\"), IF((soundLevel($T89, $AB89, BD89, $Y89, $W89,$AJ89,$AA89,\"dba\"))<15,\"<15\",soundLevel($T89, $AB89, BD89, $Y89, $W89,$AJ89,$AA89,\"dba\")+0.4),IF((soundLevel($T89, $AB89, BD89, $Y89, $W89,$AJ89,$AA89,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T89, $AB89, BD89, $Y89, $W89,$AJ89,$AA89,\"dba\")+5)<15, \"<15\", soundLevel($T89, $AB89, BD89,$Y89, $W89,$AJ89,$AA89,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T89=\"Select Model\", \"\",IF(OR($T89=\"ACBC_1W\",$T89=\"ACBC_2W\",LEFT($T89,4)=\"ACBR\",$T89=\"LIU24_2W\",LEFT($T89,3)=\"RIU\",LEFT($T89,6)=\"ACBL12\"), IF((soundLevel($T89, $AB89, BD89, $Y89, $W89,$AJ89,$AA89,\"NC\"))<15,\"<15\",soundLevel($T89, $AB89, BD89, $Y89, $W89,$AJ89,$AA89,\"NC\")+0.4),IF((soundLevel($T89, $AB89, BD89, $Y89, $W89,$AJ89,$AA89,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T89, $AB89, BD89, $Y89, $W89,$AJ89,$AA89,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T89, $AB89, BD89, $Y89, $W89,$AJ89,$AA89,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T89=\"Select Model\",\"\",IF($T89=\"LIU24_2W\",calcQwIP($Y89,$W89,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC89,$AI89,\"latent\",$U89&\"P\"&IF($V89=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T89,activeElevation),\"\"))","v":""},{"$f":"IF($T89=\"Select Model\",\"\",IF($T89=\"ACBC_1W\",calcQwIP($Y89,$W89,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC89,BD89,\"capacity\",$U89&\"P\"&IF($V89=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T89,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y89,$W89,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC89,BD89,\"capacity\",$U89&\"P\"&IF($V89=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T89,activeElevation)))","v":""},"",{"$f":"IF(T89=\"Select Model\", 0,waterPressureDrop(W89, U89 & \"P\" & IF(V89=\"Dual\",2,1) &\"C\", AC89, \"cooling\", T89))","v":0},{"$f":"IF(T89=\"Select Model\", \"\",getReturnWaterTemp(T89,AC89, activeEWTCooling, AS89, \"cooling\"))","v":""},"",{"$f":"IF($T89<>\"ACBC_1W\",\"\",IF($J89=\"\",\"\",FintubeCapacity($T89,$W89,$AE89,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T89=\"Select Model\",T89=\"PCBL\"),\"\",calcQwIP(Y89,W89,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD89,BD89,\"capacity\",U89&\"P\"&IF(V89=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T89,activeElevation))","v":""},"",{"$f":"IF(OR(T89=\"Select Model\",T89=\"PCBL\"), \"\",IF(AY89=0,\"N/A\",waterPressureDrop(W89, U89 & \"P\" & IF(V89=\"Dual\",2,1) &\"C\", AD89, \"heating\", T89)))","v":""},{"$f":"IF(OR(T89=\"Select Model\",T89=\"PCBL\"), \"\",IF(AY89=0,getReturnWaterTemp(T89,AE89, activeEWTHeating, AX89, \"heating\"),getReturnWaterTemp(T89,AD89, activeEWTHeating, AY89, \"heating\")))","v":""},"",{"$f":" getNozzle(T89, W89, Y89, Z89, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I90)),I90<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I90, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H90)),H90<0),\"\",intlEstQuantity(T90, W90*12, H90)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T90=\"Select Model\",\"\",coilCircuitChange(W90, U90, AC90, T90,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T90=\"Select Model\",\"\",beamWidth(T90))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T90=\"Select Model\",T90=\"PCBL\"), 0,getSPIP(T90, W90, Y90, BD90, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T90=\"Select Model\", \"\",IF(T90=\"PCBL\",0,primaryAirSensibleCapacityIP($T90,$W90,activeRoomTempCooling,activePriAirTempCooling,$Y90,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T90=\"Select Model\",\"\",IF($T90=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y90,activeElevation)))","v":""},{"$f":"IF(OR(T90=\"Select Model\",T90=\"PCBL\"), 0,IF(AD90=0,0,-primaryAirSensibleCapacityIP($T90,$W90,activeRoomTempHeating,activePriAirTempHeating,$Y90,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T90=\"Select Model\", \"\", InductionRatio($T90,BD90,$W90,$Y90)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T90=\"Select Model\", \"\",IF($T90=\"PCBL\",\"N/A\",minVAVSetBack(AA90, Y90))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T90=\"Select Model\", \"\",IF($T90= \"PCBL\",\"N/A\",getDischargeAirTemp($T90,$V90,$AC90,$W90,BD90,$AL90, $Y90, $AS90, \"cooling\",activeElevation,$AB90,$AJ90,$AV90,$BB90))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T90=\"Select Model\",$T90=\"PCBL\"), \"\",getDischargeAirTemp($T90,$V90,$AD90,$W90,BD90,$AL90, $Y90, $AY90, \"heating\",activeElevation,$AB90,$AJ90,$AV90,$BB90)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T90=\"Select Model\", \"\",IF(OR($T90=\"ACBC_1W\",$T90=\"ACBC_2W\",LEFT($T90,4)=\"ACBR\",$T90 = \"LIU24_2W\",LEFT($T90,3)=\"RIU\",LEFT($T90,6)=\"ACBL12\"), IF((soundLevel($T90, $AB90, BD90, $Y90, $W90,$AJ90,$AA90,\"dba\"))<15,\"<15\",soundLevel($T90, $AB90, BD90, $Y90, $W90,$AJ90,$AA90,\"dba\")+0.4),IF((soundLevel($T90, $AB90, BD90, $Y90, $W90,$AJ90,$AA90,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T90, $AB90, BD90, $Y90, $W90,$AJ90,$AA90,\"dba\")+5)<15, \"<15\", soundLevel($T90, $AB90, BD90,$Y90, $W90,$AJ90,$AA90,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T90=\"Select Model\", \"\",IF(OR($T90=\"ACBC_1W\",$T90=\"ACBC_2W\",LEFT($T90,4)=\"ACBR\",$T90=\"LIU24_2W\",LEFT($T90,3)=\"RIU\",LEFT($T90,6)=\"ACBL12\"), IF((soundLevel($T90, $AB90, BD90, $Y90, $W90,$AJ90,$AA90,\"NC\"))<15,\"<15\",soundLevel($T90, $AB90, BD90, $Y90, $W90,$AJ90,$AA90,\"NC\")+0.4),IF((soundLevel($T90, $AB90, BD90, $Y90, $W90,$AJ90,$AA90,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T90, $AB90, BD90, $Y90, $W90,$AJ90,$AA90,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T90, $AB90, BD90, $Y90, $W90,$AJ90,$AA90,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T90=\"Select Model\",\"\",IF($T90=\"LIU24_2W\",calcQwIP($Y90,$W90,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC90,$AI90,\"latent\",$U90&\"P\"&IF($V90=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T90,activeElevation),\"\"))","v":""},{"$f":"IF($T90=\"Select Model\",\"\",IF($T90=\"ACBC_1W\",calcQwIP($Y90,$W90,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC90,BD90,\"capacity\",$U90&\"P\"&IF($V90=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T90,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y90,$W90,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC90,BD90,\"capacity\",$U90&\"P\"&IF($V90=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T90,activeElevation)))","v":""},"",{"$f":"IF(T90=\"Select Model\", 0,waterPressureDrop(W90, U90 & \"P\" & IF(V90=\"Dual\",2,1) &\"C\", AC90, \"cooling\", T90))","v":0},{"$f":"IF(T90=\"Select Model\", \"\",getReturnWaterTemp(T90,AC90, activeEWTCooling, AS90, \"cooling\"))","v":""},"",{"$f":"IF($T90<>\"ACBC_1W\",\"\",IF($J90=\"\",\"\",FintubeCapacity($T90,$W90,$AE90,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T90=\"Select Model\",T90=\"PCBL\"),\"\",calcQwIP(Y90,W90,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD90,BD90,\"capacity\",U90&\"P\"&IF(V90=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T90,activeElevation))","v":""},"",{"$f":"IF(OR(T90=\"Select Model\",T90=\"PCBL\"), \"\",IF(AY90=0,\"N/A\",waterPressureDrop(W90, U90 & \"P\" & IF(V90=\"Dual\",2,1) &\"C\", AD90, \"heating\", T90)))","v":""},{"$f":"IF(OR(T90=\"Select Model\",T90=\"PCBL\"), \"\",IF(AY90=0,getReturnWaterTemp(T90,AE90, activeEWTHeating, AX90, \"heating\"),getReturnWaterTemp(T90,AD90, activeEWTHeating, AY90, \"heating\")))","v":""},"",{"$f":" getNozzle(T90, W90, Y90, Z90, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I91)),I91<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I91, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H91)),H91<0),\"\",intlEstQuantity(T91, W91*12, H91)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T91=\"Select Model\",\"\",coilCircuitChange(W91, U91, AC91, T91,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T91=\"Select Model\",\"\",beamWidth(T91))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T91=\"Select Model\",T91=\"PCBL\"), 0,getSPIP(T91, W91, Y91, BD91, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T91=\"Select Model\", \"\",IF(T91=\"PCBL\",0,primaryAirSensibleCapacityIP($T91,$W91,activeRoomTempCooling,activePriAirTempCooling,$Y91,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T91=\"Select Model\",\"\",IF($T91=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y91,activeElevation)))","v":""},{"$f":"IF(OR(T91=\"Select Model\",T91=\"PCBL\"), 0,IF(AD91=0,0,-primaryAirSensibleCapacityIP($T91,$W91,activeRoomTempHeating,activePriAirTempHeating,$Y91,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T91=\"Select Model\", \"\", InductionRatio($T91,BD91,$W91,$Y91)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T91=\"Select Model\", \"\",IF($T91=\"PCBL\",\"N/A\",minVAVSetBack(AA91, Y91))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T91=\"Select Model\", \"\",IF($T91= \"PCBL\",\"N/A\",getDischargeAirTemp($T91,$V91,$AC91,$W91,BD91,$AL91, $Y91, $AS91, \"cooling\",activeElevation,$AB91,$AJ91,$AV91,$BB91))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T91=\"Select Model\",$T91=\"PCBL\"), \"\",getDischargeAirTemp($T91,$V91,$AD91,$W91,BD91,$AL91, $Y91, $AY91, \"heating\",activeElevation,$AB91,$AJ91,$AV91,$BB91)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T91=\"Select Model\", \"\",IF(OR($T91=\"ACBC_1W\",$T91=\"ACBC_2W\",LEFT($T91,4)=\"ACBR\",$T91 = \"LIU24_2W\",LEFT($T91,3)=\"RIU\",LEFT($T91,6)=\"ACBL12\"), IF((soundLevel($T91, $AB91, BD91, $Y91, $W91,$AJ91,$AA91,\"dba\"))<15,\"<15\",soundLevel($T91, $AB91, BD91, $Y91, $W91,$AJ91,$AA91,\"dba\")+0.4),IF((soundLevel($T91, $AB91, BD91, $Y91, $W91,$AJ91,$AA91,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T91, $AB91, BD91, $Y91, $W91,$AJ91,$AA91,\"dba\")+5)<15, \"<15\", soundLevel($T91, $AB91, BD91,$Y91, $W91,$AJ91,$AA91,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T91=\"Select Model\", \"\",IF(OR($T91=\"ACBC_1W\",$T91=\"ACBC_2W\",LEFT($T91,4)=\"ACBR\",$T91=\"LIU24_2W\",LEFT($T91,3)=\"RIU\",LEFT($T91,6)=\"ACBL12\"), IF((soundLevel($T91, $AB91, BD91, $Y91, $W91,$AJ91,$AA91,\"NC\"))<15,\"<15\",soundLevel($T91, $AB91, BD91, $Y91, $W91,$AJ91,$AA91,\"NC\")+0.4),IF((soundLevel($T91, $AB91, BD91, $Y91, $W91,$AJ91,$AA91,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T91, $AB91, BD91, $Y91, $W91,$AJ91,$AA91,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T91, $AB91, BD91, $Y91, $W91,$AJ91,$AA91,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T91=\"Select Model\",\"\",IF($T91=\"LIU24_2W\",calcQwIP($Y91,$W91,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC91,$AI91,\"latent\",$U91&\"P\"&IF($V91=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T91,activeElevation),\"\"))","v":""},{"$f":"IF($T91=\"Select Model\",\"\",IF($T91=\"ACBC_1W\",calcQwIP($Y91,$W91,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC91,BD91,\"capacity\",$U91&\"P\"&IF($V91=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T91,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y91,$W91,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC91,BD91,\"capacity\",$U91&\"P\"&IF($V91=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T91,activeElevation)))","v":""},"",{"$f":"IF(T91=\"Select Model\", 0,waterPressureDrop(W91, U91 & \"P\" & IF(V91=\"Dual\",2,1) &\"C\", AC91, \"cooling\", T91))","v":0},{"$f":"IF(T91=\"Select Model\", \"\",getReturnWaterTemp(T91,AC91, activeEWTCooling, AS91, \"cooling\"))","v":""},"",{"$f":"IF($T91<>\"ACBC_1W\",\"\",IF($J91=\"\",\"\",FintubeCapacity($T91,$W91,$AE91,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T91=\"Select Model\",T91=\"PCBL\"),\"\",calcQwIP(Y91,W91,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD91,BD91,\"capacity\",U91&\"P\"&IF(V91=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T91,activeElevation))","v":""},"",{"$f":"IF(OR(T91=\"Select Model\",T91=\"PCBL\"), \"\",IF(AY91=0,\"N/A\",waterPressureDrop(W91, U91 & \"P\" & IF(V91=\"Dual\",2,1) &\"C\", AD91, \"heating\", T91)))","v":""},{"$f":"IF(OR(T91=\"Select Model\",T91=\"PCBL\"), \"\",IF(AY91=0,getReturnWaterTemp(T91,AE91, activeEWTHeating, AX91, \"heating\"),getReturnWaterTemp(T91,AD91, activeEWTHeating, AY91, \"heating\")))","v":""},"",{"$f":" getNozzle(T91, W91, Y91, Z91, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I92)),I92<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I92, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H92)),H92<0),\"\",intlEstQuantity(T92, W92*12, H92)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T92=\"Select Model\",\"\",coilCircuitChange(W92, U92, AC92, T92,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T92=\"Select Model\",\"\",beamWidth(T92))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T92=\"Select Model\",T92=\"PCBL\"), 0,getSPIP(T92, W92, Y92, BD92, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T92=\"Select Model\", \"\",IF(T92=\"PCBL\",0,primaryAirSensibleCapacityIP($T92,$W92,activeRoomTempCooling,activePriAirTempCooling,$Y92,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T92=\"Select Model\",\"\",IF($T92=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y92,activeElevation)))","v":""},{"$f":"IF(OR(T92=\"Select Model\",T92=\"PCBL\"), 0,IF(AD92=0,0,-primaryAirSensibleCapacityIP($T92,$W92,activeRoomTempHeating,activePriAirTempHeating,$Y92,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T92=\"Select Model\", \"\", InductionRatio($T92,BD92,$W92,$Y92)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T92=\"Select Model\", \"\",IF($T92=\"PCBL\",\"N/A\",minVAVSetBack(AA92, Y92))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T92=\"Select Model\", \"\",IF($T92= \"PCBL\",\"N/A\",getDischargeAirTemp($T92,$V92,$AC92,$W92,BD92,$AL92, $Y92, $AS92, \"cooling\",activeElevation,$AB92,$AJ92,$AV92,$BB92))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T92=\"Select Model\",$T92=\"PCBL\"), \"\",getDischargeAirTemp($T92,$V92,$AD92,$W92,BD92,$AL92, $Y92, $AY92, \"heating\",activeElevation,$AB92,$AJ92,$AV92,$BB92)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T92=\"Select Model\", \"\",IF(OR($T92=\"ACBC_1W\",$T92=\"ACBC_2W\",LEFT($T92,4)=\"ACBR\",$T92 = \"LIU24_2W\",LEFT($T92,3)=\"RIU\",LEFT($T92,6)=\"ACBL12\"), IF((soundLevel($T92, $AB92, BD92, $Y92, $W92,$AJ92,$AA92,\"dba\"))<15,\"<15\",soundLevel($T92, $AB92, BD92, $Y92, $W92,$AJ92,$AA92,\"dba\")+0.4),IF((soundLevel($T92, $AB92, BD92, $Y92, $W92,$AJ92,$AA92,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T92, $AB92, BD92, $Y92, $W92,$AJ92,$AA92,\"dba\")+5)<15, \"<15\", soundLevel($T92, $AB92, BD92,$Y92, $W92,$AJ92,$AA92,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T92=\"Select Model\", \"\",IF(OR($T92=\"ACBC_1W\",$T92=\"ACBC_2W\",LEFT($T92,4)=\"ACBR\",$T92=\"LIU24_2W\",LEFT($T92,3)=\"RIU\",LEFT($T92,6)=\"ACBL12\"), IF((soundLevel($T92, $AB92, BD92, $Y92, $W92,$AJ92,$AA92,\"NC\"))<15,\"<15\",soundLevel($T92, $AB92, BD92, $Y92, $W92,$AJ92,$AA92,\"NC\")+0.4),IF((soundLevel($T92, $AB92, BD92, $Y92, $W92,$AJ92,$AA92,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T92, $AB92, BD92, $Y92, $W92,$AJ92,$AA92,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T92, $AB92, BD92, $Y92, $W92,$AJ92,$AA92,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T92=\"Select Model\",\"\",IF($T92=\"LIU24_2W\",calcQwIP($Y92,$W92,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC92,$AI92,\"latent\",$U92&\"P\"&IF($V92=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T92,activeElevation),\"\"))","v":""},{"$f":"IF($T92=\"Select Model\",\"\",IF($T92=\"ACBC_1W\",calcQwIP($Y92,$W92,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC92,BD92,\"capacity\",$U92&\"P\"&IF($V92=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T92,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y92,$W92,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC92,BD92,\"capacity\",$U92&\"P\"&IF($V92=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T92,activeElevation)))","v":""},"",{"$f":"IF(T92=\"Select Model\", 0,waterPressureDrop(W92, U92 & \"P\" & IF(V92=\"Dual\",2,1) &\"C\", AC92, \"cooling\", T92))","v":0},{"$f":"IF(T92=\"Select Model\", \"\",getReturnWaterTemp(T92,AC92, activeEWTCooling, AS92, \"cooling\"))","v":""},"",{"$f":"IF($T92<>\"ACBC_1W\",\"\",IF($J92=\"\",\"\",FintubeCapacity($T92,$W92,$AE92,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T92=\"Select Model\",T92=\"PCBL\"),\"\",calcQwIP(Y92,W92,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD92,BD92,\"capacity\",U92&\"P\"&IF(V92=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T92,activeElevation))","v":""},"",{"$f":"IF(OR(T92=\"Select Model\",T92=\"PCBL\"), \"\",IF(AY92=0,\"N/A\",waterPressureDrop(W92, U92 & \"P\" & IF(V92=\"Dual\",2,1) &\"C\", AD92, \"heating\", T92)))","v":""},{"$f":"IF(OR(T92=\"Select Model\",T92=\"PCBL\"), \"\",IF(AY92=0,getReturnWaterTemp(T92,AE92, activeEWTHeating, AX92, \"heating\"),getReturnWaterTemp(T92,AD92, activeEWTHeating, AY92, \"heating\")))","v":""},"",{"$f":" getNozzle(T92, W92, Y92, Z92, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I93)),I93<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I93, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H93)),H93<0),\"\",intlEstQuantity(T93, W93*12, H93)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T93=\"Select Model\",\"\",coilCircuitChange(W93, U93, AC93, T93,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T93=\"Select Model\",\"\",beamWidth(T93))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T93=\"Select Model\",T93=\"PCBL\"), 0,getSPIP(T93, W93, Y93, BD93, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T93=\"Select Model\", \"\",IF(T93=\"PCBL\",0,primaryAirSensibleCapacityIP($T93,$W93,activeRoomTempCooling,activePriAirTempCooling,$Y93,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T93=\"Select Model\",\"\",IF($T93=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y93,activeElevation)))","v":""},{"$f":"IF(OR(T93=\"Select Model\",T93=\"PCBL\"), 0,IF(AD93=0,0,-primaryAirSensibleCapacityIP($T93,$W93,activeRoomTempHeating,activePriAirTempHeating,$Y93,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T93=\"Select Model\", \"\", InductionRatio($T93,BD93,$W93,$Y93)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T93=\"Select Model\", \"\",IF($T93=\"PCBL\",\"N/A\",minVAVSetBack(AA93, Y93))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T93=\"Select Model\", \"\",IF($T93= \"PCBL\",\"N/A\",getDischargeAirTemp($T93,$V93,$AC93,$W93,BD93,$AL93, $Y93, $AS93, \"cooling\",activeElevation,$AB93,$AJ93,$AV93,$BB93))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T93=\"Select Model\",$T93=\"PCBL\"), \"\",getDischargeAirTemp($T93,$V93,$AD93,$W93,BD93,$AL93, $Y93, $AY93, \"heating\",activeElevation,$AB93,$AJ93,$AV93,$BB93)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T93=\"Select Model\", \"\",IF(OR($T93=\"ACBC_1W\",$T93=\"ACBC_2W\",LEFT($T93,4)=\"ACBR\",$T93 = \"LIU24_2W\",LEFT($T93,3)=\"RIU\",LEFT($T93,6)=\"ACBL12\"), IF((soundLevel($T93, $AB93, BD93, $Y93, $W93,$AJ93,$AA93,\"dba\"))<15,\"<15\",soundLevel($T93, $AB93, BD93, $Y93, $W93,$AJ93,$AA93,\"dba\")+0.4),IF((soundLevel($T93, $AB93, BD93, $Y93, $W93,$AJ93,$AA93,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T93, $AB93, BD93, $Y93, $W93,$AJ93,$AA93,\"dba\")+5)<15, \"<15\", soundLevel($T93, $AB93, BD93,$Y93, $W93,$AJ93,$AA93,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T93=\"Select Model\", \"\",IF(OR($T93=\"ACBC_1W\",$T93=\"ACBC_2W\",LEFT($T93,4)=\"ACBR\",$T93=\"LIU24_2W\",LEFT($T93,3)=\"RIU\",LEFT($T93,6)=\"ACBL12\"), IF((soundLevel($T93, $AB93, BD93, $Y93, $W93,$AJ93,$AA93,\"NC\"))<15,\"<15\",soundLevel($T93, $AB93, BD93, $Y93, $W93,$AJ93,$AA93,\"NC\")+0.4),IF((soundLevel($T93, $AB93, BD93, $Y93, $W93,$AJ93,$AA93,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T93, $AB93, BD93, $Y93, $W93,$AJ93,$AA93,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T93, $AB93, BD93, $Y93, $W93,$AJ93,$AA93,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T93=\"Select Model\",\"\",IF($T93=\"LIU24_2W\",calcQwIP($Y93,$W93,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC93,$AI93,\"latent\",$U93&\"P\"&IF($V93=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T93,activeElevation),\"\"))","v":""},{"$f":"IF($T93=\"Select Model\",\"\",IF($T93=\"ACBC_1W\",calcQwIP($Y93,$W93,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC93,BD93,\"capacity\",$U93&\"P\"&IF($V93=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T93,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y93,$W93,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC93,BD93,\"capacity\",$U93&\"P\"&IF($V93=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T93,activeElevation)))","v":""},"",{"$f":"IF(T93=\"Select Model\", 0,waterPressureDrop(W93, U93 & \"P\" & IF(V93=\"Dual\",2,1) &\"C\", AC93, \"cooling\", T93))","v":0},{"$f":"IF(T93=\"Select Model\", \"\",getReturnWaterTemp(T93,AC93, activeEWTCooling, AS93, \"cooling\"))","v":""},"",{"$f":"IF($T93<>\"ACBC_1W\",\"\",IF($J93=\"\",\"\",FintubeCapacity($T93,$W93,$AE93,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T93=\"Select Model\",T93=\"PCBL\"),\"\",calcQwIP(Y93,W93,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD93,BD93,\"capacity\",U93&\"P\"&IF(V93=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T93,activeElevation))","v":""},"",{"$f":"IF(OR(T93=\"Select Model\",T93=\"PCBL\"), \"\",IF(AY93=0,\"N/A\",waterPressureDrop(W93, U93 & \"P\" & IF(V93=\"Dual\",2,1) &\"C\", AD93, \"heating\", T93)))","v":""},{"$f":"IF(OR(T93=\"Select Model\",T93=\"PCBL\"), \"\",IF(AY93=0,getReturnWaterTemp(T93,AE93, activeEWTHeating, AX93, \"heating\"),getReturnWaterTemp(T93,AD93, activeEWTHeating, AY93, \"heating\")))","v":""},"",{"$f":" getNozzle(T93, W93, Y93, Z93, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I94)),I94<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I94, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H94)),H94<0),\"\",intlEstQuantity(T94, W94*12, H94)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T94=\"Select Model\",\"\",coilCircuitChange(W94, U94, AC94, T94,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T94=\"Select Model\",\"\",beamWidth(T94))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T94=\"Select Model\",T94=\"PCBL\"), 0,getSPIP(T94, W94, Y94, BD94, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T94=\"Select Model\", \"\",IF(T94=\"PCBL\",0,primaryAirSensibleCapacityIP($T94,$W94,activeRoomTempCooling,activePriAirTempCooling,$Y94,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T94=\"Select Model\",\"\",IF($T94=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y94,activeElevation)))","v":""},{"$f":"IF(OR(T94=\"Select Model\",T94=\"PCBL\"), 0,IF(AD94=0,0,-primaryAirSensibleCapacityIP($T94,$W94,activeRoomTempHeating,activePriAirTempHeating,$Y94,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T94=\"Select Model\", \"\", InductionRatio($T94,BD94,$W94,$Y94)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T94=\"Select Model\", \"\",IF($T94=\"PCBL\",\"N/A\",minVAVSetBack(AA94, Y94))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T94=\"Select Model\", \"\",IF($T94= \"PCBL\",\"N/A\",getDischargeAirTemp($T94,$V94,$AC94,$W94,BD94,$AL94, $Y94, $AS94, \"cooling\",activeElevation,$AB94,$AJ94,$AV94,$BB94))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T94=\"Select Model\",$T94=\"PCBL\"), \"\",getDischargeAirTemp($T94,$V94,$AD94,$W94,BD94,$AL94, $Y94, $AY94, \"heating\",activeElevation,$AB94,$AJ94,$AV94,$BB94)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T94=\"Select Model\", \"\",IF(OR($T94=\"ACBC_1W\",$T94=\"ACBC_2W\",LEFT($T94,4)=\"ACBR\",$T94 = \"LIU24_2W\",LEFT($T94,3)=\"RIU\",LEFT($T94,6)=\"ACBL12\"), IF((soundLevel($T94, $AB94, BD94, $Y94, $W94,$AJ94,$AA94,\"dba\"))<15,\"<15\",soundLevel($T94, $AB94, BD94, $Y94, $W94,$AJ94,$AA94,\"dba\")+0.4),IF((soundLevel($T94, $AB94, BD94, $Y94, $W94,$AJ94,$AA94,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T94, $AB94, BD94, $Y94, $W94,$AJ94,$AA94,\"dba\")+5)<15, \"<15\", soundLevel($T94, $AB94, BD94,$Y94, $W94,$AJ94,$AA94,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T94=\"Select Model\", \"\",IF(OR($T94=\"ACBC_1W\",$T94=\"ACBC_2W\",LEFT($T94,4)=\"ACBR\",$T94=\"LIU24_2W\",LEFT($T94,3)=\"RIU\",LEFT($T94,6)=\"ACBL12\"), IF((soundLevel($T94, $AB94, BD94, $Y94, $W94,$AJ94,$AA94,\"NC\"))<15,\"<15\",soundLevel($T94, $AB94, BD94, $Y94, $W94,$AJ94,$AA94,\"NC\")+0.4),IF((soundLevel($T94, $AB94, BD94, $Y94, $W94,$AJ94,$AA94,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T94, $AB94, BD94, $Y94, $W94,$AJ94,$AA94,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T94, $AB94, BD94, $Y94, $W94,$AJ94,$AA94,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T94=\"Select Model\",\"\",IF($T94=\"LIU24_2W\",calcQwIP($Y94,$W94,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC94,$AI94,\"latent\",$U94&\"P\"&IF($V94=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T94,activeElevation),\"\"))","v":""},{"$f":"IF($T94=\"Select Model\",\"\",IF($T94=\"ACBC_1W\",calcQwIP($Y94,$W94,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC94,BD94,\"capacity\",$U94&\"P\"&IF($V94=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T94,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y94,$W94,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC94,BD94,\"capacity\",$U94&\"P\"&IF($V94=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T94,activeElevation)))","v":""},"",{"$f":"IF(T94=\"Select Model\", 0,waterPressureDrop(W94, U94 & \"P\" & IF(V94=\"Dual\",2,1) &\"C\", AC94, \"cooling\", T94))","v":0},{"$f":"IF(T94=\"Select Model\", \"\",getReturnWaterTemp(T94,AC94, activeEWTCooling, AS94, \"cooling\"))","v":""},"",{"$f":"IF($T94<>\"ACBC_1W\",\"\",IF($J94=\"\",\"\",FintubeCapacity($T94,$W94,$AE94,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T94=\"Select Model\",T94=\"PCBL\"),\"\",calcQwIP(Y94,W94,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD94,BD94,\"capacity\",U94&\"P\"&IF(V94=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T94,activeElevation))","v":""},"",{"$f":"IF(OR(T94=\"Select Model\",T94=\"PCBL\"), \"\",IF(AY94=0,\"N/A\",waterPressureDrop(W94, U94 & \"P\" & IF(V94=\"Dual\",2,1) &\"C\", AD94, \"heating\", T94)))","v":""},{"$f":"IF(OR(T94=\"Select Model\",T94=\"PCBL\"), \"\",IF(AY94=0,getReturnWaterTemp(T94,AE94, activeEWTHeating, AX94, \"heating\"),getReturnWaterTemp(T94,AD94, activeEWTHeating, AY94, \"heating\")))","v":""},"",{"$f":" getNozzle(T94, W94, Y94, Z94, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I95)),I95<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I95, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H95)),H95<0),\"\",intlEstQuantity(T95, W95*12, H95)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T95=\"Select Model\",\"\",coilCircuitChange(W95, U95, AC95, T95,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T95=\"Select Model\",\"\",beamWidth(T95))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T95=\"Select Model\",T95=\"PCBL\"), 0,getSPIP(T95, W95, Y95, BD95, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T95=\"Select Model\", \"\",IF(T95=\"PCBL\",0,primaryAirSensibleCapacityIP($T95,$W95,activeRoomTempCooling,activePriAirTempCooling,$Y95,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T95=\"Select Model\",\"\",IF($T95=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y95,activeElevation)))","v":""},{"$f":"IF(OR(T95=\"Select Model\",T95=\"PCBL\"), 0,IF(AD95=0,0,-primaryAirSensibleCapacityIP($T95,$W95,activeRoomTempHeating,activePriAirTempHeating,$Y95,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T95=\"Select Model\", \"\", InductionRatio($T95,BD95,$W95,$Y95)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T95=\"Select Model\", \"\",IF($T95=\"PCBL\",\"N/A\",minVAVSetBack(AA95, Y95))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T95=\"Select Model\", \"\",IF($T95= \"PCBL\",\"N/A\",getDischargeAirTemp($T95,$V95,$AC95,$W95,BD95,$AL95, $Y95, $AS95, \"cooling\",activeElevation,$AB95,$AJ95,$AV95,$BB95))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T95=\"Select Model\",$T95=\"PCBL\"), \"\",getDischargeAirTemp($T95,$V95,$AD95,$W95,BD95,$AL95, $Y95, $AY95, \"heating\",activeElevation,$AB95,$AJ95,$AV95,$BB95)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T95=\"Select Model\", \"\",IF(OR($T95=\"ACBC_1W\",$T95=\"ACBC_2W\",LEFT($T95,4)=\"ACBR\",$T95 = \"LIU24_2W\",LEFT($T95,3)=\"RIU\",LEFT($T95,6)=\"ACBL12\"), IF((soundLevel($T95, $AB95, BD95, $Y95, $W95,$AJ95,$AA95,\"dba\"))<15,\"<15\",soundLevel($T95, $AB95, BD95, $Y95, $W95,$AJ95,$AA95,\"dba\")+0.4),IF((soundLevel($T95, $AB95, BD95, $Y95, $W95,$AJ95,$AA95,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T95, $AB95, BD95, $Y95, $W95,$AJ95,$AA95,\"dba\")+5)<15, \"<15\", soundLevel($T95, $AB95, BD95,$Y95, $W95,$AJ95,$AA95,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T95=\"Select Model\", \"\",IF(OR($T95=\"ACBC_1W\",$T95=\"ACBC_2W\",LEFT($T95,4)=\"ACBR\",$T95=\"LIU24_2W\",LEFT($T95,3)=\"RIU\",LEFT($T95,6)=\"ACBL12\"), IF((soundLevel($T95, $AB95, BD95, $Y95, $W95,$AJ95,$AA95,\"NC\"))<15,\"<15\",soundLevel($T95, $AB95, BD95, $Y95, $W95,$AJ95,$AA95,\"NC\")+0.4),IF((soundLevel($T95, $AB95, BD95, $Y95, $W95,$AJ95,$AA95,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T95, $AB95, BD95, $Y95, $W95,$AJ95,$AA95,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T95, $AB95, BD95, $Y95, $W95,$AJ95,$AA95,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T95=\"Select Model\",\"\",IF($T95=\"LIU24_2W\",calcQwIP($Y95,$W95,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC95,$AI95,\"latent\",$U95&\"P\"&IF($V95=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T95,activeElevation),\"\"))","v":""},{"$f":"IF($T95=\"Select Model\",\"\",IF($T95=\"ACBC_1W\",calcQwIP($Y95,$W95,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC95,BD95,\"capacity\",$U95&\"P\"&IF($V95=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T95,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y95,$W95,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC95,BD95,\"capacity\",$U95&\"P\"&IF($V95=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T95,activeElevation)))","v":""},"",{"$f":"IF(T95=\"Select Model\", 0,waterPressureDrop(W95, U95 & \"P\" & IF(V95=\"Dual\",2,1) &\"C\", AC95, \"cooling\", T95))","v":0},{"$f":"IF(T95=\"Select Model\", \"\",getReturnWaterTemp(T95,AC95, activeEWTCooling, AS95, \"cooling\"))","v":""},"",{"$f":"IF($T95<>\"ACBC_1W\",\"\",IF($J95=\"\",\"\",FintubeCapacity($T95,$W95,$AE95,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T95=\"Select Model\",T95=\"PCBL\"),\"\",calcQwIP(Y95,W95,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD95,BD95,\"capacity\",U95&\"P\"&IF(V95=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T95,activeElevation))","v":""},"",{"$f":"IF(OR(T95=\"Select Model\",T95=\"PCBL\"), \"\",IF(AY95=0,\"N/A\",waterPressureDrop(W95, U95 & \"P\" & IF(V95=\"Dual\",2,1) &\"C\", AD95, \"heating\", T95)))","v":""},{"$f":"IF(OR(T95=\"Select Model\",T95=\"PCBL\"), \"\",IF(AY95=0,getReturnWaterTemp(T95,AE95, activeEWTHeating, AX95, \"heating\"),getReturnWaterTemp(T95,AD95, activeEWTHeating, AY95, \"heating\")))","v":""},"",{"$f":" getNozzle(T95, W95, Y95, Z95, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I96)),I96<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I96, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H96)),H96<0),\"\",intlEstQuantity(T96, W96*12, H96)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T96=\"Select Model\",\"\",coilCircuitChange(W96, U96, AC96, T96,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T96=\"Select Model\",\"\",beamWidth(T96))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T96=\"Select Model\",T96=\"PCBL\"), 0,getSPIP(T96, W96, Y96, BD96, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T96=\"Select Model\", \"\",IF(T96=\"PCBL\",0,primaryAirSensibleCapacityIP($T96,$W96,activeRoomTempCooling,activePriAirTempCooling,$Y96,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T96=\"Select Model\",\"\",IF($T96=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y96,activeElevation)))","v":""},{"$f":"IF(OR(T96=\"Select Model\",T96=\"PCBL\"), 0,IF(AD96=0,0,-primaryAirSensibleCapacityIP($T96,$W96,activeRoomTempHeating,activePriAirTempHeating,$Y96,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T96=\"Select Model\", \"\", InductionRatio($T96,BD96,$W96,$Y96)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T96=\"Select Model\", \"\",IF($T96=\"PCBL\",\"N/A\",minVAVSetBack(AA96, Y96))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T96=\"Select Model\", \"\",IF($T96= \"PCBL\",\"N/A\",getDischargeAirTemp($T96,$V96,$AC96,$W96,BD96,$AL96, $Y96, $AS96, \"cooling\",activeElevation,$AB96,$AJ96,$AV96,$BB96))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T96=\"Select Model\",$T96=\"PCBL\"), \"\",getDischargeAirTemp($T96,$V96,$AD96,$W96,BD96,$AL96, $Y96, $AY96, \"heating\",activeElevation,$AB96,$AJ96,$AV96,$BB96)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T96=\"Select Model\", \"\",IF(OR($T96=\"ACBC_1W\",$T96=\"ACBC_2W\",LEFT($T96,4)=\"ACBR\",$T96 = \"LIU24_2W\",LEFT($T96,3)=\"RIU\",LEFT($T96,6)=\"ACBL12\"), IF((soundLevel($T96, $AB96, BD96, $Y96, $W96,$AJ96,$AA96,\"dba\"))<15,\"<15\",soundLevel($T96, $AB96, BD96, $Y96, $W96,$AJ96,$AA96,\"dba\")+0.4),IF((soundLevel($T96, $AB96, BD96, $Y96, $W96,$AJ96,$AA96,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T96, $AB96, BD96, $Y96, $W96,$AJ96,$AA96,\"dba\")+5)<15, \"<15\", soundLevel($T96, $AB96, BD96,$Y96, $W96,$AJ96,$AA96,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T96=\"Select Model\", \"\",IF(OR($T96=\"ACBC_1W\",$T96=\"ACBC_2W\",LEFT($T96,4)=\"ACBR\",$T96=\"LIU24_2W\",LEFT($T96,3)=\"RIU\",LEFT($T96,6)=\"ACBL12\"), IF((soundLevel($T96, $AB96, BD96, $Y96, $W96,$AJ96,$AA96,\"NC\"))<15,\"<15\",soundLevel($T96, $AB96, BD96, $Y96, $W96,$AJ96,$AA96,\"NC\")+0.4),IF((soundLevel($T96, $AB96, BD96, $Y96, $W96,$AJ96,$AA96,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T96, $AB96, BD96, $Y96, $W96,$AJ96,$AA96,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T96, $AB96, BD96, $Y96, $W96,$AJ96,$AA96,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T96=\"Select Model\",\"\",IF($T96=\"LIU24_2W\",calcQwIP($Y96,$W96,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC96,$AI96,\"latent\",$U96&\"P\"&IF($V96=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T96,activeElevation),\"\"))","v":""},{"$f":"IF($T96=\"Select Model\",\"\",IF($T96=\"ACBC_1W\",calcQwIP($Y96,$W96,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC96,BD96,\"capacity\",$U96&\"P\"&IF($V96=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T96,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y96,$W96,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC96,BD96,\"capacity\",$U96&\"P\"&IF($V96=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T96,activeElevation)))","v":""},"",{"$f":"IF(T96=\"Select Model\", 0,waterPressureDrop(W96, U96 & \"P\" & IF(V96=\"Dual\",2,1) &\"C\", AC96, \"cooling\", T96))","v":0},{"$f":"IF(T96=\"Select Model\", \"\",getReturnWaterTemp(T96,AC96, activeEWTCooling, AS96, \"cooling\"))","v":""},"",{"$f":"IF($T96<>\"ACBC_1W\",\"\",IF($J96=\"\",\"\",FintubeCapacity($T96,$W96,$AE96,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T96=\"Select Model\",T96=\"PCBL\"),\"\",calcQwIP(Y96,W96,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD96,BD96,\"capacity\",U96&\"P\"&IF(V96=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T96,activeElevation))","v":""},"",{"$f":"IF(OR(T96=\"Select Model\",T96=\"PCBL\"), \"\",IF(AY96=0,\"N/A\",waterPressureDrop(W96, U96 & \"P\" & IF(V96=\"Dual\",2,1) &\"C\", AD96, \"heating\", T96)))","v":""},{"$f":"IF(OR(T96=\"Select Model\",T96=\"PCBL\"), \"\",IF(AY96=0,getReturnWaterTemp(T96,AE96, activeEWTHeating, AX96, \"heating\"),getReturnWaterTemp(T96,AD96, activeEWTHeating, AY96, \"heating\")))","v":""},"",{"$f":" getNozzle(T96, W96, Y96, Z96, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I97)),I97<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I97, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H97)),H97<0),\"\",intlEstQuantity(T97, W97*12, H97)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T97=\"Select Model\",\"\",coilCircuitChange(W97, U97, AC97, T97,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T97=\"Select Model\",\"\",beamWidth(T97))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T97=\"Select Model\",T97=\"PCBL\"), 0,getSPIP(T97, W97, Y97, BD97, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T97=\"Select Model\", \"\",IF(T97=\"PCBL\",0,primaryAirSensibleCapacityIP($T97,$W97,activeRoomTempCooling,activePriAirTempCooling,$Y97,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T97=\"Select Model\",\"\",IF($T97=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y97,activeElevation)))","v":""},{"$f":"IF(OR(T97=\"Select Model\",T97=\"PCBL\"), 0,IF(AD97=0,0,-primaryAirSensibleCapacityIP($T97,$W97,activeRoomTempHeating,activePriAirTempHeating,$Y97,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T97=\"Select Model\", \"\", InductionRatio($T97,BD97,$W97,$Y97)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T97=\"Select Model\", \"\",IF($T97=\"PCBL\",\"N/A\",minVAVSetBack(AA97, Y97))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T97=\"Select Model\", \"\",IF($T97= \"PCBL\",\"N/A\",getDischargeAirTemp($T97,$V97,$AC97,$W97,BD97,$AL97, $Y97, $AS97, \"cooling\",activeElevation,$AB97,$AJ97,$AV97,$BB97))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T97=\"Select Model\",$T97=\"PCBL\"), \"\",getDischargeAirTemp($T97,$V97,$AD97,$W97,BD97,$AL97, $Y97, $AY97, \"heating\",activeElevation,$AB97,$AJ97,$AV97,$BB97)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T97=\"Select Model\", \"\",IF(OR($T97=\"ACBC_1W\",$T97=\"ACBC_2W\",LEFT($T97,4)=\"ACBR\",$T97 = \"LIU24_2W\",LEFT($T97,3)=\"RIU\",LEFT($T97,6)=\"ACBL12\"), IF((soundLevel($T97, $AB97, BD97, $Y97, $W97,$AJ97,$AA97,\"dba\"))<15,\"<15\",soundLevel($T97, $AB97, BD97, $Y97, $W97,$AJ97,$AA97,\"dba\")+0.4),IF((soundLevel($T97, $AB97, BD97, $Y97, $W97,$AJ97,$AA97,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T97, $AB97, BD97, $Y97, $W97,$AJ97,$AA97,\"dba\")+5)<15, \"<15\", soundLevel($T97, $AB97, BD97,$Y97, $W97,$AJ97,$AA97,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T97=\"Select Model\", \"\",IF(OR($T97=\"ACBC_1W\",$T97=\"ACBC_2W\",LEFT($T97,4)=\"ACBR\",$T97=\"LIU24_2W\",LEFT($T97,3)=\"RIU\",LEFT($T97,6)=\"ACBL12\"), IF((soundLevel($T97, $AB97, BD97, $Y97, $W97,$AJ97,$AA97,\"NC\"))<15,\"<15\",soundLevel($T97, $AB97, BD97, $Y97, $W97,$AJ97,$AA97,\"NC\")+0.4),IF((soundLevel($T97, $AB97, BD97, $Y97, $W97,$AJ97,$AA97,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T97, $AB97, BD97, $Y97, $W97,$AJ97,$AA97,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T97, $AB97, BD97, $Y97, $W97,$AJ97,$AA97,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T97=\"Select Model\",\"\",IF($T97=\"LIU24_2W\",calcQwIP($Y97,$W97,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC97,$AI97,\"latent\",$U97&\"P\"&IF($V97=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T97,activeElevation),\"\"))","v":""},{"$f":"IF($T97=\"Select Model\",\"\",IF($T97=\"ACBC_1W\",calcQwIP($Y97,$W97,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC97,BD97,\"capacity\",$U97&\"P\"&IF($V97=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T97,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y97,$W97,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC97,BD97,\"capacity\",$U97&\"P\"&IF($V97=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T97,activeElevation)))","v":""},"",{"$f":"IF(T97=\"Select Model\", 0,waterPressureDrop(W97, U97 & \"P\" & IF(V97=\"Dual\",2,1) &\"C\", AC97, \"cooling\", T97))","v":0},{"$f":"IF(T97=\"Select Model\", \"\",getReturnWaterTemp(T97,AC97, activeEWTCooling, AS97, \"cooling\"))","v":""},"",{"$f":"IF($T97<>\"ACBC_1W\",\"\",IF($J97=\"\",\"\",FintubeCapacity($T97,$W97,$AE97,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T97=\"Select Model\",T97=\"PCBL\"),\"\",calcQwIP(Y97,W97,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD97,BD97,\"capacity\",U97&\"P\"&IF(V97=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T97,activeElevation))","v":""},"",{"$f":"IF(OR(T97=\"Select Model\",T97=\"PCBL\"), \"\",IF(AY97=0,\"N/A\",waterPressureDrop(W97, U97 & \"P\" & IF(V97=\"Dual\",2,1) &\"C\", AD97, \"heating\", T97)))","v":""},{"$f":"IF(OR(T97=\"Select Model\",T97=\"PCBL\"), \"\",IF(AY97=0,getReturnWaterTemp(T97,AE97, activeEWTHeating, AX97, \"heating\"),getReturnWaterTemp(T97,AD97, activeEWTHeating, AY97, \"heating\")))","v":""},"",{"$f":" getNozzle(T97, W97, Y97, Z97, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I98)),I98<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I98, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H98)),H98<0),\"\",intlEstQuantity(T98, W98*12, H98)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T98=\"Select Model\",\"\",coilCircuitChange(W98, U98, AC98, T98,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T98=\"Select Model\",\"\",beamWidth(T98))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T98=\"Select Model\",T98=\"PCBL\"), 0,getSPIP(T98, W98, Y98, BD98, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T98=\"Select Model\", \"\",IF(T98=\"PCBL\",0,primaryAirSensibleCapacityIP($T98,$W98,activeRoomTempCooling,activePriAirTempCooling,$Y98,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T98=\"Select Model\",\"\",IF($T98=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y98,activeElevation)))","v":""},{"$f":"IF(OR(T98=\"Select Model\",T98=\"PCBL\"), 0,IF(AD98=0,0,-primaryAirSensibleCapacityIP($T98,$W98,activeRoomTempHeating,activePriAirTempHeating,$Y98,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T98=\"Select Model\", \"\", InductionRatio($T98,BD98,$W98,$Y98)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T98=\"Select Model\", \"\",IF($T98=\"PCBL\",\"N/A\",minVAVSetBack(AA98, Y98))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T98=\"Select Model\", \"\",IF($T98= \"PCBL\",\"N/A\",getDischargeAirTemp($T98,$V98,$AC98,$W98,BD98,$AL98, $Y98, $AS98, \"cooling\",activeElevation,$AB98,$AJ98,$AV98,$BB98))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T98=\"Select Model\",$T98=\"PCBL\"), \"\",getDischargeAirTemp($T98,$V98,$AD98,$W98,BD98,$AL98, $Y98, $AY98, \"heating\",activeElevation,$AB98,$AJ98,$AV98,$BB98)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T98=\"Select Model\", \"\",IF(OR($T98=\"ACBC_1W\",$T98=\"ACBC_2W\",LEFT($T98,4)=\"ACBR\",$T98 = \"LIU24_2W\",LEFT($T98,3)=\"RIU\",LEFT($T98,6)=\"ACBL12\"), IF((soundLevel($T98, $AB98, BD98, $Y98, $W98,$AJ98,$AA98,\"dba\"))<15,\"<15\",soundLevel($T98, $AB98, BD98, $Y98, $W98,$AJ98,$AA98,\"dba\")+0.4),IF((soundLevel($T98, $AB98, BD98, $Y98, $W98,$AJ98,$AA98,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T98, $AB98, BD98, $Y98, $W98,$AJ98,$AA98,\"dba\")+5)<15, \"<15\", soundLevel($T98, $AB98, BD98,$Y98, $W98,$AJ98,$AA98,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T98=\"Select Model\", \"\",IF(OR($T98=\"ACBC_1W\",$T98=\"ACBC_2W\",LEFT($T98,4)=\"ACBR\",$T98=\"LIU24_2W\",LEFT($T98,3)=\"RIU\",LEFT($T98,6)=\"ACBL12\"), IF((soundLevel($T98, $AB98, BD98, $Y98, $W98,$AJ98,$AA98,\"NC\"))<15,\"<15\",soundLevel($T98, $AB98, BD98, $Y98, $W98,$AJ98,$AA98,\"NC\")+0.4),IF((soundLevel($T98, $AB98, BD98, $Y98, $W98,$AJ98,$AA98,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T98, $AB98, BD98, $Y98, $W98,$AJ98,$AA98,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T98, $AB98, BD98, $Y98, $W98,$AJ98,$AA98,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T98=\"Select Model\",\"\",IF($T98=\"LIU24_2W\",calcQwIP($Y98,$W98,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC98,$AI98,\"latent\",$U98&\"P\"&IF($V98=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T98,activeElevation),\"\"))","v":""},{"$f":"IF($T98=\"Select Model\",\"\",IF($T98=\"ACBC_1W\",calcQwIP($Y98,$W98,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC98,BD98,\"capacity\",$U98&\"P\"&IF($V98=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T98,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y98,$W98,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC98,BD98,\"capacity\",$U98&\"P\"&IF($V98=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T98,activeElevation)))","v":""},"",{"$f":"IF(T98=\"Select Model\", 0,waterPressureDrop(W98, U98 & \"P\" & IF(V98=\"Dual\",2,1) &\"C\", AC98, \"cooling\", T98))","v":0},{"$f":"IF(T98=\"Select Model\", \"\",getReturnWaterTemp(T98,AC98, activeEWTCooling, AS98, \"cooling\"))","v":""},"",{"$f":"IF($T98<>\"ACBC_1W\",\"\",IF($J98=\"\",\"\",FintubeCapacity($T98,$W98,$AE98,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T98=\"Select Model\",T98=\"PCBL\"),\"\",calcQwIP(Y98,W98,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD98,BD98,\"capacity\",U98&\"P\"&IF(V98=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T98,activeElevation))","v":""},"",{"$f":"IF(OR(T98=\"Select Model\",T98=\"PCBL\"), \"\",IF(AY98=0,\"N/A\",waterPressureDrop(W98, U98 & \"P\" & IF(V98=\"Dual\",2,1) &\"C\", AD98, \"heating\", T98)))","v":""},{"$f":"IF(OR(T98=\"Select Model\",T98=\"PCBL\"), \"\",IF(AY98=0,getReturnWaterTemp(T98,AE98, activeEWTHeating, AX98, \"heating\"),getReturnWaterTemp(T98,AD98, activeEWTHeating, AY98, \"heating\")))","v":""},"",{"$f":" getNozzle(T98, W98, Y98, Z98, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I99)),I99<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I99, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H99)),H99<0),\"\",intlEstQuantity(T99, W99*12, H99)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T99=\"Select Model\",\"\",coilCircuitChange(W99, U99, AC99, T99,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T99=\"Select Model\",\"\",beamWidth(T99))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T99=\"Select Model\",T99=\"PCBL\"), 0,getSPIP(T99, W99, Y99, BD99, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T99=\"Select Model\", \"\",IF(T99=\"PCBL\",0,primaryAirSensibleCapacityIP($T99,$W99,activeRoomTempCooling,activePriAirTempCooling,$Y99,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T99=\"Select Model\",\"\",IF($T99=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y99,activeElevation)))","v":""},{"$f":"IF(OR(T99=\"Select Model\",T99=\"PCBL\"), 0,IF(AD99=0,0,-primaryAirSensibleCapacityIP($T99,$W99,activeRoomTempHeating,activePriAirTempHeating,$Y99,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T99=\"Select Model\", \"\", InductionRatio($T99,BD99,$W99,$Y99)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T99=\"Select Model\", \"\",IF($T99=\"PCBL\",\"N/A\",minVAVSetBack(AA99, Y99))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T99=\"Select Model\", \"\",IF($T99= \"PCBL\",\"N/A\",getDischargeAirTemp($T99,$V99,$AC99,$W99,BD99,$AL99, $Y99, $AS99, \"cooling\",activeElevation,$AB99,$AJ99,$AV99,$BB99))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T99=\"Select Model\",$T99=\"PCBL\"), \"\",getDischargeAirTemp($T99,$V99,$AD99,$W99,BD99,$AL99, $Y99, $AY99, \"heating\",activeElevation,$AB99,$AJ99,$AV99,$BB99)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T99=\"Select Model\", \"\",IF(OR($T99=\"ACBC_1W\",$T99=\"ACBC_2W\",LEFT($T99,4)=\"ACBR\",$T99 = \"LIU24_2W\",LEFT($T99,3)=\"RIU\",LEFT($T99,6)=\"ACBL12\"), IF((soundLevel($T99, $AB99, BD99, $Y99, $W99,$AJ99,$AA99,\"dba\"))<15,\"<15\",soundLevel($T99, $AB99, BD99, $Y99, $W99,$AJ99,$AA99,\"dba\")+0.4),IF((soundLevel($T99, $AB99, BD99, $Y99, $W99,$AJ99,$AA99,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T99, $AB99, BD99, $Y99, $W99,$AJ99,$AA99,\"dba\")+5)<15, \"<15\", soundLevel($T99, $AB99, BD99,$Y99, $W99,$AJ99,$AA99,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T99=\"Select Model\", \"\",IF(OR($T99=\"ACBC_1W\",$T99=\"ACBC_2W\",LEFT($T99,4)=\"ACBR\",$T99=\"LIU24_2W\",LEFT($T99,3)=\"RIU\",LEFT($T99,6)=\"ACBL12\"), IF((soundLevel($T99, $AB99, BD99, $Y99, $W99,$AJ99,$AA99,\"NC\"))<15,\"<15\",soundLevel($T99, $AB99, BD99, $Y99, $W99,$AJ99,$AA99,\"NC\")+0.4),IF((soundLevel($T99, $AB99, BD99, $Y99, $W99,$AJ99,$AA99,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T99, $AB99, BD99, $Y99, $W99,$AJ99,$AA99,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T99, $AB99, BD99, $Y99, $W99,$AJ99,$AA99,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T99=\"Select Model\",\"\",IF($T99=\"LIU24_2W\",calcQwIP($Y99,$W99,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC99,$AI99,\"latent\",$U99&\"P\"&IF($V99=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T99,activeElevation),\"\"))","v":""},{"$f":"IF($T99=\"Select Model\",\"\",IF($T99=\"ACBC_1W\",calcQwIP($Y99,$W99,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC99,BD99,\"capacity\",$U99&\"P\"&IF($V99=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T99,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y99,$W99,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC99,BD99,\"capacity\",$U99&\"P\"&IF($V99=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T99,activeElevation)))","v":""},"",{"$f":"IF(T99=\"Select Model\", 0,waterPressureDrop(W99, U99 & \"P\" & IF(V99=\"Dual\",2,1) &\"C\", AC99, \"cooling\", T99))","v":0},{"$f":"IF(T99=\"Select Model\", \"\",getReturnWaterTemp(T99,AC99, activeEWTCooling, AS99, \"cooling\"))","v":""},"",{"$f":"IF($T99<>\"ACBC_1W\",\"\",IF($J99=\"\",\"\",FintubeCapacity($T99,$W99,$AE99,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T99=\"Select Model\",T99=\"PCBL\"),\"\",calcQwIP(Y99,W99,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD99,BD99,\"capacity\",U99&\"P\"&IF(V99=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T99,activeElevation))","v":""},"",{"$f":"IF(OR(T99=\"Select Model\",T99=\"PCBL\"), \"\",IF(AY99=0,\"N/A\",waterPressureDrop(W99, U99 & \"P\" & IF(V99=\"Dual\",2,1) &\"C\", AD99, \"heating\", T99)))","v":""},{"$f":"IF(OR(T99=\"Select Model\",T99=\"PCBL\"), \"\",IF(AY99=0,getReturnWaterTemp(T99,AE99, activeEWTHeating, AX99, \"heating\"),getReturnWaterTemp(T99,AD99, activeEWTHeating, AY99, \"heating\")))","v":""},"",{"$f":" getNozzle(T99, W99, Y99, Z99, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I100)),I100<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I100, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H100)),H100<0),\"\",intlEstQuantity(T100, W100*12, H100)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T100=\"Select Model\",\"\",coilCircuitChange(W100, U100, AC100, T100,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T100=\"Select Model\",\"\",beamWidth(T100))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T100=\"Select Model\",T100=\"PCBL\"), 0,getSPIP(T100, W100, Y100, BD100, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T100=\"Select Model\", \"\",IF(T100=\"PCBL\",0,primaryAirSensibleCapacityIP($T100,$W100,activeRoomTempCooling,activePriAirTempCooling,$Y100,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T100=\"Select Model\",\"\",IF($T100=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y100,activeElevation)))","v":""},{"$f":"IF(OR(T100=\"Select Model\",T100=\"PCBL\"), 0,IF(AD100=0,0,-primaryAirSensibleCapacityIP($T100,$W100,activeRoomTempHeating,activePriAirTempHeating,$Y100,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T100=\"Select Model\", \"\", InductionRatio($T100,BD100,$W100,$Y100)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T100=\"Select Model\", \"\",IF($T100=\"PCBL\",\"N/A\",minVAVSetBack(AA100, Y100))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T100=\"Select Model\", \"\",IF($T100= \"PCBL\",\"N/A\",getDischargeAirTemp($T100,$V100,$AC100,$W100,BD100,$AL100, $Y100, $AS100, \"cooling\",activeElevation,$AB100,$AJ100,$AV100,$BB100))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T100=\"Select Model\",$T100=\"PCBL\"), \"\",getDischargeAirTemp($T100,$V100,$AD100,$W100,BD100,$AL100, $Y100, $AY100, \"heating\",activeElevation,$AB100,$AJ100,$AV100,$BB100)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T100=\"Select Model\", \"\",IF(OR($T100=\"ACBC_1W\",$T100=\"ACBC_2W\",LEFT($T100,4)=\"ACBR\",$T100 = \"LIU24_2W\",LEFT($T100,3)=\"RIU\",LEFT($T100,6)=\"ACBL12\"), IF((soundLevel($T100, $AB100, BD100, $Y100, $W100,$AJ100,$AA100,\"dba\"))<15,\"<15\",soundLevel($T100, $AB100, BD100, $Y100, $W100,$AJ100,$AA100,\"dba\")+0.4),IF((soundLevel($T100, $AB100, BD100, $Y100, $W100,$AJ100,$AA100,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T100, $AB100, BD100, $Y100, $W100,$AJ100,$AA100,\"dba\")+5)<15, \"<15\", soundLevel($T100, $AB100, BD100,$Y100, $W100,$AJ100,$AA100,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T100=\"Select Model\", \"\",IF(OR($T100=\"ACBC_1W\",$T100=\"ACBC_2W\",LEFT($T100,4)=\"ACBR\",$T100=\"LIU24_2W\",LEFT($T100,3)=\"RIU\",LEFT($T100,6)=\"ACBL12\"), IF((soundLevel($T100, $AB100, BD100, $Y100, $W100,$AJ100,$AA100,\"NC\"))<15,\"<15\",soundLevel($T100, $AB100, BD100, $Y100, $W100,$AJ100,$AA100,\"NC\")+0.4),IF((soundLevel($T100, $AB100, BD100, $Y100, $W100,$AJ100,$AA100,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T100, $AB100, BD100, $Y100, $W100,$AJ100,$AA100,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T100, $AB100, BD100, $Y100, $W100,$AJ100,$AA100,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T100=\"Select Model\",\"\",IF($T100=\"LIU24_2W\",calcQwIP($Y100,$W100,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC100,$AI100,\"latent\",$U100&\"P\"&IF($V100=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T100,activeElevation),\"\"))","v":""},{"$f":"IF($T100=\"Select Model\",\"\",IF($T100=\"ACBC_1W\",calcQwIP($Y100,$W100,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC100,BD100,\"capacity\",$U100&\"P\"&IF($V100=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T100,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y100,$W100,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC100,BD100,\"capacity\",$U100&\"P\"&IF($V100=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T100,activeElevation)))","v":""},"",{"$f":"IF(T100=\"Select Model\", 0,waterPressureDrop(W100, U100 & \"P\" & IF(V100=\"Dual\",2,1) &\"C\", AC100, \"cooling\", T100))","v":0},{"$f":"IF(T100=\"Select Model\", \"\",getReturnWaterTemp(T100,AC100, activeEWTCooling, AS100, \"cooling\"))","v":""},"",{"$f":"IF($T100<>\"ACBC_1W\",\"\",IF($J100=\"\",\"\",FintubeCapacity($T100,$W100,$AE100,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T100=\"Select Model\",T100=\"PCBL\"),\"\",calcQwIP(Y100,W100,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD100,BD100,\"capacity\",U100&\"P\"&IF(V100=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T100,activeElevation))","v":""},"",{"$f":"IF(OR(T100=\"Select Model\",T100=\"PCBL\"), \"\",IF(AY100=0,\"N/A\",waterPressureDrop(W100, U100 & \"P\" & IF(V100=\"Dual\",2,1) &\"C\", AD100, \"heating\", T100)))","v":""},{"$f":"IF(OR(T100=\"Select Model\",T100=\"PCBL\"), \"\",IF(AY100=0,getReturnWaterTemp(T100,AE100, activeEWTHeating, AX100, \"heating\"),getReturnWaterTemp(T100,AD100, activeEWTHeating, AY100, \"heating\")))","v":""},"",{"$f":" getNozzle(T100, W100, Y100, Z100, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I101)),I101<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I101, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H101)),H101<0),\"\",intlEstQuantity(T101, W101*12, H101)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T101=\"Select Model\",\"\",coilCircuitChange(W101, U101, AC101, T101,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T101=\"Select Model\",\"\",beamWidth(T101))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T101=\"Select Model\",T101=\"PCBL\"), 0,getSPIP(T101, W101, Y101, BD101, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T101=\"Select Model\", \"\",IF(T101=\"PCBL\",0,primaryAirSensibleCapacityIP($T101,$W101,activeRoomTempCooling,activePriAirTempCooling,$Y101,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T101=\"Select Model\",\"\",IF($T101=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y101,activeElevation)))","v":""},{"$f":"IF(OR(T101=\"Select Model\",T101=\"PCBL\"), 0,IF(AD101=0,0,-primaryAirSensibleCapacityIP($T101,$W101,activeRoomTempHeating,activePriAirTempHeating,$Y101,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T101=\"Select Model\", \"\", InductionRatio($T101,BD101,$W101,$Y101)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T101=\"Select Model\", \"\",IF($T101=\"PCBL\",\"N/A\",minVAVSetBack(AA101, Y101))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T101=\"Select Model\", \"\",IF($T101= \"PCBL\",\"N/A\",getDischargeAirTemp($T101,$V101,$AC101,$W101,BD101,$AL101, $Y101, $AS101, \"cooling\",activeElevation,$AB101,$AJ101,$AV101,$BB101))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T101=\"Select Model\",$T101=\"PCBL\"), \"\",getDischargeAirTemp($T101,$V101,$AD101,$W101,BD101,$AL101, $Y101, $AY101, \"heating\",activeElevation,$AB101,$AJ101,$AV101,$BB101)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T101=\"Select Model\", \"\",IF(OR($T101=\"ACBC_1W\",$T101=\"ACBC_2W\",LEFT($T101,4)=\"ACBR\",$T101 = \"LIU24_2W\",LEFT($T101,3)=\"RIU\",LEFT($T101,6)=\"ACBL12\"), IF((soundLevel($T101, $AB101, BD101, $Y101, $W101,$AJ101,$AA101,\"dba\"))<15,\"<15\",soundLevel($T101, $AB101, BD101, $Y101, $W101,$AJ101,$AA101,\"dba\")+0.4),IF((soundLevel($T101, $AB101, BD101, $Y101, $W101,$AJ101,$AA101,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T101, $AB101, BD101, $Y101, $W101,$AJ101,$AA101,\"dba\")+5)<15, \"<15\", soundLevel($T101, $AB101, BD101,$Y101, $W101,$AJ101,$AA101,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T101=\"Select Model\", \"\",IF(OR($T101=\"ACBC_1W\",$T101=\"ACBC_2W\",LEFT($T101,4)=\"ACBR\",$T101=\"LIU24_2W\",LEFT($T101,3)=\"RIU\",LEFT($T101,6)=\"ACBL12\"), IF((soundLevel($T101, $AB101, BD101, $Y101, $W101,$AJ101,$AA101,\"NC\"))<15,\"<15\",soundLevel($T101, $AB101, BD101, $Y101, $W101,$AJ101,$AA101,\"NC\")+0.4),IF((soundLevel($T101, $AB101, BD101, $Y101, $W101,$AJ101,$AA101,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T101, $AB101, BD101, $Y101, $W101,$AJ101,$AA101,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T101, $AB101, BD101, $Y101, $W101,$AJ101,$AA101,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T101=\"Select Model\",\"\",IF($T101=\"LIU24_2W\",calcQwIP($Y101,$W101,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC101,$AI101,\"latent\",$U101&\"P\"&IF($V101=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T101,activeElevation),\"\"))","v":""},{"$f":"IF($T101=\"Select Model\",\"\",IF($T101=\"ACBC_1W\",calcQwIP($Y101,$W101,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC101,BD101,\"capacity\",$U101&\"P\"&IF($V101=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T101,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y101,$W101,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC101,BD101,\"capacity\",$U101&\"P\"&IF($V101=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T101,activeElevation)))","v":""},"",{"$f":"IF(T101=\"Select Model\", 0,waterPressureDrop(W101, U101 & \"P\" & IF(V101=\"Dual\",2,1) &\"C\", AC101, \"cooling\", T101))","v":0},{"$f":"IF(T101=\"Select Model\", \"\",getReturnWaterTemp(T101,AC101, activeEWTCooling, AS101, \"cooling\"))","v":""},"",{"$f":"IF($T101<>\"ACBC_1W\",\"\",IF($J101=\"\",\"\",FintubeCapacity($T101,$W101,$AE101,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T101=\"Select Model\",T101=\"PCBL\"),\"\",calcQwIP(Y101,W101,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD101,BD101,\"capacity\",U101&\"P\"&IF(V101=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T101,activeElevation))","v":""},"",{"$f":"IF(OR(T101=\"Select Model\",T101=\"PCBL\"), \"\",IF(AY101=0,\"N/A\",waterPressureDrop(W101, U101 & \"P\" & IF(V101=\"Dual\",2,1) &\"C\", AD101, \"heating\", T101)))","v":""},{"$f":"IF(OR(T101=\"Select Model\",T101=\"PCBL\"), \"\",IF(AY101=0,getReturnWaterTemp(T101,AE101, activeEWTHeating, AX101, \"heating\"),getReturnWaterTemp(T101,AD101, activeEWTHeating, AY101, \"heating\")))","v":""},"",{"$f":" getNozzle(T101, W101, Y101, Z101, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I102)),I102<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I102, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H102)),H102<0),\"\",intlEstQuantity(T102, W102*12, H102)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T102=\"Select Model\",\"\",coilCircuitChange(W102, U102, AC102, T102,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T102=\"Select Model\",\"\",beamWidth(T102))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T102=\"Select Model\",T102=\"PCBL\"), 0,getSPIP(T102, W102, Y102, BD102, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T102=\"Select Model\", \"\",IF(T102=\"PCBL\",0,primaryAirSensibleCapacityIP($T102,$W102,activeRoomTempCooling,activePriAirTempCooling,$Y102,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T102=\"Select Model\",\"\",IF($T102=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y102,activeElevation)))","v":""},{"$f":"IF(OR(T102=\"Select Model\",T102=\"PCBL\"), 0,IF(AD102=0,0,-primaryAirSensibleCapacityIP($T102,$W102,activeRoomTempHeating,activePriAirTempHeating,$Y102,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T102=\"Select Model\", \"\", InductionRatio($T102,BD102,$W102,$Y102)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T102=\"Select Model\", \"\",IF($T102=\"PCBL\",\"N/A\",minVAVSetBack(AA102, Y102))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T102=\"Select Model\", \"\",IF($T102= \"PCBL\",\"N/A\",getDischargeAirTemp($T102,$V102,$AC102,$W102,BD102,$AL102, $Y102, $AS102, \"cooling\",activeElevation,$AB102,$AJ102,$AV102,$BB102))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T102=\"Select Model\",$T102=\"PCBL\"), \"\",getDischargeAirTemp($T102,$V102,$AD102,$W102,BD102,$AL102, $Y102, $AY102, \"heating\",activeElevation,$AB102,$AJ102,$AV102,$BB102)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T102=\"Select Model\", \"\",IF(OR($T102=\"ACBC_1W\",$T102=\"ACBC_2W\",LEFT($T102,4)=\"ACBR\",$T102 = \"LIU24_2W\",LEFT($T102,3)=\"RIU\",LEFT($T102,6)=\"ACBL12\"), IF((soundLevel($T102, $AB102, BD102, $Y102, $W102,$AJ102,$AA102,\"dba\"))<15,\"<15\",soundLevel($T102, $AB102, BD102, $Y102, $W102,$AJ102,$AA102,\"dba\")+0.4),IF((soundLevel($T102, $AB102, BD102, $Y102, $W102,$AJ102,$AA102,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T102, $AB102, BD102, $Y102, $W102,$AJ102,$AA102,\"dba\")+5)<15, \"<15\", soundLevel($T102, $AB102, BD102,$Y102, $W102,$AJ102,$AA102,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T102=\"Select Model\", \"\",IF(OR($T102=\"ACBC_1W\",$T102=\"ACBC_2W\",LEFT($T102,4)=\"ACBR\",$T102=\"LIU24_2W\",LEFT($T102,3)=\"RIU\",LEFT($T102,6)=\"ACBL12\"), IF((soundLevel($T102, $AB102, BD102, $Y102, $W102,$AJ102,$AA102,\"NC\"))<15,\"<15\",soundLevel($T102, $AB102, BD102, $Y102, $W102,$AJ102,$AA102,\"NC\")+0.4),IF((soundLevel($T102, $AB102, BD102, $Y102, $W102,$AJ102,$AA102,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T102, $AB102, BD102, $Y102, $W102,$AJ102,$AA102,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T102, $AB102, BD102, $Y102, $W102,$AJ102,$AA102,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T102=\"Select Model\",\"\",IF($T102=\"LIU24_2W\",calcQwIP($Y102,$W102,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC102,$AI102,\"latent\",$U102&\"P\"&IF($V102=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T102,activeElevation),\"\"))","v":""},{"$f":"IF($T102=\"Select Model\",\"\",IF($T102=\"ACBC_1W\",calcQwIP($Y102,$W102,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC102,BD102,\"capacity\",$U102&\"P\"&IF($V102=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T102,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y102,$W102,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC102,BD102,\"capacity\",$U102&\"P\"&IF($V102=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T102,activeElevation)))","v":""},"",{"$f":"IF(T102=\"Select Model\", 0,waterPressureDrop(W102, U102 & \"P\" & IF(V102=\"Dual\",2,1) &\"C\", AC102, \"cooling\", T102))","v":0},{"$f":"IF(T102=\"Select Model\", \"\",getReturnWaterTemp(T102,AC102, activeEWTCooling, AS102, \"cooling\"))","v":""},"",{"$f":"IF($T102<>\"ACBC_1W\",\"\",IF($J102=\"\",\"\",FintubeCapacity($T102,$W102,$AE102,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T102=\"Select Model\",T102=\"PCBL\"),\"\",calcQwIP(Y102,W102,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD102,BD102,\"capacity\",U102&\"P\"&IF(V102=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T102,activeElevation))","v":""},"",{"$f":"IF(OR(T102=\"Select Model\",T102=\"PCBL\"), \"\",IF(AY102=0,\"N/A\",waterPressureDrop(W102, U102 & \"P\" & IF(V102=\"Dual\",2,1) &\"C\", AD102, \"heating\", T102)))","v":""},{"$f":"IF(OR(T102=\"Select Model\",T102=\"PCBL\"), \"\",IF(AY102=0,getReturnWaterTemp(T102,AE102, activeEWTHeating, AX102, \"heating\"),getReturnWaterTemp(T102,AD102, activeEWTHeating, AY102, \"heating\")))","v":""},"",{"$f":" getNozzle(T102, W102, Y102, Z102, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I103)),I103<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I103, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H103)),H103<0),\"\",intlEstQuantity(T103, W103*12, H103)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T103=\"Select Model\",\"\",coilCircuitChange(W103, U103, AC103, T103,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T103=\"Select Model\",\"\",beamWidth(T103))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T103=\"Select Model\",T103=\"PCBL\"), 0,getSPIP(T103, W103, Y103, BD103, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T103=\"Select Model\", \"\",IF(T103=\"PCBL\",0,primaryAirSensibleCapacityIP($T103,$W103,activeRoomTempCooling,activePriAirTempCooling,$Y103,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T103=\"Select Model\",\"\",IF($T103=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y103,activeElevation)))","v":""},{"$f":"IF(OR(T103=\"Select Model\",T103=\"PCBL\"), 0,IF(AD103=0,0,-primaryAirSensibleCapacityIP($T103,$W103,activeRoomTempHeating,activePriAirTempHeating,$Y103,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T103=\"Select Model\", \"\", InductionRatio($T103,BD103,$W103,$Y103)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T103=\"Select Model\", \"\",IF($T103=\"PCBL\",\"N/A\",minVAVSetBack(AA103, Y103))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T103=\"Select Model\", \"\",IF($T103= \"PCBL\",\"N/A\",getDischargeAirTemp($T103,$V103,$AC103,$W103,BD103,$AL103, $Y103, $AS103, \"cooling\",activeElevation,$AB103,$AJ103,$AV103,$BB103))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T103=\"Select Model\",$T103=\"PCBL\"), \"\",getDischargeAirTemp($T103,$V103,$AD103,$W103,BD103,$AL103, $Y103, $AY103, \"heating\",activeElevation,$AB103,$AJ103,$AV103,$BB103)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T103=\"Select Model\", \"\",IF(OR($T103=\"ACBC_1W\",$T103=\"ACBC_2W\",LEFT($T103,4)=\"ACBR\",$T103 = \"LIU24_2W\",LEFT($T103,3)=\"RIU\",LEFT($T103,6)=\"ACBL12\"), IF((soundLevel($T103, $AB103, BD103, $Y103, $W103,$AJ103,$AA103,\"dba\"))<15,\"<15\",soundLevel($T103, $AB103, BD103, $Y103, $W103,$AJ103,$AA103,\"dba\")+0.4),IF((soundLevel($T103, $AB103, BD103, $Y103, $W103,$AJ103,$AA103,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T103, $AB103, BD103, $Y103, $W103,$AJ103,$AA103,\"dba\")+5)<15, \"<15\", soundLevel($T103, $AB103, BD103,$Y103, $W103,$AJ103,$AA103,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T103=\"Select Model\", \"\",IF(OR($T103=\"ACBC_1W\",$T103=\"ACBC_2W\",LEFT($T103,4)=\"ACBR\",$T103=\"LIU24_2W\",LEFT($T103,3)=\"RIU\",LEFT($T103,6)=\"ACBL12\"), IF((soundLevel($T103, $AB103, BD103, $Y103, $W103,$AJ103,$AA103,\"NC\"))<15,\"<15\",soundLevel($T103, $AB103, BD103, $Y103, $W103,$AJ103,$AA103,\"NC\")+0.4),IF((soundLevel($T103, $AB103, BD103, $Y103, $W103,$AJ103,$AA103,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T103, $AB103, BD103, $Y103, $W103,$AJ103,$AA103,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T103, $AB103, BD103, $Y103, $W103,$AJ103,$AA103,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T103=\"Select Model\",\"\",IF($T103=\"LIU24_2W\",calcQwIP($Y103,$W103,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC103,$AI103,\"latent\",$U103&\"P\"&IF($V103=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T103,activeElevation),\"\"))","v":""},{"$f":"IF($T103=\"Select Model\",\"\",IF($T103=\"ACBC_1W\",calcQwIP($Y103,$W103,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC103,BD103,\"capacity\",$U103&\"P\"&IF($V103=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T103,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y103,$W103,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC103,BD103,\"capacity\",$U103&\"P\"&IF($V103=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T103,activeElevation)))","v":""},"",{"$f":"IF(T103=\"Select Model\", 0,waterPressureDrop(W103, U103 & \"P\" & IF(V103=\"Dual\",2,1) &\"C\", AC103, \"cooling\", T103))","v":0},{"$f":"IF(T103=\"Select Model\", \"\",getReturnWaterTemp(T103,AC103, activeEWTCooling, AS103, \"cooling\"))","v":""},"",{"$f":"IF($T103<>\"ACBC_1W\",\"\",IF($J103=\"\",\"\",FintubeCapacity($T103,$W103,$AE103,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T103=\"Select Model\",T103=\"PCBL\"),\"\",calcQwIP(Y103,W103,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD103,BD103,\"capacity\",U103&\"P\"&IF(V103=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T103,activeElevation))","v":""},"",{"$f":"IF(OR(T103=\"Select Model\",T103=\"PCBL\"), \"\",IF(AY103=0,\"N/A\",waterPressureDrop(W103, U103 & \"P\" & IF(V103=\"Dual\",2,1) &\"C\", AD103, \"heating\", T103)))","v":""},{"$f":"IF(OR(T103=\"Select Model\",T103=\"PCBL\"), \"\",IF(AY103=0,getReturnWaterTemp(T103,AE103, activeEWTHeating, AX103, \"heating\"),getReturnWaterTemp(T103,AD103, activeEWTHeating, AY103, \"heating\")))","v":""},"",{"$f":" getNozzle(T103, W103, Y103, Z103, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I104)),I104<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I104, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H104)),H104<0),\"\",intlEstQuantity(T104, W104*12, H104)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T104=\"Select Model\",\"\",coilCircuitChange(W104, U104, AC104, T104,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T104=\"Select Model\",\"\",beamWidth(T104))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T104=\"Select Model\",T104=\"PCBL\"), 0,getSPIP(T104, W104, Y104, BD104, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T104=\"Select Model\", \"\",IF(T104=\"PCBL\",0,primaryAirSensibleCapacityIP($T104,$W104,activeRoomTempCooling,activePriAirTempCooling,$Y104,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T104=\"Select Model\",\"\",IF($T104=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y104,activeElevation)))","v":""},{"$f":"IF(OR(T104=\"Select Model\",T104=\"PCBL\"), 0,IF(AD104=0,0,-primaryAirSensibleCapacityIP($T104,$W104,activeRoomTempHeating,activePriAirTempHeating,$Y104,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T104=\"Select Model\", \"\", InductionRatio($T104,BD104,$W104,$Y104)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T104=\"Select Model\", \"\",IF($T104=\"PCBL\",\"N/A\",minVAVSetBack(AA104, Y104))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T104=\"Select Model\", \"\",IF($T104= \"PCBL\",\"N/A\",getDischargeAirTemp($T104,$V104,$AC104,$W104,BD104,$AL104, $Y104, $AS104, \"cooling\",activeElevation,$AB104,$AJ104,$AV104,$BB104))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T104=\"Select Model\",$T104=\"PCBL\"), \"\",getDischargeAirTemp($T104,$V104,$AD104,$W104,BD104,$AL104, $Y104, $AY104, \"heating\",activeElevation,$AB104,$AJ104,$AV104,$BB104)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T104=\"Select Model\", \"\",IF(OR($T104=\"ACBC_1W\",$T104=\"ACBC_2W\",LEFT($T104,4)=\"ACBR\",$T104 = \"LIU24_2W\",LEFT($T104,3)=\"RIU\",LEFT($T104,6)=\"ACBL12\"), IF((soundLevel($T104, $AB104, BD104, $Y104, $W104,$AJ104,$AA104,\"dba\"))<15,\"<15\",soundLevel($T104, $AB104, BD104, $Y104, $W104,$AJ104,$AA104,\"dba\")+0.4),IF((soundLevel($T104, $AB104, BD104, $Y104, $W104,$AJ104,$AA104,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T104, $AB104, BD104, $Y104, $W104,$AJ104,$AA104,\"dba\")+5)<15, \"<15\", soundLevel($T104, $AB104, BD104,$Y104, $W104,$AJ104,$AA104,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T104=\"Select Model\", \"\",IF(OR($T104=\"ACBC_1W\",$T104=\"ACBC_2W\",LEFT($T104,4)=\"ACBR\",$T104=\"LIU24_2W\",LEFT($T104,3)=\"RIU\",LEFT($T104,6)=\"ACBL12\"), IF((soundLevel($T104, $AB104, BD104, $Y104, $W104,$AJ104,$AA104,\"NC\"))<15,\"<15\",soundLevel($T104, $AB104, BD104, $Y104, $W104,$AJ104,$AA104,\"NC\")+0.4),IF((soundLevel($T104, $AB104, BD104, $Y104, $W104,$AJ104,$AA104,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T104, $AB104, BD104, $Y104, $W104,$AJ104,$AA104,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T104, $AB104, BD104, $Y104, $W104,$AJ104,$AA104,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T104=\"Select Model\",\"\",IF($T104=\"LIU24_2W\",calcQwIP($Y104,$W104,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC104,$AI104,\"latent\",$U104&\"P\"&IF($V104=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T104,activeElevation),\"\"))","v":""},{"$f":"IF($T104=\"Select Model\",\"\",IF($T104=\"ACBC_1W\",calcQwIP($Y104,$W104,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC104,BD104,\"capacity\",$U104&\"P\"&IF($V104=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T104,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y104,$W104,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC104,BD104,\"capacity\",$U104&\"P\"&IF($V104=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T104,activeElevation)))","v":""},"",{"$f":"IF(T104=\"Select Model\", 0,waterPressureDrop(W104, U104 & \"P\" & IF(V104=\"Dual\",2,1) &\"C\", AC104, \"cooling\", T104))","v":0},{"$f":"IF(T104=\"Select Model\", \"\",getReturnWaterTemp(T104,AC104, activeEWTCooling, AS104, \"cooling\"))","v":""},"",{"$f":"IF($T104<>\"ACBC_1W\",\"\",IF($J104=\"\",\"\",FintubeCapacity($T104,$W104,$AE104,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T104=\"Select Model\",T104=\"PCBL\"),\"\",calcQwIP(Y104,W104,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD104,BD104,\"capacity\",U104&\"P\"&IF(V104=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T104,activeElevation))","v":""},"",{"$f":"IF(OR(T104=\"Select Model\",T104=\"PCBL\"), \"\",IF(AY104=0,\"N/A\",waterPressureDrop(W104, U104 & \"P\" & IF(V104=\"Dual\",2,1) &\"C\", AD104, \"heating\", T104)))","v":""},{"$f":"IF(OR(T104=\"Select Model\",T104=\"PCBL\"), \"\",IF(AY104=0,getReturnWaterTemp(T104,AE104, activeEWTHeating, AX104, \"heating\"),getReturnWaterTemp(T104,AD104, activeEWTHeating, AY104, \"heating\")))","v":""},"",{"$f":" getNozzle(T104, W104, Y104, Z104, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I105)),I105<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I105, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H105)),H105<0),\"\",intlEstQuantity(T105, W105*12, H105)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T105=\"Select Model\",\"\",coilCircuitChange(W105, U105, AC105, T105,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T105=\"Select Model\",\"\",beamWidth(T105))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T105=\"Select Model\",T105=\"PCBL\"), 0,getSPIP(T105, W105, Y105, BD105, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T105=\"Select Model\", \"\",IF(T105=\"PCBL\",0,primaryAirSensibleCapacityIP($T105,$W105,activeRoomTempCooling,activePriAirTempCooling,$Y105,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T105=\"Select Model\",\"\",IF($T105=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y105,activeElevation)))","v":""},{"$f":"IF(OR(T105=\"Select Model\",T105=\"PCBL\"), 0,IF(AD105=0,0,-primaryAirSensibleCapacityIP($T105,$W105,activeRoomTempHeating,activePriAirTempHeating,$Y105,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T105=\"Select Model\", \"\", InductionRatio($T105,BD105,$W105,$Y105)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T105=\"Select Model\", \"\",IF($T105=\"PCBL\",\"N/A\",minVAVSetBack(AA105, Y105))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T105=\"Select Model\", \"\",IF($T105= \"PCBL\",\"N/A\",getDischargeAirTemp($T105,$V105,$AC105,$W105,BD105,$AL105, $Y105, $AS105, \"cooling\",activeElevation,$AB105,$AJ105,$AV105,$BB105))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T105=\"Select Model\",$T105=\"PCBL\"), \"\",getDischargeAirTemp($T105,$V105,$AD105,$W105,BD105,$AL105, $Y105, $AY105, \"heating\",activeElevation,$AB105,$AJ105,$AV105,$BB105)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T105=\"Select Model\", \"\",IF(OR($T105=\"ACBC_1W\",$T105=\"ACBC_2W\",LEFT($T105,4)=\"ACBR\",$T105 = \"LIU24_2W\",LEFT($T105,3)=\"RIU\",LEFT($T105,6)=\"ACBL12\"), IF((soundLevel($T105, $AB105, BD105, $Y105, $W105,$AJ105,$AA105,\"dba\"))<15,\"<15\",soundLevel($T105, $AB105, BD105, $Y105, $W105,$AJ105,$AA105,\"dba\")+0.4),IF((soundLevel($T105, $AB105, BD105, $Y105, $W105,$AJ105,$AA105,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T105, $AB105, BD105, $Y105, $W105,$AJ105,$AA105,\"dba\")+5)<15, \"<15\", soundLevel($T105, $AB105, BD105,$Y105, $W105,$AJ105,$AA105,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T105=\"Select Model\", \"\",IF(OR($T105=\"ACBC_1W\",$T105=\"ACBC_2W\",LEFT($T105,4)=\"ACBR\",$T105=\"LIU24_2W\",LEFT($T105,3)=\"RIU\",LEFT($T105,6)=\"ACBL12\"), IF((soundLevel($T105, $AB105, BD105, $Y105, $W105,$AJ105,$AA105,\"NC\"))<15,\"<15\",soundLevel($T105, $AB105, BD105, $Y105, $W105,$AJ105,$AA105,\"NC\")+0.4),IF((soundLevel($T105, $AB105, BD105, $Y105, $W105,$AJ105,$AA105,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T105, $AB105, BD105, $Y105, $W105,$AJ105,$AA105,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T105, $AB105, BD105, $Y105, $W105,$AJ105,$AA105,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T105=\"Select Model\",\"\",IF($T105=\"LIU24_2W\",calcQwIP($Y105,$W105,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC105,$AI105,\"latent\",$U105&\"P\"&IF($V105=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T105,activeElevation),\"\"))","v":""},{"$f":"IF($T105=\"Select Model\",\"\",IF($T105=\"ACBC_1W\",calcQwIP($Y105,$W105,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC105,BD105,\"capacity\",$U105&\"P\"&IF($V105=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T105,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y105,$W105,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC105,BD105,\"capacity\",$U105&\"P\"&IF($V105=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T105,activeElevation)))","v":""},"",{"$f":"IF(T105=\"Select Model\", 0,waterPressureDrop(W105, U105 & \"P\" & IF(V105=\"Dual\",2,1) &\"C\", AC105, \"cooling\", T105))","v":0},{"$f":"IF(T105=\"Select Model\", \"\",getReturnWaterTemp(T105,AC105, activeEWTCooling, AS105, \"cooling\"))","v":""},"",{"$f":"IF($T105<>\"ACBC_1W\",\"\",IF($J105=\"\",\"\",FintubeCapacity($T105,$W105,$AE105,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T105=\"Select Model\",T105=\"PCBL\"),\"\",calcQwIP(Y105,W105,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD105,BD105,\"capacity\",U105&\"P\"&IF(V105=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T105,activeElevation))","v":""},"",{"$f":"IF(OR(T105=\"Select Model\",T105=\"PCBL\"), \"\",IF(AY105=0,\"N/A\",waterPressureDrop(W105, U105 & \"P\" & IF(V105=\"Dual\",2,1) &\"C\", AD105, \"heating\", T105)))","v":""},{"$f":"IF(OR(T105=\"Select Model\",T105=\"PCBL\"), \"\",IF(AY105=0,getReturnWaterTemp(T105,AE105, activeEWTHeating, AX105, \"heating\"),getReturnWaterTemp(T105,AD105, activeEWTHeating, AY105, \"heating\")))","v":""},"",{"$f":" getNozzle(T105, W105, Y105, Z105, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I106)),I106<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I106, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H106)),H106<0),\"\",intlEstQuantity(T106, W106*12, H106)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T106=\"Select Model\",\"\",coilCircuitChange(W106, U106, AC106, T106,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T106=\"Select Model\",\"\",beamWidth(T106))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T106=\"Select Model\",T106=\"PCBL\"), 0,getSPIP(T106, W106, Y106, BD106, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T106=\"Select Model\", \"\",IF(T106=\"PCBL\",0,primaryAirSensibleCapacityIP($T106,$W106,activeRoomTempCooling,activePriAirTempCooling,$Y106,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T106=\"Select Model\",\"\",IF($T106=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y106,activeElevation)))","v":""},{"$f":"IF(OR(T106=\"Select Model\",T106=\"PCBL\"), 0,IF(AD106=0,0,-primaryAirSensibleCapacityIP($T106,$W106,activeRoomTempHeating,activePriAirTempHeating,$Y106,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T106=\"Select Model\", \"\", InductionRatio($T106,BD106,$W106,$Y106)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T106=\"Select Model\", \"\",IF($T106=\"PCBL\",\"N/A\",minVAVSetBack(AA106, Y106))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T106=\"Select Model\", \"\",IF($T106= \"PCBL\",\"N/A\",getDischargeAirTemp($T106,$V106,$AC106,$W106,BD106,$AL106, $Y106, $AS106, \"cooling\",activeElevation,$AB106,$AJ106,$AV106,$BB106))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T106=\"Select Model\",$T106=\"PCBL\"), \"\",getDischargeAirTemp($T106,$V106,$AD106,$W106,BD106,$AL106, $Y106, $AY106, \"heating\",activeElevation,$AB106,$AJ106,$AV106,$BB106)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T106=\"Select Model\", \"\",IF(OR($T106=\"ACBC_1W\",$T106=\"ACBC_2W\",LEFT($T106,4)=\"ACBR\",$T106 = \"LIU24_2W\",LEFT($T106,3)=\"RIU\",LEFT($T106,6)=\"ACBL12\"), IF((soundLevel($T106, $AB106, BD106, $Y106, $W106,$AJ106,$AA106,\"dba\"))<15,\"<15\",soundLevel($T106, $AB106, BD106, $Y106, $W106,$AJ106,$AA106,\"dba\")+0.4),IF((soundLevel($T106, $AB106, BD106, $Y106, $W106,$AJ106,$AA106,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T106, $AB106, BD106, $Y106, $W106,$AJ106,$AA106,\"dba\")+5)<15, \"<15\", soundLevel($T106, $AB106, BD106,$Y106, $W106,$AJ106,$AA106,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T106=\"Select Model\", \"\",IF(OR($T106=\"ACBC_1W\",$T106=\"ACBC_2W\",LEFT($T106,4)=\"ACBR\",$T106=\"LIU24_2W\",LEFT($T106,3)=\"RIU\",LEFT($T106,6)=\"ACBL12\"), IF((soundLevel($T106, $AB106, BD106, $Y106, $W106,$AJ106,$AA106,\"NC\"))<15,\"<15\",soundLevel($T106, $AB106, BD106, $Y106, $W106,$AJ106,$AA106,\"NC\")+0.4),IF((soundLevel($T106, $AB106, BD106, $Y106, $W106,$AJ106,$AA106,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T106, $AB106, BD106, $Y106, $W106,$AJ106,$AA106,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T106, $AB106, BD106, $Y106, $W106,$AJ106,$AA106,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T106=\"Select Model\",\"\",IF($T106=\"LIU24_2W\",calcQwIP($Y106,$W106,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC106,$AI106,\"latent\",$U106&\"P\"&IF($V106=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T106,activeElevation),\"\"))","v":""},{"$f":"IF($T106=\"Select Model\",\"\",IF($T106=\"ACBC_1W\",calcQwIP($Y106,$W106,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC106,BD106,\"capacity\",$U106&\"P\"&IF($V106=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T106,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y106,$W106,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC106,BD106,\"capacity\",$U106&\"P\"&IF($V106=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T106,activeElevation)))","v":""},"",{"$f":"IF(T106=\"Select Model\", 0,waterPressureDrop(W106, U106 & \"P\" & IF(V106=\"Dual\",2,1) &\"C\", AC106, \"cooling\", T106))","v":0},{"$f":"IF(T106=\"Select Model\", \"\",getReturnWaterTemp(T106,AC106, activeEWTCooling, AS106, \"cooling\"))","v":""},"",{"$f":"IF($T106<>\"ACBC_1W\",\"\",IF($J106=\"\",\"\",FintubeCapacity($T106,$W106,$AE106,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T106=\"Select Model\",T106=\"PCBL\"),\"\",calcQwIP(Y106,W106,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD106,BD106,\"capacity\",U106&\"P\"&IF(V106=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T106,activeElevation))","v":""},"",{"$f":"IF(OR(T106=\"Select Model\",T106=\"PCBL\"), \"\",IF(AY106=0,\"N/A\",waterPressureDrop(W106, U106 & \"P\" & IF(V106=\"Dual\",2,1) &\"C\", AD106, \"heating\", T106)))","v":""},{"$f":"IF(OR(T106=\"Select Model\",T106=\"PCBL\"), \"\",IF(AY106=0,getReturnWaterTemp(T106,AE106, activeEWTHeating, AX106, \"heating\"),getReturnWaterTemp(T106,AD106, activeEWTHeating, AY106, \"heating\")))","v":""},"",{"$f":" getNozzle(T106, W106, Y106, Z106, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I107)),I107<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I107, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H107)),H107<0),\"\",intlEstQuantity(T107, W107*12, H107)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T107=\"Select Model\",\"\",coilCircuitChange(W107, U107, AC107, T107,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T107=\"Select Model\",\"\",beamWidth(T107))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T107=\"Select Model\",T107=\"PCBL\"), 0,getSPIP(T107, W107, Y107, BD107, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T107=\"Select Model\", \"\",IF(T107=\"PCBL\",0,primaryAirSensibleCapacityIP($T107,$W107,activeRoomTempCooling,activePriAirTempCooling,$Y107,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T107=\"Select Model\",\"\",IF($T107=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y107,activeElevation)))","v":""},{"$f":"IF(OR(T107=\"Select Model\",T107=\"PCBL\"), 0,IF(AD107=0,0,-primaryAirSensibleCapacityIP($T107,$W107,activeRoomTempHeating,activePriAirTempHeating,$Y107,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T107=\"Select Model\", \"\", InductionRatio($T107,BD107,$W107,$Y107)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T107=\"Select Model\", \"\",IF($T107=\"PCBL\",\"N/A\",minVAVSetBack(AA107, Y107))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T107=\"Select Model\", \"\",IF($T107= \"PCBL\",\"N/A\",getDischargeAirTemp($T107,$V107,$AC107,$W107,BD107,$AL107, $Y107, $AS107, \"cooling\",activeElevation,$AB107,$AJ107,$AV107,$BB107))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T107=\"Select Model\",$T107=\"PCBL\"), \"\",getDischargeAirTemp($T107,$V107,$AD107,$W107,BD107,$AL107, $Y107, $AY107, \"heating\",activeElevation,$AB107,$AJ107,$AV107,$BB107)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T107=\"Select Model\", \"\",IF(OR($T107=\"ACBC_1W\",$T107=\"ACBC_2W\",LEFT($T107,4)=\"ACBR\",$T107 = \"LIU24_2W\",LEFT($T107,3)=\"RIU\",LEFT($T107,6)=\"ACBL12\"), IF((soundLevel($T107, $AB107, BD107, $Y107, $W107,$AJ107,$AA107,\"dba\"))<15,\"<15\",soundLevel($T107, $AB107, BD107, $Y107, $W107,$AJ107,$AA107,\"dba\")+0.4),IF((soundLevel($T107, $AB107, BD107, $Y107, $W107,$AJ107,$AA107,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T107, $AB107, BD107, $Y107, $W107,$AJ107,$AA107,\"dba\")+5)<15, \"<15\", soundLevel($T107, $AB107, BD107,$Y107, $W107,$AJ107,$AA107,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T107=\"Select Model\", \"\",IF(OR($T107=\"ACBC_1W\",$T107=\"ACBC_2W\",LEFT($T107,4)=\"ACBR\",$T107=\"LIU24_2W\",LEFT($T107,3)=\"RIU\",LEFT($T107,6)=\"ACBL12\"), IF((soundLevel($T107, $AB107, BD107, $Y107, $W107,$AJ107,$AA107,\"NC\"))<15,\"<15\",soundLevel($T107, $AB107, BD107, $Y107, $W107,$AJ107,$AA107,\"NC\")+0.4),IF((soundLevel($T107, $AB107, BD107, $Y107, $W107,$AJ107,$AA107,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T107, $AB107, BD107, $Y107, $W107,$AJ107,$AA107,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T107, $AB107, BD107, $Y107, $W107,$AJ107,$AA107,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T107=\"Select Model\",\"\",IF($T107=\"LIU24_2W\",calcQwIP($Y107,$W107,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC107,$AI107,\"latent\",$U107&\"P\"&IF($V107=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T107,activeElevation),\"\"))","v":""},{"$f":"IF($T107=\"Select Model\",\"\",IF($T107=\"ACBC_1W\",calcQwIP($Y107,$W107,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC107,BD107,\"capacity\",$U107&\"P\"&IF($V107=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T107,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y107,$W107,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC107,BD107,\"capacity\",$U107&\"P\"&IF($V107=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T107,activeElevation)))","v":""},"",{"$f":"IF(T107=\"Select Model\", 0,waterPressureDrop(W107, U107 & \"P\" & IF(V107=\"Dual\",2,1) &\"C\", AC107, \"cooling\", T107))","v":0},{"$f":"IF(T107=\"Select Model\", \"\",getReturnWaterTemp(T107,AC107, activeEWTCooling, AS107, \"cooling\"))","v":""},"",{"$f":"IF($T107<>\"ACBC_1W\",\"\",IF($J107=\"\",\"\",FintubeCapacity($T107,$W107,$AE107,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T107=\"Select Model\",T107=\"PCBL\"),\"\",calcQwIP(Y107,W107,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD107,BD107,\"capacity\",U107&\"P\"&IF(V107=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T107,activeElevation))","v":""},"",{"$f":"IF(OR(T107=\"Select Model\",T107=\"PCBL\"), \"\",IF(AY107=0,\"N/A\",waterPressureDrop(W107, U107 & \"P\" & IF(V107=\"Dual\",2,1) &\"C\", AD107, \"heating\", T107)))","v":""},{"$f":"IF(OR(T107=\"Select Model\",T107=\"PCBL\"), \"\",IF(AY107=0,getReturnWaterTemp(T107,AE107, activeEWTHeating, AX107, \"heating\"),getReturnWaterTemp(T107,AD107, activeEWTHeating, AY107, \"heating\")))","v":""},"",{"$f":" getNozzle(T107, W107, Y107, Z107, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I108)),I108<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I108, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H108)),H108<0),\"\",intlEstQuantity(T108, W108*12, H108)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T108=\"Select Model\",\"\",coilCircuitChange(W108, U108, AC108, T108,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T108=\"Select Model\",\"\",beamWidth(T108))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T108=\"Select Model\",T108=\"PCBL\"), 0,getSPIP(T108, W108, Y108, BD108, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T108=\"Select Model\", \"\",IF(T108=\"PCBL\",0,primaryAirSensibleCapacityIP($T108,$W108,activeRoomTempCooling,activePriAirTempCooling,$Y108,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T108=\"Select Model\",\"\",IF($T108=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y108,activeElevation)))","v":""},{"$f":"IF(OR(T108=\"Select Model\",T108=\"PCBL\"), 0,IF(AD108=0,0,-primaryAirSensibleCapacityIP($T108,$W108,activeRoomTempHeating,activePriAirTempHeating,$Y108,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T108=\"Select Model\", \"\", InductionRatio($T108,BD108,$W108,$Y108)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T108=\"Select Model\", \"\",IF($T108=\"PCBL\",\"N/A\",minVAVSetBack(AA108, Y108))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T108=\"Select Model\", \"\",IF($T108= \"PCBL\",\"N/A\",getDischargeAirTemp($T108,$V108,$AC108,$W108,BD108,$AL108, $Y108, $AS108, \"cooling\",activeElevation,$AB108,$AJ108,$AV108,$BB108))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T108=\"Select Model\",$T108=\"PCBL\"), \"\",getDischargeAirTemp($T108,$V108,$AD108,$W108,BD108,$AL108, $Y108, $AY108, \"heating\",activeElevation,$AB108,$AJ108,$AV108,$BB108)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T108=\"Select Model\", \"\",IF(OR($T108=\"ACBC_1W\",$T108=\"ACBC_2W\",LEFT($T108,4)=\"ACBR\",$T108 = \"LIU24_2W\",LEFT($T108,3)=\"RIU\",LEFT($T108,6)=\"ACBL12\"), IF((soundLevel($T108, $AB108, BD108, $Y108, $W108,$AJ108,$AA108,\"dba\"))<15,\"<15\",soundLevel($T108, $AB108, BD108, $Y108, $W108,$AJ108,$AA108,\"dba\")+0.4),IF((soundLevel($T108, $AB108, BD108, $Y108, $W108,$AJ108,$AA108,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T108, $AB108, BD108, $Y108, $W108,$AJ108,$AA108,\"dba\")+5)<15, \"<15\", soundLevel($T108, $AB108, BD108,$Y108, $W108,$AJ108,$AA108,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T108=\"Select Model\", \"\",IF(OR($T108=\"ACBC_1W\",$T108=\"ACBC_2W\",LEFT($T108,4)=\"ACBR\",$T108=\"LIU24_2W\",LEFT($T108,3)=\"RIU\",LEFT($T108,6)=\"ACBL12\"), IF((soundLevel($T108, $AB108, BD108, $Y108, $W108,$AJ108,$AA108,\"NC\"))<15,\"<15\",soundLevel($T108, $AB108, BD108, $Y108, $W108,$AJ108,$AA108,\"NC\")+0.4),IF((soundLevel($T108, $AB108, BD108, $Y108, $W108,$AJ108,$AA108,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T108, $AB108, BD108, $Y108, $W108,$AJ108,$AA108,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T108, $AB108, BD108, $Y108, $W108,$AJ108,$AA108,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T108=\"Select Model\",\"\",IF($T108=\"LIU24_2W\",calcQwIP($Y108,$W108,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC108,$AI108,\"latent\",$U108&\"P\"&IF($V108=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T108,activeElevation),\"\"))","v":""},{"$f":"IF($T108=\"Select Model\",\"\",IF($T108=\"ACBC_1W\",calcQwIP($Y108,$W108,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC108,BD108,\"capacity\",$U108&\"P\"&IF($V108=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T108,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y108,$W108,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC108,BD108,\"capacity\",$U108&\"P\"&IF($V108=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T108,activeElevation)))","v":""},"",{"$f":"IF(T108=\"Select Model\", 0,waterPressureDrop(W108, U108 & \"P\" & IF(V108=\"Dual\",2,1) &\"C\", AC108, \"cooling\", T108))","v":0},{"$f":"IF(T108=\"Select Model\", \"\",getReturnWaterTemp(T108,AC108, activeEWTCooling, AS108, \"cooling\"))","v":""},"",{"$f":"IF($T108<>\"ACBC_1W\",\"\",IF($J108=\"\",\"\",FintubeCapacity($T108,$W108,$AE108,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T108=\"Select Model\",T108=\"PCBL\"),\"\",calcQwIP(Y108,W108,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD108,BD108,\"capacity\",U108&\"P\"&IF(V108=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T108,activeElevation))","v":""},"",{"$f":"IF(OR(T108=\"Select Model\",T108=\"PCBL\"), \"\",IF(AY108=0,\"N/A\",waterPressureDrop(W108, U108 & \"P\" & IF(V108=\"Dual\",2,1) &\"C\", AD108, \"heating\", T108)))","v":""},{"$f":"IF(OR(T108=\"Select Model\",T108=\"PCBL\"), \"\",IF(AY108=0,getReturnWaterTemp(T108,AE108, activeEWTHeating, AX108, \"heating\"),getReturnWaterTemp(T108,AD108, activeEWTHeating, AY108, \"heating\")))","v":""},"",{"$f":" getNozzle(T108, W108, Y108, Z108, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I109)),I109<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I109, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H109)),H109<0),\"\",intlEstQuantity(T109, W109*12, H109)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T109=\"Select Model\",\"\",coilCircuitChange(W109, U109, AC109, T109,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T109=\"Select Model\",\"\",beamWidth(T109))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T109=\"Select Model\",T109=\"PCBL\"), 0,getSPIP(T109, W109, Y109, BD109, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T109=\"Select Model\", \"\",IF(T109=\"PCBL\",0,primaryAirSensibleCapacityIP($T109,$W109,activeRoomTempCooling,activePriAirTempCooling,$Y109,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T109=\"Select Model\",\"\",IF($T109=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y109,activeElevation)))","v":""},{"$f":"IF(OR(T109=\"Select Model\",T109=\"PCBL\"), 0,IF(AD109=0,0,-primaryAirSensibleCapacityIP($T109,$W109,activeRoomTempHeating,activePriAirTempHeating,$Y109,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T109=\"Select Model\", \"\", InductionRatio($T109,BD109,$W109,$Y109)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T109=\"Select Model\", \"\",IF($T109=\"PCBL\",\"N/A\",minVAVSetBack(AA109, Y109))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T109=\"Select Model\", \"\",IF($T109= \"PCBL\",\"N/A\",getDischargeAirTemp($T109,$V109,$AC109,$W109,BD109,$AL109, $Y109, $AS109, \"cooling\",activeElevation,$AB109,$AJ109,$AV109,$BB109))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T109=\"Select Model\",$T109=\"PCBL\"), \"\",getDischargeAirTemp($T109,$V109,$AD109,$W109,BD109,$AL109, $Y109, $AY109, \"heating\",activeElevation,$AB109,$AJ109,$AV109,$BB109)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T109=\"Select Model\", \"\",IF(OR($T109=\"ACBC_1W\",$T109=\"ACBC_2W\",LEFT($T109,4)=\"ACBR\",$T109 = \"LIU24_2W\",LEFT($T109,3)=\"RIU\",LEFT($T109,6)=\"ACBL12\"), IF((soundLevel($T109, $AB109, BD109, $Y109, $W109,$AJ109,$AA109,\"dba\"))<15,\"<15\",soundLevel($T109, $AB109, BD109, $Y109, $W109,$AJ109,$AA109,\"dba\")+0.4),IF((soundLevel($T109, $AB109, BD109, $Y109, $W109,$AJ109,$AA109,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T109, $AB109, BD109, $Y109, $W109,$AJ109,$AA109,\"dba\")+5)<15, \"<15\", soundLevel($T109, $AB109, BD109,$Y109, $W109,$AJ109,$AA109,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T109=\"Select Model\", \"\",IF(OR($T109=\"ACBC_1W\",$T109=\"ACBC_2W\",LEFT($T109,4)=\"ACBR\",$T109=\"LIU24_2W\",LEFT($T109,3)=\"RIU\",LEFT($T109,6)=\"ACBL12\"), IF((soundLevel($T109, $AB109, BD109, $Y109, $W109,$AJ109,$AA109,\"NC\"))<15,\"<15\",soundLevel($T109, $AB109, BD109, $Y109, $W109,$AJ109,$AA109,\"NC\")+0.4),IF((soundLevel($T109, $AB109, BD109, $Y109, $W109,$AJ109,$AA109,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T109, $AB109, BD109, $Y109, $W109,$AJ109,$AA109,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T109, $AB109, BD109, $Y109, $W109,$AJ109,$AA109,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T109=\"Select Model\",\"\",IF($T109=\"LIU24_2W\",calcQwIP($Y109,$W109,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC109,$AI109,\"latent\",$U109&\"P\"&IF($V109=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T109,activeElevation),\"\"))","v":""},{"$f":"IF($T109=\"Select Model\",\"\",IF($T109=\"ACBC_1W\",calcQwIP($Y109,$W109,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC109,BD109,\"capacity\",$U109&\"P\"&IF($V109=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T109,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y109,$W109,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC109,BD109,\"capacity\",$U109&\"P\"&IF($V109=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T109,activeElevation)))","v":""},"",{"$f":"IF(T109=\"Select Model\", 0,waterPressureDrop(W109, U109 & \"P\" & IF(V109=\"Dual\",2,1) &\"C\", AC109, \"cooling\", T109))","v":0},{"$f":"IF(T109=\"Select Model\", \"\",getReturnWaterTemp(T109,AC109, activeEWTCooling, AS109, \"cooling\"))","v":""},"",{"$f":"IF($T109<>\"ACBC_1W\",\"\",IF($J109=\"\",\"\",FintubeCapacity($T109,$W109,$AE109,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T109=\"Select Model\",T109=\"PCBL\"),\"\",calcQwIP(Y109,W109,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD109,BD109,\"capacity\",U109&\"P\"&IF(V109=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T109,activeElevation))","v":""},"",{"$f":"IF(OR(T109=\"Select Model\",T109=\"PCBL\"), \"\",IF(AY109=0,\"N/A\",waterPressureDrop(W109, U109 & \"P\" & IF(V109=\"Dual\",2,1) &\"C\", AD109, \"heating\", T109)))","v":""},{"$f":"IF(OR(T109=\"Select Model\",T109=\"PCBL\"), \"\",IF(AY109=0,getReturnWaterTemp(T109,AE109, activeEWTHeating, AX109, \"heating\"),getReturnWaterTemp(T109,AD109, activeEWTHeating, AY109, \"heating\")))","v":""},"",{"$f":" getNozzle(T109, W109, Y109, Z109, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I110)),I110<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I110, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H110)),H110<0),\"\",intlEstQuantity(T110, W110*12, H110)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T110=\"Select Model\",\"\",coilCircuitChange(W110, U110, AC110, T110,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T110=\"Select Model\",\"\",beamWidth(T110))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T110=\"Select Model\",T110=\"PCBL\"), 0,getSPIP(T110, W110, Y110, BD110, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T110=\"Select Model\", \"\",IF(T110=\"PCBL\",0,primaryAirSensibleCapacityIP($T110,$W110,activeRoomTempCooling,activePriAirTempCooling,$Y110,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T110=\"Select Model\",\"\",IF($T110=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y110,activeElevation)))","v":""},{"$f":"IF(OR(T110=\"Select Model\",T110=\"PCBL\"), 0,IF(AD110=0,0,-primaryAirSensibleCapacityIP($T110,$W110,activeRoomTempHeating,activePriAirTempHeating,$Y110,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T110=\"Select Model\", \"\", InductionRatio($T110,BD110,$W110,$Y110)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T110=\"Select Model\", \"\",IF($T110=\"PCBL\",\"N/A\",minVAVSetBack(AA110, Y110))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T110=\"Select Model\", \"\",IF($T110= \"PCBL\",\"N/A\",getDischargeAirTemp($T110,$V110,$AC110,$W110,BD110,$AL110, $Y110, $AS110, \"cooling\",activeElevation,$AB110,$AJ110,$AV110,$BB110))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T110=\"Select Model\",$T110=\"PCBL\"), \"\",getDischargeAirTemp($T110,$V110,$AD110,$W110,BD110,$AL110, $Y110, $AY110, \"heating\",activeElevation,$AB110,$AJ110,$AV110,$BB110)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T110=\"Select Model\", \"\",IF(OR($T110=\"ACBC_1W\",$T110=\"ACBC_2W\",LEFT($T110,4)=\"ACBR\",$T110 = \"LIU24_2W\",LEFT($T110,3)=\"RIU\",LEFT($T110,6)=\"ACBL12\"), IF((soundLevel($T110, $AB110, BD110, $Y110, $W110,$AJ110,$AA110,\"dba\"))<15,\"<15\",soundLevel($T110, $AB110, BD110, $Y110, $W110,$AJ110,$AA110,\"dba\")+0.4),IF((soundLevel($T110, $AB110, BD110, $Y110, $W110,$AJ110,$AA110,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T110, $AB110, BD110, $Y110, $W110,$AJ110,$AA110,\"dba\")+5)<15, \"<15\", soundLevel($T110, $AB110, BD110,$Y110, $W110,$AJ110,$AA110,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T110=\"Select Model\", \"\",IF(OR($T110=\"ACBC_1W\",$T110=\"ACBC_2W\",LEFT($T110,4)=\"ACBR\",$T110=\"LIU24_2W\",LEFT($T110,3)=\"RIU\",LEFT($T110,6)=\"ACBL12\"), IF((soundLevel($T110, $AB110, BD110, $Y110, $W110,$AJ110,$AA110,\"NC\"))<15,\"<15\",soundLevel($T110, $AB110, BD110, $Y110, $W110,$AJ110,$AA110,\"NC\")+0.4),IF((soundLevel($T110, $AB110, BD110, $Y110, $W110,$AJ110,$AA110,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T110, $AB110, BD110, $Y110, $W110,$AJ110,$AA110,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T110, $AB110, BD110, $Y110, $W110,$AJ110,$AA110,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T110=\"Select Model\",\"\",IF($T110=\"LIU24_2W\",calcQwIP($Y110,$W110,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC110,$AI110,\"latent\",$U110&\"P\"&IF($V110=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T110,activeElevation),\"\"))","v":""},{"$f":"IF($T110=\"Select Model\",\"\",IF($T110=\"ACBC_1W\",calcQwIP($Y110,$W110,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC110,BD110,\"capacity\",$U110&\"P\"&IF($V110=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T110,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y110,$W110,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC110,BD110,\"capacity\",$U110&\"P\"&IF($V110=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T110,activeElevation)))","v":""},"",{"$f":"IF(T110=\"Select Model\", 0,waterPressureDrop(W110, U110 & \"P\" & IF(V110=\"Dual\",2,1) &\"C\", AC110, \"cooling\", T110))","v":0},{"$f":"IF(T110=\"Select Model\", \"\",getReturnWaterTemp(T110,AC110, activeEWTCooling, AS110, \"cooling\"))","v":""},"",{"$f":"IF($T110<>\"ACBC_1W\",\"\",IF($J110=\"\",\"\",FintubeCapacity($T110,$W110,$AE110,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T110=\"Select Model\",T110=\"PCBL\"),\"\",calcQwIP(Y110,W110,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD110,BD110,\"capacity\",U110&\"P\"&IF(V110=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T110,activeElevation))","v":""},"",{"$f":"IF(OR(T110=\"Select Model\",T110=\"PCBL\"), \"\",IF(AY110=0,\"N/A\",waterPressureDrop(W110, U110 & \"P\" & IF(V110=\"Dual\",2,1) &\"C\", AD110, \"heating\", T110)))","v":""},{"$f":"IF(OR(T110=\"Select Model\",T110=\"PCBL\"), \"\",IF(AY110=0,getReturnWaterTemp(T110,AE110, activeEWTHeating, AX110, \"heating\"),getReturnWaterTemp(T110,AD110, activeEWTHeating, AY110, \"heating\")))","v":""},"",{"$f":" getNozzle(T110, W110, Y110, Z110, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I111)),I111<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I111, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H111)),H111<0),\"\",intlEstQuantity(T111, W111*12, H111)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T111=\"Select Model\",\"\",coilCircuitChange(W111, U111, AC111, T111,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T111=\"Select Model\",\"\",beamWidth(T111))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T111=\"Select Model\",T111=\"PCBL\"), 0,getSPIP(T111, W111, Y111, BD111, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T111=\"Select Model\", \"\",IF(T111=\"PCBL\",0,primaryAirSensibleCapacityIP($T111,$W111,activeRoomTempCooling,activePriAirTempCooling,$Y111,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T111=\"Select Model\",\"\",IF($T111=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y111,activeElevation)))","v":""},{"$f":"IF(OR(T111=\"Select Model\",T111=\"PCBL\"), 0,IF(AD111=0,0,-primaryAirSensibleCapacityIP($T111,$W111,activeRoomTempHeating,activePriAirTempHeating,$Y111,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T111=\"Select Model\", \"\", InductionRatio($T111,BD111,$W111,$Y111)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T111=\"Select Model\", \"\",IF($T111=\"PCBL\",\"N/A\",minVAVSetBack(AA111, Y111))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T111=\"Select Model\", \"\",IF($T111= \"PCBL\",\"N/A\",getDischargeAirTemp($T111,$V111,$AC111,$W111,BD111,$AL111, $Y111, $AS111, \"cooling\",activeElevation,$AB111,$AJ111,$AV111,$BB111))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T111=\"Select Model\",$T111=\"PCBL\"), \"\",getDischargeAirTemp($T111,$V111,$AD111,$W111,BD111,$AL111, $Y111, $AY111, \"heating\",activeElevation,$AB111,$AJ111,$AV111,$BB111)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T111=\"Select Model\", \"\",IF(OR($T111=\"ACBC_1W\",$T111=\"ACBC_2W\",LEFT($T111,4)=\"ACBR\",$T111 = \"LIU24_2W\",LEFT($T111,3)=\"RIU\",LEFT($T111,6)=\"ACBL12\"), IF((soundLevel($T111, $AB111, BD111, $Y111, $W111,$AJ111,$AA111,\"dba\"))<15,\"<15\",soundLevel($T111, $AB111, BD111, $Y111, $W111,$AJ111,$AA111,\"dba\")+0.4),IF((soundLevel($T111, $AB111, BD111, $Y111, $W111,$AJ111,$AA111,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T111, $AB111, BD111, $Y111, $W111,$AJ111,$AA111,\"dba\")+5)<15, \"<15\", soundLevel($T111, $AB111, BD111,$Y111, $W111,$AJ111,$AA111,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T111=\"Select Model\", \"\",IF(OR($T111=\"ACBC_1W\",$T111=\"ACBC_2W\",LEFT($T111,4)=\"ACBR\",$T111=\"LIU24_2W\",LEFT($T111,3)=\"RIU\",LEFT($T111,6)=\"ACBL12\"), IF((soundLevel($T111, $AB111, BD111, $Y111, $W111,$AJ111,$AA111,\"NC\"))<15,\"<15\",soundLevel($T111, $AB111, BD111, $Y111, $W111,$AJ111,$AA111,\"NC\")+0.4),IF((soundLevel($T111, $AB111, BD111, $Y111, $W111,$AJ111,$AA111,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T111, $AB111, BD111, $Y111, $W111,$AJ111,$AA111,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T111, $AB111, BD111, $Y111, $W111,$AJ111,$AA111,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T111=\"Select Model\",\"\",IF($T111=\"LIU24_2W\",calcQwIP($Y111,$W111,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC111,$AI111,\"latent\",$U111&\"P\"&IF($V111=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T111,activeElevation),\"\"))","v":""},{"$f":"IF($T111=\"Select Model\",\"\",IF($T111=\"ACBC_1W\",calcQwIP($Y111,$W111,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC111,BD111,\"capacity\",$U111&\"P\"&IF($V111=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T111,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y111,$W111,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC111,BD111,\"capacity\",$U111&\"P\"&IF($V111=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T111,activeElevation)))","v":""},"",{"$f":"IF(T111=\"Select Model\", 0,waterPressureDrop(W111, U111 & \"P\" & IF(V111=\"Dual\",2,1) &\"C\", AC111, \"cooling\", T111))","v":0},{"$f":"IF(T111=\"Select Model\", \"\",getReturnWaterTemp(T111,AC111, activeEWTCooling, AS111, \"cooling\"))","v":""},"",{"$f":"IF($T111<>\"ACBC_1W\",\"\",IF($J111=\"\",\"\",FintubeCapacity($T111,$W111,$AE111,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T111=\"Select Model\",T111=\"PCBL\"),\"\",calcQwIP(Y111,W111,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD111,BD111,\"capacity\",U111&\"P\"&IF(V111=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T111,activeElevation))","v":""},"",{"$f":"IF(OR(T111=\"Select Model\",T111=\"PCBL\"), \"\",IF(AY111=0,\"N/A\",waterPressureDrop(W111, U111 & \"P\" & IF(V111=\"Dual\",2,1) &\"C\", AD111, \"heating\", T111)))","v":""},{"$f":"IF(OR(T111=\"Select Model\",T111=\"PCBL\"), \"\",IF(AY111=0,getReturnWaterTemp(T111,AE111, activeEWTHeating, AX111, \"heating\"),getReturnWaterTemp(T111,AD111, activeEWTHeating, AY111, \"heating\")))","v":""},"",{"$f":" getNozzle(T111, W111, Y111, Z111, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I112)),I112<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I112, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H112)),H112<0),\"\",intlEstQuantity(T112, W112*12, H112)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T112=\"Select Model\",\"\",coilCircuitChange(W112, U112, AC112, T112,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T112=\"Select Model\",\"\",beamWidth(T112))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T112=\"Select Model\",T112=\"PCBL\"), 0,getSPIP(T112, W112, Y112, BD112, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T112=\"Select Model\", \"\",IF(T112=\"PCBL\",0,primaryAirSensibleCapacityIP($T112,$W112,activeRoomTempCooling,activePriAirTempCooling,$Y112,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T112=\"Select Model\",\"\",IF($T112=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y112,activeElevation)))","v":""},{"$f":"IF(OR(T112=\"Select Model\",T112=\"PCBL\"), 0,IF(AD112=0,0,-primaryAirSensibleCapacityIP($T112,$W112,activeRoomTempHeating,activePriAirTempHeating,$Y112,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T112=\"Select Model\", \"\", InductionRatio($T112,BD112,$W112,$Y112)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T112=\"Select Model\", \"\",IF($T112=\"PCBL\",\"N/A\",minVAVSetBack(AA112, Y112))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T112=\"Select Model\", \"\",IF($T112= \"PCBL\",\"N/A\",getDischargeAirTemp($T112,$V112,$AC112,$W112,BD112,$AL112, $Y112, $AS112, \"cooling\",activeElevation,$AB112,$AJ112,$AV112,$BB112))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T112=\"Select Model\",$T112=\"PCBL\"), \"\",getDischargeAirTemp($T112,$V112,$AD112,$W112,BD112,$AL112, $Y112, $AY112, \"heating\",activeElevation,$AB112,$AJ112,$AV112,$BB112)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T112=\"Select Model\", \"\",IF(OR($T112=\"ACBC_1W\",$T112=\"ACBC_2W\",LEFT($T112,4)=\"ACBR\",$T112 = \"LIU24_2W\",LEFT($T112,3)=\"RIU\",LEFT($T112,6)=\"ACBL12\"), IF((soundLevel($T112, $AB112, BD112, $Y112, $W112,$AJ112,$AA112,\"dba\"))<15,\"<15\",soundLevel($T112, $AB112, BD112, $Y112, $W112,$AJ112,$AA112,\"dba\")+0.4),IF((soundLevel($T112, $AB112, BD112, $Y112, $W112,$AJ112,$AA112,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T112, $AB112, BD112, $Y112, $W112,$AJ112,$AA112,\"dba\")+5)<15, \"<15\", soundLevel($T112, $AB112, BD112,$Y112, $W112,$AJ112,$AA112,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T112=\"Select Model\", \"\",IF(OR($T112=\"ACBC_1W\",$T112=\"ACBC_2W\",LEFT($T112,4)=\"ACBR\",$T112=\"LIU24_2W\",LEFT($T112,3)=\"RIU\",LEFT($T112,6)=\"ACBL12\"), IF((soundLevel($T112, $AB112, BD112, $Y112, $W112,$AJ112,$AA112,\"NC\"))<15,\"<15\",soundLevel($T112, $AB112, BD112, $Y112, $W112,$AJ112,$AA112,\"NC\")+0.4),IF((soundLevel($T112, $AB112, BD112, $Y112, $W112,$AJ112,$AA112,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T112, $AB112, BD112, $Y112, $W112,$AJ112,$AA112,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T112, $AB112, BD112, $Y112, $W112,$AJ112,$AA112,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T112=\"Select Model\",\"\",IF($T112=\"LIU24_2W\",calcQwIP($Y112,$W112,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC112,$AI112,\"latent\",$U112&\"P\"&IF($V112=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T112,activeElevation),\"\"))","v":""},{"$f":"IF($T112=\"Select Model\",\"\",IF($T112=\"ACBC_1W\",calcQwIP($Y112,$W112,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC112,BD112,\"capacity\",$U112&\"P\"&IF($V112=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T112,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y112,$W112,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC112,BD112,\"capacity\",$U112&\"P\"&IF($V112=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T112,activeElevation)))","v":""},"",{"$f":"IF(T112=\"Select Model\", 0,waterPressureDrop(W112, U112 & \"P\" & IF(V112=\"Dual\",2,1) &\"C\", AC112, \"cooling\", T112))","v":0},{"$f":"IF(T112=\"Select Model\", \"\",getReturnWaterTemp(T112,AC112, activeEWTCooling, AS112, \"cooling\"))","v":""},"",{"$f":"IF($T112<>\"ACBC_1W\",\"\",IF($J112=\"\",\"\",FintubeCapacity($T112,$W112,$AE112,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T112=\"Select Model\",T112=\"PCBL\"),\"\",calcQwIP(Y112,W112,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD112,BD112,\"capacity\",U112&\"P\"&IF(V112=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T112,activeElevation))","v":""},"",{"$f":"IF(OR(T112=\"Select Model\",T112=\"PCBL\"), \"\",IF(AY112=0,\"N/A\",waterPressureDrop(W112, U112 & \"P\" & IF(V112=\"Dual\",2,1) &\"C\", AD112, \"heating\", T112)))","v":""},{"$f":"IF(OR(T112=\"Select Model\",T112=\"PCBL\"), \"\",IF(AY112=0,getReturnWaterTemp(T112,AE112, activeEWTHeating, AX112, \"heating\"),getReturnWaterTemp(T112,AD112, activeEWTHeating, AY112, \"heating\")))","v":""},"",{"$f":" getNozzle(T112, W112, Y112, Z112, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I113)),I113<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I113, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H113)),H113<0),\"\",intlEstQuantity(T113, W113*12, H113)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T113=\"Select Model\",\"\",coilCircuitChange(W113, U113, AC113, T113,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T113=\"Select Model\",\"\",beamWidth(T113))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T113=\"Select Model\",T113=\"PCBL\"), 0,getSPIP(T113, W113, Y113, BD113, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T113=\"Select Model\", \"\",IF(T113=\"PCBL\",0,primaryAirSensibleCapacityIP($T113,$W113,activeRoomTempCooling,activePriAirTempCooling,$Y113,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T113=\"Select Model\",\"\",IF($T113=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y113,activeElevation)))","v":""},{"$f":"IF(OR(T113=\"Select Model\",T113=\"PCBL\"), 0,IF(AD113=0,0,-primaryAirSensibleCapacityIP($T113,$W113,activeRoomTempHeating,activePriAirTempHeating,$Y113,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T113=\"Select Model\", \"\", InductionRatio($T113,BD113,$W113,$Y113)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T113=\"Select Model\", \"\",IF($T113=\"PCBL\",\"N/A\",minVAVSetBack(AA113, Y113))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T113=\"Select Model\", \"\",IF($T113= \"PCBL\",\"N/A\",getDischargeAirTemp($T113,$V113,$AC113,$W113,BD113,$AL113, $Y113, $AS113, \"cooling\",activeElevation,$AB113,$AJ113,$AV113,$BB113))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T113=\"Select Model\",$T113=\"PCBL\"), \"\",getDischargeAirTemp($T113,$V113,$AD113,$W113,BD113,$AL113, $Y113, $AY113, \"heating\",activeElevation,$AB113,$AJ113,$AV113,$BB113)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T113=\"Select Model\", \"\",IF(OR($T113=\"ACBC_1W\",$T113=\"ACBC_2W\",LEFT($T113,4)=\"ACBR\",$T113 = \"LIU24_2W\",LEFT($T113,3)=\"RIU\",LEFT($T113,6)=\"ACBL12\"), IF((soundLevel($T113, $AB113, BD113, $Y113, $W113,$AJ113,$AA113,\"dba\"))<15,\"<15\",soundLevel($T113, $AB113, BD113, $Y113, $W113,$AJ113,$AA113,\"dba\")+0.4),IF((soundLevel($T113, $AB113, BD113, $Y113, $W113,$AJ113,$AA113,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T113, $AB113, BD113, $Y113, $W113,$AJ113,$AA113,\"dba\")+5)<15, \"<15\", soundLevel($T113, $AB113, BD113,$Y113, $W113,$AJ113,$AA113,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T113=\"Select Model\", \"\",IF(OR($T113=\"ACBC_1W\",$T113=\"ACBC_2W\",LEFT($T113,4)=\"ACBR\",$T113=\"LIU24_2W\",LEFT($T113,3)=\"RIU\",LEFT($T113,6)=\"ACBL12\"), IF((soundLevel($T113, $AB113, BD113, $Y113, $W113,$AJ113,$AA113,\"NC\"))<15,\"<15\",soundLevel($T113, $AB113, BD113, $Y113, $W113,$AJ113,$AA113,\"NC\")+0.4),IF((soundLevel($T113, $AB113, BD113, $Y113, $W113,$AJ113,$AA113,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T113, $AB113, BD113, $Y113, $W113,$AJ113,$AA113,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T113, $AB113, BD113, $Y113, $W113,$AJ113,$AA113,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T113=\"Select Model\",\"\",IF($T113=\"LIU24_2W\",calcQwIP($Y113,$W113,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC113,$AI113,\"latent\",$U113&\"P\"&IF($V113=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T113,activeElevation),\"\"))","v":""},{"$f":"IF($T113=\"Select Model\",\"\",IF($T113=\"ACBC_1W\",calcQwIP($Y113,$W113,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC113,BD113,\"capacity\",$U113&\"P\"&IF($V113=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T113,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y113,$W113,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC113,BD113,\"capacity\",$U113&\"P\"&IF($V113=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T113,activeElevation)))","v":""},"",{"$f":"IF(T113=\"Select Model\", 0,waterPressureDrop(W113, U113 & \"P\" & IF(V113=\"Dual\",2,1) &\"C\", AC113, \"cooling\", T113))","v":0},{"$f":"IF(T113=\"Select Model\", \"\",getReturnWaterTemp(T113,AC113, activeEWTCooling, AS113, \"cooling\"))","v":""},"",{"$f":"IF($T113<>\"ACBC_1W\",\"\",IF($J113=\"\",\"\",FintubeCapacity($T113,$W113,$AE113,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T113=\"Select Model\",T113=\"PCBL\"),\"\",calcQwIP(Y113,W113,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD113,BD113,\"capacity\",U113&\"P\"&IF(V113=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T113,activeElevation))","v":""},"",{"$f":"IF(OR(T113=\"Select Model\",T113=\"PCBL\"), \"\",IF(AY113=0,\"N/A\",waterPressureDrop(W113, U113 & \"P\" & IF(V113=\"Dual\",2,1) &\"C\", AD113, \"heating\", T113)))","v":""},{"$f":"IF(OR(T113=\"Select Model\",T113=\"PCBL\"), \"\",IF(AY113=0,getReturnWaterTemp(T113,AE113, activeEWTHeating, AX113, \"heating\"),getReturnWaterTemp(T113,AD113, activeEWTHeating, AY113, \"heating\")))","v":""},"",{"$f":" getNozzle(T113, W113, Y113, Z113, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I114)),I114<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I114, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H114)),H114<0),\"\",intlEstQuantity(T114, W114*12, H114)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T114=\"Select Model\",\"\",coilCircuitChange(W114, U114, AC114, T114,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T114=\"Select Model\",\"\",beamWidth(T114))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T114=\"Select Model\",T114=\"PCBL\"), 0,getSPIP(T114, W114, Y114, BD114, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T114=\"Select Model\", \"\",IF(T114=\"PCBL\",0,primaryAirSensibleCapacityIP($T114,$W114,activeRoomTempCooling,activePriAirTempCooling,$Y114,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T114=\"Select Model\",\"\",IF($T114=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y114,activeElevation)))","v":""},{"$f":"IF(OR(T114=\"Select Model\",T114=\"PCBL\"), 0,IF(AD114=0,0,-primaryAirSensibleCapacityIP($T114,$W114,activeRoomTempHeating,activePriAirTempHeating,$Y114,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T114=\"Select Model\", \"\", InductionRatio($T114,BD114,$W114,$Y114)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T114=\"Select Model\", \"\",IF($T114=\"PCBL\",\"N/A\",minVAVSetBack(AA114, Y114))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T114=\"Select Model\", \"\",IF($T114= \"PCBL\",\"N/A\",getDischargeAirTemp($T114,$V114,$AC114,$W114,BD114,$AL114, $Y114, $AS114, \"cooling\",activeElevation,$AB114,$AJ114,$AV114,$BB114))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T114=\"Select Model\",$T114=\"PCBL\"), \"\",getDischargeAirTemp($T114,$V114,$AD114,$W114,BD114,$AL114, $Y114, $AY114, \"heating\",activeElevation,$AB114,$AJ114,$AV114,$BB114)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T114=\"Select Model\", \"\",IF(OR($T114=\"ACBC_1W\",$T114=\"ACBC_2W\",LEFT($T114,4)=\"ACBR\",$T114 = \"LIU24_2W\",LEFT($T114,3)=\"RIU\",LEFT($T114,6)=\"ACBL12\"), IF((soundLevel($T114, $AB114, BD114, $Y114, $W114,$AJ114,$AA114,\"dba\"))<15,\"<15\",soundLevel($T114, $AB114, BD114, $Y114, $W114,$AJ114,$AA114,\"dba\")+0.4),IF((soundLevel($T114, $AB114, BD114, $Y114, $W114,$AJ114,$AA114,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T114, $AB114, BD114, $Y114, $W114,$AJ114,$AA114,\"dba\")+5)<15, \"<15\", soundLevel($T114, $AB114, BD114,$Y114, $W114,$AJ114,$AA114,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T114=\"Select Model\", \"\",IF(OR($T114=\"ACBC_1W\",$T114=\"ACBC_2W\",LEFT($T114,4)=\"ACBR\",$T114=\"LIU24_2W\",LEFT($T114,3)=\"RIU\",LEFT($T114,6)=\"ACBL12\"), IF((soundLevel($T114, $AB114, BD114, $Y114, $W114,$AJ114,$AA114,\"NC\"))<15,\"<15\",soundLevel($T114, $AB114, BD114, $Y114, $W114,$AJ114,$AA114,\"NC\")+0.4),IF((soundLevel($T114, $AB114, BD114, $Y114, $W114,$AJ114,$AA114,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T114, $AB114, BD114, $Y114, $W114,$AJ114,$AA114,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T114, $AB114, BD114, $Y114, $W114,$AJ114,$AA114,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T114=\"Select Model\",\"\",IF($T114=\"LIU24_2W\",calcQwIP($Y114,$W114,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC114,$AI114,\"latent\",$U114&\"P\"&IF($V114=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T114,activeElevation),\"\"))","v":""},{"$f":"IF($T114=\"Select Model\",\"\",IF($T114=\"ACBC_1W\",calcQwIP($Y114,$W114,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC114,BD114,\"capacity\",$U114&\"P\"&IF($V114=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T114,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y114,$W114,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC114,BD114,\"capacity\",$U114&\"P\"&IF($V114=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T114,activeElevation)))","v":""},"",{"$f":"IF(T114=\"Select Model\", 0,waterPressureDrop(W114, U114 & \"P\" & IF(V114=\"Dual\",2,1) &\"C\", AC114, \"cooling\", T114))","v":0},{"$f":"IF(T114=\"Select Model\", \"\",getReturnWaterTemp(T114,AC114, activeEWTCooling, AS114, \"cooling\"))","v":""},"",{"$f":"IF($T114<>\"ACBC_1W\",\"\",IF($J114=\"\",\"\",FintubeCapacity($T114,$W114,$AE114,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T114=\"Select Model\",T114=\"PCBL\"),\"\",calcQwIP(Y114,W114,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD114,BD114,\"capacity\",U114&\"P\"&IF(V114=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T114,activeElevation))","v":""},"",{"$f":"IF(OR(T114=\"Select Model\",T114=\"PCBL\"), \"\",IF(AY114=0,\"N/A\",waterPressureDrop(W114, U114 & \"P\" & IF(V114=\"Dual\",2,1) &\"C\", AD114, \"heating\", T114)))","v":""},{"$f":"IF(OR(T114=\"Select Model\",T114=\"PCBL\"), \"\",IF(AY114=0,getReturnWaterTemp(T114,AE114, activeEWTHeating, AX114, \"heating\"),getReturnWaterTemp(T114,AD114, activeEWTHeating, AY114, \"heating\")))","v":""},"",{"$f":" getNozzle(T114, W114, Y114, Z114, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I115)),I115<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I115, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H115)),H115<0),\"\",intlEstQuantity(T115, W115*12, H115)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T115=\"Select Model\",\"\",coilCircuitChange(W115, U115, AC115, T115,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T115=\"Select Model\",\"\",beamWidth(T115))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T115=\"Select Model\",T115=\"PCBL\"), 0,getSPIP(T115, W115, Y115, BD115, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T115=\"Select Model\", \"\",IF(T115=\"PCBL\",0,primaryAirSensibleCapacityIP($T115,$W115,activeRoomTempCooling,activePriAirTempCooling,$Y115,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T115=\"Select Model\",\"\",IF($T115=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y115,activeElevation)))","v":""},{"$f":"IF(OR(T115=\"Select Model\",T115=\"PCBL\"), 0,IF(AD115=0,0,-primaryAirSensibleCapacityIP($T115,$W115,activeRoomTempHeating,activePriAirTempHeating,$Y115,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T115=\"Select Model\", \"\", InductionRatio($T115,BD115,$W115,$Y115)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T115=\"Select Model\", \"\",IF($T115=\"PCBL\",\"N/A\",minVAVSetBack(AA115, Y115))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T115=\"Select Model\", \"\",IF($T115= \"PCBL\",\"N/A\",getDischargeAirTemp($T115,$V115,$AC115,$W115,BD115,$AL115, $Y115, $AS115, \"cooling\",activeElevation,$AB115,$AJ115,$AV115,$BB115))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T115=\"Select Model\",$T115=\"PCBL\"), \"\",getDischargeAirTemp($T115,$V115,$AD115,$W115,BD115,$AL115, $Y115, $AY115, \"heating\",activeElevation,$AB115,$AJ115,$AV115,$BB115)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T115=\"Select Model\", \"\",IF(OR($T115=\"ACBC_1W\",$T115=\"ACBC_2W\",LEFT($T115,4)=\"ACBR\",$T115 = \"LIU24_2W\",LEFT($T115,3)=\"RIU\",LEFT($T115,6)=\"ACBL12\"), IF((soundLevel($T115, $AB115, BD115, $Y115, $W115,$AJ115,$AA115,\"dba\"))<15,\"<15\",soundLevel($T115, $AB115, BD115, $Y115, $W115,$AJ115,$AA115,\"dba\")+0.4),IF((soundLevel($T115, $AB115, BD115, $Y115, $W115,$AJ115,$AA115,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T115, $AB115, BD115, $Y115, $W115,$AJ115,$AA115,\"dba\")+5)<15, \"<15\", soundLevel($T115, $AB115, BD115,$Y115, $W115,$AJ115,$AA115,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T115=\"Select Model\", \"\",IF(OR($T115=\"ACBC_1W\",$T115=\"ACBC_2W\",LEFT($T115,4)=\"ACBR\",$T115=\"LIU24_2W\",LEFT($T115,3)=\"RIU\",LEFT($T115,6)=\"ACBL12\"), IF((soundLevel($T115, $AB115, BD115, $Y115, $W115,$AJ115,$AA115,\"NC\"))<15,\"<15\",soundLevel($T115, $AB115, BD115, $Y115, $W115,$AJ115,$AA115,\"NC\")+0.4),IF((soundLevel($T115, $AB115, BD115, $Y115, $W115,$AJ115,$AA115,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T115, $AB115, BD115, $Y115, $W115,$AJ115,$AA115,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T115, $AB115, BD115, $Y115, $W115,$AJ115,$AA115,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T115=\"Select Model\",\"\",IF($T115=\"LIU24_2W\",calcQwIP($Y115,$W115,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC115,$AI115,\"latent\",$U115&\"P\"&IF($V115=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T115,activeElevation),\"\"))","v":""},{"$f":"IF($T115=\"Select Model\",\"\",IF($T115=\"ACBC_1W\",calcQwIP($Y115,$W115,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC115,BD115,\"capacity\",$U115&\"P\"&IF($V115=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T115,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y115,$W115,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC115,BD115,\"capacity\",$U115&\"P\"&IF($V115=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T115,activeElevation)))","v":""},"",{"$f":"IF(T115=\"Select Model\", 0,waterPressureDrop(W115, U115 & \"P\" & IF(V115=\"Dual\",2,1) &\"C\", AC115, \"cooling\", T115))","v":0},{"$f":"IF(T115=\"Select Model\", \"\",getReturnWaterTemp(T115,AC115, activeEWTCooling, AS115, \"cooling\"))","v":""},"",{"$f":"IF($T115<>\"ACBC_1W\",\"\",IF($J115=\"\",\"\",FintubeCapacity($T115,$W115,$AE115,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T115=\"Select Model\",T115=\"PCBL\"),\"\",calcQwIP(Y115,W115,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD115,BD115,\"capacity\",U115&\"P\"&IF(V115=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T115,activeElevation))","v":""},"",{"$f":"IF(OR(T115=\"Select Model\",T115=\"PCBL\"), \"\",IF(AY115=0,\"N/A\",waterPressureDrop(W115, U115 & \"P\" & IF(V115=\"Dual\",2,1) &\"C\", AD115, \"heating\", T115)))","v":""},{"$f":"IF(OR(T115=\"Select Model\",T115=\"PCBL\"), \"\",IF(AY115=0,getReturnWaterTemp(T115,AE115, activeEWTHeating, AX115, \"heating\"),getReturnWaterTemp(T115,AD115, activeEWTHeating, AY115, \"heating\")))","v":""},"",{"$f":" getNozzle(T115, W115, Y115, Z115, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I116)),I116<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I116, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H116)),H116<0),\"\",intlEstQuantity(T116, W116*12, H116)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T116=\"Select Model\",\"\",coilCircuitChange(W116, U116, AC116, T116,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T116=\"Select Model\",\"\",beamWidth(T116))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T116=\"Select Model\",T116=\"PCBL\"), 0,getSPIP(T116, W116, Y116, BD116, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T116=\"Select Model\", \"\",IF(T116=\"PCBL\",0,primaryAirSensibleCapacityIP($T116,$W116,activeRoomTempCooling,activePriAirTempCooling,$Y116,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T116=\"Select Model\",\"\",IF($T116=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y116,activeElevation)))","v":""},{"$f":"IF(OR(T116=\"Select Model\",T116=\"PCBL\"), 0,IF(AD116=0,0,-primaryAirSensibleCapacityIP($T116,$W116,activeRoomTempHeating,activePriAirTempHeating,$Y116,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T116=\"Select Model\", \"\", InductionRatio($T116,BD116,$W116,$Y116)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T116=\"Select Model\", \"\",IF($T116=\"PCBL\",\"N/A\",minVAVSetBack(AA116, Y116))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T116=\"Select Model\", \"\",IF($T116= \"PCBL\",\"N/A\",getDischargeAirTemp($T116,$V116,$AC116,$W116,BD116,$AL116, $Y116, $AS116, \"cooling\",activeElevation,$AB116,$AJ116,$AV116,$BB116))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T116=\"Select Model\",$T116=\"PCBL\"), \"\",getDischargeAirTemp($T116,$V116,$AD116,$W116,BD116,$AL116, $Y116, $AY116, \"heating\",activeElevation,$AB116,$AJ116,$AV116,$BB116)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T116=\"Select Model\", \"\",IF(OR($T116=\"ACBC_1W\",$T116=\"ACBC_2W\",LEFT($T116,4)=\"ACBR\",$T116 = \"LIU24_2W\",LEFT($T116,3)=\"RIU\",LEFT($T116,6)=\"ACBL12\"), IF((soundLevel($T116, $AB116, BD116, $Y116, $W116,$AJ116,$AA116,\"dba\"))<15,\"<15\",soundLevel($T116, $AB116, BD116, $Y116, $W116,$AJ116,$AA116,\"dba\")+0.4),IF((soundLevel($T116, $AB116, BD116, $Y116, $W116,$AJ116,$AA116,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T116, $AB116, BD116, $Y116, $W116,$AJ116,$AA116,\"dba\")+5)<15, \"<15\", soundLevel($T116, $AB116, BD116,$Y116, $W116,$AJ116,$AA116,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T116=\"Select Model\", \"\",IF(OR($T116=\"ACBC_1W\",$T116=\"ACBC_2W\",LEFT($T116,4)=\"ACBR\",$T116=\"LIU24_2W\",LEFT($T116,3)=\"RIU\",LEFT($T116,6)=\"ACBL12\"), IF((soundLevel($T116, $AB116, BD116, $Y116, $W116,$AJ116,$AA116,\"NC\"))<15,\"<15\",soundLevel($T116, $AB116, BD116, $Y116, $W116,$AJ116,$AA116,\"NC\")+0.4),IF((soundLevel($T116, $AB116, BD116, $Y116, $W116,$AJ116,$AA116,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T116, $AB116, BD116, $Y116, $W116,$AJ116,$AA116,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T116, $AB116, BD116, $Y116, $W116,$AJ116,$AA116,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T116=\"Select Model\",\"\",IF($T116=\"LIU24_2W\",calcQwIP($Y116,$W116,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC116,$AI116,\"latent\",$U116&\"P\"&IF($V116=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T116,activeElevation),\"\"))","v":""},{"$f":"IF($T116=\"Select Model\",\"\",IF($T116=\"ACBC_1W\",calcQwIP($Y116,$W116,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC116,BD116,\"capacity\",$U116&\"P\"&IF($V116=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T116,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y116,$W116,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC116,BD116,\"capacity\",$U116&\"P\"&IF($V116=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T116,activeElevation)))","v":""},"",{"$f":"IF(T116=\"Select Model\", 0,waterPressureDrop(W116, U116 & \"P\" & IF(V116=\"Dual\",2,1) &\"C\", AC116, \"cooling\", T116))","v":0},{"$f":"IF(T116=\"Select Model\", \"\",getReturnWaterTemp(T116,AC116, activeEWTCooling, AS116, \"cooling\"))","v":""},"",{"$f":"IF($T116<>\"ACBC_1W\",\"\",IF($J116=\"\",\"\",FintubeCapacity($T116,$W116,$AE116,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T116=\"Select Model\",T116=\"PCBL\"),\"\",calcQwIP(Y116,W116,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD116,BD116,\"capacity\",U116&\"P\"&IF(V116=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T116,activeElevation))","v":""},"",{"$f":"IF(OR(T116=\"Select Model\",T116=\"PCBL\"), \"\",IF(AY116=0,\"N/A\",waterPressureDrop(W116, U116 & \"P\" & IF(V116=\"Dual\",2,1) &\"C\", AD116, \"heating\", T116)))","v":""},{"$f":"IF(OR(T116=\"Select Model\",T116=\"PCBL\"), \"\",IF(AY116=0,getReturnWaterTemp(T116,AE116, activeEWTHeating, AX116, \"heating\"),getReturnWaterTemp(T116,AD116, activeEWTHeating, AY116, \"heating\")))","v":""},"",{"$f":" getNozzle(T116, W116, Y116, Z116, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I117)),I117<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I117, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H117)),H117<0),\"\",intlEstQuantity(T117, W117*12, H117)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T117=\"Select Model\",\"\",coilCircuitChange(W117, U117, AC117, T117,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T117=\"Select Model\",\"\",beamWidth(T117))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T117=\"Select Model\",T117=\"PCBL\"), 0,getSPIP(T117, W117, Y117, BD117, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T117=\"Select Model\", \"\",IF(T117=\"PCBL\",0,primaryAirSensibleCapacityIP($T117,$W117,activeRoomTempCooling,activePriAirTempCooling,$Y117,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T117=\"Select Model\",\"\",IF($T117=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y117,activeElevation)))","v":""},{"$f":"IF(OR(T117=\"Select Model\",T117=\"PCBL\"), 0,IF(AD117=0,0,-primaryAirSensibleCapacityIP($T117,$W117,activeRoomTempHeating,activePriAirTempHeating,$Y117,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T117=\"Select Model\", \"\", InductionRatio($T117,BD117,$W117,$Y117)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T117=\"Select Model\", \"\",IF($T117=\"PCBL\",\"N/A\",minVAVSetBack(AA117, Y117))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T117=\"Select Model\", \"\",IF($T117= \"PCBL\",\"N/A\",getDischargeAirTemp($T117,$V117,$AC117,$W117,BD117,$AL117, $Y117, $AS117, \"cooling\",activeElevation,$AB117,$AJ117,$AV117,$BB117))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T117=\"Select Model\",$T117=\"PCBL\"), \"\",getDischargeAirTemp($T117,$V117,$AD117,$W117,BD117,$AL117, $Y117, $AY117, \"heating\",activeElevation,$AB117,$AJ117,$AV117,$BB117)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T117=\"Select Model\", \"\",IF(OR($T117=\"ACBC_1W\",$T117=\"ACBC_2W\",LEFT($T117,4)=\"ACBR\",$T117 = \"LIU24_2W\",LEFT($T117,3)=\"RIU\",LEFT($T117,6)=\"ACBL12\"), IF((soundLevel($T117, $AB117, BD117, $Y117, $W117,$AJ117,$AA117,\"dba\"))<15,\"<15\",soundLevel($T117, $AB117, BD117, $Y117, $W117,$AJ117,$AA117,\"dba\")+0.4),IF((soundLevel($T117, $AB117, BD117, $Y117, $W117,$AJ117,$AA117,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T117, $AB117, BD117, $Y117, $W117,$AJ117,$AA117,\"dba\")+5)<15, \"<15\", soundLevel($T117, $AB117, BD117,$Y117, $W117,$AJ117,$AA117,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T117=\"Select Model\", \"\",IF(OR($T117=\"ACBC_1W\",$T117=\"ACBC_2W\",LEFT($T117,4)=\"ACBR\",$T117=\"LIU24_2W\",LEFT($T117,3)=\"RIU\",LEFT($T117,6)=\"ACBL12\"), IF((soundLevel($T117, $AB117, BD117, $Y117, $W117,$AJ117,$AA117,\"NC\"))<15,\"<15\",soundLevel($T117, $AB117, BD117, $Y117, $W117,$AJ117,$AA117,\"NC\")+0.4),IF((soundLevel($T117, $AB117, BD117, $Y117, $W117,$AJ117,$AA117,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T117, $AB117, BD117, $Y117, $W117,$AJ117,$AA117,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T117, $AB117, BD117, $Y117, $W117,$AJ117,$AA117,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T117=\"Select Model\",\"\",IF($T117=\"LIU24_2W\",calcQwIP($Y117,$W117,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC117,$AI117,\"latent\",$U117&\"P\"&IF($V117=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T117,activeElevation),\"\"))","v":""},{"$f":"IF($T117=\"Select Model\",\"\",IF($T117=\"ACBC_1W\",calcQwIP($Y117,$W117,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC117,BD117,\"capacity\",$U117&\"P\"&IF($V117=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T117,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y117,$W117,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC117,BD117,\"capacity\",$U117&\"P\"&IF($V117=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T117,activeElevation)))","v":""},"",{"$f":"IF(T117=\"Select Model\", 0,waterPressureDrop(W117, U117 & \"P\" & IF(V117=\"Dual\",2,1) &\"C\", AC117, \"cooling\", T117))","v":0},{"$f":"IF(T117=\"Select Model\", \"\",getReturnWaterTemp(T117,AC117, activeEWTCooling, AS117, \"cooling\"))","v":""},"",{"$f":"IF($T117<>\"ACBC_1W\",\"\",IF($J117=\"\",\"\",FintubeCapacity($T117,$W117,$AE117,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T117=\"Select Model\",T117=\"PCBL\"),\"\",calcQwIP(Y117,W117,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD117,BD117,\"capacity\",U117&\"P\"&IF(V117=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T117,activeElevation))","v":""},"",{"$f":"IF(OR(T117=\"Select Model\",T117=\"PCBL\"), \"\",IF(AY117=0,\"N/A\",waterPressureDrop(W117, U117 & \"P\" & IF(V117=\"Dual\",2,1) &\"C\", AD117, \"heating\", T117)))","v":""},{"$f":"IF(OR(T117=\"Select Model\",T117=\"PCBL\"), \"\",IF(AY117=0,getReturnWaterTemp(T117,AE117, activeEWTHeating, AX117, \"heating\"),getReturnWaterTemp(T117,AD117, activeEWTHeating, AY117, \"heating\")))","v":""},"",{"$f":" getNozzle(T117, W117, Y117, Z117, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I118)),I118<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I118, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H118)),H118<0),\"\",intlEstQuantity(T118, W118*12, H118)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T118=\"Select Model\",\"\",coilCircuitChange(W118, U118, AC118, T118,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T118=\"Select Model\",\"\",beamWidth(T118))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T118=\"Select Model\",T118=\"PCBL\"), 0,getSPIP(T118, W118, Y118, BD118, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T118=\"Select Model\", \"\",IF(T118=\"PCBL\",0,primaryAirSensibleCapacityIP($T118,$W118,activeRoomTempCooling,activePriAirTempCooling,$Y118,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T118=\"Select Model\",\"\",IF($T118=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y118,activeElevation)))","v":""},{"$f":"IF(OR(T118=\"Select Model\",T118=\"PCBL\"), 0,IF(AD118=0,0,-primaryAirSensibleCapacityIP($T118,$W118,activeRoomTempHeating,activePriAirTempHeating,$Y118,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T118=\"Select Model\", \"\", InductionRatio($T118,BD118,$W118,$Y118)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T118=\"Select Model\", \"\",IF($T118=\"PCBL\",\"N/A\",minVAVSetBack(AA118, Y118))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T118=\"Select Model\", \"\",IF($T118= \"PCBL\",\"N/A\",getDischargeAirTemp($T118,$V118,$AC118,$W118,BD118,$AL118, $Y118, $AS118, \"cooling\",activeElevation,$AB118,$AJ118,$AV118,$BB118))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T118=\"Select Model\",$T118=\"PCBL\"), \"\",getDischargeAirTemp($T118,$V118,$AD118,$W118,BD118,$AL118, $Y118, $AY118, \"heating\",activeElevation,$AB118,$AJ118,$AV118,$BB118)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T118=\"Select Model\", \"\",IF(OR($T118=\"ACBC_1W\",$T118=\"ACBC_2W\",LEFT($T118,4)=\"ACBR\",$T118 = \"LIU24_2W\",LEFT($T118,3)=\"RIU\",LEFT($T118,6)=\"ACBL12\"), IF((soundLevel($T118, $AB118, BD118, $Y118, $W118,$AJ118,$AA118,\"dba\"))<15,\"<15\",soundLevel($T118, $AB118, BD118, $Y118, $W118,$AJ118,$AA118,\"dba\")+0.4),IF((soundLevel($T118, $AB118, BD118, $Y118, $W118,$AJ118,$AA118,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T118, $AB118, BD118, $Y118, $W118,$AJ118,$AA118,\"dba\")+5)<15, \"<15\", soundLevel($T118, $AB118, BD118,$Y118, $W118,$AJ118,$AA118,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T118=\"Select Model\", \"\",IF(OR($T118=\"ACBC_1W\",$T118=\"ACBC_2W\",LEFT($T118,4)=\"ACBR\",$T118=\"LIU24_2W\",LEFT($T118,3)=\"RIU\",LEFT($T118,6)=\"ACBL12\"), IF((soundLevel($T118, $AB118, BD118, $Y118, $W118,$AJ118,$AA118,\"NC\"))<15,\"<15\",soundLevel($T118, $AB118, BD118, $Y118, $W118,$AJ118,$AA118,\"NC\")+0.4),IF((soundLevel($T118, $AB118, BD118, $Y118, $W118,$AJ118,$AA118,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T118, $AB118, BD118, $Y118, $W118,$AJ118,$AA118,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T118, $AB118, BD118, $Y118, $W118,$AJ118,$AA118,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T118=\"Select Model\",\"\",IF($T118=\"LIU24_2W\",calcQwIP($Y118,$W118,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC118,$AI118,\"latent\",$U118&\"P\"&IF($V118=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T118,activeElevation),\"\"))","v":""},{"$f":"IF($T118=\"Select Model\",\"\",IF($T118=\"ACBC_1W\",calcQwIP($Y118,$W118,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC118,BD118,\"capacity\",$U118&\"P\"&IF($V118=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T118,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y118,$W118,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC118,BD118,\"capacity\",$U118&\"P\"&IF($V118=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T118,activeElevation)))","v":""},"",{"$f":"IF(T118=\"Select Model\", 0,waterPressureDrop(W118, U118 & \"P\" & IF(V118=\"Dual\",2,1) &\"C\", AC118, \"cooling\", T118))","v":0},{"$f":"IF(T118=\"Select Model\", \"\",getReturnWaterTemp(T118,AC118, activeEWTCooling, AS118, \"cooling\"))","v":""},"",{"$f":"IF($T118<>\"ACBC_1W\",\"\",IF($J118=\"\",\"\",FintubeCapacity($T118,$W118,$AE118,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T118=\"Select Model\",T118=\"PCBL\"),\"\",calcQwIP(Y118,W118,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD118,BD118,\"capacity\",U118&\"P\"&IF(V118=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T118,activeElevation))","v":""},"",{"$f":"IF(OR(T118=\"Select Model\",T118=\"PCBL\"), \"\",IF(AY118=0,\"N/A\",waterPressureDrop(W118, U118 & \"P\" & IF(V118=\"Dual\",2,1) &\"C\", AD118, \"heating\", T118)))","v":""},{"$f":"IF(OR(T118=\"Select Model\",T118=\"PCBL\"), \"\",IF(AY118=0,getReturnWaterTemp(T118,AE118, activeEWTHeating, AX118, \"heating\"),getReturnWaterTemp(T118,AD118, activeEWTHeating, AY118, \"heating\")))","v":""},"",{"$f":" getNozzle(T118, W118, Y118, Z118, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I119)),I119<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I119, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H119)),H119<0),\"\",intlEstQuantity(T119, W119*12, H119)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T119=\"Select Model\",\"\",coilCircuitChange(W119, U119, AC119, T119,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T119=\"Select Model\",\"\",beamWidth(T119))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T119=\"Select Model\",T119=\"PCBL\"), 0,getSPIP(T119, W119, Y119, BD119, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T119=\"Select Model\", \"\",IF(T119=\"PCBL\",0,primaryAirSensibleCapacityIP($T119,$W119,activeRoomTempCooling,activePriAirTempCooling,$Y119,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T119=\"Select Model\",\"\",IF($T119=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y119,activeElevation)))","v":""},{"$f":"IF(OR(T119=\"Select Model\",T119=\"PCBL\"), 0,IF(AD119=0,0,-primaryAirSensibleCapacityIP($T119,$W119,activeRoomTempHeating,activePriAirTempHeating,$Y119,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T119=\"Select Model\", \"\", InductionRatio($T119,BD119,$W119,$Y119)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T119=\"Select Model\", \"\",IF($T119=\"PCBL\",\"N/A\",minVAVSetBack(AA119, Y119))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T119=\"Select Model\", \"\",IF($T119= \"PCBL\",\"N/A\",getDischargeAirTemp($T119,$V119,$AC119,$W119,BD119,$AL119, $Y119, $AS119, \"cooling\",activeElevation,$AB119,$AJ119,$AV119,$BB119))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T119=\"Select Model\",$T119=\"PCBL\"), \"\",getDischargeAirTemp($T119,$V119,$AD119,$W119,BD119,$AL119, $Y119, $AY119, \"heating\",activeElevation,$AB119,$AJ119,$AV119,$BB119)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T119=\"Select Model\", \"\",IF(OR($T119=\"ACBC_1W\",$T119=\"ACBC_2W\",LEFT($T119,4)=\"ACBR\",$T119 = \"LIU24_2W\",LEFT($T119,3)=\"RIU\",LEFT($T119,6)=\"ACBL12\"), IF((soundLevel($T119, $AB119, BD119, $Y119, $W119,$AJ119,$AA119,\"dba\"))<15,\"<15\",soundLevel($T119, $AB119, BD119, $Y119, $W119,$AJ119,$AA119,\"dba\")+0.4),IF((soundLevel($T119, $AB119, BD119, $Y119, $W119,$AJ119,$AA119,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T119, $AB119, BD119, $Y119, $W119,$AJ119,$AA119,\"dba\")+5)<15, \"<15\", soundLevel($T119, $AB119, BD119,$Y119, $W119,$AJ119,$AA119,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T119=\"Select Model\", \"\",IF(OR($T119=\"ACBC_1W\",$T119=\"ACBC_2W\",LEFT($T119,4)=\"ACBR\",$T119=\"LIU24_2W\",LEFT($T119,3)=\"RIU\",LEFT($T119,6)=\"ACBL12\"), IF((soundLevel($T119, $AB119, BD119, $Y119, $W119,$AJ119,$AA119,\"NC\"))<15,\"<15\",soundLevel($T119, $AB119, BD119, $Y119, $W119,$AJ119,$AA119,\"NC\")+0.4),IF((soundLevel($T119, $AB119, BD119, $Y119, $W119,$AJ119,$AA119,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T119, $AB119, BD119, $Y119, $W119,$AJ119,$AA119,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T119, $AB119, BD119, $Y119, $W119,$AJ119,$AA119,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T119=\"Select Model\",\"\",IF($T119=\"LIU24_2W\",calcQwIP($Y119,$W119,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC119,$AI119,\"latent\",$U119&\"P\"&IF($V119=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T119,activeElevation),\"\"))","v":""},{"$f":"IF($T119=\"Select Model\",\"\",IF($T119=\"ACBC_1W\",calcQwIP($Y119,$W119,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC119,BD119,\"capacity\",$U119&\"P\"&IF($V119=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T119,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y119,$W119,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC119,BD119,\"capacity\",$U119&\"P\"&IF($V119=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T119,activeElevation)))","v":""},"",{"$f":"IF(T119=\"Select Model\", 0,waterPressureDrop(W119, U119 & \"P\" & IF(V119=\"Dual\",2,1) &\"C\", AC119, \"cooling\", T119))","v":0},{"$f":"IF(T119=\"Select Model\", \"\",getReturnWaterTemp(T119,AC119, activeEWTCooling, AS119, \"cooling\"))","v":""},"",{"$f":"IF($T119<>\"ACBC_1W\",\"\",IF($J119=\"\",\"\",FintubeCapacity($T119,$W119,$AE119,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T119=\"Select Model\",T119=\"PCBL\"),\"\",calcQwIP(Y119,W119,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD119,BD119,\"capacity\",U119&\"P\"&IF(V119=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T119,activeElevation))","v":""},"",{"$f":"IF(OR(T119=\"Select Model\",T119=\"PCBL\"), \"\",IF(AY119=0,\"N/A\",waterPressureDrop(W119, U119 & \"P\" & IF(V119=\"Dual\",2,1) &\"C\", AD119, \"heating\", T119)))","v":""},{"$f":"IF(OR(T119=\"Select Model\",T119=\"PCBL\"), \"\",IF(AY119=0,getReturnWaterTemp(T119,AE119, activeEWTHeating, AX119, \"heating\"),getReturnWaterTemp(T119,AD119, activeEWTHeating, AY119, \"heating\")))","v":""},"",{"$f":" getNozzle(T119, W119, Y119, Z119, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I120)),I120<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I120, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H120)),H120<0),\"\",intlEstQuantity(T120, W120*12, H120)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T120=\"Select Model\",\"\",coilCircuitChange(W120, U120, AC120, T120,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T120=\"Select Model\",\"\",beamWidth(T120))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T120=\"Select Model\",T120=\"PCBL\"), 0,getSPIP(T120, W120, Y120, BD120, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T120=\"Select Model\", \"\",IF(T120=\"PCBL\",0,primaryAirSensibleCapacityIP($T120,$W120,activeRoomTempCooling,activePriAirTempCooling,$Y120,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T120=\"Select Model\",\"\",IF($T120=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y120,activeElevation)))","v":""},{"$f":"IF(OR(T120=\"Select Model\",T120=\"PCBL\"), 0,IF(AD120=0,0,-primaryAirSensibleCapacityIP($T120,$W120,activeRoomTempHeating,activePriAirTempHeating,$Y120,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T120=\"Select Model\", \"\", InductionRatio($T120,BD120,$W120,$Y120)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T120=\"Select Model\", \"\",IF($T120=\"PCBL\",\"N/A\",minVAVSetBack(AA120, Y120))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T120=\"Select Model\", \"\",IF($T120= \"PCBL\",\"N/A\",getDischargeAirTemp($T120,$V120,$AC120,$W120,BD120,$AL120, $Y120, $AS120, \"cooling\",activeElevation,$AB120,$AJ120,$AV120,$BB120))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T120=\"Select Model\",$T120=\"PCBL\"), \"\",getDischargeAirTemp($T120,$V120,$AD120,$W120,BD120,$AL120, $Y120, $AY120, \"heating\",activeElevation,$AB120,$AJ120,$AV120,$BB120)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T120=\"Select Model\", \"\",IF(OR($T120=\"ACBC_1W\",$T120=\"ACBC_2W\",LEFT($T120,4)=\"ACBR\",$T120 = \"LIU24_2W\",LEFT($T120,3)=\"RIU\",LEFT($T120,6)=\"ACBL12\"), IF((soundLevel($T120, $AB120, BD120, $Y120, $W120,$AJ120,$AA120,\"dba\"))<15,\"<15\",soundLevel($T120, $AB120, BD120, $Y120, $W120,$AJ120,$AA120,\"dba\")+0.4),IF((soundLevel($T120, $AB120, BD120, $Y120, $W120,$AJ120,$AA120,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T120, $AB120, BD120, $Y120, $W120,$AJ120,$AA120,\"dba\")+5)<15, \"<15\", soundLevel($T120, $AB120, BD120,$Y120, $W120,$AJ120,$AA120,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T120=\"Select Model\", \"\",IF(OR($T120=\"ACBC_1W\",$T120=\"ACBC_2W\",LEFT($T120,4)=\"ACBR\",$T120=\"LIU24_2W\",LEFT($T120,3)=\"RIU\",LEFT($T120,6)=\"ACBL12\"), IF((soundLevel($T120, $AB120, BD120, $Y120, $W120,$AJ120,$AA120,\"NC\"))<15,\"<15\",soundLevel($T120, $AB120, BD120, $Y120, $W120,$AJ120,$AA120,\"NC\")+0.4),IF((soundLevel($T120, $AB120, BD120, $Y120, $W120,$AJ120,$AA120,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T120, $AB120, BD120, $Y120, $W120,$AJ120,$AA120,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T120, $AB120, BD120, $Y120, $W120,$AJ120,$AA120,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T120=\"Select Model\",\"\",IF($T120=\"LIU24_2W\",calcQwIP($Y120,$W120,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC120,$AI120,\"latent\",$U120&\"P\"&IF($V120=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T120,activeElevation),\"\"))","v":""},{"$f":"IF($T120=\"Select Model\",\"\",IF($T120=\"ACBC_1W\",calcQwIP($Y120,$W120,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC120,BD120,\"capacity\",$U120&\"P\"&IF($V120=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T120,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y120,$W120,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC120,BD120,\"capacity\",$U120&\"P\"&IF($V120=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T120,activeElevation)))","v":""},"",{"$f":"IF(T120=\"Select Model\", 0,waterPressureDrop(W120, U120 & \"P\" & IF(V120=\"Dual\",2,1) &\"C\", AC120, \"cooling\", T120))","v":0},{"$f":"IF(T120=\"Select Model\", \"\",getReturnWaterTemp(T120,AC120, activeEWTCooling, AS120, \"cooling\"))","v":""},"",{"$f":"IF($T120<>\"ACBC_1W\",\"\",IF($J120=\"\",\"\",FintubeCapacity($T120,$W120,$AE120,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T120=\"Select Model\",T120=\"PCBL\"),\"\",calcQwIP(Y120,W120,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD120,BD120,\"capacity\",U120&\"P\"&IF(V120=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T120,activeElevation))","v":""},"",{"$f":"IF(OR(T120=\"Select Model\",T120=\"PCBL\"), \"\",IF(AY120=0,\"N/A\",waterPressureDrop(W120, U120 & \"P\" & IF(V120=\"Dual\",2,1) &\"C\", AD120, \"heating\", T120)))","v":""},{"$f":"IF(OR(T120=\"Select Model\",T120=\"PCBL\"), \"\",IF(AY120=0,getReturnWaterTemp(T120,AE120, activeEWTHeating, AX120, \"heating\"),getReturnWaterTemp(T120,AD120, activeEWTHeating, AY120, \"heating\")))","v":""},"",{"$f":" getNozzle(T120, W120, Y120, Z120, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I121)),I121<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I121, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H121)),H121<0),\"\",intlEstQuantity(T121, W121*12, H121)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T121=\"Select Model\",\"\",coilCircuitChange(W121, U121, AC121, T121,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T121=\"Select Model\",\"\",beamWidth(T121))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T121=\"Select Model\",T121=\"PCBL\"), 0,getSPIP(T121, W121, Y121, BD121, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T121=\"Select Model\", \"\",IF(T121=\"PCBL\",0,primaryAirSensibleCapacityIP($T121,$W121,activeRoomTempCooling,activePriAirTempCooling,$Y121,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T121=\"Select Model\",\"\",IF($T121=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y121,activeElevation)))","v":""},{"$f":"IF(OR(T121=\"Select Model\",T121=\"PCBL\"), 0,IF(AD121=0,0,-primaryAirSensibleCapacityIP($T121,$W121,activeRoomTempHeating,activePriAirTempHeating,$Y121,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T121=\"Select Model\", \"\", InductionRatio($T121,BD121,$W121,$Y121)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T121=\"Select Model\", \"\",IF($T121=\"PCBL\",\"N/A\",minVAVSetBack(AA121, Y121))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T121=\"Select Model\", \"\",IF($T121= \"PCBL\",\"N/A\",getDischargeAirTemp($T121,$V121,$AC121,$W121,BD121,$AL121, $Y121, $AS121, \"cooling\",activeElevation,$AB121,$AJ121,$AV121,$BB121))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T121=\"Select Model\",$T121=\"PCBL\"), \"\",getDischargeAirTemp($T121,$V121,$AD121,$W121,BD121,$AL121, $Y121, $AY121, \"heating\",activeElevation,$AB121,$AJ121,$AV121,$BB121)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T121=\"Select Model\", \"\",IF(OR($T121=\"ACBC_1W\",$T121=\"ACBC_2W\",LEFT($T121,4)=\"ACBR\",$T121 = \"LIU24_2W\",LEFT($T121,3)=\"RIU\",LEFT($T121,6)=\"ACBL12\"), IF((soundLevel($T121, $AB121, BD121, $Y121, $W121,$AJ121,$AA121,\"dba\"))<15,\"<15\",soundLevel($T121, $AB121, BD121, $Y121, $W121,$AJ121,$AA121,\"dba\")+0.4),IF((soundLevel($T121, $AB121, BD121, $Y121, $W121,$AJ121,$AA121,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T121, $AB121, BD121, $Y121, $W121,$AJ121,$AA121,\"dba\")+5)<15, \"<15\", soundLevel($T121, $AB121, BD121,$Y121, $W121,$AJ121,$AA121,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T121=\"Select Model\", \"\",IF(OR($T121=\"ACBC_1W\",$T121=\"ACBC_2W\",LEFT($T121,4)=\"ACBR\",$T121=\"LIU24_2W\",LEFT($T121,3)=\"RIU\",LEFT($T121,6)=\"ACBL12\"), IF((soundLevel($T121, $AB121, BD121, $Y121, $W121,$AJ121,$AA121,\"NC\"))<15,\"<15\",soundLevel($T121, $AB121, BD121, $Y121, $W121,$AJ121,$AA121,\"NC\")+0.4),IF((soundLevel($T121, $AB121, BD121, $Y121, $W121,$AJ121,$AA121,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T121, $AB121, BD121, $Y121, $W121,$AJ121,$AA121,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T121, $AB121, BD121, $Y121, $W121,$AJ121,$AA121,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T121=\"Select Model\",\"\",IF($T121=\"LIU24_2W\",calcQwIP($Y121,$W121,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC121,$AI121,\"latent\",$U121&\"P\"&IF($V121=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T121,activeElevation),\"\"))","v":""},{"$f":"IF($T121=\"Select Model\",\"\",IF($T121=\"ACBC_1W\",calcQwIP($Y121,$W121,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC121,BD121,\"capacity\",$U121&\"P\"&IF($V121=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T121,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y121,$W121,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC121,BD121,\"capacity\",$U121&\"P\"&IF($V121=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T121,activeElevation)))","v":""},"",{"$f":"IF(T121=\"Select Model\", 0,waterPressureDrop(W121, U121 & \"P\" & IF(V121=\"Dual\",2,1) &\"C\", AC121, \"cooling\", T121))","v":0},{"$f":"IF(T121=\"Select Model\", \"\",getReturnWaterTemp(T121,AC121, activeEWTCooling, AS121, \"cooling\"))","v":""},"",{"$f":"IF($T121<>\"ACBC_1W\",\"\",IF($J121=\"\",\"\",FintubeCapacity($T121,$W121,$AE121,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T121=\"Select Model\",T121=\"PCBL\"),\"\",calcQwIP(Y121,W121,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD121,BD121,\"capacity\",U121&\"P\"&IF(V121=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T121,activeElevation))","v":""},"",{"$f":"IF(OR(T121=\"Select Model\",T121=\"PCBL\"), \"\",IF(AY121=0,\"N/A\",waterPressureDrop(W121, U121 & \"P\" & IF(V121=\"Dual\",2,1) &\"C\", AD121, \"heating\", T121)))","v":""},{"$f":"IF(OR(T121=\"Select Model\",T121=\"PCBL\"), \"\",IF(AY121=0,getReturnWaterTemp(T121,AE121, activeEWTHeating, AX121, \"heating\"),getReturnWaterTemp(T121,AD121, activeEWTHeating, AY121, \"heating\")))","v":""},"",{"$f":" getNozzle(T121, W121, Y121, Z121, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I122)),I122<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I122, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H122)),H122<0),\"\",intlEstQuantity(T122, W122*12, H122)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T122=\"Select Model\",\"\",coilCircuitChange(W122, U122, AC122, T122,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T122=\"Select Model\",\"\",beamWidth(T122))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T122=\"Select Model\",T122=\"PCBL\"), 0,getSPIP(T122, W122, Y122, BD122, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T122=\"Select Model\", \"\",IF(T122=\"PCBL\",0,primaryAirSensibleCapacityIP($T122,$W122,activeRoomTempCooling,activePriAirTempCooling,$Y122,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T122=\"Select Model\",\"\",IF($T122=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y122,activeElevation)))","v":""},{"$f":"IF(OR(T122=\"Select Model\",T122=\"PCBL\"), 0,IF(AD122=0,0,-primaryAirSensibleCapacityIP($T122,$W122,activeRoomTempHeating,activePriAirTempHeating,$Y122,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T122=\"Select Model\", \"\", InductionRatio($T122,BD122,$W122,$Y122)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T122=\"Select Model\", \"\",IF($T122=\"PCBL\",\"N/A\",minVAVSetBack(AA122, Y122))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T122=\"Select Model\", \"\",IF($T122= \"PCBL\",\"N/A\",getDischargeAirTemp($T122,$V122,$AC122,$W122,BD122,$AL122, $Y122, $AS122, \"cooling\",activeElevation,$AB122,$AJ122,$AV122,$BB122))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T122=\"Select Model\",$T122=\"PCBL\"), \"\",getDischargeAirTemp($T122,$V122,$AD122,$W122,BD122,$AL122, $Y122, $AY122, \"heating\",activeElevation,$AB122,$AJ122,$AV122,$BB122)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T122=\"Select Model\", \"\",IF(OR($T122=\"ACBC_1W\",$T122=\"ACBC_2W\",LEFT($T122,4)=\"ACBR\",$T122 = \"LIU24_2W\",LEFT($T122,3)=\"RIU\",LEFT($T122,6)=\"ACBL12\"), IF((soundLevel($T122, $AB122, BD122, $Y122, $W122,$AJ122,$AA122,\"dba\"))<15,\"<15\",soundLevel($T122, $AB122, BD122, $Y122, $W122,$AJ122,$AA122,\"dba\")+0.4),IF((soundLevel($T122, $AB122, BD122, $Y122, $W122,$AJ122,$AA122,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T122, $AB122, BD122, $Y122, $W122,$AJ122,$AA122,\"dba\")+5)<15, \"<15\", soundLevel($T122, $AB122, BD122,$Y122, $W122,$AJ122,$AA122,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T122=\"Select Model\", \"\",IF(OR($T122=\"ACBC_1W\",$T122=\"ACBC_2W\",LEFT($T122,4)=\"ACBR\",$T122=\"LIU24_2W\",LEFT($T122,3)=\"RIU\",LEFT($T122,6)=\"ACBL12\"), IF((soundLevel($T122, $AB122, BD122, $Y122, $W122,$AJ122,$AA122,\"NC\"))<15,\"<15\",soundLevel($T122, $AB122, BD122, $Y122, $W122,$AJ122,$AA122,\"NC\")+0.4),IF((soundLevel($T122, $AB122, BD122, $Y122, $W122,$AJ122,$AA122,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T122, $AB122, BD122, $Y122, $W122,$AJ122,$AA122,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T122, $AB122, BD122, $Y122, $W122,$AJ122,$AA122,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T122=\"Select Model\",\"\",IF($T122=\"LIU24_2W\",calcQwIP($Y122,$W122,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC122,$AI122,\"latent\",$U122&\"P\"&IF($V122=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T122,activeElevation),\"\"))","v":""},{"$f":"IF($T122=\"Select Model\",\"\",IF($T122=\"ACBC_1W\",calcQwIP($Y122,$W122,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC122,BD122,\"capacity\",$U122&\"P\"&IF($V122=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T122,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y122,$W122,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC122,BD122,\"capacity\",$U122&\"P\"&IF($V122=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T122,activeElevation)))","v":""},"",{"$f":"IF(T122=\"Select Model\", 0,waterPressureDrop(W122, U122 & \"P\" & IF(V122=\"Dual\",2,1) &\"C\", AC122, \"cooling\", T122))","v":0},{"$f":"IF(T122=\"Select Model\", \"\",getReturnWaterTemp(T122,AC122, activeEWTCooling, AS122, \"cooling\"))","v":""},"",{"$f":"IF($T122<>\"ACBC_1W\",\"\",IF($J122=\"\",\"\",FintubeCapacity($T122,$W122,$AE122,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T122=\"Select Model\",T122=\"PCBL\"),\"\",calcQwIP(Y122,W122,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD122,BD122,\"capacity\",U122&\"P\"&IF(V122=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T122,activeElevation))","v":""},"",{"$f":"IF(OR(T122=\"Select Model\",T122=\"PCBL\"), \"\",IF(AY122=0,\"N/A\",waterPressureDrop(W122, U122 & \"P\" & IF(V122=\"Dual\",2,1) &\"C\", AD122, \"heating\", T122)))","v":""},{"$f":"IF(OR(T122=\"Select Model\",T122=\"PCBL\"), \"\",IF(AY122=0,getReturnWaterTemp(T122,AE122, activeEWTHeating, AX122, \"heating\"),getReturnWaterTemp(T122,AD122, activeEWTHeating, AY122, \"heating\")))","v":""},"",{"$f":" getNozzle(T122, W122, Y122, Z122, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I123)),I123<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I123, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H123)),H123<0),\"\",intlEstQuantity(T123, W123*12, H123)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T123=\"Select Model\",\"\",coilCircuitChange(W123, U123, AC123, T123,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T123=\"Select Model\",\"\",beamWidth(T123))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T123=\"Select Model\",T123=\"PCBL\"), 0,getSPIP(T123, W123, Y123, BD123, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T123=\"Select Model\", \"\",IF(T123=\"PCBL\",0,primaryAirSensibleCapacityIP($T123,$W123,activeRoomTempCooling,activePriAirTempCooling,$Y123,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T123=\"Select Model\",\"\",IF($T123=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y123,activeElevation)))","v":""},{"$f":"IF(OR(T123=\"Select Model\",T123=\"PCBL\"), 0,IF(AD123=0,0,-primaryAirSensibleCapacityIP($T123,$W123,activeRoomTempHeating,activePriAirTempHeating,$Y123,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T123=\"Select Model\", \"\", InductionRatio($T123,BD123,$W123,$Y123)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T123=\"Select Model\", \"\",IF($T123=\"PCBL\",\"N/A\",minVAVSetBack(AA123, Y123))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T123=\"Select Model\", \"\",IF($T123= \"PCBL\",\"N/A\",getDischargeAirTemp($T123,$V123,$AC123,$W123,BD123,$AL123, $Y123, $AS123, \"cooling\",activeElevation,$AB123,$AJ123,$AV123,$BB123))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T123=\"Select Model\",$T123=\"PCBL\"), \"\",getDischargeAirTemp($T123,$V123,$AD123,$W123,BD123,$AL123, $Y123, $AY123, \"heating\",activeElevation,$AB123,$AJ123,$AV123,$BB123)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T123=\"Select Model\", \"\",IF(OR($T123=\"ACBC_1W\",$T123=\"ACBC_2W\",LEFT($T123,4)=\"ACBR\",$T123 = \"LIU24_2W\",LEFT($T123,3)=\"RIU\",LEFT($T123,6)=\"ACBL12\"), IF((soundLevel($T123, $AB123, BD123, $Y123, $W123,$AJ123,$AA123,\"dba\"))<15,\"<15\",soundLevel($T123, $AB123, BD123, $Y123, $W123,$AJ123,$AA123,\"dba\")+0.4),IF((soundLevel($T123, $AB123, BD123, $Y123, $W123,$AJ123,$AA123,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T123, $AB123, BD123, $Y123, $W123,$AJ123,$AA123,\"dba\")+5)<15, \"<15\", soundLevel($T123, $AB123, BD123,$Y123, $W123,$AJ123,$AA123,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T123=\"Select Model\", \"\",IF(OR($T123=\"ACBC_1W\",$T123=\"ACBC_2W\",LEFT($T123,4)=\"ACBR\",$T123=\"LIU24_2W\",LEFT($T123,3)=\"RIU\",LEFT($T123,6)=\"ACBL12\"), IF((soundLevel($T123, $AB123, BD123, $Y123, $W123,$AJ123,$AA123,\"NC\"))<15,\"<15\",soundLevel($T123, $AB123, BD123, $Y123, $W123,$AJ123,$AA123,\"NC\")+0.4),IF((soundLevel($T123, $AB123, BD123, $Y123, $W123,$AJ123,$AA123,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T123, $AB123, BD123, $Y123, $W123,$AJ123,$AA123,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T123, $AB123, BD123, $Y123, $W123,$AJ123,$AA123,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T123=\"Select Model\",\"\",IF($T123=\"LIU24_2W\",calcQwIP($Y123,$W123,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC123,$AI123,\"latent\",$U123&\"P\"&IF($V123=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T123,activeElevation),\"\"))","v":""},{"$f":"IF($T123=\"Select Model\",\"\",IF($T123=\"ACBC_1W\",calcQwIP($Y123,$W123,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC123,BD123,\"capacity\",$U123&\"P\"&IF($V123=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T123,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y123,$W123,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC123,BD123,\"capacity\",$U123&\"P\"&IF($V123=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T123,activeElevation)))","v":""},"",{"$f":"IF(T123=\"Select Model\", 0,waterPressureDrop(W123, U123 & \"P\" & IF(V123=\"Dual\",2,1) &\"C\", AC123, \"cooling\", T123))","v":0},{"$f":"IF(T123=\"Select Model\", \"\",getReturnWaterTemp(T123,AC123, activeEWTCooling, AS123, \"cooling\"))","v":""},"",{"$f":"IF($T123<>\"ACBC_1W\",\"\",IF($J123=\"\",\"\",FintubeCapacity($T123,$W123,$AE123,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T123=\"Select Model\",T123=\"PCBL\"),\"\",calcQwIP(Y123,W123,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD123,BD123,\"capacity\",U123&\"P\"&IF(V123=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T123,activeElevation))","v":""},"",{"$f":"IF(OR(T123=\"Select Model\",T123=\"PCBL\"), \"\",IF(AY123=0,\"N/A\",waterPressureDrop(W123, U123 & \"P\" & IF(V123=\"Dual\",2,1) &\"C\", AD123, \"heating\", T123)))","v":""},{"$f":"IF(OR(T123=\"Select Model\",T123=\"PCBL\"), \"\",IF(AY123=0,getReturnWaterTemp(T123,AE123, activeEWTHeating, AX123, \"heating\"),getReturnWaterTemp(T123,AD123, activeEWTHeating, AY123, \"heating\")))","v":""},"",{"$f":" getNozzle(T123, W123, Y123, Z123, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I124)),I124<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I124, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H124)),H124<0),\"\",intlEstQuantity(T124, W124*12, H124)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T124=\"Select Model\",\"\",coilCircuitChange(W124, U124, AC124, T124,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T124=\"Select Model\",\"\",beamWidth(T124))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T124=\"Select Model\",T124=\"PCBL\"), 0,getSPIP(T124, W124, Y124, BD124, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T124=\"Select Model\", \"\",IF(T124=\"PCBL\",0,primaryAirSensibleCapacityIP($T124,$W124,activeRoomTempCooling,activePriAirTempCooling,$Y124,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T124=\"Select Model\",\"\",IF($T124=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y124,activeElevation)))","v":""},{"$f":"IF(OR(T124=\"Select Model\",T124=\"PCBL\"), 0,IF(AD124=0,0,-primaryAirSensibleCapacityIP($T124,$W124,activeRoomTempHeating,activePriAirTempHeating,$Y124,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T124=\"Select Model\", \"\", InductionRatio($T124,BD124,$W124,$Y124)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T124=\"Select Model\", \"\",IF($T124=\"PCBL\",\"N/A\",minVAVSetBack(AA124, Y124))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T124=\"Select Model\", \"\",IF($T124= \"PCBL\",\"N/A\",getDischargeAirTemp($T124,$V124,$AC124,$W124,BD124,$AL124, $Y124, $AS124, \"cooling\",activeElevation,$AB124,$AJ124,$AV124,$BB124))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T124=\"Select Model\",$T124=\"PCBL\"), \"\",getDischargeAirTemp($T124,$V124,$AD124,$W124,BD124,$AL124, $Y124, $AY124, \"heating\",activeElevation,$AB124,$AJ124,$AV124,$BB124)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T124=\"Select Model\", \"\",IF(OR($T124=\"ACBC_1W\",$T124=\"ACBC_2W\",LEFT($T124,4)=\"ACBR\",$T124 = \"LIU24_2W\",LEFT($T124,3)=\"RIU\",LEFT($T124,6)=\"ACBL12\"), IF((soundLevel($T124, $AB124, BD124, $Y124, $W124,$AJ124,$AA124,\"dba\"))<15,\"<15\",soundLevel($T124, $AB124, BD124, $Y124, $W124,$AJ124,$AA124,\"dba\")+0.4),IF((soundLevel($T124, $AB124, BD124, $Y124, $W124,$AJ124,$AA124,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T124, $AB124, BD124, $Y124, $W124,$AJ124,$AA124,\"dba\")+5)<15, \"<15\", soundLevel($T124, $AB124, BD124,$Y124, $W124,$AJ124,$AA124,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T124=\"Select Model\", \"\",IF(OR($T124=\"ACBC_1W\",$T124=\"ACBC_2W\",LEFT($T124,4)=\"ACBR\",$T124=\"LIU24_2W\",LEFT($T124,3)=\"RIU\",LEFT($T124,6)=\"ACBL12\"), IF((soundLevel($T124, $AB124, BD124, $Y124, $W124,$AJ124,$AA124,\"NC\"))<15,\"<15\",soundLevel($T124, $AB124, BD124, $Y124, $W124,$AJ124,$AA124,\"NC\")+0.4),IF((soundLevel($T124, $AB124, BD124, $Y124, $W124,$AJ124,$AA124,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T124, $AB124, BD124, $Y124, $W124,$AJ124,$AA124,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T124, $AB124, BD124, $Y124, $W124,$AJ124,$AA124,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T124=\"Select Model\",\"\",IF($T124=\"LIU24_2W\",calcQwIP($Y124,$W124,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC124,$AI124,\"latent\",$U124&\"P\"&IF($V124=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T124,activeElevation),\"\"))","v":""},{"$f":"IF($T124=\"Select Model\",\"\",IF($T124=\"ACBC_1W\",calcQwIP($Y124,$W124,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC124,BD124,\"capacity\",$U124&\"P\"&IF($V124=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T124,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y124,$W124,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC124,BD124,\"capacity\",$U124&\"P\"&IF($V124=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T124,activeElevation)))","v":""},"",{"$f":"IF(T124=\"Select Model\", 0,waterPressureDrop(W124, U124 & \"P\" & IF(V124=\"Dual\",2,1) &\"C\", AC124, \"cooling\", T124))","v":0},{"$f":"IF(T124=\"Select Model\", \"\",getReturnWaterTemp(T124,AC124, activeEWTCooling, AS124, \"cooling\"))","v":""},"",{"$f":"IF($T124<>\"ACBC_1W\",\"\",IF($J124=\"\",\"\",FintubeCapacity($T124,$W124,$AE124,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T124=\"Select Model\",T124=\"PCBL\"),\"\",calcQwIP(Y124,W124,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD124,BD124,\"capacity\",U124&\"P\"&IF(V124=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T124,activeElevation))","v":""},"",{"$f":"IF(OR(T124=\"Select Model\",T124=\"PCBL\"), \"\",IF(AY124=0,\"N/A\",waterPressureDrop(W124, U124 & \"P\" & IF(V124=\"Dual\",2,1) &\"C\", AD124, \"heating\", T124)))","v":""},{"$f":"IF(OR(T124=\"Select Model\",T124=\"PCBL\"), \"\",IF(AY124=0,getReturnWaterTemp(T124,AE124, activeEWTHeating, AX124, \"heating\"),getReturnWaterTemp(T124,AD124, activeEWTHeating, AY124, \"heating\")))","v":""},"",{"$f":" getNozzle(T124, W124, Y124, Z124, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I125)),I125<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I125, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H125)),H125<0),\"\",intlEstQuantity(T125, W125*12, H125)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T125=\"Select Model\",\"\",coilCircuitChange(W125, U125, AC125, T125,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T125=\"Select Model\",\"\",beamWidth(T125))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T125=\"Select Model\",T125=\"PCBL\"), 0,getSPIP(T125, W125, Y125, BD125, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T125=\"Select Model\", \"\",IF(T125=\"PCBL\",0,primaryAirSensibleCapacityIP($T125,$W125,activeRoomTempCooling,activePriAirTempCooling,$Y125,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T125=\"Select Model\",\"\",IF($T125=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y125,activeElevation)))","v":""},{"$f":"IF(OR(T125=\"Select Model\",T125=\"PCBL\"), 0,IF(AD125=0,0,-primaryAirSensibleCapacityIP($T125,$W125,activeRoomTempHeating,activePriAirTempHeating,$Y125,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T125=\"Select Model\", \"\", InductionRatio($T125,BD125,$W125,$Y125)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T125=\"Select Model\", \"\",IF($T125=\"PCBL\",\"N/A\",minVAVSetBack(AA125, Y125))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T125=\"Select Model\", \"\",IF($T125= \"PCBL\",\"N/A\",getDischargeAirTemp($T125,$V125,$AC125,$W125,BD125,$AL125, $Y125, $AS125, \"cooling\",activeElevation,$AB125,$AJ125,$AV125,$BB125))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T125=\"Select Model\",$T125=\"PCBL\"), \"\",getDischargeAirTemp($T125,$V125,$AD125,$W125,BD125,$AL125, $Y125, $AY125, \"heating\",activeElevation,$AB125,$AJ125,$AV125,$BB125)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T125=\"Select Model\", \"\",IF(OR($T125=\"ACBC_1W\",$T125=\"ACBC_2W\",LEFT($T125,4)=\"ACBR\",$T125 = \"LIU24_2W\",LEFT($T125,3)=\"RIU\",LEFT($T125,6)=\"ACBL12\"), IF((soundLevel($T125, $AB125, BD125, $Y125, $W125,$AJ125,$AA125,\"dba\"))<15,\"<15\",soundLevel($T125, $AB125, BD125, $Y125, $W125,$AJ125,$AA125,\"dba\")+0.4),IF((soundLevel($T125, $AB125, BD125, $Y125, $W125,$AJ125,$AA125,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T125, $AB125, BD125, $Y125, $W125,$AJ125,$AA125,\"dba\")+5)<15, \"<15\", soundLevel($T125, $AB125, BD125,$Y125, $W125,$AJ125,$AA125,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T125=\"Select Model\", \"\",IF(OR($T125=\"ACBC_1W\",$T125=\"ACBC_2W\",LEFT($T125,4)=\"ACBR\",$T125=\"LIU24_2W\",LEFT($T125,3)=\"RIU\",LEFT($T125,6)=\"ACBL12\"), IF((soundLevel($T125, $AB125, BD125, $Y125, $W125,$AJ125,$AA125,\"NC\"))<15,\"<15\",soundLevel($T125, $AB125, BD125, $Y125, $W125,$AJ125,$AA125,\"NC\")+0.4),IF((soundLevel($T125, $AB125, BD125, $Y125, $W125,$AJ125,$AA125,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T125, $AB125, BD125, $Y125, $W125,$AJ125,$AA125,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T125, $AB125, BD125, $Y125, $W125,$AJ125,$AA125,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T125=\"Select Model\",\"\",IF($T125=\"LIU24_2W\",calcQwIP($Y125,$W125,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC125,$AI125,\"latent\",$U125&\"P\"&IF($V125=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T125,activeElevation),\"\"))","v":""},{"$f":"IF($T125=\"Select Model\",\"\",IF($T125=\"ACBC_1W\",calcQwIP($Y125,$W125,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC125,BD125,\"capacity\",$U125&\"P\"&IF($V125=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T125,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y125,$W125,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC125,BD125,\"capacity\",$U125&\"P\"&IF($V125=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T125,activeElevation)))","v":""},"",{"$f":"IF(T125=\"Select Model\", 0,waterPressureDrop(W125, U125 & \"P\" & IF(V125=\"Dual\",2,1) &\"C\", AC125, \"cooling\", T125))","v":0},{"$f":"IF(T125=\"Select Model\", \"\",getReturnWaterTemp(T125,AC125, activeEWTCooling, AS125, \"cooling\"))","v":""},"",{"$f":"IF($T125<>\"ACBC_1W\",\"\",IF($J125=\"\",\"\",FintubeCapacity($T125,$W125,$AE125,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T125=\"Select Model\",T125=\"PCBL\"),\"\",calcQwIP(Y125,W125,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD125,BD125,\"capacity\",U125&\"P\"&IF(V125=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T125,activeElevation))","v":""},"",{"$f":"IF(OR(T125=\"Select Model\",T125=\"PCBL\"), \"\",IF(AY125=0,\"N/A\",waterPressureDrop(W125, U125 & \"P\" & IF(V125=\"Dual\",2,1) &\"C\", AD125, \"heating\", T125)))","v":""},{"$f":"IF(OR(T125=\"Select Model\",T125=\"PCBL\"), \"\",IF(AY125=0,getReturnWaterTemp(T125,AE125, activeEWTHeating, AX125, \"heating\"),getReturnWaterTemp(T125,AD125, activeEWTHeating, AY125, \"heating\")))","v":""},"",{"$f":" getNozzle(T125, W125, Y125, Z125, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I126)),I126<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I126, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H126)),H126<0),\"\",intlEstQuantity(T126, W126*12, H126)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T126=\"Select Model\",\"\",coilCircuitChange(W126, U126, AC126, T126,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T126=\"Select Model\",\"\",beamWidth(T126))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T126=\"Select Model\",T126=\"PCBL\"), 0,getSPIP(T126, W126, Y126, BD126, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T126=\"Select Model\", \"\",IF(T126=\"PCBL\",0,primaryAirSensibleCapacityIP($T126,$W126,activeRoomTempCooling,activePriAirTempCooling,$Y126,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T126=\"Select Model\",\"\",IF($T126=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y126,activeElevation)))","v":""},{"$f":"IF(OR(T126=\"Select Model\",T126=\"PCBL\"), 0,IF(AD126=0,0,-primaryAirSensibleCapacityIP($T126,$W126,activeRoomTempHeating,activePriAirTempHeating,$Y126,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T126=\"Select Model\", \"\", InductionRatio($T126,BD126,$W126,$Y126)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T126=\"Select Model\", \"\",IF($T126=\"PCBL\",\"N/A\",minVAVSetBack(AA126, Y126))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T126=\"Select Model\", \"\",IF($T126= \"PCBL\",\"N/A\",getDischargeAirTemp($T126,$V126,$AC126,$W126,BD126,$AL126, $Y126, $AS126, \"cooling\",activeElevation,$AB126,$AJ126,$AV126,$BB126))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T126=\"Select Model\",$T126=\"PCBL\"), \"\",getDischargeAirTemp($T126,$V126,$AD126,$W126,BD126,$AL126, $Y126, $AY126, \"heating\",activeElevation,$AB126,$AJ126,$AV126,$BB126)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T126=\"Select Model\", \"\",IF(OR($T126=\"ACBC_1W\",$T126=\"ACBC_2W\",LEFT($T126,4)=\"ACBR\",$T126 = \"LIU24_2W\",LEFT($T126,3)=\"RIU\",LEFT($T126,6)=\"ACBL12\"), IF((soundLevel($T126, $AB126, BD126, $Y126, $W126,$AJ126,$AA126,\"dba\"))<15,\"<15\",soundLevel($T126, $AB126, BD126, $Y126, $W126,$AJ126,$AA126,\"dba\")+0.4),IF((soundLevel($T126, $AB126, BD126, $Y126, $W126,$AJ126,$AA126,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T126, $AB126, BD126, $Y126, $W126,$AJ126,$AA126,\"dba\")+5)<15, \"<15\", soundLevel($T126, $AB126, BD126,$Y126, $W126,$AJ126,$AA126,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T126=\"Select Model\", \"\",IF(OR($T126=\"ACBC_1W\",$T126=\"ACBC_2W\",LEFT($T126,4)=\"ACBR\",$T126=\"LIU24_2W\",LEFT($T126,3)=\"RIU\",LEFT($T126,6)=\"ACBL12\"), IF((soundLevel($T126, $AB126, BD126, $Y126, $W126,$AJ126,$AA126,\"NC\"))<15,\"<15\",soundLevel($T126, $AB126, BD126, $Y126, $W126,$AJ126,$AA126,\"NC\")+0.4),IF((soundLevel($T126, $AB126, BD126, $Y126, $W126,$AJ126,$AA126,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T126, $AB126, BD126, $Y126, $W126,$AJ126,$AA126,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T126, $AB126, BD126, $Y126, $W126,$AJ126,$AA126,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T126=\"Select Model\",\"\",IF($T126=\"LIU24_2W\",calcQwIP($Y126,$W126,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC126,$AI126,\"latent\",$U126&\"P\"&IF($V126=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T126,activeElevation),\"\"))","v":""},{"$f":"IF($T126=\"Select Model\",\"\",IF($T126=\"ACBC_1W\",calcQwIP($Y126,$W126,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC126,BD126,\"capacity\",$U126&\"P\"&IF($V126=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T126,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y126,$W126,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC126,BD126,\"capacity\",$U126&\"P\"&IF($V126=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T126,activeElevation)))","v":""},"",{"$f":"IF(T126=\"Select Model\", 0,waterPressureDrop(W126, U126 & \"P\" & IF(V126=\"Dual\",2,1) &\"C\", AC126, \"cooling\", T126))","v":0},{"$f":"IF(T126=\"Select Model\", \"\",getReturnWaterTemp(T126,AC126, activeEWTCooling, AS126, \"cooling\"))","v":""},"",{"$f":"IF($T126<>\"ACBC_1W\",\"\",IF($J126=\"\",\"\",FintubeCapacity($T126,$W126,$AE126,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T126=\"Select Model\",T126=\"PCBL\"),\"\",calcQwIP(Y126,W126,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD126,BD126,\"capacity\",U126&\"P\"&IF(V126=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T126,activeElevation))","v":""},"",{"$f":"IF(OR(T126=\"Select Model\",T126=\"PCBL\"), \"\",IF(AY126=0,\"N/A\",waterPressureDrop(W126, U126 & \"P\" & IF(V126=\"Dual\",2,1) &\"C\", AD126, \"heating\", T126)))","v":""},{"$f":"IF(OR(T126=\"Select Model\",T126=\"PCBL\"), \"\",IF(AY126=0,getReturnWaterTemp(T126,AE126, activeEWTHeating, AX126, \"heating\"),getReturnWaterTemp(T126,AD126, activeEWTHeating, AY126, \"heating\")))","v":""},"",{"$f":" getNozzle(T126, W126, Y126, Z126, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I127)),I127<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I127, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H127)),H127<0),\"\",intlEstQuantity(T127, W127*12, H127)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T127=\"Select Model\",\"\",coilCircuitChange(W127, U127, AC127, T127,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T127=\"Select Model\",\"\",beamWidth(T127))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T127=\"Select Model\",T127=\"PCBL\"), 0,getSPIP(T127, W127, Y127, BD127, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T127=\"Select Model\", \"\",IF(T127=\"PCBL\",0,primaryAirSensibleCapacityIP($T127,$W127,activeRoomTempCooling,activePriAirTempCooling,$Y127,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T127=\"Select Model\",\"\",IF($T127=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y127,activeElevation)))","v":""},{"$f":"IF(OR(T127=\"Select Model\",T127=\"PCBL\"), 0,IF(AD127=0,0,-primaryAirSensibleCapacityIP($T127,$W127,activeRoomTempHeating,activePriAirTempHeating,$Y127,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T127=\"Select Model\", \"\", InductionRatio($T127,BD127,$W127,$Y127)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T127=\"Select Model\", \"\",IF($T127=\"PCBL\",\"N/A\",minVAVSetBack(AA127, Y127))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T127=\"Select Model\", \"\",IF($T127= \"PCBL\",\"N/A\",getDischargeAirTemp($T127,$V127,$AC127,$W127,BD127,$AL127, $Y127, $AS127, \"cooling\",activeElevation,$AB127,$AJ127,$AV127,$BB127))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T127=\"Select Model\",$T127=\"PCBL\"), \"\",getDischargeAirTemp($T127,$V127,$AD127,$W127,BD127,$AL127, $Y127, $AY127, \"heating\",activeElevation,$AB127,$AJ127,$AV127,$BB127)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T127=\"Select Model\", \"\",IF(OR($T127=\"ACBC_1W\",$T127=\"ACBC_2W\",LEFT($T127,4)=\"ACBR\",$T127 = \"LIU24_2W\",LEFT($T127,3)=\"RIU\",LEFT($T127,6)=\"ACBL12\"), IF((soundLevel($T127, $AB127, BD127, $Y127, $W127,$AJ127,$AA127,\"dba\"))<15,\"<15\",soundLevel($T127, $AB127, BD127, $Y127, $W127,$AJ127,$AA127,\"dba\")+0.4),IF((soundLevel($T127, $AB127, BD127, $Y127, $W127,$AJ127,$AA127,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T127, $AB127, BD127, $Y127, $W127,$AJ127,$AA127,\"dba\")+5)<15, \"<15\", soundLevel($T127, $AB127, BD127,$Y127, $W127,$AJ127,$AA127,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T127=\"Select Model\", \"\",IF(OR($T127=\"ACBC_1W\",$T127=\"ACBC_2W\",LEFT($T127,4)=\"ACBR\",$T127=\"LIU24_2W\",LEFT($T127,3)=\"RIU\",LEFT($T127,6)=\"ACBL12\"), IF((soundLevel($T127, $AB127, BD127, $Y127, $W127,$AJ127,$AA127,\"NC\"))<15,\"<15\",soundLevel($T127, $AB127, BD127, $Y127, $W127,$AJ127,$AA127,\"NC\")+0.4),IF((soundLevel($T127, $AB127, BD127, $Y127, $W127,$AJ127,$AA127,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T127, $AB127, BD127, $Y127, $W127,$AJ127,$AA127,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T127, $AB127, BD127, $Y127, $W127,$AJ127,$AA127,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T127=\"Select Model\",\"\",IF($T127=\"LIU24_2W\",calcQwIP($Y127,$W127,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC127,$AI127,\"latent\",$U127&\"P\"&IF($V127=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T127,activeElevation),\"\"))","v":""},{"$f":"IF($T127=\"Select Model\",\"\",IF($T127=\"ACBC_1W\",calcQwIP($Y127,$W127,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC127,BD127,\"capacity\",$U127&\"P\"&IF($V127=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T127,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y127,$W127,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC127,BD127,\"capacity\",$U127&\"P\"&IF($V127=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T127,activeElevation)))","v":""},"",{"$f":"IF(T127=\"Select Model\", 0,waterPressureDrop(W127, U127 & \"P\" & IF(V127=\"Dual\",2,1) &\"C\", AC127, \"cooling\", T127))","v":0},{"$f":"IF(T127=\"Select Model\", \"\",getReturnWaterTemp(T127,AC127, activeEWTCooling, AS127, \"cooling\"))","v":""},"",{"$f":"IF($T127<>\"ACBC_1W\",\"\",IF($J127=\"\",\"\",FintubeCapacity($T127,$W127,$AE127,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T127=\"Select Model\",T127=\"PCBL\"),\"\",calcQwIP(Y127,W127,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD127,BD127,\"capacity\",U127&\"P\"&IF(V127=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T127,activeElevation))","v":""},"",{"$f":"IF(OR(T127=\"Select Model\",T127=\"PCBL\"), \"\",IF(AY127=0,\"N/A\",waterPressureDrop(W127, U127 & \"P\" & IF(V127=\"Dual\",2,1) &\"C\", AD127, \"heating\", T127)))","v":""},{"$f":"IF(OR(T127=\"Select Model\",T127=\"PCBL\"), \"\",IF(AY127=0,getReturnWaterTemp(T127,AE127, activeEWTHeating, AX127, \"heating\"),getReturnWaterTemp(T127,AD127, activeEWTHeating, AY127, \"heating\")))","v":""},"",{"$f":" getNozzle(T127, W127, Y127, Z127, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I128)),I128<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I128, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H128)),H128<0),\"\",intlEstQuantity(T128, W128*12, H128)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T128=\"Select Model\",\"\",coilCircuitChange(W128, U128, AC128, T128,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T128=\"Select Model\",\"\",beamWidth(T128))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T128=\"Select Model\",T128=\"PCBL\"), 0,getSPIP(T128, W128, Y128, BD128, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T128=\"Select Model\", \"\",IF(T128=\"PCBL\",0,primaryAirSensibleCapacityIP($T128,$W128,activeRoomTempCooling,activePriAirTempCooling,$Y128,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T128=\"Select Model\",\"\",IF($T128=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y128,activeElevation)))","v":""},{"$f":"IF(OR(T128=\"Select Model\",T128=\"PCBL\"), 0,IF(AD128=0,0,-primaryAirSensibleCapacityIP($T128,$W128,activeRoomTempHeating,activePriAirTempHeating,$Y128,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T128=\"Select Model\", \"\", InductionRatio($T128,BD128,$W128,$Y128)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T128=\"Select Model\", \"\",IF($T128=\"PCBL\",\"N/A\",minVAVSetBack(AA128, Y128))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T128=\"Select Model\", \"\",IF($T128= \"PCBL\",\"N/A\",getDischargeAirTemp($T128,$V128,$AC128,$W128,BD128,$AL128, $Y128, $AS128, \"cooling\",activeElevation,$AB128,$AJ128,$AV128,$BB128))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T128=\"Select Model\",$T128=\"PCBL\"), \"\",getDischargeAirTemp($T128,$V128,$AD128,$W128,BD128,$AL128, $Y128, $AY128, \"heating\",activeElevation,$AB128,$AJ128,$AV128,$BB128)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T128=\"Select Model\", \"\",IF(OR($T128=\"ACBC_1W\",$T128=\"ACBC_2W\",LEFT($T128,4)=\"ACBR\",$T128 = \"LIU24_2W\",LEFT($T128,3)=\"RIU\",LEFT($T128,6)=\"ACBL12\"), IF((soundLevel($T128, $AB128, BD128, $Y128, $W128,$AJ128,$AA128,\"dba\"))<15,\"<15\",soundLevel($T128, $AB128, BD128, $Y128, $W128,$AJ128,$AA128,\"dba\")+0.4),IF((soundLevel($T128, $AB128, BD128, $Y128, $W128,$AJ128,$AA128,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T128, $AB128, BD128, $Y128, $W128,$AJ128,$AA128,\"dba\")+5)<15, \"<15\", soundLevel($T128, $AB128, BD128,$Y128, $W128,$AJ128,$AA128,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T128=\"Select Model\", \"\",IF(OR($T128=\"ACBC_1W\",$T128=\"ACBC_2W\",LEFT($T128,4)=\"ACBR\",$T128=\"LIU24_2W\",LEFT($T128,3)=\"RIU\",LEFT($T128,6)=\"ACBL12\"), IF((soundLevel($T128, $AB128, BD128, $Y128, $W128,$AJ128,$AA128,\"NC\"))<15,\"<15\",soundLevel($T128, $AB128, BD128, $Y128, $W128,$AJ128,$AA128,\"NC\")+0.4),IF((soundLevel($T128, $AB128, BD128, $Y128, $W128,$AJ128,$AA128,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T128, $AB128, BD128, $Y128, $W128,$AJ128,$AA128,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T128, $AB128, BD128, $Y128, $W128,$AJ128,$AA128,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T128=\"Select Model\",\"\",IF($T128=\"LIU24_2W\",calcQwIP($Y128,$W128,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC128,$AI128,\"latent\",$U128&\"P\"&IF($V128=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T128,activeElevation),\"\"))","v":""},{"$f":"IF($T128=\"Select Model\",\"\",IF($T128=\"ACBC_1W\",calcQwIP($Y128,$W128,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC128,BD128,\"capacity\",$U128&\"P\"&IF($V128=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T128,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y128,$W128,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC128,BD128,\"capacity\",$U128&\"P\"&IF($V128=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T128,activeElevation)))","v":""},"",{"$f":"IF(T128=\"Select Model\", 0,waterPressureDrop(W128, U128 & \"P\" & IF(V128=\"Dual\",2,1) &\"C\", AC128, \"cooling\", T128))","v":0},{"$f":"IF(T128=\"Select Model\", \"\",getReturnWaterTemp(T128,AC128, activeEWTCooling, AS128, \"cooling\"))","v":""},"",{"$f":"IF($T128<>\"ACBC_1W\",\"\",IF($J128=\"\",\"\",FintubeCapacity($T128,$W128,$AE128,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T128=\"Select Model\",T128=\"PCBL\"),\"\",calcQwIP(Y128,W128,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD128,BD128,\"capacity\",U128&\"P\"&IF(V128=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T128,activeElevation))","v":""},"",{"$f":"IF(OR(T128=\"Select Model\",T128=\"PCBL\"), \"\",IF(AY128=0,\"N/A\",waterPressureDrop(W128, U128 & \"P\" & IF(V128=\"Dual\",2,1) &\"C\", AD128, \"heating\", T128)))","v":""},{"$f":"IF(OR(T128=\"Select Model\",T128=\"PCBL\"), \"\",IF(AY128=0,getReturnWaterTemp(T128,AE128, activeEWTHeating, AX128, \"heating\"),getReturnWaterTemp(T128,AD128, activeEWTHeating, AY128, \"heating\")))","v":""},"",{"$f":" getNozzle(T128, W128, Y128, Z128, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I129)),I129<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I129, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H129)),H129<0),\"\",intlEstQuantity(T129, W129*12, H129)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T129=\"Select Model\",\"\",coilCircuitChange(W129, U129, AC129, T129,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T129=\"Select Model\",\"\",beamWidth(T129))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T129=\"Select Model\",T129=\"PCBL\"), 0,getSPIP(T129, W129, Y129, BD129, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T129=\"Select Model\", \"\",IF(T129=\"PCBL\",0,primaryAirSensibleCapacityIP($T129,$W129,activeRoomTempCooling,activePriAirTempCooling,$Y129,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T129=\"Select Model\",\"\",IF($T129=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y129,activeElevation)))","v":""},{"$f":"IF(OR(T129=\"Select Model\",T129=\"PCBL\"), 0,IF(AD129=0,0,-primaryAirSensibleCapacityIP($T129,$W129,activeRoomTempHeating,activePriAirTempHeating,$Y129,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T129=\"Select Model\", \"\", InductionRatio($T129,BD129,$W129,$Y129)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T129=\"Select Model\", \"\",IF($T129=\"PCBL\",\"N/A\",minVAVSetBack(AA129, Y129))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T129=\"Select Model\", \"\",IF($T129= \"PCBL\",\"N/A\",getDischargeAirTemp($T129,$V129,$AC129,$W129,BD129,$AL129, $Y129, $AS129, \"cooling\",activeElevation,$AB129,$AJ129,$AV129,$BB129))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T129=\"Select Model\",$T129=\"PCBL\"), \"\",getDischargeAirTemp($T129,$V129,$AD129,$W129,BD129,$AL129, $Y129, $AY129, \"heating\",activeElevation,$AB129,$AJ129,$AV129,$BB129)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T129=\"Select Model\", \"\",IF(OR($T129=\"ACBC_1W\",$T129=\"ACBC_2W\",LEFT($T129,4)=\"ACBR\",$T129 = \"LIU24_2W\",LEFT($T129,3)=\"RIU\",LEFT($T129,6)=\"ACBL12\"), IF((soundLevel($T129, $AB129, BD129, $Y129, $W129,$AJ129,$AA129,\"dba\"))<15,\"<15\",soundLevel($T129, $AB129, BD129, $Y129, $W129,$AJ129,$AA129,\"dba\")+0.4),IF((soundLevel($T129, $AB129, BD129, $Y129, $W129,$AJ129,$AA129,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T129, $AB129, BD129, $Y129, $W129,$AJ129,$AA129,\"dba\")+5)<15, \"<15\", soundLevel($T129, $AB129, BD129,$Y129, $W129,$AJ129,$AA129,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T129=\"Select Model\", \"\",IF(OR($T129=\"ACBC_1W\",$T129=\"ACBC_2W\",LEFT($T129,4)=\"ACBR\",$T129=\"LIU24_2W\",LEFT($T129,3)=\"RIU\",LEFT($T129,6)=\"ACBL12\"), IF((soundLevel($T129, $AB129, BD129, $Y129, $W129,$AJ129,$AA129,\"NC\"))<15,\"<15\",soundLevel($T129, $AB129, BD129, $Y129, $W129,$AJ129,$AA129,\"NC\")+0.4),IF((soundLevel($T129, $AB129, BD129, $Y129, $W129,$AJ129,$AA129,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T129, $AB129, BD129, $Y129, $W129,$AJ129,$AA129,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T129, $AB129, BD129, $Y129, $W129,$AJ129,$AA129,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T129=\"Select Model\",\"\",IF($T129=\"LIU24_2W\",calcQwIP($Y129,$W129,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC129,$AI129,\"latent\",$U129&\"P\"&IF($V129=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T129,activeElevation),\"\"))","v":""},{"$f":"IF($T129=\"Select Model\",\"\",IF($T129=\"ACBC_1W\",calcQwIP($Y129,$W129,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC129,BD129,\"capacity\",$U129&\"P\"&IF($V129=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T129,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y129,$W129,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC129,BD129,\"capacity\",$U129&\"P\"&IF($V129=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T129,activeElevation)))","v":""},"",{"$f":"IF(T129=\"Select Model\", 0,waterPressureDrop(W129, U129 & \"P\" & IF(V129=\"Dual\",2,1) &\"C\", AC129, \"cooling\", T129))","v":0},{"$f":"IF(T129=\"Select Model\", \"\",getReturnWaterTemp(T129,AC129, activeEWTCooling, AS129, \"cooling\"))","v":""},"",{"$f":"IF($T129<>\"ACBC_1W\",\"\",IF($J129=\"\",\"\",FintubeCapacity($T129,$W129,$AE129,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T129=\"Select Model\",T129=\"PCBL\"),\"\",calcQwIP(Y129,W129,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD129,BD129,\"capacity\",U129&\"P\"&IF(V129=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T129,activeElevation))","v":""},"",{"$f":"IF(OR(T129=\"Select Model\",T129=\"PCBL\"), \"\",IF(AY129=0,\"N/A\",waterPressureDrop(W129, U129 & \"P\" & IF(V129=\"Dual\",2,1) &\"C\", AD129, \"heating\", T129)))","v":""},{"$f":"IF(OR(T129=\"Select Model\",T129=\"PCBL\"), \"\",IF(AY129=0,getReturnWaterTemp(T129,AE129, activeEWTHeating, AX129, \"heating\"),getReturnWaterTemp(T129,AD129, activeEWTHeating, AY129, \"heating\")))","v":""},"",{"$f":" getNozzle(T129, W129, Y129, Z129, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I130)),I130<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I130, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H130)),H130<0),\"\",intlEstQuantity(T130, W130*12, H130)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T130=\"Select Model\",\"\",coilCircuitChange(W130, U130, AC130, T130,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T130=\"Select Model\",\"\",beamWidth(T130))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T130=\"Select Model\",T130=\"PCBL\"), 0,getSPIP(T130, W130, Y130, BD130, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T130=\"Select Model\", \"\",IF(T130=\"PCBL\",0,primaryAirSensibleCapacityIP($T130,$W130,activeRoomTempCooling,activePriAirTempCooling,$Y130,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T130=\"Select Model\",\"\",IF($T130=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y130,activeElevation)))","v":""},{"$f":"IF(OR(T130=\"Select Model\",T130=\"PCBL\"), 0,IF(AD130=0,0,-primaryAirSensibleCapacityIP($T130,$W130,activeRoomTempHeating,activePriAirTempHeating,$Y130,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T130=\"Select Model\", \"\", InductionRatio($T130,BD130,$W130,$Y130)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T130=\"Select Model\", \"\",IF($T130=\"PCBL\",\"N/A\",minVAVSetBack(AA130, Y130))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T130=\"Select Model\", \"\",IF($T130= \"PCBL\",\"N/A\",getDischargeAirTemp($T130,$V130,$AC130,$W130,BD130,$AL130, $Y130, $AS130, \"cooling\",activeElevation,$AB130,$AJ130,$AV130,$BB130))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T130=\"Select Model\",$T130=\"PCBL\"), \"\",getDischargeAirTemp($T130,$V130,$AD130,$W130,BD130,$AL130, $Y130, $AY130, \"heating\",activeElevation,$AB130,$AJ130,$AV130,$BB130)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T130=\"Select Model\", \"\",IF(OR($T130=\"ACBC_1W\",$T130=\"ACBC_2W\",LEFT($T130,4)=\"ACBR\",$T130 = \"LIU24_2W\",LEFT($T130,3)=\"RIU\",LEFT($T130,6)=\"ACBL12\"), IF((soundLevel($T130, $AB130, BD130, $Y130, $W130,$AJ130,$AA130,\"dba\"))<15,\"<15\",soundLevel($T130, $AB130, BD130, $Y130, $W130,$AJ130,$AA130,\"dba\")+0.4),IF((soundLevel($T130, $AB130, BD130, $Y130, $W130,$AJ130,$AA130,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T130, $AB130, BD130, $Y130, $W130,$AJ130,$AA130,\"dba\")+5)<15, \"<15\", soundLevel($T130, $AB130, BD130,$Y130, $W130,$AJ130,$AA130,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T130=\"Select Model\", \"\",IF(OR($T130=\"ACBC_1W\",$T130=\"ACBC_2W\",LEFT($T130,4)=\"ACBR\",$T130=\"LIU24_2W\",LEFT($T130,3)=\"RIU\",LEFT($T130,6)=\"ACBL12\"), IF((soundLevel($T130, $AB130, BD130, $Y130, $W130,$AJ130,$AA130,\"NC\"))<15,\"<15\",soundLevel($T130, $AB130, BD130, $Y130, $W130,$AJ130,$AA130,\"NC\")+0.4),IF((soundLevel($T130, $AB130, BD130, $Y130, $W130,$AJ130,$AA130,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T130, $AB130, BD130, $Y130, $W130,$AJ130,$AA130,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T130, $AB130, BD130, $Y130, $W130,$AJ130,$AA130,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T130=\"Select Model\",\"\",IF($T130=\"LIU24_2W\",calcQwIP($Y130,$W130,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC130,$AI130,\"latent\",$U130&\"P\"&IF($V130=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T130,activeElevation),\"\"))","v":""},{"$f":"IF($T130=\"Select Model\",\"\",IF($T130=\"ACBC_1W\",calcQwIP($Y130,$W130,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC130,BD130,\"capacity\",$U130&\"P\"&IF($V130=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T130,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y130,$W130,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC130,BD130,\"capacity\",$U130&\"P\"&IF($V130=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T130,activeElevation)))","v":""},"",{"$f":"IF(T130=\"Select Model\", 0,waterPressureDrop(W130, U130 & \"P\" & IF(V130=\"Dual\",2,1) &\"C\", AC130, \"cooling\", T130))","v":0},{"$f":"IF(T130=\"Select Model\", \"\",getReturnWaterTemp(T130,AC130, activeEWTCooling, AS130, \"cooling\"))","v":""},"",{"$f":"IF($T130<>\"ACBC_1W\",\"\",IF($J130=\"\",\"\",FintubeCapacity($T130,$W130,$AE130,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T130=\"Select Model\",T130=\"PCBL\"),\"\",calcQwIP(Y130,W130,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD130,BD130,\"capacity\",U130&\"P\"&IF(V130=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T130,activeElevation))","v":""},"",{"$f":"IF(OR(T130=\"Select Model\",T130=\"PCBL\"), \"\",IF(AY130=0,\"N/A\",waterPressureDrop(W130, U130 & \"P\" & IF(V130=\"Dual\",2,1) &\"C\", AD130, \"heating\", T130)))","v":""},{"$f":"IF(OR(T130=\"Select Model\",T130=\"PCBL\"), \"\",IF(AY130=0,getReturnWaterTemp(T130,AE130, activeEWTHeating, AX130, \"heating\"),getReturnWaterTemp(T130,AD130, activeEWTHeating, AY130, \"heating\")))","v":""},"",{"$f":" getNozzle(T130, W130, Y130, Z130, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I131)),I131<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I131, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H131)),H131<0),\"\",intlEstQuantity(T131, W131*12, H131)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T131=\"Select Model\",\"\",coilCircuitChange(W131, U131, AC131, T131,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T131=\"Select Model\",\"\",beamWidth(T131))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T131=\"Select Model\",T131=\"PCBL\"), 0,getSPIP(T131, W131, Y131, BD131, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T131=\"Select Model\", \"\",IF(T131=\"PCBL\",0,primaryAirSensibleCapacityIP($T131,$W131,activeRoomTempCooling,activePriAirTempCooling,$Y131,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T131=\"Select Model\",\"\",IF($T131=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y131,activeElevation)))","v":""},{"$f":"IF(OR(T131=\"Select Model\",T131=\"PCBL\"), 0,IF(AD131=0,0,-primaryAirSensibleCapacityIP($T131,$W131,activeRoomTempHeating,activePriAirTempHeating,$Y131,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T131=\"Select Model\", \"\", InductionRatio($T131,BD131,$W131,$Y131)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T131=\"Select Model\", \"\",IF($T131=\"PCBL\",\"N/A\",minVAVSetBack(AA131, Y131))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T131=\"Select Model\", \"\",IF($T131= \"PCBL\",\"N/A\",getDischargeAirTemp($T131,$V131,$AC131,$W131,BD131,$AL131, $Y131, $AS131, \"cooling\",activeElevation,$AB131,$AJ131,$AV131,$BB131))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T131=\"Select Model\",$T131=\"PCBL\"), \"\",getDischargeAirTemp($T131,$V131,$AD131,$W131,BD131,$AL131, $Y131, $AY131, \"heating\",activeElevation,$AB131,$AJ131,$AV131,$BB131)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T131=\"Select Model\", \"\",IF(OR($T131=\"ACBC_1W\",$T131=\"ACBC_2W\",LEFT($T131,4)=\"ACBR\",$T131 = \"LIU24_2W\",LEFT($T131,3)=\"RIU\",LEFT($T131,6)=\"ACBL12\"), IF((soundLevel($T131, $AB131, BD131, $Y131, $W131,$AJ131,$AA131,\"dba\"))<15,\"<15\",soundLevel($T131, $AB131, BD131, $Y131, $W131,$AJ131,$AA131,\"dba\")+0.4),IF((soundLevel($T131, $AB131, BD131, $Y131, $W131,$AJ131,$AA131,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T131, $AB131, BD131, $Y131, $W131,$AJ131,$AA131,\"dba\")+5)<15, \"<15\", soundLevel($T131, $AB131, BD131,$Y131, $W131,$AJ131,$AA131,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T131=\"Select Model\", \"\",IF(OR($T131=\"ACBC_1W\",$T131=\"ACBC_2W\",LEFT($T131,4)=\"ACBR\",$T131=\"LIU24_2W\",LEFT($T131,3)=\"RIU\",LEFT($T131,6)=\"ACBL12\"), IF((soundLevel($T131, $AB131, BD131, $Y131, $W131,$AJ131,$AA131,\"NC\"))<15,\"<15\",soundLevel($T131, $AB131, BD131, $Y131, $W131,$AJ131,$AA131,\"NC\")+0.4),IF((soundLevel($T131, $AB131, BD131, $Y131, $W131,$AJ131,$AA131,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T131, $AB131, BD131, $Y131, $W131,$AJ131,$AA131,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T131, $AB131, BD131, $Y131, $W131,$AJ131,$AA131,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T131=\"Select Model\",\"\",IF($T131=\"LIU24_2W\",calcQwIP($Y131,$W131,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC131,$AI131,\"latent\",$U131&\"P\"&IF($V131=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T131,activeElevation),\"\"))","v":""},{"$f":"IF($T131=\"Select Model\",\"\",IF($T131=\"ACBC_1W\",calcQwIP($Y131,$W131,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC131,BD131,\"capacity\",$U131&\"P\"&IF($V131=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T131,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y131,$W131,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC131,BD131,\"capacity\",$U131&\"P\"&IF($V131=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T131,activeElevation)))","v":""},"",{"$f":"IF(T131=\"Select Model\", 0,waterPressureDrop(W131, U131 & \"P\" & IF(V131=\"Dual\",2,1) &\"C\", AC131, \"cooling\", T131))","v":0},{"$f":"IF(T131=\"Select Model\", \"\",getReturnWaterTemp(T131,AC131, activeEWTCooling, AS131, \"cooling\"))","v":""},"",{"$f":"IF($T131<>\"ACBC_1W\",\"\",IF($J131=\"\",\"\",FintubeCapacity($T131,$W131,$AE131,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T131=\"Select Model\",T131=\"PCBL\"),\"\",calcQwIP(Y131,W131,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD131,BD131,\"capacity\",U131&\"P\"&IF(V131=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T131,activeElevation))","v":""},"",{"$f":"IF(OR(T131=\"Select Model\",T131=\"PCBL\"), \"\",IF(AY131=0,\"N/A\",waterPressureDrop(W131, U131 & \"P\" & IF(V131=\"Dual\",2,1) &\"C\", AD131, \"heating\", T131)))","v":""},{"$f":"IF(OR(T131=\"Select Model\",T131=\"PCBL\"), \"\",IF(AY131=0,getReturnWaterTemp(T131,AE131, activeEWTHeating, AX131, \"heating\"),getReturnWaterTemp(T131,AD131, activeEWTHeating, AY131, \"heating\")))","v":""},"",{"$f":" getNozzle(T131, W131, Y131, Z131, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I132)),I132<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I132, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H132)),H132<0),\"\",intlEstQuantity(T132, W132*12, H132)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T132=\"Select Model\",\"\",coilCircuitChange(W132, U132, AC132, T132,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T132=\"Select Model\",\"\",beamWidth(T132))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T132=\"Select Model\",T132=\"PCBL\"), 0,getSPIP(T132, W132, Y132, BD132, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T132=\"Select Model\", \"\",IF(T132=\"PCBL\",0,primaryAirSensibleCapacityIP($T132,$W132,activeRoomTempCooling,activePriAirTempCooling,$Y132,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T132=\"Select Model\",\"\",IF($T132=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y132,activeElevation)))","v":""},{"$f":"IF(OR(T132=\"Select Model\",T132=\"PCBL\"), 0,IF(AD132=0,0,-primaryAirSensibleCapacityIP($T132,$W132,activeRoomTempHeating,activePriAirTempHeating,$Y132,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T132=\"Select Model\", \"\", InductionRatio($T132,BD132,$W132,$Y132)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T132=\"Select Model\", \"\",IF($T132=\"PCBL\",\"N/A\",minVAVSetBack(AA132, Y132))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T132=\"Select Model\", \"\",IF($T132= \"PCBL\",\"N/A\",getDischargeAirTemp($T132,$V132,$AC132,$W132,BD132,$AL132, $Y132, $AS132, \"cooling\",activeElevation,$AB132,$AJ132,$AV132,$BB132))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T132=\"Select Model\",$T132=\"PCBL\"), \"\",getDischargeAirTemp($T132,$V132,$AD132,$W132,BD132,$AL132, $Y132, $AY132, \"heating\",activeElevation,$AB132,$AJ132,$AV132,$BB132)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T132=\"Select Model\", \"\",IF(OR($T132=\"ACBC_1W\",$T132=\"ACBC_2W\",LEFT($T132,4)=\"ACBR\",$T132 = \"LIU24_2W\",LEFT($T132,3)=\"RIU\",LEFT($T132,6)=\"ACBL12\"), IF((soundLevel($T132, $AB132, BD132, $Y132, $W132,$AJ132,$AA132,\"dba\"))<15,\"<15\",soundLevel($T132, $AB132, BD132, $Y132, $W132,$AJ132,$AA132,\"dba\")+0.4),IF((soundLevel($T132, $AB132, BD132, $Y132, $W132,$AJ132,$AA132,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T132, $AB132, BD132, $Y132, $W132,$AJ132,$AA132,\"dba\")+5)<15, \"<15\", soundLevel($T132, $AB132, BD132,$Y132, $W132,$AJ132,$AA132,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T132=\"Select Model\", \"\",IF(OR($T132=\"ACBC_1W\",$T132=\"ACBC_2W\",LEFT($T132,4)=\"ACBR\",$T132=\"LIU24_2W\",LEFT($T132,3)=\"RIU\",LEFT($T132,6)=\"ACBL12\"), IF((soundLevel($T132, $AB132, BD132, $Y132, $W132,$AJ132,$AA132,\"NC\"))<15,\"<15\",soundLevel($T132, $AB132, BD132, $Y132, $W132,$AJ132,$AA132,\"NC\")+0.4),IF((soundLevel($T132, $AB132, BD132, $Y132, $W132,$AJ132,$AA132,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T132, $AB132, BD132, $Y132, $W132,$AJ132,$AA132,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T132, $AB132, BD132, $Y132, $W132,$AJ132,$AA132,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T132=\"Select Model\",\"\",IF($T132=\"LIU24_2W\",calcQwIP($Y132,$W132,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC132,$AI132,\"latent\",$U132&\"P\"&IF($V132=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T132,activeElevation),\"\"))","v":""},{"$f":"IF($T132=\"Select Model\",\"\",IF($T132=\"ACBC_1W\",calcQwIP($Y132,$W132,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC132,BD132,\"capacity\",$U132&\"P\"&IF($V132=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T132,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y132,$W132,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC132,BD132,\"capacity\",$U132&\"P\"&IF($V132=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T132,activeElevation)))","v":""},"",{"$f":"IF(T132=\"Select Model\", 0,waterPressureDrop(W132, U132 & \"P\" & IF(V132=\"Dual\",2,1) &\"C\", AC132, \"cooling\", T132))","v":0},{"$f":"IF(T132=\"Select Model\", \"\",getReturnWaterTemp(T132,AC132, activeEWTCooling, AS132, \"cooling\"))","v":""},"",{"$f":"IF($T132<>\"ACBC_1W\",\"\",IF($J132=\"\",\"\",FintubeCapacity($T132,$W132,$AE132,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T132=\"Select Model\",T132=\"PCBL\"),\"\",calcQwIP(Y132,W132,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD132,BD132,\"capacity\",U132&\"P\"&IF(V132=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T132,activeElevation))","v":""},"",{"$f":"IF(OR(T132=\"Select Model\",T132=\"PCBL\"), \"\",IF(AY132=0,\"N/A\",waterPressureDrop(W132, U132 & \"P\" & IF(V132=\"Dual\",2,1) &\"C\", AD132, \"heating\", T132)))","v":""},{"$f":"IF(OR(T132=\"Select Model\",T132=\"PCBL\"), \"\",IF(AY132=0,getReturnWaterTemp(T132,AE132, activeEWTHeating, AX132, \"heating\"),getReturnWaterTemp(T132,AD132, activeEWTHeating, AY132, \"heating\")))","v":""},"",{"$f":" getNozzle(T132, W132, Y132, Z132, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I133)),I133<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I133, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H133)),H133<0),\"\",intlEstQuantity(T133, W133*12, H133)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T133=\"Select Model\",\"\",coilCircuitChange(W133, U133, AC133, T133,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T133=\"Select Model\",\"\",beamWidth(T133))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T133=\"Select Model\",T133=\"PCBL\"), 0,getSPIP(T133, W133, Y133, BD133, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T133=\"Select Model\", \"\",IF(T133=\"PCBL\",0,primaryAirSensibleCapacityIP($T133,$W133,activeRoomTempCooling,activePriAirTempCooling,$Y133,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T133=\"Select Model\",\"\",IF($T133=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y133,activeElevation)))","v":""},{"$f":"IF(OR(T133=\"Select Model\",T133=\"PCBL\"), 0,IF(AD133=0,0,-primaryAirSensibleCapacityIP($T133,$W133,activeRoomTempHeating,activePriAirTempHeating,$Y133,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T133=\"Select Model\", \"\", InductionRatio($T133,BD133,$W133,$Y133)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T133=\"Select Model\", \"\",IF($T133=\"PCBL\",\"N/A\",minVAVSetBack(AA133, Y133))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T133=\"Select Model\", \"\",IF($T133= \"PCBL\",\"N/A\",getDischargeAirTemp($T133,$V133,$AC133,$W133,BD133,$AL133, $Y133, $AS133, \"cooling\",activeElevation,$AB133,$AJ133,$AV133,$BB133))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T133=\"Select Model\",$T133=\"PCBL\"), \"\",getDischargeAirTemp($T133,$V133,$AD133,$W133,BD133,$AL133, $Y133, $AY133, \"heating\",activeElevation,$AB133,$AJ133,$AV133,$BB133)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T133=\"Select Model\", \"\",IF(OR($T133=\"ACBC_1W\",$T133=\"ACBC_2W\",LEFT($T133,4)=\"ACBR\",$T133 = \"LIU24_2W\",LEFT($T133,3)=\"RIU\",LEFT($T133,6)=\"ACBL12\"), IF((soundLevel($T133, $AB133, BD133, $Y133, $W133,$AJ133,$AA133,\"dba\"))<15,\"<15\",soundLevel($T133, $AB133, BD133, $Y133, $W133,$AJ133,$AA133,\"dba\")+0.4),IF((soundLevel($T133, $AB133, BD133, $Y133, $W133,$AJ133,$AA133,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T133, $AB133, BD133, $Y133, $W133,$AJ133,$AA133,\"dba\")+5)<15, \"<15\", soundLevel($T133, $AB133, BD133,$Y133, $W133,$AJ133,$AA133,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T133=\"Select Model\", \"\",IF(OR($T133=\"ACBC_1W\",$T133=\"ACBC_2W\",LEFT($T133,4)=\"ACBR\",$T133=\"LIU24_2W\",LEFT($T133,3)=\"RIU\",LEFT($T133,6)=\"ACBL12\"), IF((soundLevel($T133, $AB133, BD133, $Y133, $W133,$AJ133,$AA133,\"NC\"))<15,\"<15\",soundLevel($T133, $AB133, BD133, $Y133, $W133,$AJ133,$AA133,\"NC\")+0.4),IF((soundLevel($T133, $AB133, BD133, $Y133, $W133,$AJ133,$AA133,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T133, $AB133, BD133, $Y133, $W133,$AJ133,$AA133,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T133, $AB133, BD133, $Y133, $W133,$AJ133,$AA133,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T133=\"Select Model\",\"\",IF($T133=\"LIU24_2W\",calcQwIP($Y133,$W133,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC133,$AI133,\"latent\",$U133&\"P\"&IF($V133=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T133,activeElevation),\"\"))","v":""},{"$f":"IF($T133=\"Select Model\",\"\",IF($T133=\"ACBC_1W\",calcQwIP($Y133,$W133,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC133,BD133,\"capacity\",$U133&\"P\"&IF($V133=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T133,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y133,$W133,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC133,BD133,\"capacity\",$U133&\"P\"&IF($V133=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T133,activeElevation)))","v":""},"",{"$f":"IF(T133=\"Select Model\", 0,waterPressureDrop(W133, U133 & \"P\" & IF(V133=\"Dual\",2,1) &\"C\", AC133, \"cooling\", T133))","v":0},{"$f":"IF(T133=\"Select Model\", \"\",getReturnWaterTemp(T133,AC133, activeEWTCooling, AS133, \"cooling\"))","v":""},"",{"$f":"IF($T133<>\"ACBC_1W\",\"\",IF($J133=\"\",\"\",FintubeCapacity($T133,$W133,$AE133,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T133=\"Select Model\",T133=\"PCBL\"),\"\",calcQwIP(Y133,W133,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD133,BD133,\"capacity\",U133&\"P\"&IF(V133=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T133,activeElevation))","v":""},"",{"$f":"IF(OR(T133=\"Select Model\",T133=\"PCBL\"), \"\",IF(AY133=0,\"N/A\",waterPressureDrop(W133, U133 & \"P\" & IF(V133=\"Dual\",2,1) &\"C\", AD133, \"heating\", T133)))","v":""},{"$f":"IF(OR(T133=\"Select Model\",T133=\"PCBL\"), \"\",IF(AY133=0,getReturnWaterTemp(T133,AE133, activeEWTHeating, AX133, \"heating\"),getReturnWaterTemp(T133,AD133, activeEWTHeating, AY133, \"heating\")))","v":""},"",{"$f":" getNozzle(T133, W133, Y133, Z133, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I134)),I134<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I134, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H134)),H134<0),\"\",intlEstQuantity(T134, W134*12, H134)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T134=\"Select Model\",\"\",coilCircuitChange(W134, U134, AC134, T134,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T134=\"Select Model\",\"\",beamWidth(T134))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T134=\"Select Model\",T134=\"PCBL\"), 0,getSPIP(T134, W134, Y134, BD134, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T134=\"Select Model\", \"\",IF(T134=\"PCBL\",0,primaryAirSensibleCapacityIP($T134,$W134,activeRoomTempCooling,activePriAirTempCooling,$Y134,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T134=\"Select Model\",\"\",IF($T134=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y134,activeElevation)))","v":""},{"$f":"IF(OR(T134=\"Select Model\",T134=\"PCBL\"), 0,IF(AD134=0,0,-primaryAirSensibleCapacityIP($T134,$W134,activeRoomTempHeating,activePriAirTempHeating,$Y134,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T134=\"Select Model\", \"\", InductionRatio($T134,BD134,$W134,$Y134)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T134=\"Select Model\", \"\",IF($T134=\"PCBL\",\"N/A\",minVAVSetBack(AA134, Y134))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T134=\"Select Model\", \"\",IF($T134= \"PCBL\",\"N/A\",getDischargeAirTemp($T134,$V134,$AC134,$W134,BD134,$AL134, $Y134, $AS134, \"cooling\",activeElevation,$AB134,$AJ134,$AV134,$BB134))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T134=\"Select Model\",$T134=\"PCBL\"), \"\",getDischargeAirTemp($T134,$V134,$AD134,$W134,BD134,$AL134, $Y134, $AY134, \"heating\",activeElevation,$AB134,$AJ134,$AV134,$BB134)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T134=\"Select Model\", \"\",IF(OR($T134=\"ACBC_1W\",$T134=\"ACBC_2W\",LEFT($T134,4)=\"ACBR\",$T134 = \"LIU24_2W\",LEFT($T134,3)=\"RIU\",LEFT($T134,6)=\"ACBL12\"), IF((soundLevel($T134, $AB134, BD134, $Y134, $W134,$AJ134,$AA134,\"dba\"))<15,\"<15\",soundLevel($T134, $AB134, BD134, $Y134, $W134,$AJ134,$AA134,\"dba\")+0.4),IF((soundLevel($T134, $AB134, BD134, $Y134, $W134,$AJ134,$AA134,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T134, $AB134, BD134, $Y134, $W134,$AJ134,$AA134,\"dba\")+5)<15, \"<15\", soundLevel($T134, $AB134, BD134,$Y134, $W134,$AJ134,$AA134,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T134=\"Select Model\", \"\",IF(OR($T134=\"ACBC_1W\",$T134=\"ACBC_2W\",LEFT($T134,4)=\"ACBR\",$T134=\"LIU24_2W\",LEFT($T134,3)=\"RIU\",LEFT($T134,6)=\"ACBL12\"), IF((soundLevel($T134, $AB134, BD134, $Y134, $W134,$AJ134,$AA134,\"NC\"))<15,\"<15\",soundLevel($T134, $AB134, BD134, $Y134, $W134,$AJ134,$AA134,\"NC\")+0.4),IF((soundLevel($T134, $AB134, BD134, $Y134, $W134,$AJ134,$AA134,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T134, $AB134, BD134, $Y134, $W134,$AJ134,$AA134,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T134, $AB134, BD134, $Y134, $W134,$AJ134,$AA134,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T134=\"Select Model\",\"\",IF($T134=\"LIU24_2W\",calcQwIP($Y134,$W134,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC134,$AI134,\"latent\",$U134&\"P\"&IF($V134=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T134,activeElevation),\"\"))","v":""},{"$f":"IF($T134=\"Select Model\",\"\",IF($T134=\"ACBC_1W\",calcQwIP($Y134,$W134,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC134,BD134,\"capacity\",$U134&\"P\"&IF($V134=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T134,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y134,$W134,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC134,BD134,\"capacity\",$U134&\"P\"&IF($V134=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T134,activeElevation)))","v":""},"",{"$f":"IF(T134=\"Select Model\", 0,waterPressureDrop(W134, U134 & \"P\" & IF(V134=\"Dual\",2,1) &\"C\", AC134, \"cooling\", T134))","v":0},{"$f":"IF(T134=\"Select Model\", \"\",getReturnWaterTemp(T134,AC134, activeEWTCooling, AS134, \"cooling\"))","v":""},"",{"$f":"IF($T134<>\"ACBC_1W\",\"\",IF($J134=\"\",\"\",FintubeCapacity($T134,$W134,$AE134,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T134=\"Select Model\",T134=\"PCBL\"),\"\",calcQwIP(Y134,W134,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD134,BD134,\"capacity\",U134&\"P\"&IF(V134=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T134,activeElevation))","v":""},"",{"$f":"IF(OR(T134=\"Select Model\",T134=\"PCBL\"), \"\",IF(AY134=0,\"N/A\",waterPressureDrop(W134, U134 & \"P\" & IF(V134=\"Dual\",2,1) &\"C\", AD134, \"heating\", T134)))","v":""},{"$f":"IF(OR(T134=\"Select Model\",T134=\"PCBL\"), \"\",IF(AY134=0,getReturnWaterTemp(T134,AE134, activeEWTHeating, AX134, \"heating\"),getReturnWaterTemp(T134,AD134, activeEWTHeating, AY134, \"heating\")))","v":""},"",{"$f":" getNozzle(T134, W134, Y134, Z134, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I135)),I135<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I135, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H135)),H135<0),\"\",intlEstQuantity(T135, W135*12, H135)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T135=\"Select Model\",\"\",coilCircuitChange(W135, U135, AC135, T135,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T135=\"Select Model\",\"\",beamWidth(T135))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T135=\"Select Model\",T135=\"PCBL\"), 0,getSPIP(T135, W135, Y135, BD135, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T135=\"Select Model\", \"\",IF(T135=\"PCBL\",0,primaryAirSensibleCapacityIP($T135,$W135,activeRoomTempCooling,activePriAirTempCooling,$Y135,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T135=\"Select Model\",\"\",IF($T135=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y135,activeElevation)))","v":""},{"$f":"IF(OR(T135=\"Select Model\",T135=\"PCBL\"), 0,IF(AD135=0,0,-primaryAirSensibleCapacityIP($T135,$W135,activeRoomTempHeating,activePriAirTempHeating,$Y135,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T135=\"Select Model\", \"\", InductionRatio($T135,BD135,$W135,$Y135)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T135=\"Select Model\", \"\",IF($T135=\"PCBL\",\"N/A\",minVAVSetBack(AA135, Y135))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T135=\"Select Model\", \"\",IF($T135= \"PCBL\",\"N/A\",getDischargeAirTemp($T135,$V135,$AC135,$W135,BD135,$AL135, $Y135, $AS135, \"cooling\",activeElevation,$AB135,$AJ135,$AV135,$BB135))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T135=\"Select Model\",$T135=\"PCBL\"), \"\",getDischargeAirTemp($T135,$V135,$AD135,$W135,BD135,$AL135, $Y135, $AY135, \"heating\",activeElevation,$AB135,$AJ135,$AV135,$BB135)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T135=\"Select Model\", \"\",IF(OR($T135=\"ACBC_1W\",$T135=\"ACBC_2W\",LEFT($T135,4)=\"ACBR\",$T135 = \"LIU24_2W\",LEFT($T135,3)=\"RIU\",LEFT($T135,6)=\"ACBL12\"), IF((soundLevel($T135, $AB135, BD135, $Y135, $W135,$AJ135,$AA135,\"dba\"))<15,\"<15\",soundLevel($T135, $AB135, BD135, $Y135, $W135,$AJ135,$AA135,\"dba\")+0.4),IF((soundLevel($T135, $AB135, BD135, $Y135, $W135,$AJ135,$AA135,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T135, $AB135, BD135, $Y135, $W135,$AJ135,$AA135,\"dba\")+5)<15, \"<15\", soundLevel($T135, $AB135, BD135,$Y135, $W135,$AJ135,$AA135,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T135=\"Select Model\", \"\",IF(OR($T135=\"ACBC_1W\",$T135=\"ACBC_2W\",LEFT($T135,4)=\"ACBR\",$T135=\"LIU24_2W\",LEFT($T135,3)=\"RIU\",LEFT($T135,6)=\"ACBL12\"), IF((soundLevel($T135, $AB135, BD135, $Y135, $W135,$AJ135,$AA135,\"NC\"))<15,\"<15\",soundLevel($T135, $AB135, BD135, $Y135, $W135,$AJ135,$AA135,\"NC\")+0.4),IF((soundLevel($T135, $AB135, BD135, $Y135, $W135,$AJ135,$AA135,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T135, $AB135, BD135, $Y135, $W135,$AJ135,$AA135,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T135, $AB135, BD135, $Y135, $W135,$AJ135,$AA135,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T135=\"Select Model\",\"\",IF($T135=\"LIU24_2W\",calcQwIP($Y135,$W135,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC135,$AI135,\"latent\",$U135&\"P\"&IF($V135=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T135,activeElevation),\"\"))","v":""},{"$f":"IF($T135=\"Select Model\",\"\",IF($T135=\"ACBC_1W\",calcQwIP($Y135,$W135,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC135,BD135,\"capacity\",$U135&\"P\"&IF($V135=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T135,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y135,$W135,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC135,BD135,\"capacity\",$U135&\"P\"&IF($V135=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T135,activeElevation)))","v":""},"",{"$f":"IF(T135=\"Select Model\", 0,waterPressureDrop(W135, U135 & \"P\" & IF(V135=\"Dual\",2,1) &\"C\", AC135, \"cooling\", T135))","v":0},{"$f":"IF(T135=\"Select Model\", \"\",getReturnWaterTemp(T135,AC135, activeEWTCooling, AS135, \"cooling\"))","v":""},"",{"$f":"IF($T135<>\"ACBC_1W\",\"\",IF($J135=\"\",\"\",FintubeCapacity($T135,$W135,$AE135,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T135=\"Select Model\",T135=\"PCBL\"),\"\",calcQwIP(Y135,W135,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD135,BD135,\"capacity\",U135&\"P\"&IF(V135=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T135,activeElevation))","v":""},"",{"$f":"IF(OR(T135=\"Select Model\",T135=\"PCBL\"), \"\",IF(AY135=0,\"N/A\",waterPressureDrop(W135, U135 & \"P\" & IF(V135=\"Dual\",2,1) &\"C\", AD135, \"heating\", T135)))","v":""},{"$f":"IF(OR(T135=\"Select Model\",T135=\"PCBL\"), \"\",IF(AY135=0,getReturnWaterTemp(T135,AE135, activeEWTHeating, AX135, \"heating\"),getReturnWaterTemp(T135,AD135, activeEWTHeating, AY135, \"heating\")))","v":""},"",{"$f":" getNozzle(T135, W135, Y135, Z135, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I136)),I136<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I136, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H136)),H136<0),\"\",intlEstQuantity(T136, W136*12, H136)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T136=\"Select Model\",\"\",coilCircuitChange(W136, U136, AC136, T136,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T136=\"Select Model\",\"\",beamWidth(T136))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T136=\"Select Model\",T136=\"PCBL\"), 0,getSPIP(T136, W136, Y136, BD136, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T136=\"Select Model\", \"\",IF(T136=\"PCBL\",0,primaryAirSensibleCapacityIP($T136,$W136,activeRoomTempCooling,activePriAirTempCooling,$Y136,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T136=\"Select Model\",\"\",IF($T136=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y136,activeElevation)))","v":""},{"$f":"IF(OR(T136=\"Select Model\",T136=\"PCBL\"), 0,IF(AD136=0,0,-primaryAirSensibleCapacityIP($T136,$W136,activeRoomTempHeating,activePriAirTempHeating,$Y136,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T136=\"Select Model\", \"\", InductionRatio($T136,BD136,$W136,$Y136)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T136=\"Select Model\", \"\",IF($T136=\"PCBL\",\"N/A\",minVAVSetBack(AA136, Y136))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T136=\"Select Model\", \"\",IF($T136= \"PCBL\",\"N/A\",getDischargeAirTemp($T136,$V136,$AC136,$W136,BD136,$AL136, $Y136, $AS136, \"cooling\",activeElevation,$AB136,$AJ136,$AV136,$BB136))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T136=\"Select Model\",$T136=\"PCBL\"), \"\",getDischargeAirTemp($T136,$V136,$AD136,$W136,BD136,$AL136, $Y136, $AY136, \"heating\",activeElevation,$AB136,$AJ136,$AV136,$BB136)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T136=\"Select Model\", \"\",IF(OR($T136=\"ACBC_1W\",$T136=\"ACBC_2W\",LEFT($T136,4)=\"ACBR\",$T136 = \"LIU24_2W\",LEFT($T136,3)=\"RIU\",LEFT($T136,6)=\"ACBL12\"), IF((soundLevel($T136, $AB136, BD136, $Y136, $W136,$AJ136,$AA136,\"dba\"))<15,\"<15\",soundLevel($T136, $AB136, BD136, $Y136, $W136,$AJ136,$AA136,\"dba\")+0.4),IF((soundLevel($T136, $AB136, BD136, $Y136, $W136,$AJ136,$AA136,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T136, $AB136, BD136, $Y136, $W136,$AJ136,$AA136,\"dba\")+5)<15, \"<15\", soundLevel($T136, $AB136, BD136,$Y136, $W136,$AJ136,$AA136,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T136=\"Select Model\", \"\",IF(OR($T136=\"ACBC_1W\",$T136=\"ACBC_2W\",LEFT($T136,4)=\"ACBR\",$T136=\"LIU24_2W\",LEFT($T136,3)=\"RIU\",LEFT($T136,6)=\"ACBL12\"), IF((soundLevel($T136, $AB136, BD136, $Y136, $W136,$AJ136,$AA136,\"NC\"))<15,\"<15\",soundLevel($T136, $AB136, BD136, $Y136, $W136,$AJ136,$AA136,\"NC\")+0.4),IF((soundLevel($T136, $AB136, BD136, $Y136, $W136,$AJ136,$AA136,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T136, $AB136, BD136, $Y136, $W136,$AJ136,$AA136,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T136, $AB136, BD136, $Y136, $W136,$AJ136,$AA136,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T136=\"Select Model\",\"\",IF($T136=\"LIU24_2W\",calcQwIP($Y136,$W136,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC136,$AI136,\"latent\",$U136&\"P\"&IF($V136=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T136,activeElevation),\"\"))","v":""},{"$f":"IF($T136=\"Select Model\",\"\",IF($T136=\"ACBC_1W\",calcQwIP($Y136,$W136,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC136,BD136,\"capacity\",$U136&\"P\"&IF($V136=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T136,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y136,$W136,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC136,BD136,\"capacity\",$U136&\"P\"&IF($V136=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T136,activeElevation)))","v":""},"",{"$f":"IF(T136=\"Select Model\", 0,waterPressureDrop(W136, U136 & \"P\" & IF(V136=\"Dual\",2,1) &\"C\", AC136, \"cooling\", T136))","v":0},{"$f":"IF(T136=\"Select Model\", \"\",getReturnWaterTemp(T136,AC136, activeEWTCooling, AS136, \"cooling\"))","v":""},"",{"$f":"IF($T136<>\"ACBC_1W\",\"\",IF($J136=\"\",\"\",FintubeCapacity($T136,$W136,$AE136,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T136=\"Select Model\",T136=\"PCBL\"),\"\",calcQwIP(Y136,W136,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD136,BD136,\"capacity\",U136&\"P\"&IF(V136=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T136,activeElevation))","v":""},"",{"$f":"IF(OR(T136=\"Select Model\",T136=\"PCBL\"), \"\",IF(AY136=0,\"N/A\",waterPressureDrop(W136, U136 & \"P\" & IF(V136=\"Dual\",2,1) &\"C\", AD136, \"heating\", T136)))","v":""},{"$f":"IF(OR(T136=\"Select Model\",T136=\"PCBL\"), \"\",IF(AY136=0,getReturnWaterTemp(T136,AE136, activeEWTHeating, AX136, \"heating\"),getReturnWaterTemp(T136,AD136, activeEWTHeating, AY136, \"heating\")))","v":""},"",{"$f":" getNozzle(T136, W136, Y136, Z136, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I137)),I137<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I137, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H137)),H137<0),\"\",intlEstQuantity(T137, W137*12, H137)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T137=\"Select Model\",\"\",coilCircuitChange(W137, U137, AC137, T137,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T137=\"Select Model\",\"\",beamWidth(T137))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T137=\"Select Model\",T137=\"PCBL\"), 0,getSPIP(T137, W137, Y137, BD137, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T137=\"Select Model\", \"\",IF(T137=\"PCBL\",0,primaryAirSensibleCapacityIP($T137,$W137,activeRoomTempCooling,activePriAirTempCooling,$Y137,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T137=\"Select Model\",\"\",IF($T137=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y137,activeElevation)))","v":""},{"$f":"IF(OR(T137=\"Select Model\",T137=\"PCBL\"), 0,IF(AD137=0,0,-primaryAirSensibleCapacityIP($T137,$W137,activeRoomTempHeating,activePriAirTempHeating,$Y137,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T137=\"Select Model\", \"\", InductionRatio($T137,BD137,$W137,$Y137)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T137=\"Select Model\", \"\",IF($T137=\"PCBL\",\"N/A\",minVAVSetBack(AA137, Y137))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T137=\"Select Model\", \"\",IF($T137= \"PCBL\",\"N/A\",getDischargeAirTemp($T137,$V137,$AC137,$W137,BD137,$AL137, $Y137, $AS137, \"cooling\",activeElevation,$AB137,$AJ137,$AV137,$BB137))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T137=\"Select Model\",$T137=\"PCBL\"), \"\",getDischargeAirTemp($T137,$V137,$AD137,$W137,BD137,$AL137, $Y137, $AY137, \"heating\",activeElevation,$AB137,$AJ137,$AV137,$BB137)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T137=\"Select Model\", \"\",IF(OR($T137=\"ACBC_1W\",$T137=\"ACBC_2W\",LEFT($T137,4)=\"ACBR\",$T137 = \"LIU24_2W\",LEFT($T137,3)=\"RIU\",LEFT($T137,6)=\"ACBL12\"), IF((soundLevel($T137, $AB137, BD137, $Y137, $W137,$AJ137,$AA137,\"dba\"))<15,\"<15\",soundLevel($T137, $AB137, BD137, $Y137, $W137,$AJ137,$AA137,\"dba\")+0.4),IF((soundLevel($T137, $AB137, BD137, $Y137, $W137,$AJ137,$AA137,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T137, $AB137, BD137, $Y137, $W137,$AJ137,$AA137,\"dba\")+5)<15, \"<15\", soundLevel($T137, $AB137, BD137,$Y137, $W137,$AJ137,$AA137,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T137=\"Select Model\", \"\",IF(OR($T137=\"ACBC_1W\",$T137=\"ACBC_2W\",LEFT($T137,4)=\"ACBR\",$T137=\"LIU24_2W\",LEFT($T137,3)=\"RIU\",LEFT($T137,6)=\"ACBL12\"), IF((soundLevel($T137, $AB137, BD137, $Y137, $W137,$AJ137,$AA137,\"NC\"))<15,\"<15\",soundLevel($T137, $AB137, BD137, $Y137, $W137,$AJ137,$AA137,\"NC\")+0.4),IF((soundLevel($T137, $AB137, BD137, $Y137, $W137,$AJ137,$AA137,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T137, $AB137, BD137, $Y137, $W137,$AJ137,$AA137,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T137, $AB137, BD137, $Y137, $W137,$AJ137,$AA137,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T137=\"Select Model\",\"\",IF($T137=\"LIU24_2W\",calcQwIP($Y137,$W137,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC137,$AI137,\"latent\",$U137&\"P\"&IF($V137=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T137,activeElevation),\"\"))","v":""},{"$f":"IF($T137=\"Select Model\",\"\",IF($T137=\"ACBC_1W\",calcQwIP($Y137,$W137,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC137,BD137,\"capacity\",$U137&\"P\"&IF($V137=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T137,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y137,$W137,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC137,BD137,\"capacity\",$U137&\"P\"&IF($V137=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T137,activeElevation)))","v":""},"",{"$f":"IF(T137=\"Select Model\", 0,waterPressureDrop(W137, U137 & \"P\" & IF(V137=\"Dual\",2,1) &\"C\", AC137, \"cooling\", T137))","v":0},{"$f":"IF(T137=\"Select Model\", \"\",getReturnWaterTemp(T137,AC137, activeEWTCooling, AS137, \"cooling\"))","v":""},"",{"$f":"IF($T137<>\"ACBC_1W\",\"\",IF($J137=\"\",\"\",FintubeCapacity($T137,$W137,$AE137,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T137=\"Select Model\",T137=\"PCBL\"),\"\",calcQwIP(Y137,W137,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD137,BD137,\"capacity\",U137&\"P\"&IF(V137=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T137,activeElevation))","v":""},"",{"$f":"IF(OR(T137=\"Select Model\",T137=\"PCBL\"), \"\",IF(AY137=0,\"N/A\",waterPressureDrop(W137, U137 & \"P\" & IF(V137=\"Dual\",2,1) &\"C\", AD137, \"heating\", T137)))","v":""},{"$f":"IF(OR(T137=\"Select Model\",T137=\"PCBL\"), \"\",IF(AY137=0,getReturnWaterTemp(T137,AE137, activeEWTHeating, AX137, \"heating\"),getReturnWaterTemp(T137,AD137, activeEWTHeating, AY137, \"heating\")))","v":""},"",{"$f":" getNozzle(T137, W137, Y137, Z137, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I138)),I138<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I138, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H138)),H138<0),\"\",intlEstQuantity(T138, W138*12, H138)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T138=\"Select Model\",\"\",coilCircuitChange(W138, U138, AC138, T138,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T138=\"Select Model\",\"\",beamWidth(T138))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T138=\"Select Model\",T138=\"PCBL\"), 0,getSPIP(T138, W138, Y138, BD138, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T138=\"Select Model\", \"\",IF(T138=\"PCBL\",0,primaryAirSensibleCapacityIP($T138,$W138,activeRoomTempCooling,activePriAirTempCooling,$Y138,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T138=\"Select Model\",\"\",IF($T138=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y138,activeElevation)))","v":""},{"$f":"IF(OR(T138=\"Select Model\",T138=\"PCBL\"), 0,IF(AD138=0,0,-primaryAirSensibleCapacityIP($T138,$W138,activeRoomTempHeating,activePriAirTempHeating,$Y138,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T138=\"Select Model\", \"\", InductionRatio($T138,BD138,$W138,$Y138)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T138=\"Select Model\", \"\",IF($T138=\"PCBL\",\"N/A\",minVAVSetBack(AA138, Y138))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T138=\"Select Model\", \"\",IF($T138= \"PCBL\",\"N/A\",getDischargeAirTemp($T138,$V138,$AC138,$W138,BD138,$AL138, $Y138, $AS138, \"cooling\",activeElevation,$AB138,$AJ138,$AV138,$BB138))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T138=\"Select Model\",$T138=\"PCBL\"), \"\",getDischargeAirTemp($T138,$V138,$AD138,$W138,BD138,$AL138, $Y138, $AY138, \"heating\",activeElevation,$AB138,$AJ138,$AV138,$BB138)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T138=\"Select Model\", \"\",IF(OR($T138=\"ACBC_1W\",$T138=\"ACBC_2W\",LEFT($T138,4)=\"ACBR\",$T138 = \"LIU24_2W\",LEFT($T138,3)=\"RIU\",LEFT($T138,6)=\"ACBL12\"), IF((soundLevel($T138, $AB138, BD138, $Y138, $W138,$AJ138,$AA138,\"dba\"))<15,\"<15\",soundLevel($T138, $AB138, BD138, $Y138, $W138,$AJ138,$AA138,\"dba\")+0.4),IF((soundLevel($T138, $AB138, BD138, $Y138, $W138,$AJ138,$AA138,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T138, $AB138, BD138, $Y138, $W138,$AJ138,$AA138,\"dba\")+5)<15, \"<15\", soundLevel($T138, $AB138, BD138,$Y138, $W138,$AJ138,$AA138,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T138=\"Select Model\", \"\",IF(OR($T138=\"ACBC_1W\",$T138=\"ACBC_2W\",LEFT($T138,4)=\"ACBR\",$T138=\"LIU24_2W\",LEFT($T138,3)=\"RIU\",LEFT($T138,6)=\"ACBL12\"), IF((soundLevel($T138, $AB138, BD138, $Y138, $W138,$AJ138,$AA138,\"NC\"))<15,\"<15\",soundLevel($T138, $AB138, BD138, $Y138, $W138,$AJ138,$AA138,\"NC\")+0.4),IF((soundLevel($T138, $AB138, BD138, $Y138, $W138,$AJ138,$AA138,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T138, $AB138, BD138, $Y138, $W138,$AJ138,$AA138,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T138, $AB138, BD138, $Y138, $W138,$AJ138,$AA138,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T138=\"Select Model\",\"\",IF($T138=\"LIU24_2W\",calcQwIP($Y138,$W138,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC138,$AI138,\"latent\",$U138&\"P\"&IF($V138=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T138,activeElevation),\"\"))","v":""},{"$f":"IF($T138=\"Select Model\",\"\",IF($T138=\"ACBC_1W\",calcQwIP($Y138,$W138,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC138,BD138,\"capacity\",$U138&\"P\"&IF($V138=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T138,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y138,$W138,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC138,BD138,\"capacity\",$U138&\"P\"&IF($V138=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T138,activeElevation)))","v":""},"",{"$f":"IF(T138=\"Select Model\", 0,waterPressureDrop(W138, U138 & \"P\" & IF(V138=\"Dual\",2,1) &\"C\", AC138, \"cooling\", T138))","v":0},{"$f":"IF(T138=\"Select Model\", \"\",getReturnWaterTemp(T138,AC138, activeEWTCooling, AS138, \"cooling\"))","v":""},"",{"$f":"IF($T138<>\"ACBC_1W\",\"\",IF($J138=\"\",\"\",FintubeCapacity($T138,$W138,$AE138,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T138=\"Select Model\",T138=\"PCBL\"),\"\",calcQwIP(Y138,W138,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD138,BD138,\"capacity\",U138&\"P\"&IF(V138=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T138,activeElevation))","v":""},"",{"$f":"IF(OR(T138=\"Select Model\",T138=\"PCBL\"), \"\",IF(AY138=0,\"N/A\",waterPressureDrop(W138, U138 & \"P\" & IF(V138=\"Dual\",2,1) &\"C\", AD138, \"heating\", T138)))","v":""},{"$f":"IF(OR(T138=\"Select Model\",T138=\"PCBL\"), \"\",IF(AY138=0,getReturnWaterTemp(T138,AE138, activeEWTHeating, AX138, \"heating\"),getReturnWaterTemp(T138,AD138, activeEWTHeating, AY138, \"heating\")))","v":""},"",{"$f":" getNozzle(T138, W138, Y138, Z138, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I139)),I139<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I139, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H139)),H139<0),\"\",intlEstQuantity(T139, W139*12, H139)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T139=\"Select Model\",\"\",coilCircuitChange(W139, U139, AC139, T139,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T139=\"Select Model\",\"\",beamWidth(T139))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T139=\"Select Model\",T139=\"PCBL\"), 0,getSPIP(T139, W139, Y139, BD139, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T139=\"Select Model\", \"\",IF(T139=\"PCBL\",0,primaryAirSensibleCapacityIP($T139,$W139,activeRoomTempCooling,activePriAirTempCooling,$Y139,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T139=\"Select Model\",\"\",IF($T139=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y139,activeElevation)))","v":""},{"$f":"IF(OR(T139=\"Select Model\",T139=\"PCBL\"), 0,IF(AD139=0,0,-primaryAirSensibleCapacityIP($T139,$W139,activeRoomTempHeating,activePriAirTempHeating,$Y139,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T139=\"Select Model\", \"\", InductionRatio($T139,BD139,$W139,$Y139)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T139=\"Select Model\", \"\",IF($T139=\"PCBL\",\"N/A\",minVAVSetBack(AA139, Y139))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T139=\"Select Model\", \"\",IF($T139= \"PCBL\",\"N/A\",getDischargeAirTemp($T139,$V139,$AC139,$W139,BD139,$AL139, $Y139, $AS139, \"cooling\",activeElevation,$AB139,$AJ139,$AV139,$BB139))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T139=\"Select Model\",$T139=\"PCBL\"), \"\",getDischargeAirTemp($T139,$V139,$AD139,$W139,BD139,$AL139, $Y139, $AY139, \"heating\",activeElevation,$AB139,$AJ139,$AV139,$BB139)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T139=\"Select Model\", \"\",IF(OR($T139=\"ACBC_1W\",$T139=\"ACBC_2W\",LEFT($T139,4)=\"ACBR\",$T139 = \"LIU24_2W\",LEFT($T139,3)=\"RIU\",LEFT($T139,6)=\"ACBL12\"), IF((soundLevel($T139, $AB139, BD139, $Y139, $W139,$AJ139,$AA139,\"dba\"))<15,\"<15\",soundLevel($T139, $AB139, BD139, $Y139, $W139,$AJ139,$AA139,\"dba\")+0.4),IF((soundLevel($T139, $AB139, BD139, $Y139, $W139,$AJ139,$AA139,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T139, $AB139, BD139, $Y139, $W139,$AJ139,$AA139,\"dba\")+5)<15, \"<15\", soundLevel($T139, $AB139, BD139,$Y139, $W139,$AJ139,$AA139,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T139=\"Select Model\", \"\",IF(OR($T139=\"ACBC_1W\",$T139=\"ACBC_2W\",LEFT($T139,4)=\"ACBR\",$T139=\"LIU24_2W\",LEFT($T139,3)=\"RIU\",LEFT($T139,6)=\"ACBL12\"), IF((soundLevel($T139, $AB139, BD139, $Y139, $W139,$AJ139,$AA139,\"NC\"))<15,\"<15\",soundLevel($T139, $AB139, BD139, $Y139, $W139,$AJ139,$AA139,\"NC\")+0.4),IF((soundLevel($T139, $AB139, BD139, $Y139, $W139,$AJ139,$AA139,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T139, $AB139, BD139, $Y139, $W139,$AJ139,$AA139,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T139, $AB139, BD139, $Y139, $W139,$AJ139,$AA139,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T139=\"Select Model\",\"\",IF($T139=\"LIU24_2W\",calcQwIP($Y139,$W139,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC139,$AI139,\"latent\",$U139&\"P\"&IF($V139=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T139,activeElevation),\"\"))","v":""},{"$f":"IF($T139=\"Select Model\",\"\",IF($T139=\"ACBC_1W\",calcQwIP($Y139,$W139,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC139,BD139,\"capacity\",$U139&\"P\"&IF($V139=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T139,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y139,$W139,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC139,BD139,\"capacity\",$U139&\"P\"&IF($V139=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T139,activeElevation)))","v":""},"",{"$f":"IF(T139=\"Select Model\", 0,waterPressureDrop(W139, U139 & \"P\" & IF(V139=\"Dual\",2,1) &\"C\", AC139, \"cooling\", T139))","v":0},{"$f":"IF(T139=\"Select Model\", \"\",getReturnWaterTemp(T139,AC139, activeEWTCooling, AS139, \"cooling\"))","v":""},"",{"$f":"IF($T139<>\"ACBC_1W\",\"\",IF($J139=\"\",\"\",FintubeCapacity($T139,$W139,$AE139,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T139=\"Select Model\",T139=\"PCBL\"),\"\",calcQwIP(Y139,W139,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD139,BD139,\"capacity\",U139&\"P\"&IF(V139=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T139,activeElevation))","v":""},"",{"$f":"IF(OR(T139=\"Select Model\",T139=\"PCBL\"), \"\",IF(AY139=0,\"N/A\",waterPressureDrop(W139, U139 & \"P\" & IF(V139=\"Dual\",2,1) &\"C\", AD139, \"heating\", T139)))","v":""},{"$f":"IF(OR(T139=\"Select Model\",T139=\"PCBL\"), \"\",IF(AY139=0,getReturnWaterTemp(T139,AE139, activeEWTHeating, AX139, \"heating\"),getReturnWaterTemp(T139,AD139, activeEWTHeating, AY139, \"heating\")))","v":""},"",{"$f":" getNozzle(T139, W139, Y139, Z139, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I140)),I140<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I140, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H140)),H140<0),\"\",intlEstQuantity(T140, W140*12, H140)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T140=\"Select Model\",\"\",coilCircuitChange(W140, U140, AC140, T140,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T140=\"Select Model\",\"\",beamWidth(T140))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T140=\"Select Model\",T140=\"PCBL\"), 0,getSPIP(T140, W140, Y140, BD140, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T140=\"Select Model\", \"\",IF(T140=\"PCBL\",0,primaryAirSensibleCapacityIP($T140,$W140,activeRoomTempCooling,activePriAirTempCooling,$Y140,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T140=\"Select Model\",\"\",IF($T140=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y140,activeElevation)))","v":""},{"$f":"IF(OR(T140=\"Select Model\",T140=\"PCBL\"), 0,IF(AD140=0,0,-primaryAirSensibleCapacityIP($T140,$W140,activeRoomTempHeating,activePriAirTempHeating,$Y140,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T140=\"Select Model\", \"\", InductionRatio($T140,BD140,$W140,$Y140)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T140=\"Select Model\", \"\",IF($T140=\"PCBL\",\"N/A\",minVAVSetBack(AA140, Y140))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T140=\"Select Model\", \"\",IF($T140= \"PCBL\",\"N/A\",getDischargeAirTemp($T140,$V140,$AC140,$W140,BD140,$AL140, $Y140, $AS140, \"cooling\",activeElevation,$AB140,$AJ140,$AV140,$BB140))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T140=\"Select Model\",$T140=\"PCBL\"), \"\",getDischargeAirTemp($T140,$V140,$AD140,$W140,BD140,$AL140, $Y140, $AY140, \"heating\",activeElevation,$AB140,$AJ140,$AV140,$BB140)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T140=\"Select Model\", \"\",IF(OR($T140=\"ACBC_1W\",$T140=\"ACBC_2W\",LEFT($T140,4)=\"ACBR\",$T140 = \"LIU24_2W\",LEFT($T140,3)=\"RIU\",LEFT($T140,6)=\"ACBL12\"), IF((soundLevel($T140, $AB140, BD140, $Y140, $W140,$AJ140,$AA140,\"dba\"))<15,\"<15\",soundLevel($T140, $AB140, BD140, $Y140, $W140,$AJ140,$AA140,\"dba\")+0.4),IF((soundLevel($T140, $AB140, BD140, $Y140, $W140,$AJ140,$AA140,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T140, $AB140, BD140, $Y140, $W140,$AJ140,$AA140,\"dba\")+5)<15, \"<15\", soundLevel($T140, $AB140, BD140,$Y140, $W140,$AJ140,$AA140,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T140=\"Select Model\", \"\",IF(OR($T140=\"ACBC_1W\",$T140=\"ACBC_2W\",LEFT($T140,4)=\"ACBR\",$T140=\"LIU24_2W\",LEFT($T140,3)=\"RIU\",LEFT($T140,6)=\"ACBL12\"), IF((soundLevel($T140, $AB140, BD140, $Y140, $W140,$AJ140,$AA140,\"NC\"))<15,\"<15\",soundLevel($T140, $AB140, BD140, $Y140, $W140,$AJ140,$AA140,\"NC\")+0.4),IF((soundLevel($T140, $AB140, BD140, $Y140, $W140,$AJ140,$AA140,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T140, $AB140, BD140, $Y140, $W140,$AJ140,$AA140,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T140, $AB140, BD140, $Y140, $W140,$AJ140,$AA140,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T140=\"Select Model\",\"\",IF($T140=\"LIU24_2W\",calcQwIP($Y140,$W140,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC140,$AI140,\"latent\",$U140&\"P\"&IF($V140=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T140,activeElevation),\"\"))","v":""},{"$f":"IF($T140=\"Select Model\",\"\",IF($T140=\"ACBC_1W\",calcQwIP($Y140,$W140,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC140,BD140,\"capacity\",$U140&\"P\"&IF($V140=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T140,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y140,$W140,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC140,BD140,\"capacity\",$U140&\"P\"&IF($V140=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T140,activeElevation)))","v":""},"",{"$f":"IF(T140=\"Select Model\", 0,waterPressureDrop(W140, U140 & \"P\" & IF(V140=\"Dual\",2,1) &\"C\", AC140, \"cooling\", T140))","v":0},{"$f":"IF(T140=\"Select Model\", \"\",getReturnWaterTemp(T140,AC140, activeEWTCooling, AS140, \"cooling\"))","v":""},"",{"$f":"IF($T140<>\"ACBC_1W\",\"\",IF($J140=\"\",\"\",FintubeCapacity($T140,$W140,$AE140,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T140=\"Select Model\",T140=\"PCBL\"),\"\",calcQwIP(Y140,W140,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD140,BD140,\"capacity\",U140&\"P\"&IF(V140=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T140,activeElevation))","v":""},"",{"$f":"IF(OR(T140=\"Select Model\",T140=\"PCBL\"), \"\",IF(AY140=0,\"N/A\",waterPressureDrop(W140, U140 & \"P\" & IF(V140=\"Dual\",2,1) &\"C\", AD140, \"heating\", T140)))","v":""},{"$f":"IF(OR(T140=\"Select Model\",T140=\"PCBL\"), \"\",IF(AY140=0,getReturnWaterTemp(T140,AE140, activeEWTHeating, AX140, \"heating\"),getReturnWaterTemp(T140,AD140, activeEWTHeating, AY140, \"heating\")))","v":""},"",{"$f":" getNozzle(T140, W140, Y140, Z140, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I141)),I141<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I141, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H141)),H141<0),\"\",intlEstQuantity(T141, W141*12, H141)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T141=\"Select Model\",\"\",coilCircuitChange(W141, U141, AC141, T141,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T141=\"Select Model\",\"\",beamWidth(T141))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T141=\"Select Model\",T141=\"PCBL\"), 0,getSPIP(T141, W141, Y141, BD141, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T141=\"Select Model\", \"\",IF(T141=\"PCBL\",0,primaryAirSensibleCapacityIP($T141,$W141,activeRoomTempCooling,activePriAirTempCooling,$Y141,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T141=\"Select Model\",\"\",IF($T141=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y141,activeElevation)))","v":""},{"$f":"IF(OR(T141=\"Select Model\",T141=\"PCBL\"), 0,IF(AD141=0,0,-primaryAirSensibleCapacityIP($T141,$W141,activeRoomTempHeating,activePriAirTempHeating,$Y141,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T141=\"Select Model\", \"\", InductionRatio($T141,BD141,$W141,$Y141)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T141=\"Select Model\", \"\",IF($T141=\"PCBL\",\"N/A\",minVAVSetBack(AA141, Y141))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T141=\"Select Model\", \"\",IF($T141= \"PCBL\",\"N/A\",getDischargeAirTemp($T141,$V141,$AC141,$W141,BD141,$AL141, $Y141, $AS141, \"cooling\",activeElevation,$AB141,$AJ141,$AV141,$BB141))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T141=\"Select Model\",$T141=\"PCBL\"), \"\",getDischargeAirTemp($T141,$V141,$AD141,$W141,BD141,$AL141, $Y141, $AY141, \"heating\",activeElevation,$AB141,$AJ141,$AV141,$BB141)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T141=\"Select Model\", \"\",IF(OR($T141=\"ACBC_1W\",$T141=\"ACBC_2W\",LEFT($T141,4)=\"ACBR\",$T141 = \"LIU24_2W\",LEFT($T141,3)=\"RIU\",LEFT($T141,6)=\"ACBL12\"), IF((soundLevel($T141, $AB141, BD141, $Y141, $W141,$AJ141,$AA141,\"dba\"))<15,\"<15\",soundLevel($T141, $AB141, BD141, $Y141, $W141,$AJ141,$AA141,\"dba\")+0.4),IF((soundLevel($T141, $AB141, BD141, $Y141, $W141,$AJ141,$AA141,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T141, $AB141, BD141, $Y141, $W141,$AJ141,$AA141,\"dba\")+5)<15, \"<15\", soundLevel($T141, $AB141, BD141,$Y141, $W141,$AJ141,$AA141,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T141=\"Select Model\", \"\",IF(OR($T141=\"ACBC_1W\",$T141=\"ACBC_2W\",LEFT($T141,4)=\"ACBR\",$T141=\"LIU24_2W\",LEFT($T141,3)=\"RIU\",LEFT($T141,6)=\"ACBL12\"), IF((soundLevel($T141, $AB141, BD141, $Y141, $W141,$AJ141,$AA141,\"NC\"))<15,\"<15\",soundLevel($T141, $AB141, BD141, $Y141, $W141,$AJ141,$AA141,\"NC\")+0.4),IF((soundLevel($T141, $AB141, BD141, $Y141, $W141,$AJ141,$AA141,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T141, $AB141, BD141, $Y141, $W141,$AJ141,$AA141,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T141, $AB141, BD141, $Y141, $W141,$AJ141,$AA141,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T141=\"Select Model\",\"\",IF($T141=\"LIU24_2W\",calcQwIP($Y141,$W141,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC141,$AI141,\"latent\",$U141&\"P\"&IF($V141=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T141,activeElevation),\"\"))","v":""},{"$f":"IF($T141=\"Select Model\",\"\",IF($T141=\"ACBC_1W\",calcQwIP($Y141,$W141,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC141,BD141,\"capacity\",$U141&\"P\"&IF($V141=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T141,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y141,$W141,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC141,BD141,\"capacity\",$U141&\"P\"&IF($V141=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T141,activeElevation)))","v":""},"",{"$f":"IF(T141=\"Select Model\", 0,waterPressureDrop(W141, U141 & \"P\" & IF(V141=\"Dual\",2,1) &\"C\", AC141, \"cooling\", T141))","v":0},{"$f":"IF(T141=\"Select Model\", \"\",getReturnWaterTemp(T141,AC141, activeEWTCooling, AS141, \"cooling\"))","v":""},"",{"$f":"IF($T141<>\"ACBC_1W\",\"\",IF($J141=\"\",\"\",FintubeCapacity($T141,$W141,$AE141,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T141=\"Select Model\",T141=\"PCBL\"),\"\",calcQwIP(Y141,W141,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD141,BD141,\"capacity\",U141&\"P\"&IF(V141=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T141,activeElevation))","v":""},"",{"$f":"IF(OR(T141=\"Select Model\",T141=\"PCBL\"), \"\",IF(AY141=0,\"N/A\",waterPressureDrop(W141, U141 & \"P\" & IF(V141=\"Dual\",2,1) &\"C\", AD141, \"heating\", T141)))","v":""},{"$f":"IF(OR(T141=\"Select Model\",T141=\"PCBL\"), \"\",IF(AY141=0,getReturnWaterTemp(T141,AE141, activeEWTHeating, AX141, \"heating\"),getReturnWaterTemp(T141,AD141, activeEWTHeating, AY141, \"heating\")))","v":""},"",{"$f":" getNozzle(T141, W141, Y141, Z141, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I142)),I142<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I142, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H142)),H142<0),\"\",intlEstQuantity(T142, W142*12, H142)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T142=\"Select Model\",\"\",coilCircuitChange(W142, U142, AC142, T142,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T142=\"Select Model\",\"\",beamWidth(T142))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T142=\"Select Model\",T142=\"PCBL\"), 0,getSPIP(T142, W142, Y142, BD142, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T142=\"Select Model\", \"\",IF(T142=\"PCBL\",0,primaryAirSensibleCapacityIP($T142,$W142,activeRoomTempCooling,activePriAirTempCooling,$Y142,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T142=\"Select Model\",\"\",IF($T142=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y142,activeElevation)))","v":""},{"$f":"IF(OR(T142=\"Select Model\",T142=\"PCBL\"), 0,IF(AD142=0,0,-primaryAirSensibleCapacityIP($T142,$W142,activeRoomTempHeating,activePriAirTempHeating,$Y142,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T142=\"Select Model\", \"\", InductionRatio($T142,BD142,$W142,$Y142)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T142=\"Select Model\", \"\",IF($T142=\"PCBL\",\"N/A\",minVAVSetBack(AA142, Y142))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T142=\"Select Model\", \"\",IF($T142= \"PCBL\",\"N/A\",getDischargeAirTemp($T142,$V142,$AC142,$W142,BD142,$AL142, $Y142, $AS142, \"cooling\",activeElevation,$AB142,$AJ142,$AV142,$BB142))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T142=\"Select Model\",$T142=\"PCBL\"), \"\",getDischargeAirTemp($T142,$V142,$AD142,$W142,BD142,$AL142, $Y142, $AY142, \"heating\",activeElevation,$AB142,$AJ142,$AV142,$BB142)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T142=\"Select Model\", \"\",IF(OR($T142=\"ACBC_1W\",$T142=\"ACBC_2W\",LEFT($T142,4)=\"ACBR\",$T142 = \"LIU24_2W\",LEFT($T142,3)=\"RIU\",LEFT($T142,6)=\"ACBL12\"), IF((soundLevel($T142, $AB142, BD142, $Y142, $W142,$AJ142,$AA142,\"dba\"))<15,\"<15\",soundLevel($T142, $AB142, BD142, $Y142, $W142,$AJ142,$AA142,\"dba\")+0.4),IF((soundLevel($T142, $AB142, BD142, $Y142, $W142,$AJ142,$AA142,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T142, $AB142, BD142, $Y142, $W142,$AJ142,$AA142,\"dba\")+5)<15, \"<15\", soundLevel($T142, $AB142, BD142,$Y142, $W142,$AJ142,$AA142,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T142=\"Select Model\", \"\",IF(OR($T142=\"ACBC_1W\",$T142=\"ACBC_2W\",LEFT($T142,4)=\"ACBR\",$T142=\"LIU24_2W\",LEFT($T142,3)=\"RIU\",LEFT($T142,6)=\"ACBL12\"), IF((soundLevel($T142, $AB142, BD142, $Y142, $W142,$AJ142,$AA142,\"NC\"))<15,\"<15\",soundLevel($T142, $AB142, BD142, $Y142, $W142,$AJ142,$AA142,\"NC\")+0.4),IF((soundLevel($T142, $AB142, BD142, $Y142, $W142,$AJ142,$AA142,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T142, $AB142, BD142, $Y142, $W142,$AJ142,$AA142,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T142, $AB142, BD142, $Y142, $W142,$AJ142,$AA142,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T142=\"Select Model\",\"\",IF($T142=\"LIU24_2W\",calcQwIP($Y142,$W142,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC142,$AI142,\"latent\",$U142&\"P\"&IF($V142=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T142,activeElevation),\"\"))","v":""},{"$f":"IF($T142=\"Select Model\",\"\",IF($T142=\"ACBC_1W\",calcQwIP($Y142,$W142,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC142,BD142,\"capacity\",$U142&\"P\"&IF($V142=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T142,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y142,$W142,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC142,BD142,\"capacity\",$U142&\"P\"&IF($V142=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T142,activeElevation)))","v":""},"",{"$f":"IF(T142=\"Select Model\", 0,waterPressureDrop(W142, U142 & \"P\" & IF(V142=\"Dual\",2,1) &\"C\", AC142, \"cooling\", T142))","v":0},{"$f":"IF(T142=\"Select Model\", \"\",getReturnWaterTemp(T142,AC142, activeEWTCooling, AS142, \"cooling\"))","v":""},"",{"$f":"IF($T142<>\"ACBC_1W\",\"\",IF($J142=\"\",\"\",FintubeCapacity($T142,$W142,$AE142,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T142=\"Select Model\",T142=\"PCBL\"),\"\",calcQwIP(Y142,W142,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD142,BD142,\"capacity\",U142&\"P\"&IF(V142=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T142,activeElevation))","v":""},"",{"$f":"IF(OR(T142=\"Select Model\",T142=\"PCBL\"), \"\",IF(AY142=0,\"N/A\",waterPressureDrop(W142, U142 & \"P\" & IF(V142=\"Dual\",2,1) &\"C\", AD142, \"heating\", T142)))","v":""},{"$f":"IF(OR(T142=\"Select Model\",T142=\"PCBL\"), \"\",IF(AY142=0,getReturnWaterTemp(T142,AE142, activeEWTHeating, AX142, \"heating\"),getReturnWaterTemp(T142,AD142, activeEWTHeating, AY142, \"heating\")))","v":""},"",{"$f":" getNozzle(T142, W142, Y142, Z142, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I143)),I143<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I143, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H143)),H143<0),\"\",intlEstQuantity(T143, W143*12, H143)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T143=\"Select Model\",\"\",coilCircuitChange(W143, U143, AC143, T143,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T143=\"Select Model\",\"\",beamWidth(T143))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T143=\"Select Model\",T143=\"PCBL\"), 0,getSPIP(T143, W143, Y143, BD143, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T143=\"Select Model\", \"\",IF(T143=\"PCBL\",0,primaryAirSensibleCapacityIP($T143,$W143,activeRoomTempCooling,activePriAirTempCooling,$Y143,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T143=\"Select Model\",\"\",IF($T143=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y143,activeElevation)))","v":""},{"$f":"IF(OR(T143=\"Select Model\",T143=\"PCBL\"), 0,IF(AD143=0,0,-primaryAirSensibleCapacityIP($T143,$W143,activeRoomTempHeating,activePriAirTempHeating,$Y143,activeElevation,\"heating\")))","v":0},{"$f":"getCurrentNozzleCode(T143, W143, Y143, Z143, activeElevation, TRUE)","v":""},{"$f":"IFERROR(IF(T143=\"Select Model\", \"\", InductionRatio($T143,BD143,$W143,$Y143)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T143=\"Select Model\", \"\",IF($T143=\"PCBL\",\"N/A\",minVAVSetBack(AA143, Y143))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T143=\"Select Model\", \"\",IF($T143= \"PCBL\",\"N/A\",getDischargeAirTemp($T143,$V143,$AC143,$W143,BD143,$AL143, $Y143, $AS143, \"cooling\",activeElevation,$AB143,$AJ143,$AV143,$BB143))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T143=\"Select Model\",$T143=\"PCBL\"), \"\",getDischargeAirTemp($T143,$V143,$AD143,$W143,BD143,$AL143, $Y143, $AY143, \"heating\",activeElevation,$AB143,$AJ143,$AV143,$BB143)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T143=\"Select Model\", \"\",IF(OR($T143=\"ACBC_1W\",$T143=\"ACBC_2W\",LEFT($T143,4)=\"ACBR\",$T143 = \"LIU24_2W\",LEFT($T143,3)=\"RIU\",LEFT($T143,6)=\"ACBL12\"), IF((soundLevel($T143, $AB143, BD143, $Y143, $W143,$AJ143,$AA143,\"dba\"))<15,\"<15\",soundLevel($T143, $AB143, BD143, $Y143, $W143,$AJ143,$AA143,\"dba\")+0.4),IF((soundLevel($T143, $AB143, BD143, $Y143, $W143,$AJ143,$AA143,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T143, $AB143, BD143, $Y143, $W143,$AJ143,$AA143,\"dba\")+5)<15, \"<15\", soundLevel($T143, $AB143, BD143,$Y143, $W143,$AJ143,$AA143,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T143=\"Select Model\", \"\",IF(OR($T143=\"ACBC_1W\",$T143=\"ACBC_2W\",LEFT($T143,4)=\"ACBR\",$T143=\"LIU24_2W\",LEFT($T143,3)=\"RIU\",LEFT($T143,6)=\"ACBL12\"), IF((soundLevel($T143, $AB143, BD143, $Y143, $W143,$AJ143,$AA143,\"NC\"))<15,\"<15\",soundLevel($T143, $AB143, BD143, $Y143, $W143,$AJ143,$AA143,\"NC\")+0.4),IF((soundLevel($T143, $AB143, BD143, $Y143, $W143,$AJ143,$AA143,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T143, $AB143, BD143, $Y143, $W143,$AJ143,$AA143,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T143, $AB143, BD143, $Y143, $W143,$AJ143,$AA143,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T143=\"Select Model\",\"\",IF($T143=\"LIU24_2W\",calcQwIP($Y143,$W143,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC143,$AI143,\"latent\",$U143&\"P\"&IF($V143=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T143,activeElevation),\"\"))","v":""},{"$f":"IF($T143=\"Select Model\",\"\",IF($T143=\"ACBC_1W\",calcQwIP($Y143,$W143,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC143,BD143,\"capacity\",$U143&\"P\"&IF($V143=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T143,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y143,$W143,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC143,BD143,\"capacity\",$U143&\"P\"&IF($V143=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T143,activeElevation)))","v":""},"",{"$f":"IF(T143=\"Select Model\", 0,waterPressureDrop(W143, U143 & \"P\" & IF(V143=\"Dual\",2,1) &\"C\", AC143, \"cooling\", T143))","v":0},{"$f":"IF(T143=\"Select Model\", \"\",getReturnWaterTemp(T143,AC143, activeEWTCooling, AS143, \"cooling\"))","v":""},"",{"$f":"IF($T143<>\"ACBC_1W\",\"\",IF($J143=\"\",\"\",FintubeCapacity($T143,$W143,$AE143,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T143=\"Select Model\",T143=\"PCBL\"),\"\",calcQwIP(Y143,W143,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD143,BD143,\"capacity\",U143&\"P\"&IF(V143=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T143,activeElevation))","v":""},"",{"$f":"IF(OR(T143=\"Select Model\",T143=\"PCBL\"), \"\",IF(AY143=0,\"N/A\",waterPressureDrop(W143, U143 & \"P\" & IF(V143=\"Dual\",2,1) &\"C\", AD143, \"heating\", T143)))","v":""},{"$f":"IF(OR(T143=\"Select Model\",T143=\"PCBL\"), \"\",IF(AY143=0,getReturnWaterTemp(T143,AE143, activeEWTHeating, AX143, \"heating\"),getReturnWaterTemp(T143,AD143, activeEWTHeating, AY143, \"heating\")))","v":""},"",{"$f":" getNozzle(T143, W143, Y143, Z143, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I144)),I144<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I144, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H144)),H144<0),\"\",intlEstQuantity(T144, W144*12, H144)),1)","v":""},{"$f":"IF(LEFT(T144, 4)=\"ACBC\",IF(AND(ISNUMBER(L144),ISNUMBER(AT144)),IF(AA144=-1,\"LOW CFM\",L144*AT144),\"\"),IF(AND(ISNUMBER(L144),ISNUMBER(AT144)),IF(AA144=-1,\"N/A CFM\",L144*AT144),\"\"))","v":""},{"$f":"IF(LEFT(T144,4)=\"ACBC\",IF(AND(ISNUMBER(L144),ISNUMBER(AG144)),IF(AA144=-1,\"LOW CFM\",L144*AG144),\"\"),IF(AND(ISNUMBER(L144),ISNUMBER(AG144)),IF(AA144=-1,\"N/A CFM\",L144*AG144),\"\"))","v":""},{"$f":"IF(LEFT(T144,4)=\"ACBC\",IF(AND(ISNUMBER(L144),ISNUMBER(AZ144)),IF(AA144=-1,\"LOW CFM\",L144*AZ144),\"\"),IF(AND(ISNUMBER(L144),ISNUMBER(AZ144)),IF(AA144=-1,\"N/A CFM\",L144*AZ144),\"\"))","v":""},{"$f":"IF(AND(ISNUMBER(L144),ISNUMBER(Y144)),L144*Y144,\"\")","v":""},{"$f":"IF(AND(ISNUMBER(L144),ISNUMBER(AC144)),L144*AC144,\"\")","v":""},{"$f":"IF(AND(ISNUMBER(L144),ISNUMBER(AD144)),IF(AND(T144=\"ACBC_1W\",AD144=0),AE144*L144,L144*AD144))","v":false},"Default","Select Model",2,{"$f":"IF(T144=\"Select Model\",\"\",coilCircuitChange(W144, U144, AC144, T144,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T144=\"Select Model\",\"\",beamWidth(T144))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T144=\"Select Model\",T144=\"PCBL\"), 0,getSPIP(T144, W144, Y144, BD144, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T144=\"Select Model\", \"\",IF(T144=\"PCBL\",0,primaryAirSensibleCapacityIP($T144,$W144,activeRoomTempCooling,activePriAirTempCooling,$Y144,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T144=\"Select Model\",\"\",IF($T144=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y144,activeElevation)))","v":""},{"$f":"IF(OR(T144=\"Select Model\",T144=\"PCBL\"), 0,IF(AD144=0,0,-primaryAirSensibleCapacityIP($T144,$W144,activeRoomTempHeating,activePriAirTempHeating,$Y144,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T144=\"Select Model\", \"\", InductionRatio($T144,BD144,$W144,$Y144)),\"N/A\")","v":""},{"$f":"IFERROR(AT144/Y144,\"\")","v":""},{"$f":"IFERROR(IF(T144=\"Select Model\", \"\",(1+AJ144)*Y144),\"N/A\")","v":""},{"$f":"IFERROR(IF(T144=\"Select Model\", \"\",IF($T144=\"PCBL\",\"N/A\",minVAVSetBack(AA144, Y144))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T144=\"Select Model\", \"\",IF($T144= \"PCBL\",\"N/A\",getDischargeAirTemp($T144,$V144,$AC144,$W144,BD144,$AL144, $Y144, $AS144, \"cooling\",activeElevation,$AB144,$AJ144,$AV144,$BB144))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T144=\"Select Model\",$T144=\"PCBL\"), \"\",getDischargeAirTemp($T144,$V144,$AD144,$W144,BD144,$AL144, $Y144, $AY144, \"heating\",activeElevation,$AB144,$AJ144,$AV144,$BB144)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T144=\"Select Model\", \"\",IF(OR($T144=\"ACBC_1W\",$T144=\"ACBC_2W\",LEFT($T144,4)=\"ACBR\",$T144 = \"LIU24_2W\",LEFT($T144,3)=\"RIU\",LEFT($T144,6)=\"ACBL12\"), IF((soundLevel($T144, $AB144, BD144, $Y144, $W144,$AJ144,$AA144,\"dba\"))<15,\"<15\",soundLevel($T144, $AB144, BD144, $Y144, $W144,$AJ144,$AA144,\"dba\")+0.4),IF((soundLevel($T144, $AB144, BD144, $Y144, $W144,$AJ144,$AA144,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T144, $AB144, BD144, $Y144, $W144,$AJ144,$AA144,\"dba\")+5)<15, \"<15\", soundLevel($T144, $AB144, BD144,$Y144, $W144,$AJ144,$AA144,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T144=\"Select Model\", \"\",IF(OR($T144=\"ACBC_1W\",$T144=\"ACBC_2W\",LEFT($T144,4)=\"ACBR\",$T144=\"LIU24_2W\",LEFT($T144,3)=\"RIU\",LEFT($T144,6)=\"ACBL12\"), IF((soundLevel($T144, $AB144, BD144, $Y144, $W144,$AJ144,$AA144,\"NC\"))<15,\"<15\",soundLevel($T144, $AB144, BD144, $Y144, $W144,$AJ144,$AA144,\"NC\")+0.4),IF((soundLevel($T144, $AB144, BD144, $Y144, $W144,$AJ144,$AA144,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T144, $AB144, BD144, $Y144, $W144,$AJ144,$AA144,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T144, $AB144, BD144, $Y144, $W144,$AJ144,$AA144,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T144=\"Select Model\",\"\",IF($T144=\"LIU24_2W\",calcQwIP($Y144,$W144,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC144,$AI144,\"latent\",$U144&\"P\"&IF($V144=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T144,activeElevation),\"\"))","v":""},{"$f":"IF($T144=\"Select Model\",\"\",IF($T144=\"ACBC_1W\",calcQwIP($Y144,$W144,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC144,BD144,\"capacity\",$U144&\"P\"&IF($V144=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T144,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y144,$W144,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC144,BD144,\"capacity\",$U144&\"P\"&IF($V144=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T144,activeElevation)))","v":""},{"$f":"IF(T144=\"Select Model\", \"\",IF(T144 = \"LIU24_2W\", AS144+AF144+AR144, AS144+AF144))","v":""},{"$f":"IF(T144=\"Select Model\", 0,waterPressureDrop(W144, U144 & \"P\" & IF(V144=\"Dual\",2,1) &\"C\", AC144, \"cooling\", T144))","v":0},{"$f":"IF(T144=\"Select Model\", \"\",getReturnWaterTemp(T144,AC144, activeEWTCooling, AS144, \"cooling\"))","v":""},{"$f":"IF(T144=\"Select Model\", \"\",$AV144-activeEWTCooling)","v":""},{"$f":"IF($T144<>\"ACBC_1W\",\"\",IF($J144=\"\",\"\",FintubeCapacity($T144,$W144,$AE144,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T144=\"Select Model\",T144=\"PCBL\"),\"\",calcQwIP(Y144,W144,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD144,BD144,\"capacity\",U144&\"P\"&IF(V144=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T144,activeElevation))","v":""},{"$f":"IF(OR(T144=\"Select Model\",T144=\"PCBL\"),\"\",IF(AND(AD144=0,T144=\"ACBC_1W\"),AX144+AH144,AY144+AH144))","v":""},{"$f":"IF(OR(T144=\"Select Model\",T144=\"PCBL\"), \"\",IF(AY144=0,\"N/A\",waterPressureDrop(W144, U144 & \"P\" & IF(V144=\"Dual\",2,1) &\"C\", AD144, \"heating\", T144)))","v":""},{"$f":"IF(OR(T144=\"Select Model\",T144=\"PCBL\"), \"\",IF(AY144=0,getReturnWaterTemp(T144,AE144, activeEWTHeating, AX144, \"heating\"),getReturnWaterTemp(T144,AD144, activeEWTHeating, AY144, \"heating\")))","v":""},{"$f":"IF(OR($T144=\"Select Model\",$J144=\"\",T144=\"PCBL\"), \"\",activeEWTHeating-$BB144)","v":""},{"$f":" getNozzle(T144, W144, Y144, Z144, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I145)),I145<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I145, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H145)),H145<0),\"\",intlEstQuantity(T145, W145*12, H145)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T145=\"Select Model\",\"\",coilCircuitChange(W145, U145, AC145, T145,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T145=\"Select Model\",\"\",beamWidth(T145))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T145=\"Select Model\",T145=\"PCBL\"), 0,getSPIP(T145, W145, Y145, BD145, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T145=\"Select Model\", \"\",IF(T145=\"PCBL\",0,primaryAirSensibleCapacityIP($T145,$W145,activeRoomTempCooling,activePriAirTempCooling,$Y145,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T145=\"Select Model\",\"\",IF($T145=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y145,activeElevation)))","v":""},{"$f":"IF(OR(T145=\"Select Model\",T145=\"PCBL\"), 0,IF(AD145=0,0,-primaryAirSensibleCapacityIP($T145,$W145,activeRoomTempHeating,activePriAirTempHeating,$Y145,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T145=\"Select Model\", \"\", InductionRatio($T145,BD145,$W145,$Y145)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T145=\"Select Model\", \"\",IF($T145=\"PCBL\",\"N/A\",minVAVSetBack(AA145, Y145))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T145=\"Select Model\", \"\",IF($T145= \"PCBL\",\"N/A\",getDischargeAirTemp($T145,$V145,$AC145,$W145,BD145,$AL145, $Y145, $AS145, \"cooling\",activeElevation,$AB145,$AJ145,$AV145,$BB145))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T145=\"Select Model\",$T145=\"PCBL\"), \"\",getDischargeAirTemp($T145,$V145,$AD145,$W145,BD145,$AL145, $Y145, $AY145, \"heating\",activeElevation,$AB145,$AJ145,$AV145,$BB145)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T145=\"Select Model\", \"\",IF(OR($T145=\"ACBC_1W\",$T145=\"ACBC_2W\",LEFT($T145,4)=\"ACBR\",$T145 = \"LIU24_2W\",LEFT($T145,3)=\"RIU\",LEFT($T145,6)=\"ACBL12\"), IF((soundLevel($T145, $AB145, BD145, $Y145, $W145,$AJ145,$AA145,\"dba\"))<15,\"<15\",soundLevel($T145, $AB145, BD145, $Y145, $W145,$AJ145,$AA145,\"dba\")+0.4),IF((soundLevel($T145, $AB145, BD145, $Y145, $W145,$AJ145,$AA145,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T145, $AB145, BD145, $Y145, $W145,$AJ145,$AA145,\"dba\")+5)<15, \"<15\", soundLevel($T145, $AB145, BD145,$Y145, $W145,$AJ145,$AA145,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T145=\"Select Model\", \"\",IF(OR($T145=\"ACBC_1W\",$T145=\"ACBC_2W\",LEFT($T145,4)=\"ACBR\",$T145=\"LIU24_2W\",LEFT($T145,3)=\"RIU\",LEFT($T145,6)=\"ACBL12\"), IF((soundLevel($T145, $AB145, BD145, $Y145, $W145,$AJ145,$AA145,\"NC\"))<15,\"<15\",soundLevel($T145, $AB145, BD145, $Y145, $W145,$AJ145,$AA145,\"NC\")+0.4),IF((soundLevel($T145, $AB145, BD145, $Y145, $W145,$AJ145,$AA145,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T145, $AB145, BD145, $Y145, $W145,$AJ145,$AA145,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T145, $AB145, BD145, $Y145, $W145,$AJ145,$AA145,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T145=\"Select Model\",\"\",IF($T145=\"LIU24_2W\",calcQwIP($Y145,$W145,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC145,$AI145,\"latent\",$U145&\"P\"&IF($V145=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T145,activeElevation),\"\"))","v":""},{"$f":"IF($T145=\"Select Model\",\"\",IF($T145=\"ACBC_1W\",calcQwIP($Y145,$W145,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC145,BD145,\"capacity\",$U145&\"P\"&IF($V145=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T145,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y145,$W145,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC145,BD145,\"capacity\",$U145&\"P\"&IF($V145=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T145,activeElevation)))","v":""},"",{"$f":"IF(T145=\"Select Model\", 0,waterPressureDrop(W145, U145 & \"P\" & IF(V145=\"Dual\",2,1) &\"C\", AC145, \"cooling\", T145))","v":0},{"$f":"IF(T145=\"Select Model\", \"\",getReturnWaterTemp(T145,AC145, activeEWTCooling, AS145, \"cooling\"))","v":""},"",{"$f":"IF($T145<>\"ACBC_1W\",\"\",IF($J145=\"\",\"\",FintubeCapacity($T145,$W145,$AE145,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T145=\"Select Model\",T145=\"PCBL\"),\"\",calcQwIP(Y145,W145,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD145,BD145,\"capacity\",U145&\"P\"&IF(V145=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T145,activeElevation))","v":""},"",{"$f":"IF(OR(T145=\"Select Model\",T145=\"PCBL\"), \"\",IF(AY145=0,\"N/A\",waterPressureDrop(W145, U145 & \"P\" & IF(V145=\"Dual\",2,1) &\"C\", AD145, \"heating\", T145)))","v":""},{"$f":"IF(OR(T145=\"Select Model\",T145=\"PCBL\"), \"\",IF(AY145=0,getReturnWaterTemp(T145,AE145, activeEWTHeating, AX145, \"heating\"),getReturnWaterTemp(T145,AD145, activeEWTHeating, AY145, \"heating\")))","v":""},"",{"$f":" getNozzle(T145, W145, Y145, Z145, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I146)),I146<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I146, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H146)),H146<0),\"\",intlEstQuantity(T146, W146*12, H146)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T146=\"Select Model\",\"\",coilCircuitChange(W146, U146, AC146, T146,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T146=\"Select Model\",\"\",beamWidth(T146))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T146=\"Select Model\",T146=\"PCBL\"), 0,getSPIP(T146, W146, Y146, BD146, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T146=\"Select Model\", \"\",IF(T146=\"PCBL\",0,primaryAirSensibleCapacityIP($T146,$W146,activeRoomTempCooling,activePriAirTempCooling,$Y146,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T146=\"Select Model\",\"\",IF($T146=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y146,activeElevation)))","v":""},{"$f":"IF(OR(T146=\"Select Model\",T146=\"PCBL\"), 0,IF(AD146=0,0,-primaryAirSensibleCapacityIP($T146,$W146,activeRoomTempHeating,activePriAirTempHeating,$Y146,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T146=\"Select Model\", \"\", InductionRatio($T146,BD146,$W146,$Y146)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T146=\"Select Model\", \"\",IF($T146=\"PCBL\",\"N/A\",minVAVSetBack(AA146, Y146))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T146=\"Select Model\", \"\",IF($T146= \"PCBL\",\"N/A\",getDischargeAirTemp($T146,$V146,$AC146,$W146,BD146,$AL146, $Y146, $AS146, \"cooling\",activeElevation,$AB146,$AJ146,$AV146,$BB146))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T146=\"Select Model\",$T146=\"PCBL\"), \"\",getDischargeAirTemp($T146,$V146,$AD146,$W146,BD146,$AL146, $Y146, $AY146, \"heating\",activeElevation,$AB146,$AJ146,$AV146,$BB146)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T146=\"Select Model\", \"\",IF(OR($T146=\"ACBC_1W\",$T146=\"ACBC_2W\",LEFT($T146,4)=\"ACBR\",$T146 = \"LIU24_2W\",LEFT($T146,3)=\"RIU\",LEFT($T146,6)=\"ACBL12\"), IF((soundLevel($T146, $AB146, BD146, $Y146, $W146,$AJ146,$AA146,\"dba\"))<15,\"<15\",soundLevel($T146, $AB146, BD146, $Y146, $W146,$AJ146,$AA146,\"dba\")+0.4),IF((soundLevel($T146, $AB146, BD146, $Y146, $W146,$AJ146,$AA146,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T146, $AB146, BD146, $Y146, $W146,$AJ146,$AA146,\"dba\")+5)<15, \"<15\", soundLevel($T146, $AB146, BD146,$Y146, $W146,$AJ146,$AA146,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T146=\"Select Model\", \"\",IF(OR($T146=\"ACBC_1W\",$T146=\"ACBC_2W\",LEFT($T146,4)=\"ACBR\",$T146=\"LIU24_2W\",LEFT($T146,3)=\"RIU\",LEFT($T146,6)=\"ACBL12\"), IF((soundLevel($T146, $AB146, BD146, $Y146, $W146,$AJ146,$AA146,\"NC\"))<15,\"<15\",soundLevel($T146, $AB146, BD146, $Y146, $W146,$AJ146,$AA146,\"NC\")+0.4),IF((soundLevel($T146, $AB146, BD146, $Y146, $W146,$AJ146,$AA146,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T146, $AB146, BD146, $Y146, $W146,$AJ146,$AA146,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T146, $AB146, BD146, $Y146, $W146,$AJ146,$AA146,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T146=\"Select Model\",\"\",IF($T146=\"LIU24_2W\",calcQwIP($Y146,$W146,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC146,$AI146,\"latent\",$U146&\"P\"&IF($V146=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T146,activeElevation),\"\"))","v":""},{"$f":"IF($T146=\"Select Model\",\"\",IF($T146=\"ACBC_1W\",calcQwIP($Y146,$W146,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC146,BD146,\"capacity\",$U146&\"P\"&IF($V146=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T146,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y146,$W146,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC146,BD146,\"capacity\",$U146&\"P\"&IF($V146=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T146,activeElevation)))","v":""},"",{"$f":"IF(T146=\"Select Model\", 0,waterPressureDrop(W146, U146 & \"P\" & IF(V146=\"Dual\",2,1) &\"C\", AC146, \"cooling\", T146))","v":0},{"$f":"IF(T146=\"Select Model\", \"\",getReturnWaterTemp(T146,AC146, activeEWTCooling, AS146, \"cooling\"))","v":""},"",{"$f":"IF($T146<>\"ACBC_1W\",\"\",IF($J146=\"\",\"\",FintubeCapacity($T146,$W146,$AE146,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T146=\"Select Model\",T146=\"PCBL\"),\"\",calcQwIP(Y146,W146,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD146,BD146,\"capacity\",U146&\"P\"&IF(V146=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T146,activeElevation))","v":""},"",{"$f":"IF(OR(T146=\"Select Model\",T146=\"PCBL\"), \"\",IF(AY146=0,\"N/A\",waterPressureDrop(W146, U146 & \"P\" & IF(V146=\"Dual\",2,1) &\"C\", AD146, \"heating\", T146)))","v":""},{"$f":"IF(OR(T146=\"Select Model\",T146=\"PCBL\"), \"\",IF(AY146=0,getReturnWaterTemp(T146,AE146, activeEWTHeating, AX146, \"heating\"),getReturnWaterTemp(T146,AD146, activeEWTHeating, AY146, \"heating\")))","v":""},"",{"$f":" getNozzle(T146, W146, Y146, Z146, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I147)),I147<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I147, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H147)),H147<0),\"\",intlEstQuantity(T147, W147*12, H147)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T147=\"Select Model\",\"\",coilCircuitChange(W147, U147, AC147, T147,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T147=\"Select Model\",\"\",beamWidth(T147))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T147=\"Select Model\",T147=\"PCBL\"), 0,getSPIP(T147, W147, Y147, BD147, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T147=\"Select Model\", \"\",IF(T147=\"PCBL\",0,primaryAirSensibleCapacityIP($T147,$W147,activeRoomTempCooling,activePriAirTempCooling,$Y147,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T147=\"Select Model\",\"\",IF($T147=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y147,activeElevation)))","v":""},{"$f":"IF(OR(T147=\"Select Model\",T147=\"PCBL\"), 0,IF(AD147=0,0,-primaryAirSensibleCapacityIP($T147,$W147,activeRoomTempHeating,activePriAirTempHeating,$Y147,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T147=\"Select Model\", \"\", InductionRatio($T147,BD147,$W147,$Y147)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T147=\"Select Model\", \"\",IF($T147=\"PCBL\",\"N/A\",minVAVSetBack(AA147, Y147))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T147=\"Select Model\", \"\",IF($T147= \"PCBL\",\"N/A\",getDischargeAirTemp($T147,$V147,$AC147,$W147,BD147,$AL147, $Y147, $AS147, \"cooling\",activeElevation,$AB147,$AJ147,$AV147,$BB147))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T147=\"Select Model\",$T147=\"PCBL\"), \"\",getDischargeAirTemp($T147,$V147,$AD147,$W147,BD147,$AL147, $Y147, $AY147, \"heating\",activeElevation,$AB147,$AJ147,$AV147,$BB147)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T147=\"Select Model\", \"\",IF(OR($T147=\"ACBC_1W\",$T147=\"ACBC_2W\",LEFT($T147,4)=\"ACBR\",$T147 = \"LIU24_2W\",LEFT($T147,3)=\"RIU\",LEFT($T147,6)=\"ACBL12\"), IF((soundLevel($T147, $AB147, BD147, $Y147, $W147,$AJ147,$AA147,\"dba\"))<15,\"<15\",soundLevel($T147, $AB147, BD147, $Y147, $W147,$AJ147,$AA147,\"dba\")+0.4),IF((soundLevel($T147, $AB147, BD147, $Y147, $W147,$AJ147,$AA147,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T147, $AB147, BD147, $Y147, $W147,$AJ147,$AA147,\"dba\")+5)<15, \"<15\", soundLevel($T147, $AB147, BD147,$Y147, $W147,$AJ147,$AA147,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T147=\"Select Model\", \"\",IF(OR($T147=\"ACBC_1W\",$T147=\"ACBC_2W\",LEFT($T147,4)=\"ACBR\",$T147=\"LIU24_2W\",LEFT($T147,3)=\"RIU\",LEFT($T147,6)=\"ACBL12\"), IF((soundLevel($T147, $AB147, BD147, $Y147, $W147,$AJ147,$AA147,\"NC\"))<15,\"<15\",soundLevel($T147, $AB147, BD147, $Y147, $W147,$AJ147,$AA147,\"NC\")+0.4),IF((soundLevel($T147, $AB147, BD147, $Y147, $W147,$AJ147,$AA147,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T147, $AB147, BD147, $Y147, $W147,$AJ147,$AA147,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T147, $AB147, BD147, $Y147, $W147,$AJ147,$AA147,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T147=\"Select Model\",\"\",IF($T147=\"LIU24_2W\",calcQwIP($Y147,$W147,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC147,$AI147,\"latent\",$U147&\"P\"&IF($V147=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T147,activeElevation),\"\"))","v":""},{"$f":"IF($T147=\"Select Model\",\"\",IF($T147=\"ACBC_1W\",calcQwIP($Y147,$W147,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC147,BD147,\"capacity\",$U147&\"P\"&IF($V147=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T147,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y147,$W147,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC147,BD147,\"capacity\",$U147&\"P\"&IF($V147=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T147,activeElevation)))","v":""},"",{"$f":"IF(T147=\"Select Model\", 0,waterPressureDrop(W147, U147 & \"P\" & IF(V147=\"Dual\",2,1) &\"C\", AC147, \"cooling\", T147))","v":0},{"$f":"IF(T147=\"Select Model\", \"\",getReturnWaterTemp(T147,AC147, activeEWTCooling, AS147, \"cooling\"))","v":""},"",{"$f":"IF($T147<>\"ACBC_1W\",\"\",IF($J147=\"\",\"\",FintubeCapacity($T147,$W147,$AE147,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T147=\"Select Model\",T147=\"PCBL\"),\"\",calcQwIP(Y147,W147,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD147,BD147,\"capacity\",U147&\"P\"&IF(V147=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T147,activeElevation))","v":""},"",{"$f":"IF(OR(T147=\"Select Model\",T147=\"PCBL\"), \"\",IF(AY147=0,\"N/A\",waterPressureDrop(W147, U147 & \"P\" & IF(V147=\"Dual\",2,1) &\"C\", AD147, \"heating\", T147)))","v":""},{"$f":"IF(OR(T147=\"Select Model\",T147=\"PCBL\"), \"\",IF(AY147=0,getReturnWaterTemp(T147,AE147, activeEWTHeating, AX147, \"heating\"),getReturnWaterTemp(T147,AD147, activeEWTHeating, AY147, \"heating\")))","v":""},"",{"$f":" getNozzle(T147, W147, Y147, Z147, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I148)),I148<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I148, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H148)),H148<0),\"\",intlEstQuantity(T148, W148*12, H148)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T148=\"Select Model\",\"\",coilCircuitChange(W148, U148, AC148, T148,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T148=\"Select Model\",\"\",beamWidth(T148))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T148=\"Select Model\",T148=\"PCBL\"), 0,getSPIP(T148, W148, Y148, BD148, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T148=\"Select Model\", \"\",IF(T148=\"PCBL\",0,primaryAirSensibleCapacityIP($T148,$W148,activeRoomTempCooling,activePriAirTempCooling,$Y148,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T148=\"Select Model\",\"\",IF($T148=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y148,activeElevation)))","v":""},{"$f":"IF(OR(T148=\"Select Model\",T148=\"PCBL\"), 0,IF(AD148=0,0,-primaryAirSensibleCapacityIP($T148,$W148,activeRoomTempHeating,activePriAirTempHeating,$Y148,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T148=\"Select Model\", \"\", InductionRatio($T148,BD148,$W148,$Y148)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T148=\"Select Model\", \"\",IF($T148=\"PCBL\",\"N/A\",minVAVSetBack(AA148, Y148))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T148=\"Select Model\", \"\",IF($T148= \"PCBL\",\"N/A\",getDischargeAirTemp($T148,$V148,$AC148,$W148,BD148,$AL148, $Y148, $AS148, \"cooling\",activeElevation,$AB148,$AJ148,$AV148,$BB148))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T148=\"Select Model\",$T148=\"PCBL\"), \"\",getDischargeAirTemp($T148,$V148,$AD148,$W148,BD148,$AL148, $Y148, $AY148, \"heating\",activeElevation,$AB148,$AJ148,$AV148,$BB148)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T148=\"Select Model\", \"\",IF(OR($T148=\"ACBC_1W\",$T148=\"ACBC_2W\",LEFT($T148,4)=\"ACBR\",$T148 = \"LIU24_2W\",LEFT($T148,3)=\"RIU\",LEFT($T148,6)=\"ACBL12\"), IF((soundLevel($T148, $AB148, BD148, $Y148, $W148,$AJ148,$AA148,\"dba\"))<15,\"<15\",soundLevel($T148, $AB148, BD148, $Y148, $W148,$AJ148,$AA148,\"dba\")+0.4),IF((soundLevel($T148, $AB148, BD148, $Y148, $W148,$AJ148,$AA148,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T148, $AB148, BD148, $Y148, $W148,$AJ148,$AA148,\"dba\")+5)<15, \"<15\", soundLevel($T148, $AB148, BD148,$Y148, $W148,$AJ148,$AA148,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T148=\"Select Model\", \"\",IF(OR($T148=\"ACBC_1W\",$T148=\"ACBC_2W\",LEFT($T148,4)=\"ACBR\",$T148=\"LIU24_2W\",LEFT($T148,3)=\"RIU\",LEFT($T148,6)=\"ACBL12\"), IF((soundLevel($T148, $AB148, BD148, $Y148, $W148,$AJ148,$AA148,\"NC\"))<15,\"<15\",soundLevel($T148, $AB148, BD148, $Y148, $W148,$AJ148,$AA148,\"NC\")+0.4),IF((soundLevel($T148, $AB148, BD148, $Y148, $W148,$AJ148,$AA148,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T148, $AB148, BD148, $Y148, $W148,$AJ148,$AA148,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T148, $AB148, BD148, $Y148, $W148,$AJ148,$AA148,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T148=\"Select Model\",\"\",IF($T148=\"LIU24_2W\",calcQwIP($Y148,$W148,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC148,$AI148,\"latent\",$U148&\"P\"&IF($V148=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T148,activeElevation),\"\"))","v":""},{"$f":"IF($T148=\"Select Model\",\"\",IF($T148=\"ACBC_1W\",calcQwIP($Y148,$W148,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC148,BD148,\"capacity\",$U148&\"P\"&IF($V148=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T148,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y148,$W148,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC148,BD148,\"capacity\",$U148&\"P\"&IF($V148=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T148,activeElevation)))","v":""},"",{"$f":"IF(T148=\"Select Model\", 0,waterPressureDrop(W148, U148 & \"P\" & IF(V148=\"Dual\",2,1) &\"C\", AC148, \"cooling\", T148))","v":0},{"$f":"IF(T148=\"Select Model\", \"\",getReturnWaterTemp(T148,AC148, activeEWTCooling, AS148, \"cooling\"))","v":""},"",{"$f":"IF($T148<>\"ACBC_1W\",\"\",IF($J148=\"\",\"\",FintubeCapacity($T148,$W148,$AE148,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T148=\"Select Model\",T148=\"PCBL\"),\"\",calcQwIP(Y148,W148,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD148,BD148,\"capacity\",U148&\"P\"&IF(V148=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T148,activeElevation))","v":""},"",{"$f":"IF(OR(T148=\"Select Model\",T148=\"PCBL\"), \"\",IF(AY148=0,\"N/A\",waterPressureDrop(W148, U148 & \"P\" & IF(V148=\"Dual\",2,1) &\"C\", AD148, \"heating\", T148)))","v":""},{"$f":"IF(OR(T148=\"Select Model\",T148=\"PCBL\"), \"\",IF(AY148=0,getReturnWaterTemp(T148,AE148, activeEWTHeating, AX148, \"heating\"),getReturnWaterTemp(T148,AD148, activeEWTHeating, AY148, \"heating\")))","v":""},"",{"$f":" getNozzle(T148, W148, Y148, Z148, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I149)),I149<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I149, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H149)),H149<0),\"\",intlEstQuantity(T149, W149*12, H149)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T149=\"Select Model\",\"\",coilCircuitChange(W149, U149, AC149, T149,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T149=\"Select Model\",\"\",beamWidth(T149))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T149=\"Select Model\",T149=\"PCBL\"), 0,getSPIP(T149, W149, Y149, BD149, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T149=\"Select Model\", \"\",IF(T149=\"PCBL\",0,primaryAirSensibleCapacityIP($T149,$W149,activeRoomTempCooling,activePriAirTempCooling,$Y149,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T149=\"Select Model\",\"\",IF($T149=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y149,activeElevation)))","v":""},{"$f":"IF(OR(T149=\"Select Model\",T149=\"PCBL\"), 0,IF(AD149=0,0,-primaryAirSensibleCapacityIP($T149,$W149,activeRoomTempHeating,activePriAirTempHeating,$Y149,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T149=\"Select Model\", \"\", InductionRatio($T149,BD149,$W149,$Y149)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T149=\"Select Model\", \"\",IF($T149=\"PCBL\",\"N/A\",minVAVSetBack(AA149, Y149))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T149=\"Select Model\", \"\",IF($T149= \"PCBL\",\"N/A\",getDischargeAirTemp($T149,$V149,$AC149,$W149,BD149,$AL149, $Y149, $AS149, \"cooling\",activeElevation,$AB149,$AJ149,$AV149,$BB149))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T149=\"Select Model\",$T149=\"PCBL\"), \"\",getDischargeAirTemp($T149,$V149,$AD149,$W149,BD149,$AL149, $Y149, $AY149, \"heating\",activeElevation,$AB149,$AJ149,$AV149,$BB149)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T149=\"Select Model\", \"\",IF(OR($T149=\"ACBC_1W\",$T149=\"ACBC_2W\",LEFT($T149,4)=\"ACBR\",$T149 = \"LIU24_2W\",LEFT($T149,3)=\"RIU\",LEFT($T149,6)=\"ACBL12\"), IF((soundLevel($T149, $AB149, BD149, $Y149, $W149,$AJ149,$AA149,\"dba\"))<15,\"<15\",soundLevel($T149, $AB149, BD149, $Y149, $W149,$AJ149,$AA149,\"dba\")+0.4),IF((soundLevel($T149, $AB149, BD149, $Y149, $W149,$AJ149,$AA149,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T149, $AB149, BD149, $Y149, $W149,$AJ149,$AA149,\"dba\")+5)<15, \"<15\", soundLevel($T149, $AB149, BD149,$Y149, $W149,$AJ149,$AA149,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T149=\"Select Model\", \"\",IF(OR($T149=\"ACBC_1W\",$T149=\"ACBC_2W\",LEFT($T149,4)=\"ACBR\",$T149=\"LIU24_2W\",LEFT($T149,3)=\"RIU\",LEFT($T149,6)=\"ACBL12\"), IF((soundLevel($T149, $AB149, BD149, $Y149, $W149,$AJ149,$AA149,\"NC\"))<15,\"<15\",soundLevel($T149, $AB149, BD149, $Y149, $W149,$AJ149,$AA149,\"NC\")+0.4),IF((soundLevel($T149, $AB149, BD149, $Y149, $W149,$AJ149,$AA149,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T149, $AB149, BD149, $Y149, $W149,$AJ149,$AA149,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T149, $AB149, BD149, $Y149, $W149,$AJ149,$AA149,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T149=\"Select Model\",\"\",IF($T149=\"LIU24_2W\",calcQwIP($Y149,$W149,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC149,$AI149,\"latent\",$U149&\"P\"&IF($V149=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T149,activeElevation),\"\"))","v":""},{"$f":"IF($T149=\"Select Model\",\"\",IF($T149=\"ACBC_1W\",calcQwIP($Y149,$W149,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC149,BD149,\"capacity\",$U149&\"P\"&IF($V149=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T149,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y149,$W149,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC149,BD149,\"capacity\",$U149&\"P\"&IF($V149=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T149,activeElevation)))","v":""},"",{"$f":"IF(T149=\"Select Model\", 0,waterPressureDrop(W149, U149 & \"P\" & IF(V149=\"Dual\",2,1) &\"C\", AC149, \"cooling\", T149))","v":0},{"$f":"IF(T149=\"Select Model\", \"\",getReturnWaterTemp(T149,AC149, activeEWTCooling, AS149, \"cooling\"))","v":""},"",{"$f":"IF($T149<>\"ACBC_1W\",\"\",IF($J149=\"\",\"\",FintubeCapacity($T149,$W149,$AE149,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T149=\"Select Model\",T149=\"PCBL\"),\"\",calcQwIP(Y149,W149,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD149,BD149,\"capacity\",U149&\"P\"&IF(V149=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T149,activeElevation))","v":""},"",{"$f":"IF(OR(T149=\"Select Model\",T149=\"PCBL\"), \"\",IF(AY149=0,\"N/A\",waterPressureDrop(W149, U149 & \"P\" & IF(V149=\"Dual\",2,1) &\"C\", AD149, \"heating\", T149)))","v":""},{"$f":"IF(OR(T149=\"Select Model\",T149=\"PCBL\"), \"\",IF(AY149=0,getReturnWaterTemp(T149,AE149, activeEWTHeating, AX149, \"heating\"),getReturnWaterTemp(T149,AD149, activeEWTHeating, AY149, \"heating\")))","v":""},"",{"$f":" getNozzle(T149, W149, Y149, Z149, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I150)),I150<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I150, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H150)),H150<0),\"\",intlEstQuantity(T150, W150*12, H150)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T150=\"Select Model\",\"\",coilCircuitChange(W150, U150, AC150, T150,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T150=\"Select Model\",\"\",beamWidth(T150))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T150=\"Select Model\",T150=\"PCBL\"), 0,getSPIP(T150, W150, Y150, BD150, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T150=\"Select Model\", \"\",IF(T150=\"PCBL\",0,primaryAirSensibleCapacityIP($T150,$W150,activeRoomTempCooling,activePriAirTempCooling,$Y150,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T150=\"Select Model\",\"\",IF($T150=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y150,activeElevation)))","v":""},{"$f":"IF(OR(T150=\"Select Model\",T150=\"PCBL\"), 0,IF(AD150=0,0,-primaryAirSensibleCapacityIP($T150,$W150,activeRoomTempHeating,activePriAirTempHeating,$Y150,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T150=\"Select Model\", \"\", InductionRatio($T150,BD150,$W150,$Y150)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T150=\"Select Model\", \"\",IF($T150=\"PCBL\",\"N/A\",minVAVSetBack(AA150, Y150))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T150=\"Select Model\", \"\",IF($T150= \"PCBL\",\"N/A\",getDischargeAirTemp($T150,$V150,$AC150,$W150,BD150,$AL150, $Y150, $AS150, \"cooling\",activeElevation,$AB150,$AJ150,$AV150,$BB150))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T150=\"Select Model\",$T150=\"PCBL\"), \"\",getDischargeAirTemp($T150,$V150,$AD150,$W150,BD150,$AL150, $Y150, $AY150, \"heating\",activeElevation,$AB150,$AJ150,$AV150,$BB150)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T150=\"Select Model\", \"\",IF(OR($T150=\"ACBC_1W\",$T150=\"ACBC_2W\",LEFT($T150,4)=\"ACBR\",$T150 = \"LIU24_2W\",LEFT($T150,3)=\"RIU\",LEFT($T150,6)=\"ACBL12\"), IF((soundLevel($T150, $AB150, BD150, $Y150, $W150,$AJ150,$AA150,\"dba\"))<15,\"<15\",soundLevel($T150, $AB150, BD150, $Y150, $W150,$AJ150,$AA150,\"dba\")+0.4),IF((soundLevel($T150, $AB150, BD150, $Y150, $W150,$AJ150,$AA150,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T150, $AB150, BD150, $Y150, $W150,$AJ150,$AA150,\"dba\")+5)<15, \"<15\", soundLevel($T150, $AB150, BD150,$Y150, $W150,$AJ150,$AA150,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T150=\"Select Model\", \"\",IF(OR($T150=\"ACBC_1W\",$T150=\"ACBC_2W\",LEFT($T150,4)=\"ACBR\",$T150=\"LIU24_2W\",LEFT($T150,3)=\"RIU\",LEFT($T150,6)=\"ACBL12\"), IF((soundLevel($T150, $AB150, BD150, $Y150, $W150,$AJ150,$AA150,\"NC\"))<15,\"<15\",soundLevel($T150, $AB150, BD150, $Y150, $W150,$AJ150,$AA150,\"NC\")+0.4),IF((soundLevel($T150, $AB150, BD150, $Y150, $W150,$AJ150,$AA150,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T150, $AB150, BD150, $Y150, $W150,$AJ150,$AA150,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T150, $AB150, BD150, $Y150, $W150,$AJ150,$AA150,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T150=\"Select Model\",\"\",IF($T150=\"LIU24_2W\",calcQwIP($Y150,$W150,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC150,$AI150,\"latent\",$U150&\"P\"&IF($V150=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T150,activeElevation),\"\"))","v":""},{"$f":"IF($T150=\"Select Model\",\"\",IF($T150=\"ACBC_1W\",calcQwIP($Y150,$W150,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC150,BD150,\"capacity\",$U150&\"P\"&IF($V150=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T150,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y150,$W150,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC150,BD150,\"capacity\",$U150&\"P\"&IF($V150=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T150,activeElevation)))","v":""},"",{"$f":"IF(T150=\"Select Model\", 0,waterPressureDrop(W150, U150 & \"P\" & IF(V150=\"Dual\",2,1) &\"C\", AC150, \"cooling\", T150))","v":0},{"$f":"IF(T150=\"Select Model\", \"\",getReturnWaterTemp(T150,AC150, activeEWTCooling, AS150, \"cooling\"))","v":""},"",{"$f":"IF($T150<>\"ACBC_1W\",\"\",IF($J150=\"\",\"\",FintubeCapacity($T150,$W150,$AE150,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T150=\"Select Model\",T150=\"PCBL\"),\"\",calcQwIP(Y150,W150,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD150,BD150,\"capacity\",U150&\"P\"&IF(V150=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T150,activeElevation))","v":""},"",{"$f":"IF(OR(T150=\"Select Model\",T150=\"PCBL\"), \"\",IF(AY150=0,\"N/A\",waterPressureDrop(W150, U150 & \"P\" & IF(V150=\"Dual\",2,1) &\"C\", AD150, \"heating\", T150)))","v":""},{"$f":"IF(OR(T150=\"Select Model\",T150=\"PCBL\"), \"\",IF(AY150=0,getReturnWaterTemp(T150,AE150, activeEWTHeating, AX150, \"heating\"),getReturnWaterTemp(T150,AD150, activeEWTHeating, AY150, \"heating\")))","v":""},"",{"$f":" getNozzle(T150, W150, Y150, Z150, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I151)),I151<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I151, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H151)),H151<0),\"\",intlEstQuantity(T151, W151*12, H151)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T151=\"Select Model\",\"\",coilCircuitChange(W151, U151, AC151, T151,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T151=\"Select Model\",\"\",beamWidth(T151))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T151=\"Select Model\",T151=\"PCBL\"), 0,getSPIP(T151, W151, Y151, BD151, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T151=\"Select Model\", \"\",IF(T151=\"PCBL\",0,primaryAirSensibleCapacityIP($T151,$W151,activeRoomTempCooling,activePriAirTempCooling,$Y151,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T151=\"Select Model\",\"\",IF($T151=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y151,activeElevation)))","v":""},{"$f":"IF(OR(T151=\"Select Model\",T151=\"PCBL\"), 0,IF(AD151=0,0,-primaryAirSensibleCapacityIP($T151,$W151,activeRoomTempHeating,activePriAirTempHeating,$Y151,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T151=\"Select Model\", \"\", InductionRatio($T151,BD151,$W151,$Y151)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T151=\"Select Model\", \"\",IF($T151=\"PCBL\",\"N/A\",minVAVSetBack(AA151, Y151))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T151=\"Select Model\", \"\",IF($T151= \"PCBL\",\"N/A\",getDischargeAirTemp($T151,$V151,$AC151,$W151,BD151,$AL151, $Y151, $AS151, \"cooling\",activeElevation,$AB151,$AJ151,$AV151,$BB151))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T151=\"Select Model\",$T151=\"PCBL\"), \"\",getDischargeAirTemp($T151,$V151,$AD151,$W151,BD151,$AL151, $Y151, $AY151, \"heating\",activeElevation,$AB151,$AJ151,$AV151,$BB151)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T151=\"Select Model\", \"\",IF(OR($T151=\"ACBC_1W\",$T151=\"ACBC_2W\",LEFT($T151,4)=\"ACBR\",$T151 = \"LIU24_2W\",LEFT($T151,3)=\"RIU\",LEFT($T151,6)=\"ACBL12\"), IF((soundLevel($T151, $AB151, BD151, $Y151, $W151,$AJ151,$AA151,\"dba\"))<15,\"<15\",soundLevel($T151, $AB151, BD151, $Y151, $W151,$AJ151,$AA151,\"dba\")+0.4),IF((soundLevel($T151, $AB151, BD151, $Y151, $W151,$AJ151,$AA151,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T151, $AB151, BD151, $Y151, $W151,$AJ151,$AA151,\"dba\")+5)<15, \"<15\", soundLevel($T151, $AB151, BD151,$Y151, $W151,$AJ151,$AA151,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T151=\"Select Model\", \"\",IF(OR($T151=\"ACBC_1W\",$T151=\"ACBC_2W\",LEFT($T151,4)=\"ACBR\",$T151=\"LIU24_2W\",LEFT($T151,3)=\"RIU\",LEFT($T151,6)=\"ACBL12\"), IF((soundLevel($T151, $AB151, BD151, $Y151, $W151,$AJ151,$AA151,\"NC\"))<15,\"<15\",soundLevel($T151, $AB151, BD151, $Y151, $W151,$AJ151,$AA151,\"NC\")+0.4),IF((soundLevel($T151, $AB151, BD151, $Y151, $W151,$AJ151,$AA151,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T151, $AB151, BD151, $Y151, $W151,$AJ151,$AA151,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T151, $AB151, BD151, $Y151, $W151,$AJ151,$AA151,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T151=\"Select Model\",\"\",IF($T151=\"LIU24_2W\",calcQwIP($Y151,$W151,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC151,$AI151,\"latent\",$U151&\"P\"&IF($V151=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T151,activeElevation),\"\"))","v":""},{"$f":"IF($T151=\"Select Model\",\"\",IF($T151=\"ACBC_1W\",calcQwIP($Y151,$W151,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC151,BD151,\"capacity\",$U151&\"P\"&IF($V151=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T151,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y151,$W151,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC151,BD151,\"capacity\",$U151&\"P\"&IF($V151=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T151,activeElevation)))","v":""},"",{"$f":"IF(T151=\"Select Model\", 0,waterPressureDrop(W151, U151 & \"P\" & IF(V151=\"Dual\",2,1) &\"C\", AC151, \"cooling\", T151))","v":0},{"$f":"IF(T151=\"Select Model\", \"\",getReturnWaterTemp(T151,AC151, activeEWTCooling, AS151, \"cooling\"))","v":""},"",{"$f":"IF($T151<>\"ACBC_1W\",\"\",IF($J151=\"\",\"\",FintubeCapacity($T151,$W151,$AE151,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T151=\"Select Model\",T151=\"PCBL\"),\"\",calcQwIP(Y151,W151,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD151,BD151,\"capacity\",U151&\"P\"&IF(V151=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T151,activeElevation))","v":""},"",{"$f":"IF(OR(T151=\"Select Model\",T151=\"PCBL\"), \"\",IF(AY151=0,\"N/A\",waterPressureDrop(W151, U151 & \"P\" & IF(V151=\"Dual\",2,1) &\"C\", AD151, \"heating\", T151)))","v":""},{"$f":"IF(OR(T151=\"Select Model\",T151=\"PCBL\"), \"\",IF(AY151=0,getReturnWaterTemp(T151,AE151, activeEWTHeating, AX151, \"heating\"),getReturnWaterTemp(T151,AD151, activeEWTHeating, AY151, \"heating\")))","v":""},"",{"$f":" getNozzle(T151, W151, Y151, Z151, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I152)),I152<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I152, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H152)),H152<0),\"\",intlEstQuantity(T152, W152*12, H152)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T152=\"Select Model\",\"\",coilCircuitChange(W152, U152, AC152, T152,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T152=\"Select Model\",\"\",beamWidth(T152))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T152=\"Select Model\",T152=\"PCBL\"), 0,getSPIP(T152, W152, Y152, BD152, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T152=\"Select Model\", \"\",IF(T152=\"PCBL\",0,primaryAirSensibleCapacityIP($T152,$W152,activeRoomTempCooling,activePriAirTempCooling,$Y152,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T152=\"Select Model\",\"\",IF($T152=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y152,activeElevation)))","v":""},{"$f":"IF(OR(T152=\"Select Model\",T152=\"PCBL\"), 0,IF(AD152=0,0,-primaryAirSensibleCapacityIP($T152,$W152,activeRoomTempHeating,activePriAirTempHeating,$Y152,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T152=\"Select Model\", \"\", InductionRatio($T152,BD152,$W152,$Y152)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T152=\"Select Model\", \"\",IF($T152=\"PCBL\",\"N/A\",minVAVSetBack(AA152, Y152))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T152=\"Select Model\", \"\",IF($T152= \"PCBL\",\"N/A\",getDischargeAirTemp($T152,$V152,$AC152,$W152,BD152,$AL152, $Y152, $AS152, \"cooling\",activeElevation,$AB152,$AJ152,$AV152,$BB152))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T152=\"Select Model\",$T152=\"PCBL\"), \"\",getDischargeAirTemp($T152,$V152,$AD152,$W152,BD152,$AL152, $Y152, $AY152, \"heating\",activeElevation,$AB152,$AJ152,$AV152,$BB152)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T152=\"Select Model\", \"\",IF(OR($T152=\"ACBC_1W\",$T152=\"ACBC_2W\",LEFT($T152,4)=\"ACBR\",$T152 = \"LIU24_2W\",LEFT($T152,3)=\"RIU\",LEFT($T152,6)=\"ACBL12\"), IF((soundLevel($T152, $AB152, BD152, $Y152, $W152,$AJ152,$AA152,\"dba\"))<15,\"<15\",soundLevel($T152, $AB152, BD152, $Y152, $W152,$AJ152,$AA152,\"dba\")+0.4),IF((soundLevel($T152, $AB152, BD152, $Y152, $W152,$AJ152,$AA152,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T152, $AB152, BD152, $Y152, $W152,$AJ152,$AA152,\"dba\")+5)<15, \"<15\", soundLevel($T152, $AB152, BD152,$Y152, $W152,$AJ152,$AA152,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T152=\"Select Model\", \"\",IF(OR($T152=\"ACBC_1W\",$T152=\"ACBC_2W\",LEFT($T152,4)=\"ACBR\",$T152=\"LIU24_2W\",LEFT($T152,3)=\"RIU\",LEFT($T152,6)=\"ACBL12\"), IF((soundLevel($T152, $AB152, BD152, $Y152, $W152,$AJ152,$AA152,\"NC\"))<15,\"<15\",soundLevel($T152, $AB152, BD152, $Y152, $W152,$AJ152,$AA152,\"NC\")+0.4),IF((soundLevel($T152, $AB152, BD152, $Y152, $W152,$AJ152,$AA152,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T152, $AB152, BD152, $Y152, $W152,$AJ152,$AA152,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T152, $AB152, BD152, $Y152, $W152,$AJ152,$AA152,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T152=\"Select Model\",\"\",IF($T152=\"LIU24_2W\",calcQwIP($Y152,$W152,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC152,$AI152,\"latent\",$U152&\"P\"&IF($V152=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T152,activeElevation),\"\"))","v":""},{"$f":"IF($T152=\"Select Model\",\"\",IF($T152=\"ACBC_1W\",calcQwIP($Y152,$W152,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC152,BD152,\"capacity\",$U152&\"P\"&IF($V152=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T152,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y152,$W152,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC152,BD152,\"capacity\",$U152&\"P\"&IF($V152=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T152,activeElevation)))","v":""},"",{"$f":"IF(T152=\"Select Model\", 0,waterPressureDrop(W152, U152 & \"P\" & IF(V152=\"Dual\",2,1) &\"C\", AC152, \"cooling\", T152))","v":0},{"$f":"IF(T152=\"Select Model\", \"\",getReturnWaterTemp(T152,AC152, activeEWTCooling, AS152, \"cooling\"))","v":""},"",{"$f":"IF($T152<>\"ACBC_1W\",\"\",IF($J152=\"\",\"\",FintubeCapacity($T152,$W152,$AE152,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T152=\"Select Model\",T152=\"PCBL\"),\"\",calcQwIP(Y152,W152,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD152,BD152,\"capacity\",U152&\"P\"&IF(V152=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T152,activeElevation))","v":""},"",{"$f":"IF(OR(T152=\"Select Model\",T152=\"PCBL\"), \"\",IF(AY152=0,\"N/A\",waterPressureDrop(W152, U152 & \"P\" & IF(V152=\"Dual\",2,1) &\"C\", AD152, \"heating\", T152)))","v":""},{"$f":"IF(OR(T152=\"Select Model\",T152=\"PCBL\"), \"\",IF(AY152=0,getReturnWaterTemp(T152,AE152, activeEWTHeating, AX152, \"heating\"),getReturnWaterTemp(T152,AD152, activeEWTHeating, AY152, \"heating\")))","v":""},"",{"$f":" getNozzle(T152, W152, Y152, Z152, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I153)),I153<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I153, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H153)),H153<0),\"\",intlEstQuantity(T153, W153*12, H153)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T153=\"Select Model\",\"\",coilCircuitChange(W153, U153, AC153, T153,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T153=\"Select Model\",\"\",beamWidth(T153))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T153=\"Select Model\",T153=\"PCBL\"), 0,getSPIP(T153, W153, Y153, BD153, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T153=\"Select Model\", \"\",IF(T153=\"PCBL\",0,primaryAirSensibleCapacityIP($T153,$W153,activeRoomTempCooling,activePriAirTempCooling,$Y153,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T153=\"Select Model\",\"\",IF($T153=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y153,activeElevation)))","v":""},{"$f":"IF(OR(T153=\"Select Model\",T153=\"PCBL\"), 0,IF(AD153=0,0,-primaryAirSensibleCapacityIP($T153,$W153,activeRoomTempHeating,activePriAirTempHeating,$Y153,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T153=\"Select Model\", \"\", InductionRatio($T153,BD153,$W153,$Y153)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T153=\"Select Model\", \"\",IF($T153=\"PCBL\",\"N/A\",minVAVSetBack(AA153, Y153))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T153=\"Select Model\", \"\",IF($T153= \"PCBL\",\"N/A\",getDischargeAirTemp($T153,$V153,$AC153,$W153,BD153,$AL153, $Y153, $AS153, \"cooling\",activeElevation,$AB153,$AJ153,$AV153,$BB153))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T153=\"Select Model\",$T153=\"PCBL\"), \"\",getDischargeAirTemp($T153,$V153,$AD153,$W153,BD153,$AL153, $Y153, $AY153, \"heating\",activeElevation,$AB153,$AJ153,$AV153,$BB153)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T153=\"Select Model\", \"\",IF(OR($T153=\"ACBC_1W\",$T153=\"ACBC_2W\",LEFT($T153,4)=\"ACBR\",$T153 = \"LIU24_2W\",LEFT($T153,3)=\"RIU\",LEFT($T153,6)=\"ACBL12\"), IF((soundLevel($T153, $AB153, BD153, $Y153, $W153,$AJ153,$AA153,\"dba\"))<15,\"<15\",soundLevel($T153, $AB153, BD153, $Y153, $W153,$AJ153,$AA153,\"dba\")+0.4),IF((soundLevel($T153, $AB153, BD153, $Y153, $W153,$AJ153,$AA153,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T153, $AB153, BD153, $Y153, $W153,$AJ153,$AA153,\"dba\")+5)<15, \"<15\", soundLevel($T153, $AB153, BD153,$Y153, $W153,$AJ153,$AA153,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T153=\"Select Model\", \"\",IF(OR($T153=\"ACBC_1W\",$T153=\"ACBC_2W\",LEFT($T153,4)=\"ACBR\",$T153=\"LIU24_2W\",LEFT($T153,3)=\"RIU\",LEFT($T153,6)=\"ACBL12\"), IF((soundLevel($T153, $AB153, BD153, $Y153, $W153,$AJ153,$AA153,\"NC\"))<15,\"<15\",soundLevel($T153, $AB153, BD153, $Y153, $W153,$AJ153,$AA153,\"NC\")+0.4),IF((soundLevel($T153, $AB153, BD153, $Y153, $W153,$AJ153,$AA153,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T153, $AB153, BD153, $Y153, $W153,$AJ153,$AA153,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T153, $AB153, BD153, $Y153, $W153,$AJ153,$AA153,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T153=\"Select Model\",\"\",IF($T153=\"LIU24_2W\",calcQwIP($Y153,$W153,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC153,$AI153,\"latent\",$U153&\"P\"&IF($V153=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T153,activeElevation),\"\"))","v":""},{"$f":"IF($T153=\"Select Model\",\"\",IF($T153=\"ACBC_1W\",calcQwIP($Y153,$W153,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC153,BD153,\"capacity\",$U153&\"P\"&IF($V153=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T153,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y153,$W153,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC153,BD153,\"capacity\",$U153&\"P\"&IF($V153=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T153,activeElevation)))","v":""},"",{"$f":"IF(T153=\"Select Model\", 0,waterPressureDrop(W153, U153 & \"P\" & IF(V153=\"Dual\",2,1) &\"C\", AC153, \"cooling\", T153))","v":0},{"$f":"IF(T153=\"Select Model\", \"\",getReturnWaterTemp(T153,AC153, activeEWTCooling, AS153, \"cooling\"))","v":""},"",{"$f":"IF($T153<>\"ACBC_1W\",\"\",IF($J153=\"\",\"\",FintubeCapacity($T153,$W153,$AE153,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T153=\"Select Model\",T153=\"PCBL\"),\"\",calcQwIP(Y153,W153,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD153,BD153,\"capacity\",U153&\"P\"&IF(V153=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T153,activeElevation))","v":""},"",{"$f":"IF(OR(T153=\"Select Model\",T153=\"PCBL\"), \"\",IF(AY153=0,\"N/A\",waterPressureDrop(W153, U153 & \"P\" & IF(V153=\"Dual\",2,1) &\"C\", AD153, \"heating\", T153)))","v":""},{"$f":"IF(OR(T153=\"Select Model\",T153=\"PCBL\"), \"\",IF(AY153=0,getReturnWaterTemp(T153,AE153, activeEWTHeating, AX153, \"heating\"),getReturnWaterTemp(T153,AD153, activeEWTHeating, AY153, \"heating\")))","v":""},"",{"$f":" getNozzle(T153, W153, Y153, Z153, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I154)),I154<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I154, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H154)),H154<0),\"\",intlEstQuantity(T154, W154*12, H154)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T154=\"Select Model\",\"\",coilCircuitChange(W154, U154, AC154, T154,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T154=\"Select Model\",\"\",beamWidth(T154))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T154=\"Select Model\",T154=\"PCBL\"), 0,getSPIP(T154, W154, Y154, BD154, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T154=\"Select Model\", \"\",IF(T154=\"PCBL\",0,primaryAirSensibleCapacityIP($T154,$W154,activeRoomTempCooling,activePriAirTempCooling,$Y154,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T154=\"Select Model\",\"\",IF($T154=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y154,activeElevation)))","v":""},{"$f":"IF(OR(T154=\"Select Model\",T154=\"PCBL\"), 0,IF(AD154=0,0,-primaryAirSensibleCapacityIP($T154,$W154,activeRoomTempHeating,activePriAirTempHeating,$Y154,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T154=\"Select Model\", \"\", InductionRatio($T154,BD154,$W154,$Y154)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T154=\"Select Model\", \"\",IF($T154=\"PCBL\",\"N/A\",minVAVSetBack(AA154, Y154))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T154=\"Select Model\", \"\",IF($T154= \"PCBL\",\"N/A\",getDischargeAirTemp($T154,$V154,$AC154,$W154,BD154,$AL154, $Y154, $AS154, \"cooling\",activeElevation,$AB154,$AJ154,$AV154,$BB154))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T154=\"Select Model\",$T154=\"PCBL\"), \"\",getDischargeAirTemp($T154,$V154,$AD154,$W154,BD154,$AL154, $Y154, $AY154, \"heating\",activeElevation,$AB154,$AJ154,$AV154,$BB154)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T154=\"Select Model\", \"\",IF(OR($T154=\"ACBC_1W\",$T154=\"ACBC_2W\",LEFT($T154,4)=\"ACBR\",$T154 = \"LIU24_2W\",LEFT($T154,3)=\"RIU\",LEFT($T154,6)=\"ACBL12\"), IF((soundLevel($T154, $AB154, BD154, $Y154, $W154,$AJ154,$AA154,\"dba\"))<15,\"<15\",soundLevel($T154, $AB154, BD154, $Y154, $W154,$AJ154,$AA154,\"dba\")+0.4),IF((soundLevel($T154, $AB154, BD154, $Y154, $W154,$AJ154,$AA154,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T154, $AB154, BD154, $Y154, $W154,$AJ154,$AA154,\"dba\")+5)<15, \"<15\", soundLevel($T154, $AB154, BD154,$Y154, $W154,$AJ154,$AA154,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T154=\"Select Model\", \"\",IF(OR($T154=\"ACBC_1W\",$T154=\"ACBC_2W\",LEFT($T154,4)=\"ACBR\",$T154=\"LIU24_2W\",LEFT($T154,3)=\"RIU\",LEFT($T154,6)=\"ACBL12\"), IF((soundLevel($T154, $AB154, BD154, $Y154, $W154,$AJ154,$AA154,\"NC\"))<15,\"<15\",soundLevel($T154, $AB154, BD154, $Y154, $W154,$AJ154,$AA154,\"NC\")+0.4),IF((soundLevel($T154, $AB154, BD154, $Y154, $W154,$AJ154,$AA154,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T154, $AB154, BD154, $Y154, $W154,$AJ154,$AA154,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T154, $AB154, BD154, $Y154, $W154,$AJ154,$AA154,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T154=\"Select Model\",\"\",IF($T154=\"LIU24_2W\",calcQwIP($Y154,$W154,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC154,$AI154,\"latent\",$U154&\"P\"&IF($V154=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T154,activeElevation),\"\"))","v":""},{"$f":"IF($T154=\"Select Model\",\"\",IF($T154=\"ACBC_1W\",calcQwIP($Y154,$W154,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC154,BD154,\"capacity\",$U154&\"P\"&IF($V154=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T154,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y154,$W154,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC154,BD154,\"capacity\",$U154&\"P\"&IF($V154=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T154,activeElevation)))","v":""},"",{"$f":"IF(T154=\"Select Model\", 0,waterPressureDrop(W154, U154 & \"P\" & IF(V154=\"Dual\",2,1) &\"C\", AC154, \"cooling\", T154))","v":0},{"$f":"IF(T154=\"Select Model\", \"\",getReturnWaterTemp(T154,AC154, activeEWTCooling, AS154, \"cooling\"))","v":""},"",{"$f":"IF($T154<>\"ACBC_1W\",\"\",IF($J154=\"\",\"\",FintubeCapacity($T154,$W154,$AE154,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T154=\"Select Model\",T154=\"PCBL\"),\"\",calcQwIP(Y154,W154,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD154,BD154,\"capacity\",U154&\"P\"&IF(V154=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T154,activeElevation))","v":""},"",{"$f":"IF(OR(T154=\"Select Model\",T154=\"PCBL\"), \"\",IF(AY154=0,\"N/A\",waterPressureDrop(W154, U154 & \"P\" & IF(V154=\"Dual\",2,1) &\"C\", AD154, \"heating\", T154)))","v":""},{"$f":"IF(OR(T154=\"Select Model\",T154=\"PCBL\"), \"\",IF(AY154=0,getReturnWaterTemp(T154,AE154, activeEWTHeating, AX154, \"heating\"),getReturnWaterTemp(T154,AD154, activeEWTHeating, AY154, \"heating\")))","v":""},"",{"$f":" getNozzle(T154, W154, Y154, Z154, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I155)),I155<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I155, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H155)),H155<0),\"\",intlEstQuantity(T155, W155*12, H155)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T155=\"Select Model\",\"\",coilCircuitChange(W155, U155, AC155, T155,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T155=\"Select Model\",\"\",beamWidth(T155))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T155=\"Select Model\",T155=\"PCBL\"), 0,getSPIP(T155, W155, Y155, BD155, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T155=\"Select Model\", \"\",IF(T155=\"PCBL\",0,primaryAirSensibleCapacityIP($T155,$W155,activeRoomTempCooling,activePriAirTempCooling,$Y155,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T155=\"Select Model\",\"\",IF($T155=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y155,activeElevation)))","v":""},{"$f":"IF(OR(T155=\"Select Model\",T155=\"PCBL\"), 0,IF(AD155=0,0,-primaryAirSensibleCapacityIP($T155,$W155,activeRoomTempHeating,activePriAirTempHeating,$Y155,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T155=\"Select Model\", \"\", InductionRatio($T155,BD155,$W155,$Y155)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T155=\"Select Model\", \"\",IF($T155=\"PCBL\",\"N/A\",minVAVSetBack(AA155, Y155))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T155=\"Select Model\", \"\",IF($T155= \"PCBL\",\"N/A\",getDischargeAirTemp($T155,$V155,$AC155,$W155,BD155,$AL155, $Y155, $AS155, \"cooling\",activeElevation,$AB155,$AJ155,$AV155,$BB155))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T155=\"Select Model\",$T155=\"PCBL\"), \"\",getDischargeAirTemp($T155,$V155,$AD155,$W155,BD155,$AL155, $Y155, $AY155, \"heating\",activeElevation,$AB155,$AJ155,$AV155,$BB155)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T155=\"Select Model\", \"\",IF(OR($T155=\"ACBC_1W\",$T155=\"ACBC_2W\",LEFT($T155,4)=\"ACBR\",$T155 = \"LIU24_2W\",LEFT($T155,3)=\"RIU\",LEFT($T155,6)=\"ACBL12\"), IF((soundLevel($T155, $AB155, BD155, $Y155, $W155,$AJ155,$AA155,\"dba\"))<15,\"<15\",soundLevel($T155, $AB155, BD155, $Y155, $W155,$AJ155,$AA155,\"dba\")+0.4),IF((soundLevel($T155, $AB155, BD155, $Y155, $W155,$AJ155,$AA155,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T155, $AB155, BD155, $Y155, $W155,$AJ155,$AA155,\"dba\")+5)<15, \"<15\", soundLevel($T155, $AB155, BD155,$Y155, $W155,$AJ155,$AA155,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T155=\"Select Model\", \"\",IF(OR($T155=\"ACBC_1W\",$T155=\"ACBC_2W\",LEFT($T155,4)=\"ACBR\",$T155=\"LIU24_2W\",LEFT($T155,3)=\"RIU\",LEFT($T155,6)=\"ACBL12\"), IF((soundLevel($T155, $AB155, BD155, $Y155, $W155,$AJ155,$AA155,\"NC\"))<15,\"<15\",soundLevel($T155, $AB155, BD155, $Y155, $W155,$AJ155,$AA155,\"NC\")+0.4),IF((soundLevel($T155, $AB155, BD155, $Y155, $W155,$AJ155,$AA155,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T155, $AB155, BD155, $Y155, $W155,$AJ155,$AA155,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T155, $AB155, BD155, $Y155, $W155,$AJ155,$AA155,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T155=\"Select Model\",\"\",IF($T155=\"LIU24_2W\",calcQwIP($Y155,$W155,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC155,$AI155,\"latent\",$U155&\"P\"&IF($V155=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T155,activeElevation),\"\"))","v":""},{"$f":"IF($T155=\"Select Model\",\"\",IF($T155=\"ACBC_1W\",calcQwIP($Y155,$W155,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC155,BD155,\"capacity\",$U155&\"P\"&IF($V155=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T155,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y155,$W155,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC155,BD155,\"capacity\",$U155&\"P\"&IF($V155=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T155,activeElevation)))","v":""},"",{"$f":"IF(T155=\"Select Model\", 0,waterPressureDrop(W155, U155 & \"P\" & IF(V155=\"Dual\",2,1) &\"C\", AC155, \"cooling\", T155))","v":0},{"$f":"IF(T155=\"Select Model\", \"\",getReturnWaterTemp(T155,AC155, activeEWTCooling, AS155, \"cooling\"))","v":""},"",{"$f":"IF($T155<>\"ACBC_1W\",\"\",IF($J155=\"\",\"\",FintubeCapacity($T155,$W155,$AE155,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T155=\"Select Model\",T155=\"PCBL\"),\"\",calcQwIP(Y155,W155,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD155,BD155,\"capacity\",U155&\"P\"&IF(V155=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T155,activeElevation))","v":""},"",{"$f":"IF(OR(T155=\"Select Model\",T155=\"PCBL\"), \"\",IF(AY155=0,\"N/A\",waterPressureDrop(W155, U155 & \"P\" & IF(V155=\"Dual\",2,1) &\"C\", AD155, \"heating\", T155)))","v":""},{"$f":"IF(OR(T155=\"Select Model\",T155=\"PCBL\"), \"\",IF(AY155=0,getReturnWaterTemp(T155,AE155, activeEWTHeating, AX155, \"heating\"),getReturnWaterTemp(T155,AD155, activeEWTHeating, AY155, \"heating\")))","v":""},"",{"$f":" getNozzle(T155, W155, Y155, Z155, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I156)),I156<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I156, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H156)),H156<0),\"\",intlEstQuantity(T156, W156*12, H156)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T156=\"Select Model\",\"\",coilCircuitChange(W156, U156, AC156, T156,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T156=\"Select Model\",\"\",beamWidth(T156))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T156=\"Select Model\",T156=\"PCBL\"), 0,getSPIP(T156, W156, Y156, BD156, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T156=\"Select Model\", \"\",IF(T156=\"PCBL\",0,primaryAirSensibleCapacityIP($T156,$W156,activeRoomTempCooling,activePriAirTempCooling,$Y156,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T156=\"Select Model\",\"\",IF($T156=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y156,activeElevation)))","v":""},{"$f":"IF(OR(T156=\"Select Model\",T156=\"PCBL\"), 0,IF(AD156=0,0,-primaryAirSensibleCapacityIP($T156,$W156,activeRoomTempHeating,activePriAirTempHeating,$Y156,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T156=\"Select Model\", \"\", InductionRatio($T156,BD156,$W156,$Y156)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T156=\"Select Model\", \"\",IF($T156=\"PCBL\",\"N/A\",minVAVSetBack(AA156, Y156))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T156=\"Select Model\", \"\",IF($T156= \"PCBL\",\"N/A\",getDischargeAirTemp($T156,$V156,$AC156,$W156,BD156,$AL156, $Y156, $AS156, \"cooling\",activeElevation,$AB156,$AJ156,$AV156,$BB156))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T156=\"Select Model\",$T156=\"PCBL\"), \"\",getDischargeAirTemp($T156,$V156,$AD156,$W156,BD156,$AL156, $Y156, $AY156, \"heating\",activeElevation,$AB156,$AJ156,$AV156,$BB156)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T156=\"Select Model\", \"\",IF(OR($T156=\"ACBC_1W\",$T156=\"ACBC_2W\",LEFT($T156,4)=\"ACBR\",$T156 = \"LIU24_2W\",LEFT($T156,3)=\"RIU\",LEFT($T156,6)=\"ACBL12\"), IF((soundLevel($T156, $AB156, BD156, $Y156, $W156,$AJ156,$AA156,\"dba\"))<15,\"<15\",soundLevel($T156, $AB156, BD156, $Y156, $W156,$AJ156,$AA156,\"dba\")+0.4),IF((soundLevel($T156, $AB156, BD156, $Y156, $W156,$AJ156,$AA156,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T156, $AB156, BD156, $Y156, $W156,$AJ156,$AA156,\"dba\")+5)<15, \"<15\", soundLevel($T156, $AB156, BD156,$Y156, $W156,$AJ156,$AA156,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T156=\"Select Model\", \"\",IF(OR($T156=\"ACBC_1W\",$T156=\"ACBC_2W\",LEFT($T156,4)=\"ACBR\",$T156=\"LIU24_2W\",LEFT($T156,3)=\"RIU\",LEFT($T156,6)=\"ACBL12\"), IF((soundLevel($T156, $AB156, BD156, $Y156, $W156,$AJ156,$AA156,\"NC\"))<15,\"<15\",soundLevel($T156, $AB156, BD156, $Y156, $W156,$AJ156,$AA156,\"NC\")+0.4),IF((soundLevel($T156, $AB156, BD156, $Y156, $W156,$AJ156,$AA156,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T156, $AB156, BD156, $Y156, $W156,$AJ156,$AA156,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T156, $AB156, BD156, $Y156, $W156,$AJ156,$AA156,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T156=\"Select Model\",\"\",IF($T156=\"LIU24_2W\",calcQwIP($Y156,$W156,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC156,$AI156,\"latent\",$U156&\"P\"&IF($V156=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T156,activeElevation),\"\"))","v":""},{"$f":"IF($T156=\"Select Model\",\"\",IF($T156=\"ACBC_1W\",calcQwIP($Y156,$W156,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC156,BD156,\"capacity\",$U156&\"P\"&IF($V156=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T156,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y156,$W156,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC156,BD156,\"capacity\",$U156&\"P\"&IF($V156=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T156,activeElevation)))","v":""},"",{"$f":"IF(T156=\"Select Model\", 0,waterPressureDrop(W156, U156 & \"P\" & IF(V156=\"Dual\",2,1) &\"C\", AC156, \"cooling\", T156))","v":0},{"$f":"IF(T156=\"Select Model\", \"\",getReturnWaterTemp(T156,AC156, activeEWTCooling, AS156, \"cooling\"))","v":""},"",{"$f":"IF($T156<>\"ACBC_1W\",\"\",IF($J156=\"\",\"\",FintubeCapacity($T156,$W156,$AE156,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T156=\"Select Model\",T156=\"PCBL\"),\"\",calcQwIP(Y156,W156,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD156,BD156,\"capacity\",U156&\"P\"&IF(V156=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T156,activeElevation))","v":""},"",{"$f":"IF(OR(T156=\"Select Model\",T156=\"PCBL\"), \"\",IF(AY156=0,\"N/A\",waterPressureDrop(W156, U156 & \"P\" & IF(V156=\"Dual\",2,1) &\"C\", AD156, \"heating\", T156)))","v":""},{"$f":"IF(OR(T156=\"Select Model\",T156=\"PCBL\"), \"\",IF(AY156=0,getReturnWaterTemp(T156,AE156, activeEWTHeating, AX156, \"heating\"),getReturnWaterTemp(T156,AD156, activeEWTHeating, AY156, \"heating\")))","v":""},"",{"$f":" getNozzle(T156, W156, Y156, Z156, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I157)),I157<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I157, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H157)),H157<0),\"\",intlEstQuantity(T157, W157*12, H157)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T157=\"Select Model\",\"\",coilCircuitChange(W157, U157, AC157, T157,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T157=\"Select Model\",\"\",beamWidth(T157))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T157=\"Select Model\",T157=\"PCBL\"), 0,getSPIP(T157, W157, Y157, BD157, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T157=\"Select Model\", \"\",IF(T157=\"PCBL\",0,primaryAirSensibleCapacityIP($T157,$W157,activeRoomTempCooling,activePriAirTempCooling,$Y157,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T157=\"Select Model\",\"\",IF($T157=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y157,activeElevation)))","v":""},{"$f":"IF(OR(T157=\"Select Model\",T157=\"PCBL\"), 0,IF(AD157=0,0,-primaryAirSensibleCapacityIP($T157,$W157,activeRoomTempHeating,activePriAirTempHeating,$Y157,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T157=\"Select Model\", \"\", InductionRatio($T157,BD157,$W157,$Y157)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T157=\"Select Model\", \"\",IF($T157=\"PCBL\",\"N/A\",minVAVSetBack(AA157, Y157))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T157=\"Select Model\", \"\",IF($T157= \"PCBL\",\"N/A\",getDischargeAirTemp($T157,$V157,$AC157,$W157,BD157,$AL157, $Y157, $AS157, \"cooling\",activeElevation,$AB157,$AJ157,$AV157,$BB157))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T157=\"Select Model\",$T157=\"PCBL\"), \"\",getDischargeAirTemp($T157,$V157,$AD157,$W157,BD157,$AL157, $Y157, $AY157, \"heating\",activeElevation,$AB157,$AJ157,$AV157,$BB157)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T157=\"Select Model\", \"\",IF(OR($T157=\"ACBC_1W\",$T157=\"ACBC_2W\",LEFT($T157,4)=\"ACBR\",$T157 = \"LIU24_2W\",LEFT($T157,3)=\"RIU\",LEFT($T157,6)=\"ACBL12\"), IF((soundLevel($T157, $AB157, BD157, $Y157, $W157,$AJ157,$AA157,\"dba\"))<15,\"<15\",soundLevel($T157, $AB157, BD157, $Y157, $W157,$AJ157,$AA157,\"dba\")+0.4),IF((soundLevel($T157, $AB157, BD157, $Y157, $W157,$AJ157,$AA157,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T157, $AB157, BD157, $Y157, $W157,$AJ157,$AA157,\"dba\")+5)<15, \"<15\", soundLevel($T157, $AB157, BD157,$Y157, $W157,$AJ157,$AA157,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T157=\"Select Model\", \"\",IF(OR($T157=\"ACBC_1W\",$T157=\"ACBC_2W\",LEFT($T157,4)=\"ACBR\",$T157=\"LIU24_2W\",LEFT($T157,3)=\"RIU\",LEFT($T157,6)=\"ACBL12\"), IF((soundLevel($T157, $AB157, BD157, $Y157, $W157,$AJ157,$AA157,\"NC\"))<15,\"<15\",soundLevel($T157, $AB157, BD157, $Y157, $W157,$AJ157,$AA157,\"NC\")+0.4),IF((soundLevel($T157, $AB157, BD157, $Y157, $W157,$AJ157,$AA157,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T157, $AB157, BD157, $Y157, $W157,$AJ157,$AA157,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T157, $AB157, BD157, $Y157, $W157,$AJ157,$AA157,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T157=\"Select Model\",\"\",IF($T157=\"LIU24_2W\",calcQwIP($Y157,$W157,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC157,$AI157,\"latent\",$U157&\"P\"&IF($V157=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T157,activeElevation),\"\"))","v":""},{"$f":"IF($T157=\"Select Model\",\"\",IF($T157=\"ACBC_1W\",calcQwIP($Y157,$W157,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC157,BD157,\"capacity\",$U157&\"P\"&IF($V157=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T157,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y157,$W157,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC157,BD157,\"capacity\",$U157&\"P\"&IF($V157=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T157,activeElevation)))","v":""},"",{"$f":"IF(T157=\"Select Model\", 0,waterPressureDrop(W157, U157 & \"P\" & IF(V157=\"Dual\",2,1) &\"C\", AC157, \"cooling\", T157))","v":0},{"$f":"IF(T157=\"Select Model\", \"\",getReturnWaterTemp(T157,AC157, activeEWTCooling, AS157, \"cooling\"))","v":""},"",{"$f":"IF($T157<>\"ACBC_1W\",\"\",IF($J157=\"\",\"\",FintubeCapacity($T157,$W157,$AE157,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T157=\"Select Model\",T157=\"PCBL\"),\"\",calcQwIP(Y157,W157,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD157,BD157,\"capacity\",U157&\"P\"&IF(V157=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T157,activeElevation))","v":""},"",{"$f":"IF(OR(T157=\"Select Model\",T157=\"PCBL\"), \"\",IF(AY157=0,\"N/A\",waterPressureDrop(W157, U157 & \"P\" & IF(V157=\"Dual\",2,1) &\"C\", AD157, \"heating\", T157)))","v":""},{"$f":"IF(OR(T157=\"Select Model\",T157=\"PCBL\"), \"\",IF(AY157=0,getReturnWaterTemp(T157,AE157, activeEWTHeating, AX157, \"heating\"),getReturnWaterTemp(T157,AD157, activeEWTHeating, AY157, \"heating\")))","v":""},"",{"$f":" getNozzle(T157, W157, Y157, Z157, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I158)),I158<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I158, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H158)),H158<0),\"\",intlEstQuantity(T158, W158*12, H158)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T158=\"Select Model\",\"\",coilCircuitChange(W158, U158, AC158, T158,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T158=\"Select Model\",\"\",beamWidth(T158))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T158=\"Select Model\",T158=\"PCBL\"), 0,getSPIP(T158, W158, Y158, BD158, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T158=\"Select Model\", \"\",IF(T158=\"PCBL\",0,primaryAirSensibleCapacityIP($T158,$W158,activeRoomTempCooling,activePriAirTempCooling,$Y158,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T158=\"Select Model\",\"\",IF($T158=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y158,activeElevation)))","v":""},{"$f":"IF(OR(T158=\"Select Model\",T158=\"PCBL\"), 0,IF(AD158=0,0,-primaryAirSensibleCapacityIP($T158,$W158,activeRoomTempHeating,activePriAirTempHeating,$Y158,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T158=\"Select Model\", \"\", InductionRatio($T158,BD158,$W158,$Y158)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T158=\"Select Model\", \"\",IF($T158=\"PCBL\",\"N/A\",minVAVSetBack(AA158, Y158))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T158=\"Select Model\", \"\",IF($T158= \"PCBL\",\"N/A\",getDischargeAirTemp($T158,$V158,$AC158,$W158,BD158,$AL158, $Y158, $AS158, \"cooling\",activeElevation,$AB158,$AJ158,$AV158,$BB158))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T158=\"Select Model\",$T158=\"PCBL\"), \"\",getDischargeAirTemp($T158,$V158,$AD158,$W158,BD158,$AL158, $Y158, $AY158, \"heating\",activeElevation,$AB158,$AJ158,$AV158,$BB158)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T158=\"Select Model\", \"\",IF(OR($T158=\"ACBC_1W\",$T158=\"ACBC_2W\",LEFT($T158,4)=\"ACBR\",$T158 = \"LIU24_2W\",LEFT($T158,3)=\"RIU\",LEFT($T158,6)=\"ACBL12\"), IF((soundLevel($T158, $AB158, BD158, $Y158, $W158,$AJ158,$AA158,\"dba\"))<15,\"<15\",soundLevel($T158, $AB158, BD158, $Y158, $W158,$AJ158,$AA158,\"dba\")+0.4),IF((soundLevel($T158, $AB158, BD158, $Y158, $W158,$AJ158,$AA158,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T158, $AB158, BD158, $Y158, $W158,$AJ158,$AA158,\"dba\")+5)<15, \"<15\", soundLevel($T158, $AB158, BD158,$Y158, $W158,$AJ158,$AA158,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T158=\"Select Model\", \"\",IF(OR($T158=\"ACBC_1W\",$T158=\"ACBC_2W\",LEFT($T158,4)=\"ACBR\",$T158=\"LIU24_2W\",LEFT($T158,3)=\"RIU\",LEFT($T158,6)=\"ACBL12\"), IF((soundLevel($T158, $AB158, BD158, $Y158, $W158,$AJ158,$AA158,\"NC\"))<15,\"<15\",soundLevel($T158, $AB158, BD158, $Y158, $W158,$AJ158,$AA158,\"NC\")+0.4),IF((soundLevel($T158, $AB158, BD158, $Y158, $W158,$AJ158,$AA158,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T158, $AB158, BD158, $Y158, $W158,$AJ158,$AA158,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T158, $AB158, BD158, $Y158, $W158,$AJ158,$AA158,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T158=\"Select Model\",\"\",IF($T158=\"LIU24_2W\",calcQwIP($Y158,$W158,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC158,$AI158,\"latent\",$U158&\"P\"&IF($V158=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T158,activeElevation),\"\"))","v":""},{"$f":"IF($T158=\"Select Model\",\"\",IF($T158=\"ACBC_1W\",calcQwIP($Y158,$W158,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC158,BD158,\"capacity\",$U158&\"P\"&IF($V158=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T158,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y158,$W158,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC158,BD158,\"capacity\",$U158&\"P\"&IF($V158=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T158,activeElevation)))","v":""},"",{"$f":"IF(T158=\"Select Model\", 0,waterPressureDrop(W158, U158 & \"P\" & IF(V158=\"Dual\",2,1) &\"C\", AC158, \"cooling\", T158))","v":0},{"$f":"IF(T158=\"Select Model\", \"\",getReturnWaterTemp(T158,AC158, activeEWTCooling, AS158, \"cooling\"))","v":""},"",{"$f":"IF($T158<>\"ACBC_1W\",\"\",IF($J158=\"\",\"\",FintubeCapacity($T158,$W158,$AE158,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T158=\"Select Model\",T158=\"PCBL\"),\"\",calcQwIP(Y158,W158,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD158,BD158,\"capacity\",U158&\"P\"&IF(V158=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T158,activeElevation))","v":""},"",{"$f":"IF(OR(T158=\"Select Model\",T158=\"PCBL\"), \"\",IF(AY158=0,\"N/A\",waterPressureDrop(W158, U158 & \"P\" & IF(V158=\"Dual\",2,1) &\"C\", AD158, \"heating\", T158)))","v":""},{"$f":"IF(OR(T158=\"Select Model\",T158=\"PCBL\"), \"\",IF(AY158=0,getReturnWaterTemp(T158,AE158, activeEWTHeating, AX158, \"heating\"),getReturnWaterTemp(T158,AD158, activeEWTHeating, AY158, \"heating\")))","v":""},"",{"$f":" getNozzle(T158, W158, Y158, Z158, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I159)),I159<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I159, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H159)),H159<0),\"\",intlEstQuantity(T159, W159*12, H159)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T159=\"Select Model\",\"\",coilCircuitChange(W159, U159, AC159, T159,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T159=\"Select Model\",\"\",beamWidth(T159))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T159=\"Select Model\",T159=\"PCBL\"), 0,getSPIP(T159, W159, Y159, BD159, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T159=\"Select Model\", \"\",IF(T159=\"PCBL\",0,primaryAirSensibleCapacityIP($T159,$W159,activeRoomTempCooling,activePriAirTempCooling,$Y159,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T159=\"Select Model\",\"\",IF($T159=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y159,activeElevation)))","v":""},{"$f":"IF(OR(T159=\"Select Model\",T159=\"PCBL\"), 0,IF(AD159=0,0,-primaryAirSensibleCapacityIP($T159,$W159,activeRoomTempHeating,activePriAirTempHeating,$Y159,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T159=\"Select Model\", \"\", InductionRatio($T159,BD159,$W159,$Y159)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T159=\"Select Model\", \"\",IF($T159=\"PCBL\",\"N/A\",minVAVSetBack(AA159, Y159))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T159=\"Select Model\", \"\",IF($T159= \"PCBL\",\"N/A\",getDischargeAirTemp($T159,$V159,$AC159,$W159,BD159,$AL159, $Y159, $AS159, \"cooling\",activeElevation,$AB159,$AJ159,$AV159,$BB159))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T159=\"Select Model\",$T159=\"PCBL\"), \"\",getDischargeAirTemp($T159,$V159,$AD159,$W159,BD159,$AL159, $Y159, $AY159, \"heating\",activeElevation,$AB159,$AJ159,$AV159,$BB159)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T159=\"Select Model\", \"\",IF(OR($T159=\"ACBC_1W\",$T159=\"ACBC_2W\",LEFT($T159,4)=\"ACBR\",$T159 = \"LIU24_2W\",LEFT($T159,3)=\"RIU\",LEFT($T159,6)=\"ACBL12\"), IF((soundLevel($T159, $AB159, BD159, $Y159, $W159,$AJ159,$AA159,\"dba\"))<15,\"<15\",soundLevel($T159, $AB159, BD159, $Y159, $W159,$AJ159,$AA159,\"dba\")+0.4),IF((soundLevel($T159, $AB159, BD159, $Y159, $W159,$AJ159,$AA159,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T159, $AB159, BD159, $Y159, $W159,$AJ159,$AA159,\"dba\")+5)<15, \"<15\", soundLevel($T159, $AB159, BD159,$Y159, $W159,$AJ159,$AA159,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T159=\"Select Model\", \"\",IF(OR($T159=\"ACBC_1W\",$T159=\"ACBC_2W\",LEFT($T159,4)=\"ACBR\",$T159=\"LIU24_2W\",LEFT($T159,3)=\"RIU\",LEFT($T159,6)=\"ACBL12\"), IF((soundLevel($T159, $AB159, BD159, $Y159, $W159,$AJ159,$AA159,\"NC\"))<15,\"<15\",soundLevel($T159, $AB159, BD159, $Y159, $W159,$AJ159,$AA159,\"NC\")+0.4),IF((soundLevel($T159, $AB159, BD159, $Y159, $W159,$AJ159,$AA159,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T159, $AB159, BD159, $Y159, $W159,$AJ159,$AA159,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T159, $AB159, BD159, $Y159, $W159,$AJ159,$AA159,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T159=\"Select Model\",\"\",IF($T159=\"LIU24_2W\",calcQwIP($Y159,$W159,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC159,$AI159,\"latent\",$U159&\"P\"&IF($V159=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T159,activeElevation),\"\"))","v":""},{"$f":"IF($T159=\"Select Model\",\"\",IF($T159=\"ACBC_1W\",calcQwIP($Y159,$W159,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC159,BD159,\"capacity\",$U159&\"P\"&IF($V159=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T159,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y159,$W159,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC159,BD159,\"capacity\",$U159&\"P\"&IF($V159=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T159,activeElevation)))","v":""},"",{"$f":"IF(T159=\"Select Model\", 0,waterPressureDrop(W159, U159 & \"P\" & IF(V159=\"Dual\",2,1) &\"C\", AC159, \"cooling\", T159))","v":0},{"$f":"IF(T159=\"Select Model\", \"\",getReturnWaterTemp(T159,AC159, activeEWTCooling, AS159, \"cooling\"))","v":""},"",{"$f":"IF($T159<>\"ACBC_1W\",\"\",IF($J159=\"\",\"\",FintubeCapacity($T159,$W159,$AE159,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T159=\"Select Model\",T159=\"PCBL\"),\"\",calcQwIP(Y159,W159,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD159,BD159,\"capacity\",U159&\"P\"&IF(V159=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T159,activeElevation))","v":""},"",{"$f":"IF(OR(T159=\"Select Model\",T159=\"PCBL\"), \"\",IF(AY159=0,\"N/A\",waterPressureDrop(W159, U159 & \"P\" & IF(V159=\"Dual\",2,1) &\"C\", AD159, \"heating\", T159)))","v":""},{"$f":"IF(OR(T159=\"Select Model\",T159=\"PCBL\"), \"\",IF(AY159=0,getReturnWaterTemp(T159,AE159, activeEWTHeating, AX159, \"heating\"),getReturnWaterTemp(T159,AD159, activeEWTHeating, AY159, \"heating\")))","v":""},"",{"$f":" getNozzle(T159, W159, Y159, Z159, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I160)),I160<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I160, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H160)),H160<0),\"\",intlEstQuantity(T160, W160*12, H160)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T160=\"Select Model\",\"\",coilCircuitChange(W160, U160, AC160, T160,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T160=\"Select Model\",\"\",beamWidth(T160))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T160=\"Select Model\",T160=\"PCBL\"), 0,getSPIP(T160, W160, Y160, BD160, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T160=\"Select Model\", \"\",IF(T160=\"PCBL\",0,primaryAirSensibleCapacityIP($T160,$W160,activeRoomTempCooling,activePriAirTempCooling,$Y160,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T160=\"Select Model\",\"\",IF($T160=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y160,activeElevation)))","v":""},{"$f":"IF(OR(T160=\"Select Model\",T160=\"PCBL\"), 0,IF(AD160=0,0,-primaryAirSensibleCapacityIP($T160,$W160,activeRoomTempHeating,activePriAirTempHeating,$Y160,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T160=\"Select Model\", \"\", InductionRatio($T160,BD160,$W160,$Y160)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T160=\"Select Model\", \"\",IF($T160=\"PCBL\",\"N/A\",minVAVSetBack(AA160, Y160))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T160=\"Select Model\", \"\",IF($T160= \"PCBL\",\"N/A\",getDischargeAirTemp($T160,$V160,$AC160,$W160,BD160,$AL160, $Y160, $AS160, \"cooling\",activeElevation,$AB160,$AJ160,$AV160,$BB160))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T160=\"Select Model\",$T160=\"PCBL\"), \"\",getDischargeAirTemp($T160,$V160,$AD160,$W160,BD160,$AL160, $Y160, $AY160, \"heating\",activeElevation,$AB160,$AJ160,$AV160,$BB160)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T160=\"Select Model\", \"\",IF(OR($T160=\"ACBC_1W\",$T160=\"ACBC_2W\",LEFT($T160,4)=\"ACBR\",$T160 = \"LIU24_2W\",LEFT($T160,3)=\"RIU\",LEFT($T160,6)=\"ACBL12\"), IF((soundLevel($T160, $AB160, BD160, $Y160, $W160,$AJ160,$AA160,\"dba\"))<15,\"<15\",soundLevel($T160, $AB160, BD160, $Y160, $W160,$AJ160,$AA160,\"dba\")+0.4),IF((soundLevel($T160, $AB160, BD160, $Y160, $W160,$AJ160,$AA160,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T160, $AB160, BD160, $Y160, $W160,$AJ160,$AA160,\"dba\")+5)<15, \"<15\", soundLevel($T160, $AB160, BD160,$Y160, $W160,$AJ160,$AA160,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T160=\"Select Model\", \"\",IF(OR($T160=\"ACBC_1W\",$T160=\"ACBC_2W\",LEFT($T160,4)=\"ACBR\",$T160=\"LIU24_2W\",LEFT($T160,3)=\"RIU\",LEFT($T160,6)=\"ACBL12\"), IF((soundLevel($T160, $AB160, BD160, $Y160, $W160,$AJ160,$AA160,\"NC\"))<15,\"<15\",soundLevel($T160, $AB160, BD160, $Y160, $W160,$AJ160,$AA160,\"NC\")+0.4),IF((soundLevel($T160, $AB160, BD160, $Y160, $W160,$AJ160,$AA160,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T160, $AB160, BD160, $Y160, $W160,$AJ160,$AA160,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T160, $AB160, BD160, $Y160, $W160,$AJ160,$AA160,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T160=\"Select Model\",\"\",IF($T160=\"LIU24_2W\",calcQwIP($Y160,$W160,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC160,$AI160,\"latent\",$U160&\"P\"&IF($V160=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T160,activeElevation),\"\"))","v":""},{"$f":"IF($T160=\"Select Model\",\"\",IF($T160=\"ACBC_1W\",calcQwIP($Y160,$W160,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC160,BD160,\"capacity\",$U160&\"P\"&IF($V160=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T160,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y160,$W160,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC160,BD160,\"capacity\",$U160&\"P\"&IF($V160=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T160,activeElevation)))","v":""},"",{"$f":"IF(T160=\"Select Model\", 0,waterPressureDrop(W160, U160 & \"P\" & IF(V160=\"Dual\",2,1) &\"C\", AC160, \"cooling\", T160))","v":0},{"$f":"IF(T160=\"Select Model\", \"\",getReturnWaterTemp(T160,AC160, activeEWTCooling, AS160, \"cooling\"))","v":""},"",{"$f":"IF($T160<>\"ACBC_1W\",\"\",IF($J160=\"\",\"\",FintubeCapacity($T160,$W160,$AE160,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T160=\"Select Model\",T160=\"PCBL\"),\"\",calcQwIP(Y160,W160,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD160,BD160,\"capacity\",U160&\"P\"&IF(V160=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T160,activeElevation))","v":""},"",{"$f":"IF(OR(T160=\"Select Model\",T160=\"PCBL\"), \"\",IF(AY160=0,\"N/A\",waterPressureDrop(W160, U160 & \"P\" & IF(V160=\"Dual\",2,1) &\"C\", AD160, \"heating\", T160)))","v":""},{"$f":"IF(OR(T160=\"Select Model\",T160=\"PCBL\"), \"\",IF(AY160=0,getReturnWaterTemp(T160,AE160, activeEWTHeating, AX160, \"heating\"),getReturnWaterTemp(T160,AD160, activeEWTHeating, AY160, \"heating\")))","v":""},"",{"$f":" getNozzle(T160, W160, Y160, Z160, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I161)),I161<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I161, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H161)),H161<0),\"\",intlEstQuantity(T161, W161*12, H161)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T161=\"Select Model\",\"\",coilCircuitChange(W161, U161, AC161, T161,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T161=\"Select Model\",\"\",beamWidth(T161))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T161=\"Select Model\",T161=\"PCBL\"), 0,getSPIP(T161, W161, Y161, BD161, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T161=\"Select Model\", \"\",IF(T161=\"PCBL\",0,primaryAirSensibleCapacityIP($T161,$W161,activeRoomTempCooling,activePriAirTempCooling,$Y161,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T161=\"Select Model\",\"\",IF($T161=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y161,activeElevation)))","v":""},{"$f":"IF(OR(T161=\"Select Model\",T161=\"PCBL\"), 0,IF(AD161=0,0,-primaryAirSensibleCapacityIP($T161,$W161,activeRoomTempHeating,activePriAirTempHeating,$Y161,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T161=\"Select Model\", \"\", InductionRatio($T161,BD161,$W161,$Y161)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T161=\"Select Model\", \"\",IF($T161=\"PCBL\",\"N/A\",minVAVSetBack(AA161, Y161))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T161=\"Select Model\", \"\",IF($T161= \"PCBL\",\"N/A\",getDischargeAirTemp($T161,$V161,$AC161,$W161,BD161,$AL161, $Y161, $AS161, \"cooling\",activeElevation,$AB161,$AJ161,$AV161,$BB161))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T161=\"Select Model\",$T161=\"PCBL\"), \"\",getDischargeAirTemp($T161,$V161,$AD161,$W161,BD161,$AL161, $Y161, $AY161, \"heating\",activeElevation,$AB161,$AJ161,$AV161,$BB161)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T161=\"Select Model\", \"\",IF(OR($T161=\"ACBC_1W\",$T161=\"ACBC_2W\",LEFT($T161,4)=\"ACBR\",$T161 = \"LIU24_2W\",LEFT($T161,3)=\"RIU\",LEFT($T161,6)=\"ACBL12\"), IF((soundLevel($T161, $AB161, BD161, $Y161, $W161,$AJ161,$AA161,\"dba\"))<15,\"<15\",soundLevel($T161, $AB161, BD161, $Y161, $W161,$AJ161,$AA161,\"dba\")+0.4),IF((soundLevel($T161, $AB161, BD161, $Y161, $W161,$AJ161,$AA161,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T161, $AB161, BD161, $Y161, $W161,$AJ161,$AA161,\"dba\")+5)<15, \"<15\", soundLevel($T161, $AB161, BD161,$Y161, $W161,$AJ161,$AA161,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T161=\"Select Model\", \"\",IF(OR($T161=\"ACBC_1W\",$T161=\"ACBC_2W\",LEFT($T161,4)=\"ACBR\",$T161=\"LIU24_2W\",LEFT($T161,3)=\"RIU\",LEFT($T161,6)=\"ACBL12\"), IF((soundLevel($T161, $AB161, BD161, $Y161, $W161,$AJ161,$AA161,\"NC\"))<15,\"<15\",soundLevel($T161, $AB161, BD161, $Y161, $W161,$AJ161,$AA161,\"NC\")+0.4),IF((soundLevel($T161, $AB161, BD161, $Y161, $W161,$AJ161,$AA161,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T161, $AB161, BD161, $Y161, $W161,$AJ161,$AA161,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T161, $AB161, BD161, $Y161, $W161,$AJ161,$AA161,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T161=\"Select Model\",\"\",IF($T161=\"LIU24_2W\",calcQwIP($Y161,$W161,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC161,$AI161,\"latent\",$U161&\"P\"&IF($V161=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T161,activeElevation),\"\"))","v":""},{"$f":"IF($T161=\"Select Model\",\"\",IF($T161=\"ACBC_1W\",calcQwIP($Y161,$W161,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC161,BD161,\"capacity\",$U161&\"P\"&IF($V161=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T161,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y161,$W161,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC161,BD161,\"capacity\",$U161&\"P\"&IF($V161=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T161,activeElevation)))","v":""},"",{"$f":"IF(T161=\"Select Model\", 0,waterPressureDrop(W161, U161 & \"P\" & IF(V161=\"Dual\",2,1) &\"C\", AC161, \"cooling\", T161))","v":0},{"$f":"IF(T161=\"Select Model\", \"\",getReturnWaterTemp(T161,AC161, activeEWTCooling, AS161, \"cooling\"))","v":""},"",{"$f":"IF($T161<>\"ACBC_1W\",\"\",IF($J161=\"\",\"\",FintubeCapacity($T161,$W161,$AE161,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T161=\"Select Model\",T161=\"PCBL\"),\"\",calcQwIP(Y161,W161,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD161,BD161,\"capacity\",U161&\"P\"&IF(V161=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T161,activeElevation))","v":""},"",{"$f":"IF(OR(T161=\"Select Model\",T161=\"PCBL\"), \"\",IF(AY161=0,\"N/A\",waterPressureDrop(W161, U161 & \"P\" & IF(V161=\"Dual\",2,1) &\"C\", AD161, \"heating\", T161)))","v":""},{"$f":"IF(OR(T161=\"Select Model\",T161=\"PCBL\"), \"\",IF(AY161=0,getReturnWaterTemp(T161,AE161, activeEWTHeating, AX161, \"heating\"),getReturnWaterTemp(T161,AD161, activeEWTHeating, AY161, \"heating\")))","v":""},"",{"$f":" getNozzle(T161, W161, Y161, Z161, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I162)),I162<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I162, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H162)),H162<0),\"\",intlEstQuantity(T162, W162*12, H162)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T162=\"Select Model\",\"\",coilCircuitChange(W162, U162, AC162, T162,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T162=\"Select Model\",\"\",beamWidth(T162))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T162=\"Select Model\",T162=\"PCBL\"), 0,getSPIP(T162, W162, Y162, BD162, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T162=\"Select Model\", \"\",IF(T162=\"PCBL\",0,primaryAirSensibleCapacityIP($T162,$W162,activeRoomTempCooling,activePriAirTempCooling,$Y162,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T162=\"Select Model\",\"\",IF($T162=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y162,activeElevation)))","v":""},{"$f":"IF(OR(T162=\"Select Model\",T162=\"PCBL\"), 0,IF(AD162=0,0,-primaryAirSensibleCapacityIP($T162,$W162,activeRoomTempHeating,activePriAirTempHeating,$Y162,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T162=\"Select Model\", \"\", InductionRatio($T162,BD162,$W162,$Y162)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T162=\"Select Model\", \"\",IF($T162=\"PCBL\",\"N/A\",minVAVSetBack(AA162, Y162))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T162=\"Select Model\", \"\",IF($T162= \"PCBL\",\"N/A\",getDischargeAirTemp($T162,$V162,$AC162,$W162,BD162,$AL162, $Y162, $AS162, \"cooling\",activeElevation,$AB162,$AJ162,$AV162,$BB162))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T162=\"Select Model\",$T162=\"PCBL\"), \"\",getDischargeAirTemp($T162,$V162,$AD162,$W162,BD162,$AL162, $Y162, $AY162, \"heating\",activeElevation,$AB162,$AJ162,$AV162,$BB162)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T162=\"Select Model\", \"\",IF(OR($T162=\"ACBC_1W\",$T162=\"ACBC_2W\",LEFT($T162,4)=\"ACBR\",$T162 = \"LIU24_2W\",LEFT($T162,3)=\"RIU\",LEFT($T162,6)=\"ACBL12\"), IF((soundLevel($T162, $AB162, BD162, $Y162, $W162,$AJ162,$AA162,\"dba\"))<15,\"<15\",soundLevel($T162, $AB162, BD162, $Y162, $W162,$AJ162,$AA162,\"dba\")+0.4),IF((soundLevel($T162, $AB162, BD162, $Y162, $W162,$AJ162,$AA162,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T162, $AB162, BD162, $Y162, $W162,$AJ162,$AA162,\"dba\")+5)<15, \"<15\", soundLevel($T162, $AB162, BD162,$Y162, $W162,$AJ162,$AA162,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T162=\"Select Model\", \"\",IF(OR($T162=\"ACBC_1W\",$T162=\"ACBC_2W\",LEFT($T162,4)=\"ACBR\",$T162=\"LIU24_2W\",LEFT($T162,3)=\"RIU\",LEFT($T162,6)=\"ACBL12\"), IF((soundLevel($T162, $AB162, BD162, $Y162, $W162,$AJ162,$AA162,\"NC\"))<15,\"<15\",soundLevel($T162, $AB162, BD162, $Y162, $W162,$AJ162,$AA162,\"NC\")+0.4),IF((soundLevel($T162, $AB162, BD162, $Y162, $W162,$AJ162,$AA162,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T162, $AB162, BD162, $Y162, $W162,$AJ162,$AA162,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T162, $AB162, BD162, $Y162, $W162,$AJ162,$AA162,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T162=\"Select Model\",\"\",IF($T162=\"LIU24_2W\",calcQwIP($Y162,$W162,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC162,$AI162,\"latent\",$U162&\"P\"&IF($V162=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T162,activeElevation),\"\"))","v":""},{"$f":"IF($T162=\"Select Model\",\"\",IF($T162=\"ACBC_1W\",calcQwIP($Y162,$W162,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC162,BD162,\"capacity\",$U162&\"P\"&IF($V162=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T162,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y162,$W162,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC162,BD162,\"capacity\",$U162&\"P\"&IF($V162=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T162,activeElevation)))","v":""},"",{"$f":"IF(T162=\"Select Model\", 0,waterPressureDrop(W162, U162 & \"P\" & IF(V162=\"Dual\",2,1) &\"C\", AC162, \"cooling\", T162))","v":0},{"$f":"IF(T162=\"Select Model\", \"\",getReturnWaterTemp(T162,AC162, activeEWTCooling, AS162, \"cooling\"))","v":""},"",{"$f":"IF($T162<>\"ACBC_1W\",\"\",IF($J162=\"\",\"\",FintubeCapacity($T162,$W162,$AE162,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T162=\"Select Model\",T162=\"PCBL\"),\"\",calcQwIP(Y162,W162,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD162,BD162,\"capacity\",U162&\"P\"&IF(V162=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T162,activeElevation))","v":""},"",{"$f":"IF(OR(T162=\"Select Model\",T162=\"PCBL\"), \"\",IF(AY162=0,\"N/A\",waterPressureDrop(W162, U162 & \"P\" & IF(V162=\"Dual\",2,1) &\"C\", AD162, \"heating\", T162)))","v":""},{"$f":"IF(OR(T162=\"Select Model\",T162=\"PCBL\"), \"\",IF(AY162=0,getReturnWaterTemp(T162,AE162, activeEWTHeating, AX162, \"heating\"),getReturnWaterTemp(T162,AD162, activeEWTHeating, AY162, \"heating\")))","v":""},"",{"$f":" getNozzle(T162, W162, Y162, Z162, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I163)),I163<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I163, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H163)),H163<0),\"\",intlEstQuantity(T163, W163*12, H163)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T163=\"Select Model\",\"\",coilCircuitChange(W163, U163, AC163, T163,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T163=\"Select Model\",\"\",beamWidth(T163))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T163=\"Select Model\",T163=\"PCBL\"), 0,getSPIP(T163, W163, Y163, BD163, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T163=\"Select Model\", \"\",IF(T163=\"PCBL\",0,primaryAirSensibleCapacityIP($T163,$W163,activeRoomTempCooling,activePriAirTempCooling,$Y163,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T163=\"Select Model\",\"\",IF($T163=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y163,activeElevation)))","v":""},{"$f":"IF(OR(T163=\"Select Model\",T163=\"PCBL\"), 0,IF(AD163=0,0,-primaryAirSensibleCapacityIP($T163,$W163,activeRoomTempHeating,activePriAirTempHeating,$Y163,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T163=\"Select Model\", \"\", InductionRatio($T163,BD163,$W163,$Y163)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T163=\"Select Model\", \"\",IF($T163=\"PCBL\",\"N/A\",minVAVSetBack(AA163, Y163))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T163=\"Select Model\", \"\",IF($T163= \"PCBL\",\"N/A\",getDischargeAirTemp($T163,$V163,$AC163,$W163,BD163,$AL163, $Y163, $AS163, \"cooling\",activeElevation,$AB163,$AJ163,$AV163,$BB163))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T163=\"Select Model\",$T163=\"PCBL\"), \"\",getDischargeAirTemp($T163,$V163,$AD163,$W163,BD163,$AL163, $Y163, $AY163, \"heating\",activeElevation,$AB163,$AJ163,$AV163,$BB163)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T163=\"Select Model\", \"\",IF(OR($T163=\"ACBC_1W\",$T163=\"ACBC_2W\",LEFT($T163,4)=\"ACBR\",$T163 = \"LIU24_2W\",LEFT($T163,3)=\"RIU\",LEFT($T163,6)=\"ACBL12\"), IF((soundLevel($T163, $AB163, BD163, $Y163, $W163,$AJ163,$AA163,\"dba\"))<15,\"<15\",soundLevel($T163, $AB163, BD163, $Y163, $W163,$AJ163,$AA163,\"dba\")+0.4),IF((soundLevel($T163, $AB163, BD163, $Y163, $W163,$AJ163,$AA163,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T163, $AB163, BD163, $Y163, $W163,$AJ163,$AA163,\"dba\")+5)<15, \"<15\", soundLevel($T163, $AB163, BD163,$Y163, $W163,$AJ163,$AA163,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T163=\"Select Model\", \"\",IF(OR($T163=\"ACBC_1W\",$T163=\"ACBC_2W\",LEFT($T163,4)=\"ACBR\",$T163=\"LIU24_2W\",LEFT($T163,3)=\"RIU\",LEFT($T163,6)=\"ACBL12\"), IF((soundLevel($T163, $AB163, BD163, $Y163, $W163,$AJ163,$AA163,\"NC\"))<15,\"<15\",soundLevel($T163, $AB163, BD163, $Y163, $W163,$AJ163,$AA163,\"NC\")+0.4),IF((soundLevel($T163, $AB163, BD163, $Y163, $W163,$AJ163,$AA163,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T163, $AB163, BD163, $Y163, $W163,$AJ163,$AA163,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T163, $AB163, BD163, $Y163, $W163,$AJ163,$AA163,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T163=\"Select Model\",\"\",IF($T163=\"LIU24_2W\",calcQwIP($Y163,$W163,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC163,$AI163,\"latent\",$U163&\"P\"&IF($V163=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T163,activeElevation),\"\"))","v":""},{"$f":"IF($T163=\"Select Model\",\"\",IF($T163=\"ACBC_1W\",calcQwIP($Y163,$W163,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC163,BD163,\"capacity\",$U163&\"P\"&IF($V163=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T163,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y163,$W163,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC163,BD163,\"capacity\",$U163&\"P\"&IF($V163=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T163,activeElevation)))","v":""},"",{"$f":"IF(T163=\"Select Model\", 0,waterPressureDrop(W163, U163 & \"P\" & IF(V163=\"Dual\",2,1) &\"C\", AC163, \"cooling\", T163))","v":0},{"$f":"IF(T163=\"Select Model\", \"\",getReturnWaterTemp(T163,AC163, activeEWTCooling, AS163, \"cooling\"))","v":""},"",{"$f":"IF($T163<>\"ACBC_1W\",\"\",IF($J163=\"\",\"\",FintubeCapacity($T163,$W163,$AE163,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T163=\"Select Model\",T163=\"PCBL\"),\"\",calcQwIP(Y163,W163,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD163,BD163,\"capacity\",U163&\"P\"&IF(V163=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T163,activeElevation))","v":""},"",{"$f":"IF(OR(T163=\"Select Model\",T163=\"PCBL\"), \"\",IF(AY163=0,\"N/A\",waterPressureDrop(W163, U163 & \"P\" & IF(V163=\"Dual\",2,1) &\"C\", AD163, \"heating\", T163)))","v":""},{"$f":"IF(OR(T163=\"Select Model\",T163=\"PCBL\"), \"\",IF(AY163=0,getReturnWaterTemp(T163,AE163, activeEWTHeating, AX163, \"heating\"),getReturnWaterTemp(T163,AD163, activeEWTHeating, AY163, \"heating\")))","v":""},"",{"$f":" getNozzle(T163, W163, Y163, Z163, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I164)),I164<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I164, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H164)),H164<0),\"\",intlEstQuantity(T164, W164*12, H164)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T164=\"Select Model\",\"\",coilCircuitChange(W164, U164, AC164, T164,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T164=\"Select Model\",\"\",beamWidth(T164))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T164=\"Select Model\",T164=\"PCBL\"), 0,getSPIP(T164, W164, Y164, BD164, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T164=\"Select Model\", \"\",IF(T164=\"PCBL\",0,primaryAirSensibleCapacityIP($T164,$W164,activeRoomTempCooling,activePriAirTempCooling,$Y164,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T164=\"Select Model\",\"\",IF($T164=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y164,activeElevation)))","v":""},{"$f":"IF(OR(T164=\"Select Model\",T164=\"PCBL\"), 0,IF(AD164=0,0,-primaryAirSensibleCapacityIP($T164,$W164,activeRoomTempHeating,activePriAirTempHeating,$Y164,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T164=\"Select Model\", \"\", InductionRatio($T164,BD164,$W164,$Y164)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T164=\"Select Model\", \"\",IF($T164=\"PCBL\",\"N/A\",minVAVSetBack(AA164, Y164))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T164=\"Select Model\", \"\",IF($T164= \"PCBL\",\"N/A\",getDischargeAirTemp($T164,$V164,$AC164,$W164,BD164,$AL164, $Y164, $AS164, \"cooling\",activeElevation,$AB164,$AJ164,$AV164,$BB164))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T164=\"Select Model\",$T164=\"PCBL\"), \"\",getDischargeAirTemp($T164,$V164,$AD164,$W164,BD164,$AL164, $Y164, $AY164, \"heating\",activeElevation,$AB164,$AJ164,$AV164,$BB164)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T164=\"Select Model\", \"\",IF(OR($T164=\"ACBC_1W\",$T164=\"ACBC_2W\",LEFT($T164,4)=\"ACBR\",$T164 = \"LIU24_2W\",LEFT($T164,3)=\"RIU\",LEFT($T164,6)=\"ACBL12\"), IF((soundLevel($T164, $AB164, BD164, $Y164, $W164,$AJ164,$AA164,\"dba\"))<15,\"<15\",soundLevel($T164, $AB164, BD164, $Y164, $W164,$AJ164,$AA164,\"dba\")+0.4),IF((soundLevel($T164, $AB164, BD164, $Y164, $W164,$AJ164,$AA164,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T164, $AB164, BD164, $Y164, $W164,$AJ164,$AA164,\"dba\")+5)<15, \"<15\", soundLevel($T164, $AB164, BD164,$Y164, $W164,$AJ164,$AA164,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T164=\"Select Model\", \"\",IF(OR($T164=\"ACBC_1W\",$T164=\"ACBC_2W\",LEFT($T164,4)=\"ACBR\",$T164=\"LIU24_2W\",LEFT($T164,3)=\"RIU\",LEFT($T164,6)=\"ACBL12\"), IF((soundLevel($T164, $AB164, BD164, $Y164, $W164,$AJ164,$AA164,\"NC\"))<15,\"<15\",soundLevel($T164, $AB164, BD164, $Y164, $W164,$AJ164,$AA164,\"NC\")+0.4),IF((soundLevel($T164, $AB164, BD164, $Y164, $W164,$AJ164,$AA164,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T164, $AB164, BD164, $Y164, $W164,$AJ164,$AA164,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T164, $AB164, BD164, $Y164, $W164,$AJ164,$AA164,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T164=\"Select Model\",\"\",IF($T164=\"LIU24_2W\",calcQwIP($Y164,$W164,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC164,$AI164,\"latent\",$U164&\"P\"&IF($V164=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T164,activeElevation),\"\"))","v":""},{"$f":"IF($T164=\"Select Model\",\"\",IF($T164=\"ACBC_1W\",calcQwIP($Y164,$W164,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC164,BD164,\"capacity\",$U164&\"P\"&IF($V164=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T164,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y164,$W164,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC164,BD164,\"capacity\",$U164&\"P\"&IF($V164=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T164,activeElevation)))","v":""},"",{"$f":"IF(T164=\"Select Model\", 0,waterPressureDrop(W164, U164 & \"P\" & IF(V164=\"Dual\",2,1) &\"C\", AC164, \"cooling\", T164))","v":0},{"$f":"IF(T164=\"Select Model\", \"\",getReturnWaterTemp(T164,AC164, activeEWTCooling, AS164, \"cooling\"))","v":""},"",{"$f":"IF($T164<>\"ACBC_1W\",\"\",IF($J164=\"\",\"\",FintubeCapacity($T164,$W164,$AE164,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T164=\"Select Model\",T164=\"PCBL\"),\"\",calcQwIP(Y164,W164,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD164,BD164,\"capacity\",U164&\"P\"&IF(V164=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T164,activeElevation))","v":""},"",{"$f":"IF(OR(T164=\"Select Model\",T164=\"PCBL\"), \"\",IF(AY164=0,\"N/A\",waterPressureDrop(W164, U164 & \"P\" & IF(V164=\"Dual\",2,1) &\"C\", AD164, \"heating\", T164)))","v":""},{"$f":"IF(OR(T164=\"Select Model\",T164=\"PCBL\"), \"\",IF(AY164=0,getReturnWaterTemp(T164,AE164, activeEWTHeating, AX164, \"heating\"),getReturnWaterTemp(T164,AD164, activeEWTHeating, AY164, \"heating\")))","v":""},"",{"$f":" getNozzle(T164, W164, Y164, Z164, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I165)),I165<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I165, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H165)),H165<0),\"\",intlEstQuantity(T165, W165*12, H165)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T165=\"Select Model\",\"\",coilCircuitChange(W165, U165, AC165, T165,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T165=\"Select Model\",\"\",beamWidth(T165))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T165=\"Select Model\",T165=\"PCBL\"), 0,getSPIP(T165, W165, Y165, BD165, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T165=\"Select Model\", \"\",IF(T165=\"PCBL\",0,primaryAirSensibleCapacityIP($T165,$W165,activeRoomTempCooling,activePriAirTempCooling,$Y165,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T165=\"Select Model\",\"\",IF($T165=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y165,activeElevation)))","v":""},{"$f":"IF(OR(T165=\"Select Model\",T165=\"PCBL\"), 0,IF(AD165=0,0,-primaryAirSensibleCapacityIP($T165,$W165,activeRoomTempHeating,activePriAirTempHeating,$Y165,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T165=\"Select Model\", \"\", InductionRatio($T165,BD165,$W165,$Y165)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T165=\"Select Model\", \"\",IF($T165=\"PCBL\",\"N/A\",minVAVSetBack(AA165, Y165))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T165=\"Select Model\", \"\",IF($T165= \"PCBL\",\"N/A\",getDischargeAirTemp($T165,$V165,$AC165,$W165,BD165,$AL165, $Y165, $AS165, \"cooling\",activeElevation,$AB165,$AJ165,$AV165,$BB165))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T165=\"Select Model\",$T165=\"PCBL\"), \"\",getDischargeAirTemp($T165,$V165,$AD165,$W165,BD165,$AL165, $Y165, $AY165, \"heating\",activeElevation,$AB165,$AJ165,$AV165,$BB165)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T165=\"Select Model\", \"\",IF(OR($T165=\"ACBC_1W\",$T165=\"ACBC_2W\",LEFT($T165,4)=\"ACBR\",$T165 = \"LIU24_2W\",LEFT($T165,3)=\"RIU\",LEFT($T165,6)=\"ACBL12\"), IF((soundLevel($T165, $AB165, BD165, $Y165, $W165,$AJ165,$AA165,\"dba\"))<15,\"<15\",soundLevel($T165, $AB165, BD165, $Y165, $W165,$AJ165,$AA165,\"dba\")+0.4),IF((soundLevel($T165, $AB165, BD165, $Y165, $W165,$AJ165,$AA165,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T165, $AB165, BD165, $Y165, $W165,$AJ165,$AA165,\"dba\")+5)<15, \"<15\", soundLevel($T165, $AB165, BD165,$Y165, $W165,$AJ165,$AA165,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T165=\"Select Model\", \"\",IF(OR($T165=\"ACBC_1W\",$T165=\"ACBC_2W\",LEFT($T165,4)=\"ACBR\",$T165=\"LIU24_2W\",LEFT($T165,3)=\"RIU\",LEFT($T165,6)=\"ACBL12\"), IF((soundLevel($T165, $AB165, BD165, $Y165, $W165,$AJ165,$AA165,\"NC\"))<15,\"<15\",soundLevel($T165, $AB165, BD165, $Y165, $W165,$AJ165,$AA165,\"NC\")+0.4),IF((soundLevel($T165, $AB165, BD165, $Y165, $W165,$AJ165,$AA165,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T165, $AB165, BD165, $Y165, $W165,$AJ165,$AA165,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T165, $AB165, BD165, $Y165, $W165,$AJ165,$AA165,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T165=\"Select Model\",\"\",IF($T165=\"LIU24_2W\",calcQwIP($Y165,$W165,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC165,$AI165,\"latent\",$U165&\"P\"&IF($V165=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T165,activeElevation),\"\"))","v":""},{"$f":"IF($T165=\"Select Model\",\"\",IF($T165=\"ACBC_1W\",calcQwIP($Y165,$W165,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC165,BD165,\"capacity\",$U165&\"P\"&IF($V165=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T165,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y165,$W165,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC165,BD165,\"capacity\",$U165&\"P\"&IF($V165=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T165,activeElevation)))","v":""},"",{"$f":"IF(T165=\"Select Model\", 0,waterPressureDrop(W165, U165 & \"P\" & IF(V165=\"Dual\",2,1) &\"C\", AC165, \"cooling\", T165))","v":0},{"$f":"IF(T165=\"Select Model\", \"\",getReturnWaterTemp(T165,AC165, activeEWTCooling, AS165, \"cooling\"))","v":""},"",{"$f":"IF($T165<>\"ACBC_1W\",\"\",IF($J165=\"\",\"\",FintubeCapacity($T165,$W165,$AE165,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T165=\"Select Model\",T165=\"PCBL\"),\"\",calcQwIP(Y165,W165,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD165,BD165,\"capacity\",U165&\"P\"&IF(V165=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T165,activeElevation))","v":""},"",{"$f":"IF(OR(T165=\"Select Model\",T165=\"PCBL\"), \"\",IF(AY165=0,\"N/A\",waterPressureDrop(W165, U165 & \"P\" & IF(V165=\"Dual\",2,1) &\"C\", AD165, \"heating\", T165)))","v":""},{"$f":"IF(OR(T165=\"Select Model\",T165=\"PCBL\"), \"\",IF(AY165=0,getReturnWaterTemp(T165,AE165, activeEWTHeating, AX165, \"heating\"),getReturnWaterTemp(T165,AD165, activeEWTHeating, AY165, \"heating\")))","v":""},"",{"$f":" getNozzle(T165, W165, Y165, Z165, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I166)),I166<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I166, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H166)),H166<0),\"\",intlEstQuantity(T166, W166*12, H166)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T166=\"Select Model\",\"\",coilCircuitChange(W166, U166, AC166, T166,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T166=\"Select Model\",\"\",beamWidth(T166))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T166=\"Select Model\",T166=\"PCBL\"), 0,getSPIP(T166, W166, Y166, BD166, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T166=\"Select Model\", \"\",IF(T166=\"PCBL\",0,primaryAirSensibleCapacityIP($T166,$W166,activeRoomTempCooling,activePriAirTempCooling,$Y166,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T166=\"Select Model\",\"\",IF($T166=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y166,activeElevation)))","v":""},{"$f":"IF(OR(T166=\"Select Model\",T166=\"PCBL\"), 0,IF(AD166=0,0,-primaryAirSensibleCapacityIP($T166,$W166,activeRoomTempHeating,activePriAirTempHeating,$Y166,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T166=\"Select Model\", \"\", InductionRatio($T166,BD166,$W166,$Y166)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T166=\"Select Model\", \"\",IF($T166=\"PCBL\",\"N/A\",minVAVSetBack(AA166, Y166))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T166=\"Select Model\", \"\",IF($T166= \"PCBL\",\"N/A\",getDischargeAirTemp($T166,$V166,$AC166,$W166,BD166,$AL166, $Y166, $AS166, \"cooling\",activeElevation,$AB166,$AJ166,$AV166,$BB166))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T166=\"Select Model\",$T166=\"PCBL\"), \"\",getDischargeAirTemp($T166,$V166,$AD166,$W166,BD166,$AL166, $Y166, $AY166, \"heating\",activeElevation,$AB166,$AJ166,$AV166,$BB166)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T166=\"Select Model\", \"\",IF(OR($T166=\"ACBC_1W\",$T166=\"ACBC_2W\",LEFT($T166,4)=\"ACBR\",$T166 = \"LIU24_2W\",LEFT($T166,3)=\"RIU\",LEFT($T166,6)=\"ACBL12\"), IF((soundLevel($T166, $AB166, BD166, $Y166, $W166,$AJ166,$AA166,\"dba\"))<15,\"<15\",soundLevel($T166, $AB166, BD166, $Y166, $W166,$AJ166,$AA166,\"dba\")+0.4),IF((soundLevel($T166, $AB166, BD166, $Y166, $W166,$AJ166,$AA166,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T166, $AB166, BD166, $Y166, $W166,$AJ166,$AA166,\"dba\")+5)<15, \"<15\", soundLevel($T166, $AB166, BD166,$Y166, $W166,$AJ166,$AA166,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T166=\"Select Model\", \"\",IF(OR($T166=\"ACBC_1W\",$T166=\"ACBC_2W\",LEFT($T166,4)=\"ACBR\",$T166=\"LIU24_2W\",LEFT($T166,3)=\"RIU\",LEFT($T166,6)=\"ACBL12\"), IF((soundLevel($T166, $AB166, BD166, $Y166, $W166,$AJ166,$AA166,\"NC\"))<15,\"<15\",soundLevel($T166, $AB166, BD166, $Y166, $W166,$AJ166,$AA166,\"NC\")+0.4),IF((soundLevel($T166, $AB166, BD166, $Y166, $W166,$AJ166,$AA166,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T166, $AB166, BD166, $Y166, $W166,$AJ166,$AA166,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T166, $AB166, BD166, $Y166, $W166,$AJ166,$AA166,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T166=\"Select Model\",\"\",IF($T166=\"LIU24_2W\",calcQwIP($Y166,$W166,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC166,$AI166,\"latent\",$U166&\"P\"&IF($V166=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T166,activeElevation),\"\"))","v":""},{"$f":"IF($T166=\"Select Model\",\"\",IF($T166=\"ACBC_1W\",calcQwIP($Y166,$W166,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC166,BD166,\"capacity\",$U166&\"P\"&IF($V166=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T166,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y166,$W166,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC166,BD166,\"capacity\",$U166&\"P\"&IF($V166=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T166,activeElevation)))","v":""},"",{"$f":"IF(T166=\"Select Model\", 0,waterPressureDrop(W166, U166 & \"P\" & IF(V166=\"Dual\",2,1) &\"C\", AC166, \"cooling\", T166))","v":0},{"$f":"IF(T166=\"Select Model\", \"\",getReturnWaterTemp(T166,AC166, activeEWTCooling, AS166, \"cooling\"))","v":""},"",{"$f":"IF($T166<>\"ACBC_1W\",\"\",IF($J166=\"\",\"\",FintubeCapacity($T166,$W166,$AE166,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T166=\"Select Model\",T166=\"PCBL\"),\"\",calcQwIP(Y166,W166,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD166,BD166,\"capacity\",U166&\"P\"&IF(V166=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T166,activeElevation))","v":""},"",{"$f":"IF(OR(T166=\"Select Model\",T166=\"PCBL\"), \"\",IF(AY166=0,\"N/A\",waterPressureDrop(W166, U166 & \"P\" & IF(V166=\"Dual\",2,1) &\"C\", AD166, \"heating\", T166)))","v":""},{"$f":"IF(OR(T166=\"Select Model\",T166=\"PCBL\"), \"\",IF(AY166=0,getReturnWaterTemp(T166,AE166, activeEWTHeating, AX166, \"heating\"),getReturnWaterTemp(T166,AD166, activeEWTHeating, AY166, \"heating\")))","v":""},"",{"$f":" getNozzle(T166, W166, Y166, Z166, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I167)),I167<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I167, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H167)),H167<0),\"\",intlEstQuantity(T167, W167*12, H167)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T167=\"Select Model\",\"\",coilCircuitChange(W167, U167, AC167, T167,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T167=\"Select Model\",\"\",beamWidth(T167))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T167=\"Select Model\",T167=\"PCBL\"), 0,getSPIP(T167, W167, Y167, BD167, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T167=\"Select Model\", \"\",IF(T167=\"PCBL\",0,primaryAirSensibleCapacityIP($T167,$W167,activeRoomTempCooling,activePriAirTempCooling,$Y167,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T167=\"Select Model\",\"\",IF($T167=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y167,activeElevation)))","v":""},{"$f":"IF(OR(T167=\"Select Model\",T167=\"PCBL\"), 0,IF(AD167=0,0,-primaryAirSensibleCapacityIP($T167,$W167,activeRoomTempHeating,activePriAirTempHeating,$Y167,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T167=\"Select Model\", \"\", InductionRatio($T167,BD167,$W167,$Y167)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T167=\"Select Model\", \"\",IF($T167=\"PCBL\",\"N/A\",minVAVSetBack(AA167, Y167))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T167=\"Select Model\", \"\",IF($T167= \"PCBL\",\"N/A\",getDischargeAirTemp($T167,$V167,$AC167,$W167,BD167,$AL167, $Y167, $AS167, \"cooling\",activeElevation,$AB167,$AJ167,$AV167,$BB167))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T167=\"Select Model\",$T167=\"PCBL\"), \"\",getDischargeAirTemp($T167,$V167,$AD167,$W167,BD167,$AL167, $Y167, $AY167, \"heating\",activeElevation,$AB167,$AJ167,$AV167,$BB167)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T167=\"Select Model\", \"\",IF(OR($T167=\"ACBC_1W\",$T167=\"ACBC_2W\",LEFT($T167,4)=\"ACBR\",$T167 = \"LIU24_2W\",LEFT($T167,3)=\"RIU\",LEFT($T167,6)=\"ACBL12\"), IF((soundLevel($T167, $AB167, BD167, $Y167, $W167,$AJ167,$AA167,\"dba\"))<15,\"<15\",soundLevel($T167, $AB167, BD167, $Y167, $W167,$AJ167,$AA167,\"dba\")+0.4),IF((soundLevel($T167, $AB167, BD167, $Y167, $W167,$AJ167,$AA167,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T167, $AB167, BD167, $Y167, $W167,$AJ167,$AA167,\"dba\")+5)<15, \"<15\", soundLevel($T167, $AB167, BD167,$Y167, $W167,$AJ167,$AA167,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T167=\"Select Model\", \"\",IF(OR($T167=\"ACBC_1W\",$T167=\"ACBC_2W\",LEFT($T167,4)=\"ACBR\",$T167=\"LIU24_2W\",LEFT($T167,3)=\"RIU\",LEFT($T167,6)=\"ACBL12\"), IF((soundLevel($T167, $AB167, BD167, $Y167, $W167,$AJ167,$AA167,\"NC\"))<15,\"<15\",soundLevel($T167, $AB167, BD167, $Y167, $W167,$AJ167,$AA167,\"NC\")+0.4),IF((soundLevel($T167, $AB167, BD167, $Y167, $W167,$AJ167,$AA167,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T167, $AB167, BD167, $Y167, $W167,$AJ167,$AA167,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T167, $AB167, BD167, $Y167, $W167,$AJ167,$AA167,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T167=\"Select Model\",\"\",IF($T167=\"LIU24_2W\",calcQwIP($Y167,$W167,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC167,$AI167,\"latent\",$U167&\"P\"&IF($V167=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T167,activeElevation),\"\"))","v":""},{"$f":"IF($T167=\"Select Model\",\"\",IF($T167=\"ACBC_1W\",calcQwIP($Y167,$W167,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC167,BD167,\"capacity\",$U167&\"P\"&IF($V167=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T167,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y167,$W167,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC167,BD167,\"capacity\",$U167&\"P\"&IF($V167=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T167,activeElevation)))","v":""},"",{"$f":"IF(T167=\"Select Model\", 0,waterPressureDrop(W167, U167 & \"P\" & IF(V167=\"Dual\",2,1) &\"C\", AC167, \"cooling\", T167))","v":0},{"$f":"IF(T167=\"Select Model\", \"\",getReturnWaterTemp(T167,AC167, activeEWTCooling, AS167, \"cooling\"))","v":""},"",{"$f":"IF($T167<>\"ACBC_1W\",\"\",IF($J167=\"\",\"\",FintubeCapacity($T167,$W167,$AE167,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T167=\"Select Model\",T167=\"PCBL\"),\"\",calcQwIP(Y167,W167,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD167,BD167,\"capacity\",U167&\"P\"&IF(V167=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T167,activeElevation))","v":""},"",{"$f":"IF(OR(T167=\"Select Model\",T167=\"PCBL\"), \"\",IF(AY167=0,\"N/A\",waterPressureDrop(W167, U167 & \"P\" & IF(V167=\"Dual\",2,1) &\"C\", AD167, \"heating\", T167)))","v":""},{"$f":"IF(OR(T167=\"Select Model\",T167=\"PCBL\"), \"\",IF(AY167=0,getReturnWaterTemp(T167,AE167, activeEWTHeating, AX167, \"heating\"),getReturnWaterTemp(T167,AD167, activeEWTHeating, AY167, \"heating\")))","v":""},"",{"$f":" getNozzle(T167, W167, Y167, Z167, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I168)),I168<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I168, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H168)),H168<0),\"\",intlEstQuantity(T168, W168*12, H168)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T168=\"Select Model\",\"\",coilCircuitChange(W168, U168, AC168, T168,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T168=\"Select Model\",\"\",beamWidth(T168))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T168=\"Select Model\",T168=\"PCBL\"), 0,getSPIP(T168, W168, Y168, BD168, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T168=\"Select Model\", \"\",IF(T168=\"PCBL\",0,primaryAirSensibleCapacityIP($T168,$W168,activeRoomTempCooling,activePriAirTempCooling,$Y168,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T168=\"Select Model\",\"\",IF($T168=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y168,activeElevation)))","v":""},{"$f":"IF(OR(T168=\"Select Model\",T168=\"PCBL\"), 0,IF(AD168=0,0,-primaryAirSensibleCapacityIP($T168,$W168,activeRoomTempHeating,activePriAirTempHeating,$Y168,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T168=\"Select Model\", \"\", InductionRatio($T168,BD168,$W168,$Y168)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T168=\"Select Model\", \"\",IF($T168=\"PCBL\",\"N/A\",minVAVSetBack(AA168, Y168))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T168=\"Select Model\", \"\",IF($T168= \"PCBL\",\"N/A\",getDischargeAirTemp($T168,$V168,$AC168,$W168,BD168,$AL168, $Y168, $AS168, \"cooling\",activeElevation,$AB168,$AJ168,$AV168,$BB168))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T168=\"Select Model\",$T168=\"PCBL\"), \"\",getDischargeAirTemp($T168,$V168,$AD168,$W168,BD168,$AL168, $Y168, $AY168, \"heating\",activeElevation,$AB168,$AJ168,$AV168,$BB168)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T168=\"Select Model\", \"\",IF(OR($T168=\"ACBC_1W\",$T168=\"ACBC_2W\",LEFT($T168,4)=\"ACBR\",$T168 = \"LIU24_2W\",LEFT($T168,3)=\"RIU\",LEFT($T168,6)=\"ACBL12\"), IF((soundLevel($T168, $AB168, BD168, $Y168, $W168,$AJ168,$AA168,\"dba\"))<15,\"<15\",soundLevel($T168, $AB168, BD168, $Y168, $W168,$AJ168,$AA168,\"dba\")+0.4),IF((soundLevel($T168, $AB168, BD168, $Y168, $W168,$AJ168,$AA168,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T168, $AB168, BD168, $Y168, $W168,$AJ168,$AA168,\"dba\")+5)<15, \"<15\", soundLevel($T168, $AB168, BD168,$Y168, $W168,$AJ168,$AA168,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T168=\"Select Model\", \"\",IF(OR($T168=\"ACBC_1W\",$T168=\"ACBC_2W\",LEFT($T168,4)=\"ACBR\",$T168=\"LIU24_2W\",LEFT($T168,3)=\"RIU\",LEFT($T168,6)=\"ACBL12\"), IF((soundLevel($T168, $AB168, BD168, $Y168, $W168,$AJ168,$AA168,\"NC\"))<15,\"<15\",soundLevel($T168, $AB168, BD168, $Y168, $W168,$AJ168,$AA168,\"NC\")+0.4),IF((soundLevel($T168, $AB168, BD168, $Y168, $W168,$AJ168,$AA168,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T168, $AB168, BD168, $Y168, $W168,$AJ168,$AA168,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T168, $AB168, BD168, $Y168, $W168,$AJ168,$AA168,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T168=\"Select Model\",\"\",IF($T168=\"LIU24_2W\",calcQwIP($Y168,$W168,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC168,$AI168,\"latent\",$U168&\"P\"&IF($V168=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T168,activeElevation),\"\"))","v":""},{"$f":"IF($T168=\"Select Model\",\"\",IF($T168=\"ACBC_1W\",calcQwIP($Y168,$W168,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC168,BD168,\"capacity\",$U168&\"P\"&IF($V168=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T168,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y168,$W168,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC168,BD168,\"capacity\",$U168&\"P\"&IF($V168=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T168,activeElevation)))","v":""},"",{"$f":"IF(T168=\"Select Model\", 0,waterPressureDrop(W168, U168 & \"P\" & IF(V168=\"Dual\",2,1) &\"C\", AC168, \"cooling\", T168))","v":0},{"$f":"IF(T168=\"Select Model\", \"\",getReturnWaterTemp(T168,AC168, activeEWTCooling, AS168, \"cooling\"))","v":""},"",{"$f":"IF($T168<>\"ACBC_1W\",\"\",IF($J168=\"\",\"\",FintubeCapacity($T168,$W168,$AE168,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T168=\"Select Model\",T168=\"PCBL\"),\"\",calcQwIP(Y168,W168,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD168,BD168,\"capacity\",U168&\"P\"&IF(V168=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T168,activeElevation))","v":""},"",{"$f":"IF(OR(T168=\"Select Model\",T168=\"PCBL\"), \"\",IF(AY168=0,\"N/A\",waterPressureDrop(W168, U168 & \"P\" & IF(V168=\"Dual\",2,1) &\"C\", AD168, \"heating\", T168)))","v":""},{"$f":"IF(OR(T168=\"Select Model\",T168=\"PCBL\"), \"\",IF(AY168=0,getReturnWaterTemp(T168,AE168, activeEWTHeating, AX168, \"heating\"),getReturnWaterTemp(T168,AD168, activeEWTHeating, AY168, \"heating\")))","v":""},"",{"$f":" getNozzle(T168, W168, Y168, Z168, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I169)),I169<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I169, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H169)),H169<0),\"\",intlEstQuantity(T169, W169*12, H169)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T169=\"Select Model\",\"\",coilCircuitChange(W169, U169, AC169, T169,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T169=\"Select Model\",\"\",beamWidth(T169))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T169=\"Select Model\",T169=\"PCBL\"), 0,getSPIP(T169, W169, Y169, BD169, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T169=\"Select Model\", \"\",IF(T169=\"PCBL\",0,primaryAirSensibleCapacityIP($T169,$W169,activeRoomTempCooling,activePriAirTempCooling,$Y169,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T169=\"Select Model\",\"\",IF($T169=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y169,activeElevation)))","v":""},{"$f":"IF(OR(T169=\"Select Model\",T169=\"PCBL\"), 0,IF(AD169=0,0,-primaryAirSensibleCapacityIP($T169,$W169,activeRoomTempHeating,activePriAirTempHeating,$Y169,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T169=\"Select Model\", \"\", InductionRatio($T169,BD169,$W169,$Y169)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T169=\"Select Model\", \"\",IF($T169=\"PCBL\",\"N/A\",minVAVSetBack(AA169, Y169))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T169=\"Select Model\", \"\",IF($T169= \"PCBL\",\"N/A\",getDischargeAirTemp($T169,$V169,$AC169,$W169,BD169,$AL169, $Y169, $AS169, \"cooling\",activeElevation,$AB169,$AJ169,$AV169,$BB169))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T169=\"Select Model\",$T169=\"PCBL\"), \"\",getDischargeAirTemp($T169,$V169,$AD169,$W169,BD169,$AL169, $Y169, $AY169, \"heating\",activeElevation,$AB169,$AJ169,$AV169,$BB169)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T169=\"Select Model\", \"\",IF(OR($T169=\"ACBC_1W\",$T169=\"ACBC_2W\",LEFT($T169,4)=\"ACBR\",$T169 = \"LIU24_2W\",LEFT($T169,3)=\"RIU\",LEFT($T169,6)=\"ACBL12\"), IF((soundLevel($T169, $AB169, BD169, $Y169, $W169,$AJ169,$AA169,\"dba\"))<15,\"<15\",soundLevel($T169, $AB169, BD169, $Y169, $W169,$AJ169,$AA169,\"dba\")+0.4),IF((soundLevel($T169, $AB169, BD169, $Y169, $W169,$AJ169,$AA169,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T169, $AB169, BD169, $Y169, $W169,$AJ169,$AA169,\"dba\")+5)<15, \"<15\", soundLevel($T169, $AB169, BD169,$Y169, $W169,$AJ169,$AA169,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T169=\"Select Model\", \"\",IF(OR($T169=\"ACBC_1W\",$T169=\"ACBC_2W\",LEFT($T169,4)=\"ACBR\",$T169=\"LIU24_2W\",LEFT($T169,3)=\"RIU\",LEFT($T169,6)=\"ACBL12\"), IF((soundLevel($T169, $AB169, BD169, $Y169, $W169,$AJ169,$AA169,\"NC\"))<15,\"<15\",soundLevel($T169, $AB169, BD169, $Y169, $W169,$AJ169,$AA169,\"NC\")+0.4),IF((soundLevel($T169, $AB169, BD169, $Y169, $W169,$AJ169,$AA169,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T169, $AB169, BD169, $Y169, $W169,$AJ169,$AA169,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T169, $AB169, BD169, $Y169, $W169,$AJ169,$AA169,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T169=\"Select Model\",\"\",IF($T169=\"LIU24_2W\",calcQwIP($Y169,$W169,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC169,$AI169,\"latent\",$U169&\"P\"&IF($V169=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T169,activeElevation),\"\"))","v":""},{"$f":"IF($T169=\"Select Model\",\"\",IF($T169=\"ACBC_1W\",calcQwIP($Y169,$W169,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC169,BD169,\"capacity\",$U169&\"P\"&IF($V169=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T169,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y169,$W169,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC169,BD169,\"capacity\",$U169&\"P\"&IF($V169=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T169,activeElevation)))","v":""},"",{"$f":"IF(T169=\"Select Model\", 0,waterPressureDrop(W169, U169 & \"P\" & IF(V169=\"Dual\",2,1) &\"C\", AC169, \"cooling\", T169))","v":0},{"$f":"IF(T169=\"Select Model\", \"\",getReturnWaterTemp(T169,AC169, activeEWTCooling, AS169, \"cooling\"))","v":""},"",{"$f":"IF($T169<>\"ACBC_1W\",\"\",IF($J169=\"\",\"\",FintubeCapacity($T169,$W169,$AE169,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T169=\"Select Model\",T169=\"PCBL\"),\"\",calcQwIP(Y169,W169,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD169,BD169,\"capacity\",U169&\"P\"&IF(V169=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T169,activeElevation))","v":""},"",{"$f":"IF(OR(T169=\"Select Model\",T169=\"PCBL\"), \"\",IF(AY169=0,\"N/A\",waterPressureDrop(W169, U169 & \"P\" & IF(V169=\"Dual\",2,1) &\"C\", AD169, \"heating\", T169)))","v":""},{"$f":"IF(OR(T169=\"Select Model\",T169=\"PCBL\"), \"\",IF(AY169=0,getReturnWaterTemp(T169,AE169, activeEWTHeating, AX169, \"heating\"),getReturnWaterTemp(T169,AD169, activeEWTHeating, AY169, \"heating\")))","v":""},"",{"$f":" getNozzle(T169, W169, Y169, Z169, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I170)),I170<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I170, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H170)),H170<0),\"\",intlEstQuantity(T170, W170*12, H170)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T170=\"Select Model\",\"\",coilCircuitChange(W170, U170, AC170, T170,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T170=\"Select Model\",\"\",beamWidth(T170))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T170=\"Select Model\",T170=\"PCBL\"), 0,getSPIP(T170, W170, Y170, BD170, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T170=\"Select Model\", \"\",IF(T170=\"PCBL\",0,primaryAirSensibleCapacityIP($T170,$W170,activeRoomTempCooling,activePriAirTempCooling,$Y170,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T170=\"Select Model\",\"\",IF($T170=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y170,activeElevation)))","v":""},{"$f":"IF(OR(T170=\"Select Model\",T170=\"PCBL\"), 0,IF(AD170=0,0,-primaryAirSensibleCapacityIP($T170,$W170,activeRoomTempHeating,activePriAirTempHeating,$Y170,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T170=\"Select Model\", \"\", InductionRatio($T170,BD170,$W170,$Y170)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T170=\"Select Model\", \"\",IF($T170=\"PCBL\",\"N/A\",minVAVSetBack(AA170, Y170))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T170=\"Select Model\", \"\",IF($T170= \"PCBL\",\"N/A\",getDischargeAirTemp($T170,$V170,$AC170,$W170,BD170,$AL170, $Y170, $AS170, \"cooling\",activeElevation,$AB170,$AJ170,$AV170,$BB170))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T170=\"Select Model\",$T170=\"PCBL\"), \"\",getDischargeAirTemp($T170,$V170,$AD170,$W170,BD170,$AL170, $Y170, $AY170, \"heating\",activeElevation,$AB170,$AJ170,$AV170,$BB170)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T170=\"Select Model\", \"\",IF(OR($T170=\"ACBC_1W\",$T170=\"ACBC_2W\",LEFT($T170,4)=\"ACBR\",$T170 = \"LIU24_2W\",LEFT($T170,3)=\"RIU\",LEFT($T170,6)=\"ACBL12\"), IF((soundLevel($T170, $AB170, BD170, $Y170, $W170,$AJ170,$AA170,\"dba\"))<15,\"<15\",soundLevel($T170, $AB170, BD170, $Y170, $W170,$AJ170,$AA170,\"dba\")+0.4),IF((soundLevel($T170, $AB170, BD170, $Y170, $W170,$AJ170,$AA170,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T170, $AB170, BD170, $Y170, $W170,$AJ170,$AA170,\"dba\")+5)<15, \"<15\", soundLevel($T170, $AB170, BD170,$Y170, $W170,$AJ170,$AA170,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T170=\"Select Model\", \"\",IF(OR($T170=\"ACBC_1W\",$T170=\"ACBC_2W\",LEFT($T170,4)=\"ACBR\",$T170=\"LIU24_2W\",LEFT($T170,3)=\"RIU\",LEFT($T170,6)=\"ACBL12\"), IF((soundLevel($T170, $AB170, BD170, $Y170, $W170,$AJ170,$AA170,\"NC\"))<15,\"<15\",soundLevel($T170, $AB170, BD170, $Y170, $W170,$AJ170,$AA170,\"NC\")+0.4),IF((soundLevel($T170, $AB170, BD170, $Y170, $W170,$AJ170,$AA170,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T170, $AB170, BD170, $Y170, $W170,$AJ170,$AA170,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T170, $AB170, BD170, $Y170, $W170,$AJ170,$AA170,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T170=\"Select Model\",\"\",IF($T170=\"LIU24_2W\",calcQwIP($Y170,$W170,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC170,$AI170,\"latent\",$U170&\"P\"&IF($V170=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T170,activeElevation),\"\"))","v":""},{"$f":"IF($T170=\"Select Model\",\"\",IF($T170=\"ACBC_1W\",calcQwIP($Y170,$W170,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC170,BD170,\"capacity\",$U170&\"P\"&IF($V170=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T170,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y170,$W170,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC170,BD170,\"capacity\",$U170&\"P\"&IF($V170=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T170,activeElevation)))","v":""},"",{"$f":"IF(T170=\"Select Model\", 0,waterPressureDrop(W170, U170 & \"P\" & IF(V170=\"Dual\",2,1) &\"C\", AC170, \"cooling\", T170))","v":0},{"$f":"IF(T170=\"Select Model\", \"\",getReturnWaterTemp(T170,AC170, activeEWTCooling, AS170, \"cooling\"))","v":""},"",{"$f":"IF($T170<>\"ACBC_1W\",\"\",IF($J170=\"\",\"\",FintubeCapacity($T170,$W170,$AE170,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T170=\"Select Model\",T170=\"PCBL\"),\"\",calcQwIP(Y170,W170,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD170,BD170,\"capacity\",U170&\"P\"&IF(V170=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T170,activeElevation))","v":""},"",{"$f":"IF(OR(T170=\"Select Model\",T170=\"PCBL\"), \"\",IF(AY170=0,\"N/A\",waterPressureDrop(W170, U170 & \"P\" & IF(V170=\"Dual\",2,1) &\"C\", AD170, \"heating\", T170)))","v":""},{"$f":"IF(OR(T170=\"Select Model\",T170=\"PCBL\"), \"\",IF(AY170=0,getReturnWaterTemp(T170,AE170, activeEWTHeating, AX170, \"heating\"),getReturnWaterTemp(T170,AD170, activeEWTHeating, AY170, \"heating\")))","v":""},"",{"$f":" getNozzle(T170, W170, Y170, Z170, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I171)),I171<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I171, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H171)),H171<0),\"\",intlEstQuantity(T171, W171*12, H171)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T171=\"Select Model\",\"\",coilCircuitChange(W171, U171, AC171, T171,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T171=\"Select Model\",\"\",beamWidth(T171))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T171=\"Select Model\",T171=\"PCBL\"), 0,getSPIP(T171, W171, Y171, BD171, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T171=\"Select Model\", \"\",IF(T171=\"PCBL\",0,primaryAirSensibleCapacityIP($T171,$W171,activeRoomTempCooling,activePriAirTempCooling,$Y171,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T171=\"Select Model\",\"\",IF($T171=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y171,activeElevation)))","v":""},{"$f":"IF(OR(T171=\"Select Model\",T171=\"PCBL\"), 0,IF(AD171=0,0,-primaryAirSensibleCapacityIP($T171,$W171,activeRoomTempHeating,activePriAirTempHeating,$Y171,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T171=\"Select Model\", \"\", InductionRatio($T171,BD171,$W171,$Y171)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T171=\"Select Model\", \"\",IF($T171=\"PCBL\",\"N/A\",minVAVSetBack(AA171, Y171))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T171=\"Select Model\", \"\",IF($T171= \"PCBL\",\"N/A\",getDischargeAirTemp($T171,$V171,$AC171,$W171,BD171,$AL171, $Y171, $AS171, \"cooling\",activeElevation,$AB171,$AJ171,$AV171,$BB171))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T171=\"Select Model\",$T171=\"PCBL\"), \"\",getDischargeAirTemp($T171,$V171,$AD171,$W171,BD171,$AL171, $Y171, $AY171, \"heating\",activeElevation,$AB171,$AJ171,$AV171,$BB171)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T171=\"Select Model\", \"\",IF(OR($T171=\"ACBC_1W\",$T171=\"ACBC_2W\",LEFT($T171,4)=\"ACBR\",$T171 = \"LIU24_2W\",LEFT($T171,3)=\"RIU\",LEFT($T171,6)=\"ACBL12\"), IF((soundLevel($T171, $AB171, BD171, $Y171, $W171,$AJ171,$AA171,\"dba\"))<15,\"<15\",soundLevel($T171, $AB171, BD171, $Y171, $W171,$AJ171,$AA171,\"dba\")+0.4),IF((soundLevel($T171, $AB171, BD171, $Y171, $W171,$AJ171,$AA171,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T171, $AB171, BD171, $Y171, $W171,$AJ171,$AA171,\"dba\")+5)<15, \"<15\", soundLevel($T171, $AB171, BD171,$Y171, $W171,$AJ171,$AA171,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T171=\"Select Model\", \"\",IF(OR($T171=\"ACBC_1W\",$T171=\"ACBC_2W\",LEFT($T171,4)=\"ACBR\",$T171=\"LIU24_2W\",LEFT($T171,3)=\"RIU\",LEFT($T171,6)=\"ACBL12\"), IF((soundLevel($T171, $AB171, BD171, $Y171, $W171,$AJ171,$AA171,\"NC\"))<15,\"<15\",soundLevel($T171, $AB171, BD171, $Y171, $W171,$AJ171,$AA171,\"NC\")+0.4),IF((soundLevel($T171, $AB171, BD171, $Y171, $W171,$AJ171,$AA171,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T171, $AB171, BD171, $Y171, $W171,$AJ171,$AA171,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T171, $AB171, BD171, $Y171, $W171,$AJ171,$AA171,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T171=\"Select Model\",\"\",IF($T171=\"LIU24_2W\",calcQwIP($Y171,$W171,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC171,$AI171,\"latent\",$U171&\"P\"&IF($V171=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T171,activeElevation),\"\"))","v":""},{"$f":"IF($T171=\"Select Model\",\"\",IF($T171=\"ACBC_1W\",calcQwIP($Y171,$W171,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC171,BD171,\"capacity\",$U171&\"P\"&IF($V171=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T171,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y171,$W171,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC171,BD171,\"capacity\",$U171&\"P\"&IF($V171=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T171,activeElevation)))","v":""},"",{"$f":"IF(T171=\"Select Model\", 0,waterPressureDrop(W171, U171 & \"P\" & IF(V171=\"Dual\",2,1) &\"C\", AC171, \"cooling\", T171))","v":0},{"$f":"IF(T171=\"Select Model\", \"\",getReturnWaterTemp(T171,AC171, activeEWTCooling, AS171, \"cooling\"))","v":""},"",{"$f":"IF($T171<>\"ACBC_1W\",\"\",IF($J171=\"\",\"\",FintubeCapacity($T171,$W171,$AE171,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T171=\"Select Model\",T171=\"PCBL\"),\"\",calcQwIP(Y171,W171,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD171,BD171,\"capacity\",U171&\"P\"&IF(V171=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T171,activeElevation))","v":""},"",{"$f":"IF(OR(T171=\"Select Model\",T171=\"PCBL\"), \"\",IF(AY171=0,\"N/A\",waterPressureDrop(W171, U171 & \"P\" & IF(V171=\"Dual\",2,1) &\"C\", AD171, \"heating\", T171)))","v":""},{"$f":"IF(OR(T171=\"Select Model\",T171=\"PCBL\"), \"\",IF(AY171=0,getReturnWaterTemp(T171,AE171, activeEWTHeating, AX171, \"heating\"),getReturnWaterTemp(T171,AD171, activeEWTHeating, AY171, \"heating\")))","v":""},"",{"$f":" getNozzle(T171, W171, Y171, Z171, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I172)),I172<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I172, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H172)),H172<0),\"\",intlEstQuantity(T172, W172*12, H172)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T172=\"Select Model\",\"\",coilCircuitChange(W172, U172, AC172, T172,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T172=\"Select Model\",\"\",beamWidth(T172))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T172=\"Select Model\",T172=\"PCBL\"), 0,getSPIP(T172, W172, Y172, BD172, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T172=\"Select Model\", \"\",IF(T172=\"PCBL\",0,primaryAirSensibleCapacityIP($T172,$W172,activeRoomTempCooling,activePriAirTempCooling,$Y172,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T172=\"Select Model\",\"\",IF($T172=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y172,activeElevation)))","v":""},{"$f":"IF(OR(T172=\"Select Model\",T172=\"PCBL\"), 0,IF(AD172=0,0,-primaryAirSensibleCapacityIP($T172,$W172,activeRoomTempHeating,activePriAirTempHeating,$Y172,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T172=\"Select Model\", \"\", InductionRatio($T172,BD172,$W172,$Y172)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T172=\"Select Model\", \"\",IF($T172=\"PCBL\",\"N/A\",minVAVSetBack(AA172, Y172))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T172=\"Select Model\", \"\",IF($T172= \"PCBL\",\"N/A\",getDischargeAirTemp($T172,$V172,$AC172,$W172,BD172,$AL172, $Y172, $AS172, \"cooling\",activeElevation,$AB172,$AJ172,$AV172,$BB172))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T172=\"Select Model\",$T172=\"PCBL\"), \"\",getDischargeAirTemp($T172,$V172,$AD172,$W172,BD172,$AL172, $Y172, $AY172, \"heating\",activeElevation,$AB172,$AJ172,$AV172,$BB172)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T172=\"Select Model\", \"\",IF(OR($T172=\"ACBC_1W\",$T172=\"ACBC_2W\",LEFT($T172,4)=\"ACBR\",$T172 = \"LIU24_2W\",LEFT($T172,3)=\"RIU\",LEFT($T172,6)=\"ACBL12\"), IF((soundLevel($T172, $AB172, BD172, $Y172, $W172,$AJ172,$AA172,\"dba\"))<15,\"<15\",soundLevel($T172, $AB172, BD172, $Y172, $W172,$AJ172,$AA172,\"dba\")+0.4),IF((soundLevel($T172, $AB172, BD172, $Y172, $W172,$AJ172,$AA172,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T172, $AB172, BD172, $Y172, $W172,$AJ172,$AA172,\"dba\")+5)<15, \"<15\", soundLevel($T172, $AB172, BD172,$Y172, $W172,$AJ172,$AA172,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T172=\"Select Model\", \"\",IF(OR($T172=\"ACBC_1W\",$T172=\"ACBC_2W\",LEFT($T172,4)=\"ACBR\",$T172=\"LIU24_2W\",LEFT($T172,3)=\"RIU\",LEFT($T172,6)=\"ACBL12\"), IF((soundLevel($T172, $AB172, BD172, $Y172, $W172,$AJ172,$AA172,\"NC\"))<15,\"<15\",soundLevel($T172, $AB172, BD172, $Y172, $W172,$AJ172,$AA172,\"NC\")+0.4),IF((soundLevel($T172, $AB172, BD172, $Y172, $W172,$AJ172,$AA172,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T172, $AB172, BD172, $Y172, $W172,$AJ172,$AA172,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T172, $AB172, BD172, $Y172, $W172,$AJ172,$AA172,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T172=\"Select Model\",\"\",IF($T172=\"LIU24_2W\",calcQwIP($Y172,$W172,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC172,$AI172,\"latent\",$U172&\"P\"&IF($V172=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T172,activeElevation),\"\"))","v":""},{"$f":"IF($T172=\"Select Model\",\"\",IF($T172=\"ACBC_1W\",calcQwIP($Y172,$W172,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC172,BD172,\"capacity\",$U172&\"P\"&IF($V172=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T172,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y172,$W172,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC172,BD172,\"capacity\",$U172&\"P\"&IF($V172=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T172,activeElevation)))","v":""},"",{"$f":"IF(T172=\"Select Model\", 0,waterPressureDrop(W172, U172 & \"P\" & IF(V172=\"Dual\",2,1) &\"C\", AC172, \"cooling\", T172))","v":0},{"$f":"IF(T172=\"Select Model\", \"\",getReturnWaterTemp(T172,AC172, activeEWTCooling, AS172, \"cooling\"))","v":""},"",{"$f":"IF($T172<>\"ACBC_1W\",\"\",IF($J172=\"\",\"\",FintubeCapacity($T172,$W172,$AE172,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T172=\"Select Model\",T172=\"PCBL\"),\"\",calcQwIP(Y172,W172,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD172,BD172,\"capacity\",U172&\"P\"&IF(V172=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T172,activeElevation))","v":""},"",{"$f":"IF(OR(T172=\"Select Model\",T172=\"PCBL\"), \"\",IF(AY172=0,\"N/A\",waterPressureDrop(W172, U172 & \"P\" & IF(V172=\"Dual\",2,1) &\"C\", AD172, \"heating\", T172)))","v":""},{"$f":"IF(OR(T172=\"Select Model\",T172=\"PCBL\"), \"\",IF(AY172=0,getReturnWaterTemp(T172,AE172, activeEWTHeating, AX172, \"heating\"),getReturnWaterTemp(T172,AD172, activeEWTHeating, AY172, \"heating\")))","v":""},"",{"$f":" getNozzle(T172, W172, Y172, Z172, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I173)),I173<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I173, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H173)),H173<0),\"\",intlEstQuantity(T173, W173*12, H173)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T173=\"Select Model\",\"\",coilCircuitChange(W173, U173, AC173, T173,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T173=\"Select Model\",\"\",beamWidth(T173))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T173=\"Select Model\",T173=\"PCBL\"), 0,getSPIP(T173, W173, Y173, BD173, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T173=\"Select Model\", \"\",IF(T173=\"PCBL\",0,primaryAirSensibleCapacityIP($T173,$W173,activeRoomTempCooling,activePriAirTempCooling,$Y173,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T173=\"Select Model\",\"\",IF($T173=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y173,activeElevation)))","v":""},{"$f":"IF(OR(T173=\"Select Model\",T173=\"PCBL\"), 0,IF(AD173=0,0,-primaryAirSensibleCapacityIP($T173,$W173,activeRoomTempHeating,activePriAirTempHeating,$Y173,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T173=\"Select Model\", \"\", InductionRatio($T173,BD173,$W173,$Y173)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T173=\"Select Model\", \"\",IF($T173=\"PCBL\",\"N/A\",minVAVSetBack(AA173, Y173))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T173=\"Select Model\", \"\",IF($T173= \"PCBL\",\"N/A\",getDischargeAirTemp($T173,$V173,$AC173,$W173,BD173,$AL173, $Y173, $AS173, \"cooling\",activeElevation,$AB173,$AJ173,$AV173,$BB173))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T173=\"Select Model\",$T173=\"PCBL\"), \"\",getDischargeAirTemp($T173,$V173,$AD173,$W173,BD173,$AL173, $Y173, $AY173, \"heating\",activeElevation,$AB173,$AJ173,$AV173,$BB173)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T173=\"Select Model\", \"\",IF(OR($T173=\"ACBC_1W\",$T173=\"ACBC_2W\",LEFT($T173,4)=\"ACBR\",$T173 = \"LIU24_2W\",LEFT($T173,3)=\"RIU\",LEFT($T173,6)=\"ACBL12\"), IF((soundLevel($T173, $AB173, BD173, $Y173, $W173,$AJ173,$AA173,\"dba\"))<15,\"<15\",soundLevel($T173, $AB173, BD173, $Y173, $W173,$AJ173,$AA173,\"dba\")+0.4),IF((soundLevel($T173, $AB173, BD173, $Y173, $W173,$AJ173,$AA173,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T173, $AB173, BD173, $Y173, $W173,$AJ173,$AA173,\"dba\")+5)<15, \"<15\", soundLevel($T173, $AB173, BD173,$Y173, $W173,$AJ173,$AA173,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T173=\"Select Model\", \"\",IF(OR($T173=\"ACBC_1W\",$T173=\"ACBC_2W\",LEFT($T173,4)=\"ACBR\",$T173=\"LIU24_2W\",LEFT($T173,3)=\"RIU\",LEFT($T173,6)=\"ACBL12\"), IF((soundLevel($T173, $AB173, BD173, $Y173, $W173,$AJ173,$AA173,\"NC\"))<15,\"<15\",soundLevel($T173, $AB173, BD173, $Y173, $W173,$AJ173,$AA173,\"NC\")+0.4),IF((soundLevel($T173, $AB173, BD173, $Y173, $W173,$AJ173,$AA173,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T173, $AB173, BD173, $Y173, $W173,$AJ173,$AA173,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T173, $AB173, BD173, $Y173, $W173,$AJ173,$AA173,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T173=\"Select Model\",\"\",IF($T173=\"LIU24_2W\",calcQwIP($Y173,$W173,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC173,$AI173,\"latent\",$U173&\"P\"&IF($V173=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T173,activeElevation),\"\"))","v":""},{"$f":"IF($T173=\"Select Model\",\"\",IF($T173=\"ACBC_1W\",calcQwIP($Y173,$W173,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC173,BD173,\"capacity\",$U173&\"P\"&IF($V173=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T173,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y173,$W173,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC173,BD173,\"capacity\",$U173&\"P\"&IF($V173=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T173,activeElevation)))","v":""},"",{"$f":"IF(T173=\"Select Model\", 0,waterPressureDrop(W173, U173 & \"P\" & IF(V173=\"Dual\",2,1) &\"C\", AC173, \"cooling\", T173))","v":0},{"$f":"IF(T173=\"Select Model\", \"\",getReturnWaterTemp(T173,AC173, activeEWTCooling, AS173, \"cooling\"))","v":""},"",{"$f":"IF($T173<>\"ACBC_1W\",\"\",IF($J173=\"\",\"\",FintubeCapacity($T173,$W173,$AE173,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T173=\"Select Model\",T173=\"PCBL\"),\"\",calcQwIP(Y173,W173,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD173,BD173,\"capacity\",U173&\"P\"&IF(V173=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T173,activeElevation))","v":""},"",{"$f":"IF(OR(T173=\"Select Model\",T173=\"PCBL\"), \"\",IF(AY173=0,\"N/A\",waterPressureDrop(W173, U173 & \"P\" & IF(V173=\"Dual\",2,1) &\"C\", AD173, \"heating\", T173)))","v":""},{"$f":"IF(OR(T173=\"Select Model\",T173=\"PCBL\"), \"\",IF(AY173=0,getReturnWaterTemp(T173,AE173, activeEWTHeating, AX173, \"heating\"),getReturnWaterTemp(T173,AD173, activeEWTHeating, AY173, \"heating\")))","v":""},"",{"$f":" getNozzle(T173, W173, Y173, Z173, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I174)),I174<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I174, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H174)),H174<0),\"\",intlEstQuantity(T174, W174*12, H174)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T174=\"Select Model\",\"\",coilCircuitChange(W174, U174, AC174, T174,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T174=\"Select Model\",\"\",beamWidth(T174))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T174=\"Select Model\",T174=\"PCBL\"), 0,getSPIP(T174, W174, Y174, BD174, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T174=\"Select Model\", \"\",IF(T174=\"PCBL\",0,primaryAirSensibleCapacityIP($T174,$W174,activeRoomTempCooling,activePriAirTempCooling,$Y174,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T174=\"Select Model\",\"\",IF($T174=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y174,activeElevation)))","v":""},{"$f":"IF(OR(T174=\"Select Model\",T174=\"PCBL\"), 0,IF(AD174=0,0,-primaryAirSensibleCapacityIP($T174,$W174,activeRoomTempHeating,activePriAirTempHeating,$Y174,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T174=\"Select Model\", \"\", InductionRatio($T174,BD174,$W174,$Y174)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T174=\"Select Model\", \"\",IF($T174=\"PCBL\",\"N/A\",minVAVSetBack(AA174, Y174))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T174=\"Select Model\", \"\",IF($T174= \"PCBL\",\"N/A\",getDischargeAirTemp($T174,$V174,$AC174,$W174,BD174,$AL174, $Y174, $AS174, \"cooling\",activeElevation,$AB174,$AJ174,$AV174,$BB174))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T174=\"Select Model\",$T174=\"PCBL\"), \"\",getDischargeAirTemp($T174,$V174,$AD174,$W174,BD174,$AL174, $Y174, $AY174, \"heating\",activeElevation,$AB174,$AJ174,$AV174,$BB174)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T174=\"Select Model\", \"\",IF(OR($T174=\"ACBC_1W\",$T174=\"ACBC_2W\",LEFT($T174,4)=\"ACBR\",$T174 = \"LIU24_2W\",LEFT($T174,3)=\"RIU\",LEFT($T174,6)=\"ACBL12\"), IF((soundLevel($T174, $AB174, BD174, $Y174, $W174,$AJ174,$AA174,\"dba\"))<15,\"<15\",soundLevel($T174, $AB174, BD174, $Y174, $W174,$AJ174,$AA174,\"dba\")+0.4),IF((soundLevel($T174, $AB174, BD174, $Y174, $W174,$AJ174,$AA174,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T174, $AB174, BD174, $Y174, $W174,$AJ174,$AA174,\"dba\")+5)<15, \"<15\", soundLevel($T174, $AB174, BD174,$Y174, $W174,$AJ174,$AA174,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T174=\"Select Model\", \"\",IF(OR($T174=\"ACBC_1W\",$T174=\"ACBC_2W\",LEFT($T174,4)=\"ACBR\",$T174=\"LIU24_2W\",LEFT($T174,3)=\"RIU\",LEFT($T174,6)=\"ACBL12\"), IF((soundLevel($T174, $AB174, BD174, $Y174, $W174,$AJ174,$AA174,\"NC\"))<15,\"<15\",soundLevel($T174, $AB174, BD174, $Y174, $W174,$AJ174,$AA174,\"NC\")+0.4),IF((soundLevel($T174, $AB174, BD174, $Y174, $W174,$AJ174,$AA174,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T174, $AB174, BD174, $Y174, $W174,$AJ174,$AA174,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T174, $AB174, BD174, $Y174, $W174,$AJ174,$AA174,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T174=\"Select Model\",\"\",IF($T174=\"LIU24_2W\",calcQwIP($Y174,$W174,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC174,$AI174,\"latent\",$U174&\"P\"&IF($V174=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T174,activeElevation),\"\"))","v":""},{"$f":"IF($T174=\"Select Model\",\"\",IF($T174=\"ACBC_1W\",calcQwIP($Y174,$W174,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC174,BD174,\"capacity\",$U174&\"P\"&IF($V174=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T174,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y174,$W174,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC174,BD174,\"capacity\",$U174&\"P\"&IF($V174=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T174,activeElevation)))","v":""},"",{"$f":"IF(T174=\"Select Model\", 0,waterPressureDrop(W174, U174 & \"P\" & IF(V174=\"Dual\",2,1) &\"C\", AC174, \"cooling\", T174))","v":0},{"$f":"IF(T174=\"Select Model\", \"\",getReturnWaterTemp(T174,AC174, activeEWTCooling, AS174, \"cooling\"))","v":""},"",{"$f":"IF($T174<>\"ACBC_1W\",\"\",IF($J174=\"\",\"\",FintubeCapacity($T174,$W174,$AE174,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T174=\"Select Model\",T174=\"PCBL\"),\"\",calcQwIP(Y174,W174,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD174,BD174,\"capacity\",U174&\"P\"&IF(V174=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T174,activeElevation))","v":""},"",{"$f":"IF(OR(T174=\"Select Model\",T174=\"PCBL\"), \"\",IF(AY174=0,\"N/A\",waterPressureDrop(W174, U174 & \"P\" & IF(V174=\"Dual\",2,1) &\"C\", AD174, \"heating\", T174)))","v":""},{"$f":"IF(OR(T174=\"Select Model\",T174=\"PCBL\"), \"\",IF(AY174=0,getReturnWaterTemp(T174,AE174, activeEWTHeating, AX174, \"heating\"),getReturnWaterTemp(T174,AD174, activeEWTHeating, AY174, \"heating\")))","v":""},"",{"$f":" getNozzle(T174, W174, Y174, Z174, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I175)),I175<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I175, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H175)),H175<0),\"\",intlEstQuantity(T175, W175*12, H175)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T175=\"Select Model\",\"\",coilCircuitChange(W175, U175, AC175, T175,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T175=\"Select Model\",\"\",beamWidth(T175))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T175=\"Select Model\",T175=\"PCBL\"), 0,getSPIP(T175, W175, Y175, BD175, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T175=\"Select Model\", \"\",IF(T175=\"PCBL\",0,primaryAirSensibleCapacityIP($T175,$W175,activeRoomTempCooling,activePriAirTempCooling,$Y175,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T175=\"Select Model\",\"\",IF($T175=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y175,activeElevation)))","v":""},{"$f":"IF(OR(T175=\"Select Model\",T175=\"PCBL\"), 0,IF(AD175=0,0,-primaryAirSensibleCapacityIP($T175,$W175,activeRoomTempHeating,activePriAirTempHeating,$Y175,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T175=\"Select Model\", \"\", InductionRatio($T175,BD175,$W175,$Y175)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T175=\"Select Model\", \"\",IF($T175=\"PCBL\",\"N/A\",minVAVSetBack(AA175, Y175))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T175=\"Select Model\", \"\",IF($T175= \"PCBL\",\"N/A\",getDischargeAirTemp($T175,$V175,$AC175,$W175,BD175,$AL175, $Y175, $AS175, \"cooling\",activeElevation,$AB175,$AJ175,$AV175,$BB175))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T175=\"Select Model\",$T175=\"PCBL\"), \"\",getDischargeAirTemp($T175,$V175,$AD175,$W175,BD175,$AL175, $Y175, $AY175, \"heating\",activeElevation,$AB175,$AJ175,$AV175,$BB175)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T175=\"Select Model\", \"\",IF(OR($T175=\"ACBC_1W\",$T175=\"ACBC_2W\",LEFT($T175,4)=\"ACBR\",$T175 = \"LIU24_2W\",LEFT($T175,3)=\"RIU\",LEFT($T175,6)=\"ACBL12\"), IF((soundLevel($T175, $AB175, BD175, $Y175, $W175,$AJ175,$AA175,\"dba\"))<15,\"<15\",soundLevel($T175, $AB175, BD175, $Y175, $W175,$AJ175,$AA175,\"dba\")+0.4),IF((soundLevel($T175, $AB175, BD175, $Y175, $W175,$AJ175,$AA175,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T175, $AB175, BD175, $Y175, $W175,$AJ175,$AA175,\"dba\")+5)<15, \"<15\", soundLevel($T175, $AB175, BD175,$Y175, $W175,$AJ175,$AA175,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T175=\"Select Model\", \"\",IF(OR($T175=\"ACBC_1W\",$T175=\"ACBC_2W\",LEFT($T175,4)=\"ACBR\",$T175=\"LIU24_2W\",LEFT($T175,3)=\"RIU\",LEFT($T175,6)=\"ACBL12\"), IF((soundLevel($T175, $AB175, BD175, $Y175, $W175,$AJ175,$AA175,\"NC\"))<15,\"<15\",soundLevel($T175, $AB175, BD175, $Y175, $W175,$AJ175,$AA175,\"NC\")+0.4),IF((soundLevel($T175, $AB175, BD175, $Y175, $W175,$AJ175,$AA175,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T175, $AB175, BD175, $Y175, $W175,$AJ175,$AA175,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T175, $AB175, BD175, $Y175, $W175,$AJ175,$AA175,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T175=\"Select Model\",\"\",IF($T175=\"LIU24_2W\",calcQwIP($Y175,$W175,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC175,$AI175,\"latent\",$U175&\"P\"&IF($V175=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T175,activeElevation),\"\"))","v":""},{"$f":"IF($T175=\"Select Model\",\"\",IF($T175=\"ACBC_1W\",calcQwIP($Y175,$W175,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC175,BD175,\"capacity\",$U175&\"P\"&IF($V175=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T175,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y175,$W175,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC175,BD175,\"capacity\",$U175&\"P\"&IF($V175=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T175,activeElevation)))","v":""},"",{"$f":"IF(T175=\"Select Model\", 0,waterPressureDrop(W175, U175 & \"P\" & IF(V175=\"Dual\",2,1) &\"C\", AC175, \"cooling\", T175))","v":0},{"$f":"IF(T175=\"Select Model\", \"\",getReturnWaterTemp(T175,AC175, activeEWTCooling, AS175, \"cooling\"))","v":""},"",{"$f":"IF($T175<>\"ACBC_1W\",\"\",IF($J175=\"\",\"\",FintubeCapacity($T175,$W175,$AE175,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T175=\"Select Model\",T175=\"PCBL\"),\"\",calcQwIP(Y175,W175,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD175,BD175,\"capacity\",U175&\"P\"&IF(V175=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T175,activeElevation))","v":""},"",{"$f":"IF(OR(T175=\"Select Model\",T175=\"PCBL\"), \"\",IF(AY175=0,\"N/A\",waterPressureDrop(W175, U175 & \"P\" & IF(V175=\"Dual\",2,1) &\"C\", AD175, \"heating\", T175)))","v":""},{"$f":"IF(OR(T175=\"Select Model\",T175=\"PCBL\"), \"\",IF(AY175=0,getReturnWaterTemp(T175,AE175, activeEWTHeating, AX175, \"heating\"),getReturnWaterTemp(T175,AD175, activeEWTHeating, AY175, \"heating\")))","v":""},"",{"$f":" getNozzle(T175, W175, Y175, Z175, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I176)),I176<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I176, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H176)),H176<0),\"\",intlEstQuantity(T176, W176*12, H176)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T176=\"Select Model\",\"\",coilCircuitChange(W176, U176, AC176, T176,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T176=\"Select Model\",\"\",beamWidth(T176))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T176=\"Select Model\",T176=\"PCBL\"), 0,getSPIP(T176, W176, Y176, BD176, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T176=\"Select Model\", \"\",IF(T176=\"PCBL\",0,primaryAirSensibleCapacityIP($T176,$W176,activeRoomTempCooling,activePriAirTempCooling,$Y176,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T176=\"Select Model\",\"\",IF($T176=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y176,activeElevation)))","v":""},{"$f":"IF(OR(T176=\"Select Model\",T176=\"PCBL\"), 0,IF(AD176=0,0,-primaryAirSensibleCapacityIP($T176,$W176,activeRoomTempHeating,activePriAirTempHeating,$Y176,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T176=\"Select Model\", \"\", InductionRatio($T176,BD176,$W176,$Y176)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T176=\"Select Model\", \"\",IF($T176=\"PCBL\",\"N/A\",minVAVSetBack(AA176, Y176))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T176=\"Select Model\", \"\",IF($T176= \"PCBL\",\"N/A\",getDischargeAirTemp($T176,$V176,$AC176,$W176,BD176,$AL176, $Y176, $AS176, \"cooling\",activeElevation,$AB176,$AJ176,$AV176,$BB176))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T176=\"Select Model\",$T176=\"PCBL\"), \"\",getDischargeAirTemp($T176,$V176,$AD176,$W176,BD176,$AL176, $Y176, $AY176, \"heating\",activeElevation,$AB176,$AJ176,$AV176,$BB176)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T176=\"Select Model\", \"\",IF(OR($T176=\"ACBC_1W\",$T176=\"ACBC_2W\",LEFT($T176,4)=\"ACBR\",$T176 = \"LIU24_2W\",LEFT($T176,3)=\"RIU\",LEFT($T176,6)=\"ACBL12\"), IF((soundLevel($T176, $AB176, BD176, $Y176, $W176,$AJ176,$AA176,\"dba\"))<15,\"<15\",soundLevel($T176, $AB176, BD176, $Y176, $W176,$AJ176,$AA176,\"dba\")+0.4),IF((soundLevel($T176, $AB176, BD176, $Y176, $W176,$AJ176,$AA176,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T176, $AB176, BD176, $Y176, $W176,$AJ176,$AA176,\"dba\")+5)<15, \"<15\", soundLevel($T176, $AB176, BD176,$Y176, $W176,$AJ176,$AA176,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T176=\"Select Model\", \"\",IF(OR($T176=\"ACBC_1W\",$T176=\"ACBC_2W\",LEFT($T176,4)=\"ACBR\",$T176=\"LIU24_2W\",LEFT($T176,3)=\"RIU\",LEFT($T176,6)=\"ACBL12\"), IF((soundLevel($T176, $AB176, BD176, $Y176, $W176,$AJ176,$AA176,\"NC\"))<15,\"<15\",soundLevel($T176, $AB176, BD176, $Y176, $W176,$AJ176,$AA176,\"NC\")+0.4),IF((soundLevel($T176, $AB176, BD176, $Y176, $W176,$AJ176,$AA176,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T176, $AB176, BD176, $Y176, $W176,$AJ176,$AA176,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T176, $AB176, BD176, $Y176, $W176,$AJ176,$AA176,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T176=\"Select Model\",\"\",IF($T176=\"LIU24_2W\",calcQwIP($Y176,$W176,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC176,$AI176,\"latent\",$U176&\"P\"&IF($V176=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T176,activeElevation),\"\"))","v":""},{"$f":"IF($T176=\"Select Model\",\"\",IF($T176=\"ACBC_1W\",calcQwIP($Y176,$W176,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC176,BD176,\"capacity\",$U176&\"P\"&IF($V176=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T176,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y176,$W176,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC176,BD176,\"capacity\",$U176&\"P\"&IF($V176=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T176,activeElevation)))","v":""},"",{"$f":"IF(T176=\"Select Model\", 0,waterPressureDrop(W176, U176 & \"P\" & IF(V176=\"Dual\",2,1) &\"C\", AC176, \"cooling\", T176))","v":0},{"$f":"IF(T176=\"Select Model\", \"\",getReturnWaterTemp(T176,AC176, activeEWTCooling, AS176, \"cooling\"))","v":""},"",{"$f":"IF($T176<>\"ACBC_1W\",\"\",IF($J176=\"\",\"\",FintubeCapacity($T176,$W176,$AE176,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T176=\"Select Model\",T176=\"PCBL\"),\"\",calcQwIP(Y176,W176,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD176,BD176,\"capacity\",U176&\"P\"&IF(V176=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T176,activeElevation))","v":""},"",{"$f":"IF(OR(T176=\"Select Model\",T176=\"PCBL\"), \"\",IF(AY176=0,\"N/A\",waterPressureDrop(W176, U176 & \"P\" & IF(V176=\"Dual\",2,1) &\"C\", AD176, \"heating\", T176)))","v":""},{"$f":"IF(OR(T176=\"Select Model\",T176=\"PCBL\"), \"\",IF(AY176=0,getReturnWaterTemp(T176,AE176, activeEWTHeating, AX176, \"heating\"),getReturnWaterTemp(T176,AD176, activeEWTHeating, AY176, \"heating\")))","v":""},"",{"$f":" getNozzle(T176, W176, Y176, Z176, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I177)),I177<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I177, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H177)),H177<0),\"\",intlEstQuantity(T177, W177*12, H177)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T177=\"Select Model\",\"\",coilCircuitChange(W177, U177, AC177, T177,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T177=\"Select Model\",\"\",beamWidth(T177))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T177=\"Select Model\",T177=\"PCBL\"), 0,getSPIP(T177, W177, Y177, BD177, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T177=\"Select Model\", \"\",IF(T177=\"PCBL\",0,primaryAirSensibleCapacityIP($T177,$W177,activeRoomTempCooling,activePriAirTempCooling,$Y177,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T177=\"Select Model\",\"\",IF($T177=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y177,activeElevation)))","v":""},{"$f":"IF(OR(T177=\"Select Model\",T177=\"PCBL\"), 0,IF(AD177=0,0,-primaryAirSensibleCapacityIP($T177,$W177,activeRoomTempHeating,activePriAirTempHeating,$Y177,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T177=\"Select Model\", \"\", InductionRatio($T177,BD177,$W177,$Y177)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T177=\"Select Model\", \"\",IF($T177=\"PCBL\",\"N/A\",minVAVSetBack(AA177, Y177))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T177=\"Select Model\", \"\",IF($T177= \"PCBL\",\"N/A\",getDischargeAirTemp($T177,$V177,$AC177,$W177,BD177,$AL177, $Y177, $AS177, \"cooling\",activeElevation,$AB177,$AJ177,$AV177,$BB177))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T177=\"Select Model\",$T177=\"PCBL\"), \"\",getDischargeAirTemp($T177,$V177,$AD177,$W177,BD177,$AL177, $Y177, $AY177, \"heating\",activeElevation,$AB177,$AJ177,$AV177,$BB177)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T177=\"Select Model\", \"\",IF(OR($T177=\"ACBC_1W\",$T177=\"ACBC_2W\",LEFT($T177,4)=\"ACBR\",$T177 = \"LIU24_2W\",LEFT($T177,3)=\"RIU\",LEFT($T177,6)=\"ACBL12\"), IF((soundLevel($T177, $AB177, BD177, $Y177, $W177,$AJ177,$AA177,\"dba\"))<15,\"<15\",soundLevel($T177, $AB177, BD177, $Y177, $W177,$AJ177,$AA177,\"dba\")+0.4),IF((soundLevel($T177, $AB177, BD177, $Y177, $W177,$AJ177,$AA177,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T177, $AB177, BD177, $Y177, $W177,$AJ177,$AA177,\"dba\")+5)<15, \"<15\", soundLevel($T177, $AB177, BD177,$Y177, $W177,$AJ177,$AA177,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T177=\"Select Model\", \"\",IF(OR($T177=\"ACBC_1W\",$T177=\"ACBC_2W\",LEFT($T177,4)=\"ACBR\",$T177=\"LIU24_2W\",LEFT($T177,3)=\"RIU\",LEFT($T177,6)=\"ACBL12\"), IF((soundLevel($T177, $AB177, BD177, $Y177, $W177,$AJ177,$AA177,\"NC\"))<15,\"<15\",soundLevel($T177, $AB177, BD177, $Y177, $W177,$AJ177,$AA177,\"NC\")+0.4),IF((soundLevel($T177, $AB177, BD177, $Y177, $W177,$AJ177,$AA177,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T177, $AB177, BD177, $Y177, $W177,$AJ177,$AA177,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T177, $AB177, BD177, $Y177, $W177,$AJ177,$AA177,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T177=\"Select Model\",\"\",IF($T177=\"LIU24_2W\",calcQwIP($Y177,$W177,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC177,$AI177,\"latent\",$U177&\"P\"&IF($V177=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T177,activeElevation),\"\"))","v":""},{"$f":"IF($T177=\"Select Model\",\"\",IF($T177=\"ACBC_1W\",calcQwIP($Y177,$W177,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC177,BD177,\"capacity\",$U177&\"P\"&IF($V177=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T177,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y177,$W177,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC177,BD177,\"capacity\",$U177&\"P\"&IF($V177=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T177,activeElevation)))","v":""},"",{"$f":"IF(T177=\"Select Model\", 0,waterPressureDrop(W177, U177 & \"P\" & IF(V177=\"Dual\",2,1) &\"C\", AC177, \"cooling\", T177))","v":0},{"$f":"IF(T177=\"Select Model\", \"\",getReturnWaterTemp(T177,AC177, activeEWTCooling, AS177, \"cooling\"))","v":""},"",{"$f":"IF($T177<>\"ACBC_1W\",\"\",IF($J177=\"\",\"\",FintubeCapacity($T177,$W177,$AE177,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T177=\"Select Model\",T177=\"PCBL\"),\"\",calcQwIP(Y177,W177,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD177,BD177,\"capacity\",U177&\"P\"&IF(V177=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T177,activeElevation))","v":""},"",{"$f":"IF(OR(T177=\"Select Model\",T177=\"PCBL\"), \"\",IF(AY177=0,\"N/A\",waterPressureDrop(W177, U177 & \"P\" & IF(V177=\"Dual\",2,1) &\"C\", AD177, \"heating\", T177)))","v":""},{"$f":"IF(OR(T177=\"Select Model\",T177=\"PCBL\"), \"\",IF(AY177=0,getReturnWaterTemp(T177,AE177, activeEWTHeating, AX177, \"heating\"),getReturnWaterTemp(T177,AD177, activeEWTHeating, AY177, \"heating\")))","v":""},"",{"$f":" getNozzle(T177, W177, Y177, Z177, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I178)),I178<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I178, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H178)),H178<0),\"\",intlEstQuantity(T178, W178*12, H178)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T178=\"Select Model\",\"\",coilCircuitChange(W178, U178, AC178, T178,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T178=\"Select Model\",\"\",beamWidth(T178))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T178=\"Select Model\",T178=\"PCBL\"), 0,getSPIP(T178, W178, Y178, BD178, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T178=\"Select Model\", \"\",IF(T178=\"PCBL\",0,primaryAirSensibleCapacityIP($T178,$W178,activeRoomTempCooling,activePriAirTempCooling,$Y178,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T178=\"Select Model\",\"\",IF($T178=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y178,activeElevation)))","v":""},{"$f":"IF(OR(T178=\"Select Model\",T178=\"PCBL\"), 0,IF(AD178=0,0,-primaryAirSensibleCapacityIP($T178,$W178,activeRoomTempHeating,activePriAirTempHeating,$Y178,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T178=\"Select Model\", \"\", InductionRatio($T178,BD178,$W178,$Y178)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T178=\"Select Model\", \"\",IF($T178=\"PCBL\",\"N/A\",minVAVSetBack(AA178, Y178))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T178=\"Select Model\", \"\",IF($T178= \"PCBL\",\"N/A\",getDischargeAirTemp($T178,$V178,$AC178,$W178,BD178,$AL178, $Y178, $AS178, \"cooling\",activeElevation,$AB178,$AJ178,$AV178,$BB178))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T178=\"Select Model\",$T178=\"PCBL\"), \"\",getDischargeAirTemp($T178,$V178,$AD178,$W178,BD178,$AL178, $Y178, $AY178, \"heating\",activeElevation,$AB178,$AJ178,$AV178,$BB178)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T178=\"Select Model\", \"\",IF(OR($T178=\"ACBC_1W\",$T178=\"ACBC_2W\",LEFT($T178,4)=\"ACBR\",$T178 = \"LIU24_2W\",LEFT($T178,3)=\"RIU\",LEFT($T178,6)=\"ACBL12\"), IF((soundLevel($T178, $AB178, BD178, $Y178, $W178,$AJ178,$AA178,\"dba\"))<15,\"<15\",soundLevel($T178, $AB178, BD178, $Y178, $W178,$AJ178,$AA178,\"dba\")+0.4),IF((soundLevel($T178, $AB178, BD178, $Y178, $W178,$AJ178,$AA178,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T178, $AB178, BD178, $Y178, $W178,$AJ178,$AA178,\"dba\")+5)<15, \"<15\", soundLevel($T178, $AB178, BD178,$Y178, $W178,$AJ178,$AA178,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T178=\"Select Model\", \"\",IF(OR($T178=\"ACBC_1W\",$T178=\"ACBC_2W\",LEFT($T178,4)=\"ACBR\",$T178=\"LIU24_2W\",LEFT($T178,3)=\"RIU\",LEFT($T178,6)=\"ACBL12\"), IF((soundLevel($T178, $AB178, BD178, $Y178, $W178,$AJ178,$AA178,\"NC\"))<15,\"<15\",soundLevel($T178, $AB178, BD178, $Y178, $W178,$AJ178,$AA178,\"NC\")+0.4),IF((soundLevel($T178, $AB178, BD178, $Y178, $W178,$AJ178,$AA178,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T178, $AB178, BD178, $Y178, $W178,$AJ178,$AA178,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T178, $AB178, BD178, $Y178, $W178,$AJ178,$AA178,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T178=\"Select Model\",\"\",IF($T178=\"LIU24_2W\",calcQwIP($Y178,$W178,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC178,$AI178,\"latent\",$U178&\"P\"&IF($V178=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T178,activeElevation),\"\"))","v":""},{"$f":"IF($T178=\"Select Model\",\"\",IF($T178=\"ACBC_1W\",calcQwIP($Y178,$W178,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC178,BD178,\"capacity\",$U178&\"P\"&IF($V178=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T178,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y178,$W178,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC178,BD178,\"capacity\",$U178&\"P\"&IF($V178=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T178,activeElevation)))","v":""},"",{"$f":"IF(T178=\"Select Model\", 0,waterPressureDrop(W178, U178 & \"P\" & IF(V178=\"Dual\",2,1) &\"C\", AC178, \"cooling\", T178))","v":0},{"$f":"IF(T178=\"Select Model\", \"\",getReturnWaterTemp(T178,AC178, activeEWTCooling, AS178, \"cooling\"))","v":""},"",{"$f":"IF($T178<>\"ACBC_1W\",\"\",IF($J178=\"\",\"\",FintubeCapacity($T178,$W178,$AE178,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T178=\"Select Model\",T178=\"PCBL\"),\"\",calcQwIP(Y178,W178,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD178,BD178,\"capacity\",U178&\"P\"&IF(V178=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T178,activeElevation))","v":""},"",{"$f":"IF(OR(T178=\"Select Model\",T178=\"PCBL\"), \"\",IF(AY178=0,\"N/A\",waterPressureDrop(W178, U178 & \"P\" & IF(V178=\"Dual\",2,1) &\"C\", AD178, \"heating\", T178)))","v":""},{"$f":"IF(OR(T178=\"Select Model\",T178=\"PCBL\"), \"\",IF(AY178=0,getReturnWaterTemp(T178,AE178, activeEWTHeating, AX178, \"heating\"),getReturnWaterTemp(T178,AD178, activeEWTHeating, AY178, \"heating\")))","v":""},"",{"$f":" getNozzle(T178, W178, Y178, Z178, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I179)),I179<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I179, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H179)),H179<0),\"\",intlEstQuantity(T179, W179*12, H179)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T179=\"Select Model\",\"\",coilCircuitChange(W179, U179, AC179, T179,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T179=\"Select Model\",\"\",beamWidth(T179))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T179=\"Select Model\",T179=\"PCBL\"), 0,getSPIP(T179, W179, Y179, BD179, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T179=\"Select Model\", \"\",IF(T179=\"PCBL\",0,primaryAirSensibleCapacityIP($T179,$W179,activeRoomTempCooling,activePriAirTempCooling,$Y179,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T179=\"Select Model\",\"\",IF($T179=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y179,activeElevation)))","v":""},{"$f":"IF(OR(T179=\"Select Model\",T179=\"PCBL\"), 0,IF(AD179=0,0,-primaryAirSensibleCapacityIP($T179,$W179,activeRoomTempHeating,activePriAirTempHeating,$Y179,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T179=\"Select Model\", \"\", InductionRatio($T179,BD179,$W179,$Y179)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T179=\"Select Model\", \"\",IF($T179=\"PCBL\",\"N/A\",minVAVSetBack(AA179, Y179))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T179=\"Select Model\", \"\",IF($T179= \"PCBL\",\"N/A\",getDischargeAirTemp($T179,$V179,$AC179,$W179,BD179,$AL179, $Y179, $AS179, \"cooling\",activeElevation,$AB179,$AJ179,$AV179,$BB179))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T179=\"Select Model\",$T179=\"PCBL\"), \"\",getDischargeAirTemp($T179,$V179,$AD179,$W179,BD179,$AL179, $Y179, $AY179, \"heating\",activeElevation,$AB179,$AJ179,$AV179,$BB179)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T179=\"Select Model\", \"\",IF(OR($T179=\"ACBC_1W\",$T179=\"ACBC_2W\",LEFT($T179,4)=\"ACBR\",$T179 = \"LIU24_2W\",LEFT($T179,3)=\"RIU\",LEFT($T179,6)=\"ACBL12\"), IF((soundLevel($T179, $AB179, BD179, $Y179, $W179,$AJ179,$AA179,\"dba\"))<15,\"<15\",soundLevel($T179, $AB179, BD179, $Y179, $W179,$AJ179,$AA179,\"dba\")+0.4),IF((soundLevel($T179, $AB179, BD179, $Y179, $W179,$AJ179,$AA179,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T179, $AB179, BD179, $Y179, $W179,$AJ179,$AA179,\"dba\")+5)<15, \"<15\", soundLevel($T179, $AB179, BD179,$Y179, $W179,$AJ179,$AA179,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T179=\"Select Model\", \"\",IF(OR($T179=\"ACBC_1W\",$T179=\"ACBC_2W\",LEFT($T179,4)=\"ACBR\",$T179=\"LIU24_2W\",LEFT($T179,3)=\"RIU\",LEFT($T179,6)=\"ACBL12\"), IF((soundLevel($T179, $AB179, BD179, $Y179, $W179,$AJ179,$AA179,\"NC\"))<15,\"<15\",soundLevel($T179, $AB179, BD179, $Y179, $W179,$AJ179,$AA179,\"NC\")+0.4),IF((soundLevel($T179, $AB179, BD179, $Y179, $W179,$AJ179,$AA179,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T179, $AB179, BD179, $Y179, $W179,$AJ179,$AA179,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T179, $AB179, BD179, $Y179, $W179,$AJ179,$AA179,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T179=\"Select Model\",\"\",IF($T179=\"LIU24_2W\",calcQwIP($Y179,$W179,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC179,$AI179,\"latent\",$U179&\"P\"&IF($V179=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T179,activeElevation),\"\"))","v":""},{"$f":"IF($T179=\"Select Model\",\"\",IF($T179=\"ACBC_1W\",calcQwIP($Y179,$W179,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC179,BD179,\"capacity\",$U179&\"P\"&IF($V179=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T179,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y179,$W179,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC179,BD179,\"capacity\",$U179&\"P\"&IF($V179=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T179,activeElevation)))","v":""},"",{"$f":"IF(T179=\"Select Model\", 0,waterPressureDrop(W179, U179 & \"P\" & IF(V179=\"Dual\",2,1) &\"C\", AC179, \"cooling\", T179))","v":0},{"$f":"IF(T179=\"Select Model\", \"\",getReturnWaterTemp(T179,AC179, activeEWTCooling, AS179, \"cooling\"))","v":""},"",{"$f":"IF($T179<>\"ACBC_1W\",\"\",IF($J179=\"\",\"\",FintubeCapacity($T179,$W179,$AE179,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T179=\"Select Model\",T179=\"PCBL\"),\"\",calcQwIP(Y179,W179,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD179,BD179,\"capacity\",U179&\"P\"&IF(V179=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T179,activeElevation))","v":""},"",{"$f":"IF(OR(T179=\"Select Model\",T179=\"PCBL\"), \"\",IF(AY179=0,\"N/A\",waterPressureDrop(W179, U179 & \"P\" & IF(V179=\"Dual\",2,1) &\"C\", AD179, \"heating\", T179)))","v":""},{"$f":"IF(OR(T179=\"Select Model\",T179=\"PCBL\"), \"\",IF(AY179=0,getReturnWaterTemp(T179,AE179, activeEWTHeating, AX179, \"heating\"),getReturnWaterTemp(T179,AD179, activeEWTHeating, AY179, \"heating\")))","v":""},"",{"$f":" getNozzle(T179, W179, Y179, Z179, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I180)),I180<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I180, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H180)),H180<0),\"\",intlEstQuantity(T180, W180*12, H180)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T180=\"Select Model\",\"\",coilCircuitChange(W180, U180, AC180, T180,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T180=\"Select Model\",\"\",beamWidth(T180))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T180=\"Select Model\",T180=\"PCBL\"), 0,getSPIP(T180, W180, Y180, BD180, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T180=\"Select Model\", \"\",IF(T180=\"PCBL\",0,primaryAirSensibleCapacityIP($T180,$W180,activeRoomTempCooling,activePriAirTempCooling,$Y180,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T180=\"Select Model\",\"\",IF($T180=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y180,activeElevation)))","v":""},{"$f":"IF(OR(T180=\"Select Model\",T180=\"PCBL\"), 0,IF(AD180=0,0,-primaryAirSensibleCapacityIP($T180,$W180,activeRoomTempHeating,activePriAirTempHeating,$Y180,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T180=\"Select Model\", \"\", InductionRatio($T180,BD180,$W180,$Y180)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T180=\"Select Model\", \"\",IF($T180=\"PCBL\",\"N/A\",minVAVSetBack(AA180, Y180))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T180=\"Select Model\", \"\",IF($T180= \"PCBL\",\"N/A\",getDischargeAirTemp($T180,$V180,$AC180,$W180,BD180,$AL180, $Y180, $AS180, \"cooling\",activeElevation,$AB180,$AJ180,$AV180,$BB180))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T180=\"Select Model\",$T180=\"PCBL\"), \"\",getDischargeAirTemp($T180,$V180,$AD180,$W180,BD180,$AL180, $Y180, $AY180, \"heating\",activeElevation,$AB180,$AJ180,$AV180,$BB180)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T180=\"Select Model\", \"\",IF(OR($T180=\"ACBC_1W\",$T180=\"ACBC_2W\",LEFT($T180,4)=\"ACBR\",$T180 = \"LIU24_2W\",LEFT($T180,3)=\"RIU\",LEFT($T180,6)=\"ACBL12\"), IF((soundLevel($T180, $AB180, BD180, $Y180, $W180,$AJ180,$AA180,\"dba\"))<15,\"<15\",soundLevel($T180, $AB180, BD180, $Y180, $W180,$AJ180,$AA180,\"dba\")+0.4),IF((soundLevel($T180, $AB180, BD180, $Y180, $W180,$AJ180,$AA180,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T180, $AB180, BD180, $Y180, $W180,$AJ180,$AA180,\"dba\")+5)<15, \"<15\", soundLevel($T180, $AB180, BD180,$Y180, $W180,$AJ180,$AA180,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T180=\"Select Model\", \"\",IF(OR($T180=\"ACBC_1W\",$T180=\"ACBC_2W\",LEFT($T180,4)=\"ACBR\",$T180=\"LIU24_2W\",LEFT($T180,3)=\"RIU\",LEFT($T180,6)=\"ACBL12\"), IF((soundLevel($T180, $AB180, BD180, $Y180, $W180,$AJ180,$AA180,\"NC\"))<15,\"<15\",soundLevel($T180, $AB180, BD180, $Y180, $W180,$AJ180,$AA180,\"NC\")+0.4),IF((soundLevel($T180, $AB180, BD180, $Y180, $W180,$AJ180,$AA180,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T180, $AB180, BD180, $Y180, $W180,$AJ180,$AA180,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T180, $AB180, BD180, $Y180, $W180,$AJ180,$AA180,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T180=\"Select Model\",\"\",IF($T180=\"LIU24_2W\",calcQwIP($Y180,$W180,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC180,$AI180,\"latent\",$U180&\"P\"&IF($V180=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T180,activeElevation),\"\"))","v":""},{"$f":"IF($T180=\"Select Model\",\"\",IF($T180=\"ACBC_1W\",calcQwIP($Y180,$W180,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC180,BD180,\"capacity\",$U180&\"P\"&IF($V180=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T180,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y180,$W180,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC180,BD180,\"capacity\",$U180&\"P\"&IF($V180=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T180,activeElevation)))","v":""},"",{"$f":"IF(T180=\"Select Model\", 0,waterPressureDrop(W180, U180 & \"P\" & IF(V180=\"Dual\",2,1) &\"C\", AC180, \"cooling\", T180))","v":0},{"$f":"IF(T180=\"Select Model\", \"\",getReturnWaterTemp(T180,AC180, activeEWTCooling, AS180, \"cooling\"))","v":""},"",{"$f":"IF($T180<>\"ACBC_1W\",\"\",IF($J180=\"\",\"\",FintubeCapacity($T180,$W180,$AE180,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T180=\"Select Model\",T180=\"PCBL\"),\"\",calcQwIP(Y180,W180,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD180,BD180,\"capacity\",U180&\"P\"&IF(V180=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T180,activeElevation))","v":""},"",{"$f":"IF(OR(T180=\"Select Model\",T180=\"PCBL\"), \"\",IF(AY180=0,\"N/A\",waterPressureDrop(W180, U180 & \"P\" & IF(V180=\"Dual\",2,1) &\"C\", AD180, \"heating\", T180)))","v":""},{"$f":"IF(OR(T180=\"Select Model\",T180=\"PCBL\"), \"\",IF(AY180=0,getReturnWaterTemp(T180,AE180, activeEWTHeating, AX180, \"heating\"),getReturnWaterTemp(T180,AD180, activeEWTHeating, AY180, \"heating\")))","v":""},"",{"$f":" getNozzle(T180, W180, Y180, Z180, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I181)),I181<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I181, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H181)),H181<0),\"\",intlEstQuantity(T181, W181*12, H181)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T181=\"Select Model\",\"\",coilCircuitChange(W181, U181, AC181, T181,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T181=\"Select Model\",\"\",beamWidth(T181))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T181=\"Select Model\",T181=\"PCBL\"), 0,getSPIP(T181, W181, Y181, BD181, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T181=\"Select Model\", \"\",IF(T181=\"PCBL\",0,primaryAirSensibleCapacityIP($T181,$W181,activeRoomTempCooling,activePriAirTempCooling,$Y181,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T181=\"Select Model\",\"\",IF($T181=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y181,activeElevation)))","v":""},{"$f":"IF(OR(T181=\"Select Model\",T181=\"PCBL\"), 0,IF(AD181=0,0,-primaryAirSensibleCapacityIP($T181,$W181,activeRoomTempHeating,activePriAirTempHeating,$Y181,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T181=\"Select Model\", \"\", InductionRatio($T181,BD181,$W181,$Y181)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T181=\"Select Model\", \"\",IF($T181=\"PCBL\",\"N/A\",minVAVSetBack(AA181, Y181))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T181=\"Select Model\", \"\",IF($T181= \"PCBL\",\"N/A\",getDischargeAirTemp($T181,$V181,$AC181,$W181,BD181,$AL181, $Y181, $AS181, \"cooling\",activeElevation,$AB181,$AJ181,$AV181,$BB181))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T181=\"Select Model\",$T181=\"PCBL\"), \"\",getDischargeAirTemp($T181,$V181,$AD181,$W181,BD181,$AL181, $Y181, $AY181, \"heating\",activeElevation,$AB181,$AJ181,$AV181,$BB181)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T181=\"Select Model\", \"\",IF(OR($T181=\"ACBC_1W\",$T181=\"ACBC_2W\",LEFT($T181,4)=\"ACBR\",$T181 = \"LIU24_2W\",LEFT($T181,3)=\"RIU\",LEFT($T181,6)=\"ACBL12\"), IF((soundLevel($T181, $AB181, BD181, $Y181, $W181,$AJ181,$AA181,\"dba\"))<15,\"<15\",soundLevel($T181, $AB181, BD181, $Y181, $W181,$AJ181,$AA181,\"dba\")+0.4),IF((soundLevel($T181, $AB181, BD181, $Y181, $W181,$AJ181,$AA181,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T181, $AB181, BD181, $Y181, $W181,$AJ181,$AA181,\"dba\")+5)<15, \"<15\", soundLevel($T181, $AB181, BD181,$Y181, $W181,$AJ181,$AA181,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T181=\"Select Model\", \"\",IF(OR($T181=\"ACBC_1W\",$T181=\"ACBC_2W\",LEFT($T181,4)=\"ACBR\",$T181=\"LIU24_2W\",LEFT($T181,3)=\"RIU\",LEFT($T181,6)=\"ACBL12\"), IF((soundLevel($T181, $AB181, BD181, $Y181, $W181,$AJ181,$AA181,\"NC\"))<15,\"<15\",soundLevel($T181, $AB181, BD181, $Y181, $W181,$AJ181,$AA181,\"NC\")+0.4),IF((soundLevel($T181, $AB181, BD181, $Y181, $W181,$AJ181,$AA181,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T181, $AB181, BD181, $Y181, $W181,$AJ181,$AA181,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T181, $AB181, BD181, $Y181, $W181,$AJ181,$AA181,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T181=\"Select Model\",\"\",IF($T181=\"LIU24_2W\",calcQwIP($Y181,$W181,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC181,$AI181,\"latent\",$U181&\"P\"&IF($V181=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T181,activeElevation),\"\"))","v":""},{"$f":"IF($T181=\"Select Model\",\"\",IF($T181=\"ACBC_1W\",calcQwIP($Y181,$W181,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC181,BD181,\"capacity\",$U181&\"P\"&IF($V181=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T181,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y181,$W181,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC181,BD181,\"capacity\",$U181&\"P\"&IF($V181=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T181,activeElevation)))","v":""},"",{"$f":"IF(T181=\"Select Model\", 0,waterPressureDrop(W181, U181 & \"P\" & IF(V181=\"Dual\",2,1) &\"C\", AC181, \"cooling\", T181))","v":0},{"$f":"IF(T181=\"Select Model\", \"\",getReturnWaterTemp(T181,AC181, activeEWTCooling, AS181, \"cooling\"))","v":""},"",{"$f":"IF($T181<>\"ACBC_1W\",\"\",IF($J181=\"\",\"\",FintubeCapacity($T181,$W181,$AE181,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T181=\"Select Model\",T181=\"PCBL\"),\"\",calcQwIP(Y181,W181,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD181,BD181,\"capacity\",U181&\"P\"&IF(V181=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T181,activeElevation))","v":""},"",{"$f":"IF(OR(T181=\"Select Model\",T181=\"PCBL\"), \"\",IF(AY181=0,\"N/A\",waterPressureDrop(W181, U181 & \"P\" & IF(V181=\"Dual\",2,1) &\"C\", AD181, \"heating\", T181)))","v":""},{"$f":"IF(OR(T181=\"Select Model\",T181=\"PCBL\"), \"\",IF(AY181=0,getReturnWaterTemp(T181,AE181, activeEWTHeating, AX181, \"heating\"),getReturnWaterTemp(T181,AD181, activeEWTHeating, AY181, \"heating\")))","v":""},"",{"$f":" getNozzle(T181, W181, Y181, Z181, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I182)),I182<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I182, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H182)),H182<0),\"\",intlEstQuantity(T182, W182*12, H182)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T182=\"Select Model\",\"\",coilCircuitChange(W182, U182, AC182, T182,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T182=\"Select Model\",\"\",beamWidth(T182))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T182=\"Select Model\",T182=\"PCBL\"), 0,getSPIP(T182, W182, Y182, BD182, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T182=\"Select Model\", \"\",IF(T182=\"PCBL\",0,primaryAirSensibleCapacityIP($T182,$W182,activeRoomTempCooling,activePriAirTempCooling,$Y182,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T182=\"Select Model\",\"\",IF($T182=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y182,activeElevation)))","v":""},{"$f":"IF(OR(T182=\"Select Model\",T182=\"PCBL\"), 0,IF(AD182=0,0,-primaryAirSensibleCapacityIP($T182,$W182,activeRoomTempHeating,activePriAirTempHeating,$Y182,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T182=\"Select Model\", \"\", InductionRatio($T182,BD182,$W182,$Y182)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T182=\"Select Model\", \"\",IF($T182=\"PCBL\",\"N/A\",minVAVSetBack(AA182, Y182))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T182=\"Select Model\", \"\",IF($T182= \"PCBL\",\"N/A\",getDischargeAirTemp($T182,$V182,$AC182,$W182,BD182,$AL182, $Y182, $AS182, \"cooling\",activeElevation,$AB182,$AJ182,$AV182,$BB182))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T182=\"Select Model\",$T182=\"PCBL\"), \"\",getDischargeAirTemp($T182,$V182,$AD182,$W182,BD182,$AL182, $Y182, $AY182, \"heating\",activeElevation,$AB182,$AJ182,$AV182,$BB182)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T182=\"Select Model\", \"\",IF(OR($T182=\"ACBC_1W\",$T182=\"ACBC_2W\",LEFT($T182,4)=\"ACBR\",$T182 = \"LIU24_2W\",LEFT($T182,3)=\"RIU\",LEFT($T182,6)=\"ACBL12\"), IF((soundLevel($T182, $AB182, BD182, $Y182, $W182,$AJ182,$AA182,\"dba\"))<15,\"<15\",soundLevel($T182, $AB182, BD182, $Y182, $W182,$AJ182,$AA182,\"dba\")+0.4),IF((soundLevel($T182, $AB182, BD182, $Y182, $W182,$AJ182,$AA182,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T182, $AB182, BD182, $Y182, $W182,$AJ182,$AA182,\"dba\")+5)<15, \"<15\", soundLevel($T182, $AB182, BD182,$Y182, $W182,$AJ182,$AA182,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T182=\"Select Model\", \"\",IF(OR($T182=\"ACBC_1W\",$T182=\"ACBC_2W\",LEFT($T182,4)=\"ACBR\",$T182=\"LIU24_2W\",LEFT($T182,3)=\"RIU\",LEFT($T182,6)=\"ACBL12\"), IF((soundLevel($T182, $AB182, BD182, $Y182, $W182,$AJ182,$AA182,\"NC\"))<15,\"<15\",soundLevel($T182, $AB182, BD182, $Y182, $W182,$AJ182,$AA182,\"NC\")+0.4),IF((soundLevel($T182, $AB182, BD182, $Y182, $W182,$AJ182,$AA182,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T182, $AB182, BD182, $Y182, $W182,$AJ182,$AA182,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T182, $AB182, BD182, $Y182, $W182,$AJ182,$AA182,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T182=\"Select Model\",\"\",IF($T182=\"LIU24_2W\",calcQwIP($Y182,$W182,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC182,$AI182,\"latent\",$U182&\"P\"&IF($V182=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T182,activeElevation),\"\"))","v":""},{"$f":"IF($T182=\"Select Model\",\"\",IF($T182=\"ACBC_1W\",calcQwIP($Y182,$W182,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC182,BD182,\"capacity\",$U182&\"P\"&IF($V182=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T182,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y182,$W182,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC182,BD182,\"capacity\",$U182&\"P\"&IF($V182=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T182,activeElevation)))","v":""},"",{"$f":"IF(T182=\"Select Model\", 0,waterPressureDrop(W182, U182 & \"P\" & IF(V182=\"Dual\",2,1) &\"C\", AC182, \"cooling\", T182))","v":0},{"$f":"IF(T182=\"Select Model\", \"\",getReturnWaterTemp(T182,AC182, activeEWTCooling, AS182, \"cooling\"))","v":""},"",{"$f":"IF($T182<>\"ACBC_1W\",\"\",IF($J182=\"\",\"\",FintubeCapacity($T182,$W182,$AE182,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T182=\"Select Model\",T182=\"PCBL\"),\"\",calcQwIP(Y182,W182,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD182,BD182,\"capacity\",U182&\"P\"&IF(V182=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T182,activeElevation))","v":""},"",{"$f":"IF(OR(T182=\"Select Model\",T182=\"PCBL\"), \"\",IF(AY182=0,\"N/A\",waterPressureDrop(W182, U182 & \"P\" & IF(V182=\"Dual\",2,1) &\"C\", AD182, \"heating\", T182)))","v":""},{"$f":"IF(OR(T182=\"Select Model\",T182=\"PCBL\"), \"\",IF(AY182=0,getReturnWaterTemp(T182,AE182, activeEWTHeating, AX182, \"heating\"),getReturnWaterTemp(T182,AD182, activeEWTHeating, AY182, \"heating\")))","v":""},"",{"$f":" getNozzle(T182, W182, Y182, Z182, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I183)),I183<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I183, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H183)),H183<0),\"\",intlEstQuantity(T183, W183*12, H183)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T183=\"Select Model\",\"\",coilCircuitChange(W183, U183, AC183, T183,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T183=\"Select Model\",\"\",beamWidth(T183))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T183=\"Select Model\",T183=\"PCBL\"), 0,getSPIP(T183, W183, Y183, BD183, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T183=\"Select Model\", \"\",IF(T183=\"PCBL\",0,primaryAirSensibleCapacityIP($T183,$W183,activeRoomTempCooling,activePriAirTempCooling,$Y183,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T183=\"Select Model\",\"\",IF($T183=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y183,activeElevation)))","v":""},{"$f":"IF(OR(T183=\"Select Model\",T183=\"PCBL\"), 0,IF(AD183=0,0,-primaryAirSensibleCapacityIP($T183,$W183,activeRoomTempHeating,activePriAirTempHeating,$Y183,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T183=\"Select Model\", \"\", InductionRatio($T183,BD183,$W183,$Y183)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T183=\"Select Model\", \"\",IF($T183=\"PCBL\",\"N/A\",minVAVSetBack(AA183, Y183))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T183=\"Select Model\", \"\",IF($T183= \"PCBL\",\"N/A\",getDischargeAirTemp($T183,$V183,$AC183,$W183,BD183,$AL183, $Y183, $AS183, \"cooling\",activeElevation,$AB183,$AJ183,$AV183,$BB183))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T183=\"Select Model\",$T183=\"PCBL\"), \"\",getDischargeAirTemp($T183,$V183,$AD183,$W183,BD183,$AL183, $Y183, $AY183, \"heating\",activeElevation,$AB183,$AJ183,$AV183,$BB183)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T183=\"Select Model\", \"\",IF(OR($T183=\"ACBC_1W\",$T183=\"ACBC_2W\",LEFT($T183,4)=\"ACBR\",$T183 = \"LIU24_2W\",LEFT($T183,3)=\"RIU\",LEFT($T183,6)=\"ACBL12\"), IF((soundLevel($T183, $AB183, BD183, $Y183, $W183,$AJ183,$AA183,\"dba\"))<15,\"<15\",soundLevel($T183, $AB183, BD183, $Y183, $W183,$AJ183,$AA183,\"dba\")+0.4),IF((soundLevel($T183, $AB183, BD183, $Y183, $W183,$AJ183,$AA183,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T183, $AB183, BD183, $Y183, $W183,$AJ183,$AA183,\"dba\")+5)<15, \"<15\", soundLevel($T183, $AB183, BD183,$Y183, $W183,$AJ183,$AA183,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T183=\"Select Model\", \"\",IF(OR($T183=\"ACBC_1W\",$T183=\"ACBC_2W\",LEFT($T183,4)=\"ACBR\",$T183=\"LIU24_2W\",LEFT($T183,3)=\"RIU\",LEFT($T183,6)=\"ACBL12\"), IF((soundLevel($T183, $AB183, BD183, $Y183, $W183,$AJ183,$AA183,\"NC\"))<15,\"<15\",soundLevel($T183, $AB183, BD183, $Y183, $W183,$AJ183,$AA183,\"NC\")+0.4),IF((soundLevel($T183, $AB183, BD183, $Y183, $W183,$AJ183,$AA183,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T183, $AB183, BD183, $Y183, $W183,$AJ183,$AA183,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T183, $AB183, BD183, $Y183, $W183,$AJ183,$AA183,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T183=\"Select Model\",\"\",IF($T183=\"LIU24_2W\",calcQwIP($Y183,$W183,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC183,$AI183,\"latent\",$U183&\"P\"&IF($V183=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T183,activeElevation),\"\"))","v":""},{"$f":"IF($T183=\"Select Model\",\"\",IF($T183=\"ACBC_1W\",calcQwIP($Y183,$W183,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC183,BD183,\"capacity\",$U183&\"P\"&IF($V183=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T183,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y183,$W183,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC183,BD183,\"capacity\",$U183&\"P\"&IF($V183=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T183,activeElevation)))","v":""},"",{"$f":"IF(T183=\"Select Model\", 0,waterPressureDrop(W183, U183 & \"P\" & IF(V183=\"Dual\",2,1) &\"C\", AC183, \"cooling\", T183))","v":0},{"$f":"IF(T183=\"Select Model\", \"\",getReturnWaterTemp(T183,AC183, activeEWTCooling, AS183, \"cooling\"))","v":""},"",{"$f":"IF($T183<>\"ACBC_1W\",\"\",IF($J183=\"\",\"\",FintubeCapacity($T183,$W183,$AE183,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T183=\"Select Model\",T183=\"PCBL\"),\"\",calcQwIP(Y183,W183,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD183,BD183,\"capacity\",U183&\"P\"&IF(V183=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T183,activeElevation))","v":""},"",{"$f":"IF(OR(T183=\"Select Model\",T183=\"PCBL\"), \"\",IF(AY183=0,\"N/A\",waterPressureDrop(W183, U183 & \"P\" & IF(V183=\"Dual\",2,1) &\"C\", AD183, \"heating\", T183)))","v":""},{"$f":"IF(OR(T183=\"Select Model\",T183=\"PCBL\"), \"\",IF(AY183=0,getReturnWaterTemp(T183,AE183, activeEWTHeating, AX183, \"heating\"),getReturnWaterTemp(T183,AD183, activeEWTHeating, AY183, \"heating\")))","v":""},"",{"$f":" getNozzle(T183, W183, Y183, Z183, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I184)),I184<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I184, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H184)),H184<0),\"\",intlEstQuantity(T184, W184*12, H184)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T184=\"Select Model\",\"\",coilCircuitChange(W184, U184, AC184, T184,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T184=\"Select Model\",\"\",beamWidth(T184))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T184=\"Select Model\",T184=\"PCBL\"), 0,getSPIP(T184, W184, Y184, BD184, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T184=\"Select Model\", \"\",IF(T184=\"PCBL\",0,primaryAirSensibleCapacityIP($T184,$W184,activeRoomTempCooling,activePriAirTempCooling,$Y184,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T184=\"Select Model\",\"\",IF($T184=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y184,activeElevation)))","v":""},{"$f":"IF(OR(T184=\"Select Model\",T184=\"PCBL\"), 0,IF(AD184=0,0,-primaryAirSensibleCapacityIP($T184,$W184,activeRoomTempHeating,activePriAirTempHeating,$Y184,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T184=\"Select Model\", \"\", InductionRatio($T184,BD184,$W184,$Y184)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T184=\"Select Model\", \"\",IF($T184=\"PCBL\",\"N/A\",minVAVSetBack(AA184, Y184))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T184=\"Select Model\", \"\",IF($T184= \"PCBL\",\"N/A\",getDischargeAirTemp($T184,$V184,$AC184,$W184,BD184,$AL184, $Y184, $AS184, \"cooling\",activeElevation,$AB184,$AJ184,$AV184,$BB184))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T184=\"Select Model\",$T184=\"PCBL\"), \"\",getDischargeAirTemp($T184,$V184,$AD184,$W184,BD184,$AL184, $Y184, $AY184, \"heating\",activeElevation,$AB184,$AJ184,$AV184,$BB184)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T184=\"Select Model\", \"\",IF(OR($T184=\"ACBC_1W\",$T184=\"ACBC_2W\",LEFT($T184,4)=\"ACBR\",$T184 = \"LIU24_2W\",LEFT($T184,3)=\"RIU\",LEFT($T184,6)=\"ACBL12\"), IF((soundLevel($T184, $AB184, BD184, $Y184, $W184,$AJ184,$AA184,\"dba\"))<15,\"<15\",soundLevel($T184, $AB184, BD184, $Y184, $W184,$AJ184,$AA184,\"dba\")+0.4),IF((soundLevel($T184, $AB184, BD184, $Y184, $W184,$AJ184,$AA184,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T184, $AB184, BD184, $Y184, $W184,$AJ184,$AA184,\"dba\")+5)<15, \"<15\", soundLevel($T184, $AB184, BD184,$Y184, $W184,$AJ184,$AA184,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T184=\"Select Model\", \"\",IF(OR($T184=\"ACBC_1W\",$T184=\"ACBC_2W\",LEFT($T184,4)=\"ACBR\",$T184=\"LIU24_2W\",LEFT($T184,3)=\"RIU\",LEFT($T184,6)=\"ACBL12\"), IF((soundLevel($T184, $AB184, BD184, $Y184, $W184,$AJ184,$AA184,\"NC\"))<15,\"<15\",soundLevel($T184, $AB184, BD184, $Y184, $W184,$AJ184,$AA184,\"NC\")+0.4),IF((soundLevel($T184, $AB184, BD184, $Y184, $W184,$AJ184,$AA184,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T184, $AB184, BD184, $Y184, $W184,$AJ184,$AA184,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T184, $AB184, BD184, $Y184, $W184,$AJ184,$AA184,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T184=\"Select Model\",\"\",IF($T184=\"LIU24_2W\",calcQwIP($Y184,$W184,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC184,$AI184,\"latent\",$U184&\"P\"&IF($V184=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T184,activeElevation),\"\"))","v":""},{"$f":"IF($T184=\"Select Model\",\"\",IF($T184=\"ACBC_1W\",calcQwIP($Y184,$W184,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC184,BD184,\"capacity\",$U184&\"P\"&IF($V184=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T184,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y184,$W184,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC184,BD184,\"capacity\",$U184&\"P\"&IF($V184=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T184,activeElevation)))","v":""},"",{"$f":"IF(T184=\"Select Model\", 0,waterPressureDrop(W184, U184 & \"P\" & IF(V184=\"Dual\",2,1) &\"C\", AC184, \"cooling\", T184))","v":0},{"$f":"IF(T184=\"Select Model\", \"\",getReturnWaterTemp(T184,AC184, activeEWTCooling, AS184, \"cooling\"))","v":""},"",{"$f":"IF($T184<>\"ACBC_1W\",\"\",IF($J184=\"\",\"\",FintubeCapacity($T184,$W184,$AE184,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T184=\"Select Model\",T184=\"PCBL\"),\"\",calcQwIP(Y184,W184,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD184,BD184,\"capacity\",U184&\"P\"&IF(V184=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T184,activeElevation))","v":""},"",{"$f":"IF(OR(T184=\"Select Model\",T184=\"PCBL\"), \"\",IF(AY184=0,\"N/A\",waterPressureDrop(W184, U184 & \"P\" & IF(V184=\"Dual\",2,1) &\"C\", AD184, \"heating\", T184)))","v":""},{"$f":"IF(OR(T184=\"Select Model\",T184=\"PCBL\"), \"\",IF(AY184=0,getReturnWaterTemp(T184,AE184, activeEWTHeating, AX184, \"heating\"),getReturnWaterTemp(T184,AD184, activeEWTHeating, AY184, \"heating\")))","v":""},"",{"$f":" getNozzle(T184, W184, Y184, Z184, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I185)),I185<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I185, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H185)),H185<0),\"\",intlEstQuantity(T185, W185*12, H185)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T185=\"Select Model\",\"\",coilCircuitChange(W185, U185, AC185, T185,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T185=\"Select Model\",\"\",beamWidth(T185))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T185=\"Select Model\",T185=\"PCBL\"), 0,getSPIP(T185, W185, Y185, BD185, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T185=\"Select Model\", \"\",IF(T185=\"PCBL\",0,primaryAirSensibleCapacityIP($T185,$W185,activeRoomTempCooling,activePriAirTempCooling,$Y185,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T185=\"Select Model\",\"\",IF($T185=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y185,activeElevation)))","v":""},{"$f":"IF(OR(T185=\"Select Model\",T185=\"PCBL\"), 0,IF(AD185=0,0,-primaryAirSensibleCapacityIP($T185,$W185,activeRoomTempHeating,activePriAirTempHeating,$Y185,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T185=\"Select Model\", \"\", InductionRatio($T185,BD185,$W185,$Y185)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T185=\"Select Model\", \"\",IF($T185=\"PCBL\",\"N/A\",minVAVSetBack(AA185, Y185))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T185=\"Select Model\", \"\",IF($T185= \"PCBL\",\"N/A\",getDischargeAirTemp($T185,$V185,$AC185,$W185,BD185,$AL185, $Y185, $AS185, \"cooling\",activeElevation,$AB185,$AJ185,$AV185,$BB185))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T185=\"Select Model\",$T185=\"PCBL\"), \"\",getDischargeAirTemp($T185,$V185,$AD185,$W185,BD185,$AL185, $Y185, $AY185, \"heating\",activeElevation,$AB185,$AJ185,$AV185,$BB185)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T185=\"Select Model\", \"\",IF(OR($T185=\"ACBC_1W\",$T185=\"ACBC_2W\",LEFT($T185,4)=\"ACBR\",$T185 = \"LIU24_2W\",LEFT($T185,3)=\"RIU\",LEFT($T185,6)=\"ACBL12\"), IF((soundLevel($T185, $AB185, BD185, $Y185, $W185,$AJ185,$AA185,\"dba\"))<15,\"<15\",soundLevel($T185, $AB185, BD185, $Y185, $W185,$AJ185,$AA185,\"dba\")+0.4),IF((soundLevel($T185, $AB185, BD185, $Y185, $W185,$AJ185,$AA185,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T185, $AB185, BD185, $Y185, $W185,$AJ185,$AA185,\"dba\")+5)<15, \"<15\", soundLevel($T185, $AB185, BD185,$Y185, $W185,$AJ185,$AA185,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T185=\"Select Model\", \"\",IF(OR($T185=\"ACBC_1W\",$T185=\"ACBC_2W\",LEFT($T185,4)=\"ACBR\",$T185=\"LIU24_2W\",LEFT($T185,3)=\"RIU\",LEFT($T185,6)=\"ACBL12\"), IF((soundLevel($T185, $AB185, BD185, $Y185, $W185,$AJ185,$AA185,\"NC\"))<15,\"<15\",soundLevel($T185, $AB185, BD185, $Y185, $W185,$AJ185,$AA185,\"NC\")+0.4),IF((soundLevel($T185, $AB185, BD185, $Y185, $W185,$AJ185,$AA185,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T185, $AB185, BD185, $Y185, $W185,$AJ185,$AA185,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T185, $AB185, BD185, $Y185, $W185,$AJ185,$AA185,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T185=\"Select Model\",\"\",IF($T185=\"LIU24_2W\",calcQwIP($Y185,$W185,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC185,$AI185,\"latent\",$U185&\"P\"&IF($V185=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T185,activeElevation),\"\"))","v":""},{"$f":"IF($T185=\"Select Model\",\"\",IF($T185=\"ACBC_1W\",calcQwIP($Y185,$W185,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC185,BD185,\"capacity\",$U185&\"P\"&IF($V185=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T185,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y185,$W185,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC185,BD185,\"capacity\",$U185&\"P\"&IF($V185=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T185,activeElevation)))","v":""},"",{"$f":"IF(T185=\"Select Model\", 0,waterPressureDrop(W185, U185 & \"P\" & IF(V185=\"Dual\",2,1) &\"C\", AC185, \"cooling\", T185))","v":0},{"$f":"IF(T185=\"Select Model\", \"\",getReturnWaterTemp(T185,AC185, activeEWTCooling, AS185, \"cooling\"))","v":""},"",{"$f":"IF($T185<>\"ACBC_1W\",\"\",IF($J185=\"\",\"\",FintubeCapacity($T185,$W185,$AE185,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T185=\"Select Model\",T185=\"PCBL\"),\"\",calcQwIP(Y185,W185,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD185,BD185,\"capacity\",U185&\"P\"&IF(V185=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T185,activeElevation))","v":""},"",{"$f":"IF(OR(T185=\"Select Model\",T185=\"PCBL\"), \"\",IF(AY185=0,\"N/A\",waterPressureDrop(W185, U185 & \"P\" & IF(V185=\"Dual\",2,1) &\"C\", AD185, \"heating\", T185)))","v":""},{"$f":"IF(OR(T185=\"Select Model\",T185=\"PCBL\"), \"\",IF(AY185=0,getReturnWaterTemp(T185,AE185, activeEWTHeating, AX185, \"heating\"),getReturnWaterTemp(T185,AD185, activeEWTHeating, AY185, \"heating\")))","v":""},"",{"$f":" getNozzle(T185, W185, Y185, Z185, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I186)),I186<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I186, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H186)),H186<0),\"\",intlEstQuantity(T186, W186*12, H186)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T186=\"Select Model\",\"\",coilCircuitChange(W186, U186, AC186, T186,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T186=\"Select Model\",\"\",beamWidth(T186))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T186=\"Select Model\",T186=\"PCBL\"), 0,getSPIP(T186, W186, Y186, BD186, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T186=\"Select Model\", \"\",IF(T186=\"PCBL\",0,primaryAirSensibleCapacityIP($T186,$W186,activeRoomTempCooling,activePriAirTempCooling,$Y186,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T186=\"Select Model\",\"\",IF($T186=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y186,activeElevation)))","v":""},{"$f":"IF(OR(T186=\"Select Model\",T186=\"PCBL\"), 0,IF(AD186=0,0,-primaryAirSensibleCapacityIP($T186,$W186,activeRoomTempHeating,activePriAirTempHeating,$Y186,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T186=\"Select Model\", \"\", InductionRatio($T186,BD186,$W186,$Y186)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T186=\"Select Model\", \"\",IF($T186=\"PCBL\",\"N/A\",minVAVSetBack(AA186, Y186))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T186=\"Select Model\", \"\",IF($T186= \"PCBL\",\"N/A\",getDischargeAirTemp($T186,$V186,$AC186,$W186,BD186,$AL186, $Y186, $AS186, \"cooling\",activeElevation,$AB186,$AJ186,$AV186,$BB186))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T186=\"Select Model\",$T186=\"PCBL\"), \"\",getDischargeAirTemp($T186,$V186,$AD186,$W186,BD186,$AL186, $Y186, $AY186, \"heating\",activeElevation,$AB186,$AJ186,$AV186,$BB186)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T186=\"Select Model\", \"\",IF(OR($T186=\"ACBC_1W\",$T186=\"ACBC_2W\",LEFT($T186,4)=\"ACBR\",$T186 = \"LIU24_2W\",LEFT($T186,3)=\"RIU\",LEFT($T186,6)=\"ACBL12\"), IF((soundLevel($T186, $AB186, BD186, $Y186, $W186,$AJ186,$AA186,\"dba\"))<15,\"<15\",soundLevel($T186, $AB186, BD186, $Y186, $W186,$AJ186,$AA186,\"dba\")+0.4),IF((soundLevel($T186, $AB186, BD186, $Y186, $W186,$AJ186,$AA186,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T186, $AB186, BD186, $Y186, $W186,$AJ186,$AA186,\"dba\")+5)<15, \"<15\", soundLevel($T186, $AB186, BD186,$Y186, $W186,$AJ186,$AA186,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T186=\"Select Model\", \"\",IF(OR($T186=\"ACBC_1W\",$T186=\"ACBC_2W\",LEFT($T186,4)=\"ACBR\",$T186=\"LIU24_2W\",LEFT($T186,3)=\"RIU\",LEFT($T186,6)=\"ACBL12\"), IF((soundLevel($T186, $AB186, BD186, $Y186, $W186,$AJ186,$AA186,\"NC\"))<15,\"<15\",soundLevel($T186, $AB186, BD186, $Y186, $W186,$AJ186,$AA186,\"NC\")+0.4),IF((soundLevel($T186, $AB186, BD186, $Y186, $W186,$AJ186,$AA186,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T186, $AB186, BD186, $Y186, $W186,$AJ186,$AA186,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T186, $AB186, BD186, $Y186, $W186,$AJ186,$AA186,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T186=\"Select Model\",\"\",IF($T186=\"LIU24_2W\",calcQwIP($Y186,$W186,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC186,$AI186,\"latent\",$U186&\"P\"&IF($V186=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T186,activeElevation),\"\"))","v":""},{"$f":"IF($T186=\"Select Model\",\"\",IF($T186=\"ACBC_1W\",calcQwIP($Y186,$W186,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC186,BD186,\"capacity\",$U186&\"P\"&IF($V186=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T186,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y186,$W186,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC186,BD186,\"capacity\",$U186&\"P\"&IF($V186=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T186,activeElevation)))","v":""},"",{"$f":"IF(T186=\"Select Model\", 0,waterPressureDrop(W186, U186 & \"P\" & IF(V186=\"Dual\",2,1) &\"C\", AC186, \"cooling\", T186))","v":0},{"$f":"IF(T186=\"Select Model\", \"\",getReturnWaterTemp(T186,AC186, activeEWTCooling, AS186, \"cooling\"))","v":""},"",{"$f":"IF($T186<>\"ACBC_1W\",\"\",IF($J186=\"\",\"\",FintubeCapacity($T186,$W186,$AE186,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T186=\"Select Model\",T186=\"PCBL\"),\"\",calcQwIP(Y186,W186,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD186,BD186,\"capacity\",U186&\"P\"&IF(V186=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T186,activeElevation))","v":""},"",{"$f":"IF(OR(T186=\"Select Model\",T186=\"PCBL\"), \"\",IF(AY186=0,\"N/A\",waterPressureDrop(W186, U186 & \"P\" & IF(V186=\"Dual\",2,1) &\"C\", AD186, \"heating\", T186)))","v":""},{"$f":"IF(OR(T186=\"Select Model\",T186=\"PCBL\"), \"\",IF(AY186=0,getReturnWaterTemp(T186,AE186, activeEWTHeating, AX186, \"heating\"),getReturnWaterTemp(T186,AD186, activeEWTHeating, AY186, \"heating\")))","v":""},"",{"$f":" getNozzle(T186, W186, Y186, Z186, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I187)),I187<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I187, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H187)),H187<0),\"\",intlEstQuantity(T187, W187*12, H187)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T187=\"Select Model\",\"\",coilCircuitChange(W187, U187, AC187, T187,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T187=\"Select Model\",\"\",beamWidth(T187))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T187=\"Select Model\",T187=\"PCBL\"), 0,getSPIP(T187, W187, Y187, BD187, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T187=\"Select Model\", \"\",IF(T187=\"PCBL\",0,primaryAirSensibleCapacityIP($T187,$W187,activeRoomTempCooling,activePriAirTempCooling,$Y187,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T187=\"Select Model\",\"\",IF($T187=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y187,activeElevation)))","v":""},{"$f":"IF(OR(T187=\"Select Model\",T187=\"PCBL\"), 0,IF(AD187=0,0,-primaryAirSensibleCapacityIP($T187,$W187,activeRoomTempHeating,activePriAirTempHeating,$Y187,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T187=\"Select Model\", \"\", InductionRatio($T187,BD187,$W187,$Y187)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T187=\"Select Model\", \"\",IF($T187=\"PCBL\",\"N/A\",minVAVSetBack(AA187, Y187))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T187=\"Select Model\", \"\",IF($T187= \"PCBL\",\"N/A\",getDischargeAirTemp($T187,$V187,$AC187,$W187,BD187,$AL187, $Y187, $AS187, \"cooling\",activeElevation,$AB187,$AJ187,$AV187,$BB187))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T187=\"Select Model\",$T187=\"PCBL\"), \"\",getDischargeAirTemp($T187,$V187,$AD187,$W187,BD187,$AL187, $Y187, $AY187, \"heating\",activeElevation,$AB187,$AJ187,$AV187,$BB187)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T187=\"Select Model\", \"\",IF(OR($T187=\"ACBC_1W\",$T187=\"ACBC_2W\",LEFT($T187,4)=\"ACBR\",$T187 = \"LIU24_2W\",LEFT($T187,3)=\"RIU\",LEFT($T187,6)=\"ACBL12\"), IF((soundLevel($T187, $AB187, BD187, $Y187, $W187,$AJ187,$AA187,\"dba\"))<15,\"<15\",soundLevel($T187, $AB187, BD187, $Y187, $W187,$AJ187,$AA187,\"dba\")+0.4),IF((soundLevel($T187, $AB187, BD187, $Y187, $W187,$AJ187,$AA187,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T187, $AB187, BD187, $Y187, $W187,$AJ187,$AA187,\"dba\")+5)<15, \"<15\", soundLevel($T187, $AB187, BD187,$Y187, $W187,$AJ187,$AA187,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T187=\"Select Model\", \"\",IF(OR($T187=\"ACBC_1W\",$T187=\"ACBC_2W\",LEFT($T187,4)=\"ACBR\",$T187=\"LIU24_2W\",LEFT($T187,3)=\"RIU\",LEFT($T187,6)=\"ACBL12\"), IF((soundLevel($T187, $AB187, BD187, $Y187, $W187,$AJ187,$AA187,\"NC\"))<15,\"<15\",soundLevel($T187, $AB187, BD187, $Y187, $W187,$AJ187,$AA187,\"NC\")+0.4),IF((soundLevel($T187, $AB187, BD187, $Y187, $W187,$AJ187,$AA187,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T187, $AB187, BD187, $Y187, $W187,$AJ187,$AA187,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T187, $AB187, BD187, $Y187, $W187,$AJ187,$AA187,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T187=\"Select Model\",\"\",IF($T187=\"LIU24_2W\",calcQwIP($Y187,$W187,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC187,$AI187,\"latent\",$U187&\"P\"&IF($V187=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T187,activeElevation),\"\"))","v":""},{"$f":"IF($T187=\"Select Model\",\"\",IF($T187=\"ACBC_1W\",calcQwIP($Y187,$W187,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC187,BD187,\"capacity\",$U187&\"P\"&IF($V187=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T187,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y187,$W187,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC187,BD187,\"capacity\",$U187&\"P\"&IF($V187=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T187,activeElevation)))","v":""},"",{"$f":"IF(T187=\"Select Model\", 0,waterPressureDrop(W187, U187 & \"P\" & IF(V187=\"Dual\",2,1) &\"C\", AC187, \"cooling\", T187))","v":0},{"$f":"IF(T187=\"Select Model\", \"\",getReturnWaterTemp(T187,AC187, activeEWTCooling, AS187, \"cooling\"))","v":""},"",{"$f":"IF($T187<>\"ACBC_1W\",\"\",IF($J187=\"\",\"\",FintubeCapacity($T187,$W187,$AE187,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T187=\"Select Model\",T187=\"PCBL\"),\"\",calcQwIP(Y187,W187,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD187,BD187,\"capacity\",U187&\"P\"&IF(V187=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T187,activeElevation))","v":""},"",{"$f":"IF(OR(T187=\"Select Model\",T187=\"PCBL\"), \"\",IF(AY187=0,\"N/A\",waterPressureDrop(W187, U187 & \"P\" & IF(V187=\"Dual\",2,1) &\"C\", AD187, \"heating\", T187)))","v":""},{"$f":"IF(OR(T187=\"Select Model\",T187=\"PCBL\"), \"\",IF(AY187=0,getReturnWaterTemp(T187,AE187, activeEWTHeating, AX187, \"heating\"),getReturnWaterTemp(T187,AD187, activeEWTHeating, AY187, \"heating\")))","v":""},"",{"$f":" getNozzle(T187, W187, Y187, Z187, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I188)),I188<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I188, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H188)),H188<0),\"\",intlEstQuantity(T188, W188*12, H188)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T188=\"Select Model\",\"\",coilCircuitChange(W188, U188, AC188, T188,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T188=\"Select Model\",\"\",beamWidth(T188))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T188=\"Select Model\",T188=\"PCBL\"), 0,getSPIP(T188, W188, Y188, BD188, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T188=\"Select Model\", \"\",IF(T188=\"PCBL\",0,primaryAirSensibleCapacityIP($T188,$W188,activeRoomTempCooling,activePriAirTempCooling,$Y188,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T188=\"Select Model\",\"\",IF($T188=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y188,activeElevation)))","v":""},{"$f":"IF(OR(T188=\"Select Model\",T188=\"PCBL\"), 0,IF(AD188=0,0,-primaryAirSensibleCapacityIP($T188,$W188,activeRoomTempHeating,activePriAirTempHeating,$Y188,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T188=\"Select Model\", \"\", InductionRatio($T188,BD188,$W188,$Y188)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T188=\"Select Model\", \"\",IF($T188=\"PCBL\",\"N/A\",minVAVSetBack(AA188, Y188))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T188=\"Select Model\", \"\",IF($T188= \"PCBL\",\"N/A\",getDischargeAirTemp($T188,$V188,$AC188,$W188,BD188,$AL188, $Y188, $AS188, \"cooling\",activeElevation,$AB188,$AJ188,$AV188,$BB188))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T188=\"Select Model\",$T188=\"PCBL\"), \"\",getDischargeAirTemp($T188,$V188,$AD188,$W188,BD188,$AL188, $Y188, $AY188, \"heating\",activeElevation,$AB188,$AJ188,$AV188,$BB188)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T188=\"Select Model\", \"\",IF(OR($T188=\"ACBC_1W\",$T188=\"ACBC_2W\",LEFT($T188,4)=\"ACBR\",$T188 = \"LIU24_2W\",LEFT($T188,3)=\"RIU\",LEFT($T188,6)=\"ACBL12\"), IF((soundLevel($T188, $AB188, BD188, $Y188, $W188,$AJ188,$AA188,\"dba\"))<15,\"<15\",soundLevel($T188, $AB188, BD188, $Y188, $W188,$AJ188,$AA188,\"dba\")+0.4),IF((soundLevel($T188, $AB188, BD188, $Y188, $W188,$AJ188,$AA188,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T188, $AB188, BD188, $Y188, $W188,$AJ188,$AA188,\"dba\")+5)<15, \"<15\", soundLevel($T188, $AB188, BD188,$Y188, $W188,$AJ188,$AA188,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T188=\"Select Model\", \"\",IF(OR($T188=\"ACBC_1W\",$T188=\"ACBC_2W\",LEFT($T188,4)=\"ACBR\",$T188=\"LIU24_2W\",LEFT($T188,3)=\"RIU\",LEFT($T188,6)=\"ACBL12\"), IF((soundLevel($T188, $AB188, BD188, $Y188, $W188,$AJ188,$AA188,\"NC\"))<15,\"<15\",soundLevel($T188, $AB188, BD188, $Y188, $W188,$AJ188,$AA188,\"NC\")+0.4),IF((soundLevel($T188, $AB188, BD188, $Y188, $W188,$AJ188,$AA188,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T188, $AB188, BD188, $Y188, $W188,$AJ188,$AA188,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T188, $AB188, BD188, $Y188, $W188,$AJ188,$AA188,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T188=\"Select Model\",\"\",IF($T188=\"LIU24_2W\",calcQwIP($Y188,$W188,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC188,$AI188,\"latent\",$U188&\"P\"&IF($V188=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T188,activeElevation),\"\"))","v":""},{"$f":"IF($T188=\"Select Model\",\"\",IF($T188=\"ACBC_1W\",calcQwIP($Y188,$W188,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC188,BD188,\"capacity\",$U188&\"P\"&IF($V188=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T188,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y188,$W188,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC188,BD188,\"capacity\",$U188&\"P\"&IF($V188=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T188,activeElevation)))","v":""},"",{"$f":"IF(T188=\"Select Model\", 0,waterPressureDrop(W188, U188 & \"P\" & IF(V188=\"Dual\",2,1) &\"C\", AC188, \"cooling\", T188))","v":0},{"$f":"IF(T188=\"Select Model\", \"\",getReturnWaterTemp(T188,AC188, activeEWTCooling, AS188, \"cooling\"))","v":""},"",{"$f":"IF($T188<>\"ACBC_1W\",\"\",IF($J188=\"\",\"\",FintubeCapacity($T188,$W188,$AE188,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T188=\"Select Model\",T188=\"PCBL\"),\"\",calcQwIP(Y188,W188,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD188,BD188,\"capacity\",U188&\"P\"&IF(V188=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T188,activeElevation))","v":""},"",{"$f":"IF(OR(T188=\"Select Model\",T188=\"PCBL\"), \"\",IF(AY188=0,\"N/A\",waterPressureDrop(W188, U188 & \"P\" & IF(V188=\"Dual\",2,1) &\"C\", AD188, \"heating\", T188)))","v":""},{"$f":"IF(OR(T188=\"Select Model\",T188=\"PCBL\"), \"\",IF(AY188=0,getReturnWaterTemp(T188,AE188, activeEWTHeating, AX188, \"heating\"),getReturnWaterTemp(T188,AD188, activeEWTHeating, AY188, \"heating\")))","v":""},"",{"$f":" getNozzle(T188, W188, Y188, Z188, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I189)),I189<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I189, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H189)),H189<0),\"\",intlEstQuantity(T189, W189*12, H189)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T189=\"Select Model\",\"\",coilCircuitChange(W189, U189, AC189, T189,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T189=\"Select Model\",\"\",beamWidth(T189))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T189=\"Select Model\",T189=\"PCBL\"), 0,getSPIP(T189, W189, Y189, BD189, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T189=\"Select Model\", \"\",IF(T189=\"PCBL\",0,primaryAirSensibleCapacityIP($T189,$W189,activeRoomTempCooling,activePriAirTempCooling,$Y189,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T189=\"Select Model\",\"\",IF($T189=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y189,activeElevation)))","v":""},{"$f":"IF(OR(T189=\"Select Model\",T189=\"PCBL\"), 0,IF(AD189=0,0,-primaryAirSensibleCapacityIP($T189,$W189,activeRoomTempHeating,activePriAirTempHeating,$Y189,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T189=\"Select Model\", \"\", InductionRatio($T189,BD189,$W189,$Y189)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T189=\"Select Model\", \"\",IF($T189=\"PCBL\",\"N/A\",minVAVSetBack(AA189, Y189))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T189=\"Select Model\", \"\",IF($T189= \"PCBL\",\"N/A\",getDischargeAirTemp($T189,$V189,$AC189,$W189,BD189,$AL189, $Y189, $AS189, \"cooling\",activeElevation,$AB189,$AJ189,$AV189,$BB189))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T189=\"Select Model\",$T189=\"PCBL\"), \"\",getDischargeAirTemp($T189,$V189,$AD189,$W189,BD189,$AL189, $Y189, $AY189, \"heating\",activeElevation,$AB189,$AJ189,$AV189,$BB189)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T189=\"Select Model\", \"\",IF(OR($T189=\"ACBC_1W\",$T189=\"ACBC_2W\",LEFT($T189,4)=\"ACBR\",$T189 = \"LIU24_2W\",LEFT($T189,3)=\"RIU\",LEFT($T189,6)=\"ACBL12\"), IF((soundLevel($T189, $AB189, BD189, $Y189, $W189,$AJ189,$AA189,\"dba\"))<15,\"<15\",soundLevel($T189, $AB189, BD189, $Y189, $W189,$AJ189,$AA189,\"dba\")+0.4),IF((soundLevel($T189, $AB189, BD189, $Y189, $W189,$AJ189,$AA189,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T189, $AB189, BD189, $Y189, $W189,$AJ189,$AA189,\"dba\")+5)<15, \"<15\", soundLevel($T189, $AB189, BD189,$Y189, $W189,$AJ189,$AA189,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T189=\"Select Model\", \"\",IF(OR($T189=\"ACBC_1W\",$T189=\"ACBC_2W\",LEFT($T189,4)=\"ACBR\",$T189=\"LIU24_2W\",LEFT($T189,3)=\"RIU\",LEFT($T189,6)=\"ACBL12\"), IF((soundLevel($T189, $AB189, BD189, $Y189, $W189,$AJ189,$AA189,\"NC\"))<15,\"<15\",soundLevel($T189, $AB189, BD189, $Y189, $W189,$AJ189,$AA189,\"NC\")+0.4),IF((soundLevel($T189, $AB189, BD189, $Y189, $W189,$AJ189,$AA189,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T189, $AB189, BD189, $Y189, $W189,$AJ189,$AA189,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T189, $AB189, BD189, $Y189, $W189,$AJ189,$AA189,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T189=\"Select Model\",\"\",IF($T189=\"LIU24_2W\",calcQwIP($Y189,$W189,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC189,$AI189,\"latent\",$U189&\"P\"&IF($V189=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T189,activeElevation),\"\"))","v":""},{"$f":"IF($T189=\"Select Model\",\"\",IF($T189=\"ACBC_1W\",calcQwIP($Y189,$W189,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC189,BD189,\"capacity\",$U189&\"P\"&IF($V189=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T189,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y189,$W189,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC189,BD189,\"capacity\",$U189&\"P\"&IF($V189=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T189,activeElevation)))","v":""},"",{"$f":"IF(T189=\"Select Model\", 0,waterPressureDrop(W189, U189 & \"P\" & IF(V189=\"Dual\",2,1) &\"C\", AC189, \"cooling\", T189))","v":0},{"$f":"IF(T189=\"Select Model\", \"\",getReturnWaterTemp(T189,AC189, activeEWTCooling, AS189, \"cooling\"))","v":""},"",{"$f":"IF($T189<>\"ACBC_1W\",\"\",IF($J189=\"\",\"\",FintubeCapacity($T189,$W189,$AE189,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T189=\"Select Model\",T189=\"PCBL\"),\"\",calcQwIP(Y189,W189,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD189,BD189,\"capacity\",U189&\"P\"&IF(V189=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T189,activeElevation))","v":""},"",{"$f":"IF(OR(T189=\"Select Model\",T189=\"PCBL\"), \"\",IF(AY189=0,\"N/A\",waterPressureDrop(W189, U189 & \"P\" & IF(V189=\"Dual\",2,1) &\"C\", AD189, \"heating\", T189)))","v":""},{"$f":"IF(OR(T189=\"Select Model\",T189=\"PCBL\"), \"\",IF(AY189=0,getReturnWaterTemp(T189,AE189, activeEWTHeating, AX189, \"heating\"),getReturnWaterTemp(T189,AD189, activeEWTHeating, AY189, \"heating\")))","v":""},"",{"$f":" getNozzle(T189, W189, Y189, Z189, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I190)),I190<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I190, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H190)),H190<0),\"\",intlEstQuantity(T190, W190*12, H190)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T190=\"Select Model\",\"\",coilCircuitChange(W190, U190, AC190, T190,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T190=\"Select Model\",\"\",beamWidth(T190))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T190=\"Select Model\",T190=\"PCBL\"), 0,getSPIP(T190, W190, Y190, BD190, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T190=\"Select Model\", \"\",IF(T190=\"PCBL\",0,primaryAirSensibleCapacityIP($T190,$W190,activeRoomTempCooling,activePriAirTempCooling,$Y190,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T190=\"Select Model\",\"\",IF($T190=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y190,activeElevation)))","v":""},{"$f":"IF(OR(T190=\"Select Model\",T190=\"PCBL\"), 0,IF(AD190=0,0,-primaryAirSensibleCapacityIP($T190,$W190,activeRoomTempHeating,activePriAirTempHeating,$Y190,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T190=\"Select Model\", \"\", InductionRatio($T190,BD190,$W190,$Y190)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T190=\"Select Model\", \"\",IF($T190=\"PCBL\",\"N/A\",minVAVSetBack(AA190, Y190))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T190=\"Select Model\", \"\",IF($T190= \"PCBL\",\"N/A\",getDischargeAirTemp($T190,$V190,$AC190,$W190,BD190,$AL190, $Y190, $AS190, \"cooling\",activeElevation,$AB190,$AJ190,$AV190,$BB190))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T190=\"Select Model\",$T190=\"PCBL\"), \"\",getDischargeAirTemp($T190,$V190,$AD190,$W190,BD190,$AL190, $Y190, $AY190, \"heating\",activeElevation,$AB190,$AJ190,$AV190,$BB190)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T190=\"Select Model\", \"\",IF(OR($T190=\"ACBC_1W\",$T190=\"ACBC_2W\",LEFT($T190,4)=\"ACBR\",$T190 = \"LIU24_2W\",LEFT($T190,3)=\"RIU\",LEFT($T190,6)=\"ACBL12\"), IF((soundLevel($T190, $AB190, BD190, $Y190, $W190,$AJ190,$AA190,\"dba\"))<15,\"<15\",soundLevel($T190, $AB190, BD190, $Y190, $W190,$AJ190,$AA190,\"dba\")+0.4),IF((soundLevel($T190, $AB190, BD190, $Y190, $W190,$AJ190,$AA190,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T190, $AB190, BD190, $Y190, $W190,$AJ190,$AA190,\"dba\")+5)<15, \"<15\", soundLevel($T190, $AB190, BD190,$Y190, $W190,$AJ190,$AA190,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T190=\"Select Model\", \"\",IF(OR($T190=\"ACBC_1W\",$T190=\"ACBC_2W\",LEFT($T190,4)=\"ACBR\",$T190=\"LIU24_2W\",LEFT($T190,3)=\"RIU\",LEFT($T190,6)=\"ACBL12\"), IF((soundLevel($T190, $AB190, BD190, $Y190, $W190,$AJ190,$AA190,\"NC\"))<15,\"<15\",soundLevel($T190, $AB190, BD190, $Y190, $W190,$AJ190,$AA190,\"NC\")+0.4),IF((soundLevel($T190, $AB190, BD190, $Y190, $W190,$AJ190,$AA190,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T190, $AB190, BD190, $Y190, $W190,$AJ190,$AA190,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T190, $AB190, BD190, $Y190, $W190,$AJ190,$AA190,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T190=\"Select Model\",\"\",IF($T190=\"LIU24_2W\",calcQwIP($Y190,$W190,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC190,$AI190,\"latent\",$U190&\"P\"&IF($V190=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T190,activeElevation),\"\"))","v":""},{"$f":"IF($T190=\"Select Model\",\"\",IF($T190=\"ACBC_1W\",calcQwIP($Y190,$W190,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC190,BD190,\"capacity\",$U190&\"P\"&IF($V190=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T190,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y190,$W190,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC190,BD190,\"capacity\",$U190&\"P\"&IF($V190=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T190,activeElevation)))","v":""},"",{"$f":"IF(T190=\"Select Model\", 0,waterPressureDrop(W190, U190 & \"P\" & IF(V190=\"Dual\",2,1) &\"C\", AC190, \"cooling\", T190))","v":0},{"$f":"IF(T190=\"Select Model\", \"\",getReturnWaterTemp(T190,AC190, activeEWTCooling, AS190, \"cooling\"))","v":""},"",{"$f":"IF($T190<>\"ACBC_1W\",\"\",IF($J190=\"\",\"\",FintubeCapacity($T190,$W190,$AE190,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T190=\"Select Model\",T190=\"PCBL\"),\"\",calcQwIP(Y190,W190,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD190,BD190,\"capacity\",U190&\"P\"&IF(V190=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T190,activeElevation))","v":""},"",{"$f":"IF(OR(T190=\"Select Model\",T190=\"PCBL\"), \"\",IF(AY190=0,\"N/A\",waterPressureDrop(W190, U190 & \"P\" & IF(V190=\"Dual\",2,1) &\"C\", AD190, \"heating\", T190)))","v":""},{"$f":"IF(OR(T190=\"Select Model\",T190=\"PCBL\"), \"\",IF(AY190=0,getReturnWaterTemp(T190,AE190, activeEWTHeating, AX190, \"heating\"),getReturnWaterTemp(T190,AD190, activeEWTHeating, AY190, \"heating\")))","v":""},"",{"$f":" getNozzle(T190, W190, Y190, Z190, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I191)),I191<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I191, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H191)),H191<0),\"\",intlEstQuantity(T191, W191*12, H191)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T191=\"Select Model\",\"\",coilCircuitChange(W191, U191, AC191, T191,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T191=\"Select Model\",\"\",beamWidth(T191))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T191=\"Select Model\",T191=\"PCBL\"), 0,getSPIP(T191, W191, Y191, BD191, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T191=\"Select Model\", \"\",IF(T191=\"PCBL\",0,primaryAirSensibleCapacityIP($T191,$W191,activeRoomTempCooling,activePriAirTempCooling,$Y191,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T191=\"Select Model\",\"\",IF($T191=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y191,activeElevation)))","v":""},{"$f":"IF(OR(T191=\"Select Model\",T191=\"PCBL\"), 0,IF(AD191=0,0,-primaryAirSensibleCapacityIP($T191,$W191,activeRoomTempHeating,activePriAirTempHeating,$Y191,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T191=\"Select Model\", \"\", InductionRatio($T191,BD191,$W191,$Y191)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T191=\"Select Model\", \"\",IF($T191=\"PCBL\",\"N/A\",minVAVSetBack(AA191, Y191))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T191=\"Select Model\", \"\",IF($T191= \"PCBL\",\"N/A\",getDischargeAirTemp($T191,$V191,$AC191,$W191,BD191,$AL191, $Y191, $AS191, \"cooling\",activeElevation,$AB191,$AJ191,$AV191,$BB191))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T191=\"Select Model\",$T191=\"PCBL\"), \"\",getDischargeAirTemp($T191,$V191,$AD191,$W191,BD191,$AL191, $Y191, $AY191, \"heating\",activeElevation,$AB191,$AJ191,$AV191,$BB191)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T191=\"Select Model\", \"\",IF(OR($T191=\"ACBC_1W\",$T191=\"ACBC_2W\",LEFT($T191,4)=\"ACBR\",$T191 = \"LIU24_2W\",LEFT($T191,3)=\"RIU\",LEFT($T191,6)=\"ACBL12\"), IF((soundLevel($T191, $AB191, BD191, $Y191, $W191,$AJ191,$AA191,\"dba\"))<15,\"<15\",soundLevel($T191, $AB191, BD191, $Y191, $W191,$AJ191,$AA191,\"dba\")+0.4),IF((soundLevel($T191, $AB191, BD191, $Y191, $W191,$AJ191,$AA191,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T191, $AB191, BD191, $Y191, $W191,$AJ191,$AA191,\"dba\")+5)<15, \"<15\", soundLevel($T191, $AB191, BD191,$Y191, $W191,$AJ191,$AA191,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T191=\"Select Model\", \"\",IF(OR($T191=\"ACBC_1W\",$T191=\"ACBC_2W\",LEFT($T191,4)=\"ACBR\",$T191=\"LIU24_2W\",LEFT($T191,3)=\"RIU\",LEFT($T191,6)=\"ACBL12\"), IF((soundLevel($T191, $AB191, BD191, $Y191, $W191,$AJ191,$AA191,\"NC\"))<15,\"<15\",soundLevel($T191, $AB191, BD191, $Y191, $W191,$AJ191,$AA191,\"NC\")+0.4),IF((soundLevel($T191, $AB191, BD191, $Y191, $W191,$AJ191,$AA191,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T191, $AB191, BD191, $Y191, $W191,$AJ191,$AA191,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T191, $AB191, BD191, $Y191, $W191,$AJ191,$AA191,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T191=\"Select Model\",\"\",IF($T191=\"LIU24_2W\",calcQwIP($Y191,$W191,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC191,$AI191,\"latent\",$U191&\"P\"&IF($V191=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T191,activeElevation),\"\"))","v":""},{"$f":"IF($T191=\"Select Model\",\"\",IF($T191=\"ACBC_1W\",calcQwIP($Y191,$W191,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC191,BD191,\"capacity\",$U191&\"P\"&IF($V191=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T191,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y191,$W191,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC191,BD191,\"capacity\",$U191&\"P\"&IF($V191=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T191,activeElevation)))","v":""},"",{"$f":"IF(T191=\"Select Model\", 0,waterPressureDrop(W191, U191 & \"P\" & IF(V191=\"Dual\",2,1) &\"C\", AC191, \"cooling\", T191))","v":0},{"$f":"IF(T191=\"Select Model\", \"\",getReturnWaterTemp(T191,AC191, activeEWTCooling, AS191, \"cooling\"))","v":""},"",{"$f":"IF($T191<>\"ACBC_1W\",\"\",IF($J191=\"\",\"\",FintubeCapacity($T191,$W191,$AE191,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T191=\"Select Model\",T191=\"PCBL\"),\"\",calcQwIP(Y191,W191,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD191,BD191,\"capacity\",U191&\"P\"&IF(V191=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T191,activeElevation))","v":""},"",{"$f":"IF(OR(T191=\"Select Model\",T191=\"PCBL\"), \"\",IF(AY191=0,\"N/A\",waterPressureDrop(W191, U191 & \"P\" & IF(V191=\"Dual\",2,1) &\"C\", AD191, \"heating\", T191)))","v":""},{"$f":"IF(OR(T191=\"Select Model\",T191=\"PCBL\"), \"\",IF(AY191=0,getReturnWaterTemp(T191,AE191, activeEWTHeating, AX191, \"heating\"),getReturnWaterTemp(T191,AD191, activeEWTHeating, AY191, \"heating\")))","v":""},"",{"$f":" getNozzle(T191, W191, Y191, Z191, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I192)),I192<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I192, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H192)),H192<0),\"\",intlEstQuantity(T192, W192*12, H192)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T192=\"Select Model\",\"\",coilCircuitChange(W192, U192, AC192, T192,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T192=\"Select Model\",\"\",beamWidth(T192))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T192=\"Select Model\",T192=\"PCBL\"), 0,getSPIP(T192, W192, Y192, BD192, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T192=\"Select Model\", \"\",IF(T192=\"PCBL\",0,primaryAirSensibleCapacityIP($T192,$W192,activeRoomTempCooling,activePriAirTempCooling,$Y192,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T192=\"Select Model\",\"\",IF($T192=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y192,activeElevation)))","v":""},{"$f":"IF(OR(T192=\"Select Model\",T192=\"PCBL\"), 0,IF(AD192=0,0,-primaryAirSensibleCapacityIP($T192,$W192,activeRoomTempHeating,activePriAirTempHeating,$Y192,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T192=\"Select Model\", \"\", InductionRatio($T192,BD192,$W192,$Y192)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T192=\"Select Model\", \"\",IF($T192=\"PCBL\",\"N/A\",minVAVSetBack(AA192, Y192))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T192=\"Select Model\", \"\",IF($T192= \"PCBL\",\"N/A\",getDischargeAirTemp($T192,$V192,$AC192,$W192,BD192,$AL192, $Y192, $AS192, \"cooling\",activeElevation,$AB192,$AJ192,$AV192,$BB192))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T192=\"Select Model\",$T192=\"PCBL\"), \"\",getDischargeAirTemp($T192,$V192,$AD192,$W192,BD192,$AL192, $Y192, $AY192, \"heating\",activeElevation,$AB192,$AJ192,$AV192,$BB192)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T192=\"Select Model\", \"\",IF(OR($T192=\"ACBC_1W\",$T192=\"ACBC_2W\",LEFT($T192,4)=\"ACBR\",$T192 = \"LIU24_2W\",LEFT($T192,3)=\"RIU\",LEFT($T192,6)=\"ACBL12\"), IF((soundLevel($T192, $AB192, BD192, $Y192, $W192,$AJ192,$AA192,\"dba\"))<15,\"<15\",soundLevel($T192, $AB192, BD192, $Y192, $W192,$AJ192,$AA192,\"dba\")+0.4),IF((soundLevel($T192, $AB192, BD192, $Y192, $W192,$AJ192,$AA192,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T192, $AB192, BD192, $Y192, $W192,$AJ192,$AA192,\"dba\")+5)<15, \"<15\", soundLevel($T192, $AB192, BD192,$Y192, $W192,$AJ192,$AA192,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T192=\"Select Model\", \"\",IF(OR($T192=\"ACBC_1W\",$T192=\"ACBC_2W\",LEFT($T192,4)=\"ACBR\",$T192=\"LIU24_2W\",LEFT($T192,3)=\"RIU\",LEFT($T192,6)=\"ACBL12\"), IF((soundLevel($T192, $AB192, BD192, $Y192, $W192,$AJ192,$AA192,\"NC\"))<15,\"<15\",soundLevel($T192, $AB192, BD192, $Y192, $W192,$AJ192,$AA192,\"NC\")+0.4),IF((soundLevel($T192, $AB192, BD192, $Y192, $W192,$AJ192,$AA192,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T192, $AB192, BD192, $Y192, $W192,$AJ192,$AA192,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T192, $AB192, BD192, $Y192, $W192,$AJ192,$AA192,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T192=\"Select Model\",\"\",IF($T192=\"LIU24_2W\",calcQwIP($Y192,$W192,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC192,$AI192,\"latent\",$U192&\"P\"&IF($V192=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T192,activeElevation),\"\"))","v":""},{"$f":"IF($T192=\"Select Model\",\"\",IF($T192=\"ACBC_1W\",calcQwIP($Y192,$W192,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC192,BD192,\"capacity\",$U192&\"P\"&IF($V192=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T192,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y192,$W192,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC192,BD192,\"capacity\",$U192&\"P\"&IF($V192=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T192,activeElevation)))","v":""},"",{"$f":"IF(T192=\"Select Model\", 0,waterPressureDrop(W192, U192 & \"P\" & IF(V192=\"Dual\",2,1) &\"C\", AC192, \"cooling\", T192))","v":0},{"$f":"IF(T192=\"Select Model\", \"\",getReturnWaterTemp(T192,AC192, activeEWTCooling, AS192, \"cooling\"))","v":""},"",{"$f":"IF($T192<>\"ACBC_1W\",\"\",IF($J192=\"\",\"\",FintubeCapacity($T192,$W192,$AE192,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T192=\"Select Model\",T192=\"PCBL\"),\"\",calcQwIP(Y192,W192,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD192,BD192,\"capacity\",U192&\"P\"&IF(V192=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T192,activeElevation))","v":""},"",{"$f":"IF(OR(T192=\"Select Model\",T192=\"PCBL\"), \"\",IF(AY192=0,\"N/A\",waterPressureDrop(W192, U192 & \"P\" & IF(V192=\"Dual\",2,1) &\"C\", AD192, \"heating\", T192)))","v":""},{"$f":"IF(OR(T192=\"Select Model\",T192=\"PCBL\"), \"\",IF(AY192=0,getReturnWaterTemp(T192,AE192, activeEWTHeating, AX192, \"heating\"),getReturnWaterTemp(T192,AD192, activeEWTHeating, AY192, \"heating\")))","v":""},"",{"$f":" getNozzle(T192, W192, Y192, Z192, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I193)),I193<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I193, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H193)),H193<0),\"\",intlEstQuantity(T193, W193*12, H193)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T193=\"Select Model\",\"\",coilCircuitChange(W193, U193, AC193, T193,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T193=\"Select Model\",\"\",beamWidth(T193))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T193=\"Select Model\",T193=\"PCBL\"), 0,getSPIP(T193, W193, Y193, BD193, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T193=\"Select Model\", \"\",IF(T193=\"PCBL\",0,primaryAirSensibleCapacityIP($T193,$W193,activeRoomTempCooling,activePriAirTempCooling,$Y193,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T193=\"Select Model\",\"\",IF($T193=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y193,activeElevation)))","v":""},{"$f":"IF(OR(T193=\"Select Model\",T193=\"PCBL\"), 0,IF(AD193=0,0,-primaryAirSensibleCapacityIP($T193,$W193,activeRoomTempHeating,activePriAirTempHeating,$Y193,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T193=\"Select Model\", \"\", InductionRatio($T193,BD193,$W193,$Y193)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T193=\"Select Model\", \"\",IF($T193=\"PCBL\",\"N/A\",minVAVSetBack(AA193, Y193))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T193=\"Select Model\", \"\",IF($T193= \"PCBL\",\"N/A\",getDischargeAirTemp($T193,$V193,$AC193,$W193,BD193,$AL193, $Y193, $AS193, \"cooling\",activeElevation,$AB193,$AJ193,$AV193,$BB193))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T193=\"Select Model\",$T193=\"PCBL\"), \"\",getDischargeAirTemp($T193,$V193,$AD193,$W193,BD193,$AL193, $Y193, $AY193, \"heating\",activeElevation,$AB193,$AJ193,$AV193,$BB193)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T193=\"Select Model\", \"\",IF(OR($T193=\"ACBC_1W\",$T193=\"ACBC_2W\",LEFT($T193,4)=\"ACBR\",$T193 = \"LIU24_2W\",LEFT($T193,3)=\"RIU\",LEFT($T193,6)=\"ACBL12\"), IF((soundLevel($T193, $AB193, BD193, $Y193, $W193,$AJ193,$AA193,\"dba\"))<15,\"<15\",soundLevel($T193, $AB193, BD193, $Y193, $W193,$AJ193,$AA193,\"dba\")+0.4),IF((soundLevel($T193, $AB193, BD193, $Y193, $W193,$AJ193,$AA193,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T193, $AB193, BD193, $Y193, $W193,$AJ193,$AA193,\"dba\")+5)<15, \"<15\", soundLevel($T193, $AB193, BD193,$Y193, $W193,$AJ193,$AA193,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T193=\"Select Model\", \"\",IF(OR($T193=\"ACBC_1W\",$T193=\"ACBC_2W\",LEFT($T193,4)=\"ACBR\",$T193=\"LIU24_2W\",LEFT($T193,3)=\"RIU\",LEFT($T193,6)=\"ACBL12\"), IF((soundLevel($T193, $AB193, BD193, $Y193, $W193,$AJ193,$AA193,\"NC\"))<15,\"<15\",soundLevel($T193, $AB193, BD193, $Y193, $W193,$AJ193,$AA193,\"NC\")+0.4),IF((soundLevel($T193, $AB193, BD193, $Y193, $W193,$AJ193,$AA193,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T193, $AB193, BD193, $Y193, $W193,$AJ193,$AA193,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T193, $AB193, BD193, $Y193, $W193,$AJ193,$AA193,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T193=\"Select Model\",\"\",IF($T193=\"LIU24_2W\",calcQwIP($Y193,$W193,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC193,$AI193,\"latent\",$U193&\"P\"&IF($V193=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T193,activeElevation),\"\"))","v":""},{"$f":"IF($T193=\"Select Model\",\"\",IF($T193=\"ACBC_1W\",calcQwIP($Y193,$W193,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC193,BD193,\"capacity\",$U193&\"P\"&IF($V193=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T193,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y193,$W193,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC193,BD193,\"capacity\",$U193&\"P\"&IF($V193=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T193,activeElevation)))","v":""},"",{"$f":"IF(T193=\"Select Model\", 0,waterPressureDrop(W193, U193 & \"P\" & IF(V193=\"Dual\",2,1) &\"C\", AC193, \"cooling\", T193))","v":0},{"$f":"IF(T193=\"Select Model\", \"\",getReturnWaterTemp(T193,AC193, activeEWTCooling, AS193, \"cooling\"))","v":""},"",{"$f":"IF($T193<>\"ACBC_1W\",\"\",IF($J193=\"\",\"\",FintubeCapacity($T193,$W193,$AE193,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T193=\"Select Model\",T193=\"PCBL\"),\"\",calcQwIP(Y193,W193,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD193,BD193,\"capacity\",U193&\"P\"&IF(V193=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T193,activeElevation))","v":""},"",{"$f":"IF(OR(T193=\"Select Model\",T193=\"PCBL\"), \"\",IF(AY193=0,\"N/A\",waterPressureDrop(W193, U193 & \"P\" & IF(V193=\"Dual\",2,1) &\"C\", AD193, \"heating\", T193)))","v":""},{"$f":"IF(OR(T193=\"Select Model\",T193=\"PCBL\"), \"\",IF(AY193=0,getReturnWaterTemp(T193,AE193, activeEWTHeating, AX193, \"heating\"),getReturnWaterTemp(T193,AD193, activeEWTHeating, AY193, \"heating\")))","v":""},"",{"$f":" getNozzle(T193, W193, Y193, Z193, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I194)),I194<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I194, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H194)),H194<0),\"\",intlEstQuantity(T194, W194*12, H194)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T194=\"Select Model\",\"\",coilCircuitChange(W194, U194, AC194, T194,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T194=\"Select Model\",\"\",beamWidth(T194))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T194=\"Select Model\",T194=\"PCBL\"), 0,getSPIP(T194, W194, Y194, BD194, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T194=\"Select Model\", \"\",IF(T194=\"PCBL\",0,primaryAirSensibleCapacityIP($T194,$W194,activeRoomTempCooling,activePriAirTempCooling,$Y194,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T194=\"Select Model\",\"\",IF($T194=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y194,activeElevation)))","v":""},{"$f":"IF(OR(T194=\"Select Model\",T194=\"PCBL\"), 0,IF(AD194=0,0,-primaryAirSensibleCapacityIP($T194,$W194,activeRoomTempHeating,activePriAirTempHeating,$Y194,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T194=\"Select Model\", \"\", InductionRatio($T194,BD194,$W194,$Y194)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T194=\"Select Model\", \"\",IF($T194=\"PCBL\",\"N/A\",minVAVSetBack(AA194, Y194))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T194=\"Select Model\", \"\",IF($T194= \"PCBL\",\"N/A\",getDischargeAirTemp($T194,$V194,$AC194,$W194,BD194,$AL194, $Y194, $AS194, \"cooling\",activeElevation,$AB194,$AJ194,$AV194,$BB194))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T194=\"Select Model\",$T194=\"PCBL\"), \"\",getDischargeAirTemp($T194,$V194,$AD194,$W194,BD194,$AL194, $Y194, $AY194, \"heating\",activeElevation,$AB194,$AJ194,$AV194,$BB194)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T194=\"Select Model\", \"\",IF(OR($T194=\"ACBC_1W\",$T194=\"ACBC_2W\",LEFT($T194,4)=\"ACBR\",$T194 = \"LIU24_2W\",LEFT($T194,3)=\"RIU\",LEFT($T194,6)=\"ACBL12\"), IF((soundLevel($T194, $AB194, BD194, $Y194, $W194,$AJ194,$AA194,\"dba\"))<15,\"<15\",soundLevel($T194, $AB194, BD194, $Y194, $W194,$AJ194,$AA194,\"dba\")+0.4),IF((soundLevel($T194, $AB194, BD194, $Y194, $W194,$AJ194,$AA194,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T194, $AB194, BD194, $Y194, $W194,$AJ194,$AA194,\"dba\")+5)<15, \"<15\", soundLevel($T194, $AB194, BD194,$Y194, $W194,$AJ194,$AA194,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T194=\"Select Model\", \"\",IF(OR($T194=\"ACBC_1W\",$T194=\"ACBC_2W\",LEFT($T194,4)=\"ACBR\",$T194=\"LIU24_2W\",LEFT($T194,3)=\"RIU\",LEFT($T194,6)=\"ACBL12\"), IF((soundLevel($T194, $AB194, BD194, $Y194, $W194,$AJ194,$AA194,\"NC\"))<15,\"<15\",soundLevel($T194, $AB194, BD194, $Y194, $W194,$AJ194,$AA194,\"NC\")+0.4),IF((soundLevel($T194, $AB194, BD194, $Y194, $W194,$AJ194,$AA194,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T194, $AB194, BD194, $Y194, $W194,$AJ194,$AA194,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T194, $AB194, BD194, $Y194, $W194,$AJ194,$AA194,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T194=\"Select Model\",\"\",IF($T194=\"LIU24_2W\",calcQwIP($Y194,$W194,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC194,$AI194,\"latent\",$U194&\"P\"&IF($V194=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T194,activeElevation),\"\"))","v":""},{"$f":"IF($T194=\"Select Model\",\"\",IF($T194=\"ACBC_1W\",calcQwIP($Y194,$W194,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC194,BD194,\"capacity\",$U194&\"P\"&IF($V194=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T194,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y194,$W194,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC194,BD194,\"capacity\",$U194&\"P\"&IF($V194=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T194,activeElevation)))","v":""},"",{"$f":"IF(T194=\"Select Model\", 0,waterPressureDrop(W194, U194 & \"P\" & IF(V194=\"Dual\",2,1) &\"C\", AC194, \"cooling\", T194))","v":0},{"$f":"IF(T194=\"Select Model\", \"\",getReturnWaterTemp(T194,AC194, activeEWTCooling, AS194, \"cooling\"))","v":""},"",{"$f":"IF($T194<>\"ACBC_1W\",\"\",IF($J194=\"\",\"\",FintubeCapacity($T194,$W194,$AE194,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T194=\"Select Model\",T194=\"PCBL\"),\"\",calcQwIP(Y194,W194,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD194,BD194,\"capacity\",U194&\"P\"&IF(V194=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T194,activeElevation))","v":""},"",{"$f":"IF(OR(T194=\"Select Model\",T194=\"PCBL\"), \"\",IF(AY194=0,\"N/A\",waterPressureDrop(W194, U194 & \"P\" & IF(V194=\"Dual\",2,1) &\"C\", AD194, \"heating\", T194)))","v":""},{"$f":"IF(OR(T194=\"Select Model\",T194=\"PCBL\"), \"\",IF(AY194=0,getReturnWaterTemp(T194,AE194, activeEWTHeating, AX194, \"heating\"),getReturnWaterTemp(T194,AD194, activeEWTHeating, AY194, \"heating\")))","v":""},"",{"$f":" getNozzle(T194, W194, Y194, Z194, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I195)),I195<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I195, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H195)),H195<0),\"\",intlEstQuantity(T195, W195*12, H195)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T195=\"Select Model\",\"\",coilCircuitChange(W195, U195, AC195, T195,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T195=\"Select Model\",\"\",beamWidth(T195))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T195=\"Select Model\",T195=\"PCBL\"), 0,getSPIP(T195, W195, Y195, BD195, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T195=\"Select Model\", \"\",IF(T195=\"PCBL\",0,primaryAirSensibleCapacityIP($T195,$W195,activeRoomTempCooling,activePriAirTempCooling,$Y195,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T195=\"Select Model\",\"\",IF($T195=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y195,activeElevation)))","v":""},{"$f":"IF(OR(T195=\"Select Model\",T195=\"PCBL\"), 0,IF(AD195=0,0,-primaryAirSensibleCapacityIP($T195,$W195,activeRoomTempHeating,activePriAirTempHeating,$Y195,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T195=\"Select Model\", \"\", InductionRatio($T195,BD195,$W195,$Y195)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T195=\"Select Model\", \"\",IF($T195=\"PCBL\",\"N/A\",minVAVSetBack(AA195, Y195))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T195=\"Select Model\", \"\",IF($T195= \"PCBL\",\"N/A\",getDischargeAirTemp($T195,$V195,$AC195,$W195,BD195,$AL195, $Y195, $AS195, \"cooling\",activeElevation,$AB195,$AJ195,$AV195,$BB195))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T195=\"Select Model\",$T195=\"PCBL\"), \"\",getDischargeAirTemp($T195,$V195,$AD195,$W195,BD195,$AL195, $Y195, $AY195, \"heating\",activeElevation,$AB195,$AJ195,$AV195,$BB195)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T195=\"Select Model\", \"\",IF(OR($T195=\"ACBC_1W\",$T195=\"ACBC_2W\",LEFT($T195,4)=\"ACBR\",$T195 = \"LIU24_2W\",LEFT($T195,3)=\"RIU\",LEFT($T195,6)=\"ACBL12\"), IF((soundLevel($T195, $AB195, BD195, $Y195, $W195,$AJ195,$AA195,\"dba\"))<15,\"<15\",soundLevel($T195, $AB195, BD195, $Y195, $W195,$AJ195,$AA195,\"dba\")+0.4),IF((soundLevel($T195, $AB195, BD195, $Y195, $W195,$AJ195,$AA195,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T195, $AB195, BD195, $Y195, $W195,$AJ195,$AA195,\"dba\")+5)<15, \"<15\", soundLevel($T195, $AB195, BD195,$Y195, $W195,$AJ195,$AA195,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T195=\"Select Model\", \"\",IF(OR($T195=\"ACBC_1W\",$T195=\"ACBC_2W\",LEFT($T195,4)=\"ACBR\",$T195=\"LIU24_2W\",LEFT($T195,3)=\"RIU\",LEFT($T195,6)=\"ACBL12\"), IF((soundLevel($T195, $AB195, BD195, $Y195, $W195,$AJ195,$AA195,\"NC\"))<15,\"<15\",soundLevel($T195, $AB195, BD195, $Y195, $W195,$AJ195,$AA195,\"NC\")+0.4),IF((soundLevel($T195, $AB195, BD195, $Y195, $W195,$AJ195,$AA195,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T195, $AB195, BD195, $Y195, $W195,$AJ195,$AA195,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T195, $AB195, BD195, $Y195, $W195,$AJ195,$AA195,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T195=\"Select Model\",\"\",IF($T195=\"LIU24_2W\",calcQwIP($Y195,$W195,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC195,$AI195,\"latent\",$U195&\"P\"&IF($V195=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T195,activeElevation),\"\"))","v":""},{"$f":"IF($T195=\"Select Model\",\"\",IF($T195=\"ACBC_1W\",calcQwIP($Y195,$W195,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC195,BD195,\"capacity\",$U195&\"P\"&IF($V195=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T195,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y195,$W195,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC195,BD195,\"capacity\",$U195&\"P\"&IF($V195=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T195,activeElevation)))","v":""},"",{"$f":"IF(T195=\"Select Model\", 0,waterPressureDrop(W195, U195 & \"P\" & IF(V195=\"Dual\",2,1) &\"C\", AC195, \"cooling\", T195))","v":0},{"$f":"IF(T195=\"Select Model\", \"\",getReturnWaterTemp(T195,AC195, activeEWTCooling, AS195, \"cooling\"))","v":""},"",{"$f":"IF($T195<>\"ACBC_1W\",\"\",IF($J195=\"\",\"\",FintubeCapacity($T195,$W195,$AE195,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T195=\"Select Model\",T195=\"PCBL\"),\"\",calcQwIP(Y195,W195,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD195,BD195,\"capacity\",U195&\"P\"&IF(V195=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T195,activeElevation))","v":""},"",{"$f":"IF(OR(T195=\"Select Model\",T195=\"PCBL\"), \"\",IF(AY195=0,\"N/A\",waterPressureDrop(W195, U195 & \"P\" & IF(V195=\"Dual\",2,1) &\"C\", AD195, \"heating\", T195)))","v":""},{"$f":"IF(OR(T195=\"Select Model\",T195=\"PCBL\"), \"\",IF(AY195=0,getReturnWaterTemp(T195,AE195, activeEWTHeating, AX195, \"heating\"),getReturnWaterTemp(T195,AD195, activeEWTHeating, AY195, \"heating\")))","v":""},"",{"$f":" getNozzle(T195, W195, Y195, Z195, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I196)),I196<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I196, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H196)),H196<0),\"\",intlEstQuantity(T196, W196*12, H196)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T196=\"Select Model\",\"\",coilCircuitChange(W196, U196, AC196, T196,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T196=\"Select Model\",\"\",beamWidth(T196))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T196=\"Select Model\",T196=\"PCBL\"), 0,getSPIP(T196, W196, Y196, BD196, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T196=\"Select Model\", \"\",IF(T196=\"PCBL\",0,primaryAirSensibleCapacityIP($T196,$W196,activeRoomTempCooling,activePriAirTempCooling,$Y196,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T196=\"Select Model\",\"\",IF($T196=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y196,activeElevation)))","v":""},{"$f":"IF(OR(T196=\"Select Model\",T196=\"PCBL\"), 0,IF(AD196=0,0,-primaryAirSensibleCapacityIP($T196,$W196,activeRoomTempHeating,activePriAirTempHeating,$Y196,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T196=\"Select Model\", \"\", InductionRatio($T196,BD196,$W196,$Y196)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T196=\"Select Model\", \"\",IF($T196=\"PCBL\",\"N/A\",minVAVSetBack(AA196, Y196))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T196=\"Select Model\", \"\",IF($T196= \"PCBL\",\"N/A\",getDischargeAirTemp($T196,$V196,$AC196,$W196,BD196,$AL196, $Y196, $AS196, \"cooling\",activeElevation,$AB196,$AJ196,$AV196,$BB196))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T196=\"Select Model\",$T196=\"PCBL\"), \"\",getDischargeAirTemp($T196,$V196,$AD196,$W196,BD196,$AL196, $Y196, $AY196, \"heating\",activeElevation,$AB196,$AJ196,$AV196,$BB196)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T196=\"Select Model\", \"\",IF(OR($T196=\"ACBC_1W\",$T196=\"ACBC_2W\",LEFT($T196,4)=\"ACBR\",$T196 = \"LIU24_2W\",LEFT($T196,3)=\"RIU\",LEFT($T196,6)=\"ACBL12\"), IF((soundLevel($T196, $AB196, BD196, $Y196, $W196,$AJ196,$AA196,\"dba\"))<15,\"<15\",soundLevel($T196, $AB196, BD196, $Y196, $W196,$AJ196,$AA196,\"dba\")+0.4),IF((soundLevel($T196, $AB196, BD196, $Y196, $W196,$AJ196,$AA196,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T196, $AB196, BD196, $Y196, $W196,$AJ196,$AA196,\"dba\")+5)<15, \"<15\", soundLevel($T196, $AB196, BD196,$Y196, $W196,$AJ196,$AA196,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T196=\"Select Model\", \"\",IF(OR($T196=\"ACBC_1W\",$T196=\"ACBC_2W\",LEFT($T196,4)=\"ACBR\",$T196=\"LIU24_2W\",LEFT($T196,3)=\"RIU\",LEFT($T196,6)=\"ACBL12\"), IF((soundLevel($T196, $AB196, BD196, $Y196, $W196,$AJ196,$AA196,\"NC\"))<15,\"<15\",soundLevel($T196, $AB196, BD196, $Y196, $W196,$AJ196,$AA196,\"NC\")+0.4),IF((soundLevel($T196, $AB196, BD196, $Y196, $W196,$AJ196,$AA196,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T196, $AB196, BD196, $Y196, $W196,$AJ196,$AA196,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T196, $AB196, BD196, $Y196, $W196,$AJ196,$AA196,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T196=\"Select Model\",\"\",IF($T196=\"LIU24_2W\",calcQwIP($Y196,$W196,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC196,$AI196,\"latent\",$U196&\"P\"&IF($V196=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T196,activeElevation),\"\"))","v":""},{"$f":"IF($T196=\"Select Model\",\"\",IF($T196=\"ACBC_1W\",calcQwIP($Y196,$W196,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC196,BD196,\"capacity\",$U196&\"P\"&IF($V196=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T196,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y196,$W196,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC196,BD196,\"capacity\",$U196&\"P\"&IF($V196=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T196,activeElevation)))","v":""},"",{"$f":"IF(T196=\"Select Model\", 0,waterPressureDrop(W196, U196 & \"P\" & IF(V196=\"Dual\",2,1) &\"C\", AC196, \"cooling\", T196))","v":0},{"$f":"IF(T196=\"Select Model\", \"\",getReturnWaterTemp(T196,AC196, activeEWTCooling, AS196, \"cooling\"))","v":""},"",{"$f":"IF($T196<>\"ACBC_1W\",\"\",IF($J196=\"\",\"\",FintubeCapacity($T196,$W196,$AE196,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T196=\"Select Model\",T196=\"PCBL\"),\"\",calcQwIP(Y196,W196,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD196,BD196,\"capacity\",U196&\"P\"&IF(V196=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T196,activeElevation))","v":""},"",{"$f":"IF(OR(T196=\"Select Model\",T196=\"PCBL\"), \"\",IF(AY196=0,\"N/A\",waterPressureDrop(W196, U196 & \"P\" & IF(V196=\"Dual\",2,1) &\"C\", AD196, \"heating\", T196)))","v":""},{"$f":"IF(OR(T196=\"Select Model\",T196=\"PCBL\"), \"\",IF(AY196=0,getReturnWaterTemp(T196,AE196, activeEWTHeating, AX196, \"heating\"),getReturnWaterTemp(T196,AD196, activeEWTHeating, AY196, \"heating\")))","v":""},"",{"$f":" getNozzle(T196, W196, Y196, Z196, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I197)),I197<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I197, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H197)),H197<0),\"\",intlEstQuantity(T197, W197*12, H197)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T197=\"Select Model\",\"\",coilCircuitChange(W197, U197, AC197, T197,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T197=\"Select Model\",\"\",beamWidth(T197))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T197=\"Select Model\",T197=\"PCBL\"), 0,getSPIP(T197, W197, Y197, BD197, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T197=\"Select Model\", \"\",IF(T197=\"PCBL\",0,primaryAirSensibleCapacityIP($T197,$W197,activeRoomTempCooling,activePriAirTempCooling,$Y197,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T197=\"Select Model\",\"\",IF($T197=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y197,activeElevation)))","v":""},{"$f":"IF(OR(T197=\"Select Model\",T197=\"PCBL\"), 0,IF(AD197=0,0,-primaryAirSensibleCapacityIP($T197,$W197,activeRoomTempHeating,activePriAirTempHeating,$Y197,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T197=\"Select Model\", \"\", InductionRatio($T197,BD197,$W197,$Y197)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T197=\"Select Model\", \"\",IF($T197=\"PCBL\",\"N/A\",minVAVSetBack(AA197, Y197))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T197=\"Select Model\", \"\",IF($T197= \"PCBL\",\"N/A\",getDischargeAirTemp($T197,$V197,$AC197,$W197,BD197,$AL197, $Y197, $AS197, \"cooling\",activeElevation,$AB197,$AJ197,$AV197,$BB197))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T197=\"Select Model\",$T197=\"PCBL\"), \"\",getDischargeAirTemp($T197,$V197,$AD197,$W197,BD197,$AL197, $Y197, $AY197, \"heating\",activeElevation,$AB197,$AJ197,$AV197,$BB197)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T197=\"Select Model\", \"\",IF(OR($T197=\"ACBC_1W\",$T197=\"ACBC_2W\",LEFT($T197,4)=\"ACBR\",$T197 = \"LIU24_2W\",LEFT($T197,3)=\"RIU\",LEFT($T197,6)=\"ACBL12\"), IF((soundLevel($T197, $AB197, BD197, $Y197, $W197,$AJ197,$AA197,\"dba\"))<15,\"<15\",soundLevel($T197, $AB197, BD197, $Y197, $W197,$AJ197,$AA197,\"dba\")+0.4),IF((soundLevel($T197, $AB197, BD197, $Y197, $W197,$AJ197,$AA197,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T197, $AB197, BD197, $Y197, $W197,$AJ197,$AA197,\"dba\")+5)<15, \"<15\", soundLevel($T197, $AB197, BD197,$Y197, $W197,$AJ197,$AA197,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T197=\"Select Model\", \"\",IF(OR($T197=\"ACBC_1W\",$T197=\"ACBC_2W\",LEFT($T197,4)=\"ACBR\",$T197=\"LIU24_2W\",LEFT($T197,3)=\"RIU\",LEFT($T197,6)=\"ACBL12\"), IF((soundLevel($T197, $AB197, BD197, $Y197, $W197,$AJ197,$AA197,\"NC\"))<15,\"<15\",soundLevel($T197, $AB197, BD197, $Y197, $W197,$AJ197,$AA197,\"NC\")+0.4),IF((soundLevel($T197, $AB197, BD197, $Y197, $W197,$AJ197,$AA197,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T197, $AB197, BD197, $Y197, $W197,$AJ197,$AA197,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T197, $AB197, BD197, $Y197, $W197,$AJ197,$AA197,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T197=\"Select Model\",\"\",IF($T197=\"LIU24_2W\",calcQwIP($Y197,$W197,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC197,$AI197,\"latent\",$U197&\"P\"&IF($V197=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T197,activeElevation),\"\"))","v":""},{"$f":"IF($T197=\"Select Model\",\"\",IF($T197=\"ACBC_1W\",calcQwIP($Y197,$W197,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC197,BD197,\"capacity\",$U197&\"P\"&IF($V197=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T197,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y197,$W197,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC197,BD197,\"capacity\",$U197&\"P\"&IF($V197=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T197,activeElevation)))","v":""},"",{"$f":"IF(T197=\"Select Model\", 0,waterPressureDrop(W197, U197 & \"P\" & IF(V197=\"Dual\",2,1) &\"C\", AC197, \"cooling\", T197))","v":0},{"$f":"IF(T197=\"Select Model\", \"\",getReturnWaterTemp(T197,AC197, activeEWTCooling, AS197, \"cooling\"))","v":""},"",{"$f":"IF($T197<>\"ACBC_1W\",\"\",IF($J197=\"\",\"\",FintubeCapacity($T197,$W197,$AE197,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T197=\"Select Model\",T197=\"PCBL\"),\"\",calcQwIP(Y197,W197,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD197,BD197,\"capacity\",U197&\"P\"&IF(V197=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T197,activeElevation))","v":""},"",{"$f":"IF(OR(T197=\"Select Model\",T197=\"PCBL\"), \"\",IF(AY197=0,\"N/A\",waterPressureDrop(W197, U197 & \"P\" & IF(V197=\"Dual\",2,1) &\"C\", AD197, \"heating\", T197)))","v":""},{"$f":"IF(OR(T197=\"Select Model\",T197=\"PCBL\"), \"\",IF(AY197=0,getReturnWaterTemp(T197,AE197, activeEWTHeating, AX197, \"heating\"),getReturnWaterTemp(T197,AD197, activeEWTHeating, AY197, \"heating\")))","v":""},"",{"$f":" getNozzle(T197, W197, Y197, Z197, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I198)),I198<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I198, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H198)),H198<0),\"\",intlEstQuantity(T198, W198*12, H198)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T198=\"Select Model\",\"\",coilCircuitChange(W198, U198, AC198, T198,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T198=\"Select Model\",\"\",beamWidth(T198))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T198=\"Select Model\",T198=\"PCBL\"), 0,getSPIP(T198, W198, Y198, BD198, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T198=\"Select Model\", \"\",IF(T198=\"PCBL\",0,primaryAirSensibleCapacityIP($T198,$W198,activeRoomTempCooling,activePriAirTempCooling,$Y198,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T198=\"Select Model\",\"\",IF($T198=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y198,activeElevation)))","v":""},{"$f":"IF(OR(T198=\"Select Model\",T198=\"PCBL\"), 0,IF(AD198=0,0,-primaryAirSensibleCapacityIP($T198,$W198,activeRoomTempHeating,activePriAirTempHeating,$Y198,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T198=\"Select Model\", \"\", InductionRatio($T198,BD198,$W198,$Y198)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T198=\"Select Model\", \"\",IF($T198=\"PCBL\",\"N/A\",minVAVSetBack(AA198, Y198))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T198=\"Select Model\", \"\",IF($T198= \"PCBL\",\"N/A\",getDischargeAirTemp($T198,$V198,$AC198,$W198,BD198,$AL198, $Y198, $AS198, \"cooling\",activeElevation,$AB198,$AJ198,$AV198,$BB198))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T198=\"Select Model\",$T198=\"PCBL\"), \"\",getDischargeAirTemp($T198,$V198,$AD198,$W198,BD198,$AL198, $Y198, $AY198, \"heating\",activeElevation,$AB198,$AJ198,$AV198,$BB198)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T198=\"Select Model\", \"\",IF(OR($T198=\"ACBC_1W\",$T198=\"ACBC_2W\",LEFT($T198,4)=\"ACBR\",$T198 = \"LIU24_2W\",LEFT($T198,3)=\"RIU\",LEFT($T198,6)=\"ACBL12\"), IF((soundLevel($T198, $AB198, BD198, $Y198, $W198,$AJ198,$AA198,\"dba\"))<15,\"<15\",soundLevel($T198, $AB198, BD198, $Y198, $W198,$AJ198,$AA198,\"dba\")+0.4),IF((soundLevel($T198, $AB198, BD198, $Y198, $W198,$AJ198,$AA198,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T198, $AB198, BD198, $Y198, $W198,$AJ198,$AA198,\"dba\")+5)<15, \"<15\", soundLevel($T198, $AB198, BD198,$Y198, $W198,$AJ198,$AA198,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T198=\"Select Model\", \"\",IF(OR($T198=\"ACBC_1W\",$T198=\"ACBC_2W\",LEFT($T198,4)=\"ACBR\",$T198=\"LIU24_2W\",LEFT($T198,3)=\"RIU\",LEFT($T198,6)=\"ACBL12\"), IF((soundLevel($T198, $AB198, BD198, $Y198, $W198,$AJ198,$AA198,\"NC\"))<15,\"<15\",soundLevel($T198, $AB198, BD198, $Y198, $W198,$AJ198,$AA198,\"NC\")+0.4),IF((soundLevel($T198, $AB198, BD198, $Y198, $W198,$AJ198,$AA198,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T198, $AB198, BD198, $Y198, $W198,$AJ198,$AA198,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T198, $AB198, BD198, $Y198, $W198,$AJ198,$AA198,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T198=\"Select Model\",\"\",IF($T198=\"LIU24_2W\",calcQwIP($Y198,$W198,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC198,$AI198,\"latent\",$U198&\"P\"&IF($V198=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T198,activeElevation),\"\"))","v":""},{"$f":"IF($T198=\"Select Model\",\"\",IF($T198=\"ACBC_1W\",calcQwIP($Y198,$W198,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC198,BD198,\"capacity\",$U198&\"P\"&IF($V198=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T198,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y198,$W198,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC198,BD198,\"capacity\",$U198&\"P\"&IF($V198=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T198,activeElevation)))","v":""},"",{"$f":"IF(T198=\"Select Model\", 0,waterPressureDrop(W198, U198 & \"P\" & IF(V198=\"Dual\",2,1) &\"C\", AC198, \"cooling\", T198))","v":0},{"$f":"IF(T198=\"Select Model\", \"\",getReturnWaterTemp(T198,AC198, activeEWTCooling, AS198, \"cooling\"))","v":""},"",{"$f":"IF($T198<>\"ACBC_1W\",\"\",IF($J198=\"\",\"\",FintubeCapacity($T198,$W198,$AE198,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T198=\"Select Model\",T198=\"PCBL\"),\"\",calcQwIP(Y198,W198,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD198,BD198,\"capacity\",U198&\"P\"&IF(V198=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T198,activeElevation))","v":""},"",{"$f":"IF(OR(T198=\"Select Model\",T198=\"PCBL\"), \"\",IF(AY198=0,\"N/A\",waterPressureDrop(W198, U198 & \"P\" & IF(V198=\"Dual\",2,1) &\"C\", AD198, \"heating\", T198)))","v":""},{"$f":"IF(OR(T198=\"Select Model\",T198=\"PCBL\"), \"\",IF(AY198=0,getReturnWaterTemp(T198,AE198, activeEWTHeating, AX198, \"heating\"),getReturnWaterTemp(T198,AD198, activeEWTHeating, AY198, \"heating\")))","v":""},"",{"$f":" getNozzle(T198, W198, Y198, Z198, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I199)),I199<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I199, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H199)),H199<0),\"\",intlEstQuantity(T199, W199*12, H199)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T199=\"Select Model\",\"\",coilCircuitChange(W199, U199, AC199, T199,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T199=\"Select Model\",\"\",beamWidth(T199))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T199=\"Select Model\",T199=\"PCBL\"), 0,getSPIP(T199, W199, Y199, BD199, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T199=\"Select Model\", \"\",IF(T199=\"PCBL\",0,primaryAirSensibleCapacityIP($T199,$W199,activeRoomTempCooling,activePriAirTempCooling,$Y199,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T199=\"Select Model\",\"\",IF($T199=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y199,activeElevation)))","v":""},{"$f":"IF(OR(T199=\"Select Model\",T199=\"PCBL\"), 0,IF(AD199=0,0,-primaryAirSensibleCapacityIP($T199,$W199,activeRoomTempHeating,activePriAirTempHeating,$Y199,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T199=\"Select Model\", \"\", InductionRatio($T199,BD199,$W199,$Y199)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T199=\"Select Model\", \"\",IF($T199=\"PCBL\",\"N/A\",minVAVSetBack(AA199, Y199))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T199=\"Select Model\", \"\",IF($T199= \"PCBL\",\"N/A\",getDischargeAirTemp($T199,$V199,$AC199,$W199,BD199,$AL199, $Y199, $AS199, \"cooling\",activeElevation,$AB199,$AJ199,$AV199,$BB199))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T199=\"Select Model\",$T199=\"PCBL\"), \"\",getDischargeAirTemp($T199,$V199,$AD199,$W199,BD199,$AL199, $Y199, $AY199, \"heating\",activeElevation,$AB199,$AJ199,$AV199,$BB199)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T199=\"Select Model\", \"\",IF(OR($T199=\"ACBC_1W\",$T199=\"ACBC_2W\",LEFT($T199,4)=\"ACBR\",$T199 = \"LIU24_2W\",LEFT($T199,3)=\"RIU\",LEFT($T199,6)=\"ACBL12\"), IF((soundLevel($T199, $AB199, BD199, $Y199, $W199,$AJ199,$AA199,\"dba\"))<15,\"<15\",soundLevel($T199, $AB199, BD199, $Y199, $W199,$AJ199,$AA199,\"dba\")+0.4),IF((soundLevel($T199, $AB199, BD199, $Y199, $W199,$AJ199,$AA199,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T199, $AB199, BD199, $Y199, $W199,$AJ199,$AA199,\"dba\")+5)<15, \"<15\", soundLevel($T199, $AB199, BD199,$Y199, $W199,$AJ199,$AA199,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T199=\"Select Model\", \"\",IF(OR($T199=\"ACBC_1W\",$T199=\"ACBC_2W\",LEFT($T199,4)=\"ACBR\",$T199=\"LIU24_2W\",LEFT($T199,3)=\"RIU\",LEFT($T199,6)=\"ACBL12\"), IF((soundLevel($T199, $AB199, BD199, $Y199, $W199,$AJ199,$AA199,\"NC\"))<15,\"<15\",soundLevel($T199, $AB199, BD199, $Y199, $W199,$AJ199,$AA199,\"NC\")+0.4),IF((soundLevel($T199, $AB199, BD199, $Y199, $W199,$AJ199,$AA199,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T199, $AB199, BD199, $Y199, $W199,$AJ199,$AA199,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T199, $AB199, BD199, $Y199, $W199,$AJ199,$AA199,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T199=\"Select Model\",\"\",IF($T199=\"LIU24_2W\",calcQwIP($Y199,$W199,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC199,$AI199,\"latent\",$U199&\"P\"&IF($V199=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T199,activeElevation),\"\"))","v":""},{"$f":"IF($T199=\"Select Model\",\"\",IF($T199=\"ACBC_1W\",calcQwIP($Y199,$W199,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC199,BD199,\"capacity\",$U199&\"P\"&IF($V199=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T199,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y199,$W199,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC199,BD199,\"capacity\",$U199&\"P\"&IF($V199=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T199,activeElevation)))","v":""},"",{"$f":"IF(T199=\"Select Model\", 0,waterPressureDrop(W199, U199 & \"P\" & IF(V199=\"Dual\",2,1) &\"C\", AC199, \"cooling\", T199))","v":0},{"$f":"IF(T199=\"Select Model\", \"\",getReturnWaterTemp(T199,AC199, activeEWTCooling, AS199, \"cooling\"))","v":""},"",{"$f":"IF($T199<>\"ACBC_1W\",\"\",IF($J199=\"\",\"\",FintubeCapacity($T199,$W199,$AE199,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T199=\"Select Model\",T199=\"PCBL\"),\"\",calcQwIP(Y199,W199,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD199,BD199,\"capacity\",U199&\"P\"&IF(V199=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T199,activeElevation))","v":""},"",{"$f":"IF(OR(T199=\"Select Model\",T199=\"PCBL\"), \"\",IF(AY199=0,\"N/A\",waterPressureDrop(W199, U199 & \"P\" & IF(V199=\"Dual\",2,1) &\"C\", AD199, \"heating\", T199)))","v":""},{"$f":"IF(OR(T199=\"Select Model\",T199=\"PCBL\"), \"\",IF(AY199=0,getReturnWaterTemp(T199,AE199, activeEWTHeating, AX199, \"heating\"),getReturnWaterTemp(T199,AD199, activeEWTHeating, AY199, \"heating\")))","v":""},"",{"$f":" getNozzle(T199, W199, Y199, Z199, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I200)),I200<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I200, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H200)),H200<0),\"\",intlEstQuantity(T200, W200*12, H200)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T200=\"Select Model\",\"\",coilCircuitChange(W200, U200, AC200, T200,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T200=\"Select Model\",\"\",beamWidth(T200))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T200=\"Select Model\",T200=\"PCBL\"), 0,getSPIP(T200, W200, Y200, BD200, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T200=\"Select Model\", \"\",IF(T200=\"PCBL\",0,primaryAirSensibleCapacityIP($T200,$W200,activeRoomTempCooling,activePriAirTempCooling,$Y200,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T200=\"Select Model\",\"\",IF($T200=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y200,activeElevation)))","v":""},{"$f":"IF(OR(T200=\"Select Model\",T200=\"PCBL\"), 0,IF(AD200=0,0,-primaryAirSensibleCapacityIP($T200,$W200,activeRoomTempHeating,activePriAirTempHeating,$Y200,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T200=\"Select Model\", \"\", InductionRatio($T200,BD200,$W200,$Y200)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T200=\"Select Model\", \"\",IF($T200=\"PCBL\",\"N/A\",minVAVSetBack(AA200, Y200))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T200=\"Select Model\", \"\",IF($T200= \"PCBL\",\"N/A\",getDischargeAirTemp($T200,$V200,$AC200,$W200,BD200,$AL200, $Y200, $AS200, \"cooling\",activeElevation,$AB200,$AJ200,$AV200,$BB200))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T200=\"Select Model\",$T200=\"PCBL\"), \"\",getDischargeAirTemp($T200,$V200,$AD200,$W200,BD200,$AL200, $Y200, $AY200, \"heating\",activeElevation,$AB200,$AJ200,$AV200,$BB200)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T200=\"Select Model\", \"\",IF(OR($T200=\"ACBC_1W\",$T200=\"ACBC_2W\",LEFT($T200,4)=\"ACBR\",$T200 = \"LIU24_2W\",LEFT($T200,3)=\"RIU\",LEFT($T200,6)=\"ACBL12\"), IF((soundLevel($T200, $AB200, BD200, $Y200, $W200,$AJ200,$AA200,\"dba\"))<15,\"<15\",soundLevel($T200, $AB200, BD200, $Y200, $W200,$AJ200,$AA200,\"dba\")+0.4),IF((soundLevel($T200, $AB200, BD200, $Y200, $W200,$AJ200,$AA200,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T200, $AB200, BD200, $Y200, $W200,$AJ200,$AA200,\"dba\")+5)<15, \"<15\", soundLevel($T200, $AB200, BD200,$Y200, $W200,$AJ200,$AA200,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T200=\"Select Model\", \"\",IF(OR($T200=\"ACBC_1W\",$T200=\"ACBC_2W\",LEFT($T200,4)=\"ACBR\",$T200=\"LIU24_2W\",LEFT($T200,3)=\"RIU\",LEFT($T200,6)=\"ACBL12\"), IF((soundLevel($T200, $AB200, BD200, $Y200, $W200,$AJ200,$AA200,\"NC\"))<15,\"<15\",soundLevel($T200, $AB200, BD200, $Y200, $W200,$AJ200,$AA200,\"NC\")+0.4),IF((soundLevel($T200, $AB200, BD200, $Y200, $W200,$AJ200,$AA200,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T200, $AB200, BD200, $Y200, $W200,$AJ200,$AA200,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T200, $AB200, BD200, $Y200, $W200,$AJ200,$AA200,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T200=\"Select Model\",\"\",IF($T200=\"LIU24_2W\",calcQwIP($Y200,$W200,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC200,$AI200,\"latent\",$U200&\"P\"&IF($V200=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T200,activeElevation),\"\"))","v":""},{"$f":"IF($T200=\"Select Model\",\"\",IF($T200=\"ACBC_1W\",calcQwIP($Y200,$W200,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC200,BD200,\"capacity\",$U200&\"P\"&IF($V200=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T200,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y200,$W200,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC200,BD200,\"capacity\",$U200&\"P\"&IF($V200=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T200,activeElevation)))","v":""},"",{"$f":"IF(T200=\"Select Model\", 0,waterPressureDrop(W200, U200 & \"P\" & IF(V200=\"Dual\",2,1) &\"C\", AC200, \"cooling\", T200))","v":0},{"$f":"IF(T200=\"Select Model\", \"\",getReturnWaterTemp(T200,AC200, activeEWTCooling, AS200, \"cooling\"))","v":""},"",{"$f":"IF($T200<>\"ACBC_1W\",\"\",IF($J200=\"\",\"\",FintubeCapacity($T200,$W200,$AE200,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T200=\"Select Model\",T200=\"PCBL\"),\"\",calcQwIP(Y200,W200,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD200,BD200,\"capacity\",U200&\"P\"&IF(V200=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T200,activeElevation))","v":""},"",{"$f":"IF(OR(T200=\"Select Model\",T200=\"PCBL\"), \"\",IF(AY200=0,\"N/A\",waterPressureDrop(W200, U200 & \"P\" & IF(V200=\"Dual\",2,1) &\"C\", AD200, \"heating\", T200)))","v":""},{"$f":"IF(OR(T200=\"Select Model\",T200=\"PCBL\"), \"\",IF(AY200=0,getReturnWaterTemp(T200,AE200, activeEWTHeating, AX200, \"heating\"),getReturnWaterTemp(T200,AD200, activeEWTHeating, AY200, \"heating\")))","v":""},"",{"$f":" getNozzle(T200, W200, Y200, Z200, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I201)),I201<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I201, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H201)),H201<0),\"\",intlEstQuantity(T201, W201*12, H201)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T201=\"Select Model\",\"\",coilCircuitChange(W201, U201, AC201, T201,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T201=\"Select Model\",\"\",beamWidth(T201))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T201=\"Select Model\",T201=\"PCBL\"), 0,getSPIP(T201, W201, Y201, BD201, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T201=\"Select Model\", \"\",IF(T201=\"PCBL\",0,primaryAirSensibleCapacityIP($T201,$W201,activeRoomTempCooling,activePriAirTempCooling,$Y201,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T201=\"Select Model\",\"\",IF($T201=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y201,activeElevation)))","v":""},{"$f":"IF(OR(T201=\"Select Model\",T201=\"PCBL\"), 0,IF(AD201=0,0,-primaryAirSensibleCapacityIP($T201,$W201,activeRoomTempHeating,activePriAirTempHeating,$Y201,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T201=\"Select Model\", \"\", InductionRatio($T201,BD201,$W201,$Y201)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T201=\"Select Model\", \"\",IF($T201=\"PCBL\",\"N/A\",minVAVSetBack(AA201, Y201))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T201=\"Select Model\", \"\",IF($T201= \"PCBL\",\"N/A\",getDischargeAirTemp($T201,$V201,$AC201,$W201,BD201,$AL201, $Y201, $AS201, \"cooling\",activeElevation,$AB201,$AJ201,$AV201,$BB201))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T201=\"Select Model\",$T201=\"PCBL\"), \"\",getDischargeAirTemp($T201,$V201,$AD201,$W201,BD201,$AL201, $Y201, $AY201, \"heating\",activeElevation,$AB201,$AJ201,$AV201,$BB201)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T201=\"Select Model\", \"\",IF(OR($T201=\"ACBC_1W\",$T201=\"ACBC_2W\",LEFT($T201,4)=\"ACBR\",$T201 = \"LIU24_2W\",LEFT($T201,3)=\"RIU\",LEFT($T201,6)=\"ACBL12\"), IF((soundLevel($T201, $AB201, BD201, $Y201, $W201,$AJ201,$AA201,\"dba\"))<15,\"<15\",soundLevel($T201, $AB201, BD201, $Y201, $W201,$AJ201,$AA201,\"dba\")+0.4),IF((soundLevel($T201, $AB201, BD201, $Y201, $W201,$AJ201,$AA201,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T201, $AB201, BD201, $Y201, $W201,$AJ201,$AA201,\"dba\")+5)<15, \"<15\", soundLevel($T201, $AB201, BD201,$Y201, $W201,$AJ201,$AA201,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T201=\"Select Model\", \"\",IF(OR($T201=\"ACBC_1W\",$T201=\"ACBC_2W\",LEFT($T201,4)=\"ACBR\",$T201=\"LIU24_2W\",LEFT($T201,3)=\"RIU\",LEFT($T201,6)=\"ACBL12\"), IF((soundLevel($T201, $AB201, BD201, $Y201, $W201,$AJ201,$AA201,\"NC\"))<15,\"<15\",soundLevel($T201, $AB201, BD201, $Y201, $W201,$AJ201,$AA201,\"NC\")+0.4),IF((soundLevel($T201, $AB201, BD201, $Y201, $W201,$AJ201,$AA201,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T201, $AB201, BD201, $Y201, $W201,$AJ201,$AA201,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T201, $AB201, BD201, $Y201, $W201,$AJ201,$AA201,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T201=\"Select Model\",\"\",IF($T201=\"LIU24_2W\",calcQwIP($Y201,$W201,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC201,$AI201,\"latent\",$U201&\"P\"&IF($V201=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T201,activeElevation),\"\"))","v":""},{"$f":"IF($T201=\"Select Model\",\"\",IF($T201=\"ACBC_1W\",calcQwIP($Y201,$W201,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC201,BD201,\"capacity\",$U201&\"P\"&IF($V201=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T201,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y201,$W201,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC201,BD201,\"capacity\",$U201&\"P\"&IF($V201=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T201,activeElevation)))","v":""},"",{"$f":"IF(T201=\"Select Model\", 0,waterPressureDrop(W201, U201 & \"P\" & IF(V201=\"Dual\",2,1) &\"C\", AC201, \"cooling\", T201))","v":0},{"$f":"IF(T201=\"Select Model\", \"\",getReturnWaterTemp(T201,AC201, activeEWTCooling, AS201, \"cooling\"))","v":""},"",{"$f":"IF($T201<>\"ACBC_1W\",\"\",IF($J201=\"\",\"\",FintubeCapacity($T201,$W201,$AE201,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T201=\"Select Model\",T201=\"PCBL\"),\"\",calcQwIP(Y201,W201,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD201,BD201,\"capacity\",U201&\"P\"&IF(V201=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T201,activeElevation))","v":""},"",{"$f":"IF(OR(T201=\"Select Model\",T201=\"PCBL\"), \"\",IF(AY201=0,\"N/A\",waterPressureDrop(W201, U201 & \"P\" & IF(V201=\"Dual\",2,1) &\"C\", AD201, \"heating\", T201)))","v":""},{"$f":"IF(OR(T201=\"Select Model\",T201=\"PCBL\"), \"\",IF(AY201=0,getReturnWaterTemp(T201,AE201, activeEWTHeating, AX201, \"heating\"),getReturnWaterTemp(T201,AD201, activeEWTHeating, AY201, \"heating\")))","v":""},"",{"$f":" getNozzle(T201, W201, Y201, Z201, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I202)),I202<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I202, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H202)),H202<0),\"\",intlEstQuantity(T202, W202*12, H202)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T202=\"Select Model\",\"\",coilCircuitChange(W202, U202, AC202, T202,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T202=\"Select Model\",\"\",beamWidth(T202))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T202=\"Select Model\",T202=\"PCBL\"), 0,getSPIP(T202, W202, Y202, BD202, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T202=\"Select Model\", \"\",IF(T202=\"PCBL\",0,primaryAirSensibleCapacityIP($T202,$W202,activeRoomTempCooling,activePriAirTempCooling,$Y202,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T202=\"Select Model\",\"\",IF($T202=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y202,activeElevation)))","v":""},{"$f":"IF(OR(T202=\"Select Model\",T202=\"PCBL\"), 0,IF(AD202=0,0,-primaryAirSensibleCapacityIP($T202,$W202,activeRoomTempHeating,activePriAirTempHeating,$Y202,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T202=\"Select Model\", \"\", InductionRatio($T202,BD202,$W202,$Y202)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T202=\"Select Model\", \"\",IF($T202=\"PCBL\",\"N/A\",minVAVSetBack(AA202, Y202))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T202=\"Select Model\", \"\",IF($T202= \"PCBL\",\"N/A\",getDischargeAirTemp($T202,$V202,$AC202,$W202,BD202,$AL202, $Y202, $AS202, \"cooling\",activeElevation,$AB202,$AJ202,$AV202,$BB202))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T202=\"Select Model\",$T202=\"PCBL\"), \"\",getDischargeAirTemp($T202,$V202,$AD202,$W202,BD202,$AL202, $Y202, $AY202, \"heating\",activeElevation,$AB202,$AJ202,$AV202,$BB202)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T202=\"Select Model\", \"\",IF(OR($T202=\"ACBC_1W\",$T202=\"ACBC_2W\",LEFT($T202,4)=\"ACBR\",$T202 = \"LIU24_2W\",LEFT($T202,3)=\"RIU\",LEFT($T202,6)=\"ACBL12\"), IF((soundLevel($T202, $AB202, BD202, $Y202, $W202,$AJ202,$AA202,\"dba\"))<15,\"<15\",soundLevel($T202, $AB202, BD202, $Y202, $W202,$AJ202,$AA202,\"dba\")+0.4),IF((soundLevel($T202, $AB202, BD202, $Y202, $W202,$AJ202,$AA202,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T202, $AB202, BD202, $Y202, $W202,$AJ202,$AA202,\"dba\")+5)<15, \"<15\", soundLevel($T202, $AB202, BD202,$Y202, $W202,$AJ202,$AA202,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T202=\"Select Model\", \"\",IF(OR($T202=\"ACBC_1W\",$T202=\"ACBC_2W\",LEFT($T202,4)=\"ACBR\",$T202=\"LIU24_2W\",LEFT($T202,3)=\"RIU\",LEFT($T202,6)=\"ACBL12\"), IF((soundLevel($T202, $AB202, BD202, $Y202, $W202,$AJ202,$AA202,\"NC\"))<15,\"<15\",soundLevel($T202, $AB202, BD202, $Y202, $W202,$AJ202,$AA202,\"NC\")+0.4),IF((soundLevel($T202, $AB202, BD202, $Y202, $W202,$AJ202,$AA202,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T202, $AB202, BD202, $Y202, $W202,$AJ202,$AA202,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T202, $AB202, BD202, $Y202, $W202,$AJ202,$AA202,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T202=\"Select Model\",\"\",IF($T202=\"LIU24_2W\",calcQwIP($Y202,$W202,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC202,$AI202,\"latent\",$U202&\"P\"&IF($V202=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T202,activeElevation),\"\"))","v":""},{"$f":"IF($T202=\"Select Model\",\"\",IF($T202=\"ACBC_1W\",calcQwIP($Y202,$W202,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC202,BD202,\"capacity\",$U202&\"P\"&IF($V202=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T202,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y202,$W202,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC202,BD202,\"capacity\",$U202&\"P\"&IF($V202=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T202,activeElevation)))","v":""},"",{"$f":"IF(T202=\"Select Model\", 0,waterPressureDrop(W202, U202 & \"P\" & IF(V202=\"Dual\",2,1) &\"C\", AC202, \"cooling\", T202))","v":0},{"$f":"IF(T202=\"Select Model\", \"\",getReturnWaterTemp(T202,AC202, activeEWTCooling, AS202, \"cooling\"))","v":""},"",{"$f":"IF($T202<>\"ACBC_1W\",\"\",IF($J202=\"\",\"\",FintubeCapacity($T202,$W202,$AE202,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T202=\"Select Model\",T202=\"PCBL\"),\"\",calcQwIP(Y202,W202,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD202,BD202,\"capacity\",U202&\"P\"&IF(V202=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T202,activeElevation))","v":""},"",{"$f":"IF(OR(T202=\"Select Model\",T202=\"PCBL\"), \"\",IF(AY202=0,\"N/A\",waterPressureDrop(W202, U202 & \"P\" & IF(V202=\"Dual\",2,1) &\"C\", AD202, \"heating\", T202)))","v":""},{"$f":"IF(OR(T202=\"Select Model\",T202=\"PCBL\"), \"\",IF(AY202=0,getReturnWaterTemp(T202,AE202, activeEWTHeating, AX202, \"heating\"),getReturnWaterTemp(T202,AD202, activeEWTHeating, AY202, \"heating\")))","v":""},"",{"$f":" getNozzle(T202, W202, Y202, Z202, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I203)),I203<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I203, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H203)),H203<0),\"\",intlEstQuantity(T203, W203*12, H203)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T203=\"Select Model\",\"\",coilCircuitChange(W203, U203, AC203, T203,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T203=\"Select Model\",\"\",beamWidth(T203))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T203=\"Select Model\",T203=\"PCBL\"), 0,getSPIP(T203, W203, Y203, BD203, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T203=\"Select Model\", \"\",IF(T203=\"PCBL\",0,primaryAirSensibleCapacityIP($T203,$W203,activeRoomTempCooling,activePriAirTempCooling,$Y203,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T203=\"Select Model\",\"\",IF($T203=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y203,activeElevation)))","v":""},{"$f":"IF(OR(T203=\"Select Model\",T203=\"PCBL\"), 0,IF(AD203=0,0,-primaryAirSensibleCapacityIP($T203,$W203,activeRoomTempHeating,activePriAirTempHeating,$Y203,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T203=\"Select Model\", \"\", InductionRatio($T203,BD203,$W203,$Y203)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T203=\"Select Model\", \"\",IF($T203=\"PCBL\",\"N/A\",minVAVSetBack(AA203, Y203))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T203=\"Select Model\", \"\",IF($T203= \"PCBL\",\"N/A\",getDischargeAirTemp($T203,$V203,$AC203,$W203,BD203,$AL203, $Y203, $AS203, \"cooling\",activeElevation,$AB203,$AJ203,$AV203,$BB203))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T203=\"Select Model\",$T203=\"PCBL\"), \"\",getDischargeAirTemp($T203,$V203,$AD203,$W203,BD203,$AL203, $Y203, $AY203, \"heating\",activeElevation,$AB203,$AJ203,$AV203,$BB203)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T203=\"Select Model\", \"\",IF(OR($T203=\"ACBC_1W\",$T203=\"ACBC_2W\",LEFT($T203,4)=\"ACBR\",$T203 = \"LIU24_2W\",LEFT($T203,3)=\"RIU\",LEFT($T203,6)=\"ACBL12\"), IF((soundLevel($T203, $AB203, BD203, $Y203, $W203,$AJ203,$AA203,\"dba\"))<15,\"<15\",soundLevel($T203, $AB203, BD203, $Y203, $W203,$AJ203,$AA203,\"dba\")+0.4),IF((soundLevel($T203, $AB203, BD203, $Y203, $W203,$AJ203,$AA203,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T203, $AB203, BD203, $Y203, $W203,$AJ203,$AA203,\"dba\")+5)<15, \"<15\", soundLevel($T203, $AB203, BD203,$Y203, $W203,$AJ203,$AA203,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T203=\"Select Model\", \"\",IF(OR($T203=\"ACBC_1W\",$T203=\"ACBC_2W\",LEFT($T203,4)=\"ACBR\",$T203=\"LIU24_2W\",LEFT($T203,3)=\"RIU\",LEFT($T203,6)=\"ACBL12\"), IF((soundLevel($T203, $AB203, BD203, $Y203, $W203,$AJ203,$AA203,\"NC\"))<15,\"<15\",soundLevel($T203, $AB203, BD203, $Y203, $W203,$AJ203,$AA203,\"NC\")+0.4),IF((soundLevel($T203, $AB203, BD203, $Y203, $W203,$AJ203,$AA203,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T203, $AB203, BD203, $Y203, $W203,$AJ203,$AA203,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T203, $AB203, BD203, $Y203, $W203,$AJ203,$AA203,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T203=\"Select Model\",\"\",IF($T203=\"LIU24_2W\",calcQwIP($Y203,$W203,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC203,$AI203,\"latent\",$U203&\"P\"&IF($V203=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T203,activeElevation),\"\"))","v":""},{"$f":"IF($T203=\"Select Model\",\"\",IF($T203=\"ACBC_1W\",calcQwIP($Y203,$W203,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC203,BD203,\"capacity\",$U203&\"P\"&IF($V203=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T203,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y203,$W203,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC203,BD203,\"capacity\",$U203&\"P\"&IF($V203=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T203,activeElevation)))","v":""},"",{"$f":"IF(T203=\"Select Model\", 0,waterPressureDrop(W203, U203 & \"P\" & IF(V203=\"Dual\",2,1) &\"C\", AC203, \"cooling\", T203))","v":0},{"$f":"IF(T203=\"Select Model\", \"\",getReturnWaterTemp(T203,AC203, activeEWTCooling, AS203, \"cooling\"))","v":""},"",{"$f":"IF($T203<>\"ACBC_1W\",\"\",IF($J203=\"\",\"\",FintubeCapacity($T203,$W203,$AE203,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T203=\"Select Model\",T203=\"PCBL\"),\"\",calcQwIP(Y203,W203,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD203,BD203,\"capacity\",U203&\"P\"&IF(V203=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T203,activeElevation))","v":""},"",{"$f":"IF(OR(T203=\"Select Model\",T203=\"PCBL\"), \"\",IF(AY203=0,\"N/A\",waterPressureDrop(W203, U203 & \"P\" & IF(V203=\"Dual\",2,1) &\"C\", AD203, \"heating\", T203)))","v":""},{"$f":"IF(OR(T203=\"Select Model\",T203=\"PCBL\"), \"\",IF(AY203=0,getReturnWaterTemp(T203,AE203, activeEWTHeating, AX203, \"heating\"),getReturnWaterTemp(T203,AD203, activeEWTHeating, AY203, \"heating\")))","v":""},"",{"$f":" getNozzle(T203, W203, Y203, Z203, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I204)),I204<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I204, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H204)),H204<0),\"\",intlEstQuantity(T204, W204*12, H204)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T204=\"Select Model\",\"\",coilCircuitChange(W204, U204, AC204, T204,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T204=\"Select Model\",\"\",beamWidth(T204))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T204=\"Select Model\",T204=\"PCBL\"), 0,getSPIP(T204, W204, Y204, BD204, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T204=\"Select Model\", \"\",IF(T204=\"PCBL\",0,primaryAirSensibleCapacityIP($T204,$W204,activeRoomTempCooling,activePriAirTempCooling,$Y204,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T204=\"Select Model\",\"\",IF($T204=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y204,activeElevation)))","v":""},{"$f":"IF(OR(T204=\"Select Model\",T204=\"PCBL\"), 0,IF(AD204=0,0,-primaryAirSensibleCapacityIP($T204,$W204,activeRoomTempHeating,activePriAirTempHeating,$Y204,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T204=\"Select Model\", \"\", InductionRatio($T204,BD204,$W204,$Y204)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T204=\"Select Model\", \"\",IF($T204=\"PCBL\",\"N/A\",minVAVSetBack(AA204, Y204))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T204=\"Select Model\", \"\",IF($T204= \"PCBL\",\"N/A\",getDischargeAirTemp($T204,$V204,$AC204,$W204,BD204,$AL204, $Y204, $AS204, \"cooling\",activeElevation,$AB204,$AJ204,$AV204,$BB204))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T204=\"Select Model\",$T204=\"PCBL\"), \"\",getDischargeAirTemp($T204,$V204,$AD204,$W204,BD204,$AL204, $Y204, $AY204, \"heating\",activeElevation,$AB204,$AJ204,$AV204,$BB204)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T204=\"Select Model\", \"\",IF(OR($T204=\"ACBC_1W\",$T204=\"ACBC_2W\",LEFT($T204,4)=\"ACBR\",$T204 = \"LIU24_2W\",LEFT($T204,3)=\"RIU\",LEFT($T204,6)=\"ACBL12\"), IF((soundLevel($T204, $AB204, BD204, $Y204, $W204,$AJ204,$AA204,\"dba\"))<15,\"<15\",soundLevel($T204, $AB204, BD204, $Y204, $W204,$AJ204,$AA204,\"dba\")+0.4),IF((soundLevel($T204, $AB204, BD204, $Y204, $W204,$AJ204,$AA204,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T204, $AB204, BD204, $Y204, $W204,$AJ204,$AA204,\"dba\")+5)<15, \"<15\", soundLevel($T204, $AB204, BD204,$Y204, $W204,$AJ204,$AA204,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T204=\"Select Model\", \"\",IF(OR($T204=\"ACBC_1W\",$T204=\"ACBC_2W\",LEFT($T204,4)=\"ACBR\",$T204=\"LIU24_2W\",LEFT($T204,3)=\"RIU\",LEFT($T204,6)=\"ACBL12\"), IF((soundLevel($T204, $AB204, BD204, $Y204, $W204,$AJ204,$AA204,\"NC\"))<15,\"<15\",soundLevel($T204, $AB204, BD204, $Y204, $W204,$AJ204,$AA204,\"NC\")+0.4),IF((soundLevel($T204, $AB204, BD204, $Y204, $W204,$AJ204,$AA204,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T204, $AB204, BD204, $Y204, $W204,$AJ204,$AA204,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T204, $AB204, BD204, $Y204, $W204,$AJ204,$AA204,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T204=\"Select Model\",\"\",IF($T204=\"LIU24_2W\",calcQwIP($Y204,$W204,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC204,$AI204,\"latent\",$U204&\"P\"&IF($V204=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T204,activeElevation),\"\"))","v":""},{"$f":"IF($T204=\"Select Model\",\"\",IF($T204=\"ACBC_1W\",calcQwIP($Y204,$W204,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC204,BD204,\"capacity\",$U204&\"P\"&IF($V204=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T204,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y204,$W204,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC204,BD204,\"capacity\",$U204&\"P\"&IF($V204=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T204,activeElevation)))","v":""},"",{"$f":"IF(T204=\"Select Model\", 0,waterPressureDrop(W204, U204 & \"P\" & IF(V204=\"Dual\",2,1) &\"C\", AC204, \"cooling\", T204))","v":0},{"$f":"IF(T204=\"Select Model\", \"\",getReturnWaterTemp(T204,AC204, activeEWTCooling, AS204, \"cooling\"))","v":""},"",{"$f":"IF($T204<>\"ACBC_1W\",\"\",IF($J204=\"\",\"\",FintubeCapacity($T204,$W204,$AE204,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T204=\"Select Model\",T204=\"PCBL\"),\"\",calcQwIP(Y204,W204,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD204,BD204,\"capacity\",U204&\"P\"&IF(V204=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T204,activeElevation))","v":""},"",{"$f":"IF(OR(T204=\"Select Model\",T204=\"PCBL\"), \"\",IF(AY204=0,\"N/A\",waterPressureDrop(W204, U204 & \"P\" & IF(V204=\"Dual\",2,1) &\"C\", AD204, \"heating\", T204)))","v":""},{"$f":"IF(OR(T204=\"Select Model\",T204=\"PCBL\"), \"\",IF(AY204=0,getReturnWaterTemp(T204,AE204, activeEWTHeating, AX204, \"heating\"),getReturnWaterTemp(T204,AD204, activeEWTHeating, AY204, \"heating\")))","v":""},"",{"$f":" getNozzle(T204, W204, Y204, Z204, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I205)),I205<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I205, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H205)),H205<0),\"\",intlEstQuantity(T205, W205*12, H205)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T205=\"Select Model\",\"\",coilCircuitChange(W205, U205, AC205, T205,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T205=\"Select Model\",\"\",beamWidth(T205))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T205=\"Select Model\",T205=\"PCBL\"), 0,getSPIP(T205, W205, Y205, BD205, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T205=\"Select Model\", \"\",IF(T205=\"PCBL\",0,primaryAirSensibleCapacityIP($T205,$W205,activeRoomTempCooling,activePriAirTempCooling,$Y205,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T205=\"Select Model\",\"\",IF($T205=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y205,activeElevation)))","v":""},{"$f":"IF(OR(T205=\"Select Model\",T205=\"PCBL\"), 0,IF(AD205=0,0,-primaryAirSensibleCapacityIP($T205,$W205,activeRoomTempHeating,activePriAirTempHeating,$Y205,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T205=\"Select Model\", \"\", InductionRatio($T205,BD205,$W205,$Y205)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T205=\"Select Model\", \"\",IF($T205=\"PCBL\",\"N/A\",minVAVSetBack(AA205, Y205))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T205=\"Select Model\", \"\",IF($T205= \"PCBL\",\"N/A\",getDischargeAirTemp($T205,$V205,$AC205,$W205,BD205,$AL205, $Y205, $AS205, \"cooling\",activeElevation,$AB205,$AJ205,$AV205,$BB205))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T205=\"Select Model\",$T205=\"PCBL\"), \"\",getDischargeAirTemp($T205,$V205,$AD205,$W205,BD205,$AL205, $Y205, $AY205, \"heating\",activeElevation,$AB205,$AJ205,$AV205,$BB205)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T205=\"Select Model\", \"\",IF(OR($T205=\"ACBC_1W\",$T205=\"ACBC_2W\",LEFT($T205,4)=\"ACBR\",$T205 = \"LIU24_2W\",LEFT($T205,3)=\"RIU\",LEFT($T205,6)=\"ACBL12\"), IF((soundLevel($T205, $AB205, BD205, $Y205, $W205,$AJ205,$AA205,\"dba\"))<15,\"<15\",soundLevel($T205, $AB205, BD205, $Y205, $W205,$AJ205,$AA205,\"dba\")+0.4),IF((soundLevel($T205, $AB205, BD205, $Y205, $W205,$AJ205,$AA205,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T205, $AB205, BD205, $Y205, $W205,$AJ205,$AA205,\"dba\")+5)<15, \"<15\", soundLevel($T205, $AB205, BD205,$Y205, $W205,$AJ205,$AA205,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T205=\"Select Model\", \"\",IF(OR($T205=\"ACBC_1W\",$T205=\"ACBC_2W\",LEFT($T205,4)=\"ACBR\",$T205=\"LIU24_2W\",LEFT($T205,3)=\"RIU\",LEFT($T205,6)=\"ACBL12\"), IF((soundLevel($T205, $AB205, BD205, $Y205, $W205,$AJ205,$AA205,\"NC\"))<15,\"<15\",soundLevel($T205, $AB205, BD205, $Y205, $W205,$AJ205,$AA205,\"NC\")+0.4),IF((soundLevel($T205, $AB205, BD205, $Y205, $W205,$AJ205,$AA205,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T205, $AB205, BD205, $Y205, $W205,$AJ205,$AA205,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T205, $AB205, BD205, $Y205, $W205,$AJ205,$AA205,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T205=\"Select Model\",\"\",IF($T205=\"LIU24_2W\",calcQwIP($Y205,$W205,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC205,$AI205,\"latent\",$U205&\"P\"&IF($V205=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T205,activeElevation),\"\"))","v":""},{"$f":"IF($T205=\"Select Model\",\"\",IF($T205=\"ACBC_1W\",calcQwIP($Y205,$W205,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC205,BD205,\"capacity\",$U205&\"P\"&IF($V205=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T205,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y205,$W205,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC205,BD205,\"capacity\",$U205&\"P\"&IF($V205=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T205,activeElevation)))","v":""},"",{"$f":"IF(T205=\"Select Model\", 0,waterPressureDrop(W205, U205 & \"P\" & IF(V205=\"Dual\",2,1) &\"C\", AC205, \"cooling\", T205))","v":0},{"$f":"IF(T205=\"Select Model\", \"\",getReturnWaterTemp(T205,AC205, activeEWTCooling, AS205, \"cooling\"))","v":""},"",{"$f":"IF($T205<>\"ACBC_1W\",\"\",IF($J205=\"\",\"\",FintubeCapacity($T205,$W205,$AE205,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T205=\"Select Model\",T205=\"PCBL\"),\"\",calcQwIP(Y205,W205,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD205,BD205,\"capacity\",U205&\"P\"&IF(V205=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T205,activeElevation))","v":""},"",{"$f":"IF(OR(T205=\"Select Model\",T205=\"PCBL\"), \"\",IF(AY205=0,\"N/A\",waterPressureDrop(W205, U205 & \"P\" & IF(V205=\"Dual\",2,1) &\"C\", AD205, \"heating\", T205)))","v":""},{"$f":"IF(OR(T205=\"Select Model\",T205=\"PCBL\"), \"\",IF(AY205=0,getReturnWaterTemp(T205,AE205, activeEWTHeating, AX205, \"heating\"),getReturnWaterTemp(T205,AD205, activeEWTHeating, AY205, \"heating\")))","v":""},"",{"$f":" getNozzle(T205, W205, Y205, Z205, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I206)),I206<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I206, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H206)),H206<0),\"\",intlEstQuantity(T206, W206*12, H206)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T206=\"Select Model\",\"\",coilCircuitChange(W206, U206, AC206, T206,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T206=\"Select Model\",\"\",beamWidth(T206))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T206=\"Select Model\",T206=\"PCBL\"), 0,getSPIP(T206, W206, Y206, BD206, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T206=\"Select Model\", \"\",IF(T206=\"PCBL\",0,primaryAirSensibleCapacityIP($T206,$W206,activeRoomTempCooling,activePriAirTempCooling,$Y206,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T206=\"Select Model\",\"\",IF($T206=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y206,activeElevation)))","v":""},{"$f":"IF(OR(T206=\"Select Model\",T206=\"PCBL\"), 0,IF(AD206=0,0,-primaryAirSensibleCapacityIP($T206,$W206,activeRoomTempHeating,activePriAirTempHeating,$Y206,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T206=\"Select Model\", \"\", InductionRatio($T206,BD206,$W206,$Y206)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T206=\"Select Model\", \"\",IF($T206=\"PCBL\",\"N/A\",minVAVSetBack(AA206, Y206))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T206=\"Select Model\", \"\",IF($T206= \"PCBL\",\"N/A\",getDischargeAirTemp($T206,$V206,$AC206,$W206,BD206,$AL206, $Y206, $AS206, \"cooling\",activeElevation,$AB206,$AJ206,$AV206,$BB206))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T206=\"Select Model\",$T206=\"PCBL\"), \"\",getDischargeAirTemp($T206,$V206,$AD206,$W206,BD206,$AL206, $Y206, $AY206, \"heating\",activeElevation,$AB206,$AJ206,$AV206,$BB206)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T206=\"Select Model\", \"\",IF(OR($T206=\"ACBC_1W\",$T206=\"ACBC_2W\",LEFT($T206,4)=\"ACBR\",$T206 = \"LIU24_2W\",LEFT($T206,3)=\"RIU\",LEFT($T206,6)=\"ACBL12\"), IF((soundLevel($T206, $AB206, BD206, $Y206, $W206,$AJ206,$AA206,\"dba\"))<15,\"<15\",soundLevel($T206, $AB206, BD206, $Y206, $W206,$AJ206,$AA206,\"dba\")+0.4),IF((soundLevel($T206, $AB206, BD206, $Y206, $W206,$AJ206,$AA206,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T206, $AB206, BD206, $Y206, $W206,$AJ206,$AA206,\"dba\")+5)<15, \"<15\", soundLevel($T206, $AB206, BD206,$Y206, $W206,$AJ206,$AA206,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T206=\"Select Model\", \"\",IF(OR($T206=\"ACBC_1W\",$T206=\"ACBC_2W\",LEFT($T206,4)=\"ACBR\",$T206=\"LIU24_2W\",LEFT($T206,3)=\"RIU\",LEFT($T206,6)=\"ACBL12\"), IF((soundLevel($T206, $AB206, BD206, $Y206, $W206,$AJ206,$AA206,\"NC\"))<15,\"<15\",soundLevel($T206, $AB206, BD206, $Y206, $W206,$AJ206,$AA206,\"NC\")+0.4),IF((soundLevel($T206, $AB206, BD206, $Y206, $W206,$AJ206,$AA206,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T206, $AB206, BD206, $Y206, $W206,$AJ206,$AA206,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T206, $AB206, BD206, $Y206, $W206,$AJ206,$AA206,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T206=\"Select Model\",\"\",IF($T206=\"LIU24_2W\",calcQwIP($Y206,$W206,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC206,$AI206,\"latent\",$U206&\"P\"&IF($V206=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T206,activeElevation),\"\"))","v":""},{"$f":"IF($T206=\"Select Model\",\"\",IF($T206=\"ACBC_1W\",calcQwIP($Y206,$W206,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC206,BD206,\"capacity\",$U206&\"P\"&IF($V206=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T206,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y206,$W206,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC206,BD206,\"capacity\",$U206&\"P\"&IF($V206=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T206,activeElevation)))","v":""},"",{"$f":"IF(T206=\"Select Model\", 0,waterPressureDrop(W206, U206 & \"P\" & IF(V206=\"Dual\",2,1) &\"C\", AC206, \"cooling\", T206))","v":0},{"$f":"IF(T206=\"Select Model\", \"\",getReturnWaterTemp(T206,AC206, activeEWTCooling, AS206, \"cooling\"))","v":""},"",{"$f":"IF($T206<>\"ACBC_1W\",\"\",IF($J206=\"\",\"\",FintubeCapacity($T206,$W206,$AE206,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T206=\"Select Model\",T206=\"PCBL\"),\"\",calcQwIP(Y206,W206,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD206,BD206,\"capacity\",U206&\"P\"&IF(V206=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T206,activeElevation))","v":""},"",{"$f":"IF(OR(T206=\"Select Model\",T206=\"PCBL\"), \"\",IF(AY206=0,\"N/A\",waterPressureDrop(W206, U206 & \"P\" & IF(V206=\"Dual\",2,1) &\"C\", AD206, \"heating\", T206)))","v":""},{"$f":"IF(OR(T206=\"Select Model\",T206=\"PCBL\"), \"\",IF(AY206=0,getReturnWaterTemp(T206,AE206, activeEWTHeating, AX206, \"heating\"),getReturnWaterTemp(T206,AD206, activeEWTHeating, AY206, \"heating\")))","v":""},"",{"$f":" getNozzle(T206, W206, Y206, Z206, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I207)),I207<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I207, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H207)),H207<0),\"\",intlEstQuantity(T207, W207*12, H207)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T207=\"Select Model\",\"\",coilCircuitChange(W207, U207, AC207, T207,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T207=\"Select Model\",\"\",beamWidth(T207))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T207=\"Select Model\",T207=\"PCBL\"), 0,getSPIP(T207, W207, Y207, BD207, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T207=\"Select Model\", \"\",IF(T207=\"PCBL\",0,primaryAirSensibleCapacityIP($T207,$W207,activeRoomTempCooling,activePriAirTempCooling,$Y207,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T207=\"Select Model\",\"\",IF($T207=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y207,activeElevation)))","v":""},{"$f":"IF(OR(T207=\"Select Model\",T207=\"PCBL\"), 0,IF(AD207=0,0,-primaryAirSensibleCapacityIP($T207,$W207,activeRoomTempHeating,activePriAirTempHeating,$Y207,activeElevation,\"heating\")))","v":0},{"$f":"getCurrentNozzleCode(T207, W207, Y207, Z207, activeElevation, TRUE)","v":""},{"$f":"IFERROR(IF(T207=\"Select Model\", \"\", InductionRatio($T207,BD207,$W207,$Y207)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T207=\"Select Model\", \"\",IF($T207=\"PCBL\",\"N/A\",minVAVSetBack(AA207, Y207))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T207=\"Select Model\", \"\",IF($T207= \"PCBL\",\"N/A\",getDischargeAirTemp($T207,$V207,$AC207,$W207,BD207,$AL207, $Y207, $AS207, \"cooling\",activeElevation,$AB207,$AJ207,$AV207,$BB207))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T207=\"Select Model\",$T207=\"PCBL\"), \"\",getDischargeAirTemp($T207,$V207,$AD207,$W207,BD207,$AL207, $Y207, $AY207, \"heating\",activeElevation,$AB207,$AJ207,$AV207,$BB207)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T207=\"Select Model\", \"\",IF(OR($T207=\"ACBC_1W\",$T207=\"ACBC_2W\",LEFT($T207,4)=\"ACBR\",$T207 = \"LIU24_2W\",LEFT($T207,3)=\"RIU\",LEFT($T207,6)=\"ACBL12\"), IF((soundLevel($T207, $AB207, BD207, $Y207, $W207,$AJ207,$AA207,\"dba\"))<15,\"<15\",soundLevel($T207, $AB207, BD207, $Y207, $W207,$AJ207,$AA207,\"dba\")+0.4),IF((soundLevel($T207, $AB207, BD207, $Y207, $W207,$AJ207,$AA207,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T207, $AB207, BD207, $Y207, $W207,$AJ207,$AA207,\"dba\")+5)<15, \"<15\", soundLevel($T207, $AB207, BD207,$Y207, $W207,$AJ207,$AA207,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T207=\"Select Model\", \"\",IF(OR($T207=\"ACBC_1W\",$T207=\"ACBC_2W\",LEFT($T207,4)=\"ACBR\",$T207=\"LIU24_2W\",LEFT($T207,3)=\"RIU\",LEFT($T207,6)=\"ACBL12\"), IF((soundLevel($T207, $AB207, BD207, $Y207, $W207,$AJ207,$AA207,\"NC\"))<15,\"<15\",soundLevel($T207, $AB207, BD207, $Y207, $W207,$AJ207,$AA207,\"NC\")+0.4),IF((soundLevel($T207, $AB207, BD207, $Y207, $W207,$AJ207,$AA207,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T207, $AB207, BD207, $Y207, $W207,$AJ207,$AA207,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T207, $AB207, BD207, $Y207, $W207,$AJ207,$AA207,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T207=\"Select Model\",\"\",IF($T207=\"LIU24_2W\",calcQwIP($Y207,$W207,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC207,$AI207,\"latent\",$U207&\"P\"&IF($V207=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T207,activeElevation),\"\"))","v":""},{"$f":"IF($T207=\"Select Model\",\"\",IF($T207=\"ACBC_1W\",calcQwIP($Y207,$W207,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC207,BD207,\"capacity\",$U207&\"P\"&IF($V207=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T207,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y207,$W207,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC207,BD207,\"capacity\",$U207&\"P\"&IF($V207=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T207,activeElevation)))","v":""},"",{"$f":"IF(T207=\"Select Model\", 0,waterPressureDrop(W207, U207 & \"P\" & IF(V207=\"Dual\",2,1) &\"C\", AC207, \"cooling\", T207))","v":0},{"$f":"IF(T207=\"Select Model\", \"\",getReturnWaterTemp(T207,AC207, activeEWTCooling, AS207, \"cooling\"))","v":""},"",{"$f":"IF($T207<>\"ACBC_1W\",\"\",IF($J207=\"\",\"\",FintubeCapacity($T207,$W207,$AE207,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T207=\"Select Model\",T207=\"PCBL\"),\"\",calcQwIP(Y207,W207,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD207,BD207,\"capacity\",U207&\"P\"&IF(V207=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T207,activeElevation))","v":""},"",{"$f":"IF(OR(T207=\"Select Model\",T207=\"PCBL\"), \"\",IF(AY207=0,\"N/A\",waterPressureDrop(W207, U207 & \"P\" & IF(V207=\"Dual\",2,1) &\"C\", AD207, \"heating\", T207)))","v":""},{"$f":"IF(OR(T207=\"Select Model\",T207=\"PCBL\"), \"\",IF(AY207=0,getReturnWaterTemp(T207,AE207, activeEWTHeating, AX207, \"heating\"),getReturnWaterTemp(T207,AD207, activeEWTHeating, AY207, \"heating\")))","v":""},"",{"$f":" getNozzle(T207, W207, Y207, Z207, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I208)),I208<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I208, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H208)),H208<0),\"\",intlEstQuantity(T208, W208*12, H208)),1)","v":""},{"$f":"IF(LEFT(T208, 4)=\"ACBC\",IF(AND(ISNUMBER(L208),ISNUMBER(AT208)),IF(AA208=-1,\"LOW CFM\",L208*AT208),\"\"),IF(AND(ISNUMBER(L208),ISNUMBER(AT208)),IF(AA208=-1,\"N/A CFM\",L208*AT208),\"\"))","v":""},{"$f":"IF(LEFT(T208,4)=\"ACBC\",IF(AND(ISNUMBER(L208),ISNUMBER(AG208)),IF(AA208=-1,\"LOW CFM\",L208*AG208),\"\"),IF(AND(ISNUMBER(L208),ISNUMBER(AG208)),IF(AA208=-1,\"N/A CFM\",L208*AG208),\"\"))","v":""},{"$f":"IF(LEFT(T208,4)=\"ACBC\",IF(AND(ISNUMBER(L208),ISNUMBER(AZ208)),IF(AA208=-1,\"LOW CFM\",L208*AZ208),\"\"),IF(AND(ISNUMBER(L208),ISNUMBER(AZ208)),IF(AA208=-1,\"N/A CFM\",L208*AZ208),\"\"))","v":""},{"$f":"IF(AND(ISNUMBER(L208),ISNUMBER(Y208)),L208*Y208,\"\")","v":""},{"$f":"IF(AND(ISNUMBER(L208),ISNUMBER(AC208)),L208*AC208,\"\")","v":""},{"$f":"IF(AND(ISNUMBER(L208),ISNUMBER(AD208)),IF(AND(T208=\"ACBC_1W\",AD208=0),AE208*L208,L208*AD208))","v":false},"Default","Select Model",2,{"$f":"IF(T208=\"Select Model\",\"\",coilCircuitChange(W208, U208, AC208, T208,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T208=\"Select Model\",\"\",beamWidth(T208))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T208=\"Select Model\",T208=\"PCBL\"), 0,getSPIP(T208, W208, Y208, BD208, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T208=\"Select Model\", \"\",IF(T208=\"PCBL\",0,primaryAirSensibleCapacityIP($T208,$W208,activeRoomTempCooling,activePriAirTempCooling,$Y208,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T208=\"Select Model\",\"\",IF($T208=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y208,activeElevation)))","v":""},{"$f":"IF(OR(T208=\"Select Model\",T208=\"PCBL\"), 0,IF(AD208=0,0,-primaryAirSensibleCapacityIP($T208,$W208,activeRoomTempHeating,activePriAirTempHeating,$Y208,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T208=\"Select Model\", \"\", InductionRatio($T208,BD208,$W208,$Y208)),\"N/A\")","v":""},{"$f":"IFERROR(AT208/Y208,\"\")","v":""},{"$f":"IFERROR(IF(T208=\"Select Model\", \"\",(1+AJ208)*Y208),\"N/A\")","v":""},{"$f":"IFERROR(IF(T208=\"Select Model\", \"\",IF($T208=\"PCBL\",\"N/A\",minVAVSetBack(AA208, Y208))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T208=\"Select Model\", \"\",IF($T208= \"PCBL\",\"N/A\",getDischargeAirTemp($T208,$V208,$AC208,$W208,BD208,$AL208, $Y208, $AS208, \"cooling\",activeElevation,$AB208,$AJ208,$AV208,$BB208))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T208=\"Select Model\",$T208=\"PCBL\"), \"\",getDischargeAirTemp($T208,$V208,$AD208,$W208,BD208,$AL208, $Y208, $AY208, \"heating\",activeElevation,$AB208,$AJ208,$AV208,$BB208)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T208=\"Select Model\", \"\",IF(OR($T208=\"ACBC_1W\",$T208=\"ACBC_2W\",LEFT($T208,4)=\"ACBR\",$T208 = \"LIU24_2W\",LEFT($T208,3)=\"RIU\",LEFT($T208,6)=\"ACBL12\"), IF((soundLevel($T208, $AB208, BD208, $Y208, $W208,$AJ208,$AA208,\"dba\"))<15,\"<15\",soundLevel($T208, $AB208, BD208, $Y208, $W208,$AJ208,$AA208,\"dba\")+0.4),IF((soundLevel($T208, $AB208, BD208, $Y208, $W208,$AJ208,$AA208,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T208, $AB208, BD208, $Y208, $W208,$AJ208,$AA208,\"dba\")+5)<15, \"<15\", soundLevel($T208, $AB208, BD208,$Y208, $W208,$AJ208,$AA208,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T208=\"Select Model\", \"\",IF(OR($T208=\"ACBC_1W\",$T208=\"ACBC_2W\",LEFT($T208,4)=\"ACBR\",$T208=\"LIU24_2W\",LEFT($T208,3)=\"RIU\",LEFT($T208,6)=\"ACBL12\"), IF((soundLevel($T208, $AB208, BD208, $Y208, $W208,$AJ208,$AA208,\"NC\"))<15,\"<15\",soundLevel($T208, $AB208, BD208, $Y208, $W208,$AJ208,$AA208,\"NC\")+0.4),IF((soundLevel($T208, $AB208, BD208, $Y208, $W208,$AJ208,$AA208,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T208, $AB208, BD208, $Y208, $W208,$AJ208,$AA208,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T208, $AB208, BD208, $Y208, $W208,$AJ208,$AA208,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T208=\"Select Model\",\"\",IF($T208=\"LIU24_2W\",calcQwIP($Y208,$W208,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC208,$AI208,\"latent\",$U208&\"P\"&IF($V208=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T208,activeElevation),\"\"))","v":""},{"$f":"IF($T208=\"Select Model\",\"\",IF($T208=\"ACBC_1W\",calcQwIP($Y208,$W208,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC208,BD208,\"capacity\",$U208&\"P\"&IF($V208=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T208,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y208,$W208,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC208,BD208,\"capacity\",$U208&\"P\"&IF($V208=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T208,activeElevation)))","v":""},{"$f":"IF(T208=\"Select Model\", \"\",IF(T208 = \"LIU24_2W\", AS208+AF208+AR208, AS208+AF208))","v":""},{"$f":"IF(T208=\"Select Model\", 0,waterPressureDrop(W208, U208 & \"P\" & IF(V208=\"Dual\",2,1) &\"C\", AC208, \"cooling\", T208))","v":0},{"$f":"IF(T208=\"Select Model\", \"\",getReturnWaterTemp(T208,AC208, activeEWTCooling, AS208, \"cooling\"))","v":""},{"$f":"IF(T208=\"Select Model\", \"\",$AV208-activeEWTCooling)","v":""},{"$f":"IF($T208<>\"ACBC_1W\",\"\",IF($J208=\"\",\"\",FintubeCapacity($T208,$W208,$AE208,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T208=\"Select Model\",T208=\"PCBL\"),\"\",calcQwIP(Y208,W208,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD208,BD208,\"capacity\",U208&\"P\"&IF(V208=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T208,activeElevation))","v":""},{"$f":"IF(OR(T208=\"Select Model\",T208=\"PCBL\"),\"\",IF(AND(AD208=0,T208=\"ACBC_1W\"),AX208+AH208,AY208+AH208))","v":""},{"$f":"IF(OR(T208=\"Select Model\",T208=\"PCBL\"), \"\",IF(AY208=0,\"N/A\",waterPressureDrop(W208, U208 & \"P\" & IF(V208=\"Dual\",2,1) &\"C\", AD208, \"heating\", T208)))","v":""},{"$f":"IF(OR(T208=\"Select Model\",T208=\"PCBL\"), \"\",IF(AY208=0,getReturnWaterTemp(T208,AE208, activeEWTHeating, AX208, \"heating\"),getReturnWaterTemp(T208,AD208, activeEWTHeating, AY208, \"heating\")))","v":""},{"$f":"IF(OR($T208=\"Select Model\",$J208=\"\",T208=\"PCBL\"), \"\",activeEWTHeating-$BB208)","v":""},{"$f":" getNozzle(T208, W208, Y208, Z208, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I209)),I209<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I209, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H209)),H209<0),\"\",intlEstQuantity(T209, W209*12, H209)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T209=\"Select Model\",\"\",coilCircuitChange(W209, U209, AC209, T209,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T209=\"Select Model\",\"\",beamWidth(T209))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T209=\"Select Model\",T209=\"PCBL\"), 0,getSPIP(T209, W209, Y209, BD209, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T209=\"Select Model\", \"\",IF(T209=\"PCBL\",0,primaryAirSensibleCapacityIP($T209,$W209,activeRoomTempCooling,activePriAirTempCooling,$Y209,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T209=\"Select Model\",\"\",IF($T209=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y209,activeElevation)))","v":""},{"$f":"IF(OR(T209=\"Select Model\",T209=\"PCBL\"), 0,IF(AD209=0,0,-primaryAirSensibleCapacityIP($T209,$W209,activeRoomTempHeating,activePriAirTempHeating,$Y209,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T209=\"Select Model\", \"\", InductionRatio($T209,BD209,$W209,$Y209)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T209=\"Select Model\", \"\",IF($T209=\"PCBL\",\"N/A\",minVAVSetBack(AA209, Y209))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T209=\"Select Model\", \"\",IF($T209= \"PCBL\",\"N/A\",getDischargeAirTemp($T209,$V209,$AC209,$W209,BD209,$AL209, $Y209, $AS209, \"cooling\",activeElevation,$AB209,$AJ209,$AV209,$BB209))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T209=\"Select Model\",$T209=\"PCBL\"), \"\",getDischargeAirTemp($T209,$V209,$AD209,$W209,BD209,$AL209, $Y209, $AY209, \"heating\",activeElevation,$AB209,$AJ209,$AV209,$BB209)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T209=\"Select Model\", \"\",IF(OR($T209=\"ACBC_1W\",$T209=\"ACBC_2W\",LEFT($T209,4)=\"ACBR\",$T209 = \"LIU24_2W\",LEFT($T209,3)=\"RIU\",LEFT($T209,6)=\"ACBL12\"), IF((soundLevel($T209, $AB209, BD209, $Y209, $W209,$AJ209,$AA209,\"dba\"))<15,\"<15\",soundLevel($T209, $AB209, BD209, $Y209, $W209,$AJ209,$AA209,\"dba\")+0.4),IF((soundLevel($T209, $AB209, BD209, $Y209, $W209,$AJ209,$AA209,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T209, $AB209, BD209, $Y209, $W209,$AJ209,$AA209,\"dba\")+5)<15, \"<15\", soundLevel($T209, $AB209, BD209,$Y209, $W209,$AJ209,$AA209,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T209=\"Select Model\", \"\",IF(OR($T209=\"ACBC_1W\",$T209=\"ACBC_2W\",LEFT($T209,4)=\"ACBR\",$T209=\"LIU24_2W\",LEFT($T209,3)=\"RIU\",LEFT($T209,6)=\"ACBL12\"), IF((soundLevel($T209, $AB209, BD209, $Y209, $W209,$AJ209,$AA209,\"NC\"))<15,\"<15\",soundLevel($T209, $AB209, BD209, $Y209, $W209,$AJ209,$AA209,\"NC\")+0.4),IF((soundLevel($T209, $AB209, BD209, $Y209, $W209,$AJ209,$AA209,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T209, $AB209, BD209, $Y209, $W209,$AJ209,$AA209,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T209, $AB209, BD209, $Y209, $W209,$AJ209,$AA209,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T209=\"Select Model\",\"\",IF($T209=\"LIU24_2W\",calcQwIP($Y209,$W209,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC209,$AI209,\"latent\",$U209&\"P\"&IF($V209=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T209,activeElevation),\"\"))","v":""},{"$f":"IF($T209=\"Select Model\",\"\",IF($T209=\"ACBC_1W\",calcQwIP($Y209,$W209,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC209,BD209,\"capacity\",$U209&\"P\"&IF($V209=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T209,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y209,$W209,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC209,BD209,\"capacity\",$U209&\"P\"&IF($V209=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T209,activeElevation)))","v":""},"",{"$f":"IF(T209=\"Select Model\", 0,waterPressureDrop(W209, U209 & \"P\" & IF(V209=\"Dual\",2,1) &\"C\", AC209, \"cooling\", T209))","v":0},{"$f":"IF(T209=\"Select Model\", \"\",getReturnWaterTemp(T209,AC209, activeEWTCooling, AS209, \"cooling\"))","v":""},"",{"$f":"IF($T209<>\"ACBC_1W\",\"\",IF($J209=\"\",\"\",FintubeCapacity($T209,$W209,$AE209,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T209=\"Select Model\",T209=\"PCBL\"),\"\",calcQwIP(Y209,W209,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD209,BD209,\"capacity\",U209&\"P\"&IF(V209=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T209,activeElevation))","v":""},"",{"$f":"IF(OR(T209=\"Select Model\",T209=\"PCBL\"), \"\",IF(AY209=0,\"N/A\",waterPressureDrop(W209, U209 & \"P\" & IF(V209=\"Dual\",2,1) &\"C\", AD209, \"heating\", T209)))","v":""},{"$f":"IF(OR(T209=\"Select Model\",T209=\"PCBL\"), \"\",IF(AY209=0,getReturnWaterTemp(T209,AE209, activeEWTHeating, AX209, \"heating\"),getReturnWaterTemp(T209,AD209, activeEWTHeating, AY209, \"heating\")))","v":""},"",{"$f":" getNozzle(T209, W209, Y209, Z209, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I210)),I210<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I210, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H210)),H210<0),\"\",intlEstQuantity(T210, W210*12, H210)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T210=\"Select Model\",\"\",coilCircuitChange(W210, U210, AC210, T210,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T210=\"Select Model\",\"\",beamWidth(T210))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T210=\"Select Model\",T210=\"PCBL\"), 0,getSPIP(T210, W210, Y210, BD210, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T210=\"Select Model\", \"\",IF(T210=\"PCBL\",0,primaryAirSensibleCapacityIP($T210,$W210,activeRoomTempCooling,activePriAirTempCooling,$Y210,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T210=\"Select Model\",\"\",IF($T210=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y210,activeElevation)))","v":""},{"$f":"IF(OR(T210=\"Select Model\",T210=\"PCBL\"), 0,IF(AD210=0,0,-primaryAirSensibleCapacityIP($T210,$W210,activeRoomTempHeating,activePriAirTempHeating,$Y210,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T210=\"Select Model\", \"\", InductionRatio($T210,BD210,$W210,$Y210)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T210=\"Select Model\", \"\",IF($T210=\"PCBL\",\"N/A\",minVAVSetBack(AA210, Y210))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T210=\"Select Model\", \"\",IF($T210= \"PCBL\",\"N/A\",getDischargeAirTemp($T210,$V210,$AC210,$W210,BD210,$AL210, $Y210, $AS210, \"cooling\",activeElevation,$AB210,$AJ210,$AV210,$BB210))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T210=\"Select Model\",$T210=\"PCBL\"), \"\",getDischargeAirTemp($T210,$V210,$AD210,$W210,BD210,$AL210, $Y210, $AY210, \"heating\",activeElevation,$AB210,$AJ210,$AV210,$BB210)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T210=\"Select Model\", \"\",IF(OR($T210=\"ACBC_1W\",$T210=\"ACBC_2W\",LEFT($T210,4)=\"ACBR\",$T210 = \"LIU24_2W\",LEFT($T210,3)=\"RIU\",LEFT($T210,6)=\"ACBL12\"), IF((soundLevel($T210, $AB210, BD210, $Y210, $W210,$AJ210,$AA210,\"dba\"))<15,\"<15\",soundLevel($T210, $AB210, BD210, $Y210, $W210,$AJ210,$AA210,\"dba\")+0.4),IF((soundLevel($T210, $AB210, BD210, $Y210, $W210,$AJ210,$AA210,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T210, $AB210, BD210, $Y210, $W210,$AJ210,$AA210,\"dba\")+5)<15, \"<15\", soundLevel($T210, $AB210, BD210,$Y210, $W210,$AJ210,$AA210,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T210=\"Select Model\", \"\",IF(OR($T210=\"ACBC_1W\",$T210=\"ACBC_2W\",LEFT($T210,4)=\"ACBR\",$T210=\"LIU24_2W\",LEFT($T210,3)=\"RIU\",LEFT($T210,6)=\"ACBL12\"), IF((soundLevel($T210, $AB210, BD210, $Y210, $W210,$AJ210,$AA210,\"NC\"))<15,\"<15\",soundLevel($T210, $AB210, BD210, $Y210, $W210,$AJ210,$AA210,\"NC\")+0.4),IF((soundLevel($T210, $AB210, BD210, $Y210, $W210,$AJ210,$AA210,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T210, $AB210, BD210, $Y210, $W210,$AJ210,$AA210,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T210, $AB210, BD210, $Y210, $W210,$AJ210,$AA210,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T210=\"Select Model\",\"\",IF($T210=\"LIU24_2W\",calcQwIP($Y210,$W210,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC210,$AI210,\"latent\",$U210&\"P\"&IF($V210=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T210,activeElevation),\"\"))","v":""},{"$f":"IF($T210=\"Select Model\",\"\",IF($T210=\"ACBC_1W\",calcQwIP($Y210,$W210,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC210,BD210,\"capacity\",$U210&\"P\"&IF($V210=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T210,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y210,$W210,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC210,BD210,\"capacity\",$U210&\"P\"&IF($V210=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T210,activeElevation)))","v":""},"",{"$f":"IF(T210=\"Select Model\", 0,waterPressureDrop(W210, U210 & \"P\" & IF(V210=\"Dual\",2,1) &\"C\", AC210, \"cooling\", T210))","v":0},{"$f":"IF(T210=\"Select Model\", \"\",getReturnWaterTemp(T210,AC210, activeEWTCooling, AS210, \"cooling\"))","v":""},"",{"$f":"IF($T210<>\"ACBC_1W\",\"\",IF($J210=\"\",\"\",FintubeCapacity($T210,$W210,$AE210,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T210=\"Select Model\",T210=\"PCBL\"),\"\",calcQwIP(Y210,W210,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD210,BD210,\"capacity\",U210&\"P\"&IF(V210=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T210,activeElevation))","v":""},"",{"$f":"IF(OR(T210=\"Select Model\",T210=\"PCBL\"), \"\",IF(AY210=0,\"N/A\",waterPressureDrop(W210, U210 & \"P\" & IF(V210=\"Dual\",2,1) &\"C\", AD210, \"heating\", T210)))","v":""},{"$f":"IF(OR(T210=\"Select Model\",T210=\"PCBL\"), \"\",IF(AY210=0,getReturnWaterTemp(T210,AE210, activeEWTHeating, AX210, \"heating\"),getReturnWaterTemp(T210,AD210, activeEWTHeating, AY210, \"heating\")))","v":""},"",{"$f":" getNozzle(T210, W210, Y210, Z210, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I211)),I211<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I211, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H211)),H211<0),\"\",intlEstQuantity(T211, W211*12, H211)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T211=\"Select Model\",\"\",coilCircuitChange(W211, U211, AC211, T211,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T211=\"Select Model\",\"\",beamWidth(T211))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T211=\"Select Model\",T211=\"PCBL\"), 0,getSPIP(T211, W211, Y211, BD211, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T211=\"Select Model\", \"\",IF(T211=\"PCBL\",0,primaryAirSensibleCapacityIP($T211,$W211,activeRoomTempCooling,activePriAirTempCooling,$Y211,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T211=\"Select Model\",\"\",IF($T211=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y211,activeElevation)))","v":""},{"$f":"IF(OR(T211=\"Select Model\",T211=\"PCBL\"), 0,IF(AD211=0,0,-primaryAirSensibleCapacityIP($T211,$W211,activeRoomTempHeating,activePriAirTempHeating,$Y211,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T211=\"Select Model\", \"\", InductionRatio($T211,BD211,$W211,$Y211)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T211=\"Select Model\", \"\",IF($T211=\"PCBL\",\"N/A\",minVAVSetBack(AA211, Y211))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T211=\"Select Model\", \"\",IF($T211= \"PCBL\",\"N/A\",getDischargeAirTemp($T211,$V211,$AC211,$W211,BD211,$AL211, $Y211, $AS211, \"cooling\",activeElevation,$AB211,$AJ211,$AV211,$BB211))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T211=\"Select Model\",$T211=\"PCBL\"), \"\",getDischargeAirTemp($T211,$V211,$AD211,$W211,BD211,$AL211, $Y211, $AY211, \"heating\",activeElevation,$AB211,$AJ211,$AV211,$BB211)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T211=\"Select Model\", \"\",IF(OR($T211=\"ACBC_1W\",$T211=\"ACBC_2W\",LEFT($T211,4)=\"ACBR\",$T211 = \"LIU24_2W\",LEFT($T211,3)=\"RIU\",LEFT($T211,6)=\"ACBL12\"), IF((soundLevel($T211, $AB211, BD211, $Y211, $W211,$AJ211,$AA211,\"dba\"))<15,\"<15\",soundLevel($T211, $AB211, BD211, $Y211, $W211,$AJ211,$AA211,\"dba\")+0.4),IF((soundLevel($T211, $AB211, BD211, $Y211, $W211,$AJ211,$AA211,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T211, $AB211, BD211, $Y211, $W211,$AJ211,$AA211,\"dba\")+5)<15, \"<15\", soundLevel($T211, $AB211, BD211,$Y211, $W211,$AJ211,$AA211,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T211=\"Select Model\", \"\",IF(OR($T211=\"ACBC_1W\",$T211=\"ACBC_2W\",LEFT($T211,4)=\"ACBR\",$T211=\"LIU24_2W\",LEFT($T211,3)=\"RIU\",LEFT($T211,6)=\"ACBL12\"), IF((soundLevel($T211, $AB211, BD211, $Y211, $W211,$AJ211,$AA211,\"NC\"))<15,\"<15\",soundLevel($T211, $AB211, BD211, $Y211, $W211,$AJ211,$AA211,\"NC\")+0.4),IF((soundLevel($T211, $AB211, BD211, $Y211, $W211,$AJ211,$AA211,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T211, $AB211, BD211, $Y211, $W211,$AJ211,$AA211,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T211, $AB211, BD211, $Y211, $W211,$AJ211,$AA211,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T211=\"Select Model\",\"\",IF($T211=\"LIU24_2W\",calcQwIP($Y211,$W211,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC211,$AI211,\"latent\",$U211&\"P\"&IF($V211=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T211,activeElevation),\"\"))","v":""},{"$f":"IF($T211=\"Select Model\",\"\",IF($T211=\"ACBC_1W\",calcQwIP($Y211,$W211,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC211,BD211,\"capacity\",$U211&\"P\"&IF($V211=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T211,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y211,$W211,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC211,BD211,\"capacity\",$U211&\"P\"&IF($V211=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T211,activeElevation)))","v":""},"",{"$f":"IF(T211=\"Select Model\", 0,waterPressureDrop(W211, U211 & \"P\" & IF(V211=\"Dual\",2,1) &\"C\", AC211, \"cooling\", T211))","v":0},{"$f":"IF(T211=\"Select Model\", \"\",getReturnWaterTemp(T211,AC211, activeEWTCooling, AS211, \"cooling\"))","v":""},"",{"$f":"IF($T211<>\"ACBC_1W\",\"\",IF($J211=\"\",\"\",FintubeCapacity($T211,$W211,$AE211,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T211=\"Select Model\",T211=\"PCBL\"),\"\",calcQwIP(Y211,W211,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD211,BD211,\"capacity\",U211&\"P\"&IF(V211=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T211,activeElevation))","v":""},"",{"$f":"IF(OR(T211=\"Select Model\",T211=\"PCBL\"), \"\",IF(AY211=0,\"N/A\",waterPressureDrop(W211, U211 & \"P\" & IF(V211=\"Dual\",2,1) &\"C\", AD211, \"heating\", T211)))","v":""},{"$f":"IF(OR(T211=\"Select Model\",T211=\"PCBL\"), \"\",IF(AY211=0,getReturnWaterTemp(T211,AE211, activeEWTHeating, AX211, \"heating\"),getReturnWaterTemp(T211,AD211, activeEWTHeating, AY211, \"heating\")))","v":""},"",{"$f":" getNozzle(T211, W211, Y211, Z211, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I212)),I212<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I212, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H212)),H212<0),\"\",intlEstQuantity(T212, W212*12, H212)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T212=\"Select Model\",\"\",coilCircuitChange(W212, U212, AC212, T212,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T212=\"Select Model\",\"\",beamWidth(T212))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T212=\"Select Model\",T212=\"PCBL\"), 0,getSPIP(T212, W212, Y212, BD212, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T212=\"Select Model\", \"\",IF(T212=\"PCBL\",0,primaryAirSensibleCapacityIP($T212,$W212,activeRoomTempCooling,activePriAirTempCooling,$Y212,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T212=\"Select Model\",\"\",IF($T212=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y212,activeElevation)))","v":""},{"$f":"IF(OR(T212=\"Select Model\",T212=\"PCBL\"), 0,IF(AD212=0,0,-primaryAirSensibleCapacityIP($T212,$W212,activeRoomTempHeating,activePriAirTempHeating,$Y212,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T212=\"Select Model\", \"\", InductionRatio($T212,BD212,$W212,$Y212)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T212=\"Select Model\", \"\",IF($T212=\"PCBL\",\"N/A\",minVAVSetBack(AA212, Y212))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T212=\"Select Model\", \"\",IF($T212= \"PCBL\",\"N/A\",getDischargeAirTemp($T212,$V212,$AC212,$W212,BD212,$AL212, $Y212, $AS212, \"cooling\",activeElevation,$AB212,$AJ212,$AV212,$BB212))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T212=\"Select Model\",$T212=\"PCBL\"), \"\",getDischargeAirTemp($T212,$V212,$AD212,$W212,BD212,$AL212, $Y212, $AY212, \"heating\",activeElevation,$AB212,$AJ212,$AV212,$BB212)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T212=\"Select Model\", \"\",IF(OR($T212=\"ACBC_1W\",$T212=\"ACBC_2W\",LEFT($T212,4)=\"ACBR\",$T212 = \"LIU24_2W\",LEFT($T212,3)=\"RIU\",LEFT($T212,6)=\"ACBL12\"), IF((soundLevel($T212, $AB212, BD212, $Y212, $W212,$AJ212,$AA212,\"dba\"))<15,\"<15\",soundLevel($T212, $AB212, BD212, $Y212, $W212,$AJ212,$AA212,\"dba\")+0.4),IF((soundLevel($T212, $AB212, BD212, $Y212, $W212,$AJ212,$AA212,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T212, $AB212, BD212, $Y212, $W212,$AJ212,$AA212,\"dba\")+5)<15, \"<15\", soundLevel($T212, $AB212, BD212,$Y212, $W212,$AJ212,$AA212,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T212=\"Select Model\", \"\",IF(OR($T212=\"ACBC_1W\",$T212=\"ACBC_2W\",LEFT($T212,4)=\"ACBR\",$T212=\"LIU24_2W\",LEFT($T212,3)=\"RIU\",LEFT($T212,6)=\"ACBL12\"), IF((soundLevel($T212, $AB212, BD212, $Y212, $W212,$AJ212,$AA212,\"NC\"))<15,\"<15\",soundLevel($T212, $AB212, BD212, $Y212, $W212,$AJ212,$AA212,\"NC\")+0.4),IF((soundLevel($T212, $AB212, BD212, $Y212, $W212,$AJ212,$AA212,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T212, $AB212, BD212, $Y212, $W212,$AJ212,$AA212,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T212, $AB212, BD212, $Y212, $W212,$AJ212,$AA212,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T212=\"Select Model\",\"\",IF($T212=\"LIU24_2W\",calcQwIP($Y212,$W212,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC212,$AI212,\"latent\",$U212&\"P\"&IF($V212=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T212,activeElevation),\"\"))","v":""},{"$f":"IF($T212=\"Select Model\",\"\",IF($T212=\"ACBC_1W\",calcQwIP($Y212,$W212,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC212,BD212,\"capacity\",$U212&\"P\"&IF($V212=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T212,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y212,$W212,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC212,BD212,\"capacity\",$U212&\"P\"&IF($V212=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T212,activeElevation)))","v":""},"",{"$f":"IF(T212=\"Select Model\", 0,waterPressureDrop(W212, U212 & \"P\" & IF(V212=\"Dual\",2,1) &\"C\", AC212, \"cooling\", T212))","v":0},{"$f":"IF(T212=\"Select Model\", \"\",getReturnWaterTemp(T212,AC212, activeEWTCooling, AS212, \"cooling\"))","v":""},"",{"$f":"IF($T212<>\"ACBC_1W\",\"\",IF($J212=\"\",\"\",FintubeCapacity($T212,$W212,$AE212,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T212=\"Select Model\",T212=\"PCBL\"),\"\",calcQwIP(Y212,W212,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD212,BD212,\"capacity\",U212&\"P\"&IF(V212=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T212,activeElevation))","v":""},"",{"$f":"IF(OR(T212=\"Select Model\",T212=\"PCBL\"), \"\",IF(AY212=0,\"N/A\",waterPressureDrop(W212, U212 & \"P\" & IF(V212=\"Dual\",2,1) &\"C\", AD212, \"heating\", T212)))","v":""},{"$f":"IF(OR(T212=\"Select Model\",T212=\"PCBL\"), \"\",IF(AY212=0,getReturnWaterTemp(T212,AE212, activeEWTHeating, AX212, \"heating\"),getReturnWaterTemp(T212,AD212, activeEWTHeating, AY212, \"heating\")))","v":""},"",{"$f":" getNozzle(T212, W212, Y212, Z212, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I213)),I213<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I213, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H213)),H213<0),\"\",intlEstQuantity(T213, W213*12, H213)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T213=\"Select Model\",\"\",coilCircuitChange(W213, U213, AC213, T213,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T213=\"Select Model\",\"\",beamWidth(T213))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T213=\"Select Model\",T213=\"PCBL\"), 0,getSPIP(T213, W213, Y213, BD213, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T213=\"Select Model\", \"\",IF(T213=\"PCBL\",0,primaryAirSensibleCapacityIP($T213,$W213,activeRoomTempCooling,activePriAirTempCooling,$Y213,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T213=\"Select Model\",\"\",IF($T213=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y213,activeElevation)))","v":""},{"$f":"IF(OR(T213=\"Select Model\",T213=\"PCBL\"), 0,IF(AD213=0,0,-primaryAirSensibleCapacityIP($T213,$W213,activeRoomTempHeating,activePriAirTempHeating,$Y213,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T213=\"Select Model\", \"\", InductionRatio($T213,BD213,$W213,$Y213)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T213=\"Select Model\", \"\",IF($T213=\"PCBL\",\"N/A\",minVAVSetBack(AA213, Y213))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T213=\"Select Model\", \"\",IF($T213= \"PCBL\",\"N/A\",getDischargeAirTemp($T213,$V213,$AC213,$W213,BD213,$AL213, $Y213, $AS213, \"cooling\",activeElevation,$AB213,$AJ213,$AV213,$BB213))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T213=\"Select Model\",$T213=\"PCBL\"), \"\",getDischargeAirTemp($T213,$V213,$AD213,$W213,BD213,$AL213, $Y213, $AY213, \"heating\",activeElevation,$AB213,$AJ213,$AV213,$BB213)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T213=\"Select Model\", \"\",IF(OR($T213=\"ACBC_1W\",$T213=\"ACBC_2W\",LEFT($T213,4)=\"ACBR\",$T213 = \"LIU24_2W\",LEFT($T213,3)=\"RIU\",LEFT($T213,6)=\"ACBL12\"), IF((soundLevel($T213, $AB213, BD213, $Y213, $W213,$AJ213,$AA213,\"dba\"))<15,\"<15\",soundLevel($T213, $AB213, BD213, $Y213, $W213,$AJ213,$AA213,\"dba\")+0.4),IF((soundLevel($T213, $AB213, BD213, $Y213, $W213,$AJ213,$AA213,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T213, $AB213, BD213, $Y213, $W213,$AJ213,$AA213,\"dba\")+5)<15, \"<15\", soundLevel($T213, $AB213, BD213,$Y213, $W213,$AJ213,$AA213,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T213=\"Select Model\", \"\",IF(OR($T213=\"ACBC_1W\",$T213=\"ACBC_2W\",LEFT($T213,4)=\"ACBR\",$T213=\"LIU24_2W\",LEFT($T213,3)=\"RIU\",LEFT($T213,6)=\"ACBL12\"), IF((soundLevel($T213, $AB213, BD213, $Y213, $W213,$AJ213,$AA213,\"NC\"))<15,\"<15\",soundLevel($T213, $AB213, BD213, $Y213, $W213,$AJ213,$AA213,\"NC\")+0.4),IF((soundLevel($T213, $AB213, BD213, $Y213, $W213,$AJ213,$AA213,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T213, $AB213, BD213, $Y213, $W213,$AJ213,$AA213,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T213, $AB213, BD213, $Y213, $W213,$AJ213,$AA213,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T213=\"Select Model\",\"\",IF($T213=\"LIU24_2W\",calcQwIP($Y213,$W213,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC213,$AI213,\"latent\",$U213&\"P\"&IF($V213=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T213,activeElevation),\"\"))","v":""},{"$f":"IF($T213=\"Select Model\",\"\",IF($T213=\"ACBC_1W\",calcQwIP($Y213,$W213,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC213,BD213,\"capacity\",$U213&\"P\"&IF($V213=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T213,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y213,$W213,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC213,BD213,\"capacity\",$U213&\"P\"&IF($V213=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T213,activeElevation)))","v":""},"",{"$f":"IF(T213=\"Select Model\", 0,waterPressureDrop(W213, U213 & \"P\" & IF(V213=\"Dual\",2,1) &\"C\", AC213, \"cooling\", T213))","v":0},{"$f":"IF(T213=\"Select Model\", \"\",getReturnWaterTemp(T213,AC213, activeEWTCooling, AS213, \"cooling\"))","v":""},"",{"$f":"IF($T213<>\"ACBC_1W\",\"\",IF($J213=\"\",\"\",FintubeCapacity($T213,$W213,$AE213,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T213=\"Select Model\",T213=\"PCBL\"),\"\",calcQwIP(Y213,W213,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD213,BD213,\"capacity\",U213&\"P\"&IF(V213=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T213,activeElevation))","v":""},"",{"$f":"IF(OR(T213=\"Select Model\",T213=\"PCBL\"), \"\",IF(AY213=0,\"N/A\",waterPressureDrop(W213, U213 & \"P\" & IF(V213=\"Dual\",2,1) &\"C\", AD213, \"heating\", T213)))","v":""},{"$f":"IF(OR(T213=\"Select Model\",T213=\"PCBL\"), \"\",IF(AY213=0,getReturnWaterTemp(T213,AE213, activeEWTHeating, AX213, \"heating\"),getReturnWaterTemp(T213,AD213, activeEWTHeating, AY213, \"heating\")))","v":""},"",{"$f":" getNozzle(T213, W213, Y213, Z213, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I214)),I214<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I214, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H214)),H214<0),\"\",intlEstQuantity(T214, W214*12, H214)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T214=\"Select Model\",\"\",coilCircuitChange(W214, U214, AC214, T214,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T214=\"Select Model\",\"\",beamWidth(T214))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T214=\"Select Model\",T214=\"PCBL\"), 0,getSPIP(T214, W214, Y214, BD214, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T214=\"Select Model\", \"\",IF(T214=\"PCBL\",0,primaryAirSensibleCapacityIP($T214,$W214,activeRoomTempCooling,activePriAirTempCooling,$Y214,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T214=\"Select Model\",\"\",IF($T214=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y214,activeElevation)))","v":""},{"$f":"IF(OR(T214=\"Select Model\",T214=\"PCBL\"), 0,IF(AD214=0,0,-primaryAirSensibleCapacityIP($T214,$W214,activeRoomTempHeating,activePriAirTempHeating,$Y214,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T214=\"Select Model\", \"\", InductionRatio($T214,BD214,$W214,$Y214)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T214=\"Select Model\", \"\",IF($T214=\"PCBL\",\"N/A\",minVAVSetBack(AA214, Y214))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T214=\"Select Model\", \"\",IF($T214= \"PCBL\",\"N/A\",getDischargeAirTemp($T214,$V214,$AC214,$W214,BD214,$AL214, $Y214, $AS214, \"cooling\",activeElevation,$AB214,$AJ214,$AV214,$BB214))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T214=\"Select Model\",$T214=\"PCBL\"), \"\",getDischargeAirTemp($T214,$V214,$AD214,$W214,BD214,$AL214, $Y214, $AY214, \"heating\",activeElevation,$AB214,$AJ214,$AV214,$BB214)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T214=\"Select Model\", \"\",IF(OR($T214=\"ACBC_1W\",$T214=\"ACBC_2W\",LEFT($T214,4)=\"ACBR\",$T214 = \"LIU24_2W\",LEFT($T214,3)=\"RIU\",LEFT($T214,6)=\"ACBL12\"), IF((soundLevel($T214, $AB214, BD214, $Y214, $W214,$AJ214,$AA214,\"dba\"))<15,\"<15\",soundLevel($T214, $AB214, BD214, $Y214, $W214,$AJ214,$AA214,\"dba\")+0.4),IF((soundLevel($T214, $AB214, BD214, $Y214, $W214,$AJ214,$AA214,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T214, $AB214, BD214, $Y214, $W214,$AJ214,$AA214,\"dba\")+5)<15, \"<15\", soundLevel($T214, $AB214, BD214,$Y214, $W214,$AJ214,$AA214,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T214=\"Select Model\", \"\",IF(OR($T214=\"ACBC_1W\",$T214=\"ACBC_2W\",LEFT($T214,4)=\"ACBR\",$T214=\"LIU24_2W\",LEFT($T214,3)=\"RIU\",LEFT($T214,6)=\"ACBL12\"), IF((soundLevel($T214, $AB214, BD214, $Y214, $W214,$AJ214,$AA214,\"NC\"))<15,\"<15\",soundLevel($T214, $AB214, BD214, $Y214, $W214,$AJ214,$AA214,\"NC\")+0.4),IF((soundLevel($T214, $AB214, BD214, $Y214, $W214,$AJ214,$AA214,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T214, $AB214, BD214, $Y214, $W214,$AJ214,$AA214,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T214, $AB214, BD214, $Y214, $W214,$AJ214,$AA214,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T214=\"Select Model\",\"\",IF($T214=\"LIU24_2W\",calcQwIP($Y214,$W214,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC214,$AI214,\"latent\",$U214&\"P\"&IF($V214=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T214,activeElevation),\"\"))","v":""},{"$f":"IF($T214=\"Select Model\",\"\",IF($T214=\"ACBC_1W\",calcQwIP($Y214,$W214,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC214,BD214,\"capacity\",$U214&\"P\"&IF($V214=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T214,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y214,$W214,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC214,BD214,\"capacity\",$U214&\"P\"&IF($V214=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T214,activeElevation)))","v":""},"",{"$f":"IF(T214=\"Select Model\", 0,waterPressureDrop(W214, U214 & \"P\" & IF(V214=\"Dual\",2,1) &\"C\", AC214, \"cooling\", T214))","v":0},{"$f":"IF(T214=\"Select Model\", \"\",getReturnWaterTemp(T214,AC214, activeEWTCooling, AS214, \"cooling\"))","v":""},"",{"$f":"IF($T214<>\"ACBC_1W\",\"\",IF($J214=\"\",\"\",FintubeCapacity($T214,$W214,$AE214,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T214=\"Select Model\",T214=\"PCBL\"),\"\",calcQwIP(Y214,W214,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD214,BD214,\"capacity\",U214&\"P\"&IF(V214=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T214,activeElevation))","v":""},"",{"$f":"IF(OR(T214=\"Select Model\",T214=\"PCBL\"), \"\",IF(AY214=0,\"N/A\",waterPressureDrop(W214, U214 & \"P\" & IF(V214=\"Dual\",2,1) &\"C\", AD214, \"heating\", T214)))","v":""},{"$f":"IF(OR(T214=\"Select Model\",T214=\"PCBL\"), \"\",IF(AY214=0,getReturnWaterTemp(T214,AE214, activeEWTHeating, AX214, \"heating\"),getReturnWaterTemp(T214,AD214, activeEWTHeating, AY214, \"heating\")))","v":""},"",{"$f":" getNozzle(T214, W214, Y214, Z214, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I215)),I215<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I215, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H215)),H215<0),\"\",intlEstQuantity(T215, W215*12, H215)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T215=\"Select Model\",\"\",coilCircuitChange(W215, U215, AC215, T215,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T215=\"Select Model\",\"\",beamWidth(T215))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T215=\"Select Model\",T215=\"PCBL\"), 0,getSPIP(T215, W215, Y215, BD215, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T215=\"Select Model\", \"\",IF(T215=\"PCBL\",0,primaryAirSensibleCapacityIP($T215,$W215,activeRoomTempCooling,activePriAirTempCooling,$Y215,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T215=\"Select Model\",\"\",IF($T215=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y215,activeElevation)))","v":""},{"$f":"IF(OR(T215=\"Select Model\",T215=\"PCBL\"), 0,IF(AD215=0,0,-primaryAirSensibleCapacityIP($T215,$W215,activeRoomTempHeating,activePriAirTempHeating,$Y215,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T215=\"Select Model\", \"\", InductionRatio($T215,BD215,$W215,$Y215)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T215=\"Select Model\", \"\",IF($T215=\"PCBL\",\"N/A\",minVAVSetBack(AA215, Y215))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T215=\"Select Model\", \"\",IF($T215= \"PCBL\",\"N/A\",getDischargeAirTemp($T215,$V215,$AC215,$W215,BD215,$AL215, $Y215, $AS215, \"cooling\",activeElevation,$AB215,$AJ215,$AV215,$BB215))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T215=\"Select Model\",$T215=\"PCBL\"), \"\",getDischargeAirTemp($T215,$V215,$AD215,$W215,BD215,$AL215, $Y215, $AY215, \"heating\",activeElevation,$AB215,$AJ215,$AV215,$BB215)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T215=\"Select Model\", \"\",IF(OR($T215=\"ACBC_1W\",$T215=\"ACBC_2W\",LEFT($T215,4)=\"ACBR\",$T215 = \"LIU24_2W\",LEFT($T215,3)=\"RIU\",LEFT($T215,6)=\"ACBL12\"), IF((soundLevel($T215, $AB215, BD215, $Y215, $W215,$AJ215,$AA215,\"dba\"))<15,\"<15\",soundLevel($T215, $AB215, BD215, $Y215, $W215,$AJ215,$AA215,\"dba\")+0.4),IF((soundLevel($T215, $AB215, BD215, $Y215, $W215,$AJ215,$AA215,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T215, $AB215, BD215, $Y215, $W215,$AJ215,$AA215,\"dba\")+5)<15, \"<15\", soundLevel($T215, $AB215, BD215,$Y215, $W215,$AJ215,$AA215,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T215=\"Select Model\", \"\",IF(OR($T215=\"ACBC_1W\",$T215=\"ACBC_2W\",LEFT($T215,4)=\"ACBR\",$T215=\"LIU24_2W\",LEFT($T215,3)=\"RIU\",LEFT($T215,6)=\"ACBL12\"), IF((soundLevel($T215, $AB215, BD215, $Y215, $W215,$AJ215,$AA215,\"NC\"))<15,\"<15\",soundLevel($T215, $AB215, BD215, $Y215, $W215,$AJ215,$AA215,\"NC\")+0.4),IF((soundLevel($T215, $AB215, BD215, $Y215, $W215,$AJ215,$AA215,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T215, $AB215, BD215, $Y215, $W215,$AJ215,$AA215,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T215, $AB215, BD215, $Y215, $W215,$AJ215,$AA215,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T215=\"Select Model\",\"\",IF($T215=\"LIU24_2W\",calcQwIP($Y215,$W215,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC215,$AI215,\"latent\",$U215&\"P\"&IF($V215=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T215,activeElevation),\"\"))","v":""},{"$f":"IF($T215=\"Select Model\",\"\",IF($T215=\"ACBC_1W\",calcQwIP($Y215,$W215,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC215,BD215,\"capacity\",$U215&\"P\"&IF($V215=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T215,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y215,$W215,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC215,BD215,\"capacity\",$U215&\"P\"&IF($V215=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T215,activeElevation)))","v":""},"",{"$f":"IF(T215=\"Select Model\", 0,waterPressureDrop(W215, U215 & \"P\" & IF(V215=\"Dual\",2,1) &\"C\", AC215, \"cooling\", T215))","v":0},{"$f":"IF(T215=\"Select Model\", \"\",getReturnWaterTemp(T215,AC215, activeEWTCooling, AS215, \"cooling\"))","v":""},"",{"$f":"IF($T215<>\"ACBC_1W\",\"\",IF($J215=\"\",\"\",FintubeCapacity($T215,$W215,$AE215,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T215=\"Select Model\",T215=\"PCBL\"),\"\",calcQwIP(Y215,W215,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD215,BD215,\"capacity\",U215&\"P\"&IF(V215=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T215,activeElevation))","v":""},"",{"$f":"IF(OR(T215=\"Select Model\",T215=\"PCBL\"), \"\",IF(AY215=0,\"N/A\",waterPressureDrop(W215, U215 & \"P\" & IF(V215=\"Dual\",2,1) &\"C\", AD215, \"heating\", T215)))","v":""},{"$f":"IF(OR(T215=\"Select Model\",T215=\"PCBL\"), \"\",IF(AY215=0,getReturnWaterTemp(T215,AE215, activeEWTHeating, AX215, \"heating\"),getReturnWaterTemp(T215,AD215, activeEWTHeating, AY215, \"heating\")))","v":""},"",{"$f":" getNozzle(T215, W215, Y215, Z215, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I216)),I216<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I216, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H216)),H216<0),\"\",intlEstQuantity(T216, W216*12, H216)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T216=\"Select Model\",\"\",coilCircuitChange(W216, U216, AC216, T216,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T216=\"Select Model\",\"\",beamWidth(T216))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T216=\"Select Model\",T216=\"PCBL\"), 0,getSPIP(T216, W216, Y216, BD216, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T216=\"Select Model\", \"\",IF(T216=\"PCBL\",0,primaryAirSensibleCapacityIP($T216,$W216,activeRoomTempCooling,activePriAirTempCooling,$Y216,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T216=\"Select Model\",\"\",IF($T216=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y216,activeElevation)))","v":""},{"$f":"IF(OR(T216=\"Select Model\",T216=\"PCBL\"), 0,IF(AD216=0,0,-primaryAirSensibleCapacityIP($T216,$W216,activeRoomTempHeating,activePriAirTempHeating,$Y216,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T216=\"Select Model\", \"\", InductionRatio($T216,BD216,$W216,$Y216)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T216=\"Select Model\", \"\",IF($T216=\"PCBL\",\"N/A\",minVAVSetBack(AA216, Y216))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T216=\"Select Model\", \"\",IF($T216= \"PCBL\",\"N/A\",getDischargeAirTemp($T216,$V216,$AC216,$W216,BD216,$AL216, $Y216, $AS216, \"cooling\",activeElevation,$AB216,$AJ216,$AV216,$BB216))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T216=\"Select Model\",$T216=\"PCBL\"), \"\",getDischargeAirTemp($T216,$V216,$AD216,$W216,BD216,$AL216, $Y216, $AY216, \"heating\",activeElevation,$AB216,$AJ216,$AV216,$BB216)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T216=\"Select Model\", \"\",IF(OR($T216=\"ACBC_1W\",$T216=\"ACBC_2W\",LEFT($T216,4)=\"ACBR\",$T216 = \"LIU24_2W\",LEFT($T216,3)=\"RIU\",LEFT($T216,6)=\"ACBL12\"), IF((soundLevel($T216, $AB216, BD216, $Y216, $W216,$AJ216,$AA216,\"dba\"))<15,\"<15\",soundLevel($T216, $AB216, BD216, $Y216, $W216,$AJ216,$AA216,\"dba\")+0.4),IF((soundLevel($T216, $AB216, BD216, $Y216, $W216,$AJ216,$AA216,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T216, $AB216, BD216, $Y216, $W216,$AJ216,$AA216,\"dba\")+5)<15, \"<15\", soundLevel($T216, $AB216, BD216,$Y216, $W216,$AJ216,$AA216,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T216=\"Select Model\", \"\",IF(OR($T216=\"ACBC_1W\",$T216=\"ACBC_2W\",LEFT($T216,4)=\"ACBR\",$T216=\"LIU24_2W\",LEFT($T216,3)=\"RIU\",LEFT($T216,6)=\"ACBL12\"), IF((soundLevel($T216, $AB216, BD216, $Y216, $W216,$AJ216,$AA216,\"NC\"))<15,\"<15\",soundLevel($T216, $AB216, BD216, $Y216, $W216,$AJ216,$AA216,\"NC\")+0.4),IF((soundLevel($T216, $AB216, BD216, $Y216, $W216,$AJ216,$AA216,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T216, $AB216, BD216, $Y216, $W216,$AJ216,$AA216,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T216, $AB216, BD216, $Y216, $W216,$AJ216,$AA216,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T216=\"Select Model\",\"\",IF($T216=\"LIU24_2W\",calcQwIP($Y216,$W216,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC216,$AI216,\"latent\",$U216&\"P\"&IF($V216=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T216,activeElevation),\"\"))","v":""},{"$f":"IF($T216=\"Select Model\",\"\",IF($T216=\"ACBC_1W\",calcQwIP($Y216,$W216,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC216,BD216,\"capacity\",$U216&\"P\"&IF($V216=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T216,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y216,$W216,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC216,BD216,\"capacity\",$U216&\"P\"&IF($V216=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T216,activeElevation)))","v":""},"",{"$f":"IF(T216=\"Select Model\", 0,waterPressureDrop(W216, U216 & \"P\" & IF(V216=\"Dual\",2,1) &\"C\", AC216, \"cooling\", T216))","v":0},{"$f":"IF(T216=\"Select Model\", \"\",getReturnWaterTemp(T216,AC216, activeEWTCooling, AS216, \"cooling\"))","v":""},"",{"$f":"IF($T216<>\"ACBC_1W\",\"\",IF($J216=\"\",\"\",FintubeCapacity($T216,$W216,$AE216,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T216=\"Select Model\",T216=\"PCBL\"),\"\",calcQwIP(Y216,W216,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD216,BD216,\"capacity\",U216&\"P\"&IF(V216=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T216,activeElevation))","v":""},"",{"$f":"IF(OR(T216=\"Select Model\",T216=\"PCBL\"), \"\",IF(AY216=0,\"N/A\",waterPressureDrop(W216, U216 & \"P\" & IF(V216=\"Dual\",2,1) &\"C\", AD216, \"heating\", T216)))","v":""},{"$f":"IF(OR(T216=\"Select Model\",T216=\"PCBL\"), \"\",IF(AY216=0,getReturnWaterTemp(T216,AE216, activeEWTHeating, AX216, \"heating\"),getReturnWaterTemp(T216,AD216, activeEWTHeating, AY216, \"heating\")))","v":""},"",{"$f":" getNozzle(T216, W216, Y216, Z216, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I217)),I217<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I217, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H217)),H217<0),\"\",intlEstQuantity(T217, W217*12, H217)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T217=\"Select Model\",\"\",coilCircuitChange(W217, U217, AC217, T217,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T217=\"Select Model\",\"\",beamWidth(T217))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T217=\"Select Model\",T217=\"PCBL\"), 0,getSPIP(T217, W217, Y217, BD217, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T217=\"Select Model\", \"\",IF(T217=\"PCBL\",0,primaryAirSensibleCapacityIP($T217,$W217,activeRoomTempCooling,activePriAirTempCooling,$Y217,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T217=\"Select Model\",\"\",IF($T217=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y217,activeElevation)))","v":""},{"$f":"IF(OR(T217=\"Select Model\",T217=\"PCBL\"), 0,IF(AD217=0,0,-primaryAirSensibleCapacityIP($T217,$W217,activeRoomTempHeating,activePriAirTempHeating,$Y217,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T217=\"Select Model\", \"\", InductionRatio($T217,BD217,$W217,$Y217)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T217=\"Select Model\", \"\",IF($T217=\"PCBL\",\"N/A\",minVAVSetBack(AA217, Y217))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T217=\"Select Model\", \"\",IF($T217= \"PCBL\",\"N/A\",getDischargeAirTemp($T217,$V217,$AC217,$W217,BD217,$AL217, $Y217, $AS217, \"cooling\",activeElevation,$AB217,$AJ217,$AV217,$BB217))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T217=\"Select Model\",$T217=\"PCBL\"), \"\",getDischargeAirTemp($T217,$V217,$AD217,$W217,BD217,$AL217, $Y217, $AY217, \"heating\",activeElevation,$AB217,$AJ217,$AV217,$BB217)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T217=\"Select Model\", \"\",IF(OR($T217=\"ACBC_1W\",$T217=\"ACBC_2W\",LEFT($T217,4)=\"ACBR\",$T217 = \"LIU24_2W\",LEFT($T217,3)=\"RIU\",LEFT($T217,6)=\"ACBL12\"), IF((soundLevel($T217, $AB217, BD217, $Y217, $W217,$AJ217,$AA217,\"dba\"))<15,\"<15\",soundLevel($T217, $AB217, BD217, $Y217, $W217,$AJ217,$AA217,\"dba\")+0.4),IF((soundLevel($T217, $AB217, BD217, $Y217, $W217,$AJ217,$AA217,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T217, $AB217, BD217, $Y217, $W217,$AJ217,$AA217,\"dba\")+5)<15, \"<15\", soundLevel($T217, $AB217, BD217,$Y217, $W217,$AJ217,$AA217,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T217=\"Select Model\", \"\",IF(OR($T217=\"ACBC_1W\",$T217=\"ACBC_2W\",LEFT($T217,4)=\"ACBR\",$T217=\"LIU24_2W\",LEFT($T217,3)=\"RIU\",LEFT($T217,6)=\"ACBL12\"), IF((soundLevel($T217, $AB217, BD217, $Y217, $W217,$AJ217,$AA217,\"NC\"))<15,\"<15\",soundLevel($T217, $AB217, BD217, $Y217, $W217,$AJ217,$AA217,\"NC\")+0.4),IF((soundLevel($T217, $AB217, BD217, $Y217, $W217,$AJ217,$AA217,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T217, $AB217, BD217, $Y217, $W217,$AJ217,$AA217,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T217, $AB217, BD217, $Y217, $W217,$AJ217,$AA217,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T217=\"Select Model\",\"\",IF($T217=\"LIU24_2W\",calcQwIP($Y217,$W217,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC217,$AI217,\"latent\",$U217&\"P\"&IF($V217=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T217,activeElevation),\"\"))","v":""},{"$f":"IF($T217=\"Select Model\",\"\",IF($T217=\"ACBC_1W\",calcQwIP($Y217,$W217,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC217,BD217,\"capacity\",$U217&\"P\"&IF($V217=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T217,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y217,$W217,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC217,BD217,\"capacity\",$U217&\"P\"&IF($V217=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T217,activeElevation)))","v":""},"",{"$f":"IF(T217=\"Select Model\", 0,waterPressureDrop(W217, U217 & \"P\" & IF(V217=\"Dual\",2,1) &\"C\", AC217, \"cooling\", T217))","v":0},{"$f":"IF(T217=\"Select Model\", \"\",getReturnWaterTemp(T217,AC217, activeEWTCooling, AS217, \"cooling\"))","v":""},"",{"$f":"IF($T217<>\"ACBC_1W\",\"\",IF($J217=\"\",\"\",FintubeCapacity($T217,$W217,$AE217,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T217=\"Select Model\",T217=\"PCBL\"),\"\",calcQwIP(Y217,W217,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD217,BD217,\"capacity\",U217&\"P\"&IF(V217=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T217,activeElevation))","v":""},"",{"$f":"IF(OR(T217=\"Select Model\",T217=\"PCBL\"), \"\",IF(AY217=0,\"N/A\",waterPressureDrop(W217, U217 & \"P\" & IF(V217=\"Dual\",2,1) &\"C\", AD217, \"heating\", T217)))","v":""},{"$f":"IF(OR(T217=\"Select Model\",T217=\"PCBL\"), \"\",IF(AY217=0,getReturnWaterTemp(T217,AE217, activeEWTHeating, AX217, \"heating\"),getReturnWaterTemp(T217,AD217, activeEWTHeating, AY217, \"heating\")))","v":""},"",{"$f":" getNozzle(T217, W217, Y217, Z217, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I218)),I218<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I218, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H218)),H218<0),\"\",intlEstQuantity(T218, W218*12, H218)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T218=\"Select Model\",\"\",coilCircuitChange(W218, U218, AC218, T218,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T218=\"Select Model\",\"\",beamWidth(T218))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T218=\"Select Model\",T218=\"PCBL\"), 0,getSPIP(T218, W218, Y218, BD218, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T218=\"Select Model\", \"\",IF(T218=\"PCBL\",0,primaryAirSensibleCapacityIP($T218,$W218,activeRoomTempCooling,activePriAirTempCooling,$Y218,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T218=\"Select Model\",\"\",IF($T218=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y218,activeElevation)))","v":""},{"$f":"IF(OR(T218=\"Select Model\",T218=\"PCBL\"), 0,IF(AD218=0,0,-primaryAirSensibleCapacityIP($T218,$W218,activeRoomTempHeating,activePriAirTempHeating,$Y218,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T218=\"Select Model\", \"\", InductionRatio($T218,BD218,$W218,$Y218)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T218=\"Select Model\", \"\",IF($T218=\"PCBL\",\"N/A\",minVAVSetBack(AA218, Y218))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T218=\"Select Model\", \"\",IF($T218= \"PCBL\",\"N/A\",getDischargeAirTemp($T218,$V218,$AC218,$W218,BD218,$AL218, $Y218, $AS218, \"cooling\",activeElevation,$AB218,$AJ218,$AV218,$BB218))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T218=\"Select Model\",$T218=\"PCBL\"), \"\",getDischargeAirTemp($T218,$V218,$AD218,$W218,BD218,$AL218, $Y218, $AY218, \"heating\",activeElevation,$AB218,$AJ218,$AV218,$BB218)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T218=\"Select Model\", \"\",IF(OR($T218=\"ACBC_1W\",$T218=\"ACBC_2W\",LEFT($T218,4)=\"ACBR\",$T218 = \"LIU24_2W\",LEFT($T218,3)=\"RIU\",LEFT($T218,6)=\"ACBL12\"), IF((soundLevel($T218, $AB218, BD218, $Y218, $W218,$AJ218,$AA218,\"dba\"))<15,\"<15\",soundLevel($T218, $AB218, BD218, $Y218, $W218,$AJ218,$AA218,\"dba\")+0.4),IF((soundLevel($T218, $AB218, BD218, $Y218, $W218,$AJ218,$AA218,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T218, $AB218, BD218, $Y218, $W218,$AJ218,$AA218,\"dba\")+5)<15, \"<15\", soundLevel($T218, $AB218, BD218,$Y218, $W218,$AJ218,$AA218,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T218=\"Select Model\", \"\",IF(OR($T218=\"ACBC_1W\",$T218=\"ACBC_2W\",LEFT($T218,4)=\"ACBR\",$T218=\"LIU24_2W\",LEFT($T218,3)=\"RIU\",LEFT($T218,6)=\"ACBL12\"), IF((soundLevel($T218, $AB218, BD218, $Y218, $W218,$AJ218,$AA218,\"NC\"))<15,\"<15\",soundLevel($T218, $AB218, BD218, $Y218, $W218,$AJ218,$AA218,\"NC\")+0.4),IF((soundLevel($T218, $AB218, BD218, $Y218, $W218,$AJ218,$AA218,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T218, $AB218, BD218, $Y218, $W218,$AJ218,$AA218,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T218, $AB218, BD218, $Y218, $W218,$AJ218,$AA218,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T218=\"Select Model\",\"\",IF($T218=\"LIU24_2W\",calcQwIP($Y218,$W218,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC218,$AI218,\"latent\",$U218&\"P\"&IF($V218=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T218,activeElevation),\"\"))","v":""},{"$f":"IF($T218=\"Select Model\",\"\",IF($T218=\"ACBC_1W\",calcQwIP($Y218,$W218,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC218,BD218,\"capacity\",$U218&\"P\"&IF($V218=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T218,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y218,$W218,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC218,BD218,\"capacity\",$U218&\"P\"&IF($V218=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T218,activeElevation)))","v":""},"",{"$f":"IF(T218=\"Select Model\", 0,waterPressureDrop(W218, U218 & \"P\" & IF(V218=\"Dual\",2,1) &\"C\", AC218, \"cooling\", T218))","v":0},{"$f":"IF(T218=\"Select Model\", \"\",getReturnWaterTemp(T218,AC218, activeEWTCooling, AS218, \"cooling\"))","v":""},"",{"$f":"IF($T218<>\"ACBC_1W\",\"\",IF($J218=\"\",\"\",FintubeCapacity($T218,$W218,$AE218,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T218=\"Select Model\",T218=\"PCBL\"),\"\",calcQwIP(Y218,W218,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD218,BD218,\"capacity\",U218&\"P\"&IF(V218=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T218,activeElevation))","v":""},"",{"$f":"IF(OR(T218=\"Select Model\",T218=\"PCBL\"), \"\",IF(AY218=0,\"N/A\",waterPressureDrop(W218, U218 & \"P\" & IF(V218=\"Dual\",2,1) &\"C\", AD218, \"heating\", T218)))","v":""},{"$f":"IF(OR(T218=\"Select Model\",T218=\"PCBL\"), \"\",IF(AY218=0,getReturnWaterTemp(T218,AE218, activeEWTHeating, AX218, \"heating\"),getReturnWaterTemp(T218,AD218, activeEWTHeating, AY218, \"heating\")))","v":""},"",{"$f":" getNozzle(T218, W218, Y218, Z218, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I219)),I219<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I219, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H219)),H219<0),\"\",intlEstQuantity(T219, W219*12, H219)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T219=\"Select Model\",\"\",coilCircuitChange(W219, U219, AC219, T219,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T219=\"Select Model\",\"\",beamWidth(T219))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T219=\"Select Model\",T219=\"PCBL\"), 0,getSPIP(T219, W219, Y219, BD219, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T219=\"Select Model\", \"\",IF(T219=\"PCBL\",0,primaryAirSensibleCapacityIP($T219,$W219,activeRoomTempCooling,activePriAirTempCooling,$Y219,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T219=\"Select Model\",\"\",IF($T219=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y219,activeElevation)))","v":""},{"$f":"IF(OR(T219=\"Select Model\",T219=\"PCBL\"), 0,IF(AD219=0,0,-primaryAirSensibleCapacityIP($T219,$W219,activeRoomTempHeating,activePriAirTempHeating,$Y219,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T219=\"Select Model\", \"\", InductionRatio($T219,BD219,$W219,$Y219)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T219=\"Select Model\", \"\",IF($T219=\"PCBL\",\"N/A\",minVAVSetBack(AA219, Y219))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T219=\"Select Model\", \"\",IF($T219= \"PCBL\",\"N/A\",getDischargeAirTemp($T219,$V219,$AC219,$W219,BD219,$AL219, $Y219, $AS219, \"cooling\",activeElevation,$AB219,$AJ219,$AV219,$BB219))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T219=\"Select Model\",$T219=\"PCBL\"), \"\",getDischargeAirTemp($T219,$V219,$AD219,$W219,BD219,$AL219, $Y219, $AY219, \"heating\",activeElevation,$AB219,$AJ219,$AV219,$BB219)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T219=\"Select Model\", \"\",IF(OR($T219=\"ACBC_1W\",$T219=\"ACBC_2W\",LEFT($T219,4)=\"ACBR\",$T219 = \"LIU24_2W\",LEFT($T219,3)=\"RIU\",LEFT($T219,6)=\"ACBL12\"), IF((soundLevel($T219, $AB219, BD219, $Y219, $W219,$AJ219,$AA219,\"dba\"))<15,\"<15\",soundLevel($T219, $AB219, BD219, $Y219, $W219,$AJ219,$AA219,\"dba\")+0.4),IF((soundLevel($T219, $AB219, BD219, $Y219, $W219,$AJ219,$AA219,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T219, $AB219, BD219, $Y219, $W219,$AJ219,$AA219,\"dba\")+5)<15, \"<15\", soundLevel($T219, $AB219, BD219,$Y219, $W219,$AJ219,$AA219,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T219=\"Select Model\", \"\",IF(OR($T219=\"ACBC_1W\",$T219=\"ACBC_2W\",LEFT($T219,4)=\"ACBR\",$T219=\"LIU24_2W\",LEFT($T219,3)=\"RIU\",LEFT($T219,6)=\"ACBL12\"), IF((soundLevel($T219, $AB219, BD219, $Y219, $W219,$AJ219,$AA219,\"NC\"))<15,\"<15\",soundLevel($T219, $AB219, BD219, $Y219, $W219,$AJ219,$AA219,\"NC\")+0.4),IF((soundLevel($T219, $AB219, BD219, $Y219, $W219,$AJ219,$AA219,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T219, $AB219, BD219, $Y219, $W219,$AJ219,$AA219,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T219, $AB219, BD219, $Y219, $W219,$AJ219,$AA219,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T219=\"Select Model\",\"\",IF($T219=\"LIU24_2W\",calcQwIP($Y219,$W219,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC219,$AI219,\"latent\",$U219&\"P\"&IF($V219=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T219,activeElevation),\"\"))","v":""},{"$f":"IF($T219=\"Select Model\",\"\",IF($T219=\"ACBC_1W\",calcQwIP($Y219,$W219,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC219,BD219,\"capacity\",$U219&\"P\"&IF($V219=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T219,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y219,$W219,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC219,BD219,\"capacity\",$U219&\"P\"&IF($V219=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T219,activeElevation)))","v":""},"",{"$f":"IF(T219=\"Select Model\", 0,waterPressureDrop(W219, U219 & \"P\" & IF(V219=\"Dual\",2,1) &\"C\", AC219, \"cooling\", T219))","v":0},{"$f":"IF(T219=\"Select Model\", \"\",getReturnWaterTemp(T219,AC219, activeEWTCooling, AS219, \"cooling\"))","v":""},"",{"$f":"IF($T219<>\"ACBC_1W\",\"\",IF($J219=\"\",\"\",FintubeCapacity($T219,$W219,$AE219,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T219=\"Select Model\",T219=\"PCBL\"),\"\",calcQwIP(Y219,W219,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD219,BD219,\"capacity\",U219&\"P\"&IF(V219=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T219,activeElevation))","v":""},"",{"$f":"IF(OR(T219=\"Select Model\",T219=\"PCBL\"), \"\",IF(AY219=0,\"N/A\",waterPressureDrop(W219, U219 & \"P\" & IF(V219=\"Dual\",2,1) &\"C\", AD219, \"heating\", T219)))","v":""},{"$f":"IF(OR(T219=\"Select Model\",T219=\"PCBL\"), \"\",IF(AY219=0,getReturnWaterTemp(T219,AE219, activeEWTHeating, AX219, \"heating\"),getReturnWaterTemp(T219,AD219, activeEWTHeating, AY219, \"heating\")))","v":""},"",{"$f":" getNozzle(T219, W219, Y219, Z219, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I220)),I220<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I220, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H220)),H220<0),\"\",intlEstQuantity(T220, W220*12, H220)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T220=\"Select Model\",\"\",coilCircuitChange(W220, U220, AC220, T220,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T220=\"Select Model\",\"\",beamWidth(T220))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T220=\"Select Model\",T220=\"PCBL\"), 0,getSPIP(T220, W220, Y220, BD220, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T220=\"Select Model\", \"\",IF(T220=\"PCBL\",0,primaryAirSensibleCapacityIP($T220,$W220,activeRoomTempCooling,activePriAirTempCooling,$Y220,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T220=\"Select Model\",\"\",IF($T220=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y220,activeElevation)))","v":""},{"$f":"IF(OR(T220=\"Select Model\",T220=\"PCBL\"), 0,IF(AD220=0,0,-primaryAirSensibleCapacityIP($T220,$W220,activeRoomTempHeating,activePriAirTempHeating,$Y220,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T220=\"Select Model\", \"\", InductionRatio($T220,BD220,$W220,$Y220)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T220=\"Select Model\", \"\",IF($T220=\"PCBL\",\"N/A\",minVAVSetBack(AA220, Y220))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T220=\"Select Model\", \"\",IF($T220= \"PCBL\",\"N/A\",getDischargeAirTemp($T220,$V220,$AC220,$W220,BD220,$AL220, $Y220, $AS220, \"cooling\",activeElevation,$AB220,$AJ220,$AV220,$BB220))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T220=\"Select Model\",$T220=\"PCBL\"), \"\",getDischargeAirTemp($T220,$V220,$AD220,$W220,BD220,$AL220, $Y220, $AY220, \"heating\",activeElevation,$AB220,$AJ220,$AV220,$BB220)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T220=\"Select Model\", \"\",IF(OR($T220=\"ACBC_1W\",$T220=\"ACBC_2W\",LEFT($T220,4)=\"ACBR\",$T220 = \"LIU24_2W\",LEFT($T220,3)=\"RIU\",LEFT($T220,6)=\"ACBL12\"), IF((soundLevel($T220, $AB220, BD220, $Y220, $W220,$AJ220,$AA220,\"dba\"))<15,\"<15\",soundLevel($T220, $AB220, BD220, $Y220, $W220,$AJ220,$AA220,\"dba\")+0.4),IF((soundLevel($T220, $AB220, BD220, $Y220, $W220,$AJ220,$AA220,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T220, $AB220, BD220, $Y220, $W220,$AJ220,$AA220,\"dba\")+5)<15, \"<15\", soundLevel($T220, $AB220, BD220,$Y220, $W220,$AJ220,$AA220,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T220=\"Select Model\", \"\",IF(OR($T220=\"ACBC_1W\",$T220=\"ACBC_2W\",LEFT($T220,4)=\"ACBR\",$T220=\"LIU24_2W\",LEFT($T220,3)=\"RIU\",LEFT($T220,6)=\"ACBL12\"), IF((soundLevel($T220, $AB220, BD220, $Y220, $W220,$AJ220,$AA220,\"NC\"))<15,\"<15\",soundLevel($T220, $AB220, BD220, $Y220, $W220,$AJ220,$AA220,\"NC\")+0.4),IF((soundLevel($T220, $AB220, BD220, $Y220, $W220,$AJ220,$AA220,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T220, $AB220, BD220, $Y220, $W220,$AJ220,$AA220,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T220, $AB220, BD220, $Y220, $W220,$AJ220,$AA220,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T220=\"Select Model\",\"\",IF($T220=\"LIU24_2W\",calcQwIP($Y220,$W220,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC220,$AI220,\"latent\",$U220&\"P\"&IF($V220=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T220,activeElevation),\"\"))","v":""},{"$f":"IF($T220=\"Select Model\",\"\",IF($T220=\"ACBC_1W\",calcQwIP($Y220,$W220,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC220,BD220,\"capacity\",$U220&\"P\"&IF($V220=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T220,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y220,$W220,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC220,BD220,\"capacity\",$U220&\"P\"&IF($V220=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T220,activeElevation)))","v":""},"",{"$f":"IF(T220=\"Select Model\", 0,waterPressureDrop(W220, U220 & \"P\" & IF(V220=\"Dual\",2,1) &\"C\", AC220, \"cooling\", T220))","v":0},{"$f":"IF(T220=\"Select Model\", \"\",getReturnWaterTemp(T220,AC220, activeEWTCooling, AS220, \"cooling\"))","v":""},"",{"$f":"IF($T220<>\"ACBC_1W\",\"\",IF($J220=\"\",\"\",FintubeCapacity($T220,$W220,$AE220,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T220=\"Select Model\",T220=\"PCBL\"),\"\",calcQwIP(Y220,W220,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD220,BD220,\"capacity\",U220&\"P\"&IF(V220=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T220,activeElevation))","v":""},"",{"$f":"IF(OR(T220=\"Select Model\",T220=\"PCBL\"), \"\",IF(AY220=0,\"N/A\",waterPressureDrop(W220, U220 & \"P\" & IF(V220=\"Dual\",2,1) &\"C\", AD220, \"heating\", T220)))","v":""},{"$f":"IF(OR(T220=\"Select Model\",T220=\"PCBL\"), \"\",IF(AY220=0,getReturnWaterTemp(T220,AE220, activeEWTHeating, AX220, \"heating\"),getReturnWaterTemp(T220,AD220, activeEWTHeating, AY220, \"heating\")))","v":""},"",{"$f":" getNozzle(T220, W220, Y220, Z220, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I221)),I221<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I221, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H221)),H221<0),\"\",intlEstQuantity(T221, W221*12, H221)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T221=\"Select Model\",\"\",coilCircuitChange(W221, U221, AC221, T221,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T221=\"Select Model\",\"\",beamWidth(T221))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T221=\"Select Model\",T221=\"PCBL\"), 0,getSPIP(T221, W221, Y221, BD221, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T221=\"Select Model\", \"\",IF(T221=\"PCBL\",0,primaryAirSensibleCapacityIP($T221,$W221,activeRoomTempCooling,activePriAirTempCooling,$Y221,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T221=\"Select Model\",\"\",IF($T221=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y221,activeElevation)))","v":""},{"$f":"IF(OR(T221=\"Select Model\",T221=\"PCBL\"), 0,IF(AD221=0,0,-primaryAirSensibleCapacityIP($T221,$W221,activeRoomTempHeating,activePriAirTempHeating,$Y221,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T221=\"Select Model\", \"\", InductionRatio($T221,BD221,$W221,$Y221)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T221=\"Select Model\", \"\",IF($T221=\"PCBL\",\"N/A\",minVAVSetBack(AA221, Y221))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T221=\"Select Model\", \"\",IF($T221= \"PCBL\",\"N/A\",getDischargeAirTemp($T221,$V221,$AC221,$W221,BD221,$AL221, $Y221, $AS221, \"cooling\",activeElevation,$AB221,$AJ221,$AV221,$BB221))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T221=\"Select Model\",$T221=\"PCBL\"), \"\",getDischargeAirTemp($T221,$V221,$AD221,$W221,BD221,$AL221, $Y221, $AY221, \"heating\",activeElevation,$AB221,$AJ221,$AV221,$BB221)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T221=\"Select Model\", \"\",IF(OR($T221=\"ACBC_1W\",$T221=\"ACBC_2W\",LEFT($T221,4)=\"ACBR\",$T221 = \"LIU24_2W\",LEFT($T221,3)=\"RIU\",LEFT($T221,6)=\"ACBL12\"), IF((soundLevel($T221, $AB221, BD221, $Y221, $W221,$AJ221,$AA221,\"dba\"))<15,\"<15\",soundLevel($T221, $AB221, BD221, $Y221, $W221,$AJ221,$AA221,\"dba\")+0.4),IF((soundLevel($T221, $AB221, BD221, $Y221, $W221,$AJ221,$AA221,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T221, $AB221, BD221, $Y221, $W221,$AJ221,$AA221,\"dba\")+5)<15, \"<15\", soundLevel($T221, $AB221, BD221,$Y221, $W221,$AJ221,$AA221,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T221=\"Select Model\", \"\",IF(OR($T221=\"ACBC_1W\",$T221=\"ACBC_2W\",LEFT($T221,4)=\"ACBR\",$T221=\"LIU24_2W\",LEFT($T221,3)=\"RIU\",LEFT($T221,6)=\"ACBL12\"), IF((soundLevel($T221, $AB221, BD221, $Y221, $W221,$AJ221,$AA221,\"NC\"))<15,\"<15\",soundLevel($T221, $AB221, BD221, $Y221, $W221,$AJ221,$AA221,\"NC\")+0.4),IF((soundLevel($T221, $AB221, BD221, $Y221, $W221,$AJ221,$AA221,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T221, $AB221, BD221, $Y221, $W221,$AJ221,$AA221,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T221, $AB221, BD221, $Y221, $W221,$AJ221,$AA221,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T221=\"Select Model\",\"\",IF($T221=\"LIU24_2W\",calcQwIP($Y221,$W221,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC221,$AI221,\"latent\",$U221&\"P\"&IF($V221=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T221,activeElevation),\"\"))","v":""},{"$f":"IF($T221=\"Select Model\",\"\",IF($T221=\"ACBC_1W\",calcQwIP($Y221,$W221,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC221,BD221,\"capacity\",$U221&\"P\"&IF($V221=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T221,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y221,$W221,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC221,BD221,\"capacity\",$U221&\"P\"&IF($V221=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T221,activeElevation)))","v":""},"",{"$f":"IF(T221=\"Select Model\", 0,waterPressureDrop(W221, U221 & \"P\" & IF(V221=\"Dual\",2,1) &\"C\", AC221, \"cooling\", T221))","v":0},{"$f":"IF(T221=\"Select Model\", \"\",getReturnWaterTemp(T221,AC221, activeEWTCooling, AS221, \"cooling\"))","v":""},"",{"$f":"IF($T221<>\"ACBC_1W\",\"\",IF($J221=\"\",\"\",FintubeCapacity($T221,$W221,$AE221,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T221=\"Select Model\",T221=\"PCBL\"),\"\",calcQwIP(Y221,W221,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD221,BD221,\"capacity\",U221&\"P\"&IF(V221=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T221,activeElevation))","v":""},"",{"$f":"IF(OR(T221=\"Select Model\",T221=\"PCBL\"), \"\",IF(AY221=0,\"N/A\",waterPressureDrop(W221, U221 & \"P\" & IF(V221=\"Dual\",2,1) &\"C\", AD221, \"heating\", T221)))","v":""},{"$f":"IF(OR(T221=\"Select Model\",T221=\"PCBL\"), \"\",IF(AY221=0,getReturnWaterTemp(T221,AE221, activeEWTHeating, AX221, \"heating\"),getReturnWaterTemp(T221,AD221, activeEWTHeating, AY221, \"heating\")))","v":""},"",{"$f":" getNozzle(T221, W221, Y221, Z221, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I222)),I222<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I222, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H222)),H222<0),\"\",intlEstQuantity(T222, W222*12, H222)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T222=\"Select Model\",\"\",coilCircuitChange(W222, U222, AC222, T222,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T222=\"Select Model\",\"\",beamWidth(T222))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T222=\"Select Model\",T222=\"PCBL\"), 0,getSPIP(T222, W222, Y222, BD222, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T222=\"Select Model\", \"\",IF(T222=\"PCBL\",0,primaryAirSensibleCapacityIP($T222,$W222,activeRoomTempCooling,activePriAirTempCooling,$Y222,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T222=\"Select Model\",\"\",IF($T222=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y222,activeElevation)))","v":""},{"$f":"IF(OR(T222=\"Select Model\",T222=\"PCBL\"), 0,IF(AD222=0,0,-primaryAirSensibleCapacityIP($T222,$W222,activeRoomTempHeating,activePriAirTempHeating,$Y222,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T222=\"Select Model\", \"\", InductionRatio($T222,BD222,$W222,$Y222)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T222=\"Select Model\", \"\",IF($T222=\"PCBL\",\"N/A\",minVAVSetBack(AA222, Y222))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T222=\"Select Model\", \"\",IF($T222= \"PCBL\",\"N/A\",getDischargeAirTemp($T222,$V222,$AC222,$W222,BD222,$AL222, $Y222, $AS222, \"cooling\",activeElevation,$AB222,$AJ222,$AV222,$BB222))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T222=\"Select Model\",$T222=\"PCBL\"), \"\",getDischargeAirTemp($T222,$V222,$AD222,$W222,BD222,$AL222, $Y222, $AY222, \"heating\",activeElevation,$AB222,$AJ222,$AV222,$BB222)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T222=\"Select Model\", \"\",IF(OR($T222=\"ACBC_1W\",$T222=\"ACBC_2W\",LEFT($T222,4)=\"ACBR\",$T222 = \"LIU24_2W\",LEFT($T222,3)=\"RIU\",LEFT($T222,6)=\"ACBL12\"), IF((soundLevel($T222, $AB222, BD222, $Y222, $W222,$AJ222,$AA222,\"dba\"))<15,\"<15\",soundLevel($T222, $AB222, BD222, $Y222, $W222,$AJ222,$AA222,\"dba\")+0.4),IF((soundLevel($T222, $AB222, BD222, $Y222, $W222,$AJ222,$AA222,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T222, $AB222, BD222, $Y222, $W222,$AJ222,$AA222,\"dba\")+5)<15, \"<15\", soundLevel($T222, $AB222, BD222,$Y222, $W222,$AJ222,$AA222,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T222=\"Select Model\", \"\",IF(OR($T222=\"ACBC_1W\",$T222=\"ACBC_2W\",LEFT($T222,4)=\"ACBR\",$T222=\"LIU24_2W\",LEFT($T222,3)=\"RIU\",LEFT($T222,6)=\"ACBL12\"), IF((soundLevel($T222, $AB222, BD222, $Y222, $W222,$AJ222,$AA222,\"NC\"))<15,\"<15\",soundLevel($T222, $AB222, BD222, $Y222, $W222,$AJ222,$AA222,\"NC\")+0.4),IF((soundLevel($T222, $AB222, BD222, $Y222, $W222,$AJ222,$AA222,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T222, $AB222, BD222, $Y222, $W222,$AJ222,$AA222,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T222, $AB222, BD222, $Y222, $W222,$AJ222,$AA222,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T222=\"Select Model\",\"\",IF($T222=\"LIU24_2W\",calcQwIP($Y222,$W222,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC222,$AI222,\"latent\",$U222&\"P\"&IF($V222=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T222,activeElevation),\"\"))","v":""},{"$f":"IF($T222=\"Select Model\",\"\",IF($T222=\"ACBC_1W\",calcQwIP($Y222,$W222,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC222,BD222,\"capacity\",$U222&\"P\"&IF($V222=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T222,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y222,$W222,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC222,BD222,\"capacity\",$U222&\"P\"&IF($V222=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T222,activeElevation)))","v":""},"",{"$f":"IF(T222=\"Select Model\", 0,waterPressureDrop(W222, U222 & \"P\" & IF(V222=\"Dual\",2,1) &\"C\", AC222, \"cooling\", T222))","v":0},{"$f":"IF(T222=\"Select Model\", \"\",getReturnWaterTemp(T222,AC222, activeEWTCooling, AS222, \"cooling\"))","v":""},"",{"$f":"IF($T222<>\"ACBC_1W\",\"\",IF($J222=\"\",\"\",FintubeCapacity($T222,$W222,$AE222,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T222=\"Select Model\",T222=\"PCBL\"),\"\",calcQwIP(Y222,W222,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD222,BD222,\"capacity\",U222&\"P\"&IF(V222=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T222,activeElevation))","v":""},"",{"$f":"IF(OR(T222=\"Select Model\",T222=\"PCBL\"), \"\",IF(AY222=0,\"N/A\",waterPressureDrop(W222, U222 & \"P\" & IF(V222=\"Dual\",2,1) &\"C\", AD222, \"heating\", T222)))","v":""},{"$f":"IF(OR(T222=\"Select Model\",T222=\"PCBL\"), \"\",IF(AY222=0,getReturnWaterTemp(T222,AE222, activeEWTHeating, AX222, \"heating\"),getReturnWaterTemp(T222,AD222, activeEWTHeating, AY222, \"heating\")))","v":""},"",{"$f":" getNozzle(T222, W222, Y222, Z222, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I223)),I223<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I223, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H223)),H223<0),\"\",intlEstQuantity(T223, W223*12, H223)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T223=\"Select Model\",\"\",coilCircuitChange(W223, U223, AC223, T223,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T223=\"Select Model\",\"\",beamWidth(T223))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T223=\"Select Model\",T223=\"PCBL\"), 0,getSPIP(T223, W223, Y223, BD223, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T223=\"Select Model\", \"\",IF(T223=\"PCBL\",0,primaryAirSensibleCapacityIP($T223,$W223,activeRoomTempCooling,activePriAirTempCooling,$Y223,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T223=\"Select Model\",\"\",IF($T223=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y223,activeElevation)))","v":""},{"$f":"IF(OR(T223=\"Select Model\",T223=\"PCBL\"), 0,IF(AD223=0,0,-primaryAirSensibleCapacityIP($T223,$W223,activeRoomTempHeating,activePriAirTempHeating,$Y223,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T223=\"Select Model\", \"\", InductionRatio($T223,BD223,$W223,$Y223)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T223=\"Select Model\", \"\",IF($T223=\"PCBL\",\"N/A\",minVAVSetBack(AA223, Y223))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T223=\"Select Model\", \"\",IF($T223= \"PCBL\",\"N/A\",getDischargeAirTemp($T223,$V223,$AC223,$W223,BD223,$AL223, $Y223, $AS223, \"cooling\",activeElevation,$AB223,$AJ223,$AV223,$BB223))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T223=\"Select Model\",$T223=\"PCBL\"), \"\",getDischargeAirTemp($T223,$V223,$AD223,$W223,BD223,$AL223, $Y223, $AY223, \"heating\",activeElevation,$AB223,$AJ223,$AV223,$BB223)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T223=\"Select Model\", \"\",IF(OR($T223=\"ACBC_1W\",$T223=\"ACBC_2W\",LEFT($T223,4)=\"ACBR\",$T223 = \"LIU24_2W\",LEFT($T223,3)=\"RIU\",LEFT($T223,6)=\"ACBL12\"), IF((soundLevel($T223, $AB223, BD223, $Y223, $W223,$AJ223,$AA223,\"dba\"))<15,\"<15\",soundLevel($T223, $AB223, BD223, $Y223, $W223,$AJ223,$AA223,\"dba\")+0.4),IF((soundLevel($T223, $AB223, BD223, $Y223, $W223,$AJ223,$AA223,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T223, $AB223, BD223, $Y223, $W223,$AJ223,$AA223,\"dba\")+5)<15, \"<15\", soundLevel($T223, $AB223, BD223,$Y223, $W223,$AJ223,$AA223,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T223=\"Select Model\", \"\",IF(OR($T223=\"ACBC_1W\",$T223=\"ACBC_2W\",LEFT($T223,4)=\"ACBR\",$T223=\"LIU24_2W\",LEFT($T223,3)=\"RIU\",LEFT($T223,6)=\"ACBL12\"), IF((soundLevel($T223, $AB223, BD223, $Y223, $W223,$AJ223,$AA223,\"NC\"))<15,\"<15\",soundLevel($T223, $AB223, BD223, $Y223, $W223,$AJ223,$AA223,\"NC\")+0.4),IF((soundLevel($T223, $AB223, BD223, $Y223, $W223,$AJ223,$AA223,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T223, $AB223, BD223, $Y223, $W223,$AJ223,$AA223,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T223, $AB223, BD223, $Y223, $W223,$AJ223,$AA223,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T223=\"Select Model\",\"\",IF($T223=\"LIU24_2W\",calcQwIP($Y223,$W223,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC223,$AI223,\"latent\",$U223&\"P\"&IF($V223=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T223,activeElevation),\"\"))","v":""},{"$f":"IF($T223=\"Select Model\",\"\",IF($T223=\"ACBC_1W\",calcQwIP($Y223,$W223,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC223,BD223,\"capacity\",$U223&\"P\"&IF($V223=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T223,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y223,$W223,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC223,BD223,\"capacity\",$U223&\"P\"&IF($V223=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T223,activeElevation)))","v":""},"",{"$f":"IF(T223=\"Select Model\", 0,waterPressureDrop(W223, U223 & \"P\" & IF(V223=\"Dual\",2,1) &\"C\", AC223, \"cooling\", T223))","v":0},{"$f":"IF(T223=\"Select Model\", \"\",getReturnWaterTemp(T223,AC223, activeEWTCooling, AS223, \"cooling\"))","v":""},"",{"$f":"IF($T223<>\"ACBC_1W\",\"\",IF($J223=\"\",\"\",FintubeCapacity($T223,$W223,$AE223,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T223=\"Select Model\",T223=\"PCBL\"),\"\",calcQwIP(Y223,W223,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD223,BD223,\"capacity\",U223&\"P\"&IF(V223=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T223,activeElevation))","v":""},"",{"$f":"IF(OR(T223=\"Select Model\",T223=\"PCBL\"), \"\",IF(AY223=0,\"N/A\",waterPressureDrop(W223, U223 & \"P\" & IF(V223=\"Dual\",2,1) &\"C\", AD223, \"heating\", T223)))","v":""},{"$f":"IF(OR(T223=\"Select Model\",T223=\"PCBL\"), \"\",IF(AY223=0,getReturnWaterTemp(T223,AE223, activeEWTHeating, AX223, \"heating\"),getReturnWaterTemp(T223,AD223, activeEWTHeating, AY223, \"heating\")))","v":""},"",{"$f":" getNozzle(T223, W223, Y223, Z223, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I224)),I224<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I224, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H224)),H224<0),\"\",intlEstQuantity(T224, W224*12, H224)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T224=\"Select Model\",\"\",coilCircuitChange(W224, U224, AC224, T224,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T224=\"Select Model\",\"\",beamWidth(T224))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T224=\"Select Model\",T224=\"PCBL\"), 0,getSPIP(T224, W224, Y224, BD224, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T224=\"Select Model\", \"\",IF(T224=\"PCBL\",0,primaryAirSensibleCapacityIP($T224,$W224,activeRoomTempCooling,activePriAirTempCooling,$Y224,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T224=\"Select Model\",\"\",IF($T224=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y224,activeElevation)))","v":""},{"$f":"IF(OR(T224=\"Select Model\",T224=\"PCBL\"), 0,IF(AD224=0,0,-primaryAirSensibleCapacityIP($T224,$W224,activeRoomTempHeating,activePriAirTempHeating,$Y224,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T224=\"Select Model\", \"\", InductionRatio($T224,BD224,$W224,$Y224)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T224=\"Select Model\", \"\",IF($T224=\"PCBL\",\"N/A\",minVAVSetBack(AA224, Y224))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T224=\"Select Model\", \"\",IF($T224= \"PCBL\",\"N/A\",getDischargeAirTemp($T224,$V224,$AC224,$W224,BD224,$AL224, $Y224, $AS224, \"cooling\",activeElevation,$AB224,$AJ224,$AV224,$BB224))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T224=\"Select Model\",$T224=\"PCBL\"), \"\",getDischargeAirTemp($T224,$V224,$AD224,$W224,BD224,$AL224, $Y224, $AY224, \"heating\",activeElevation,$AB224,$AJ224,$AV224,$BB224)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T224=\"Select Model\", \"\",IF(OR($T224=\"ACBC_1W\",$T224=\"ACBC_2W\",LEFT($T224,4)=\"ACBR\",$T224 = \"LIU24_2W\",LEFT($T224,3)=\"RIU\",LEFT($T224,6)=\"ACBL12\"), IF((soundLevel($T224, $AB224, BD224, $Y224, $W224,$AJ224,$AA224,\"dba\"))<15,\"<15\",soundLevel($T224, $AB224, BD224, $Y224, $W224,$AJ224,$AA224,\"dba\")+0.4),IF((soundLevel($T224, $AB224, BD224, $Y224, $W224,$AJ224,$AA224,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T224, $AB224, BD224, $Y224, $W224,$AJ224,$AA224,\"dba\")+5)<15, \"<15\", soundLevel($T224, $AB224, BD224,$Y224, $W224,$AJ224,$AA224,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T224=\"Select Model\", \"\",IF(OR($T224=\"ACBC_1W\",$T224=\"ACBC_2W\",LEFT($T224,4)=\"ACBR\",$T224=\"LIU24_2W\",LEFT($T224,3)=\"RIU\",LEFT($T224,6)=\"ACBL12\"), IF((soundLevel($T224, $AB224, BD224, $Y224, $W224,$AJ224,$AA224,\"NC\"))<15,\"<15\",soundLevel($T224, $AB224, BD224, $Y224, $W224,$AJ224,$AA224,\"NC\")+0.4),IF((soundLevel($T224, $AB224, BD224, $Y224, $W224,$AJ224,$AA224,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T224, $AB224, BD224, $Y224, $W224,$AJ224,$AA224,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T224, $AB224, BD224, $Y224, $W224,$AJ224,$AA224,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T224=\"Select Model\",\"\",IF($T224=\"LIU24_2W\",calcQwIP($Y224,$W224,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC224,$AI224,\"latent\",$U224&\"P\"&IF($V224=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T224,activeElevation),\"\"))","v":""},{"$f":"IF($T224=\"Select Model\",\"\",IF($T224=\"ACBC_1W\",calcQwIP($Y224,$W224,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC224,BD224,\"capacity\",$U224&\"P\"&IF($V224=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T224,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y224,$W224,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC224,BD224,\"capacity\",$U224&\"P\"&IF($V224=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T224,activeElevation)))","v":""},"",{"$f":"IF(T224=\"Select Model\", 0,waterPressureDrop(W224, U224 & \"P\" & IF(V224=\"Dual\",2,1) &\"C\", AC224, \"cooling\", T224))","v":0},{"$f":"IF(T224=\"Select Model\", \"\",getReturnWaterTemp(T224,AC224, activeEWTCooling, AS224, \"cooling\"))","v":""},"",{"$f":"IF($T224<>\"ACBC_1W\",\"\",IF($J224=\"\",\"\",FintubeCapacity($T224,$W224,$AE224,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T224=\"Select Model\",T224=\"PCBL\"),\"\",calcQwIP(Y224,W224,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD224,BD224,\"capacity\",U224&\"P\"&IF(V224=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T224,activeElevation))","v":""},"",{"$f":"IF(OR(T224=\"Select Model\",T224=\"PCBL\"), \"\",IF(AY224=0,\"N/A\",waterPressureDrop(W224, U224 & \"P\" & IF(V224=\"Dual\",2,1) &\"C\", AD224, \"heating\", T224)))","v":""},{"$f":"IF(OR(T224=\"Select Model\",T224=\"PCBL\"), \"\",IF(AY224=0,getReturnWaterTemp(T224,AE224, activeEWTHeating, AX224, \"heating\"),getReturnWaterTemp(T224,AD224, activeEWTHeating, AY224, \"heating\")))","v":""},"",{"$f":" getNozzle(T224, W224, Y224, Z224, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I225)),I225<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I225, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H225)),H225<0),\"\",intlEstQuantity(T225, W225*12, H225)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T225=\"Select Model\",\"\",coilCircuitChange(W225, U225, AC225, T225,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T225=\"Select Model\",\"\",beamWidth(T225))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T225=\"Select Model\",T225=\"PCBL\"), 0,getSPIP(T225, W225, Y225, BD225, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T225=\"Select Model\", \"\",IF(T225=\"PCBL\",0,primaryAirSensibleCapacityIP($T225,$W225,activeRoomTempCooling,activePriAirTempCooling,$Y225,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T225=\"Select Model\",\"\",IF($T225=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y225,activeElevation)))","v":""},{"$f":"IF(OR(T225=\"Select Model\",T225=\"PCBL\"), 0,IF(AD225=0,0,-primaryAirSensibleCapacityIP($T225,$W225,activeRoomTempHeating,activePriAirTempHeating,$Y225,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T225=\"Select Model\", \"\", InductionRatio($T225,BD225,$W225,$Y225)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T225=\"Select Model\", \"\",IF($T225=\"PCBL\",\"N/A\",minVAVSetBack(AA225, Y225))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T225=\"Select Model\", \"\",IF($T225= \"PCBL\",\"N/A\",getDischargeAirTemp($T225,$V225,$AC225,$W225,BD225,$AL225, $Y225, $AS225, \"cooling\",activeElevation,$AB225,$AJ225,$AV225,$BB225))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T225=\"Select Model\",$T225=\"PCBL\"), \"\",getDischargeAirTemp($T225,$V225,$AD225,$W225,BD225,$AL225, $Y225, $AY225, \"heating\",activeElevation,$AB225,$AJ225,$AV225,$BB225)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T225=\"Select Model\", \"\",IF(OR($T225=\"ACBC_1W\",$T225=\"ACBC_2W\",LEFT($T225,4)=\"ACBR\",$T225 = \"LIU24_2W\",LEFT($T225,3)=\"RIU\",LEFT($T225,6)=\"ACBL12\"), IF((soundLevel($T225, $AB225, BD225, $Y225, $W225,$AJ225,$AA225,\"dba\"))<15,\"<15\",soundLevel($T225, $AB225, BD225, $Y225, $W225,$AJ225,$AA225,\"dba\")+0.4),IF((soundLevel($T225, $AB225, BD225, $Y225, $W225,$AJ225,$AA225,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T225, $AB225, BD225, $Y225, $W225,$AJ225,$AA225,\"dba\")+5)<15, \"<15\", soundLevel($T225, $AB225, BD225,$Y225, $W225,$AJ225,$AA225,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T225=\"Select Model\", \"\",IF(OR($T225=\"ACBC_1W\",$T225=\"ACBC_2W\",LEFT($T225,4)=\"ACBR\",$T225=\"LIU24_2W\",LEFT($T225,3)=\"RIU\",LEFT($T225,6)=\"ACBL12\"), IF((soundLevel($T225, $AB225, BD225, $Y225, $W225,$AJ225,$AA225,\"NC\"))<15,\"<15\",soundLevel($T225, $AB225, BD225, $Y225, $W225,$AJ225,$AA225,\"NC\")+0.4),IF((soundLevel($T225, $AB225, BD225, $Y225, $W225,$AJ225,$AA225,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T225, $AB225, BD225, $Y225, $W225,$AJ225,$AA225,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T225, $AB225, BD225, $Y225, $W225,$AJ225,$AA225,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T225=\"Select Model\",\"\",IF($T225=\"LIU24_2W\",calcQwIP($Y225,$W225,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC225,$AI225,\"latent\",$U225&\"P\"&IF($V225=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T225,activeElevation),\"\"))","v":""},{"$f":"IF($T225=\"Select Model\",\"\",IF($T225=\"ACBC_1W\",calcQwIP($Y225,$W225,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC225,BD225,\"capacity\",$U225&\"P\"&IF($V225=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T225,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y225,$W225,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC225,BD225,\"capacity\",$U225&\"P\"&IF($V225=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T225,activeElevation)))","v":""},"",{"$f":"IF(T225=\"Select Model\", 0,waterPressureDrop(W225, U225 & \"P\" & IF(V225=\"Dual\",2,1) &\"C\", AC225, \"cooling\", T225))","v":0},{"$f":"IF(T225=\"Select Model\", \"\",getReturnWaterTemp(T225,AC225, activeEWTCooling, AS225, \"cooling\"))","v":""},"",{"$f":"IF($T225<>\"ACBC_1W\",\"\",IF($J225=\"\",\"\",FintubeCapacity($T225,$W225,$AE225,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T225=\"Select Model\",T225=\"PCBL\"),\"\",calcQwIP(Y225,W225,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD225,BD225,\"capacity\",U225&\"P\"&IF(V225=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T225,activeElevation))","v":""},"",{"$f":"IF(OR(T225=\"Select Model\",T225=\"PCBL\"), \"\",IF(AY225=0,\"N/A\",waterPressureDrop(W225, U225 & \"P\" & IF(V225=\"Dual\",2,1) &\"C\", AD225, \"heating\", T225)))","v":""},{"$f":"IF(OR(T225=\"Select Model\",T225=\"PCBL\"), \"\",IF(AY225=0,getReturnWaterTemp(T225,AE225, activeEWTHeating, AX225, \"heating\"),getReturnWaterTemp(T225,AD225, activeEWTHeating, AY225, \"heating\")))","v":""},"",{"$f":" getNozzle(T225, W225, Y225, Z225, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I226)),I226<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I226, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H226)),H226<0),\"\",intlEstQuantity(T226, W226*12, H226)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T226=\"Select Model\",\"\",coilCircuitChange(W226, U226, AC226, T226,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T226=\"Select Model\",\"\",beamWidth(T226))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T226=\"Select Model\",T226=\"PCBL\"), 0,getSPIP(T226, W226, Y226, BD226, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T226=\"Select Model\", \"\",IF(T226=\"PCBL\",0,primaryAirSensibleCapacityIP($T226,$W226,activeRoomTempCooling,activePriAirTempCooling,$Y226,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T226=\"Select Model\",\"\",IF($T226=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y226,activeElevation)))","v":""},{"$f":"IF(OR(T226=\"Select Model\",T226=\"PCBL\"), 0,IF(AD226=0,0,-primaryAirSensibleCapacityIP($T226,$W226,activeRoomTempHeating,activePriAirTempHeating,$Y226,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T226=\"Select Model\", \"\", InductionRatio($T226,BD226,$W226,$Y226)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T226=\"Select Model\", \"\",IF($T226=\"PCBL\",\"N/A\",minVAVSetBack(AA226, Y226))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T226=\"Select Model\", \"\",IF($T226= \"PCBL\",\"N/A\",getDischargeAirTemp($T226,$V226,$AC226,$W226,BD226,$AL226, $Y226, $AS226, \"cooling\",activeElevation,$AB226,$AJ226,$AV226,$BB226))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T226=\"Select Model\",$T226=\"PCBL\"), \"\",getDischargeAirTemp($T226,$V226,$AD226,$W226,BD226,$AL226, $Y226, $AY226, \"heating\",activeElevation,$AB226,$AJ226,$AV226,$BB226)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T226=\"Select Model\", \"\",IF(OR($T226=\"ACBC_1W\",$T226=\"ACBC_2W\",LEFT($T226,4)=\"ACBR\",$T226 = \"LIU24_2W\",LEFT($T226,3)=\"RIU\",LEFT($T226,6)=\"ACBL12\"), IF((soundLevel($T226, $AB226, BD226, $Y226, $W226,$AJ226,$AA226,\"dba\"))<15,\"<15\",soundLevel($T226, $AB226, BD226, $Y226, $W226,$AJ226,$AA226,\"dba\")+0.4),IF((soundLevel($T226, $AB226, BD226, $Y226, $W226,$AJ226,$AA226,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T226, $AB226, BD226, $Y226, $W226,$AJ226,$AA226,\"dba\")+5)<15, \"<15\", soundLevel($T226, $AB226, BD226,$Y226, $W226,$AJ226,$AA226,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T226=\"Select Model\", \"\",IF(OR($T226=\"ACBC_1W\",$T226=\"ACBC_2W\",LEFT($T226,4)=\"ACBR\",$T226=\"LIU24_2W\",LEFT($T226,3)=\"RIU\",LEFT($T226,6)=\"ACBL12\"), IF((soundLevel($T226, $AB226, BD226, $Y226, $W226,$AJ226,$AA226,\"NC\"))<15,\"<15\",soundLevel($T226, $AB226, BD226, $Y226, $W226,$AJ226,$AA226,\"NC\")+0.4),IF((soundLevel($T226, $AB226, BD226, $Y226, $W226,$AJ226,$AA226,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T226, $AB226, BD226, $Y226, $W226,$AJ226,$AA226,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T226, $AB226, BD226, $Y226, $W226,$AJ226,$AA226,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T226=\"Select Model\",\"\",IF($T226=\"LIU24_2W\",calcQwIP($Y226,$W226,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC226,$AI226,\"latent\",$U226&\"P\"&IF($V226=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T226,activeElevation),\"\"))","v":""},{"$f":"IF($T226=\"Select Model\",\"\",IF($T226=\"ACBC_1W\",calcQwIP($Y226,$W226,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC226,BD226,\"capacity\",$U226&\"P\"&IF($V226=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T226,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y226,$W226,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC226,BD226,\"capacity\",$U226&\"P\"&IF($V226=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T226,activeElevation)))","v":""},"",{"$f":"IF(T226=\"Select Model\", 0,waterPressureDrop(W226, U226 & \"P\" & IF(V226=\"Dual\",2,1) &\"C\", AC226, \"cooling\", T226))","v":0},{"$f":"IF(T226=\"Select Model\", \"\",getReturnWaterTemp(T226,AC226, activeEWTCooling, AS226, \"cooling\"))","v":""},"",{"$f":"IF($T226<>\"ACBC_1W\",\"\",IF($J226=\"\",\"\",FintubeCapacity($T226,$W226,$AE226,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T226=\"Select Model\",T226=\"PCBL\"),\"\",calcQwIP(Y226,W226,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD226,BD226,\"capacity\",U226&\"P\"&IF(V226=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T226,activeElevation))","v":""},"",{"$f":"IF(OR(T226=\"Select Model\",T226=\"PCBL\"), \"\",IF(AY226=0,\"N/A\",waterPressureDrop(W226, U226 & \"P\" & IF(V226=\"Dual\",2,1) &\"C\", AD226, \"heating\", T226)))","v":""},{"$f":"IF(OR(T226=\"Select Model\",T226=\"PCBL\"), \"\",IF(AY226=0,getReturnWaterTemp(T226,AE226, activeEWTHeating, AX226, \"heating\"),getReturnWaterTemp(T226,AD226, activeEWTHeating, AY226, \"heating\")))","v":""},"",{"$f":" getNozzle(T226, W226, Y226, Z226, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I227)),I227<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I227, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H227)),H227<0),\"\",intlEstQuantity(T227, W227*12, H227)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T227=\"Select Model\",\"\",coilCircuitChange(W227, U227, AC227, T227,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T227=\"Select Model\",\"\",beamWidth(T227))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T227=\"Select Model\",T227=\"PCBL\"), 0,getSPIP(T227, W227, Y227, BD227, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T227=\"Select Model\", \"\",IF(T227=\"PCBL\",0,primaryAirSensibleCapacityIP($T227,$W227,activeRoomTempCooling,activePriAirTempCooling,$Y227,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T227=\"Select Model\",\"\",IF($T227=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y227,activeElevation)))","v":""},{"$f":"IF(OR(T227=\"Select Model\",T227=\"PCBL\"), 0,IF(AD227=0,0,-primaryAirSensibleCapacityIP($T227,$W227,activeRoomTempHeating,activePriAirTempHeating,$Y227,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T227=\"Select Model\", \"\", InductionRatio($T227,BD227,$W227,$Y227)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T227=\"Select Model\", \"\",IF($T227=\"PCBL\",\"N/A\",minVAVSetBack(AA227, Y227))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T227=\"Select Model\", \"\",IF($T227= \"PCBL\",\"N/A\",getDischargeAirTemp($T227,$V227,$AC227,$W227,BD227,$AL227, $Y227, $AS227, \"cooling\",activeElevation,$AB227,$AJ227,$AV227,$BB227))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T227=\"Select Model\",$T227=\"PCBL\"), \"\",getDischargeAirTemp($T227,$V227,$AD227,$W227,BD227,$AL227, $Y227, $AY227, \"heating\",activeElevation,$AB227,$AJ227,$AV227,$BB227)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T227=\"Select Model\", \"\",IF(OR($T227=\"ACBC_1W\",$T227=\"ACBC_2W\",LEFT($T227,4)=\"ACBR\",$T227 = \"LIU24_2W\",LEFT($T227,3)=\"RIU\",LEFT($T227,6)=\"ACBL12\"), IF((soundLevel($T227, $AB227, BD227, $Y227, $W227,$AJ227,$AA227,\"dba\"))<15,\"<15\",soundLevel($T227, $AB227, BD227, $Y227, $W227,$AJ227,$AA227,\"dba\")+0.4),IF((soundLevel($T227, $AB227, BD227, $Y227, $W227,$AJ227,$AA227,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T227, $AB227, BD227, $Y227, $W227,$AJ227,$AA227,\"dba\")+5)<15, \"<15\", soundLevel($T227, $AB227, BD227,$Y227, $W227,$AJ227,$AA227,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T227=\"Select Model\", \"\",IF(OR($T227=\"ACBC_1W\",$T227=\"ACBC_2W\",LEFT($T227,4)=\"ACBR\",$T227=\"LIU24_2W\",LEFT($T227,3)=\"RIU\",LEFT($T227,6)=\"ACBL12\"), IF((soundLevel($T227, $AB227, BD227, $Y227, $W227,$AJ227,$AA227,\"NC\"))<15,\"<15\",soundLevel($T227, $AB227, BD227, $Y227, $W227,$AJ227,$AA227,\"NC\")+0.4),IF((soundLevel($T227, $AB227, BD227, $Y227, $W227,$AJ227,$AA227,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T227, $AB227, BD227, $Y227, $W227,$AJ227,$AA227,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T227, $AB227, BD227, $Y227, $W227,$AJ227,$AA227,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T227=\"Select Model\",\"\",IF($T227=\"LIU24_2W\",calcQwIP($Y227,$W227,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC227,$AI227,\"latent\",$U227&\"P\"&IF($V227=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T227,activeElevation),\"\"))","v":""},{"$f":"IF($T227=\"Select Model\",\"\",IF($T227=\"ACBC_1W\",calcQwIP($Y227,$W227,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC227,BD227,\"capacity\",$U227&\"P\"&IF($V227=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T227,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y227,$W227,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC227,BD227,\"capacity\",$U227&\"P\"&IF($V227=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T227,activeElevation)))","v":""},"",{"$f":"IF(T227=\"Select Model\", 0,waterPressureDrop(W227, U227 & \"P\" & IF(V227=\"Dual\",2,1) &\"C\", AC227, \"cooling\", T227))","v":0},{"$f":"IF(T227=\"Select Model\", \"\",getReturnWaterTemp(T227,AC227, activeEWTCooling, AS227, \"cooling\"))","v":""},"",{"$f":"IF($T227<>\"ACBC_1W\",\"\",IF($J227=\"\",\"\",FintubeCapacity($T227,$W227,$AE227,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T227=\"Select Model\",T227=\"PCBL\"),\"\",calcQwIP(Y227,W227,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD227,BD227,\"capacity\",U227&\"P\"&IF(V227=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T227,activeElevation))","v":""},"",{"$f":"IF(OR(T227=\"Select Model\",T227=\"PCBL\"), \"\",IF(AY227=0,\"N/A\",waterPressureDrop(W227, U227 & \"P\" & IF(V227=\"Dual\",2,1) &\"C\", AD227, \"heating\", T227)))","v":""},{"$f":"IF(OR(T227=\"Select Model\",T227=\"PCBL\"), \"\",IF(AY227=0,getReturnWaterTemp(T227,AE227, activeEWTHeating, AX227, \"heating\"),getReturnWaterTemp(T227,AD227, activeEWTHeating, AY227, \"heating\")))","v":""},"",{"$f":" getNozzle(T227, W227, Y227, Z227, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I228)),I228<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I228, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H228)),H228<0),\"\",intlEstQuantity(T228, W228*12, H228)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T228=\"Select Model\",\"\",coilCircuitChange(W228, U228, AC228, T228,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T228=\"Select Model\",\"\",beamWidth(T228))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T228=\"Select Model\",T228=\"PCBL\"), 0,getSPIP(T228, W228, Y228, BD228, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T228=\"Select Model\", \"\",IF(T228=\"PCBL\",0,primaryAirSensibleCapacityIP($T228,$W228,activeRoomTempCooling,activePriAirTempCooling,$Y228,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T228=\"Select Model\",\"\",IF($T228=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y228,activeElevation)))","v":""},{"$f":"IF(OR(T228=\"Select Model\",T228=\"PCBL\"), 0,IF(AD228=0,0,-primaryAirSensibleCapacityIP($T228,$W228,activeRoomTempHeating,activePriAirTempHeating,$Y228,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T228=\"Select Model\", \"\", InductionRatio($T228,BD228,$W228,$Y228)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T228=\"Select Model\", \"\",IF($T228=\"PCBL\",\"N/A\",minVAVSetBack(AA228, Y228))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T228=\"Select Model\", \"\",IF($T228= \"PCBL\",\"N/A\",getDischargeAirTemp($T228,$V228,$AC228,$W228,BD228,$AL228, $Y228, $AS228, \"cooling\",activeElevation,$AB228,$AJ228,$AV228,$BB228))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T228=\"Select Model\",$T228=\"PCBL\"), \"\",getDischargeAirTemp($T228,$V228,$AD228,$W228,BD228,$AL228, $Y228, $AY228, \"heating\",activeElevation,$AB228,$AJ228,$AV228,$BB228)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T228=\"Select Model\", \"\",IF(OR($T228=\"ACBC_1W\",$T228=\"ACBC_2W\",LEFT($T228,4)=\"ACBR\",$T228 = \"LIU24_2W\",LEFT($T228,3)=\"RIU\",LEFT($T228,6)=\"ACBL12\"), IF((soundLevel($T228, $AB228, BD228, $Y228, $W228,$AJ228,$AA228,\"dba\"))<15,\"<15\",soundLevel($T228, $AB228, BD228, $Y228, $W228,$AJ228,$AA228,\"dba\")+0.4),IF((soundLevel($T228, $AB228, BD228, $Y228, $W228,$AJ228,$AA228,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T228, $AB228, BD228, $Y228, $W228,$AJ228,$AA228,\"dba\")+5)<15, \"<15\", soundLevel($T228, $AB228, BD228,$Y228, $W228,$AJ228,$AA228,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T228=\"Select Model\", \"\",IF(OR($T228=\"ACBC_1W\",$T228=\"ACBC_2W\",LEFT($T228,4)=\"ACBR\",$T228=\"LIU24_2W\",LEFT($T228,3)=\"RIU\",LEFT($T228,6)=\"ACBL12\"), IF((soundLevel($T228, $AB228, BD228, $Y228, $W228,$AJ228,$AA228,\"NC\"))<15,\"<15\",soundLevel($T228, $AB228, BD228, $Y228, $W228,$AJ228,$AA228,\"NC\")+0.4),IF((soundLevel($T228, $AB228, BD228, $Y228, $W228,$AJ228,$AA228,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T228, $AB228, BD228, $Y228, $W228,$AJ228,$AA228,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T228, $AB228, BD228, $Y228, $W228,$AJ228,$AA228,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T228=\"Select Model\",\"\",IF($T228=\"LIU24_2W\",calcQwIP($Y228,$W228,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC228,$AI228,\"latent\",$U228&\"P\"&IF($V228=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T228,activeElevation),\"\"))","v":""},{"$f":"IF($T228=\"Select Model\",\"\",IF($T228=\"ACBC_1W\",calcQwIP($Y228,$W228,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC228,BD228,\"capacity\",$U228&\"P\"&IF($V228=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T228,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y228,$W228,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC228,BD228,\"capacity\",$U228&\"P\"&IF($V228=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T228,activeElevation)))","v":""},"",{"$f":"IF(T228=\"Select Model\", 0,waterPressureDrop(W228, U228 & \"P\" & IF(V228=\"Dual\",2,1) &\"C\", AC228, \"cooling\", T228))","v":0},{"$f":"IF(T228=\"Select Model\", \"\",getReturnWaterTemp(T228,AC228, activeEWTCooling, AS228, \"cooling\"))","v":""},"",{"$f":"IF($T228<>\"ACBC_1W\",\"\",IF($J228=\"\",\"\",FintubeCapacity($T228,$W228,$AE228,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T228=\"Select Model\",T228=\"PCBL\"),\"\",calcQwIP(Y228,W228,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD228,BD228,\"capacity\",U228&\"P\"&IF(V228=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T228,activeElevation))","v":""},"",{"$f":"IF(OR(T228=\"Select Model\",T228=\"PCBL\"), \"\",IF(AY228=0,\"N/A\",waterPressureDrop(W228, U228 & \"P\" & IF(V228=\"Dual\",2,1) &\"C\", AD228, \"heating\", T228)))","v":""},{"$f":"IF(OR(T228=\"Select Model\",T228=\"PCBL\"), \"\",IF(AY228=0,getReturnWaterTemp(T228,AE228, activeEWTHeating, AX228, \"heating\"),getReturnWaterTemp(T228,AD228, activeEWTHeating, AY228, \"heating\")))","v":""},"",{"$f":" getNozzle(T228, W228, Y228, Z228, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I229)),I229<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I229, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H229)),H229<0),\"\",intlEstQuantity(T229, W229*12, H229)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T229=\"Select Model\",\"\",coilCircuitChange(W229, U229, AC229, T229,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T229=\"Select Model\",\"\",beamWidth(T229))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T229=\"Select Model\",T229=\"PCBL\"), 0,getSPIP(T229, W229, Y229, BD229, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T229=\"Select Model\", \"\",IF(T229=\"PCBL\",0,primaryAirSensibleCapacityIP($T229,$W229,activeRoomTempCooling,activePriAirTempCooling,$Y229,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T229=\"Select Model\",\"\",IF($T229=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y229,activeElevation)))","v":""},{"$f":"IF(OR(T229=\"Select Model\",T229=\"PCBL\"), 0,IF(AD229=0,0,-primaryAirSensibleCapacityIP($T229,$W229,activeRoomTempHeating,activePriAirTempHeating,$Y229,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T229=\"Select Model\", \"\", InductionRatio($T229,BD229,$W229,$Y229)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T229=\"Select Model\", \"\",IF($T229=\"PCBL\",\"N/A\",minVAVSetBack(AA229, Y229))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T229=\"Select Model\", \"\",IF($T229= \"PCBL\",\"N/A\",getDischargeAirTemp($T229,$V229,$AC229,$W229,BD229,$AL229, $Y229, $AS229, \"cooling\",activeElevation,$AB229,$AJ229,$AV229,$BB229))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T229=\"Select Model\",$T229=\"PCBL\"), \"\",getDischargeAirTemp($T229,$V229,$AD229,$W229,BD229,$AL229, $Y229, $AY229, \"heating\",activeElevation,$AB229,$AJ229,$AV229,$BB229)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T229=\"Select Model\", \"\",IF(OR($T229=\"ACBC_1W\",$T229=\"ACBC_2W\",LEFT($T229,4)=\"ACBR\",$T229 = \"LIU24_2W\",LEFT($T229,3)=\"RIU\",LEFT($T229,6)=\"ACBL12\"), IF((soundLevel($T229, $AB229, BD229, $Y229, $W229,$AJ229,$AA229,\"dba\"))<15,\"<15\",soundLevel($T229, $AB229, BD229, $Y229, $W229,$AJ229,$AA229,\"dba\")+0.4),IF((soundLevel($T229, $AB229, BD229, $Y229, $W229,$AJ229,$AA229,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T229, $AB229, BD229, $Y229, $W229,$AJ229,$AA229,\"dba\")+5)<15, \"<15\", soundLevel($T229, $AB229, BD229,$Y229, $W229,$AJ229,$AA229,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T229=\"Select Model\", \"\",IF(OR($T229=\"ACBC_1W\",$T229=\"ACBC_2W\",LEFT($T229,4)=\"ACBR\",$T229=\"LIU24_2W\",LEFT($T229,3)=\"RIU\",LEFT($T229,6)=\"ACBL12\"), IF((soundLevel($T229, $AB229, BD229, $Y229, $W229,$AJ229,$AA229,\"NC\"))<15,\"<15\",soundLevel($T229, $AB229, BD229, $Y229, $W229,$AJ229,$AA229,\"NC\")+0.4),IF((soundLevel($T229, $AB229, BD229, $Y229, $W229,$AJ229,$AA229,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T229, $AB229, BD229, $Y229, $W229,$AJ229,$AA229,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T229, $AB229, BD229, $Y229, $W229,$AJ229,$AA229,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T229=\"Select Model\",\"\",IF($T229=\"LIU24_2W\",calcQwIP($Y229,$W229,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC229,$AI229,\"latent\",$U229&\"P\"&IF($V229=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T229,activeElevation),\"\"))","v":""},{"$f":"IF($T229=\"Select Model\",\"\",IF($T229=\"ACBC_1W\",calcQwIP($Y229,$W229,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC229,BD229,\"capacity\",$U229&\"P\"&IF($V229=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T229,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y229,$W229,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC229,BD229,\"capacity\",$U229&\"P\"&IF($V229=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T229,activeElevation)))","v":""},"",{"$f":"IF(T229=\"Select Model\", 0,waterPressureDrop(W229, U229 & \"P\" & IF(V229=\"Dual\",2,1) &\"C\", AC229, \"cooling\", T229))","v":0},{"$f":"IF(T229=\"Select Model\", \"\",getReturnWaterTemp(T229,AC229, activeEWTCooling, AS229, \"cooling\"))","v":""},"",{"$f":"IF($T229<>\"ACBC_1W\",\"\",IF($J229=\"\",\"\",FintubeCapacity($T229,$W229,$AE229,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T229=\"Select Model\",T229=\"PCBL\"),\"\",calcQwIP(Y229,W229,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD229,BD229,\"capacity\",U229&\"P\"&IF(V229=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T229,activeElevation))","v":""},"",{"$f":"IF(OR(T229=\"Select Model\",T229=\"PCBL\"), \"\",IF(AY229=0,\"N/A\",waterPressureDrop(W229, U229 & \"P\" & IF(V229=\"Dual\",2,1) &\"C\", AD229, \"heating\", T229)))","v":""},{"$f":"IF(OR(T229=\"Select Model\",T229=\"PCBL\"), \"\",IF(AY229=0,getReturnWaterTemp(T229,AE229, activeEWTHeating, AX229, \"heating\"),getReturnWaterTemp(T229,AD229, activeEWTHeating, AY229, \"heating\")))","v":""},"",{"$f":" getNozzle(T229, W229, Y229, Z229, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I230)),I230<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I230, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H230)),H230<0),\"\",intlEstQuantity(T230, W230*12, H230)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T230=\"Select Model\",\"\",coilCircuitChange(W230, U230, AC230, T230,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T230=\"Select Model\",\"\",beamWidth(T230))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T230=\"Select Model\",T230=\"PCBL\"), 0,getSPIP(T230, W230, Y230, BD230, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T230=\"Select Model\", \"\",IF(T230=\"PCBL\",0,primaryAirSensibleCapacityIP($T230,$W230,activeRoomTempCooling,activePriAirTempCooling,$Y230,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T230=\"Select Model\",\"\",IF($T230=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y230,activeElevation)))","v":""},{"$f":"IF(OR(T230=\"Select Model\",T230=\"PCBL\"), 0,IF(AD230=0,0,-primaryAirSensibleCapacityIP($T230,$W230,activeRoomTempHeating,activePriAirTempHeating,$Y230,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T230=\"Select Model\", \"\", InductionRatio($T230,BD230,$W230,$Y230)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T230=\"Select Model\", \"\",IF($T230=\"PCBL\",\"N/A\",minVAVSetBack(AA230, Y230))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T230=\"Select Model\", \"\",IF($T230= \"PCBL\",\"N/A\",getDischargeAirTemp($T230,$V230,$AC230,$W230,BD230,$AL230, $Y230, $AS230, \"cooling\",activeElevation,$AB230,$AJ230,$AV230,$BB230))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T230=\"Select Model\",$T230=\"PCBL\"), \"\",getDischargeAirTemp($T230,$V230,$AD230,$W230,BD230,$AL230, $Y230, $AY230, \"heating\",activeElevation,$AB230,$AJ230,$AV230,$BB230)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T230=\"Select Model\", \"\",IF(OR($T230=\"ACBC_1W\",$T230=\"ACBC_2W\",LEFT($T230,4)=\"ACBR\",$T230 = \"LIU24_2W\",LEFT($T230,3)=\"RIU\",LEFT($T230,6)=\"ACBL12\"), IF((soundLevel($T230, $AB230, BD230, $Y230, $W230,$AJ230,$AA230,\"dba\"))<15,\"<15\",soundLevel($T230, $AB230, BD230, $Y230, $W230,$AJ230,$AA230,\"dba\")+0.4),IF((soundLevel($T230, $AB230, BD230, $Y230, $W230,$AJ230,$AA230,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T230, $AB230, BD230, $Y230, $W230,$AJ230,$AA230,\"dba\")+5)<15, \"<15\", soundLevel($T230, $AB230, BD230,$Y230, $W230,$AJ230,$AA230,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T230=\"Select Model\", \"\",IF(OR($T230=\"ACBC_1W\",$T230=\"ACBC_2W\",LEFT($T230,4)=\"ACBR\",$T230=\"LIU24_2W\",LEFT($T230,3)=\"RIU\",LEFT($T230,6)=\"ACBL12\"), IF((soundLevel($T230, $AB230, BD230, $Y230, $W230,$AJ230,$AA230,\"NC\"))<15,\"<15\",soundLevel($T230, $AB230, BD230, $Y230, $W230,$AJ230,$AA230,\"NC\")+0.4),IF((soundLevel($T230, $AB230, BD230, $Y230, $W230,$AJ230,$AA230,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T230, $AB230, BD230, $Y230, $W230,$AJ230,$AA230,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T230, $AB230, BD230, $Y230, $W230,$AJ230,$AA230,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T230=\"Select Model\",\"\",IF($T230=\"LIU24_2W\",calcQwIP($Y230,$W230,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC230,$AI230,\"latent\",$U230&\"P\"&IF($V230=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T230,activeElevation),\"\"))","v":""},{"$f":"IF($T230=\"Select Model\",\"\",IF($T230=\"ACBC_1W\",calcQwIP($Y230,$W230,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC230,BD230,\"capacity\",$U230&\"P\"&IF($V230=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T230,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y230,$W230,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC230,BD230,\"capacity\",$U230&\"P\"&IF($V230=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T230,activeElevation)))","v":""},"",{"$f":"IF(T230=\"Select Model\", 0,waterPressureDrop(W230, U230 & \"P\" & IF(V230=\"Dual\",2,1) &\"C\", AC230, \"cooling\", T230))","v":0},{"$f":"IF(T230=\"Select Model\", \"\",getReturnWaterTemp(T230,AC230, activeEWTCooling, AS230, \"cooling\"))","v":""},"",{"$f":"IF($T230<>\"ACBC_1W\",\"\",IF($J230=\"\",\"\",FintubeCapacity($T230,$W230,$AE230,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T230=\"Select Model\",T230=\"PCBL\"),\"\",calcQwIP(Y230,W230,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD230,BD230,\"capacity\",U230&\"P\"&IF(V230=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T230,activeElevation))","v":""},"",{"$f":"IF(OR(T230=\"Select Model\",T230=\"PCBL\"), \"\",IF(AY230=0,\"N/A\",waterPressureDrop(W230, U230 & \"P\" & IF(V230=\"Dual\",2,1) &\"C\", AD230, \"heating\", T230)))","v":""},{"$f":"IF(OR(T230=\"Select Model\",T230=\"PCBL\"), \"\",IF(AY230=0,getReturnWaterTemp(T230,AE230, activeEWTHeating, AX230, \"heating\"),getReturnWaterTemp(T230,AD230, activeEWTHeating, AY230, \"heating\")))","v":""},"",{"$f":" getNozzle(T230, W230, Y230, Z230, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I231)),I231<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I231, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H231)),H231<0),\"\",intlEstQuantity(T231, W231*12, H231)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T231=\"Select Model\",\"\",coilCircuitChange(W231, U231, AC231, T231,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T231=\"Select Model\",\"\",beamWidth(T231))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T231=\"Select Model\",T231=\"PCBL\"), 0,getSPIP(T231, W231, Y231, BD231, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T231=\"Select Model\", \"\",IF(T231=\"PCBL\",0,primaryAirSensibleCapacityIP($T231,$W231,activeRoomTempCooling,activePriAirTempCooling,$Y231,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T231=\"Select Model\",\"\",IF($T231=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y231,activeElevation)))","v":""},{"$f":"IF(OR(T231=\"Select Model\",T231=\"PCBL\"), 0,IF(AD231=0,0,-primaryAirSensibleCapacityIP($T231,$W231,activeRoomTempHeating,activePriAirTempHeating,$Y231,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T231=\"Select Model\", \"\", InductionRatio($T231,BD231,$W231,$Y231)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T231=\"Select Model\", \"\",IF($T231=\"PCBL\",\"N/A\",minVAVSetBack(AA231, Y231))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T231=\"Select Model\", \"\",IF($T231= \"PCBL\",\"N/A\",getDischargeAirTemp($T231,$V231,$AC231,$W231,BD231,$AL231, $Y231, $AS231, \"cooling\",activeElevation,$AB231,$AJ231,$AV231,$BB231))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T231=\"Select Model\",$T231=\"PCBL\"), \"\",getDischargeAirTemp($T231,$V231,$AD231,$W231,BD231,$AL231, $Y231, $AY231, \"heating\",activeElevation,$AB231,$AJ231,$AV231,$BB231)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T231=\"Select Model\", \"\",IF(OR($T231=\"ACBC_1W\",$T231=\"ACBC_2W\",LEFT($T231,4)=\"ACBR\",$T231 = \"LIU24_2W\",LEFT($T231,3)=\"RIU\",LEFT($T231,6)=\"ACBL12\"), IF((soundLevel($T231, $AB231, BD231, $Y231, $W231,$AJ231,$AA231,\"dba\"))<15,\"<15\",soundLevel($T231, $AB231, BD231, $Y231, $W231,$AJ231,$AA231,\"dba\")+0.4),IF((soundLevel($T231, $AB231, BD231, $Y231, $W231,$AJ231,$AA231,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T231, $AB231, BD231, $Y231, $W231,$AJ231,$AA231,\"dba\")+5)<15, \"<15\", soundLevel($T231, $AB231, BD231,$Y231, $W231,$AJ231,$AA231,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T231=\"Select Model\", \"\",IF(OR($T231=\"ACBC_1W\",$T231=\"ACBC_2W\",LEFT($T231,4)=\"ACBR\",$T231=\"LIU24_2W\",LEFT($T231,3)=\"RIU\",LEFT($T231,6)=\"ACBL12\"), IF((soundLevel($T231, $AB231, BD231, $Y231, $W231,$AJ231,$AA231,\"NC\"))<15,\"<15\",soundLevel($T231, $AB231, BD231, $Y231, $W231,$AJ231,$AA231,\"NC\")+0.4),IF((soundLevel($T231, $AB231, BD231, $Y231, $W231,$AJ231,$AA231,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T231, $AB231, BD231, $Y231, $W231,$AJ231,$AA231,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T231, $AB231, BD231, $Y231, $W231,$AJ231,$AA231,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T231=\"Select Model\",\"\",IF($T231=\"LIU24_2W\",calcQwIP($Y231,$W231,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC231,$AI231,\"latent\",$U231&\"P\"&IF($V231=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T231,activeElevation),\"\"))","v":""},{"$f":"IF($T231=\"Select Model\",\"\",IF($T231=\"ACBC_1W\",calcQwIP($Y231,$W231,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC231,BD231,\"capacity\",$U231&\"P\"&IF($V231=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T231,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y231,$W231,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC231,BD231,\"capacity\",$U231&\"P\"&IF($V231=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T231,activeElevation)))","v":""},"",{"$f":"IF(T231=\"Select Model\", 0,waterPressureDrop(W231, U231 & \"P\" & IF(V231=\"Dual\",2,1) &\"C\", AC231, \"cooling\", T231))","v":0},{"$f":"IF(T231=\"Select Model\", \"\",getReturnWaterTemp(T231,AC231, activeEWTCooling, AS231, \"cooling\"))","v":""},"",{"$f":"IF($T231<>\"ACBC_1W\",\"\",IF($J231=\"\",\"\",FintubeCapacity($T231,$W231,$AE231,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T231=\"Select Model\",T231=\"PCBL\"),\"\",calcQwIP(Y231,W231,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD231,BD231,\"capacity\",U231&\"P\"&IF(V231=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T231,activeElevation))","v":""},"",{"$f":"IF(OR(T231=\"Select Model\",T231=\"PCBL\"), \"\",IF(AY231=0,\"N/A\",waterPressureDrop(W231, U231 & \"P\" & IF(V231=\"Dual\",2,1) &\"C\", AD231, \"heating\", T231)))","v":""},{"$f":"IF(OR(T231=\"Select Model\",T231=\"PCBL\"), \"\",IF(AY231=0,getReturnWaterTemp(T231,AE231, activeEWTHeating, AX231, \"heating\"),getReturnWaterTemp(T231,AD231, activeEWTHeating, AY231, \"heating\")))","v":""},"",{"$f":" getNozzle(T231, W231, Y231, Z231, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I232)),I232<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I232, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H232)),H232<0),\"\",intlEstQuantity(T232, W232*12, H232)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T232=\"Select Model\",\"\",coilCircuitChange(W232, U232, AC232, T232,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T232=\"Select Model\",\"\",beamWidth(T232))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T232=\"Select Model\",T232=\"PCBL\"), 0,getSPIP(T232, W232, Y232, BD232, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T232=\"Select Model\", \"\",IF(T232=\"PCBL\",0,primaryAirSensibleCapacityIP($T232,$W232,activeRoomTempCooling,activePriAirTempCooling,$Y232,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T232=\"Select Model\",\"\",IF($T232=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y232,activeElevation)))","v":""},{"$f":"IF(OR(T232=\"Select Model\",T232=\"PCBL\"), 0,IF(AD232=0,0,-primaryAirSensibleCapacityIP($T232,$W232,activeRoomTempHeating,activePriAirTempHeating,$Y232,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T232=\"Select Model\", \"\", InductionRatio($T232,BD232,$W232,$Y232)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T232=\"Select Model\", \"\",IF($T232=\"PCBL\",\"N/A\",minVAVSetBack(AA232, Y232))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T232=\"Select Model\", \"\",IF($T232= \"PCBL\",\"N/A\",getDischargeAirTemp($T232,$V232,$AC232,$W232,BD232,$AL232, $Y232, $AS232, \"cooling\",activeElevation,$AB232,$AJ232,$AV232,$BB232))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T232=\"Select Model\",$T232=\"PCBL\"), \"\",getDischargeAirTemp($T232,$V232,$AD232,$W232,BD232,$AL232, $Y232, $AY232, \"heating\",activeElevation,$AB232,$AJ232,$AV232,$BB232)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T232=\"Select Model\", \"\",IF(OR($T232=\"ACBC_1W\",$T232=\"ACBC_2W\",LEFT($T232,4)=\"ACBR\",$T232 = \"LIU24_2W\",LEFT($T232,3)=\"RIU\",LEFT($T232,6)=\"ACBL12\"), IF((soundLevel($T232, $AB232, BD232, $Y232, $W232,$AJ232,$AA232,\"dba\"))<15,\"<15\",soundLevel($T232, $AB232, BD232, $Y232, $W232,$AJ232,$AA232,\"dba\")+0.4),IF((soundLevel($T232, $AB232, BD232, $Y232, $W232,$AJ232,$AA232,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T232, $AB232, BD232, $Y232, $W232,$AJ232,$AA232,\"dba\")+5)<15, \"<15\", soundLevel($T232, $AB232, BD232,$Y232, $W232,$AJ232,$AA232,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T232=\"Select Model\", \"\",IF(OR($T232=\"ACBC_1W\",$T232=\"ACBC_2W\",LEFT($T232,4)=\"ACBR\",$T232=\"LIU24_2W\",LEFT($T232,3)=\"RIU\",LEFT($T232,6)=\"ACBL12\"), IF((soundLevel($T232, $AB232, BD232, $Y232, $W232,$AJ232,$AA232,\"NC\"))<15,\"<15\",soundLevel($T232, $AB232, BD232, $Y232, $W232,$AJ232,$AA232,\"NC\")+0.4),IF((soundLevel($T232, $AB232, BD232, $Y232, $W232,$AJ232,$AA232,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T232, $AB232, BD232, $Y232, $W232,$AJ232,$AA232,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T232, $AB232, BD232, $Y232, $W232,$AJ232,$AA232,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T232=\"Select Model\",\"\",IF($T232=\"LIU24_2W\",calcQwIP($Y232,$W232,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC232,$AI232,\"latent\",$U232&\"P\"&IF($V232=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T232,activeElevation),\"\"))","v":""},{"$f":"IF($T232=\"Select Model\",\"\",IF($T232=\"ACBC_1W\",calcQwIP($Y232,$W232,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC232,BD232,\"capacity\",$U232&\"P\"&IF($V232=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T232,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y232,$W232,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC232,BD232,\"capacity\",$U232&\"P\"&IF($V232=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T232,activeElevation)))","v":""},"",{"$f":"IF(T232=\"Select Model\", 0,waterPressureDrop(W232, U232 & \"P\" & IF(V232=\"Dual\",2,1) &\"C\", AC232, \"cooling\", T232))","v":0},{"$f":"IF(T232=\"Select Model\", \"\",getReturnWaterTemp(T232,AC232, activeEWTCooling, AS232, \"cooling\"))","v":""},"",{"$f":"IF($T232<>\"ACBC_1W\",\"\",IF($J232=\"\",\"\",FintubeCapacity($T232,$W232,$AE232,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T232=\"Select Model\",T232=\"PCBL\"),\"\",calcQwIP(Y232,W232,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD232,BD232,\"capacity\",U232&\"P\"&IF(V232=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T232,activeElevation))","v":""},"",{"$f":"IF(OR(T232=\"Select Model\",T232=\"PCBL\"), \"\",IF(AY232=0,\"N/A\",waterPressureDrop(W232, U232 & \"P\" & IF(V232=\"Dual\",2,1) &\"C\", AD232, \"heating\", T232)))","v":""},{"$f":"IF(OR(T232=\"Select Model\",T232=\"PCBL\"), \"\",IF(AY232=0,getReturnWaterTemp(T232,AE232, activeEWTHeating, AX232, \"heating\"),getReturnWaterTemp(T232,AD232, activeEWTHeating, AY232, \"heating\")))","v":""},"",{"$f":" getNozzle(T232, W232, Y232, Z232, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I233)),I233<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I233, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H233)),H233<0),\"\",intlEstQuantity(T233, W233*12, H233)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T233=\"Select Model\",\"\",coilCircuitChange(W233, U233, AC233, T233,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T233=\"Select Model\",\"\",beamWidth(T233))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T233=\"Select Model\",T233=\"PCBL\"), 0,getSPIP(T233, W233, Y233, BD233, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T233=\"Select Model\", \"\",IF(T233=\"PCBL\",0,primaryAirSensibleCapacityIP($T233,$W233,activeRoomTempCooling,activePriAirTempCooling,$Y233,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T233=\"Select Model\",\"\",IF($T233=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y233,activeElevation)))","v":""},{"$f":"IF(OR(T233=\"Select Model\",T233=\"PCBL\"), 0,IF(AD233=0,0,-primaryAirSensibleCapacityIP($T233,$W233,activeRoomTempHeating,activePriAirTempHeating,$Y233,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T233=\"Select Model\", \"\", InductionRatio($T233,BD233,$W233,$Y233)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T233=\"Select Model\", \"\",IF($T233=\"PCBL\",\"N/A\",minVAVSetBack(AA233, Y233))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T233=\"Select Model\", \"\",IF($T233= \"PCBL\",\"N/A\",getDischargeAirTemp($T233,$V233,$AC233,$W233,BD233,$AL233, $Y233, $AS233, \"cooling\",activeElevation,$AB233,$AJ233,$AV233,$BB233))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T233=\"Select Model\",$T233=\"PCBL\"), \"\",getDischargeAirTemp($T233,$V233,$AD233,$W233,BD233,$AL233, $Y233, $AY233, \"heating\",activeElevation,$AB233,$AJ233,$AV233,$BB233)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T233=\"Select Model\", \"\",IF(OR($T233=\"ACBC_1W\",$T233=\"ACBC_2W\",LEFT($T233,4)=\"ACBR\",$T233 = \"LIU24_2W\",LEFT($T233,3)=\"RIU\",LEFT($T233,6)=\"ACBL12\"), IF((soundLevel($T233, $AB233, BD233, $Y233, $W233,$AJ233,$AA233,\"dba\"))<15,\"<15\",soundLevel($T233, $AB233, BD233, $Y233, $W233,$AJ233,$AA233,\"dba\")+0.4),IF((soundLevel($T233, $AB233, BD233, $Y233, $W233,$AJ233,$AA233,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T233, $AB233, BD233, $Y233, $W233,$AJ233,$AA233,\"dba\")+5)<15, \"<15\", soundLevel($T233, $AB233, BD233,$Y233, $W233,$AJ233,$AA233,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T233=\"Select Model\", \"\",IF(OR($T233=\"ACBC_1W\",$T233=\"ACBC_2W\",LEFT($T233,4)=\"ACBR\",$T233=\"LIU24_2W\",LEFT($T233,3)=\"RIU\",LEFT($T233,6)=\"ACBL12\"), IF((soundLevel($T233, $AB233, BD233, $Y233, $W233,$AJ233,$AA233,\"NC\"))<15,\"<15\",soundLevel($T233, $AB233, BD233, $Y233, $W233,$AJ233,$AA233,\"NC\")+0.4),IF((soundLevel($T233, $AB233, BD233, $Y233, $W233,$AJ233,$AA233,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T233, $AB233, BD233, $Y233, $W233,$AJ233,$AA233,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T233, $AB233, BD233, $Y233, $W233,$AJ233,$AA233,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T233=\"Select Model\",\"\",IF($T233=\"LIU24_2W\",calcQwIP($Y233,$W233,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC233,$AI233,\"latent\",$U233&\"P\"&IF($V233=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T233,activeElevation),\"\"))","v":""},{"$f":"IF($T233=\"Select Model\",\"\",IF($T233=\"ACBC_1W\",calcQwIP($Y233,$W233,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC233,BD233,\"capacity\",$U233&\"P\"&IF($V233=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T233,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y233,$W233,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC233,BD233,\"capacity\",$U233&\"P\"&IF($V233=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T233,activeElevation)))","v":""},"",{"$f":"IF(T233=\"Select Model\", 0,waterPressureDrop(W233, U233 & \"P\" & IF(V233=\"Dual\",2,1) &\"C\", AC233, \"cooling\", T233))","v":0},{"$f":"IF(T233=\"Select Model\", \"\",getReturnWaterTemp(T233,AC233, activeEWTCooling, AS233, \"cooling\"))","v":""},"",{"$f":"IF($T233<>\"ACBC_1W\",\"\",IF($J233=\"\",\"\",FintubeCapacity($T233,$W233,$AE233,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T233=\"Select Model\",T233=\"PCBL\"),\"\",calcQwIP(Y233,W233,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD233,BD233,\"capacity\",U233&\"P\"&IF(V233=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T233,activeElevation))","v":""},"",{"$f":"IF(OR(T233=\"Select Model\",T233=\"PCBL\"), \"\",IF(AY233=0,\"N/A\",waterPressureDrop(W233, U233 & \"P\" & IF(V233=\"Dual\",2,1) &\"C\", AD233, \"heating\", T233)))","v":""},{"$f":"IF(OR(T233=\"Select Model\",T233=\"PCBL\"), \"\",IF(AY233=0,getReturnWaterTemp(T233,AE233, activeEWTHeating, AX233, \"heating\"),getReturnWaterTemp(T233,AD233, activeEWTHeating, AY233, \"heating\")))","v":""},"",{"$f":" getNozzle(T233, W233, Y233, Z233, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I234)),I234<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I234, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H234)),H234<0),\"\",intlEstQuantity(T234, W234*12, H234)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T234=\"Select Model\",\"\",coilCircuitChange(W234, U234, AC234, T234,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T234=\"Select Model\",\"\",beamWidth(T234))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T234=\"Select Model\",T234=\"PCBL\"), 0,getSPIP(T234, W234, Y234, BD234, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T234=\"Select Model\", \"\",IF(T234=\"PCBL\",0,primaryAirSensibleCapacityIP($T234,$W234,activeRoomTempCooling,activePriAirTempCooling,$Y234,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T234=\"Select Model\",\"\",IF($T234=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y234,activeElevation)))","v":""},{"$f":"IF(OR(T234=\"Select Model\",T234=\"PCBL\"), 0,IF(AD234=0,0,-primaryAirSensibleCapacityIP($T234,$W234,activeRoomTempHeating,activePriAirTempHeating,$Y234,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T234=\"Select Model\", \"\", InductionRatio($T234,BD234,$W234,$Y234)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T234=\"Select Model\", \"\",IF($T234=\"PCBL\",\"N/A\",minVAVSetBack(AA234, Y234))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T234=\"Select Model\", \"\",IF($T234= \"PCBL\",\"N/A\",getDischargeAirTemp($T234,$V234,$AC234,$W234,BD234,$AL234, $Y234, $AS234, \"cooling\",activeElevation,$AB234,$AJ234,$AV234,$BB234))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T234=\"Select Model\",$T234=\"PCBL\"), \"\",getDischargeAirTemp($T234,$V234,$AD234,$W234,BD234,$AL234, $Y234, $AY234, \"heating\",activeElevation,$AB234,$AJ234,$AV234,$BB234)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T234=\"Select Model\", \"\",IF(OR($T234=\"ACBC_1W\",$T234=\"ACBC_2W\",LEFT($T234,4)=\"ACBR\",$T234 = \"LIU24_2W\",LEFT($T234,3)=\"RIU\",LEFT($T234,6)=\"ACBL12\"), IF((soundLevel($T234, $AB234, BD234, $Y234, $W234,$AJ234,$AA234,\"dba\"))<15,\"<15\",soundLevel($T234, $AB234, BD234, $Y234, $W234,$AJ234,$AA234,\"dba\")+0.4),IF((soundLevel($T234, $AB234, BD234, $Y234, $W234,$AJ234,$AA234,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T234, $AB234, BD234, $Y234, $W234,$AJ234,$AA234,\"dba\")+5)<15, \"<15\", soundLevel($T234, $AB234, BD234,$Y234, $W234,$AJ234,$AA234,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T234=\"Select Model\", \"\",IF(OR($T234=\"ACBC_1W\",$T234=\"ACBC_2W\",LEFT($T234,4)=\"ACBR\",$T234=\"LIU24_2W\",LEFT($T234,3)=\"RIU\",LEFT($T234,6)=\"ACBL12\"), IF((soundLevel($T234, $AB234, BD234, $Y234, $W234,$AJ234,$AA234,\"NC\"))<15,\"<15\",soundLevel($T234, $AB234, BD234, $Y234, $W234,$AJ234,$AA234,\"NC\")+0.4),IF((soundLevel($T234, $AB234, BD234, $Y234, $W234,$AJ234,$AA234,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T234, $AB234, BD234, $Y234, $W234,$AJ234,$AA234,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T234, $AB234, BD234, $Y234, $W234,$AJ234,$AA234,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T234=\"Select Model\",\"\",IF($T234=\"LIU24_2W\",calcQwIP($Y234,$W234,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC234,$AI234,\"latent\",$U234&\"P\"&IF($V234=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T234,activeElevation),\"\"))","v":""},{"$f":"IF($T234=\"Select Model\",\"\",IF($T234=\"ACBC_1W\",calcQwIP($Y234,$W234,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC234,BD234,\"capacity\",$U234&\"P\"&IF($V234=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T234,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y234,$W234,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC234,BD234,\"capacity\",$U234&\"P\"&IF($V234=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T234,activeElevation)))","v":""},"",{"$f":"IF(T234=\"Select Model\", 0,waterPressureDrop(W234, U234 & \"P\" & IF(V234=\"Dual\",2,1) &\"C\", AC234, \"cooling\", T234))","v":0},{"$f":"IF(T234=\"Select Model\", \"\",getReturnWaterTemp(T234,AC234, activeEWTCooling, AS234, \"cooling\"))","v":""},"",{"$f":"IF($T234<>\"ACBC_1W\",\"\",IF($J234=\"\",\"\",FintubeCapacity($T234,$W234,$AE234,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T234=\"Select Model\",T234=\"PCBL\"),\"\",calcQwIP(Y234,W234,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD234,BD234,\"capacity\",U234&\"P\"&IF(V234=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T234,activeElevation))","v":""},"",{"$f":"IF(OR(T234=\"Select Model\",T234=\"PCBL\"), \"\",IF(AY234=0,\"N/A\",waterPressureDrop(W234, U234 & \"P\" & IF(V234=\"Dual\",2,1) &\"C\", AD234, \"heating\", T234)))","v":""},{"$f":"IF(OR(T234=\"Select Model\",T234=\"PCBL\"), \"\",IF(AY234=0,getReturnWaterTemp(T234,AE234, activeEWTHeating, AX234, \"heating\"),getReturnWaterTemp(T234,AD234, activeEWTHeating, AY234, \"heating\")))","v":""},"",{"$f":" getNozzle(T234, W234, Y234, Z234, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I235)),I235<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I235, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H235)),H235<0),\"\",intlEstQuantity(T235, W235*12, H235)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T235=\"Select Model\",\"\",coilCircuitChange(W235, U235, AC235, T235,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T235=\"Select Model\",\"\",beamWidth(T235))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T235=\"Select Model\",T235=\"PCBL\"), 0,getSPIP(T235, W235, Y235, BD235, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T235=\"Select Model\", \"\",IF(T235=\"PCBL\",0,primaryAirSensibleCapacityIP($T235,$W235,activeRoomTempCooling,activePriAirTempCooling,$Y235,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T235=\"Select Model\",\"\",IF($T235=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y235,activeElevation)))","v":""},{"$f":"IF(OR(T235=\"Select Model\",T235=\"PCBL\"), 0,IF(AD235=0,0,-primaryAirSensibleCapacityIP($T235,$W235,activeRoomTempHeating,activePriAirTempHeating,$Y235,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T235=\"Select Model\", \"\", InductionRatio($T235,BD235,$W235,$Y235)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T235=\"Select Model\", \"\",IF($T235=\"PCBL\",\"N/A\",minVAVSetBack(AA235, Y235))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T235=\"Select Model\", \"\",IF($T235= \"PCBL\",\"N/A\",getDischargeAirTemp($T235,$V235,$AC235,$W235,BD235,$AL235, $Y235, $AS235, \"cooling\",activeElevation,$AB235,$AJ235,$AV235,$BB235))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T235=\"Select Model\",$T235=\"PCBL\"), \"\",getDischargeAirTemp($T235,$V235,$AD235,$W235,BD235,$AL235, $Y235, $AY235, \"heating\",activeElevation,$AB235,$AJ235,$AV235,$BB235)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T235=\"Select Model\", \"\",IF(OR($T235=\"ACBC_1W\",$T235=\"ACBC_2W\",LEFT($T235,4)=\"ACBR\",$T235 = \"LIU24_2W\",LEFT($T235,3)=\"RIU\",LEFT($T235,6)=\"ACBL12\"), IF((soundLevel($T235, $AB235, BD235, $Y235, $W235,$AJ235,$AA235,\"dba\"))<15,\"<15\",soundLevel($T235, $AB235, BD235, $Y235, $W235,$AJ235,$AA235,\"dba\")+0.4),IF((soundLevel($T235, $AB235, BD235, $Y235, $W235,$AJ235,$AA235,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T235, $AB235, BD235, $Y235, $W235,$AJ235,$AA235,\"dba\")+5)<15, \"<15\", soundLevel($T235, $AB235, BD235,$Y235, $W235,$AJ235,$AA235,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T235=\"Select Model\", \"\",IF(OR($T235=\"ACBC_1W\",$T235=\"ACBC_2W\",LEFT($T235,4)=\"ACBR\",$T235=\"LIU24_2W\",LEFT($T235,3)=\"RIU\",LEFT($T235,6)=\"ACBL12\"), IF((soundLevel($T235, $AB235, BD235, $Y235, $W235,$AJ235,$AA235,\"NC\"))<15,\"<15\",soundLevel($T235, $AB235, BD235, $Y235, $W235,$AJ235,$AA235,\"NC\")+0.4),IF((soundLevel($T235, $AB235, BD235, $Y235, $W235,$AJ235,$AA235,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T235, $AB235, BD235, $Y235, $W235,$AJ235,$AA235,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T235, $AB235, BD235, $Y235, $W235,$AJ235,$AA235,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T235=\"Select Model\",\"\",IF($T235=\"LIU24_2W\",calcQwIP($Y235,$W235,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC235,$AI235,\"latent\",$U235&\"P\"&IF($V235=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T235,activeElevation),\"\"))","v":""},{"$f":"IF($T235=\"Select Model\",\"\",IF($T235=\"ACBC_1W\",calcQwIP($Y235,$W235,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC235,BD235,\"capacity\",$U235&\"P\"&IF($V235=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T235,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y235,$W235,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC235,BD235,\"capacity\",$U235&\"P\"&IF($V235=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T235,activeElevation)))","v":""},"",{"$f":"IF(T235=\"Select Model\", 0,waterPressureDrop(W235, U235 & \"P\" & IF(V235=\"Dual\",2,1) &\"C\", AC235, \"cooling\", T235))","v":0},{"$f":"IF(T235=\"Select Model\", \"\",getReturnWaterTemp(T235,AC235, activeEWTCooling, AS235, \"cooling\"))","v":""},"",{"$f":"IF($T235<>\"ACBC_1W\",\"\",IF($J235=\"\",\"\",FintubeCapacity($T235,$W235,$AE235,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T235=\"Select Model\",T235=\"PCBL\"),\"\",calcQwIP(Y235,W235,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD235,BD235,\"capacity\",U235&\"P\"&IF(V235=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T235,activeElevation))","v":""},"",{"$f":"IF(OR(T235=\"Select Model\",T235=\"PCBL\"), \"\",IF(AY235=0,\"N/A\",waterPressureDrop(W235, U235 & \"P\" & IF(V235=\"Dual\",2,1) &\"C\", AD235, \"heating\", T235)))","v":""},{"$f":"IF(OR(T235=\"Select Model\",T235=\"PCBL\"), \"\",IF(AY235=0,getReturnWaterTemp(T235,AE235, activeEWTHeating, AX235, \"heating\"),getReturnWaterTemp(T235,AD235, activeEWTHeating, AY235, \"heating\")))","v":""},"",{"$f":" getNozzle(T235, W235, Y235, Z235, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I236)),I236<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I236, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H236)),H236<0),\"\",intlEstQuantity(T236, W236*12, H236)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T236=\"Select Model\",\"\",coilCircuitChange(W236, U236, AC236, T236,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T236=\"Select Model\",\"\",beamWidth(T236))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T236=\"Select Model\",T236=\"PCBL\"), 0,getSPIP(T236, W236, Y236, BD236, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T236=\"Select Model\", \"\",IF(T236=\"PCBL\",0,primaryAirSensibleCapacityIP($T236,$W236,activeRoomTempCooling,activePriAirTempCooling,$Y236,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T236=\"Select Model\",\"\",IF($T236=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y236,activeElevation)))","v":""},{"$f":"IF(OR(T236=\"Select Model\",T236=\"PCBL\"), 0,IF(AD236=0,0,-primaryAirSensibleCapacityIP($T236,$W236,activeRoomTempHeating,activePriAirTempHeating,$Y236,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T236=\"Select Model\", \"\", InductionRatio($T236,BD236,$W236,$Y236)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T236=\"Select Model\", \"\",IF($T236=\"PCBL\",\"N/A\",minVAVSetBack(AA236, Y236))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T236=\"Select Model\", \"\",IF($T236= \"PCBL\",\"N/A\",getDischargeAirTemp($T236,$V236,$AC236,$W236,BD236,$AL236, $Y236, $AS236, \"cooling\",activeElevation,$AB236,$AJ236,$AV236,$BB236))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T236=\"Select Model\",$T236=\"PCBL\"), \"\",getDischargeAirTemp($T236,$V236,$AD236,$W236,BD236,$AL236, $Y236, $AY236, \"heating\",activeElevation,$AB236,$AJ236,$AV236,$BB236)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T236=\"Select Model\", \"\",IF(OR($T236=\"ACBC_1W\",$T236=\"ACBC_2W\",LEFT($T236,4)=\"ACBR\",$T236 = \"LIU24_2W\",LEFT($T236,3)=\"RIU\",LEFT($T236,6)=\"ACBL12\"), IF((soundLevel($T236, $AB236, BD236, $Y236, $W236,$AJ236,$AA236,\"dba\"))<15,\"<15\",soundLevel($T236, $AB236, BD236, $Y236, $W236,$AJ236,$AA236,\"dba\")+0.4),IF((soundLevel($T236, $AB236, BD236, $Y236, $W236,$AJ236,$AA236,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T236, $AB236, BD236, $Y236, $W236,$AJ236,$AA236,\"dba\")+5)<15, \"<15\", soundLevel($T236, $AB236, BD236,$Y236, $W236,$AJ236,$AA236,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T236=\"Select Model\", \"\",IF(OR($T236=\"ACBC_1W\",$T236=\"ACBC_2W\",LEFT($T236,4)=\"ACBR\",$T236=\"LIU24_2W\",LEFT($T236,3)=\"RIU\",LEFT($T236,6)=\"ACBL12\"), IF((soundLevel($T236, $AB236, BD236, $Y236, $W236,$AJ236,$AA236,\"NC\"))<15,\"<15\",soundLevel($T236, $AB236, BD236, $Y236, $W236,$AJ236,$AA236,\"NC\")+0.4),IF((soundLevel($T236, $AB236, BD236, $Y236, $W236,$AJ236,$AA236,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T236, $AB236, BD236, $Y236, $W236,$AJ236,$AA236,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T236, $AB236, BD236, $Y236, $W236,$AJ236,$AA236,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T236=\"Select Model\",\"\",IF($T236=\"LIU24_2W\",calcQwIP($Y236,$W236,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC236,$AI236,\"latent\",$U236&\"P\"&IF($V236=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T236,activeElevation),\"\"))","v":""},{"$f":"IF($T236=\"Select Model\",\"\",IF($T236=\"ACBC_1W\",calcQwIP($Y236,$W236,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC236,BD236,\"capacity\",$U236&\"P\"&IF($V236=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T236,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y236,$W236,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC236,BD236,\"capacity\",$U236&\"P\"&IF($V236=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T236,activeElevation)))","v":""},"",{"$f":"IF(T236=\"Select Model\", 0,waterPressureDrop(W236, U236 & \"P\" & IF(V236=\"Dual\",2,1) &\"C\", AC236, \"cooling\", T236))","v":0},{"$f":"IF(T236=\"Select Model\", \"\",getReturnWaterTemp(T236,AC236, activeEWTCooling, AS236, \"cooling\"))","v":""},"",{"$f":"IF($T236<>\"ACBC_1W\",\"\",IF($J236=\"\",\"\",FintubeCapacity($T236,$W236,$AE236,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T236=\"Select Model\",T236=\"PCBL\"),\"\",calcQwIP(Y236,W236,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD236,BD236,\"capacity\",U236&\"P\"&IF(V236=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T236,activeElevation))","v":""},"",{"$f":"IF(OR(T236=\"Select Model\",T236=\"PCBL\"), \"\",IF(AY236=0,\"N/A\",waterPressureDrop(W236, U236 & \"P\" & IF(V236=\"Dual\",2,1) &\"C\", AD236, \"heating\", T236)))","v":""},{"$f":"IF(OR(T236=\"Select Model\",T236=\"PCBL\"), \"\",IF(AY236=0,getReturnWaterTemp(T236,AE236, activeEWTHeating, AX236, \"heating\"),getReturnWaterTemp(T236,AD236, activeEWTHeating, AY236, \"heating\")))","v":""},"",{"$f":" getNozzle(T236, W236, Y236, Z236, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I237)),I237<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I237, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H237)),H237<0),\"\",intlEstQuantity(T237, W237*12, H237)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T237=\"Select Model\",\"\",coilCircuitChange(W237, U237, AC237, T237,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T237=\"Select Model\",\"\",beamWidth(T237))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T237=\"Select Model\",T237=\"PCBL\"), 0,getSPIP(T237, W237, Y237, BD237, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T237=\"Select Model\", \"\",IF(T237=\"PCBL\",0,primaryAirSensibleCapacityIP($T237,$W237,activeRoomTempCooling,activePriAirTempCooling,$Y237,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T237=\"Select Model\",\"\",IF($T237=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y237,activeElevation)))","v":""},{"$f":"IF(OR(T237=\"Select Model\",T237=\"PCBL\"), 0,IF(AD237=0,0,-primaryAirSensibleCapacityIP($T237,$W237,activeRoomTempHeating,activePriAirTempHeating,$Y237,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T237=\"Select Model\", \"\", InductionRatio($T237,BD237,$W237,$Y237)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T237=\"Select Model\", \"\",IF($T237=\"PCBL\",\"N/A\",minVAVSetBack(AA237, Y237))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T237=\"Select Model\", \"\",IF($T237= \"PCBL\",\"N/A\",getDischargeAirTemp($T237,$V237,$AC237,$W237,BD237,$AL237, $Y237, $AS237, \"cooling\",activeElevation,$AB237,$AJ237,$AV237,$BB237))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T237=\"Select Model\",$T237=\"PCBL\"), \"\",getDischargeAirTemp($T237,$V237,$AD237,$W237,BD237,$AL237, $Y237, $AY237, \"heating\",activeElevation,$AB237,$AJ237,$AV237,$BB237)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T237=\"Select Model\", \"\",IF(OR($T237=\"ACBC_1W\",$T237=\"ACBC_2W\",LEFT($T237,4)=\"ACBR\",$T237 = \"LIU24_2W\",LEFT($T237,3)=\"RIU\",LEFT($T237,6)=\"ACBL12\"), IF((soundLevel($T237, $AB237, BD237, $Y237, $W237,$AJ237,$AA237,\"dba\"))<15,\"<15\",soundLevel($T237, $AB237, BD237, $Y237, $W237,$AJ237,$AA237,\"dba\")+0.4),IF((soundLevel($T237, $AB237, BD237, $Y237, $W237,$AJ237,$AA237,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T237, $AB237, BD237, $Y237, $W237,$AJ237,$AA237,\"dba\")+5)<15, \"<15\", soundLevel($T237, $AB237, BD237,$Y237, $W237,$AJ237,$AA237,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T237=\"Select Model\", \"\",IF(OR($T237=\"ACBC_1W\",$T237=\"ACBC_2W\",LEFT($T237,4)=\"ACBR\",$T237=\"LIU24_2W\",LEFT($T237,3)=\"RIU\",LEFT($T237,6)=\"ACBL12\"), IF((soundLevel($T237, $AB237, BD237, $Y237, $W237,$AJ237,$AA237,\"NC\"))<15,\"<15\",soundLevel($T237, $AB237, BD237, $Y237, $W237,$AJ237,$AA237,\"NC\")+0.4),IF((soundLevel($T237, $AB237, BD237, $Y237, $W237,$AJ237,$AA237,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T237, $AB237, BD237, $Y237, $W237,$AJ237,$AA237,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T237, $AB237, BD237, $Y237, $W237,$AJ237,$AA237,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T237=\"Select Model\",\"\",IF($T237=\"LIU24_2W\",calcQwIP($Y237,$W237,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC237,$AI237,\"latent\",$U237&\"P\"&IF($V237=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T237,activeElevation),\"\"))","v":""},{"$f":"IF($T237=\"Select Model\",\"\",IF($T237=\"ACBC_1W\",calcQwIP($Y237,$W237,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC237,BD237,\"capacity\",$U237&\"P\"&IF($V237=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T237,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y237,$W237,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC237,BD237,\"capacity\",$U237&\"P\"&IF($V237=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T237,activeElevation)))","v":""},"",{"$f":"IF(T237=\"Select Model\", 0,waterPressureDrop(W237, U237 & \"P\" & IF(V237=\"Dual\",2,1) &\"C\", AC237, \"cooling\", T237))","v":0},{"$f":"IF(T237=\"Select Model\", \"\",getReturnWaterTemp(T237,AC237, activeEWTCooling, AS237, \"cooling\"))","v":""},"",{"$f":"IF($T237<>\"ACBC_1W\",\"\",IF($J237=\"\",\"\",FintubeCapacity($T237,$W237,$AE237,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T237=\"Select Model\",T237=\"PCBL\"),\"\",calcQwIP(Y237,W237,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD237,BD237,\"capacity\",U237&\"P\"&IF(V237=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T237,activeElevation))","v":""},"",{"$f":"IF(OR(T237=\"Select Model\",T237=\"PCBL\"), \"\",IF(AY237=0,\"N/A\",waterPressureDrop(W237, U237 & \"P\" & IF(V237=\"Dual\",2,1) &\"C\", AD237, \"heating\", T237)))","v":""},{"$f":"IF(OR(T237=\"Select Model\",T237=\"PCBL\"), \"\",IF(AY237=0,getReturnWaterTemp(T237,AE237, activeEWTHeating, AX237, \"heating\"),getReturnWaterTemp(T237,AD237, activeEWTHeating, AY237, \"heating\")))","v":""},"",{"$f":" getNozzle(T237, W237, Y237, Z237, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I238)),I238<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I238, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H238)),H238<0),\"\",intlEstQuantity(T238, W238*12, H238)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T238=\"Select Model\",\"\",coilCircuitChange(W238, U238, AC238, T238,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T238=\"Select Model\",\"\",beamWidth(T238))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T238=\"Select Model\",T238=\"PCBL\"), 0,getSPIP(T238, W238, Y238, BD238, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T238=\"Select Model\", \"\",IF(T238=\"PCBL\",0,primaryAirSensibleCapacityIP($T238,$W238,activeRoomTempCooling,activePriAirTempCooling,$Y238,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T238=\"Select Model\",\"\",IF($T238=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y238,activeElevation)))","v":""},{"$f":"IF(OR(T238=\"Select Model\",T238=\"PCBL\"), 0,IF(AD238=0,0,-primaryAirSensibleCapacityIP($T238,$W238,activeRoomTempHeating,activePriAirTempHeating,$Y238,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T238=\"Select Model\", \"\", InductionRatio($T238,BD238,$W238,$Y238)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T238=\"Select Model\", \"\",IF($T238=\"PCBL\",\"N/A\",minVAVSetBack(AA238, Y238))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T238=\"Select Model\", \"\",IF($T238= \"PCBL\",\"N/A\",getDischargeAirTemp($T238,$V238,$AC238,$W238,BD238,$AL238, $Y238, $AS238, \"cooling\",activeElevation,$AB238,$AJ238,$AV238,$BB238))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T238=\"Select Model\",$T238=\"PCBL\"), \"\",getDischargeAirTemp($T238,$V238,$AD238,$W238,BD238,$AL238, $Y238, $AY238, \"heating\",activeElevation,$AB238,$AJ238,$AV238,$BB238)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T238=\"Select Model\", \"\",IF(OR($T238=\"ACBC_1W\",$T238=\"ACBC_2W\",LEFT($T238,4)=\"ACBR\",$T238 = \"LIU24_2W\",LEFT($T238,3)=\"RIU\",LEFT($T238,6)=\"ACBL12\"), IF((soundLevel($T238, $AB238, BD238, $Y238, $W238,$AJ238,$AA238,\"dba\"))<15,\"<15\",soundLevel($T238, $AB238, BD238, $Y238, $W238,$AJ238,$AA238,\"dba\")+0.4),IF((soundLevel($T238, $AB238, BD238, $Y238, $W238,$AJ238,$AA238,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T238, $AB238, BD238, $Y238, $W238,$AJ238,$AA238,\"dba\")+5)<15, \"<15\", soundLevel($T238, $AB238, BD238,$Y238, $W238,$AJ238,$AA238,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T238=\"Select Model\", \"\",IF(OR($T238=\"ACBC_1W\",$T238=\"ACBC_2W\",LEFT($T238,4)=\"ACBR\",$T238=\"LIU24_2W\",LEFT($T238,3)=\"RIU\",LEFT($T238,6)=\"ACBL12\"), IF((soundLevel($T238, $AB238, BD238, $Y238, $W238,$AJ238,$AA238,\"NC\"))<15,\"<15\",soundLevel($T238, $AB238, BD238, $Y238, $W238,$AJ238,$AA238,\"NC\")+0.4),IF((soundLevel($T238, $AB238, BD238, $Y238, $W238,$AJ238,$AA238,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T238, $AB238, BD238, $Y238, $W238,$AJ238,$AA238,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T238, $AB238, BD238, $Y238, $W238,$AJ238,$AA238,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T238=\"Select Model\",\"\",IF($T238=\"LIU24_2W\",calcQwIP($Y238,$W238,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC238,$AI238,\"latent\",$U238&\"P\"&IF($V238=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T238,activeElevation),\"\"))","v":""},{"$f":"IF($T238=\"Select Model\",\"\",IF($T238=\"ACBC_1W\",calcQwIP($Y238,$W238,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC238,BD238,\"capacity\",$U238&\"P\"&IF($V238=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T238,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y238,$W238,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC238,BD238,\"capacity\",$U238&\"P\"&IF($V238=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T238,activeElevation)))","v":""},"",{"$f":"IF(T238=\"Select Model\", 0,waterPressureDrop(W238, U238 & \"P\" & IF(V238=\"Dual\",2,1) &\"C\", AC238, \"cooling\", T238))","v":0},{"$f":"IF(T238=\"Select Model\", \"\",getReturnWaterTemp(T238,AC238, activeEWTCooling, AS238, \"cooling\"))","v":""},"",{"$f":"IF($T238<>\"ACBC_1W\",\"\",IF($J238=\"\",\"\",FintubeCapacity($T238,$W238,$AE238,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T238=\"Select Model\",T238=\"PCBL\"),\"\",calcQwIP(Y238,W238,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD238,BD238,\"capacity\",U238&\"P\"&IF(V238=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T238,activeElevation))","v":""},"",{"$f":"IF(OR(T238=\"Select Model\",T238=\"PCBL\"), \"\",IF(AY238=0,\"N/A\",waterPressureDrop(W238, U238 & \"P\" & IF(V238=\"Dual\",2,1) &\"C\", AD238, \"heating\", T238)))","v":""},{"$f":"IF(OR(T238=\"Select Model\",T238=\"PCBL\"), \"\",IF(AY238=0,getReturnWaterTemp(T238,AE238, activeEWTHeating, AX238, \"heating\"),getReturnWaterTemp(T238,AD238, activeEWTHeating, AY238, \"heating\")))","v":""},"",{"$f":" getNozzle(T238, W238, Y238, Z238, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I239)),I239<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I239, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H239)),H239<0),\"\",intlEstQuantity(T239, W239*12, H239)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T239=\"Select Model\",\"\",coilCircuitChange(W239, U239, AC239, T239,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T239=\"Select Model\",\"\",beamWidth(T239))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T239=\"Select Model\",T239=\"PCBL\"), 0,getSPIP(T239, W239, Y239, BD239, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T239=\"Select Model\", \"\",IF(T239=\"PCBL\",0,primaryAirSensibleCapacityIP($T239,$W239,activeRoomTempCooling,activePriAirTempCooling,$Y239,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T239=\"Select Model\",\"\",IF($T239=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y239,activeElevation)))","v":""},{"$f":"IF(OR(T239=\"Select Model\",T239=\"PCBL\"), 0,IF(AD239=0,0,-primaryAirSensibleCapacityIP($T239,$W239,activeRoomTempHeating,activePriAirTempHeating,$Y239,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T239=\"Select Model\", \"\", InductionRatio($T239,BD239,$W239,$Y239)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T239=\"Select Model\", \"\",IF($T239=\"PCBL\",\"N/A\",minVAVSetBack(AA239, Y239))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T239=\"Select Model\", \"\",IF($T239= \"PCBL\",\"N/A\",getDischargeAirTemp($T239,$V239,$AC239,$W239,BD239,$AL239, $Y239, $AS239, \"cooling\",activeElevation,$AB239,$AJ239,$AV239,$BB239))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T239=\"Select Model\",$T239=\"PCBL\"), \"\",getDischargeAirTemp($T239,$V239,$AD239,$W239,BD239,$AL239, $Y239, $AY239, \"heating\",activeElevation,$AB239,$AJ239,$AV239,$BB239)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T239=\"Select Model\", \"\",IF(OR($T239=\"ACBC_1W\",$T239=\"ACBC_2W\",LEFT($T239,4)=\"ACBR\",$T239 = \"LIU24_2W\",LEFT($T239,3)=\"RIU\",LEFT($T239,6)=\"ACBL12\"), IF((soundLevel($T239, $AB239, BD239, $Y239, $W239,$AJ239,$AA239,\"dba\"))<15,\"<15\",soundLevel($T239, $AB239, BD239, $Y239, $W239,$AJ239,$AA239,\"dba\")+0.4),IF((soundLevel($T239, $AB239, BD239, $Y239, $W239,$AJ239,$AA239,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T239, $AB239, BD239, $Y239, $W239,$AJ239,$AA239,\"dba\")+5)<15, \"<15\", soundLevel($T239, $AB239, BD239,$Y239, $W239,$AJ239,$AA239,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T239=\"Select Model\", \"\",IF(OR($T239=\"ACBC_1W\",$T239=\"ACBC_2W\",LEFT($T239,4)=\"ACBR\",$T239=\"LIU24_2W\",LEFT($T239,3)=\"RIU\",LEFT($T239,6)=\"ACBL12\"), IF((soundLevel($T239, $AB239, BD239, $Y239, $W239,$AJ239,$AA239,\"NC\"))<15,\"<15\",soundLevel($T239, $AB239, BD239, $Y239, $W239,$AJ239,$AA239,\"NC\")+0.4),IF((soundLevel($T239, $AB239, BD239, $Y239, $W239,$AJ239,$AA239,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T239, $AB239, BD239, $Y239, $W239,$AJ239,$AA239,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T239, $AB239, BD239, $Y239, $W239,$AJ239,$AA239,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T239=\"Select Model\",\"\",IF($T239=\"LIU24_2W\",calcQwIP($Y239,$W239,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC239,$AI239,\"latent\",$U239&\"P\"&IF($V239=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T239,activeElevation),\"\"))","v":""},{"$f":"IF($T239=\"Select Model\",\"\",IF($T239=\"ACBC_1W\",calcQwIP($Y239,$W239,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC239,BD239,\"capacity\",$U239&\"P\"&IF($V239=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T239,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y239,$W239,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC239,BD239,\"capacity\",$U239&\"P\"&IF($V239=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T239,activeElevation)))","v":""},"",{"$f":"IF(T239=\"Select Model\", 0,waterPressureDrop(W239, U239 & \"P\" & IF(V239=\"Dual\",2,1) &\"C\", AC239, \"cooling\", T239))","v":0},{"$f":"IF(T239=\"Select Model\", \"\",getReturnWaterTemp(T239,AC239, activeEWTCooling, AS239, \"cooling\"))","v":""},"",{"$f":"IF($T239<>\"ACBC_1W\",\"\",IF($J239=\"\",\"\",FintubeCapacity($T239,$W239,$AE239,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T239=\"Select Model\",T239=\"PCBL\"),\"\",calcQwIP(Y239,W239,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD239,BD239,\"capacity\",U239&\"P\"&IF(V239=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T239,activeElevation))","v":""},"",{"$f":"IF(OR(T239=\"Select Model\",T239=\"PCBL\"), \"\",IF(AY239=0,\"N/A\",waterPressureDrop(W239, U239 & \"P\" & IF(V239=\"Dual\",2,1) &\"C\", AD239, \"heating\", T239)))","v":""},{"$f":"IF(OR(T239=\"Select Model\",T239=\"PCBL\"), \"\",IF(AY239=0,getReturnWaterTemp(T239,AE239, activeEWTHeating, AX239, \"heating\"),getReturnWaterTemp(T239,AD239, activeEWTHeating, AY239, \"heating\")))","v":""},"",{"$f":" getNozzle(T239, W239, Y239, Z239, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I240)),I240<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I240, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H240)),H240<0),\"\",intlEstQuantity(T240, W240*12, H240)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T240=\"Select Model\",\"\",coilCircuitChange(W240, U240, AC240, T240,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T240=\"Select Model\",\"\",beamWidth(T240))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T240=\"Select Model\",T240=\"PCBL\"), 0,getSPIP(T240, W240, Y240, BD240, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T240=\"Select Model\", \"\",IF(T240=\"PCBL\",0,primaryAirSensibleCapacityIP($T240,$W240,activeRoomTempCooling,activePriAirTempCooling,$Y240,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T240=\"Select Model\",\"\",IF($T240=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y240,activeElevation)))","v":""},{"$f":"IF(OR(T240=\"Select Model\",T240=\"PCBL\"), 0,IF(AD240=0,0,-primaryAirSensibleCapacityIP($T240,$W240,activeRoomTempHeating,activePriAirTempHeating,$Y240,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T240=\"Select Model\", \"\", InductionRatio($T240,BD240,$W240,$Y240)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T240=\"Select Model\", \"\",IF($T240=\"PCBL\",\"N/A\",minVAVSetBack(AA240, Y240))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T240=\"Select Model\", \"\",IF($T240= \"PCBL\",\"N/A\",getDischargeAirTemp($T240,$V240,$AC240,$W240,BD240,$AL240, $Y240, $AS240, \"cooling\",activeElevation,$AB240,$AJ240,$AV240,$BB240))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T240=\"Select Model\",$T240=\"PCBL\"), \"\",getDischargeAirTemp($T240,$V240,$AD240,$W240,BD240,$AL240, $Y240, $AY240, \"heating\",activeElevation,$AB240,$AJ240,$AV240,$BB240)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T240=\"Select Model\", \"\",IF(OR($T240=\"ACBC_1W\",$T240=\"ACBC_2W\",LEFT($T240,4)=\"ACBR\",$T240 = \"LIU24_2W\",LEFT($T240,3)=\"RIU\",LEFT($T240,6)=\"ACBL12\"), IF((soundLevel($T240, $AB240, BD240, $Y240, $W240,$AJ240,$AA240,\"dba\"))<15,\"<15\",soundLevel($T240, $AB240, BD240, $Y240, $W240,$AJ240,$AA240,\"dba\")+0.4),IF((soundLevel($T240, $AB240, BD240, $Y240, $W240,$AJ240,$AA240,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T240, $AB240, BD240, $Y240, $W240,$AJ240,$AA240,\"dba\")+5)<15, \"<15\", soundLevel($T240, $AB240, BD240,$Y240, $W240,$AJ240,$AA240,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T240=\"Select Model\", \"\",IF(OR($T240=\"ACBC_1W\",$T240=\"ACBC_2W\",LEFT($T240,4)=\"ACBR\",$T240=\"LIU24_2W\",LEFT($T240,3)=\"RIU\",LEFT($T240,6)=\"ACBL12\"), IF((soundLevel($T240, $AB240, BD240, $Y240, $W240,$AJ240,$AA240,\"NC\"))<15,\"<15\",soundLevel($T240, $AB240, BD240, $Y240, $W240,$AJ240,$AA240,\"NC\")+0.4),IF((soundLevel($T240, $AB240, BD240, $Y240, $W240,$AJ240,$AA240,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T240, $AB240, BD240, $Y240, $W240,$AJ240,$AA240,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T240, $AB240, BD240, $Y240, $W240,$AJ240,$AA240,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T240=\"Select Model\",\"\",IF($T240=\"LIU24_2W\",calcQwIP($Y240,$W240,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC240,$AI240,\"latent\",$U240&\"P\"&IF($V240=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T240,activeElevation),\"\"))","v":""},{"$f":"IF($T240=\"Select Model\",\"\",IF($T240=\"ACBC_1W\",calcQwIP($Y240,$W240,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC240,BD240,\"capacity\",$U240&\"P\"&IF($V240=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T240,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y240,$W240,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC240,BD240,\"capacity\",$U240&\"P\"&IF($V240=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T240,activeElevation)))","v":""},"",{"$f":"IF(T240=\"Select Model\", 0,waterPressureDrop(W240, U240 & \"P\" & IF(V240=\"Dual\",2,1) &\"C\", AC240, \"cooling\", T240))","v":0},{"$f":"IF(T240=\"Select Model\", \"\",getReturnWaterTemp(T240,AC240, activeEWTCooling, AS240, \"cooling\"))","v":""},"",{"$f":"IF($T240<>\"ACBC_1W\",\"\",IF($J240=\"\",\"\",FintubeCapacity($T240,$W240,$AE240,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T240=\"Select Model\",T240=\"PCBL\"),\"\",calcQwIP(Y240,W240,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD240,BD240,\"capacity\",U240&\"P\"&IF(V240=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T240,activeElevation))","v":""},"",{"$f":"IF(OR(T240=\"Select Model\",T240=\"PCBL\"), \"\",IF(AY240=0,\"N/A\",waterPressureDrop(W240, U240 & \"P\" & IF(V240=\"Dual\",2,1) &\"C\", AD240, \"heating\", T240)))","v":""},{"$f":"IF(OR(T240=\"Select Model\",T240=\"PCBL\"), \"\",IF(AY240=0,getReturnWaterTemp(T240,AE240, activeEWTHeating, AX240, \"heating\"),getReturnWaterTemp(T240,AD240, activeEWTHeating, AY240, \"heating\")))","v":""},"",{"$f":" getNozzle(T240, W240, Y240, Z240, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I241)),I241<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I241, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H241)),H241<0),\"\",intlEstQuantity(T241, W241*12, H241)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T241=\"Select Model\",\"\",coilCircuitChange(W241, U241, AC241, T241,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T241=\"Select Model\",\"\",beamWidth(T241))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T241=\"Select Model\",T241=\"PCBL\"), 0,getSPIP(T241, W241, Y241, BD241, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T241=\"Select Model\", \"\",IF(T241=\"PCBL\",0,primaryAirSensibleCapacityIP($T241,$W241,activeRoomTempCooling,activePriAirTempCooling,$Y241,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T241=\"Select Model\",\"\",IF($T241=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y241,activeElevation)))","v":""},{"$f":"IF(OR(T241=\"Select Model\",T241=\"PCBL\"), 0,IF(AD241=0,0,-primaryAirSensibleCapacityIP($T241,$W241,activeRoomTempHeating,activePriAirTempHeating,$Y241,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T241=\"Select Model\", \"\", InductionRatio($T241,BD241,$W241,$Y241)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T241=\"Select Model\", \"\",IF($T241=\"PCBL\",\"N/A\",minVAVSetBack(AA241, Y241))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T241=\"Select Model\", \"\",IF($T241= \"PCBL\",\"N/A\",getDischargeAirTemp($T241,$V241,$AC241,$W241,BD241,$AL241, $Y241, $AS241, \"cooling\",activeElevation,$AB241,$AJ241,$AV241,$BB241))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T241=\"Select Model\",$T241=\"PCBL\"), \"\",getDischargeAirTemp($T241,$V241,$AD241,$W241,BD241,$AL241, $Y241, $AY241, \"heating\",activeElevation,$AB241,$AJ241,$AV241,$BB241)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T241=\"Select Model\", \"\",IF(OR($T241=\"ACBC_1W\",$T241=\"ACBC_2W\",LEFT($T241,4)=\"ACBR\",$T241 = \"LIU24_2W\",LEFT($T241,3)=\"RIU\",LEFT($T241,6)=\"ACBL12\"), IF((soundLevel($T241, $AB241, BD241, $Y241, $W241,$AJ241,$AA241,\"dba\"))<15,\"<15\",soundLevel($T241, $AB241, BD241, $Y241, $W241,$AJ241,$AA241,\"dba\")+0.4),IF((soundLevel($T241, $AB241, BD241, $Y241, $W241,$AJ241,$AA241,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T241, $AB241, BD241, $Y241, $W241,$AJ241,$AA241,\"dba\")+5)<15, \"<15\", soundLevel($T241, $AB241, BD241,$Y241, $W241,$AJ241,$AA241,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T241=\"Select Model\", \"\",IF(OR($T241=\"ACBC_1W\",$T241=\"ACBC_2W\",LEFT($T241,4)=\"ACBR\",$T241=\"LIU24_2W\",LEFT($T241,3)=\"RIU\",LEFT($T241,6)=\"ACBL12\"), IF((soundLevel($T241, $AB241, BD241, $Y241, $W241,$AJ241,$AA241,\"NC\"))<15,\"<15\",soundLevel($T241, $AB241, BD241, $Y241, $W241,$AJ241,$AA241,\"NC\")+0.4),IF((soundLevel($T241, $AB241, BD241, $Y241, $W241,$AJ241,$AA241,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T241, $AB241, BD241, $Y241, $W241,$AJ241,$AA241,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T241, $AB241, BD241, $Y241, $W241,$AJ241,$AA241,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T241=\"Select Model\",\"\",IF($T241=\"LIU24_2W\",calcQwIP($Y241,$W241,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC241,$AI241,\"latent\",$U241&\"P\"&IF($V241=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T241,activeElevation),\"\"))","v":""},{"$f":"IF($T241=\"Select Model\",\"\",IF($T241=\"ACBC_1W\",calcQwIP($Y241,$W241,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC241,BD241,\"capacity\",$U241&\"P\"&IF($V241=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T241,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y241,$W241,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC241,BD241,\"capacity\",$U241&\"P\"&IF($V241=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T241,activeElevation)))","v":""},"",{"$f":"IF(T241=\"Select Model\", 0,waterPressureDrop(W241, U241 & \"P\" & IF(V241=\"Dual\",2,1) &\"C\", AC241, \"cooling\", T241))","v":0},{"$f":"IF(T241=\"Select Model\", \"\",getReturnWaterTemp(T241,AC241, activeEWTCooling, AS241, \"cooling\"))","v":""},"",{"$f":"IF($T241<>\"ACBC_1W\",\"\",IF($J241=\"\",\"\",FintubeCapacity($T241,$W241,$AE241,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T241=\"Select Model\",T241=\"PCBL\"),\"\",calcQwIP(Y241,W241,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD241,BD241,\"capacity\",U241&\"P\"&IF(V241=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T241,activeElevation))","v":""},"",{"$f":"IF(OR(T241=\"Select Model\",T241=\"PCBL\"), \"\",IF(AY241=0,\"N/A\",waterPressureDrop(W241, U241 & \"P\" & IF(V241=\"Dual\",2,1) &\"C\", AD241, \"heating\", T241)))","v":""},{"$f":"IF(OR(T241=\"Select Model\",T241=\"PCBL\"), \"\",IF(AY241=0,getReturnWaterTemp(T241,AE241, activeEWTHeating, AX241, \"heating\"),getReturnWaterTemp(T241,AD241, activeEWTHeating, AY241, \"heating\")))","v":""},"",{"$f":" getNozzle(T241, W241, Y241, Z241, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I242)),I242<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I242, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H242)),H242<0),\"\",intlEstQuantity(T242, W242*12, H242)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T242=\"Select Model\",\"\",coilCircuitChange(W242, U242, AC242, T242,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T242=\"Select Model\",\"\",beamWidth(T242))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T242=\"Select Model\",T242=\"PCBL\"), 0,getSPIP(T242, W242, Y242, BD242, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T242=\"Select Model\", \"\",IF(T242=\"PCBL\",0,primaryAirSensibleCapacityIP($T242,$W242,activeRoomTempCooling,activePriAirTempCooling,$Y242,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T242=\"Select Model\",\"\",IF($T242=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y242,activeElevation)))","v":""},{"$f":"IF(OR(T242=\"Select Model\",T242=\"PCBL\"), 0,IF(AD242=0,0,-primaryAirSensibleCapacityIP($T242,$W242,activeRoomTempHeating,activePriAirTempHeating,$Y242,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T242=\"Select Model\", \"\", InductionRatio($T242,BD242,$W242,$Y242)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T242=\"Select Model\", \"\",IF($T242=\"PCBL\",\"N/A\",minVAVSetBack(AA242, Y242))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T242=\"Select Model\", \"\",IF($T242= \"PCBL\",\"N/A\",getDischargeAirTemp($T242,$V242,$AC242,$W242,BD242,$AL242, $Y242, $AS242, \"cooling\",activeElevation,$AB242,$AJ242,$AV242,$BB242))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T242=\"Select Model\",$T242=\"PCBL\"), \"\",getDischargeAirTemp($T242,$V242,$AD242,$W242,BD242,$AL242, $Y242, $AY242, \"heating\",activeElevation,$AB242,$AJ242,$AV242,$BB242)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T242=\"Select Model\", \"\",IF(OR($T242=\"ACBC_1W\",$T242=\"ACBC_2W\",LEFT($T242,4)=\"ACBR\",$T242 = \"LIU24_2W\",LEFT($T242,3)=\"RIU\",LEFT($T242,6)=\"ACBL12\"), IF((soundLevel($T242, $AB242, BD242, $Y242, $W242,$AJ242,$AA242,\"dba\"))<15,\"<15\",soundLevel($T242, $AB242, BD242, $Y242, $W242,$AJ242,$AA242,\"dba\")+0.4),IF((soundLevel($T242, $AB242, BD242, $Y242, $W242,$AJ242,$AA242,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T242, $AB242, BD242, $Y242, $W242,$AJ242,$AA242,\"dba\")+5)<15, \"<15\", soundLevel($T242, $AB242, BD242,$Y242, $W242,$AJ242,$AA242,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T242=\"Select Model\", \"\",IF(OR($T242=\"ACBC_1W\",$T242=\"ACBC_2W\",LEFT($T242,4)=\"ACBR\",$T242=\"LIU24_2W\",LEFT($T242,3)=\"RIU\",LEFT($T242,6)=\"ACBL12\"), IF((soundLevel($T242, $AB242, BD242, $Y242, $W242,$AJ242,$AA242,\"NC\"))<15,\"<15\",soundLevel($T242, $AB242, BD242, $Y242, $W242,$AJ242,$AA242,\"NC\")+0.4),IF((soundLevel($T242, $AB242, BD242, $Y242, $W242,$AJ242,$AA242,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T242, $AB242, BD242, $Y242, $W242,$AJ242,$AA242,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T242, $AB242, BD242, $Y242, $W242,$AJ242,$AA242,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T242=\"Select Model\",\"\",IF($T242=\"LIU24_2W\",calcQwIP($Y242,$W242,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC242,$AI242,\"latent\",$U242&\"P\"&IF($V242=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T242,activeElevation),\"\"))","v":""},{"$f":"IF($T242=\"Select Model\",\"\",IF($T242=\"ACBC_1W\",calcQwIP($Y242,$W242,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC242,BD242,\"capacity\",$U242&\"P\"&IF($V242=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T242,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y242,$W242,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC242,BD242,\"capacity\",$U242&\"P\"&IF($V242=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T242,activeElevation)))","v":""},"",{"$f":"IF(T242=\"Select Model\", 0,waterPressureDrop(W242, U242 & \"P\" & IF(V242=\"Dual\",2,1) &\"C\", AC242, \"cooling\", T242))","v":0},{"$f":"IF(T242=\"Select Model\", \"\",getReturnWaterTemp(T242,AC242, activeEWTCooling, AS242, \"cooling\"))","v":""},"",{"$f":"IF($T242<>\"ACBC_1W\",\"\",IF($J242=\"\",\"\",FintubeCapacity($T242,$W242,$AE242,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T242=\"Select Model\",T242=\"PCBL\"),\"\",calcQwIP(Y242,W242,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD242,BD242,\"capacity\",U242&\"P\"&IF(V242=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T242,activeElevation))","v":""},"",{"$f":"IF(OR(T242=\"Select Model\",T242=\"PCBL\"), \"\",IF(AY242=0,\"N/A\",waterPressureDrop(W242, U242 & \"P\" & IF(V242=\"Dual\",2,1) &\"C\", AD242, \"heating\", T242)))","v":""},{"$f":"IF(OR(T242=\"Select Model\",T242=\"PCBL\"), \"\",IF(AY242=0,getReturnWaterTemp(T242,AE242, activeEWTHeating, AX242, \"heating\"),getReturnWaterTemp(T242,AD242, activeEWTHeating, AY242, \"heating\")))","v":""},"",{"$f":" getNozzle(T242, W242, Y242, Z242, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I243)),I243<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I243, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H243)),H243<0),\"\",intlEstQuantity(T243, W243*12, H243)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T243=\"Select Model\",\"\",coilCircuitChange(W243, U243, AC243, T243,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T243=\"Select Model\",\"\",beamWidth(T243))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T243=\"Select Model\",T243=\"PCBL\"), 0,getSPIP(T243, W243, Y243, BD243, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T243=\"Select Model\", \"\",IF(T243=\"PCBL\",0,primaryAirSensibleCapacityIP($T243,$W243,activeRoomTempCooling,activePriAirTempCooling,$Y243,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T243=\"Select Model\",\"\",IF($T243=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y243,activeElevation)))","v":""},{"$f":"IF(OR(T243=\"Select Model\",T243=\"PCBL\"), 0,IF(AD243=0,0,-primaryAirSensibleCapacityIP($T243,$W243,activeRoomTempHeating,activePriAirTempHeating,$Y243,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T243=\"Select Model\", \"\", InductionRatio($T243,BD243,$W243,$Y243)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T243=\"Select Model\", \"\",IF($T243=\"PCBL\",\"N/A\",minVAVSetBack(AA243, Y243))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T243=\"Select Model\", \"\",IF($T243= \"PCBL\",\"N/A\",getDischargeAirTemp($T243,$V243,$AC243,$W243,BD243,$AL243, $Y243, $AS243, \"cooling\",activeElevation,$AB243,$AJ243,$AV243,$BB243))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T243=\"Select Model\",$T243=\"PCBL\"), \"\",getDischargeAirTemp($T243,$V243,$AD243,$W243,BD243,$AL243, $Y243, $AY243, \"heating\",activeElevation,$AB243,$AJ243,$AV243,$BB243)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T243=\"Select Model\", \"\",IF(OR($T243=\"ACBC_1W\",$T243=\"ACBC_2W\",LEFT($T243,4)=\"ACBR\",$T243 = \"LIU24_2W\",LEFT($T243,3)=\"RIU\",LEFT($T243,6)=\"ACBL12\"), IF((soundLevel($T243, $AB243, BD243, $Y243, $W243,$AJ243,$AA243,\"dba\"))<15,\"<15\",soundLevel($T243, $AB243, BD243, $Y243, $W243,$AJ243,$AA243,\"dba\")+0.4),IF((soundLevel($T243, $AB243, BD243, $Y243, $W243,$AJ243,$AA243,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T243, $AB243, BD243, $Y243, $W243,$AJ243,$AA243,\"dba\")+5)<15, \"<15\", soundLevel($T243, $AB243, BD243,$Y243, $W243,$AJ243,$AA243,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T243=\"Select Model\", \"\",IF(OR($T243=\"ACBC_1W\",$T243=\"ACBC_2W\",LEFT($T243,4)=\"ACBR\",$T243=\"LIU24_2W\",LEFT($T243,3)=\"RIU\",LEFT($T243,6)=\"ACBL12\"), IF((soundLevel($T243, $AB243, BD243, $Y243, $W243,$AJ243,$AA243,\"NC\"))<15,\"<15\",soundLevel($T243, $AB243, BD243, $Y243, $W243,$AJ243,$AA243,\"NC\")+0.4),IF((soundLevel($T243, $AB243, BD243, $Y243, $W243,$AJ243,$AA243,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T243, $AB243, BD243, $Y243, $W243,$AJ243,$AA243,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T243, $AB243, BD243, $Y243, $W243,$AJ243,$AA243,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T243=\"Select Model\",\"\",IF($T243=\"LIU24_2W\",calcQwIP($Y243,$W243,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC243,$AI243,\"latent\",$U243&\"P\"&IF($V243=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T243,activeElevation),\"\"))","v":""},{"$f":"IF($T243=\"Select Model\",\"\",IF($T243=\"ACBC_1W\",calcQwIP($Y243,$W243,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC243,BD243,\"capacity\",$U243&\"P\"&IF($V243=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T243,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y243,$W243,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC243,BD243,\"capacity\",$U243&\"P\"&IF($V243=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T243,activeElevation)))","v":""},"",{"$f":"IF(T243=\"Select Model\", 0,waterPressureDrop(W243, U243 & \"P\" & IF(V243=\"Dual\",2,1) &\"C\", AC243, \"cooling\", T243))","v":0},{"$f":"IF(T243=\"Select Model\", \"\",getReturnWaterTemp(T243,AC243, activeEWTCooling, AS243, \"cooling\"))","v":""},"",{"$f":"IF($T243<>\"ACBC_1W\",\"\",IF($J243=\"\",\"\",FintubeCapacity($T243,$W243,$AE243,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T243=\"Select Model\",T243=\"PCBL\"),\"\",calcQwIP(Y243,W243,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD243,BD243,\"capacity\",U243&\"P\"&IF(V243=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T243,activeElevation))","v":""},"",{"$f":"IF(OR(T243=\"Select Model\",T243=\"PCBL\"), \"\",IF(AY243=0,\"N/A\",waterPressureDrop(W243, U243 & \"P\" & IF(V243=\"Dual\",2,1) &\"C\", AD243, \"heating\", T243)))","v":""},{"$f":"IF(OR(T243=\"Select Model\",T243=\"PCBL\"), \"\",IF(AY243=0,getReturnWaterTemp(T243,AE243, activeEWTHeating, AX243, \"heating\"),getReturnWaterTemp(T243,AD243, activeEWTHeating, AY243, \"heating\")))","v":""},"",{"$f":" getNozzle(T243, W243, Y243, Z243, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I244)),I244<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I244, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H244)),H244<0),\"\",intlEstQuantity(T244, W244*12, H244)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T244=\"Select Model\",\"\",coilCircuitChange(W244, U244, AC244, T244,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T244=\"Select Model\",\"\",beamWidth(T244))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T244=\"Select Model\",T244=\"PCBL\"), 0,getSPIP(T244, W244, Y244, BD244, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T244=\"Select Model\", \"\",IF(T244=\"PCBL\",0,primaryAirSensibleCapacityIP($T244,$W244,activeRoomTempCooling,activePriAirTempCooling,$Y244,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T244=\"Select Model\",\"\",IF($T244=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y244,activeElevation)))","v":""},{"$f":"IF(OR(T244=\"Select Model\",T244=\"PCBL\"), 0,IF(AD244=0,0,-primaryAirSensibleCapacityIP($T244,$W244,activeRoomTempHeating,activePriAirTempHeating,$Y244,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T244=\"Select Model\", \"\", InductionRatio($T244,BD244,$W244,$Y244)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T244=\"Select Model\", \"\",IF($T244=\"PCBL\",\"N/A\",minVAVSetBack(AA244, Y244))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T244=\"Select Model\", \"\",IF($T244= \"PCBL\",\"N/A\",getDischargeAirTemp($T244,$V244,$AC244,$W244,BD244,$AL244, $Y244, $AS244, \"cooling\",activeElevation,$AB244,$AJ244,$AV244,$BB244))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T244=\"Select Model\",$T244=\"PCBL\"), \"\",getDischargeAirTemp($T244,$V244,$AD244,$W244,BD244,$AL244, $Y244, $AY244, \"heating\",activeElevation,$AB244,$AJ244,$AV244,$BB244)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T244=\"Select Model\", \"\",IF(OR($T244=\"ACBC_1W\",$T244=\"ACBC_2W\",LEFT($T244,4)=\"ACBR\",$T244 = \"LIU24_2W\",LEFT($T244,3)=\"RIU\",LEFT($T244,6)=\"ACBL12\"), IF((soundLevel($T244, $AB244, BD244, $Y244, $W244,$AJ244,$AA244,\"dba\"))<15,\"<15\",soundLevel($T244, $AB244, BD244, $Y244, $W244,$AJ244,$AA244,\"dba\")+0.4),IF((soundLevel($T244, $AB244, BD244, $Y244, $W244,$AJ244,$AA244,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T244, $AB244, BD244, $Y244, $W244,$AJ244,$AA244,\"dba\")+5)<15, \"<15\", soundLevel($T244, $AB244, BD244,$Y244, $W244,$AJ244,$AA244,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T244=\"Select Model\", \"\",IF(OR($T244=\"ACBC_1W\",$T244=\"ACBC_2W\",LEFT($T244,4)=\"ACBR\",$T244=\"LIU24_2W\",LEFT($T244,3)=\"RIU\",LEFT($T244,6)=\"ACBL12\"), IF((soundLevel($T244, $AB244, BD244, $Y244, $W244,$AJ244,$AA244,\"NC\"))<15,\"<15\",soundLevel($T244, $AB244, BD244, $Y244, $W244,$AJ244,$AA244,\"NC\")+0.4),IF((soundLevel($T244, $AB244, BD244, $Y244, $W244,$AJ244,$AA244,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T244, $AB244, BD244, $Y244, $W244,$AJ244,$AA244,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T244, $AB244, BD244, $Y244, $W244,$AJ244,$AA244,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T244=\"Select Model\",\"\",IF($T244=\"LIU24_2W\",calcQwIP($Y244,$W244,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC244,$AI244,\"latent\",$U244&\"P\"&IF($V244=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T244,activeElevation),\"\"))","v":""},{"$f":"IF($T244=\"Select Model\",\"\",IF($T244=\"ACBC_1W\",calcQwIP($Y244,$W244,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC244,BD244,\"capacity\",$U244&\"P\"&IF($V244=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T244,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y244,$W244,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC244,BD244,\"capacity\",$U244&\"P\"&IF($V244=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T244,activeElevation)))","v":""},"",{"$f":"IF(T244=\"Select Model\", 0,waterPressureDrop(W244, U244 & \"P\" & IF(V244=\"Dual\",2,1) &\"C\", AC244, \"cooling\", T244))","v":0},{"$f":"IF(T244=\"Select Model\", \"\",getReturnWaterTemp(T244,AC244, activeEWTCooling, AS244, \"cooling\"))","v":""},"",{"$f":"IF($T244<>\"ACBC_1W\",\"\",IF($J244=\"\",\"\",FintubeCapacity($T244,$W244,$AE244,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T244=\"Select Model\",T244=\"PCBL\"),\"\",calcQwIP(Y244,W244,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD244,BD244,\"capacity\",U244&\"P\"&IF(V244=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T244,activeElevation))","v":""},"",{"$f":"IF(OR(T244=\"Select Model\",T244=\"PCBL\"), \"\",IF(AY244=0,\"N/A\",waterPressureDrop(W244, U244 & \"P\" & IF(V244=\"Dual\",2,1) &\"C\", AD244, \"heating\", T244)))","v":""},{"$f":"IF(OR(T244=\"Select Model\",T244=\"PCBL\"), \"\",IF(AY244=0,getReturnWaterTemp(T244,AE244, activeEWTHeating, AX244, \"heating\"),getReturnWaterTemp(T244,AD244, activeEWTHeating, AY244, \"heating\")))","v":""},"",{"$f":" getNozzle(T244, W244, Y244, Z244, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I245)),I245<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I245, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H245)),H245<0),\"\",intlEstQuantity(T245, W245*12, H245)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T245=\"Select Model\",\"\",coilCircuitChange(W245, U245, AC245, T245,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T245=\"Select Model\",\"\",beamWidth(T245))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T245=\"Select Model\",T245=\"PCBL\"), 0,getSPIP(T245, W245, Y245, BD245, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T245=\"Select Model\", \"\",IF(T245=\"PCBL\",0,primaryAirSensibleCapacityIP($T245,$W245,activeRoomTempCooling,activePriAirTempCooling,$Y245,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T245=\"Select Model\",\"\",IF($T245=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y245,activeElevation)))","v":""},{"$f":"IF(OR(T245=\"Select Model\",T245=\"PCBL\"), 0,IF(AD245=0,0,-primaryAirSensibleCapacityIP($T245,$W245,activeRoomTempHeating,activePriAirTempHeating,$Y245,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T245=\"Select Model\", \"\", InductionRatio($T245,BD245,$W245,$Y245)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T245=\"Select Model\", \"\",IF($T245=\"PCBL\",\"N/A\",minVAVSetBack(AA245, Y245))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T245=\"Select Model\", \"\",IF($T245= \"PCBL\",\"N/A\",getDischargeAirTemp($T245,$V245,$AC245,$W245,BD245,$AL245, $Y245, $AS245, \"cooling\",activeElevation,$AB245,$AJ245,$AV245,$BB245))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T245=\"Select Model\",$T245=\"PCBL\"), \"\",getDischargeAirTemp($T245,$V245,$AD245,$W245,BD245,$AL245, $Y245, $AY245, \"heating\",activeElevation,$AB245,$AJ245,$AV245,$BB245)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T245=\"Select Model\", \"\",IF(OR($T245=\"ACBC_1W\",$T245=\"ACBC_2W\",LEFT($T245,4)=\"ACBR\",$T245 = \"LIU24_2W\",LEFT($T245,3)=\"RIU\",LEFT($T245,6)=\"ACBL12\"), IF((soundLevel($T245, $AB245, BD245, $Y245, $W245,$AJ245,$AA245,\"dba\"))<15,\"<15\",soundLevel($T245, $AB245, BD245, $Y245, $W245,$AJ245,$AA245,\"dba\")+0.4),IF((soundLevel($T245, $AB245, BD245, $Y245, $W245,$AJ245,$AA245,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T245, $AB245, BD245, $Y245, $W245,$AJ245,$AA245,\"dba\")+5)<15, \"<15\", soundLevel($T245, $AB245, BD245,$Y245, $W245,$AJ245,$AA245,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T245=\"Select Model\", \"\",IF(OR($T245=\"ACBC_1W\",$T245=\"ACBC_2W\",LEFT($T245,4)=\"ACBR\",$T245=\"LIU24_2W\",LEFT($T245,3)=\"RIU\",LEFT($T245,6)=\"ACBL12\"), IF((soundLevel($T245, $AB245, BD245, $Y245, $W245,$AJ245,$AA245,\"NC\"))<15,\"<15\",soundLevel($T245, $AB245, BD245, $Y245, $W245,$AJ245,$AA245,\"NC\")+0.4),IF((soundLevel($T245, $AB245, BD245, $Y245, $W245,$AJ245,$AA245,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T245, $AB245, BD245, $Y245, $W245,$AJ245,$AA245,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T245, $AB245, BD245, $Y245, $W245,$AJ245,$AA245,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T245=\"Select Model\",\"\",IF($T245=\"LIU24_2W\",calcQwIP($Y245,$W245,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC245,$AI245,\"latent\",$U245&\"P\"&IF($V245=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T245,activeElevation),\"\"))","v":""},{"$f":"IF($T245=\"Select Model\",\"\",IF($T245=\"ACBC_1W\",calcQwIP($Y245,$W245,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC245,BD245,\"capacity\",$U245&\"P\"&IF($V245=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T245,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y245,$W245,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC245,BD245,\"capacity\",$U245&\"P\"&IF($V245=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T245,activeElevation)))","v":""},"",{"$f":"IF(T245=\"Select Model\", 0,waterPressureDrop(W245, U245 & \"P\" & IF(V245=\"Dual\",2,1) &\"C\", AC245, \"cooling\", T245))","v":0},{"$f":"IF(T245=\"Select Model\", \"\",getReturnWaterTemp(T245,AC245, activeEWTCooling, AS245, \"cooling\"))","v":""},"",{"$f":"IF($T245<>\"ACBC_1W\",\"\",IF($J245=\"\",\"\",FintubeCapacity($T245,$W245,$AE245,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T245=\"Select Model\",T245=\"PCBL\"),\"\",calcQwIP(Y245,W245,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD245,BD245,\"capacity\",U245&\"P\"&IF(V245=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T245,activeElevation))","v":""},"",{"$f":"IF(OR(T245=\"Select Model\",T245=\"PCBL\"), \"\",IF(AY245=0,\"N/A\",waterPressureDrop(W245, U245 & \"P\" & IF(V245=\"Dual\",2,1) &\"C\", AD245, \"heating\", T245)))","v":""},{"$f":"IF(OR(T245=\"Select Model\",T245=\"PCBL\"), \"\",IF(AY245=0,getReturnWaterTemp(T245,AE245, activeEWTHeating, AX245, \"heating\"),getReturnWaterTemp(T245,AD245, activeEWTHeating, AY245, \"heating\")))","v":""},"",{"$f":" getNozzle(T245, W245, Y245, Z245, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I246)),I246<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I246, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H246)),H246<0),\"\",intlEstQuantity(T246, W246*12, H246)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T246=\"Select Model\",\"\",coilCircuitChange(W246, U246, AC246, T246,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T246=\"Select Model\",\"\",beamWidth(T246))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T246=\"Select Model\",T246=\"PCBL\"), 0,getSPIP(T246, W246, Y246, BD246, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T246=\"Select Model\", \"\",IF(T246=\"PCBL\",0,primaryAirSensibleCapacityIP($T246,$W246,activeRoomTempCooling,activePriAirTempCooling,$Y246,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T246=\"Select Model\",\"\",IF($T246=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y246,activeElevation)))","v":""},{"$f":"IF(OR(T246=\"Select Model\",T246=\"PCBL\"), 0,IF(AD246=0,0,-primaryAirSensibleCapacityIP($T246,$W246,activeRoomTempHeating,activePriAirTempHeating,$Y246,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T246=\"Select Model\", \"\", InductionRatio($T246,BD246,$W246,$Y246)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T246=\"Select Model\", \"\",IF($T246=\"PCBL\",\"N/A\",minVAVSetBack(AA246, Y246))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T246=\"Select Model\", \"\",IF($T246= \"PCBL\",\"N/A\",getDischargeAirTemp($T246,$V246,$AC246,$W246,BD246,$AL246, $Y246, $AS246, \"cooling\",activeElevation,$AB246,$AJ246,$AV246,$BB246))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T246=\"Select Model\",$T246=\"PCBL\"), \"\",getDischargeAirTemp($T246,$V246,$AD246,$W246,BD246,$AL246, $Y246, $AY246, \"heating\",activeElevation,$AB246,$AJ246,$AV246,$BB246)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T246=\"Select Model\", \"\",IF(OR($T246=\"ACBC_1W\",$T246=\"ACBC_2W\",LEFT($T246,4)=\"ACBR\",$T246 = \"LIU24_2W\",LEFT($T246,3)=\"RIU\",LEFT($T246,6)=\"ACBL12\"), IF((soundLevel($T246, $AB246, BD246, $Y246, $W246,$AJ246,$AA246,\"dba\"))<15,\"<15\",soundLevel($T246, $AB246, BD246, $Y246, $W246,$AJ246,$AA246,\"dba\")+0.4),IF((soundLevel($T246, $AB246, BD246, $Y246, $W246,$AJ246,$AA246,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T246, $AB246, BD246, $Y246, $W246,$AJ246,$AA246,\"dba\")+5)<15, \"<15\", soundLevel($T246, $AB246, BD246,$Y246, $W246,$AJ246,$AA246,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T246=\"Select Model\", \"\",IF(OR($T246=\"ACBC_1W\",$T246=\"ACBC_2W\",LEFT($T246,4)=\"ACBR\",$T246=\"LIU24_2W\",LEFT($T246,3)=\"RIU\",LEFT($T246,6)=\"ACBL12\"), IF((soundLevel($T246, $AB246, BD246, $Y246, $W246,$AJ246,$AA246,\"NC\"))<15,\"<15\",soundLevel($T246, $AB246, BD246, $Y246, $W246,$AJ246,$AA246,\"NC\")+0.4),IF((soundLevel($T246, $AB246, BD246, $Y246, $W246,$AJ246,$AA246,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T246, $AB246, BD246, $Y246, $W246,$AJ246,$AA246,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T246, $AB246, BD246, $Y246, $W246,$AJ246,$AA246,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T246=\"Select Model\",\"\",IF($T246=\"LIU24_2W\",calcQwIP($Y246,$W246,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC246,$AI246,\"latent\",$U246&\"P\"&IF($V246=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T246,activeElevation),\"\"))","v":""},{"$f":"IF($T246=\"Select Model\",\"\",IF($T246=\"ACBC_1W\",calcQwIP($Y246,$W246,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC246,BD246,\"capacity\",$U246&\"P\"&IF($V246=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T246,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y246,$W246,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC246,BD246,\"capacity\",$U246&\"P\"&IF($V246=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T246,activeElevation)))","v":""},"",{"$f":"IF(T246=\"Select Model\", 0,waterPressureDrop(W246, U246 & \"P\" & IF(V246=\"Dual\",2,1) &\"C\", AC246, \"cooling\", T246))","v":0},{"$f":"IF(T246=\"Select Model\", \"\",getReturnWaterTemp(T246,AC246, activeEWTCooling, AS246, \"cooling\"))","v":""},"",{"$f":"IF($T246<>\"ACBC_1W\",\"\",IF($J246=\"\",\"\",FintubeCapacity($T246,$W246,$AE246,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T246=\"Select Model\",T246=\"PCBL\"),\"\",calcQwIP(Y246,W246,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD246,BD246,\"capacity\",U246&\"P\"&IF(V246=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T246,activeElevation))","v":""},"",{"$f":"IF(OR(T246=\"Select Model\",T246=\"PCBL\"), \"\",IF(AY246=0,\"N/A\",waterPressureDrop(W246, U246 & \"P\" & IF(V246=\"Dual\",2,1) &\"C\", AD246, \"heating\", T246)))","v":""},{"$f":"IF(OR(T246=\"Select Model\",T246=\"PCBL\"), \"\",IF(AY246=0,getReturnWaterTemp(T246,AE246, activeEWTHeating, AX246, \"heating\"),getReturnWaterTemp(T246,AD246, activeEWTHeating, AY246, \"heating\")))","v":""},"",{"$f":" getNozzle(T246, W246, Y246, Z246, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I247)),I247<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I247, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H247)),H247<0),\"\",intlEstQuantity(T247, W247*12, H247)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T247=\"Select Model\",\"\",coilCircuitChange(W247, U247, AC247, T247,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T247=\"Select Model\",\"\",beamWidth(T247))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T247=\"Select Model\",T247=\"PCBL\"), 0,getSPIP(T247, W247, Y247, BD247, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T247=\"Select Model\", \"\",IF(T247=\"PCBL\",0,primaryAirSensibleCapacityIP($T247,$W247,activeRoomTempCooling,activePriAirTempCooling,$Y247,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T247=\"Select Model\",\"\",IF($T247=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y247,activeElevation)))","v":""},{"$f":"IF(OR(T247=\"Select Model\",T247=\"PCBL\"), 0,IF(AD247=0,0,-primaryAirSensibleCapacityIP($T247,$W247,activeRoomTempHeating,activePriAirTempHeating,$Y247,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T247=\"Select Model\", \"\", InductionRatio($T247,BD247,$W247,$Y247)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T247=\"Select Model\", \"\",IF($T247=\"PCBL\",\"N/A\",minVAVSetBack(AA247, Y247))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T247=\"Select Model\", \"\",IF($T247= \"PCBL\",\"N/A\",getDischargeAirTemp($T247,$V247,$AC247,$W247,BD247,$AL247, $Y247, $AS247, \"cooling\",activeElevation,$AB247,$AJ247,$AV247,$BB247))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T247=\"Select Model\",$T247=\"PCBL\"), \"\",getDischargeAirTemp($T247,$V247,$AD247,$W247,BD247,$AL247, $Y247, $AY247, \"heating\",activeElevation,$AB247,$AJ247,$AV247,$BB247)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T247=\"Select Model\", \"\",IF(OR($T247=\"ACBC_1W\",$T247=\"ACBC_2W\",LEFT($T247,4)=\"ACBR\",$T247 = \"LIU24_2W\",LEFT($T247,3)=\"RIU\",LEFT($T247,6)=\"ACBL12\"), IF((soundLevel($T247, $AB247, BD247, $Y247, $W247,$AJ247,$AA247,\"dba\"))<15,\"<15\",soundLevel($T247, $AB247, BD247, $Y247, $W247,$AJ247,$AA247,\"dba\")+0.4),IF((soundLevel($T247, $AB247, BD247, $Y247, $W247,$AJ247,$AA247,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T247, $AB247, BD247, $Y247, $W247,$AJ247,$AA247,\"dba\")+5)<15, \"<15\", soundLevel($T247, $AB247, BD247,$Y247, $W247,$AJ247,$AA247,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T247=\"Select Model\", \"\",IF(OR($T247=\"ACBC_1W\",$T247=\"ACBC_2W\",LEFT($T247,4)=\"ACBR\",$T247=\"LIU24_2W\",LEFT($T247,3)=\"RIU\",LEFT($T247,6)=\"ACBL12\"), IF((soundLevel($T247, $AB247, BD247, $Y247, $W247,$AJ247,$AA247,\"NC\"))<15,\"<15\",soundLevel($T247, $AB247, BD247, $Y247, $W247,$AJ247,$AA247,\"NC\")+0.4),IF((soundLevel($T247, $AB247, BD247, $Y247, $W247,$AJ247,$AA247,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T247, $AB247, BD247, $Y247, $W247,$AJ247,$AA247,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T247, $AB247, BD247, $Y247, $W247,$AJ247,$AA247,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T247=\"Select Model\",\"\",IF($T247=\"LIU24_2W\",calcQwIP($Y247,$W247,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC247,$AI247,\"latent\",$U247&\"P\"&IF($V247=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T247,activeElevation),\"\"))","v":""},{"$f":"IF($T247=\"Select Model\",\"\",IF($T247=\"ACBC_1W\",calcQwIP($Y247,$W247,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC247,BD247,\"capacity\",$U247&\"P\"&IF($V247=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T247,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y247,$W247,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC247,BD247,\"capacity\",$U247&\"P\"&IF($V247=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T247,activeElevation)))","v":""},"",{"$f":"IF(T247=\"Select Model\", 0,waterPressureDrop(W247, U247 & \"P\" & IF(V247=\"Dual\",2,1) &\"C\", AC247, \"cooling\", T247))","v":0},{"$f":"IF(T247=\"Select Model\", \"\",getReturnWaterTemp(T247,AC247, activeEWTCooling, AS247, \"cooling\"))","v":""},"",{"$f":"IF($T247<>\"ACBC_1W\",\"\",IF($J247=\"\",\"\",FintubeCapacity($T247,$W247,$AE247,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T247=\"Select Model\",T247=\"PCBL\"),\"\",calcQwIP(Y247,W247,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD247,BD247,\"capacity\",U247&\"P\"&IF(V247=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T247,activeElevation))","v":""},"",{"$f":"IF(OR(T247=\"Select Model\",T247=\"PCBL\"), \"\",IF(AY247=0,\"N/A\",waterPressureDrop(W247, U247 & \"P\" & IF(V247=\"Dual\",2,1) &\"C\", AD247, \"heating\", T247)))","v":""},{"$f":"IF(OR(T247=\"Select Model\",T247=\"PCBL\"), \"\",IF(AY247=0,getReturnWaterTemp(T247,AE247, activeEWTHeating, AX247, \"heating\"),getReturnWaterTemp(T247,AD247, activeEWTHeating, AY247, \"heating\")))","v":""},"",{"$f":" getNozzle(T247, W247, Y247, Z247, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I248)),I248<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I248, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H248)),H248<0),\"\",intlEstQuantity(T248, W248*12, H248)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T248=\"Select Model\",\"\",coilCircuitChange(W248, U248, AC248, T248,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T248=\"Select Model\",\"\",beamWidth(T248))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T248=\"Select Model\",T248=\"PCBL\"), 0,getSPIP(T248, W248, Y248, BD248, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T248=\"Select Model\", \"\",IF(T248=\"PCBL\",0,primaryAirSensibleCapacityIP($T248,$W248,activeRoomTempCooling,activePriAirTempCooling,$Y248,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T248=\"Select Model\",\"\",IF($T248=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y248,activeElevation)))","v":""},{"$f":"IF(OR(T248=\"Select Model\",T248=\"PCBL\"), 0,IF(AD248=0,0,-primaryAirSensibleCapacityIP($T248,$W248,activeRoomTempHeating,activePriAirTempHeating,$Y248,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T248=\"Select Model\", \"\", InductionRatio($T248,BD248,$W248,$Y248)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T248=\"Select Model\", \"\",IF($T248=\"PCBL\",\"N/A\",minVAVSetBack(AA248, Y248))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T248=\"Select Model\", \"\",IF($T248= \"PCBL\",\"N/A\",getDischargeAirTemp($T248,$V248,$AC248,$W248,BD248,$AL248, $Y248, $AS248, \"cooling\",activeElevation,$AB248,$AJ248,$AV248,$BB248))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T248=\"Select Model\",$T248=\"PCBL\"), \"\",getDischargeAirTemp($T248,$V248,$AD248,$W248,BD248,$AL248, $Y248, $AY248, \"heating\",activeElevation,$AB248,$AJ248,$AV248,$BB248)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T248=\"Select Model\", \"\",IF(OR($T248=\"ACBC_1W\",$T248=\"ACBC_2W\",LEFT($T248,4)=\"ACBR\",$T248 = \"LIU24_2W\",LEFT($T248,3)=\"RIU\",LEFT($T248,6)=\"ACBL12\"), IF((soundLevel($T248, $AB248, BD248, $Y248, $W248,$AJ248,$AA248,\"dba\"))<15,\"<15\",soundLevel($T248, $AB248, BD248, $Y248, $W248,$AJ248,$AA248,\"dba\")+0.4),IF((soundLevel($T248, $AB248, BD248, $Y248, $W248,$AJ248,$AA248,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T248, $AB248, BD248, $Y248, $W248,$AJ248,$AA248,\"dba\")+5)<15, \"<15\", soundLevel($T248, $AB248, BD248,$Y248, $W248,$AJ248,$AA248,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T248=\"Select Model\", \"\",IF(OR($T248=\"ACBC_1W\",$T248=\"ACBC_2W\",LEFT($T248,4)=\"ACBR\",$T248=\"LIU24_2W\",LEFT($T248,3)=\"RIU\",LEFT($T248,6)=\"ACBL12\"), IF((soundLevel($T248, $AB248, BD248, $Y248, $W248,$AJ248,$AA248,\"NC\"))<15,\"<15\",soundLevel($T248, $AB248, BD248, $Y248, $W248,$AJ248,$AA248,\"NC\")+0.4),IF((soundLevel($T248, $AB248, BD248, $Y248, $W248,$AJ248,$AA248,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T248, $AB248, BD248, $Y248, $W248,$AJ248,$AA248,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T248, $AB248, BD248, $Y248, $W248,$AJ248,$AA248,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T248=\"Select Model\",\"\",IF($T248=\"LIU24_2W\",calcQwIP($Y248,$W248,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC248,$AI248,\"latent\",$U248&\"P\"&IF($V248=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T248,activeElevation),\"\"))","v":""},{"$f":"IF($T248=\"Select Model\",\"\",IF($T248=\"ACBC_1W\",calcQwIP($Y248,$W248,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC248,BD248,\"capacity\",$U248&\"P\"&IF($V248=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T248,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y248,$W248,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC248,BD248,\"capacity\",$U248&\"P\"&IF($V248=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T248,activeElevation)))","v":""},"",{"$f":"IF(T248=\"Select Model\", 0,waterPressureDrop(W248, U248 & \"P\" & IF(V248=\"Dual\",2,1) &\"C\", AC248, \"cooling\", T248))","v":0},{"$f":"IF(T248=\"Select Model\", \"\",getReturnWaterTemp(T248,AC248, activeEWTCooling, AS248, \"cooling\"))","v":""},"",{"$f":"IF($T248<>\"ACBC_1W\",\"\",IF($J248=\"\",\"\",FintubeCapacity($T248,$W248,$AE248,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T248=\"Select Model\",T248=\"PCBL\"),\"\",calcQwIP(Y248,W248,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD248,BD248,\"capacity\",U248&\"P\"&IF(V248=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T248,activeElevation))","v":""},"",{"$f":"IF(OR(T248=\"Select Model\",T248=\"PCBL\"), \"\",IF(AY248=0,\"N/A\",waterPressureDrop(W248, U248 & \"P\" & IF(V248=\"Dual\",2,1) &\"C\", AD248, \"heating\", T248)))","v":""},{"$f":"IF(OR(T248=\"Select Model\",T248=\"PCBL\"), \"\",IF(AY248=0,getReturnWaterTemp(T248,AE248, activeEWTHeating, AX248, \"heating\"),getReturnWaterTemp(T248,AD248, activeEWTHeating, AY248, \"heating\")))","v":""},"",{"$f":" getNozzle(T248, W248, Y248, Z248, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I249)),I249<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I249, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H249)),H249<0),\"\",intlEstQuantity(T249, W249*12, H249)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T249=\"Select Model\",\"\",coilCircuitChange(W249, U249, AC249, T249,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T249=\"Select Model\",\"\",beamWidth(T249))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T249=\"Select Model\",T249=\"PCBL\"), 0,getSPIP(T249, W249, Y249, BD249, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T249=\"Select Model\", \"\",IF(T249=\"PCBL\",0,primaryAirSensibleCapacityIP($T249,$W249,activeRoomTempCooling,activePriAirTempCooling,$Y249,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T249=\"Select Model\",\"\",IF($T249=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y249,activeElevation)))","v":""},{"$f":"IF(OR(T249=\"Select Model\",T249=\"PCBL\"), 0,IF(AD249=0,0,-primaryAirSensibleCapacityIP($T249,$W249,activeRoomTempHeating,activePriAirTempHeating,$Y249,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T249=\"Select Model\", \"\", InductionRatio($T249,BD249,$W249,$Y249)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T249=\"Select Model\", \"\",IF($T249=\"PCBL\",\"N/A\",minVAVSetBack(AA249, Y249))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T249=\"Select Model\", \"\",IF($T249= \"PCBL\",\"N/A\",getDischargeAirTemp($T249,$V249,$AC249,$W249,BD249,$AL249, $Y249, $AS249, \"cooling\",activeElevation,$AB249,$AJ249,$AV249,$BB249))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T249=\"Select Model\",$T249=\"PCBL\"), \"\",getDischargeAirTemp($T249,$V249,$AD249,$W249,BD249,$AL249, $Y249, $AY249, \"heating\",activeElevation,$AB249,$AJ249,$AV249,$BB249)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T249=\"Select Model\", \"\",IF(OR($T249=\"ACBC_1W\",$T249=\"ACBC_2W\",LEFT($T249,4)=\"ACBR\",$T249 = \"LIU24_2W\",LEFT($T249,3)=\"RIU\",LEFT($T249,6)=\"ACBL12\"), IF((soundLevel($T249, $AB249, BD249, $Y249, $W249,$AJ249,$AA249,\"dba\"))<15,\"<15\",soundLevel($T249, $AB249, BD249, $Y249, $W249,$AJ249,$AA249,\"dba\")+0.4),IF((soundLevel($T249, $AB249, BD249, $Y249, $W249,$AJ249,$AA249,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T249, $AB249, BD249, $Y249, $W249,$AJ249,$AA249,\"dba\")+5)<15, \"<15\", soundLevel($T249, $AB249, BD249,$Y249, $W249,$AJ249,$AA249,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T249=\"Select Model\", \"\",IF(OR($T249=\"ACBC_1W\",$T249=\"ACBC_2W\",LEFT($T249,4)=\"ACBR\",$T249=\"LIU24_2W\",LEFT($T249,3)=\"RIU\",LEFT($T249,6)=\"ACBL12\"), IF((soundLevel($T249, $AB249, BD249, $Y249, $W249,$AJ249,$AA249,\"NC\"))<15,\"<15\",soundLevel($T249, $AB249, BD249, $Y249, $W249,$AJ249,$AA249,\"NC\")+0.4),IF((soundLevel($T249, $AB249, BD249, $Y249, $W249,$AJ249,$AA249,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T249, $AB249, BD249, $Y249, $W249,$AJ249,$AA249,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T249, $AB249, BD249, $Y249, $W249,$AJ249,$AA249,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T249=\"Select Model\",\"\",IF($T249=\"LIU24_2W\",calcQwIP($Y249,$W249,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC249,$AI249,\"latent\",$U249&\"P\"&IF($V249=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T249,activeElevation),\"\"))","v":""},{"$f":"IF($T249=\"Select Model\",\"\",IF($T249=\"ACBC_1W\",calcQwIP($Y249,$W249,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC249,BD249,\"capacity\",$U249&\"P\"&IF($V249=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T249,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y249,$W249,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC249,BD249,\"capacity\",$U249&\"P\"&IF($V249=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T249,activeElevation)))","v":""},"",{"$f":"IF(T249=\"Select Model\", 0,waterPressureDrop(W249, U249 & \"P\" & IF(V249=\"Dual\",2,1) &\"C\", AC249, \"cooling\", T249))","v":0},{"$f":"IF(T249=\"Select Model\", \"\",getReturnWaterTemp(T249,AC249, activeEWTCooling, AS249, \"cooling\"))","v":""},"",{"$f":"IF($T249<>\"ACBC_1W\",\"\",IF($J249=\"\",\"\",FintubeCapacity($T249,$W249,$AE249,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T249=\"Select Model\",T249=\"PCBL\"),\"\",calcQwIP(Y249,W249,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD249,BD249,\"capacity\",U249&\"P\"&IF(V249=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T249,activeElevation))","v":""},"",{"$f":"IF(OR(T249=\"Select Model\",T249=\"PCBL\"), \"\",IF(AY249=0,\"N/A\",waterPressureDrop(W249, U249 & \"P\" & IF(V249=\"Dual\",2,1) &\"C\", AD249, \"heating\", T249)))","v":""},{"$f":"IF(OR(T249=\"Select Model\",T249=\"PCBL\"), \"\",IF(AY249=0,getReturnWaterTemp(T249,AE249, activeEWTHeating, AX249, \"heating\"),getReturnWaterTemp(T249,AD249, activeEWTHeating, AY249, \"heating\")))","v":""},"",{"$f":" getNozzle(T249, W249, Y249, Z249, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I250)),I250<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I250, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H250)),H250<0),\"\",intlEstQuantity(T250, W250*12, H250)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T250=\"Select Model\",\"\",coilCircuitChange(W250, U250, AC250, T250,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T250=\"Select Model\",\"\",beamWidth(T250))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T250=\"Select Model\",T250=\"PCBL\"), 0,getSPIP(T250, W250, Y250, BD250, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T250=\"Select Model\", \"\",IF(T250=\"PCBL\",0,primaryAirSensibleCapacityIP($T250,$W250,activeRoomTempCooling,activePriAirTempCooling,$Y250,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T250=\"Select Model\",\"\",IF($T250=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y250,activeElevation)))","v":""},{"$f":"IF(OR(T250=\"Select Model\",T250=\"PCBL\"), 0,IF(AD250=0,0,-primaryAirSensibleCapacityIP($T250,$W250,activeRoomTempHeating,activePriAirTempHeating,$Y250,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T250=\"Select Model\", \"\", InductionRatio($T250,BD250,$W250,$Y250)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T250=\"Select Model\", \"\",IF($T250=\"PCBL\",\"N/A\",minVAVSetBack(AA250, Y250))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T250=\"Select Model\", \"\",IF($T250= \"PCBL\",\"N/A\",getDischargeAirTemp($T250,$V250,$AC250,$W250,BD250,$AL250, $Y250, $AS250, \"cooling\",activeElevation,$AB250,$AJ250,$AV250,$BB250))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T250=\"Select Model\",$T250=\"PCBL\"), \"\",getDischargeAirTemp($T250,$V250,$AD250,$W250,BD250,$AL250, $Y250, $AY250, \"heating\",activeElevation,$AB250,$AJ250,$AV250,$BB250)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T250=\"Select Model\", \"\",IF(OR($T250=\"ACBC_1W\",$T250=\"ACBC_2W\",LEFT($T250,4)=\"ACBR\",$T250 = \"LIU24_2W\",LEFT($T250,3)=\"RIU\",LEFT($T250,6)=\"ACBL12\"), IF((soundLevel($T250, $AB250, BD250, $Y250, $W250,$AJ250,$AA250,\"dba\"))<15,\"<15\",soundLevel($T250, $AB250, BD250, $Y250, $W250,$AJ250,$AA250,\"dba\")+0.4),IF((soundLevel($T250, $AB250, BD250, $Y250, $W250,$AJ250,$AA250,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T250, $AB250, BD250, $Y250, $W250,$AJ250,$AA250,\"dba\")+5)<15, \"<15\", soundLevel($T250, $AB250, BD250,$Y250, $W250,$AJ250,$AA250,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T250=\"Select Model\", \"\",IF(OR($T250=\"ACBC_1W\",$T250=\"ACBC_2W\",LEFT($T250,4)=\"ACBR\",$T250=\"LIU24_2W\",LEFT($T250,3)=\"RIU\",LEFT($T250,6)=\"ACBL12\"), IF((soundLevel($T250, $AB250, BD250, $Y250, $W250,$AJ250,$AA250,\"NC\"))<15,\"<15\",soundLevel($T250, $AB250, BD250, $Y250, $W250,$AJ250,$AA250,\"NC\")+0.4),IF((soundLevel($T250, $AB250, BD250, $Y250, $W250,$AJ250,$AA250,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T250, $AB250, BD250, $Y250, $W250,$AJ250,$AA250,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T250, $AB250, BD250, $Y250, $W250,$AJ250,$AA250,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T250=\"Select Model\",\"\",IF($T250=\"LIU24_2W\",calcQwIP($Y250,$W250,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC250,$AI250,\"latent\",$U250&\"P\"&IF($V250=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T250,activeElevation),\"\"))","v":""},{"$f":"IF($T250=\"Select Model\",\"\",IF($T250=\"ACBC_1W\",calcQwIP($Y250,$W250,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC250,BD250,\"capacity\",$U250&\"P\"&IF($V250=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T250,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y250,$W250,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC250,BD250,\"capacity\",$U250&\"P\"&IF($V250=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T250,activeElevation)))","v":""},"",{"$f":"IF(T250=\"Select Model\", 0,waterPressureDrop(W250, U250 & \"P\" & IF(V250=\"Dual\",2,1) &\"C\", AC250, \"cooling\", T250))","v":0},{"$f":"IF(T250=\"Select Model\", \"\",getReturnWaterTemp(T250,AC250, activeEWTCooling, AS250, \"cooling\"))","v":""},"",{"$f":"IF($T250<>\"ACBC_1W\",\"\",IF($J250=\"\",\"\",FintubeCapacity($T250,$W250,$AE250,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T250=\"Select Model\",T250=\"PCBL\"),\"\",calcQwIP(Y250,W250,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD250,BD250,\"capacity\",U250&\"P\"&IF(V250=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T250,activeElevation))","v":""},"",{"$f":"IF(OR(T250=\"Select Model\",T250=\"PCBL\"), \"\",IF(AY250=0,\"N/A\",waterPressureDrop(W250, U250 & \"P\" & IF(V250=\"Dual\",2,1) &\"C\", AD250, \"heating\", T250)))","v":""},{"$f":"IF(OR(T250=\"Select Model\",T250=\"PCBL\"), \"\",IF(AY250=0,getReturnWaterTemp(T250,AE250, activeEWTHeating, AX250, \"heating\"),getReturnWaterTemp(T250,AD250, activeEWTHeating, AY250, \"heating\")))","v":""},"",{"$f":" getNozzle(T250, W250, Y250, Z250, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I251)),I251<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I251, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H251)),H251<0),\"\",intlEstQuantity(T251, W251*12, H251)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T251=\"Select Model\",\"\",coilCircuitChange(W251, U251, AC251, T251,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T251=\"Select Model\",\"\",beamWidth(T251))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T251=\"Select Model\",T251=\"PCBL\"), 0,getSPIP(T251, W251, Y251, BD251, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T251=\"Select Model\", \"\",IF(T251=\"PCBL\",0,primaryAirSensibleCapacityIP($T251,$W251,activeRoomTempCooling,activePriAirTempCooling,$Y251,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T251=\"Select Model\",\"\",IF($T251=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y251,activeElevation)))","v":""},{"$f":"IF(OR(T251=\"Select Model\",T251=\"PCBL\"), 0,IF(AD251=0,0,-primaryAirSensibleCapacityIP($T251,$W251,activeRoomTempHeating,activePriAirTempHeating,$Y251,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T251=\"Select Model\", \"\", InductionRatio($T251,BD251,$W251,$Y251)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T251=\"Select Model\", \"\",IF($T251=\"PCBL\",\"N/A\",minVAVSetBack(AA251, Y251))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T251=\"Select Model\", \"\",IF($T251= \"PCBL\",\"N/A\",getDischargeAirTemp($T251,$V251,$AC251,$W251,BD251,$AL251, $Y251, $AS251, \"cooling\",activeElevation,$AB251,$AJ251,$AV251,$BB251))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T251=\"Select Model\",$T251=\"PCBL\"), \"\",getDischargeAirTemp($T251,$V251,$AD251,$W251,BD251,$AL251, $Y251, $AY251, \"heating\",activeElevation,$AB251,$AJ251,$AV251,$BB251)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T251=\"Select Model\", \"\",IF(OR($T251=\"ACBC_1W\",$T251=\"ACBC_2W\",LEFT($T251,4)=\"ACBR\",$T251 = \"LIU24_2W\",LEFT($T251,3)=\"RIU\",LEFT($T251,6)=\"ACBL12\"), IF((soundLevel($T251, $AB251, BD251, $Y251, $W251,$AJ251,$AA251,\"dba\"))<15,\"<15\",soundLevel($T251, $AB251, BD251, $Y251, $W251,$AJ251,$AA251,\"dba\")+0.4),IF((soundLevel($T251, $AB251, BD251, $Y251, $W251,$AJ251,$AA251,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T251, $AB251, BD251, $Y251, $W251,$AJ251,$AA251,\"dba\")+5)<15, \"<15\", soundLevel($T251, $AB251, BD251,$Y251, $W251,$AJ251,$AA251,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T251=\"Select Model\", \"\",IF(OR($T251=\"ACBC_1W\",$T251=\"ACBC_2W\",LEFT($T251,4)=\"ACBR\",$T251=\"LIU24_2W\",LEFT($T251,3)=\"RIU\",LEFT($T251,6)=\"ACBL12\"), IF((soundLevel($T251, $AB251, BD251, $Y251, $W251,$AJ251,$AA251,\"NC\"))<15,\"<15\",soundLevel($T251, $AB251, BD251, $Y251, $W251,$AJ251,$AA251,\"NC\")+0.4),IF((soundLevel($T251, $AB251, BD251, $Y251, $W251,$AJ251,$AA251,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T251, $AB251, BD251, $Y251, $W251,$AJ251,$AA251,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T251, $AB251, BD251, $Y251, $W251,$AJ251,$AA251,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T251=\"Select Model\",\"\",IF($T251=\"LIU24_2W\",calcQwIP($Y251,$W251,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC251,$AI251,\"latent\",$U251&\"P\"&IF($V251=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T251,activeElevation),\"\"))","v":""},{"$f":"IF($T251=\"Select Model\",\"\",IF($T251=\"ACBC_1W\",calcQwIP($Y251,$W251,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC251,BD251,\"capacity\",$U251&\"P\"&IF($V251=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T251,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y251,$W251,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC251,BD251,\"capacity\",$U251&\"P\"&IF($V251=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T251,activeElevation)))","v":""},"",{"$f":"IF(T251=\"Select Model\", 0,waterPressureDrop(W251, U251 & \"P\" & IF(V251=\"Dual\",2,1) &\"C\", AC251, \"cooling\", T251))","v":0},{"$f":"IF(T251=\"Select Model\", \"\",getReturnWaterTemp(T251,AC251, activeEWTCooling, AS251, \"cooling\"))","v":""},"",{"$f":"IF($T251<>\"ACBC_1W\",\"\",IF($J251=\"\",\"\",FintubeCapacity($T251,$W251,$AE251,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T251=\"Select Model\",T251=\"PCBL\"),\"\",calcQwIP(Y251,W251,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD251,BD251,\"capacity\",U251&\"P\"&IF(V251=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T251,activeElevation))","v":""},"",{"$f":"IF(OR(T251=\"Select Model\",T251=\"PCBL\"), \"\",IF(AY251=0,\"N/A\",waterPressureDrop(W251, U251 & \"P\" & IF(V251=\"Dual\",2,1) &\"C\", AD251, \"heating\", T251)))","v":""},{"$f":"IF(OR(T251=\"Select Model\",T251=\"PCBL\"), \"\",IF(AY251=0,getReturnWaterTemp(T251,AE251, activeEWTHeating, AX251, \"heating\"),getReturnWaterTemp(T251,AD251, activeEWTHeating, AY251, \"heating\")))","v":""},"",{"$f":" getNozzle(T251, W251, Y251, Z251, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I252)),I252<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I252, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H252)),H252<0),\"\",intlEstQuantity(T252, W252*12, H252)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T252=\"Select Model\",\"\",coilCircuitChange(W252, U252, AC252, T252,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T252=\"Select Model\",\"\",beamWidth(T252))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T252=\"Select Model\",T252=\"PCBL\"), 0,getSPIP(T252, W252, Y252, BD252, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T252=\"Select Model\", \"\",IF(T252=\"PCBL\",0,primaryAirSensibleCapacityIP($T252,$W252,activeRoomTempCooling,activePriAirTempCooling,$Y252,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T252=\"Select Model\",\"\",IF($T252=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y252,activeElevation)))","v":""},{"$f":"IF(OR(T252=\"Select Model\",T252=\"PCBL\"), 0,IF(AD252=0,0,-primaryAirSensibleCapacityIP($T252,$W252,activeRoomTempHeating,activePriAirTempHeating,$Y252,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T252=\"Select Model\", \"\", InductionRatio($T252,BD252,$W252,$Y252)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T252=\"Select Model\", \"\",IF($T252=\"PCBL\",\"N/A\",minVAVSetBack(AA252, Y252))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T252=\"Select Model\", \"\",IF($T252= \"PCBL\",\"N/A\",getDischargeAirTemp($T252,$V252,$AC252,$W252,BD252,$AL252, $Y252, $AS252, \"cooling\",activeElevation,$AB252,$AJ252,$AV252,$BB252))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T252=\"Select Model\",$T252=\"PCBL\"), \"\",getDischargeAirTemp($T252,$V252,$AD252,$W252,BD252,$AL252, $Y252, $AY252, \"heating\",activeElevation,$AB252,$AJ252,$AV252,$BB252)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T252=\"Select Model\", \"\",IF(OR($T252=\"ACBC_1W\",$T252=\"ACBC_2W\",LEFT($T252,4)=\"ACBR\",$T252 = \"LIU24_2W\",LEFT($T252,3)=\"RIU\",LEFT($T252,6)=\"ACBL12\"), IF((soundLevel($T252, $AB252, BD252, $Y252, $W252,$AJ252,$AA252,\"dba\"))<15,\"<15\",soundLevel($T252, $AB252, BD252, $Y252, $W252,$AJ252,$AA252,\"dba\")+0.4),IF((soundLevel($T252, $AB252, BD252, $Y252, $W252,$AJ252,$AA252,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T252, $AB252, BD252, $Y252, $W252,$AJ252,$AA252,\"dba\")+5)<15, \"<15\", soundLevel($T252, $AB252, BD252,$Y252, $W252,$AJ252,$AA252,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T252=\"Select Model\", \"\",IF(OR($T252=\"ACBC_1W\",$T252=\"ACBC_2W\",LEFT($T252,4)=\"ACBR\",$T252=\"LIU24_2W\",LEFT($T252,3)=\"RIU\",LEFT($T252,6)=\"ACBL12\"), IF((soundLevel($T252, $AB252, BD252, $Y252, $W252,$AJ252,$AA252,\"NC\"))<15,\"<15\",soundLevel($T252, $AB252, BD252, $Y252, $W252,$AJ252,$AA252,\"NC\")+0.4),IF((soundLevel($T252, $AB252, BD252, $Y252, $W252,$AJ252,$AA252,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T252, $AB252, BD252, $Y252, $W252,$AJ252,$AA252,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T252, $AB252, BD252, $Y252, $W252,$AJ252,$AA252,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T252=\"Select Model\",\"\",IF($T252=\"LIU24_2W\",calcQwIP($Y252,$W252,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC252,$AI252,\"latent\",$U252&\"P\"&IF($V252=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T252,activeElevation),\"\"))","v":""},{"$f":"IF($T252=\"Select Model\",\"\",IF($T252=\"ACBC_1W\",calcQwIP($Y252,$W252,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC252,BD252,\"capacity\",$U252&\"P\"&IF($V252=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T252,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y252,$W252,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC252,BD252,\"capacity\",$U252&\"P\"&IF($V252=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T252,activeElevation)))","v":""},"",{"$f":"IF(T252=\"Select Model\", 0,waterPressureDrop(W252, U252 & \"P\" & IF(V252=\"Dual\",2,1) &\"C\", AC252, \"cooling\", T252))","v":0},{"$f":"IF(T252=\"Select Model\", \"\",getReturnWaterTemp(T252,AC252, activeEWTCooling, AS252, \"cooling\"))","v":""},"",{"$f":"IF($T252<>\"ACBC_1W\",\"\",IF($J252=\"\",\"\",FintubeCapacity($T252,$W252,$AE252,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T252=\"Select Model\",T252=\"PCBL\"),\"\",calcQwIP(Y252,W252,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD252,BD252,\"capacity\",U252&\"P\"&IF(V252=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T252,activeElevation))","v":""},"",{"$f":"IF(OR(T252=\"Select Model\",T252=\"PCBL\"), \"\",IF(AY252=0,\"N/A\",waterPressureDrop(W252, U252 & \"P\" & IF(V252=\"Dual\",2,1) &\"C\", AD252, \"heating\", T252)))","v":""},{"$f":"IF(OR(T252=\"Select Model\",T252=\"PCBL\"), \"\",IF(AY252=0,getReturnWaterTemp(T252,AE252, activeEWTHeating, AX252, \"heating\"),getReturnWaterTemp(T252,AD252, activeEWTHeating, AY252, \"heating\")))","v":""},"",{"$f":" getNozzle(T252, W252, Y252, Z252, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I253)),I253<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I253, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H253)),H253<0),\"\",intlEstQuantity(T253, W253*12, H253)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T253=\"Select Model\",\"\",coilCircuitChange(W253, U253, AC253, T253,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T253=\"Select Model\",\"\",beamWidth(T253))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T253=\"Select Model\",T253=\"PCBL\"), 0,getSPIP(T253, W253, Y253, BD253, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T253=\"Select Model\", \"\",IF(T253=\"PCBL\",0,primaryAirSensibleCapacityIP($T253,$W253,activeRoomTempCooling,activePriAirTempCooling,$Y253,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T253=\"Select Model\",\"\",IF($T253=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y253,activeElevation)))","v":""},{"$f":"IF(OR(T253=\"Select Model\",T253=\"PCBL\"), 0,IF(AD253=0,0,-primaryAirSensibleCapacityIP($T253,$W253,activeRoomTempHeating,activePriAirTempHeating,$Y253,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T253=\"Select Model\", \"\", InductionRatio($T253,BD253,$W253,$Y253)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T253=\"Select Model\", \"\",IF($T253=\"PCBL\",\"N/A\",minVAVSetBack(AA253, Y253))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T253=\"Select Model\", \"\",IF($T253= \"PCBL\",\"N/A\",getDischargeAirTemp($T253,$V253,$AC253,$W253,BD253,$AL253, $Y253, $AS253, \"cooling\",activeElevation,$AB253,$AJ253,$AV253,$BB253))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T253=\"Select Model\",$T253=\"PCBL\"), \"\",getDischargeAirTemp($T253,$V253,$AD253,$W253,BD253,$AL253, $Y253, $AY253, \"heating\",activeElevation,$AB253,$AJ253,$AV253,$BB253)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T253=\"Select Model\", \"\",IF(OR($T253=\"ACBC_1W\",$T253=\"ACBC_2W\",LEFT($T253,4)=\"ACBR\",$T253 = \"LIU24_2W\",LEFT($T253,3)=\"RIU\",LEFT($T253,6)=\"ACBL12\"), IF((soundLevel($T253, $AB253, BD253, $Y253, $W253,$AJ253,$AA253,\"dba\"))<15,\"<15\",soundLevel($T253, $AB253, BD253, $Y253, $W253,$AJ253,$AA253,\"dba\")+0.4),IF((soundLevel($T253, $AB253, BD253, $Y253, $W253,$AJ253,$AA253,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T253, $AB253, BD253, $Y253, $W253,$AJ253,$AA253,\"dba\")+5)<15, \"<15\", soundLevel($T253, $AB253, BD253,$Y253, $W253,$AJ253,$AA253,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T253=\"Select Model\", \"\",IF(OR($T253=\"ACBC_1W\",$T253=\"ACBC_2W\",LEFT($T253,4)=\"ACBR\",$T253=\"LIU24_2W\",LEFT($T253,3)=\"RIU\",LEFT($T253,6)=\"ACBL12\"), IF((soundLevel($T253, $AB253, BD253, $Y253, $W253,$AJ253,$AA253,\"NC\"))<15,\"<15\",soundLevel($T253, $AB253, BD253, $Y253, $W253,$AJ253,$AA253,\"NC\")+0.4),IF((soundLevel($T253, $AB253, BD253, $Y253, $W253,$AJ253,$AA253,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T253, $AB253, BD253, $Y253, $W253,$AJ253,$AA253,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T253, $AB253, BD253, $Y253, $W253,$AJ253,$AA253,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T253=\"Select Model\",\"\",IF($T253=\"LIU24_2W\",calcQwIP($Y253,$W253,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC253,$AI253,\"latent\",$U253&\"P\"&IF($V253=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T253,activeElevation),\"\"))","v":""},{"$f":"IF($T253=\"Select Model\",\"\",IF($T253=\"ACBC_1W\",calcQwIP($Y253,$W253,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC253,BD253,\"capacity\",$U253&\"P\"&IF($V253=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T253,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y253,$W253,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC253,BD253,\"capacity\",$U253&\"P\"&IF($V253=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T253,activeElevation)))","v":""},"",{"$f":"IF(T253=\"Select Model\", 0,waterPressureDrop(W253, U253 & \"P\" & IF(V253=\"Dual\",2,1) &\"C\", AC253, \"cooling\", T253))","v":0},{"$f":"IF(T253=\"Select Model\", \"\",getReturnWaterTemp(T253,AC253, activeEWTCooling, AS253, \"cooling\"))","v":""},"",{"$f":"IF($T253<>\"ACBC_1W\",\"\",IF($J253=\"\",\"\",FintubeCapacity($T253,$W253,$AE253,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T253=\"Select Model\",T253=\"PCBL\"),\"\",calcQwIP(Y253,W253,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD253,BD253,\"capacity\",U253&\"P\"&IF(V253=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T253,activeElevation))","v":""},"",{"$f":"IF(OR(T253=\"Select Model\",T253=\"PCBL\"), \"\",IF(AY253=0,\"N/A\",waterPressureDrop(W253, U253 & \"P\" & IF(V253=\"Dual\",2,1) &\"C\", AD253, \"heating\", T253)))","v":""},{"$f":"IF(OR(T253=\"Select Model\",T253=\"PCBL\"), \"\",IF(AY253=0,getReturnWaterTemp(T253,AE253, activeEWTHeating, AX253, \"heating\"),getReturnWaterTemp(T253,AD253, activeEWTHeating, AY253, \"heating\")))","v":""},"",{"$f":" getNozzle(T253, W253, Y253, Z253, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I254)),I254<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I254, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H254)),H254<0),\"\",intlEstQuantity(T254, W254*12, H254)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T254=\"Select Model\",\"\",coilCircuitChange(W254, U254, AC254, T254,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T254=\"Select Model\",\"\",beamWidth(T254))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T254=\"Select Model\",T254=\"PCBL\"), 0,getSPIP(T254, W254, Y254, BD254, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T254=\"Select Model\", \"\",IF(T254=\"PCBL\",0,primaryAirSensibleCapacityIP($T254,$W254,activeRoomTempCooling,activePriAirTempCooling,$Y254,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T254=\"Select Model\",\"\",IF($T254=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y254,activeElevation)))","v":""},{"$f":"IF(OR(T254=\"Select Model\",T254=\"PCBL\"), 0,IF(AD254=0,0,-primaryAirSensibleCapacityIP($T254,$W254,activeRoomTempHeating,activePriAirTempHeating,$Y254,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T254=\"Select Model\", \"\", InductionRatio($T254,BD254,$W254,$Y254)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T254=\"Select Model\", \"\",IF($T254=\"PCBL\",\"N/A\",minVAVSetBack(AA254, Y254))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T254=\"Select Model\", \"\",IF($T254= \"PCBL\",\"N/A\",getDischargeAirTemp($T254,$V254,$AC254,$W254,BD254,$AL254, $Y254, $AS254, \"cooling\",activeElevation,$AB254,$AJ254,$AV254,$BB254))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T254=\"Select Model\",$T254=\"PCBL\"), \"\",getDischargeAirTemp($T254,$V254,$AD254,$W254,BD254,$AL254, $Y254, $AY254, \"heating\",activeElevation,$AB254,$AJ254,$AV254,$BB254)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T254=\"Select Model\", \"\",IF(OR($T254=\"ACBC_1W\",$T254=\"ACBC_2W\",LEFT($T254,4)=\"ACBR\",$T254 = \"LIU24_2W\",LEFT($T254,3)=\"RIU\",LEFT($T254,6)=\"ACBL12\"), IF((soundLevel($T254, $AB254, BD254, $Y254, $W254,$AJ254,$AA254,\"dba\"))<15,\"<15\",soundLevel($T254, $AB254, BD254, $Y254, $W254,$AJ254,$AA254,\"dba\")+0.4),IF((soundLevel($T254, $AB254, BD254, $Y254, $W254,$AJ254,$AA254,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T254, $AB254, BD254, $Y254, $W254,$AJ254,$AA254,\"dba\")+5)<15, \"<15\", soundLevel($T254, $AB254, BD254,$Y254, $W254,$AJ254,$AA254,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T254=\"Select Model\", \"\",IF(OR($T254=\"ACBC_1W\",$T254=\"ACBC_2W\",LEFT($T254,4)=\"ACBR\",$T254=\"LIU24_2W\",LEFT($T254,3)=\"RIU\",LEFT($T254,6)=\"ACBL12\"), IF((soundLevel($T254, $AB254, BD254, $Y254, $W254,$AJ254,$AA254,\"NC\"))<15,\"<15\",soundLevel($T254, $AB254, BD254, $Y254, $W254,$AJ254,$AA254,\"NC\")+0.4),IF((soundLevel($T254, $AB254, BD254, $Y254, $W254,$AJ254,$AA254,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T254, $AB254, BD254, $Y254, $W254,$AJ254,$AA254,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T254, $AB254, BD254, $Y254, $W254,$AJ254,$AA254,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T254=\"Select Model\",\"\",IF($T254=\"LIU24_2W\",calcQwIP($Y254,$W254,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC254,$AI254,\"latent\",$U254&\"P\"&IF($V254=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T254,activeElevation),\"\"))","v":""},{"$f":"IF($T254=\"Select Model\",\"\",IF($T254=\"ACBC_1W\",calcQwIP($Y254,$W254,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC254,BD254,\"capacity\",$U254&\"P\"&IF($V254=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T254,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y254,$W254,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC254,BD254,\"capacity\",$U254&\"P\"&IF($V254=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T254,activeElevation)))","v":""},"",{"$f":"IF(T254=\"Select Model\", 0,waterPressureDrop(W254, U254 & \"P\" & IF(V254=\"Dual\",2,1) &\"C\", AC254, \"cooling\", T254))","v":0},{"$f":"IF(T254=\"Select Model\", \"\",getReturnWaterTemp(T254,AC254, activeEWTCooling, AS254, \"cooling\"))","v":""},"",{"$f":"IF($T254<>\"ACBC_1W\",\"\",IF($J254=\"\",\"\",FintubeCapacity($T254,$W254,$AE254,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T254=\"Select Model\",T254=\"PCBL\"),\"\",calcQwIP(Y254,W254,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD254,BD254,\"capacity\",U254&\"P\"&IF(V254=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T254,activeElevation))","v":""},"",{"$f":"IF(OR(T254=\"Select Model\",T254=\"PCBL\"), \"\",IF(AY254=0,\"N/A\",waterPressureDrop(W254, U254 & \"P\" & IF(V254=\"Dual\",2,1) &\"C\", AD254, \"heating\", T254)))","v":""},{"$f":"IF(OR(T254=\"Select Model\",T254=\"PCBL\"), \"\",IF(AY254=0,getReturnWaterTemp(T254,AE254, activeEWTHeating, AX254, \"heating\"),getReturnWaterTemp(T254,AD254, activeEWTHeating, AY254, \"heating\")))","v":""},"",{"$f":" getNozzle(T254, W254, Y254, Z254, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I255)),I255<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I255, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H255)),H255<0),\"\",intlEstQuantity(T255, W255*12, H255)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T255=\"Select Model\",\"\",coilCircuitChange(W255, U255, AC255, T255,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T255=\"Select Model\",\"\",beamWidth(T255))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T255=\"Select Model\",T255=\"PCBL\"), 0,getSPIP(T255, W255, Y255, BD255, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T255=\"Select Model\", \"\",IF(T255=\"PCBL\",0,primaryAirSensibleCapacityIP($T255,$W255,activeRoomTempCooling,activePriAirTempCooling,$Y255,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T255=\"Select Model\",\"\",IF($T255=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y255,activeElevation)))","v":""},{"$f":"IF(OR(T255=\"Select Model\",T255=\"PCBL\"), 0,IF(AD255=0,0,-primaryAirSensibleCapacityIP($T255,$W255,activeRoomTempHeating,activePriAirTempHeating,$Y255,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T255=\"Select Model\", \"\", InductionRatio($T255,BD255,$W255,$Y255)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T255=\"Select Model\", \"\",IF($T255=\"PCBL\",\"N/A\",minVAVSetBack(AA255, Y255))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T255=\"Select Model\", \"\",IF($T255= \"PCBL\",\"N/A\",getDischargeAirTemp($T255,$V255,$AC255,$W255,BD255,$AL255, $Y255, $AS255, \"cooling\",activeElevation,$AB255,$AJ255,$AV255,$BB255))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T255=\"Select Model\",$T255=\"PCBL\"), \"\",getDischargeAirTemp($T255,$V255,$AD255,$W255,BD255,$AL255, $Y255, $AY255, \"heating\",activeElevation,$AB255,$AJ255,$AV255,$BB255)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T255=\"Select Model\", \"\",IF(OR($T255=\"ACBC_1W\",$T255=\"ACBC_2W\",LEFT($T255,4)=\"ACBR\",$T255 = \"LIU24_2W\",LEFT($T255,3)=\"RIU\",LEFT($T255,6)=\"ACBL12\"), IF((soundLevel($T255, $AB255, BD255, $Y255, $W255,$AJ255,$AA255,\"dba\"))<15,\"<15\",soundLevel($T255, $AB255, BD255, $Y255, $W255,$AJ255,$AA255,\"dba\")+0.4),IF((soundLevel($T255, $AB255, BD255, $Y255, $W255,$AJ255,$AA255,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T255, $AB255, BD255, $Y255, $W255,$AJ255,$AA255,\"dba\")+5)<15, \"<15\", soundLevel($T255, $AB255, BD255,$Y255, $W255,$AJ255,$AA255,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T255=\"Select Model\", \"\",IF(OR($T255=\"ACBC_1W\",$T255=\"ACBC_2W\",LEFT($T255,4)=\"ACBR\",$T255=\"LIU24_2W\",LEFT($T255,3)=\"RIU\",LEFT($T255,6)=\"ACBL12\"), IF((soundLevel($T255, $AB255, BD255, $Y255, $W255,$AJ255,$AA255,\"NC\"))<15,\"<15\",soundLevel($T255, $AB255, BD255, $Y255, $W255,$AJ255,$AA255,\"NC\")+0.4),IF((soundLevel($T255, $AB255, BD255, $Y255, $W255,$AJ255,$AA255,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T255, $AB255, BD255, $Y255, $W255,$AJ255,$AA255,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T255, $AB255, BD255, $Y255, $W255,$AJ255,$AA255,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T255=\"Select Model\",\"\",IF($T255=\"LIU24_2W\",calcQwIP($Y255,$W255,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC255,$AI255,\"latent\",$U255&\"P\"&IF($V255=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T255,activeElevation),\"\"))","v":""},{"$f":"IF($T255=\"Select Model\",\"\",IF($T255=\"ACBC_1W\",calcQwIP($Y255,$W255,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC255,BD255,\"capacity\",$U255&\"P\"&IF($V255=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T255,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y255,$W255,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC255,BD255,\"capacity\",$U255&\"P\"&IF($V255=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T255,activeElevation)))","v":""},"",{"$f":"IF(T255=\"Select Model\", 0,waterPressureDrop(W255, U255 & \"P\" & IF(V255=\"Dual\",2,1) &\"C\", AC255, \"cooling\", T255))","v":0},{"$f":"IF(T255=\"Select Model\", \"\",getReturnWaterTemp(T255,AC255, activeEWTCooling, AS255, \"cooling\"))","v":""},"",{"$f":"IF($T255<>\"ACBC_1W\",\"\",IF($J255=\"\",\"\",FintubeCapacity($T255,$W255,$AE255,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T255=\"Select Model\",T255=\"PCBL\"),\"\",calcQwIP(Y255,W255,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD255,BD255,\"capacity\",U255&\"P\"&IF(V255=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T255,activeElevation))","v":""},"",{"$f":"IF(OR(T255=\"Select Model\",T255=\"PCBL\"), \"\",IF(AY255=0,\"N/A\",waterPressureDrop(W255, U255 & \"P\" & IF(V255=\"Dual\",2,1) &\"C\", AD255, \"heating\", T255)))","v":""},{"$f":"IF(OR(T255=\"Select Model\",T255=\"PCBL\"), \"\",IF(AY255=0,getReturnWaterTemp(T255,AE255, activeEWTHeating, AX255, \"heating\"),getReturnWaterTemp(T255,AD255, activeEWTHeating, AY255, \"heating\")))","v":""},"",{"$f":" getNozzle(T255, W255, Y255, Z255, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I256)),I256<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I256, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H256)),H256<0),\"\",intlEstQuantity(T256, W256*12, H256)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T256=\"Select Model\",\"\",coilCircuitChange(W256, U256, AC256, T256,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T256=\"Select Model\",\"\",beamWidth(T256))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T256=\"Select Model\",T256=\"PCBL\"), 0,getSPIP(T256, W256, Y256, BD256, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T256=\"Select Model\", \"\",IF(T256=\"PCBL\",0,primaryAirSensibleCapacityIP($T256,$W256,activeRoomTempCooling,activePriAirTempCooling,$Y256,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T256=\"Select Model\",\"\",IF($T256=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y256,activeElevation)))","v":""},{"$f":"IF(OR(T256=\"Select Model\",T256=\"PCBL\"), 0,IF(AD256=0,0,-primaryAirSensibleCapacityIP($T256,$W256,activeRoomTempHeating,activePriAirTempHeating,$Y256,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T256=\"Select Model\", \"\", InductionRatio($T256,BD256,$W256,$Y256)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T256=\"Select Model\", \"\",IF($T256=\"PCBL\",\"N/A\",minVAVSetBack(AA256, Y256))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T256=\"Select Model\", \"\",IF($T256= \"PCBL\",\"N/A\",getDischargeAirTemp($T256,$V256,$AC256,$W256,BD256,$AL256, $Y256, $AS256, \"cooling\",activeElevation,$AB256,$AJ256,$AV256,$BB256))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T256=\"Select Model\",$T256=\"PCBL\"), \"\",getDischargeAirTemp($T256,$V256,$AD256,$W256,BD256,$AL256, $Y256, $AY256, \"heating\",activeElevation,$AB256,$AJ256,$AV256,$BB256)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T256=\"Select Model\", \"\",IF(OR($T256=\"ACBC_1W\",$T256=\"ACBC_2W\",LEFT($T256,4)=\"ACBR\",$T256 = \"LIU24_2W\",LEFT($T256,3)=\"RIU\",LEFT($T256,6)=\"ACBL12\"), IF((soundLevel($T256, $AB256, BD256, $Y256, $W256,$AJ256,$AA256,\"dba\"))<15,\"<15\",soundLevel($T256, $AB256, BD256, $Y256, $W256,$AJ256,$AA256,\"dba\")+0.4),IF((soundLevel($T256, $AB256, BD256, $Y256, $W256,$AJ256,$AA256,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T256, $AB256, BD256, $Y256, $W256,$AJ256,$AA256,\"dba\")+5)<15, \"<15\", soundLevel($T256, $AB256, BD256,$Y256, $W256,$AJ256,$AA256,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T256=\"Select Model\", \"\",IF(OR($T256=\"ACBC_1W\",$T256=\"ACBC_2W\",LEFT($T256,4)=\"ACBR\",$T256=\"LIU24_2W\",LEFT($T256,3)=\"RIU\",LEFT($T256,6)=\"ACBL12\"), IF((soundLevel($T256, $AB256, BD256, $Y256, $W256,$AJ256,$AA256,\"NC\"))<15,\"<15\",soundLevel($T256, $AB256, BD256, $Y256, $W256,$AJ256,$AA256,\"NC\")+0.4),IF((soundLevel($T256, $AB256, BD256, $Y256, $W256,$AJ256,$AA256,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T256, $AB256, BD256, $Y256, $W256,$AJ256,$AA256,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T256, $AB256, BD256, $Y256, $W256,$AJ256,$AA256,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T256=\"Select Model\",\"\",IF($T256=\"LIU24_2W\",calcQwIP($Y256,$W256,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC256,$AI256,\"latent\",$U256&\"P\"&IF($V256=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T256,activeElevation),\"\"))","v":""},{"$f":"IF($T256=\"Select Model\",\"\",IF($T256=\"ACBC_1W\",calcQwIP($Y256,$W256,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC256,BD256,\"capacity\",$U256&\"P\"&IF($V256=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T256,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y256,$W256,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC256,BD256,\"capacity\",$U256&\"P\"&IF($V256=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T256,activeElevation)))","v":""},"",{"$f":"IF(T256=\"Select Model\", 0,waterPressureDrop(W256, U256 & \"P\" & IF(V256=\"Dual\",2,1) &\"C\", AC256, \"cooling\", T256))","v":0},{"$f":"IF(T256=\"Select Model\", \"\",getReturnWaterTemp(T256,AC256, activeEWTCooling, AS256, \"cooling\"))","v":""},"",{"$f":"IF($T256<>\"ACBC_1W\",\"\",IF($J256=\"\",\"\",FintubeCapacity($T256,$W256,$AE256,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T256=\"Select Model\",T256=\"PCBL\"),\"\",calcQwIP(Y256,W256,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD256,BD256,\"capacity\",U256&\"P\"&IF(V256=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T256,activeElevation))","v":""},"",{"$f":"IF(OR(T256=\"Select Model\",T256=\"PCBL\"), \"\",IF(AY256=0,\"N/A\",waterPressureDrop(W256, U256 & \"P\" & IF(V256=\"Dual\",2,1) &\"C\", AD256, \"heating\", T256)))","v":""},{"$f":"IF(OR(T256=\"Select Model\",T256=\"PCBL\"), \"\",IF(AY256=0,getReturnWaterTemp(T256,AE256, activeEWTHeating, AX256, \"heating\"),getReturnWaterTemp(T256,AD256, activeEWTHeating, AY256, \"heating\")))","v":""},"",{"$f":" getNozzle(T256, W256, Y256, Z256, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I257)),I257<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I257, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H257)),H257<0),\"\",intlEstQuantity(T257, W257*12, H257)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T257=\"Select Model\",\"\",coilCircuitChange(W257, U257, AC257, T257,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T257=\"Select Model\",\"\",beamWidth(T257))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T257=\"Select Model\",T257=\"PCBL\"), 0,getSPIP(T257, W257, Y257, BD257, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T257=\"Select Model\", \"\",IF(T257=\"PCBL\",0,primaryAirSensibleCapacityIP($T257,$W257,activeRoomTempCooling,activePriAirTempCooling,$Y257,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T257=\"Select Model\",\"\",IF($T257=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y257,activeElevation)))","v":""},{"$f":"IF(OR(T257=\"Select Model\",T257=\"PCBL\"), 0,IF(AD257=0,0,-primaryAirSensibleCapacityIP($T257,$W257,activeRoomTempHeating,activePriAirTempHeating,$Y257,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T257=\"Select Model\", \"\", InductionRatio($T257,BD257,$W257,$Y257)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T257=\"Select Model\", \"\",IF($T257=\"PCBL\",\"N/A\",minVAVSetBack(AA257, Y257))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T257=\"Select Model\", \"\",IF($T257= \"PCBL\",\"N/A\",getDischargeAirTemp($T257,$V257,$AC257,$W257,BD257,$AL257, $Y257, $AS257, \"cooling\",activeElevation,$AB257,$AJ257,$AV257,$BB257))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T257=\"Select Model\",$T257=\"PCBL\"), \"\",getDischargeAirTemp($T257,$V257,$AD257,$W257,BD257,$AL257, $Y257, $AY257, \"heating\",activeElevation,$AB257,$AJ257,$AV257,$BB257)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T257=\"Select Model\", \"\",IF(OR($T257=\"ACBC_1W\",$T257=\"ACBC_2W\",LEFT($T257,4)=\"ACBR\",$T257 = \"LIU24_2W\",LEFT($T257,3)=\"RIU\",LEFT($T257,6)=\"ACBL12\"), IF((soundLevel($T257, $AB257, BD257, $Y257, $W257,$AJ257,$AA257,\"dba\"))<15,\"<15\",soundLevel($T257, $AB257, BD257, $Y257, $W257,$AJ257,$AA257,\"dba\")+0.4),IF((soundLevel($T257, $AB257, BD257, $Y257, $W257,$AJ257,$AA257,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T257, $AB257, BD257, $Y257, $W257,$AJ257,$AA257,\"dba\")+5)<15, \"<15\", soundLevel($T257, $AB257, BD257,$Y257, $W257,$AJ257,$AA257,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T257=\"Select Model\", \"\",IF(OR($T257=\"ACBC_1W\",$T257=\"ACBC_2W\",LEFT($T257,4)=\"ACBR\",$T257=\"LIU24_2W\",LEFT($T257,3)=\"RIU\",LEFT($T257,6)=\"ACBL12\"), IF((soundLevel($T257, $AB257, BD257, $Y257, $W257,$AJ257,$AA257,\"NC\"))<15,\"<15\",soundLevel($T257, $AB257, BD257, $Y257, $W257,$AJ257,$AA257,\"NC\")+0.4),IF((soundLevel($T257, $AB257, BD257, $Y257, $W257,$AJ257,$AA257,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T257, $AB257, BD257, $Y257, $W257,$AJ257,$AA257,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T257, $AB257, BD257, $Y257, $W257,$AJ257,$AA257,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T257=\"Select Model\",\"\",IF($T257=\"LIU24_2W\",calcQwIP($Y257,$W257,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC257,$AI257,\"latent\",$U257&\"P\"&IF($V257=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T257,activeElevation),\"\"))","v":""},{"$f":"IF($T257=\"Select Model\",\"\",IF($T257=\"ACBC_1W\",calcQwIP($Y257,$W257,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC257,BD257,\"capacity\",$U257&\"P\"&IF($V257=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T257,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y257,$W257,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC257,BD257,\"capacity\",$U257&\"P\"&IF($V257=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T257,activeElevation)))","v":""},"",{"$f":"IF(T257=\"Select Model\", 0,waterPressureDrop(W257, U257 & \"P\" & IF(V257=\"Dual\",2,1) &\"C\", AC257, \"cooling\", T257))","v":0},{"$f":"IF(T257=\"Select Model\", \"\",getReturnWaterTemp(T257,AC257, activeEWTCooling, AS257, \"cooling\"))","v":""},"",{"$f":"IF($T257<>\"ACBC_1W\",\"\",IF($J257=\"\",\"\",FintubeCapacity($T257,$W257,$AE257,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T257=\"Select Model\",T257=\"PCBL\"),\"\",calcQwIP(Y257,W257,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD257,BD257,\"capacity\",U257&\"P\"&IF(V257=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T257,activeElevation))","v":""},"",{"$f":"IF(OR(T257=\"Select Model\",T257=\"PCBL\"), \"\",IF(AY257=0,\"N/A\",waterPressureDrop(W257, U257 & \"P\" & IF(V257=\"Dual\",2,1) &\"C\", AD257, \"heating\", T257)))","v":""},{"$f":"IF(OR(T257=\"Select Model\",T257=\"PCBL\"), \"\",IF(AY257=0,getReturnWaterTemp(T257,AE257, activeEWTHeating, AX257, \"heating\"),getReturnWaterTemp(T257,AD257, activeEWTHeating, AY257, \"heating\")))","v":""},"",{"$f":" getNozzle(T257, W257, Y257, Z257, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I258)),I258<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I258, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H258)),H258<0),\"\",intlEstQuantity(T258, W258*12, H258)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T258=\"Select Model\",\"\",coilCircuitChange(W258, U258, AC258, T258,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T258=\"Select Model\",\"\",beamWidth(T258))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T258=\"Select Model\",T258=\"PCBL\"), 0,getSPIP(T258, W258, Y258, BD258, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T258=\"Select Model\", \"\",IF(T258=\"PCBL\",0,primaryAirSensibleCapacityIP($T258,$W258,activeRoomTempCooling,activePriAirTempCooling,$Y258,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T258=\"Select Model\",\"\",IF($T258=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y258,activeElevation)))","v":""},{"$f":"IF(OR(T258=\"Select Model\",T258=\"PCBL\"), 0,IF(AD258=0,0,-primaryAirSensibleCapacityIP($T258,$W258,activeRoomTempHeating,activePriAirTempHeating,$Y258,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T258=\"Select Model\", \"\", InductionRatio($T258,BD258,$W258,$Y258)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T258=\"Select Model\", \"\",IF($T258=\"PCBL\",\"N/A\",minVAVSetBack(AA258, Y258))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T258=\"Select Model\", \"\",IF($T258= \"PCBL\",\"N/A\",getDischargeAirTemp($T258,$V258,$AC258,$W258,BD258,$AL258, $Y258, $AS258, \"cooling\",activeElevation,$AB258,$AJ258,$AV258,$BB258))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T258=\"Select Model\",$T258=\"PCBL\"), \"\",getDischargeAirTemp($T258,$V258,$AD258,$W258,BD258,$AL258, $Y258, $AY258, \"heating\",activeElevation,$AB258,$AJ258,$AV258,$BB258)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T258=\"Select Model\", \"\",IF(OR($T258=\"ACBC_1W\",$T258=\"ACBC_2W\",LEFT($T258,4)=\"ACBR\",$T258 = \"LIU24_2W\",LEFT($T258,3)=\"RIU\",LEFT($T258,6)=\"ACBL12\"), IF((soundLevel($T258, $AB258, BD258, $Y258, $W258,$AJ258,$AA258,\"dba\"))<15,\"<15\",soundLevel($T258, $AB258, BD258, $Y258, $W258,$AJ258,$AA258,\"dba\")+0.4),IF((soundLevel($T258, $AB258, BD258, $Y258, $W258,$AJ258,$AA258,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T258, $AB258, BD258, $Y258, $W258,$AJ258,$AA258,\"dba\")+5)<15, \"<15\", soundLevel($T258, $AB258, BD258,$Y258, $W258,$AJ258,$AA258,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T258=\"Select Model\", \"\",IF(OR($T258=\"ACBC_1W\",$T258=\"ACBC_2W\",LEFT($T258,4)=\"ACBR\",$T258=\"LIU24_2W\",LEFT($T258,3)=\"RIU\",LEFT($T258,6)=\"ACBL12\"), IF((soundLevel($T258, $AB258, BD258, $Y258, $W258,$AJ258,$AA258,\"NC\"))<15,\"<15\",soundLevel($T258, $AB258, BD258, $Y258, $W258,$AJ258,$AA258,\"NC\")+0.4),IF((soundLevel($T258, $AB258, BD258, $Y258, $W258,$AJ258,$AA258,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T258, $AB258, BD258, $Y258, $W258,$AJ258,$AA258,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T258, $AB258, BD258, $Y258, $W258,$AJ258,$AA258,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T258=\"Select Model\",\"\",IF($T258=\"LIU24_2W\",calcQwIP($Y258,$W258,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC258,$AI258,\"latent\",$U258&\"P\"&IF($V258=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T258,activeElevation),\"\"))","v":""},{"$f":"IF($T258=\"Select Model\",\"\",IF($T258=\"ACBC_1W\",calcQwIP($Y258,$W258,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC258,BD258,\"capacity\",$U258&\"P\"&IF($V258=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T258,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y258,$W258,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC258,BD258,\"capacity\",$U258&\"P\"&IF($V258=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T258,activeElevation)))","v":""},"",{"$f":"IF(T258=\"Select Model\", 0,waterPressureDrop(W258, U258 & \"P\" & IF(V258=\"Dual\",2,1) &\"C\", AC258, \"cooling\", T258))","v":0},{"$f":"IF(T258=\"Select Model\", \"\",getReturnWaterTemp(T258,AC258, activeEWTCooling, AS258, \"cooling\"))","v":""},"",{"$f":"IF($T258<>\"ACBC_1W\",\"\",IF($J258=\"\",\"\",FintubeCapacity($T258,$W258,$AE258,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T258=\"Select Model\",T258=\"PCBL\"),\"\",calcQwIP(Y258,W258,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD258,BD258,\"capacity\",U258&\"P\"&IF(V258=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T258,activeElevation))","v":""},"",{"$f":"IF(OR(T258=\"Select Model\",T258=\"PCBL\"), \"\",IF(AY258=0,\"N/A\",waterPressureDrop(W258, U258 & \"P\" & IF(V258=\"Dual\",2,1) &\"C\", AD258, \"heating\", T258)))","v":""},{"$f":"IF(OR(T258=\"Select Model\",T258=\"PCBL\"), \"\",IF(AY258=0,getReturnWaterTemp(T258,AE258, activeEWTHeating, AX258, \"heating\"),getReturnWaterTemp(T258,AD258, activeEWTHeating, AY258, \"heating\")))","v":""},"",{"$f":" getNozzle(T258, W258, Y258, Z258, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I259)),I259<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I259, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H259)),H259<0),\"\",intlEstQuantity(T259, W259*12, H259)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T259=\"Select Model\",\"\",coilCircuitChange(W259, U259, AC259, T259,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T259=\"Select Model\",\"\",beamWidth(T259))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T259=\"Select Model\",T259=\"PCBL\"), 0,getSPIP(T259, W259, Y259, BD259, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T259=\"Select Model\", \"\",IF(T259=\"PCBL\",0,primaryAirSensibleCapacityIP($T259,$W259,activeRoomTempCooling,activePriAirTempCooling,$Y259,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T259=\"Select Model\",\"\",IF($T259=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y259,activeElevation)))","v":""},{"$f":"IF(OR(T259=\"Select Model\",T259=\"PCBL\"), 0,IF(AD259=0,0,-primaryAirSensibleCapacityIP($T259,$W259,activeRoomTempHeating,activePriAirTempHeating,$Y259,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T259=\"Select Model\", \"\", InductionRatio($T259,BD259,$W259,$Y259)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T259=\"Select Model\", \"\",IF($T259=\"PCBL\",\"N/A\",minVAVSetBack(AA259, Y259))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T259=\"Select Model\", \"\",IF($T259= \"PCBL\",\"N/A\",getDischargeAirTemp($T259,$V259,$AC259,$W259,BD259,$AL259, $Y259, $AS259, \"cooling\",activeElevation,$AB259,$AJ259,$AV259,$BB259))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T259=\"Select Model\",$T259=\"PCBL\"), \"\",getDischargeAirTemp($T259,$V259,$AD259,$W259,BD259,$AL259, $Y259, $AY259, \"heating\",activeElevation,$AB259,$AJ259,$AV259,$BB259)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T259=\"Select Model\", \"\",IF(OR($T259=\"ACBC_1W\",$T259=\"ACBC_2W\",LEFT($T259,4)=\"ACBR\",$T259 = \"LIU24_2W\",LEFT($T259,3)=\"RIU\",LEFT($T259,6)=\"ACBL12\"), IF((soundLevel($T259, $AB259, BD259, $Y259, $W259,$AJ259,$AA259,\"dba\"))<15,\"<15\",soundLevel($T259, $AB259, BD259, $Y259, $W259,$AJ259,$AA259,\"dba\")+0.4),IF((soundLevel($T259, $AB259, BD259, $Y259, $W259,$AJ259,$AA259,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T259, $AB259, BD259, $Y259, $W259,$AJ259,$AA259,\"dba\")+5)<15, \"<15\", soundLevel($T259, $AB259, BD259,$Y259, $W259,$AJ259,$AA259,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T259=\"Select Model\", \"\",IF(OR($T259=\"ACBC_1W\",$T259=\"ACBC_2W\",LEFT($T259,4)=\"ACBR\",$T259=\"LIU24_2W\",LEFT($T259,3)=\"RIU\",LEFT($T259,6)=\"ACBL12\"), IF((soundLevel($T259, $AB259, BD259, $Y259, $W259,$AJ259,$AA259,\"NC\"))<15,\"<15\",soundLevel($T259, $AB259, BD259, $Y259, $W259,$AJ259,$AA259,\"NC\")+0.4),IF((soundLevel($T259, $AB259, BD259, $Y259, $W259,$AJ259,$AA259,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T259, $AB259, BD259, $Y259, $W259,$AJ259,$AA259,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T259, $AB259, BD259, $Y259, $W259,$AJ259,$AA259,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T259=\"Select Model\",\"\",IF($T259=\"LIU24_2W\",calcQwIP($Y259,$W259,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC259,$AI259,\"latent\",$U259&\"P\"&IF($V259=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T259,activeElevation),\"\"))","v":""},{"$f":"IF($T259=\"Select Model\",\"\",IF($T259=\"ACBC_1W\",calcQwIP($Y259,$W259,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC259,BD259,\"capacity\",$U259&\"P\"&IF($V259=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T259,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y259,$W259,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC259,BD259,\"capacity\",$U259&\"P\"&IF($V259=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T259,activeElevation)))","v":""},"",{"$f":"IF(T259=\"Select Model\", 0,waterPressureDrop(W259, U259 & \"P\" & IF(V259=\"Dual\",2,1) &\"C\", AC259, \"cooling\", T259))","v":0},{"$f":"IF(T259=\"Select Model\", \"\",getReturnWaterTemp(T259,AC259, activeEWTCooling, AS259, \"cooling\"))","v":""},"",{"$f":"IF($T259<>\"ACBC_1W\",\"\",IF($J259=\"\",\"\",FintubeCapacity($T259,$W259,$AE259,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T259=\"Select Model\",T259=\"PCBL\"),\"\",calcQwIP(Y259,W259,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD259,BD259,\"capacity\",U259&\"P\"&IF(V259=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T259,activeElevation))","v":""},"",{"$f":"IF(OR(T259=\"Select Model\",T259=\"PCBL\"), \"\",IF(AY259=0,\"N/A\",waterPressureDrop(W259, U259 & \"P\" & IF(V259=\"Dual\",2,1) &\"C\", AD259, \"heating\", T259)))","v":""},{"$f":"IF(OR(T259=\"Select Model\",T259=\"PCBL\"), \"\",IF(AY259=0,getReturnWaterTemp(T259,AE259, activeEWTHeating, AX259, \"heating\"),getReturnWaterTemp(T259,AD259, activeEWTHeating, AY259, \"heating\")))","v":""},"",{"$f":" getNozzle(T259, W259, Y259, Z259, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I260)),I260<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I260, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H260)),H260<0),\"\",intlEstQuantity(T260, W260*12, H260)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T260=\"Select Model\",\"\",coilCircuitChange(W260, U260, AC260, T260,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T260=\"Select Model\",\"\",beamWidth(T260))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T260=\"Select Model\",T260=\"PCBL\"), 0,getSPIP(T260, W260, Y260, BD260, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T260=\"Select Model\", \"\",IF(T260=\"PCBL\",0,primaryAirSensibleCapacityIP($T260,$W260,activeRoomTempCooling,activePriAirTempCooling,$Y260,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T260=\"Select Model\",\"\",IF($T260=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y260,activeElevation)))","v":""},{"$f":"IF(OR(T260=\"Select Model\",T260=\"PCBL\"), 0,IF(AD260=0,0,-primaryAirSensibleCapacityIP($T260,$W260,activeRoomTempHeating,activePriAirTempHeating,$Y260,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T260=\"Select Model\", \"\", InductionRatio($T260,BD260,$W260,$Y260)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T260=\"Select Model\", \"\",IF($T260=\"PCBL\",\"N/A\",minVAVSetBack(AA260, Y260))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T260=\"Select Model\", \"\",IF($T260= \"PCBL\",\"N/A\",getDischargeAirTemp($T260,$V260,$AC260,$W260,BD260,$AL260, $Y260, $AS260, \"cooling\",activeElevation,$AB260,$AJ260,$AV260,$BB260))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T260=\"Select Model\",$T260=\"PCBL\"), \"\",getDischargeAirTemp($T260,$V260,$AD260,$W260,BD260,$AL260, $Y260, $AY260, \"heating\",activeElevation,$AB260,$AJ260,$AV260,$BB260)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T260=\"Select Model\", \"\",IF(OR($T260=\"ACBC_1W\",$T260=\"ACBC_2W\",LEFT($T260,4)=\"ACBR\",$T260 = \"LIU24_2W\",LEFT($T260,3)=\"RIU\",LEFT($T260,6)=\"ACBL12\"), IF((soundLevel($T260, $AB260, BD260, $Y260, $W260,$AJ260,$AA260,\"dba\"))<15,\"<15\",soundLevel($T260, $AB260, BD260, $Y260, $W260,$AJ260,$AA260,\"dba\")+0.4),IF((soundLevel($T260, $AB260, BD260, $Y260, $W260,$AJ260,$AA260,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T260, $AB260, BD260, $Y260, $W260,$AJ260,$AA260,\"dba\")+5)<15, \"<15\", soundLevel($T260, $AB260, BD260,$Y260, $W260,$AJ260,$AA260,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T260=\"Select Model\", \"\",IF(OR($T260=\"ACBC_1W\",$T260=\"ACBC_2W\",LEFT($T260,4)=\"ACBR\",$T260=\"LIU24_2W\",LEFT($T260,3)=\"RIU\",LEFT($T260,6)=\"ACBL12\"), IF((soundLevel($T260, $AB260, BD260, $Y260, $W260,$AJ260,$AA260,\"NC\"))<15,\"<15\",soundLevel($T260, $AB260, BD260, $Y260, $W260,$AJ260,$AA260,\"NC\")+0.4),IF((soundLevel($T260, $AB260, BD260, $Y260, $W260,$AJ260,$AA260,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T260, $AB260, BD260, $Y260, $W260,$AJ260,$AA260,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T260, $AB260, BD260, $Y260, $W260,$AJ260,$AA260,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T260=\"Select Model\",\"\",IF($T260=\"LIU24_2W\",calcQwIP($Y260,$W260,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC260,$AI260,\"latent\",$U260&\"P\"&IF($V260=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T260,activeElevation),\"\"))","v":""},{"$f":"IF($T260=\"Select Model\",\"\",IF($T260=\"ACBC_1W\",calcQwIP($Y260,$W260,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC260,BD260,\"capacity\",$U260&\"P\"&IF($V260=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T260,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y260,$W260,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC260,BD260,\"capacity\",$U260&\"P\"&IF($V260=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T260,activeElevation)))","v":""},"",{"$f":"IF(T260=\"Select Model\", 0,waterPressureDrop(W260, U260 & \"P\" & IF(V260=\"Dual\",2,1) &\"C\", AC260, \"cooling\", T260))","v":0},{"$f":"IF(T260=\"Select Model\", \"\",getReturnWaterTemp(T260,AC260, activeEWTCooling, AS260, \"cooling\"))","v":""},"",{"$f":"IF($T260<>\"ACBC_1W\",\"\",IF($J260=\"\",\"\",FintubeCapacity($T260,$W260,$AE260,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T260=\"Select Model\",T260=\"PCBL\"),\"\",calcQwIP(Y260,W260,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD260,BD260,\"capacity\",U260&\"P\"&IF(V260=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T260,activeElevation))","v":""},"",{"$f":"IF(OR(T260=\"Select Model\",T260=\"PCBL\"), \"\",IF(AY260=0,\"N/A\",waterPressureDrop(W260, U260 & \"P\" & IF(V260=\"Dual\",2,1) &\"C\", AD260, \"heating\", T260)))","v":""},{"$f":"IF(OR(T260=\"Select Model\",T260=\"PCBL\"), \"\",IF(AY260=0,getReturnWaterTemp(T260,AE260, activeEWTHeating, AX260, \"heating\"),getReturnWaterTemp(T260,AD260, activeEWTHeating, AY260, \"heating\")))","v":""},"",{"$f":" getNozzle(T260, W260, Y260, Z260, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I261)),I261<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I261, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H261)),H261<0),\"\",intlEstQuantity(T261, W261*12, H261)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T261=\"Select Model\",\"\",coilCircuitChange(W261, U261, AC261, T261,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T261=\"Select Model\",\"\",beamWidth(T261))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T261=\"Select Model\",T261=\"PCBL\"), 0,getSPIP(T261, W261, Y261, BD261, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T261=\"Select Model\", \"\",IF(T261=\"PCBL\",0,primaryAirSensibleCapacityIP($T261,$W261,activeRoomTempCooling,activePriAirTempCooling,$Y261,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T261=\"Select Model\",\"\",IF($T261=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y261,activeElevation)))","v":""},{"$f":"IF(OR(T261=\"Select Model\",T261=\"PCBL\"), 0,IF(AD261=0,0,-primaryAirSensibleCapacityIP($T261,$W261,activeRoomTempHeating,activePriAirTempHeating,$Y261,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T261=\"Select Model\", \"\", InductionRatio($T261,BD261,$W261,$Y261)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T261=\"Select Model\", \"\",IF($T261=\"PCBL\",\"N/A\",minVAVSetBack(AA261, Y261))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T261=\"Select Model\", \"\",IF($T261= \"PCBL\",\"N/A\",getDischargeAirTemp($T261,$V261,$AC261,$W261,BD261,$AL261, $Y261, $AS261, \"cooling\",activeElevation,$AB261,$AJ261,$AV261,$BB261))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T261=\"Select Model\",$T261=\"PCBL\"), \"\",getDischargeAirTemp($T261,$V261,$AD261,$W261,BD261,$AL261, $Y261, $AY261, \"heating\",activeElevation,$AB261,$AJ261,$AV261,$BB261)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T261=\"Select Model\", \"\",IF(OR($T261=\"ACBC_1W\",$T261=\"ACBC_2W\",LEFT($T261,4)=\"ACBR\",$T261 = \"LIU24_2W\",LEFT($T261,3)=\"RIU\",LEFT($T261,6)=\"ACBL12\"), IF((soundLevel($T261, $AB261, BD261, $Y261, $W261,$AJ261,$AA261,\"dba\"))<15,\"<15\",soundLevel($T261, $AB261, BD261, $Y261, $W261,$AJ261,$AA261,\"dba\")+0.4),IF((soundLevel($T261, $AB261, BD261, $Y261, $W261,$AJ261,$AA261,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T261, $AB261, BD261, $Y261, $W261,$AJ261,$AA261,\"dba\")+5)<15, \"<15\", soundLevel($T261, $AB261, BD261,$Y261, $W261,$AJ261,$AA261,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T261=\"Select Model\", \"\",IF(OR($T261=\"ACBC_1W\",$T261=\"ACBC_2W\",LEFT($T261,4)=\"ACBR\",$T261=\"LIU24_2W\",LEFT($T261,3)=\"RIU\",LEFT($T261,6)=\"ACBL12\"), IF((soundLevel($T261, $AB261, BD261, $Y261, $W261,$AJ261,$AA261,\"NC\"))<15,\"<15\",soundLevel($T261, $AB261, BD261, $Y261, $W261,$AJ261,$AA261,\"NC\")+0.4),IF((soundLevel($T261, $AB261, BD261, $Y261, $W261,$AJ261,$AA261,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T261, $AB261, BD261, $Y261, $W261,$AJ261,$AA261,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T261, $AB261, BD261, $Y261, $W261,$AJ261,$AA261,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T261=\"Select Model\",\"\",IF($T261=\"LIU24_2W\",calcQwIP($Y261,$W261,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC261,$AI261,\"latent\",$U261&\"P\"&IF($V261=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T261,activeElevation),\"\"))","v":""},{"$f":"IF($T261=\"Select Model\",\"\",IF($T261=\"ACBC_1W\",calcQwIP($Y261,$W261,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC261,BD261,\"capacity\",$U261&\"P\"&IF($V261=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T261,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y261,$W261,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC261,BD261,\"capacity\",$U261&\"P\"&IF($V261=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T261,activeElevation)))","v":""},"",{"$f":"IF(T261=\"Select Model\", 0,waterPressureDrop(W261, U261 & \"P\" & IF(V261=\"Dual\",2,1) &\"C\", AC261, \"cooling\", T261))","v":0},{"$f":"IF(T261=\"Select Model\", \"\",getReturnWaterTemp(T261,AC261, activeEWTCooling, AS261, \"cooling\"))","v":""},"",{"$f":"IF($T261<>\"ACBC_1W\",\"\",IF($J261=\"\",\"\",FintubeCapacity($T261,$W261,$AE261,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T261=\"Select Model\",T261=\"PCBL\"),\"\",calcQwIP(Y261,W261,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD261,BD261,\"capacity\",U261&\"P\"&IF(V261=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T261,activeElevation))","v":""},"",{"$f":"IF(OR(T261=\"Select Model\",T261=\"PCBL\"), \"\",IF(AY261=0,\"N/A\",waterPressureDrop(W261, U261 & \"P\" & IF(V261=\"Dual\",2,1) &\"C\", AD261, \"heating\", T261)))","v":""},{"$f":"IF(OR(T261=\"Select Model\",T261=\"PCBL\"), \"\",IF(AY261=0,getReturnWaterTemp(T261,AE261, activeEWTHeating, AX261, \"heating\"),getReturnWaterTemp(T261,AD261, activeEWTHeating, AY261, \"heating\")))","v":""},"",{"$f":" getNozzle(T261, W261, Y261, Z261, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I262)),I262<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I262, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H262)),H262<0),\"\",intlEstQuantity(T262, W262*12, H262)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T262=\"Select Model\",\"\",coilCircuitChange(W262, U262, AC262, T262,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T262=\"Select Model\",\"\",beamWidth(T262))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T262=\"Select Model\",T262=\"PCBL\"), 0,getSPIP(T262, W262, Y262, BD262, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T262=\"Select Model\", \"\",IF(T262=\"PCBL\",0,primaryAirSensibleCapacityIP($T262,$W262,activeRoomTempCooling,activePriAirTempCooling,$Y262,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T262=\"Select Model\",\"\",IF($T262=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y262,activeElevation)))","v":""},{"$f":"IF(OR(T262=\"Select Model\",T262=\"PCBL\"), 0,IF(AD262=0,0,-primaryAirSensibleCapacityIP($T262,$W262,activeRoomTempHeating,activePriAirTempHeating,$Y262,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T262=\"Select Model\", \"\", InductionRatio($T262,BD262,$W262,$Y262)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T262=\"Select Model\", \"\",IF($T262=\"PCBL\",\"N/A\",minVAVSetBack(AA262, Y262))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T262=\"Select Model\", \"\",IF($T262= \"PCBL\",\"N/A\",getDischargeAirTemp($T262,$V262,$AC262,$W262,BD262,$AL262, $Y262, $AS262, \"cooling\",activeElevation,$AB262,$AJ262,$AV262,$BB262))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T262=\"Select Model\",$T262=\"PCBL\"), \"\",getDischargeAirTemp($T262,$V262,$AD262,$W262,BD262,$AL262, $Y262, $AY262, \"heating\",activeElevation,$AB262,$AJ262,$AV262,$BB262)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T262=\"Select Model\", \"\",IF(OR($T262=\"ACBC_1W\",$T262=\"ACBC_2W\",LEFT($T262,4)=\"ACBR\",$T262 = \"LIU24_2W\",LEFT($T262,3)=\"RIU\",LEFT($T262,6)=\"ACBL12\"), IF((soundLevel($T262, $AB262, BD262, $Y262, $W262,$AJ262,$AA262,\"dba\"))<15,\"<15\",soundLevel($T262, $AB262, BD262, $Y262, $W262,$AJ262,$AA262,\"dba\")+0.4),IF((soundLevel($T262, $AB262, BD262, $Y262, $W262,$AJ262,$AA262,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T262, $AB262, BD262, $Y262, $W262,$AJ262,$AA262,\"dba\")+5)<15, \"<15\", soundLevel($T262, $AB262, BD262,$Y262, $W262,$AJ262,$AA262,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T262=\"Select Model\", \"\",IF(OR($T262=\"ACBC_1W\",$T262=\"ACBC_2W\",LEFT($T262,4)=\"ACBR\",$T262=\"LIU24_2W\",LEFT($T262,3)=\"RIU\",LEFT($T262,6)=\"ACBL12\"), IF((soundLevel($T262, $AB262, BD262, $Y262, $W262,$AJ262,$AA262,\"NC\"))<15,\"<15\",soundLevel($T262, $AB262, BD262, $Y262, $W262,$AJ262,$AA262,\"NC\")+0.4),IF((soundLevel($T262, $AB262, BD262, $Y262, $W262,$AJ262,$AA262,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T262, $AB262, BD262, $Y262, $W262,$AJ262,$AA262,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T262, $AB262, BD262, $Y262, $W262,$AJ262,$AA262,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T262=\"Select Model\",\"\",IF($T262=\"LIU24_2W\",calcQwIP($Y262,$W262,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC262,$AI262,\"latent\",$U262&\"P\"&IF($V262=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T262,activeElevation),\"\"))","v":""},{"$f":"IF($T262=\"Select Model\",\"\",IF($T262=\"ACBC_1W\",calcQwIP($Y262,$W262,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC262,BD262,\"capacity\",$U262&\"P\"&IF($V262=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T262,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y262,$W262,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC262,BD262,\"capacity\",$U262&\"P\"&IF($V262=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T262,activeElevation)))","v":""},"",{"$f":"IF(T262=\"Select Model\", 0,waterPressureDrop(W262, U262 & \"P\" & IF(V262=\"Dual\",2,1) &\"C\", AC262, \"cooling\", T262))","v":0},{"$f":"IF(T262=\"Select Model\", \"\",getReturnWaterTemp(T262,AC262, activeEWTCooling, AS262, \"cooling\"))","v":""},"",{"$f":"IF($T262<>\"ACBC_1W\",\"\",IF($J262=\"\",\"\",FintubeCapacity($T262,$W262,$AE262,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T262=\"Select Model\",T262=\"PCBL\"),\"\",calcQwIP(Y262,W262,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD262,BD262,\"capacity\",U262&\"P\"&IF(V262=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T262,activeElevation))","v":""},"",{"$f":"IF(OR(T262=\"Select Model\",T262=\"PCBL\"), \"\",IF(AY262=0,\"N/A\",waterPressureDrop(W262, U262 & \"P\" & IF(V262=\"Dual\",2,1) &\"C\", AD262, \"heating\", T262)))","v":""},{"$f":"IF(OR(T262=\"Select Model\",T262=\"PCBL\"), \"\",IF(AY262=0,getReturnWaterTemp(T262,AE262, activeEWTHeating, AX262, \"heating\"),getReturnWaterTemp(T262,AD262, activeEWTHeating, AY262, \"heating\")))","v":""},"",{"$f":" getNozzle(T262, W262, Y262, Z262, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I263)),I263<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I263, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H263)),H263<0),\"\",intlEstQuantity(T263, W263*12, H263)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T263=\"Select Model\",\"\",coilCircuitChange(W263, U263, AC263, T263,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T263=\"Select Model\",\"\",beamWidth(T263))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T263=\"Select Model\",T263=\"PCBL\"), 0,getSPIP(T263, W263, Y263, BD263, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T263=\"Select Model\", \"\",IF(T263=\"PCBL\",0,primaryAirSensibleCapacityIP($T263,$W263,activeRoomTempCooling,activePriAirTempCooling,$Y263,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T263=\"Select Model\",\"\",IF($T263=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y263,activeElevation)))","v":""},{"$f":"IF(OR(T263=\"Select Model\",T263=\"PCBL\"), 0,IF(AD263=0,0,-primaryAirSensibleCapacityIP($T263,$W263,activeRoomTempHeating,activePriAirTempHeating,$Y263,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T263=\"Select Model\", \"\", InductionRatio($T263,BD263,$W263,$Y263)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T263=\"Select Model\", \"\",IF($T263=\"PCBL\",\"N/A\",minVAVSetBack(AA263, Y263))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T263=\"Select Model\", \"\",IF($T263= \"PCBL\",\"N/A\",getDischargeAirTemp($T263,$V263,$AC263,$W263,BD263,$AL263, $Y263, $AS263, \"cooling\",activeElevation,$AB263,$AJ263,$AV263,$BB263))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T263=\"Select Model\",$T263=\"PCBL\"), \"\",getDischargeAirTemp($T263,$V263,$AD263,$W263,BD263,$AL263, $Y263, $AY263, \"heating\",activeElevation,$AB263,$AJ263,$AV263,$BB263)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T263=\"Select Model\", \"\",IF(OR($T263=\"ACBC_1W\",$T263=\"ACBC_2W\",LEFT($T263,4)=\"ACBR\",$T263 = \"LIU24_2W\",LEFT($T263,3)=\"RIU\",LEFT($T263,6)=\"ACBL12\"), IF((soundLevel($T263, $AB263, BD263, $Y263, $W263,$AJ263,$AA263,\"dba\"))<15,\"<15\",soundLevel($T263, $AB263, BD263, $Y263, $W263,$AJ263,$AA263,\"dba\")+0.4),IF((soundLevel($T263, $AB263, BD263, $Y263, $W263,$AJ263,$AA263,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T263, $AB263, BD263, $Y263, $W263,$AJ263,$AA263,\"dba\")+5)<15, \"<15\", soundLevel($T263, $AB263, BD263,$Y263, $W263,$AJ263,$AA263,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T263=\"Select Model\", \"\",IF(OR($T263=\"ACBC_1W\",$T263=\"ACBC_2W\",LEFT($T263,4)=\"ACBR\",$T263=\"LIU24_2W\",LEFT($T263,3)=\"RIU\",LEFT($T263,6)=\"ACBL12\"), IF((soundLevel($T263, $AB263, BD263, $Y263, $W263,$AJ263,$AA263,\"NC\"))<15,\"<15\",soundLevel($T263, $AB263, BD263, $Y263, $W263,$AJ263,$AA263,\"NC\")+0.4),IF((soundLevel($T263, $AB263, BD263, $Y263, $W263,$AJ263,$AA263,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T263, $AB263, BD263, $Y263, $W263,$AJ263,$AA263,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T263, $AB263, BD263, $Y263, $W263,$AJ263,$AA263,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T263=\"Select Model\",\"\",IF($T263=\"LIU24_2W\",calcQwIP($Y263,$W263,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC263,$AI263,\"latent\",$U263&\"P\"&IF($V263=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T263,activeElevation),\"\"))","v":""},{"$f":"IF($T263=\"Select Model\",\"\",IF($T263=\"ACBC_1W\",calcQwIP($Y263,$W263,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC263,BD263,\"capacity\",$U263&\"P\"&IF($V263=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T263,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y263,$W263,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC263,BD263,\"capacity\",$U263&\"P\"&IF($V263=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T263,activeElevation)))","v":""},"",{"$f":"IF(T263=\"Select Model\", 0,waterPressureDrop(W263, U263 & \"P\" & IF(V263=\"Dual\",2,1) &\"C\", AC263, \"cooling\", T263))","v":0},{"$f":"IF(T263=\"Select Model\", \"\",getReturnWaterTemp(T263,AC263, activeEWTCooling, AS263, \"cooling\"))","v":""},"",{"$f":"IF($T263<>\"ACBC_1W\",\"\",IF($J263=\"\",\"\",FintubeCapacity($T263,$W263,$AE263,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T263=\"Select Model\",T263=\"PCBL\"),\"\",calcQwIP(Y263,W263,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD263,BD263,\"capacity\",U263&\"P\"&IF(V263=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T263,activeElevation))","v":""},"",{"$f":"IF(OR(T263=\"Select Model\",T263=\"PCBL\"), \"\",IF(AY263=0,\"N/A\",waterPressureDrop(W263, U263 & \"P\" & IF(V263=\"Dual\",2,1) &\"C\", AD263, \"heating\", T263)))","v":""},{"$f":"IF(OR(T263=\"Select Model\",T263=\"PCBL\"), \"\",IF(AY263=0,getReturnWaterTemp(T263,AE263, activeEWTHeating, AX263, \"heating\"),getReturnWaterTemp(T263,AD263, activeEWTHeating, AY263, \"heating\")))","v":""},"",{"$f":" getNozzle(T263, W263, Y263, Z263, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I264)),I264<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I264, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H264)),H264<0),\"\",intlEstQuantity(T264, W264*12, H264)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T264=\"Select Model\",\"\",coilCircuitChange(W264, U264, AC264, T264,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T264=\"Select Model\",\"\",beamWidth(T264))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T264=\"Select Model\",T264=\"PCBL\"), 0,getSPIP(T264, W264, Y264, BD264, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T264=\"Select Model\", \"\",IF(T264=\"PCBL\",0,primaryAirSensibleCapacityIP($T264,$W264,activeRoomTempCooling,activePriAirTempCooling,$Y264,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T264=\"Select Model\",\"\",IF($T264=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y264,activeElevation)))","v":""},{"$f":"IF(OR(T264=\"Select Model\",T264=\"PCBL\"), 0,IF(AD264=0,0,-primaryAirSensibleCapacityIP($T264,$W264,activeRoomTempHeating,activePriAirTempHeating,$Y264,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T264=\"Select Model\", \"\", InductionRatio($T264,BD264,$W264,$Y264)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T264=\"Select Model\", \"\",IF($T264=\"PCBL\",\"N/A\",minVAVSetBack(AA264, Y264))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T264=\"Select Model\", \"\",IF($T264= \"PCBL\",\"N/A\",getDischargeAirTemp($T264,$V264,$AC264,$W264,BD264,$AL264, $Y264, $AS264, \"cooling\",activeElevation,$AB264,$AJ264,$AV264,$BB264))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T264=\"Select Model\",$T264=\"PCBL\"), \"\",getDischargeAirTemp($T264,$V264,$AD264,$W264,BD264,$AL264, $Y264, $AY264, \"heating\",activeElevation,$AB264,$AJ264,$AV264,$BB264)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T264=\"Select Model\", \"\",IF(OR($T264=\"ACBC_1W\",$T264=\"ACBC_2W\",LEFT($T264,4)=\"ACBR\",$T264 = \"LIU24_2W\",LEFT($T264,3)=\"RIU\",LEFT($T264,6)=\"ACBL12\"), IF((soundLevel($T264, $AB264, BD264, $Y264, $W264,$AJ264,$AA264,\"dba\"))<15,\"<15\",soundLevel($T264, $AB264, BD264, $Y264, $W264,$AJ264,$AA264,\"dba\")+0.4),IF((soundLevel($T264, $AB264, BD264, $Y264, $W264,$AJ264,$AA264,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T264, $AB264, BD264, $Y264, $W264,$AJ264,$AA264,\"dba\")+5)<15, \"<15\", soundLevel($T264, $AB264, BD264,$Y264, $W264,$AJ264,$AA264,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T264=\"Select Model\", \"\",IF(OR($T264=\"ACBC_1W\",$T264=\"ACBC_2W\",LEFT($T264,4)=\"ACBR\",$T264=\"LIU24_2W\",LEFT($T264,3)=\"RIU\",LEFT($T264,6)=\"ACBL12\"), IF((soundLevel($T264, $AB264, BD264, $Y264, $W264,$AJ264,$AA264,\"NC\"))<15,\"<15\",soundLevel($T264, $AB264, BD264, $Y264, $W264,$AJ264,$AA264,\"NC\")+0.4),IF((soundLevel($T264, $AB264, BD264, $Y264, $W264,$AJ264,$AA264,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T264, $AB264, BD264, $Y264, $W264,$AJ264,$AA264,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T264, $AB264, BD264, $Y264, $W264,$AJ264,$AA264,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T264=\"Select Model\",\"\",IF($T264=\"LIU24_2W\",calcQwIP($Y264,$W264,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC264,$AI264,\"latent\",$U264&\"P\"&IF($V264=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T264,activeElevation),\"\"))","v":""},{"$f":"IF($T264=\"Select Model\",\"\",IF($T264=\"ACBC_1W\",calcQwIP($Y264,$W264,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC264,BD264,\"capacity\",$U264&\"P\"&IF($V264=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T264,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y264,$W264,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC264,BD264,\"capacity\",$U264&\"P\"&IF($V264=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T264,activeElevation)))","v":""},"",{"$f":"IF(T264=\"Select Model\", 0,waterPressureDrop(W264, U264 & \"P\" & IF(V264=\"Dual\",2,1) &\"C\", AC264, \"cooling\", T264))","v":0},{"$f":"IF(T264=\"Select Model\", \"\",getReturnWaterTemp(T264,AC264, activeEWTCooling, AS264, \"cooling\"))","v":""},"",{"$f":"IF($T264<>\"ACBC_1W\",\"\",IF($J264=\"\",\"\",FintubeCapacity($T264,$W264,$AE264,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T264=\"Select Model\",T264=\"PCBL\"),\"\",calcQwIP(Y264,W264,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD264,BD264,\"capacity\",U264&\"P\"&IF(V264=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T264,activeElevation))","v":""},"",{"$f":"IF(OR(T264=\"Select Model\",T264=\"PCBL\"), \"\",IF(AY264=0,\"N/A\",waterPressureDrop(W264, U264 & \"P\" & IF(V264=\"Dual\",2,1) &\"C\", AD264, \"heating\", T264)))","v":""},{"$f":"IF(OR(T264=\"Select Model\",T264=\"PCBL\"), \"\",IF(AY264=0,getReturnWaterTemp(T264,AE264, activeEWTHeating, AX264, \"heating\"),getReturnWaterTemp(T264,AD264, activeEWTHeating, AY264, \"heating\")))","v":""},"",{"$f":" getNozzle(T264, W264, Y264, Z264, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I265)),I265<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I265, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H265)),H265<0),\"\",intlEstQuantity(T265, W265*12, H265)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T265=\"Select Model\",\"\",coilCircuitChange(W265, U265, AC265, T265,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T265=\"Select Model\",\"\",beamWidth(T265))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T265=\"Select Model\",T265=\"PCBL\"), 0,getSPIP(T265, W265, Y265, BD265, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T265=\"Select Model\", \"\",IF(T265=\"PCBL\",0,primaryAirSensibleCapacityIP($T265,$W265,activeRoomTempCooling,activePriAirTempCooling,$Y265,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T265=\"Select Model\",\"\",IF($T265=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y265,activeElevation)))","v":""},{"$f":"IF(OR(T265=\"Select Model\",T265=\"PCBL\"), 0,IF(AD265=0,0,-primaryAirSensibleCapacityIP($T265,$W265,activeRoomTempHeating,activePriAirTempHeating,$Y265,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T265=\"Select Model\", \"\", InductionRatio($T265,BD265,$W265,$Y265)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T265=\"Select Model\", \"\",IF($T265=\"PCBL\",\"N/A\",minVAVSetBack(AA265, Y265))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T265=\"Select Model\", \"\",IF($T265= \"PCBL\",\"N/A\",getDischargeAirTemp($T265,$V265,$AC265,$W265,BD265,$AL265, $Y265, $AS265, \"cooling\",activeElevation,$AB265,$AJ265,$AV265,$BB265))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T265=\"Select Model\",$T265=\"PCBL\"), \"\",getDischargeAirTemp($T265,$V265,$AD265,$W265,BD265,$AL265, $Y265, $AY265, \"heating\",activeElevation,$AB265,$AJ265,$AV265,$BB265)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T265=\"Select Model\", \"\",IF(OR($T265=\"ACBC_1W\",$T265=\"ACBC_2W\",LEFT($T265,4)=\"ACBR\",$T265 = \"LIU24_2W\",LEFT($T265,3)=\"RIU\",LEFT($T265,6)=\"ACBL12\"), IF((soundLevel($T265, $AB265, BD265, $Y265, $W265,$AJ265,$AA265,\"dba\"))<15,\"<15\",soundLevel($T265, $AB265, BD265, $Y265, $W265,$AJ265,$AA265,\"dba\")+0.4),IF((soundLevel($T265, $AB265, BD265, $Y265, $W265,$AJ265,$AA265,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T265, $AB265, BD265, $Y265, $W265,$AJ265,$AA265,\"dba\")+5)<15, \"<15\", soundLevel($T265, $AB265, BD265,$Y265, $W265,$AJ265,$AA265,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T265=\"Select Model\", \"\",IF(OR($T265=\"ACBC_1W\",$T265=\"ACBC_2W\",LEFT($T265,4)=\"ACBR\",$T265=\"LIU24_2W\",LEFT($T265,3)=\"RIU\",LEFT($T265,6)=\"ACBL12\"), IF((soundLevel($T265, $AB265, BD265, $Y265, $W265,$AJ265,$AA265,\"NC\"))<15,\"<15\",soundLevel($T265, $AB265, BD265, $Y265, $W265,$AJ265,$AA265,\"NC\")+0.4),IF((soundLevel($T265, $AB265, BD265, $Y265, $W265,$AJ265,$AA265,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T265, $AB265, BD265, $Y265, $W265,$AJ265,$AA265,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T265, $AB265, BD265, $Y265, $W265,$AJ265,$AA265,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T265=\"Select Model\",\"\",IF($T265=\"LIU24_2W\",calcQwIP($Y265,$W265,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC265,$AI265,\"latent\",$U265&\"P\"&IF($V265=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T265,activeElevation),\"\"))","v":""},{"$f":"IF($T265=\"Select Model\",\"\",IF($T265=\"ACBC_1W\",calcQwIP($Y265,$W265,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC265,BD265,\"capacity\",$U265&\"P\"&IF($V265=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T265,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y265,$W265,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC265,BD265,\"capacity\",$U265&\"P\"&IF($V265=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T265,activeElevation)))","v":""},"",{"$f":"IF(T265=\"Select Model\", 0,waterPressureDrop(W265, U265 & \"P\" & IF(V265=\"Dual\",2,1) &\"C\", AC265, \"cooling\", T265))","v":0},{"$f":"IF(T265=\"Select Model\", \"\",getReturnWaterTemp(T265,AC265, activeEWTCooling, AS265, \"cooling\"))","v":""},"",{"$f":"IF($T265<>\"ACBC_1W\",\"\",IF($J265=\"\",\"\",FintubeCapacity($T265,$W265,$AE265,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T265=\"Select Model\",T265=\"PCBL\"),\"\",calcQwIP(Y265,W265,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD265,BD265,\"capacity\",U265&\"P\"&IF(V265=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T265,activeElevation))","v":""},"",{"$f":"IF(OR(T265=\"Select Model\",T265=\"PCBL\"), \"\",IF(AY265=0,\"N/A\",waterPressureDrop(W265, U265 & \"P\" & IF(V265=\"Dual\",2,1) &\"C\", AD265, \"heating\", T265)))","v":""},{"$f":"IF(OR(T265=\"Select Model\",T265=\"PCBL\"), \"\",IF(AY265=0,getReturnWaterTemp(T265,AE265, activeEWTHeating, AX265, \"heating\"),getReturnWaterTemp(T265,AD265, activeEWTHeating, AY265, \"heating\")))","v":""},"",{"$f":" getNozzle(T265, W265, Y265, Z265, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I266)),I266<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I266, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H266)),H266<0),\"\",intlEstQuantity(T266, W266*12, H266)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T266=\"Select Model\",\"\",coilCircuitChange(W266, U266, AC266, T266,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T266=\"Select Model\",\"\",beamWidth(T266))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T266=\"Select Model\",T266=\"PCBL\"), 0,getSPIP(T266, W266, Y266, BD266, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T266=\"Select Model\", \"\",IF(T266=\"PCBL\",0,primaryAirSensibleCapacityIP($T266,$W266,activeRoomTempCooling,activePriAirTempCooling,$Y266,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T266=\"Select Model\",\"\",IF($T266=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y266,activeElevation)))","v":""},{"$f":"IF(OR(T266=\"Select Model\",T266=\"PCBL\"), 0,IF(AD266=0,0,-primaryAirSensibleCapacityIP($T266,$W266,activeRoomTempHeating,activePriAirTempHeating,$Y266,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T266=\"Select Model\", \"\", InductionRatio($T266,BD266,$W266,$Y266)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T266=\"Select Model\", \"\",IF($T266=\"PCBL\",\"N/A\",minVAVSetBack(AA266, Y266))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T266=\"Select Model\", \"\",IF($T266= \"PCBL\",\"N/A\",getDischargeAirTemp($T266,$V266,$AC266,$W266,BD266,$AL266, $Y266, $AS266, \"cooling\",activeElevation,$AB266,$AJ266,$AV266,$BB266))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T266=\"Select Model\",$T266=\"PCBL\"), \"\",getDischargeAirTemp($T266,$V266,$AD266,$W266,BD266,$AL266, $Y266, $AY266, \"heating\",activeElevation,$AB266,$AJ266,$AV266,$BB266)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T266=\"Select Model\", \"\",IF(OR($T266=\"ACBC_1W\",$T266=\"ACBC_2W\",LEFT($T266,4)=\"ACBR\",$T266 = \"LIU24_2W\",LEFT($T266,3)=\"RIU\",LEFT($T266,6)=\"ACBL12\"), IF((soundLevel($T266, $AB266, BD266, $Y266, $W266,$AJ266,$AA266,\"dba\"))<15,\"<15\",soundLevel($T266, $AB266, BD266, $Y266, $W266,$AJ266,$AA266,\"dba\")+0.4),IF((soundLevel($T266, $AB266, BD266, $Y266, $W266,$AJ266,$AA266,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T266, $AB266, BD266, $Y266, $W266,$AJ266,$AA266,\"dba\")+5)<15, \"<15\", soundLevel($T266, $AB266, BD266,$Y266, $W266,$AJ266,$AA266,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T266=\"Select Model\", \"\",IF(OR($T266=\"ACBC_1W\",$T266=\"ACBC_2W\",LEFT($T266,4)=\"ACBR\",$T266=\"LIU24_2W\",LEFT($T266,3)=\"RIU\",LEFT($T266,6)=\"ACBL12\"), IF((soundLevel($T266, $AB266, BD266, $Y266, $W266,$AJ266,$AA266,\"NC\"))<15,\"<15\",soundLevel($T266, $AB266, BD266, $Y266, $W266,$AJ266,$AA266,\"NC\")+0.4),IF((soundLevel($T266, $AB266, BD266, $Y266, $W266,$AJ266,$AA266,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T266, $AB266, BD266, $Y266, $W266,$AJ266,$AA266,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T266, $AB266, BD266, $Y266, $W266,$AJ266,$AA266,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T266=\"Select Model\",\"\",IF($T266=\"LIU24_2W\",calcQwIP($Y266,$W266,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC266,$AI266,\"latent\",$U266&\"P\"&IF($V266=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T266,activeElevation),\"\"))","v":""},{"$f":"IF($T266=\"Select Model\",\"\",IF($T266=\"ACBC_1W\",calcQwIP($Y266,$W266,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC266,BD266,\"capacity\",$U266&\"P\"&IF($V266=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T266,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y266,$W266,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC266,BD266,\"capacity\",$U266&\"P\"&IF($V266=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T266,activeElevation)))","v":""},"",{"$f":"IF(T266=\"Select Model\", 0,waterPressureDrop(W266, U266 & \"P\" & IF(V266=\"Dual\",2,1) &\"C\", AC266, \"cooling\", T266))","v":0},{"$f":"IF(T266=\"Select Model\", \"\",getReturnWaterTemp(T266,AC266, activeEWTCooling, AS266, \"cooling\"))","v":""},"",{"$f":"IF($T266<>\"ACBC_1W\",\"\",IF($J266=\"\",\"\",FintubeCapacity($T266,$W266,$AE266,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T266=\"Select Model\",T266=\"PCBL\"),\"\",calcQwIP(Y266,W266,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD266,BD266,\"capacity\",U266&\"P\"&IF(V266=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T266,activeElevation))","v":""},"",{"$f":"IF(OR(T266=\"Select Model\",T266=\"PCBL\"), \"\",IF(AY266=0,\"N/A\",waterPressureDrop(W266, U266 & \"P\" & IF(V266=\"Dual\",2,1) &\"C\", AD266, \"heating\", T266)))","v":""},{"$f":"IF(OR(T266=\"Select Model\",T266=\"PCBL\"), \"\",IF(AY266=0,getReturnWaterTemp(T266,AE266, activeEWTHeating, AX266, \"heating\"),getReturnWaterTemp(T266,AD266, activeEWTHeating, AY266, \"heating\")))","v":""},"",{"$f":" getNozzle(T266, W266, Y266, Z266, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I267)),I267<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I267, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H267)),H267<0),\"\",intlEstQuantity(T267, W267*12, H267)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T267=\"Select Model\",\"\",coilCircuitChange(W267, U267, AC267, T267,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T267=\"Select Model\",\"\",beamWidth(T267))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T267=\"Select Model\",T267=\"PCBL\"), 0,getSPIP(T267, W267, Y267, BD267, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T267=\"Select Model\", \"\",IF(T267=\"PCBL\",0,primaryAirSensibleCapacityIP($T267,$W267,activeRoomTempCooling,activePriAirTempCooling,$Y267,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T267=\"Select Model\",\"\",IF($T267=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y267,activeElevation)))","v":""},{"$f":"IF(OR(T267=\"Select Model\",T267=\"PCBL\"), 0,IF(AD267=0,0,-primaryAirSensibleCapacityIP($T267,$W267,activeRoomTempHeating,activePriAirTempHeating,$Y267,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T267=\"Select Model\", \"\", InductionRatio($T267,BD267,$W267,$Y267)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T267=\"Select Model\", \"\",IF($T267=\"PCBL\",\"N/A\",minVAVSetBack(AA267, Y267))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T267=\"Select Model\", \"\",IF($T267= \"PCBL\",\"N/A\",getDischargeAirTemp($T267,$V267,$AC267,$W267,BD267,$AL267, $Y267, $AS267, \"cooling\",activeElevation,$AB267,$AJ267,$AV267,$BB267))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T267=\"Select Model\",$T267=\"PCBL\"), \"\",getDischargeAirTemp($T267,$V267,$AD267,$W267,BD267,$AL267, $Y267, $AY267, \"heating\",activeElevation,$AB267,$AJ267,$AV267,$BB267)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T267=\"Select Model\", \"\",IF(OR($T267=\"ACBC_1W\",$T267=\"ACBC_2W\",LEFT($T267,4)=\"ACBR\",$T267 = \"LIU24_2W\",LEFT($T267,3)=\"RIU\",LEFT($T267,6)=\"ACBL12\"), IF((soundLevel($T267, $AB267, BD267, $Y267, $W267,$AJ267,$AA267,\"dba\"))<15,\"<15\",soundLevel($T267, $AB267, BD267, $Y267, $W267,$AJ267,$AA267,\"dba\")+0.4),IF((soundLevel($T267, $AB267, BD267, $Y267, $W267,$AJ267,$AA267,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T267, $AB267, BD267, $Y267, $W267,$AJ267,$AA267,\"dba\")+5)<15, \"<15\", soundLevel($T267, $AB267, BD267,$Y267, $W267,$AJ267,$AA267,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T267=\"Select Model\", \"\",IF(OR($T267=\"ACBC_1W\",$T267=\"ACBC_2W\",LEFT($T267,4)=\"ACBR\",$T267=\"LIU24_2W\",LEFT($T267,3)=\"RIU\",LEFT($T267,6)=\"ACBL12\"), IF((soundLevel($T267, $AB267, BD267, $Y267, $W267,$AJ267,$AA267,\"NC\"))<15,\"<15\",soundLevel($T267, $AB267, BD267, $Y267, $W267,$AJ267,$AA267,\"NC\")+0.4),IF((soundLevel($T267, $AB267, BD267, $Y267, $W267,$AJ267,$AA267,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T267, $AB267, BD267, $Y267, $W267,$AJ267,$AA267,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T267, $AB267, BD267, $Y267, $W267,$AJ267,$AA267,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T267=\"Select Model\",\"\",IF($T267=\"LIU24_2W\",calcQwIP($Y267,$W267,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC267,$AI267,\"latent\",$U267&\"P\"&IF($V267=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T267,activeElevation),\"\"))","v":""},{"$f":"IF($T267=\"Select Model\",\"\",IF($T267=\"ACBC_1W\",calcQwIP($Y267,$W267,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC267,BD267,\"capacity\",$U267&\"P\"&IF($V267=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T267,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y267,$W267,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC267,BD267,\"capacity\",$U267&\"P\"&IF($V267=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T267,activeElevation)))","v":""},"",{"$f":"IF(T267=\"Select Model\", 0,waterPressureDrop(W267, U267 & \"P\" & IF(V267=\"Dual\",2,1) &\"C\", AC267, \"cooling\", T267))","v":0},{"$f":"IF(T267=\"Select Model\", \"\",getReturnWaterTemp(T267,AC267, activeEWTCooling, AS267, \"cooling\"))","v":""},"",{"$f":"IF($T267<>\"ACBC_1W\",\"\",IF($J267=\"\",\"\",FintubeCapacity($T267,$W267,$AE267,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T267=\"Select Model\",T267=\"PCBL\"),\"\",calcQwIP(Y267,W267,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD267,BD267,\"capacity\",U267&\"P\"&IF(V267=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T267,activeElevation))","v":""},"",{"$f":"IF(OR(T267=\"Select Model\",T267=\"PCBL\"), \"\",IF(AY267=0,\"N/A\",waterPressureDrop(W267, U267 & \"P\" & IF(V267=\"Dual\",2,1) &\"C\", AD267, \"heating\", T267)))","v":""},{"$f":"IF(OR(T267=\"Select Model\",T267=\"PCBL\"), \"\",IF(AY267=0,getReturnWaterTemp(T267,AE267, activeEWTHeating, AX267, \"heating\"),getReturnWaterTemp(T267,AD267, activeEWTHeating, AY267, \"heating\")))","v":""},"",{"$f":" getNozzle(T267, W267, Y267, Z267, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I268)),I268<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I268, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H268)),H268<0),\"\",intlEstQuantity(T268, W268*12, H268)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T268=\"Select Model\",\"\",coilCircuitChange(W268, U268, AC268, T268,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T268=\"Select Model\",\"\",beamWidth(T268))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T268=\"Select Model\",T268=\"PCBL\"), 0,getSPIP(T268, W268, Y268, BD268, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T268=\"Select Model\", \"\",IF(T268=\"PCBL\",0,primaryAirSensibleCapacityIP($T268,$W268,activeRoomTempCooling,activePriAirTempCooling,$Y268,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T268=\"Select Model\",\"\",IF($T268=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y268,activeElevation)))","v":""},{"$f":"IF(OR(T268=\"Select Model\",T268=\"PCBL\"), 0,IF(AD268=0,0,-primaryAirSensibleCapacityIP($T268,$W268,activeRoomTempHeating,activePriAirTempHeating,$Y268,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T268=\"Select Model\", \"\", InductionRatio($T268,BD268,$W268,$Y268)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T268=\"Select Model\", \"\",IF($T268=\"PCBL\",\"N/A\",minVAVSetBack(AA268, Y268))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T268=\"Select Model\", \"\",IF($T268= \"PCBL\",\"N/A\",getDischargeAirTemp($T268,$V268,$AC268,$W268,BD268,$AL268, $Y268, $AS268, \"cooling\",activeElevation,$AB268,$AJ268,$AV268,$BB268))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T268=\"Select Model\",$T268=\"PCBL\"), \"\",getDischargeAirTemp($T268,$V268,$AD268,$W268,BD268,$AL268, $Y268, $AY268, \"heating\",activeElevation,$AB268,$AJ268,$AV268,$BB268)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T268=\"Select Model\", \"\",IF(OR($T268=\"ACBC_1W\",$T268=\"ACBC_2W\",LEFT($T268,4)=\"ACBR\",$T268 = \"LIU24_2W\",LEFT($T268,3)=\"RIU\",LEFT($T268,6)=\"ACBL12\"), IF((soundLevel($T268, $AB268, BD268, $Y268, $W268,$AJ268,$AA268,\"dba\"))<15,\"<15\",soundLevel($T268, $AB268, BD268, $Y268, $W268,$AJ268,$AA268,\"dba\")+0.4),IF((soundLevel($T268, $AB268, BD268, $Y268, $W268,$AJ268,$AA268,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T268, $AB268, BD268, $Y268, $W268,$AJ268,$AA268,\"dba\")+5)<15, \"<15\", soundLevel($T268, $AB268, BD268,$Y268, $W268,$AJ268,$AA268,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T268=\"Select Model\", \"\",IF(OR($T268=\"ACBC_1W\",$T268=\"ACBC_2W\",LEFT($T268,4)=\"ACBR\",$T268=\"LIU24_2W\",LEFT($T268,3)=\"RIU\",LEFT($T268,6)=\"ACBL12\"), IF((soundLevel($T268, $AB268, BD268, $Y268, $W268,$AJ268,$AA268,\"NC\"))<15,\"<15\",soundLevel($T268, $AB268, BD268, $Y268, $W268,$AJ268,$AA268,\"NC\")+0.4),IF((soundLevel($T268, $AB268, BD268, $Y268, $W268,$AJ268,$AA268,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T268, $AB268, BD268, $Y268, $W268,$AJ268,$AA268,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T268, $AB268, BD268, $Y268, $W268,$AJ268,$AA268,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T268=\"Select Model\",\"\",IF($T268=\"LIU24_2W\",calcQwIP($Y268,$W268,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC268,$AI268,\"latent\",$U268&\"P\"&IF($V268=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T268,activeElevation),\"\"))","v":""},{"$f":"IF($T268=\"Select Model\",\"\",IF($T268=\"ACBC_1W\",calcQwIP($Y268,$W268,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC268,BD268,\"capacity\",$U268&\"P\"&IF($V268=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T268,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y268,$W268,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC268,BD268,\"capacity\",$U268&\"P\"&IF($V268=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T268,activeElevation)))","v":""},"",{"$f":"IF(T268=\"Select Model\", 0,waterPressureDrop(W268, U268 & \"P\" & IF(V268=\"Dual\",2,1) &\"C\", AC268, \"cooling\", T268))","v":0},{"$f":"IF(T268=\"Select Model\", \"\",getReturnWaterTemp(T268,AC268, activeEWTCooling, AS268, \"cooling\"))","v":""},"",{"$f":"IF($T268<>\"ACBC_1W\",\"\",IF($J268=\"\",\"\",FintubeCapacity($T268,$W268,$AE268,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T268=\"Select Model\",T268=\"PCBL\"),\"\",calcQwIP(Y268,W268,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD268,BD268,\"capacity\",U268&\"P\"&IF(V268=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T268,activeElevation))","v":""},"",{"$f":"IF(OR(T268=\"Select Model\",T268=\"PCBL\"), \"\",IF(AY268=0,\"N/A\",waterPressureDrop(W268, U268 & \"P\" & IF(V268=\"Dual\",2,1) &\"C\", AD268, \"heating\", T268)))","v":""},{"$f":"IF(OR(T268=\"Select Model\",T268=\"PCBL\"), \"\",IF(AY268=0,getReturnWaterTemp(T268,AE268, activeEWTHeating, AX268, \"heating\"),getReturnWaterTemp(T268,AD268, activeEWTHeating, AY268, \"heating\")))","v":""},"",{"$f":" getNozzle(T268, W268, Y268, Z268, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I269)),I269<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I269, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H269)),H269<0),\"\",intlEstQuantity(T269, W269*12, H269)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T269=\"Select Model\",\"\",coilCircuitChange(W269, U269, AC269, T269,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T269=\"Select Model\",\"\",beamWidth(T269))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T269=\"Select Model\",T269=\"PCBL\"), 0,getSPIP(T269, W269, Y269, BD269, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T269=\"Select Model\", \"\",IF(T269=\"PCBL\",0,primaryAirSensibleCapacityIP($T269,$W269,activeRoomTempCooling,activePriAirTempCooling,$Y269,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T269=\"Select Model\",\"\",IF($T269=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y269,activeElevation)))","v":""},{"$f":"IF(OR(T269=\"Select Model\",T269=\"PCBL\"), 0,IF(AD269=0,0,-primaryAirSensibleCapacityIP($T269,$W269,activeRoomTempHeating,activePriAirTempHeating,$Y269,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T269=\"Select Model\", \"\", InductionRatio($T269,BD269,$W269,$Y269)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T269=\"Select Model\", \"\",IF($T269=\"PCBL\",\"N/A\",minVAVSetBack(AA269, Y269))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T269=\"Select Model\", \"\",IF($T269= \"PCBL\",\"N/A\",getDischargeAirTemp($T269,$V269,$AC269,$W269,BD269,$AL269, $Y269, $AS269, \"cooling\",activeElevation,$AB269,$AJ269,$AV269,$BB269))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T269=\"Select Model\",$T269=\"PCBL\"), \"\",getDischargeAirTemp($T269,$V269,$AD269,$W269,BD269,$AL269, $Y269, $AY269, \"heating\",activeElevation,$AB269,$AJ269,$AV269,$BB269)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T269=\"Select Model\", \"\",IF(OR($T269=\"ACBC_1W\",$T269=\"ACBC_2W\",LEFT($T269,4)=\"ACBR\",$T269 = \"LIU24_2W\",LEFT($T269,3)=\"RIU\",LEFT($T269,6)=\"ACBL12\"), IF((soundLevel($T269, $AB269, BD269, $Y269, $W269,$AJ269,$AA269,\"dba\"))<15,\"<15\",soundLevel($T269, $AB269, BD269, $Y269, $W269,$AJ269,$AA269,\"dba\")+0.4),IF((soundLevel($T269, $AB269, BD269, $Y269, $W269,$AJ269,$AA269,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T269, $AB269, BD269, $Y269, $W269,$AJ269,$AA269,\"dba\")+5)<15, \"<15\", soundLevel($T269, $AB269, BD269,$Y269, $W269,$AJ269,$AA269,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T269=\"Select Model\", \"\",IF(OR($T269=\"ACBC_1W\",$T269=\"ACBC_2W\",LEFT($T269,4)=\"ACBR\",$T269=\"LIU24_2W\",LEFT($T269,3)=\"RIU\",LEFT($T269,6)=\"ACBL12\"), IF((soundLevel($T269, $AB269, BD269, $Y269, $W269,$AJ269,$AA269,\"NC\"))<15,\"<15\",soundLevel($T269, $AB269, BD269, $Y269, $W269,$AJ269,$AA269,\"NC\")+0.4),IF((soundLevel($T269, $AB269, BD269, $Y269, $W269,$AJ269,$AA269,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T269, $AB269, BD269, $Y269, $W269,$AJ269,$AA269,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T269, $AB269, BD269, $Y269, $W269,$AJ269,$AA269,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T269=\"Select Model\",\"\",IF($T269=\"LIU24_2W\",calcQwIP($Y269,$W269,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC269,$AI269,\"latent\",$U269&\"P\"&IF($V269=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T269,activeElevation),\"\"))","v":""},{"$f":"IF($T269=\"Select Model\",\"\",IF($T269=\"ACBC_1W\",calcQwIP($Y269,$W269,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC269,BD269,\"capacity\",$U269&\"P\"&IF($V269=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T269,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y269,$W269,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC269,BD269,\"capacity\",$U269&\"P\"&IF($V269=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T269,activeElevation)))","v":""},"",{"$f":"IF(T269=\"Select Model\", 0,waterPressureDrop(W269, U269 & \"P\" & IF(V269=\"Dual\",2,1) &\"C\", AC269, \"cooling\", T269))","v":0},{"$f":"IF(T269=\"Select Model\", \"\",getReturnWaterTemp(T269,AC269, activeEWTCooling, AS269, \"cooling\"))","v":""},"",{"$f":"IF($T269<>\"ACBC_1W\",\"\",IF($J269=\"\",\"\",FintubeCapacity($T269,$W269,$AE269,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T269=\"Select Model\",T269=\"PCBL\"),\"\",calcQwIP(Y269,W269,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD269,BD269,\"capacity\",U269&\"P\"&IF(V269=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T269,activeElevation))","v":""},"",{"$f":"IF(OR(T269=\"Select Model\",T269=\"PCBL\"), \"\",IF(AY269=0,\"N/A\",waterPressureDrop(W269, U269 & \"P\" & IF(V269=\"Dual\",2,1) &\"C\", AD269, \"heating\", T269)))","v":""},{"$f":"IF(OR(T269=\"Select Model\",T269=\"PCBL\"), \"\",IF(AY269=0,getReturnWaterTemp(T269,AE269, activeEWTHeating, AX269, \"heating\"),getReturnWaterTemp(T269,AD269, activeEWTHeating, AY269, \"heating\")))","v":""},"",{"$f":" getNozzle(T269, W269, Y269, Z269, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I270)),I270<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I270, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H270)),H270<0),\"\",intlEstQuantity(T270, W270*12, H270)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T270=\"Select Model\",\"\",coilCircuitChange(W270, U270, AC270, T270,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T270=\"Select Model\",\"\",beamWidth(T270))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T270=\"Select Model\",T270=\"PCBL\"), 0,getSPIP(T270, W270, Y270, BD270, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T270=\"Select Model\", \"\",IF(T270=\"PCBL\",0,primaryAirSensibleCapacityIP($T270,$W270,activeRoomTempCooling,activePriAirTempCooling,$Y270,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T270=\"Select Model\",\"\",IF($T270=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y270,activeElevation)))","v":""},{"$f":"IF(OR(T270=\"Select Model\",T270=\"PCBL\"), 0,IF(AD270=0,0,-primaryAirSensibleCapacityIP($T270,$W270,activeRoomTempHeating,activePriAirTempHeating,$Y270,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T270=\"Select Model\", \"\", InductionRatio($T270,BD270,$W270,$Y270)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T270=\"Select Model\", \"\",IF($T270=\"PCBL\",\"N/A\",minVAVSetBack(AA270, Y270))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T270=\"Select Model\", \"\",IF($T270= \"PCBL\",\"N/A\",getDischargeAirTemp($T270,$V270,$AC270,$W270,BD270,$AL270, $Y270, $AS270, \"cooling\",activeElevation,$AB270,$AJ270,$AV270,$BB270))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T270=\"Select Model\",$T270=\"PCBL\"), \"\",getDischargeAirTemp($T270,$V270,$AD270,$W270,BD270,$AL270, $Y270, $AY270, \"heating\",activeElevation,$AB270,$AJ270,$AV270,$BB270)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T270=\"Select Model\", \"\",IF(OR($T270=\"ACBC_1W\",$T270=\"ACBC_2W\",LEFT($T270,4)=\"ACBR\",$T270 = \"LIU24_2W\",LEFT($T270,3)=\"RIU\",LEFT($T270,6)=\"ACBL12\"), IF((soundLevel($T270, $AB270, BD270, $Y270, $W270,$AJ270,$AA270,\"dba\"))<15,\"<15\",soundLevel($T270, $AB270, BD270, $Y270, $W270,$AJ270,$AA270,\"dba\")+0.4),IF((soundLevel($T270, $AB270, BD270, $Y270, $W270,$AJ270,$AA270,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T270, $AB270, BD270, $Y270, $W270,$AJ270,$AA270,\"dba\")+5)<15, \"<15\", soundLevel($T270, $AB270, BD270,$Y270, $W270,$AJ270,$AA270,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T270=\"Select Model\", \"\",IF(OR($T270=\"ACBC_1W\",$T270=\"ACBC_2W\",LEFT($T270,4)=\"ACBR\",$T270=\"LIU24_2W\",LEFT($T270,3)=\"RIU\",LEFT($T270,6)=\"ACBL12\"), IF((soundLevel($T270, $AB270, BD270, $Y270, $W270,$AJ270,$AA270,\"NC\"))<15,\"<15\",soundLevel($T270, $AB270, BD270, $Y270, $W270,$AJ270,$AA270,\"NC\")+0.4),IF((soundLevel($T270, $AB270, BD270, $Y270, $W270,$AJ270,$AA270,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T270, $AB270, BD270, $Y270, $W270,$AJ270,$AA270,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T270, $AB270, BD270, $Y270, $W270,$AJ270,$AA270,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T270=\"Select Model\",\"\",IF($T270=\"LIU24_2W\",calcQwIP($Y270,$W270,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC270,$AI270,\"latent\",$U270&\"P\"&IF($V270=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T270,activeElevation),\"\"))","v":""},{"$f":"IF($T270=\"Select Model\",\"\",IF($T270=\"ACBC_1W\",calcQwIP($Y270,$W270,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC270,BD270,\"capacity\",$U270&\"P\"&IF($V270=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T270,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y270,$W270,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC270,BD270,\"capacity\",$U270&\"P\"&IF($V270=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T270,activeElevation)))","v":""},"",{"$f":"IF(T270=\"Select Model\", 0,waterPressureDrop(W270, U270 & \"P\" & IF(V270=\"Dual\",2,1) &\"C\", AC270, \"cooling\", T270))","v":0},{"$f":"IF(T270=\"Select Model\", \"\",getReturnWaterTemp(T270,AC270, activeEWTCooling, AS270, \"cooling\"))","v":""},"",{"$f":"IF($T270<>\"ACBC_1W\",\"\",IF($J270=\"\",\"\",FintubeCapacity($T270,$W270,$AE270,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T270=\"Select Model\",T270=\"PCBL\"),\"\",calcQwIP(Y270,W270,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD270,BD270,\"capacity\",U270&\"P\"&IF(V270=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T270,activeElevation))","v":""},"",{"$f":"IF(OR(T270=\"Select Model\",T270=\"PCBL\"), \"\",IF(AY270=0,\"N/A\",waterPressureDrop(W270, U270 & \"P\" & IF(V270=\"Dual\",2,1) &\"C\", AD270, \"heating\", T270)))","v":""},{"$f":"IF(OR(T270=\"Select Model\",T270=\"PCBL\"), \"\",IF(AY270=0,getReturnWaterTemp(T270,AE270, activeEWTHeating, AX270, \"heating\"),getReturnWaterTemp(T270,AD270, activeEWTHeating, AY270, \"heating\")))","v":""},"",{"$f":" getNozzle(T270, W270, Y270, Z270, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I271)),I271<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I271, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H271)),H271<0),\"\",intlEstQuantity(T271, W271*12, H271)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T271=\"Select Model\",\"\",coilCircuitChange(W271, U271, AC271, T271,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T271=\"Select Model\",\"\",beamWidth(T271))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T271=\"Select Model\",T271=\"PCBL\"), 0,getSPIP(T271, W271, Y271, BD271, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T271=\"Select Model\", \"\",IF(T271=\"PCBL\",0,primaryAirSensibleCapacityIP($T271,$W271,activeRoomTempCooling,activePriAirTempCooling,$Y271,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T271=\"Select Model\",\"\",IF($T271=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y271,activeElevation)))","v":""},{"$f":"IF(OR(T271=\"Select Model\",T271=\"PCBL\"), 0,IF(AD271=0,0,-primaryAirSensibleCapacityIP($T271,$W271,activeRoomTempHeating,activePriAirTempHeating,$Y271,activeElevation,\"heating\")))","v":0},{"$f":"getCurrentNozzleCode(T271, W271, Y271, Z271, activeElevation, TRUE)","v":""},{"$f":"IFERROR(IF(T271=\"Select Model\", \"\", InductionRatio($T271,BD271,$W271,$Y271)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T271=\"Select Model\", \"\",IF($T271=\"PCBL\",\"N/A\",minVAVSetBack(AA271, Y271))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T271=\"Select Model\", \"\",IF($T271= \"PCBL\",\"N/A\",getDischargeAirTemp($T271,$V271,$AC271,$W271,BD271,$AL271, $Y271, $AS271, \"cooling\",activeElevation,$AB271,$AJ271,$AV271,$BB271))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T271=\"Select Model\",$T271=\"PCBL\"), \"\",getDischargeAirTemp($T271,$V271,$AD271,$W271,BD271,$AL271, $Y271, $AY271, \"heating\",activeElevation,$AB271,$AJ271,$AV271,$BB271)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T271=\"Select Model\", \"\",IF(OR($T271=\"ACBC_1W\",$T271=\"ACBC_2W\",LEFT($T271,4)=\"ACBR\",$T271 = \"LIU24_2W\",LEFT($T271,3)=\"RIU\",LEFT($T271,6)=\"ACBL12\"), IF((soundLevel($T271, $AB271, BD271, $Y271, $W271,$AJ271,$AA271,\"dba\"))<15,\"<15\",soundLevel($T271, $AB271, BD271, $Y271, $W271,$AJ271,$AA271,\"dba\")+0.4),IF((soundLevel($T271, $AB271, BD271, $Y271, $W271,$AJ271,$AA271,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T271, $AB271, BD271, $Y271, $W271,$AJ271,$AA271,\"dba\")+5)<15, \"<15\", soundLevel($T271, $AB271, BD271,$Y271, $W271,$AJ271,$AA271,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T271=\"Select Model\", \"\",IF(OR($T271=\"ACBC_1W\",$T271=\"ACBC_2W\",LEFT($T271,4)=\"ACBR\",$T271=\"LIU24_2W\",LEFT($T271,3)=\"RIU\",LEFT($T271,6)=\"ACBL12\"), IF((soundLevel($T271, $AB271, BD271, $Y271, $W271,$AJ271,$AA271,\"NC\"))<15,\"<15\",soundLevel($T271, $AB271, BD271, $Y271, $W271,$AJ271,$AA271,\"NC\")+0.4),IF((soundLevel($T271, $AB271, BD271, $Y271, $W271,$AJ271,$AA271,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T271, $AB271, BD271, $Y271, $W271,$AJ271,$AA271,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T271, $AB271, BD271, $Y271, $W271,$AJ271,$AA271,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T271=\"Select Model\",\"\",IF($T271=\"LIU24_2W\",calcQwIP($Y271,$W271,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC271,$AI271,\"latent\",$U271&\"P\"&IF($V271=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T271,activeElevation),\"\"))","v":""},{"$f":"IF($T271=\"Select Model\",\"\",IF($T271=\"ACBC_1W\",calcQwIP($Y271,$W271,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC271,BD271,\"capacity\",$U271&\"P\"&IF($V271=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T271,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y271,$W271,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC271,BD271,\"capacity\",$U271&\"P\"&IF($V271=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T271,activeElevation)))","v":""},"",{"$f":"IF(T271=\"Select Model\", 0,waterPressureDrop(W271, U271 & \"P\" & IF(V271=\"Dual\",2,1) &\"C\", AC271, \"cooling\", T271))","v":0},{"$f":"IF(T271=\"Select Model\", \"\",getReturnWaterTemp(T271,AC271, activeEWTCooling, AS271, \"cooling\"))","v":""},"",{"$f":"IF($T271<>\"ACBC_1W\",\"\",IF($J271=\"\",\"\",FintubeCapacity($T271,$W271,$AE271,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T271=\"Select Model\",T271=\"PCBL\"),\"\",calcQwIP(Y271,W271,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD271,BD271,\"capacity\",U271&\"P\"&IF(V271=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T271,activeElevation))","v":""},"",{"$f":"IF(OR(T271=\"Select Model\",T271=\"PCBL\"), \"\",IF(AY271=0,\"N/A\",waterPressureDrop(W271, U271 & \"P\" & IF(V271=\"Dual\",2,1) &\"C\", AD271, \"heating\", T271)))","v":""},{"$f":"IF(OR(T271=\"Select Model\",T271=\"PCBL\"), \"\",IF(AY271=0,getReturnWaterTemp(T271,AE271, activeEWTHeating, AX271, \"heating\"),getReturnWaterTemp(T271,AD271, activeEWTHeating, AY271, \"heating\")))","v":""},"",{"$f":" getNozzle(T271, W271, Y271, Z271, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I272)),I272<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I272, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H272)),H272<0),\"\",intlEstQuantity(T272, W272*12, H272)),1)","v":""},{"$f":"IF(LEFT(T272, 4)=\"ACBC\",IF(AND(ISNUMBER(L272),ISNUMBER(AT272)),IF(AA272=-1,\"LOW CFM\",L272*AT272),\"\"),IF(AND(ISNUMBER(L272),ISNUMBER(AT272)),IF(AA272=-1,\"N/A CFM\",L272*AT272),\"\"))","v":""},{"$f":"IF(LEFT(T272,4)=\"ACBC\",IF(AND(ISNUMBER(L272),ISNUMBER(AG272)),IF(AA272=-1,\"LOW CFM\",L272*AG272),\"\"),IF(AND(ISNUMBER(L272),ISNUMBER(AG272)),IF(AA272=-1,\"N/A CFM\",L272*AG272),\"\"))","v":""},{"$f":"IF(LEFT(T272,4)=\"ACBC\",IF(AND(ISNUMBER(L272),ISNUMBER(AZ272)),IF(AA272=-1,\"LOW CFM\",L272*AZ272),\"\"),IF(AND(ISNUMBER(L272),ISNUMBER(AZ272)),IF(AA272=-1,\"N/A CFM\",L272*AZ272),\"\"))","v":""},{"$f":"IF(AND(ISNUMBER(L272),ISNUMBER(Y272)),L272*Y272,\"\")","v":""},{"$f":"IF(AND(ISNUMBER(L272),ISNUMBER(AC272)),L272*AC272,\"\")","v":""},{"$f":"IF(AND(ISNUMBER(L272),ISNUMBER(AD272)),IF(AND(T272=\"ACBC_1W\",AD272=0),AE272*L272,L272*AD272))","v":false},"Default","Select Model",2,{"$f":"IF(T272=\"Select Model\",\"\",coilCircuitChange(W272, U272, AC272, T272,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T272=\"Select Model\",\"\",beamWidth(T272))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T272=\"Select Model\",T272=\"PCBL\"), 0,getSPIP(T272, W272, Y272, BD272, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T272=\"Select Model\", \"\",IF(T272=\"PCBL\",0,primaryAirSensibleCapacityIP($T272,$W272,activeRoomTempCooling,activePriAirTempCooling,$Y272,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T272=\"Select Model\",\"\",IF($T272=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y272,activeElevation)))","v":""},{"$f":"IF(OR(T272=\"Select Model\",T272=\"PCBL\"), 0,IF(AD272=0,0,-primaryAirSensibleCapacityIP($T272,$W272,activeRoomTempHeating,activePriAirTempHeating,$Y272,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T272=\"Select Model\", \"\", InductionRatio($T272,BD272,$W272,$Y272)),\"N/A\")","v":""},{"$f":"IFERROR(AT272/Y272,\"\")","v":""},{"$f":"IFERROR(IF(T272=\"Select Model\", \"\",(1+AJ272)*Y272),\"N/A\")","v":""},{"$f":"IFERROR(IF(T272=\"Select Model\", \"\",IF($T272=\"PCBL\",\"N/A\",minVAVSetBack(AA272, Y272))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T272=\"Select Model\", \"\",IF($T272= \"PCBL\",\"N/A\",getDischargeAirTemp($T272,$V272,$AC272,$W272,BD272,$AL272, $Y272, $AS272, \"cooling\",activeElevation,$AB272,$AJ272,$AV272,$BB272))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T272=\"Select Model\",$T272=\"PCBL\"), \"\",getDischargeAirTemp($T272,$V272,$AD272,$W272,BD272,$AL272, $Y272, $AY272, \"heating\",activeElevation,$AB272,$AJ272,$AV272,$BB272)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T272=\"Select Model\", \"\",IF(OR($T272=\"ACBC_1W\",$T272=\"ACBC_2W\",LEFT($T272,4)=\"ACBR\",$T272 = \"LIU24_2W\",LEFT($T272,3)=\"RIU\",LEFT($T272,6)=\"ACBL12\"), IF((soundLevel($T272, $AB272, BD272, $Y272, $W272,$AJ272,$AA272,\"dba\"))<15,\"<15\",soundLevel($T272, $AB272, BD272, $Y272, $W272,$AJ272,$AA272,\"dba\")+0.4),IF((soundLevel($T272, $AB272, BD272, $Y272, $W272,$AJ272,$AA272,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T272, $AB272, BD272, $Y272, $W272,$AJ272,$AA272,\"dba\")+5)<15, \"<15\", soundLevel($T272, $AB272, BD272,$Y272, $W272,$AJ272,$AA272,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T272=\"Select Model\", \"\",IF(OR($T272=\"ACBC_1W\",$T272=\"ACBC_2W\",LEFT($T272,4)=\"ACBR\",$T272=\"LIU24_2W\",LEFT($T272,3)=\"RIU\",LEFT($T272,6)=\"ACBL12\"), IF((soundLevel($T272, $AB272, BD272, $Y272, $W272,$AJ272,$AA272,\"NC\"))<15,\"<15\",soundLevel($T272, $AB272, BD272, $Y272, $W272,$AJ272,$AA272,\"NC\")+0.4),IF((soundLevel($T272, $AB272, BD272, $Y272, $W272,$AJ272,$AA272,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T272, $AB272, BD272, $Y272, $W272,$AJ272,$AA272,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T272, $AB272, BD272, $Y272, $W272,$AJ272,$AA272,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T272=\"Select Model\",\"\",IF($T272=\"LIU24_2W\",calcQwIP($Y272,$W272,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC272,$AI272,\"latent\",$U272&\"P\"&IF($V272=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T272,activeElevation),\"\"))","v":""},{"$f":"IF($T272=\"Select Model\",\"\",IF($T272=\"ACBC_1W\",calcQwIP($Y272,$W272,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC272,BD272,\"capacity\",$U272&\"P\"&IF($V272=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T272,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y272,$W272,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC272,BD272,\"capacity\",$U272&\"P\"&IF($V272=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T272,activeElevation)))","v":""},{"$f":"IF(T272=\"Select Model\", \"\",IF(T272 = \"LIU24_2W\", AS272+AF272+AR272, AS272+AF272))","v":""},{"$f":"IF(T272=\"Select Model\", 0,waterPressureDrop(W272, U272 & \"P\" & IF(V272=\"Dual\",2,1) &\"C\", AC272, \"cooling\", T272))","v":0},{"$f":"IF(T272=\"Select Model\", \"\",getReturnWaterTemp(T272,AC272, activeEWTCooling, AS272, \"cooling\"))","v":""},{"$f":"IF(T272=\"Select Model\", \"\",$AV272-activeEWTCooling)","v":""},{"$f":"IF($T272<>\"ACBC_1W\",\"\",IF($J272=\"\",\"\",FintubeCapacity($T272,$W272,$AE272,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T272=\"Select Model\",T272=\"PCBL\"),\"\",calcQwIP(Y272,W272,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD272,BD272,\"capacity\",U272&\"P\"&IF(V272=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T272,activeElevation))","v":""},{"$f":"IF(OR(T272=\"Select Model\",T272=\"PCBL\"),\"\",IF(AND(AD272=0,T272=\"ACBC_1W\"),AX272+AH272,AY272+AH272))","v":""},{"$f":"IF(OR(T272=\"Select Model\",T272=\"PCBL\"), \"\",IF(AY272=0,\"N/A\",waterPressureDrop(W272, U272 & \"P\" & IF(V272=\"Dual\",2,1) &\"C\", AD272, \"heating\", T272)))","v":""},{"$f":"IF(OR(T272=\"Select Model\",T272=\"PCBL\"), \"\",IF(AY272=0,getReturnWaterTemp(T272,AE272, activeEWTHeating, AX272, \"heating\"),getReturnWaterTemp(T272,AD272, activeEWTHeating, AY272, \"heating\")))","v":""},{"$f":"IF(OR($T272=\"Select Model\",$J272=\"\",T272=\"PCBL\"), \"\",activeEWTHeating-$BB272)","v":""},{"$f":" getNozzle(T272, W272, Y272, Z272, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I273)),I273<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I273, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H273)),H273<0),\"\",intlEstQuantity(T273, W273*12, H273)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T273=\"Select Model\",\"\",coilCircuitChange(W273, U273, AC273, T273,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T273=\"Select Model\",\"\",beamWidth(T273))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T273=\"Select Model\",T273=\"PCBL\"), 0,getSPIP(T273, W273, Y273, BD273, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T273=\"Select Model\", \"\",IF(T273=\"PCBL\",0,primaryAirSensibleCapacityIP($T273,$W273,activeRoomTempCooling,activePriAirTempCooling,$Y273,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T273=\"Select Model\",\"\",IF($T273=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y273,activeElevation)))","v":""},{"$f":"IF(OR(T273=\"Select Model\",T273=\"PCBL\"), 0,IF(AD273=0,0,-primaryAirSensibleCapacityIP($T273,$W273,activeRoomTempHeating,activePriAirTempHeating,$Y273,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T273=\"Select Model\", \"\", InductionRatio($T273,BD273,$W273,$Y273)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T273=\"Select Model\", \"\",IF($T273=\"PCBL\",\"N/A\",minVAVSetBack(AA273, Y273))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T273=\"Select Model\", \"\",IF($T273= \"PCBL\",\"N/A\",getDischargeAirTemp($T273,$V273,$AC273,$W273,BD273,$AL273, $Y273, $AS273, \"cooling\",activeElevation,$AB273,$AJ273,$AV273,$BB273))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T273=\"Select Model\",$T273=\"PCBL\"), \"\",getDischargeAirTemp($T273,$V273,$AD273,$W273,BD273,$AL273, $Y273, $AY273, \"heating\",activeElevation,$AB273,$AJ273,$AV273,$BB273)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T273=\"Select Model\", \"\",IF(OR($T273=\"ACBC_1W\",$T273=\"ACBC_2W\",LEFT($T273,4)=\"ACBR\",$T273 = \"LIU24_2W\",LEFT($T273,3)=\"RIU\",LEFT($T273,6)=\"ACBL12\"), IF((soundLevel($T273, $AB273, BD273, $Y273, $W273,$AJ273,$AA273,\"dba\"))<15,\"<15\",soundLevel($T273, $AB273, BD273, $Y273, $W273,$AJ273,$AA273,\"dba\")+0.4),IF((soundLevel($T273, $AB273, BD273, $Y273, $W273,$AJ273,$AA273,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T273, $AB273, BD273, $Y273, $W273,$AJ273,$AA273,\"dba\")+5)<15, \"<15\", soundLevel($T273, $AB273, BD273,$Y273, $W273,$AJ273,$AA273,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T273=\"Select Model\", \"\",IF(OR($T273=\"ACBC_1W\",$T273=\"ACBC_2W\",LEFT($T273,4)=\"ACBR\",$T273=\"LIU24_2W\",LEFT($T273,3)=\"RIU\",LEFT($T273,6)=\"ACBL12\"), IF((soundLevel($T273, $AB273, BD273, $Y273, $W273,$AJ273,$AA273,\"NC\"))<15,\"<15\",soundLevel($T273, $AB273, BD273, $Y273, $W273,$AJ273,$AA273,\"NC\")+0.4),IF((soundLevel($T273, $AB273, BD273, $Y273, $W273,$AJ273,$AA273,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T273, $AB273, BD273, $Y273, $W273,$AJ273,$AA273,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T273, $AB273, BD273, $Y273, $W273,$AJ273,$AA273,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T273=\"Select Model\",\"\",IF($T273=\"LIU24_2W\",calcQwIP($Y273,$W273,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC273,$AI273,\"latent\",$U273&\"P\"&IF($V273=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T273,activeElevation),\"\"))","v":""},{"$f":"IF($T273=\"Select Model\",\"\",IF($T273=\"ACBC_1W\",calcQwIP($Y273,$W273,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC273,BD273,\"capacity\",$U273&\"P\"&IF($V273=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T273,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y273,$W273,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC273,BD273,\"capacity\",$U273&\"P\"&IF($V273=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T273,activeElevation)))","v":""},"",{"$f":"IF(T273=\"Select Model\", 0,waterPressureDrop(W273, U273 & \"P\" & IF(V273=\"Dual\",2,1) &\"C\", AC273, \"cooling\", T273))","v":0},{"$f":"IF(T273=\"Select Model\", \"\",getReturnWaterTemp(T273,AC273, activeEWTCooling, AS273, \"cooling\"))","v":""},"",{"$f":"IF($T273<>\"ACBC_1W\",\"\",IF($J273=\"\",\"\",FintubeCapacity($T273,$W273,$AE273,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T273=\"Select Model\",T273=\"PCBL\"),\"\",calcQwIP(Y273,W273,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD273,BD273,\"capacity\",U273&\"P\"&IF(V273=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T273,activeElevation))","v":""},"",{"$f":"IF(OR(T273=\"Select Model\",T273=\"PCBL\"), \"\",IF(AY273=0,\"N/A\",waterPressureDrop(W273, U273 & \"P\" & IF(V273=\"Dual\",2,1) &\"C\", AD273, \"heating\", T273)))","v":""},{"$f":"IF(OR(T273=\"Select Model\",T273=\"PCBL\"), \"\",IF(AY273=0,getReturnWaterTemp(T273,AE273, activeEWTHeating, AX273, \"heating\"),getReturnWaterTemp(T273,AD273, activeEWTHeating, AY273, \"heating\")))","v":""},"",{"$f":" getNozzle(T273, W273, Y273, Z273, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I274)),I274<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I274, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H274)),H274<0),\"\",intlEstQuantity(T274, W274*12, H274)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T274=\"Select Model\",\"\",coilCircuitChange(W274, U274, AC274, T274,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T274=\"Select Model\",\"\",beamWidth(T274))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T274=\"Select Model\",T274=\"PCBL\"), 0,getSPIP(T274, W274, Y274, BD274, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T274=\"Select Model\", \"\",IF(T274=\"PCBL\",0,primaryAirSensibleCapacityIP($T274,$W274,activeRoomTempCooling,activePriAirTempCooling,$Y274,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T274=\"Select Model\",\"\",IF($T274=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y274,activeElevation)))","v":""},{"$f":"IF(OR(T274=\"Select Model\",T274=\"PCBL\"), 0,IF(AD274=0,0,-primaryAirSensibleCapacityIP($T274,$W274,activeRoomTempHeating,activePriAirTempHeating,$Y274,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T274=\"Select Model\", \"\", InductionRatio($T274,BD274,$W274,$Y274)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T274=\"Select Model\", \"\",IF($T274=\"PCBL\",\"N/A\",minVAVSetBack(AA274, Y274))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T274=\"Select Model\", \"\",IF($T274= \"PCBL\",\"N/A\",getDischargeAirTemp($T274,$V274,$AC274,$W274,BD274,$AL274, $Y274, $AS274, \"cooling\",activeElevation,$AB274,$AJ274,$AV274,$BB274))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T274=\"Select Model\",$T274=\"PCBL\"), \"\",getDischargeAirTemp($T274,$V274,$AD274,$W274,BD274,$AL274, $Y274, $AY274, \"heating\",activeElevation,$AB274,$AJ274,$AV274,$BB274)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T274=\"Select Model\", \"\",IF(OR($T274=\"ACBC_1W\",$T274=\"ACBC_2W\",LEFT($T274,4)=\"ACBR\",$T274 = \"LIU24_2W\",LEFT($T274,3)=\"RIU\",LEFT($T274,6)=\"ACBL12\"), IF((soundLevel($T274, $AB274, BD274, $Y274, $W274,$AJ274,$AA274,\"dba\"))<15,\"<15\",soundLevel($T274, $AB274, BD274, $Y274, $W274,$AJ274,$AA274,\"dba\")+0.4),IF((soundLevel($T274, $AB274, BD274, $Y274, $W274,$AJ274,$AA274,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T274, $AB274, BD274, $Y274, $W274,$AJ274,$AA274,\"dba\")+5)<15, \"<15\", soundLevel($T274, $AB274, BD274,$Y274, $W274,$AJ274,$AA274,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T274=\"Select Model\", \"\",IF(OR($T274=\"ACBC_1W\",$T274=\"ACBC_2W\",LEFT($T274,4)=\"ACBR\",$T274=\"LIU24_2W\",LEFT($T274,3)=\"RIU\",LEFT($T274,6)=\"ACBL12\"), IF((soundLevel($T274, $AB274, BD274, $Y274, $W274,$AJ274,$AA274,\"NC\"))<15,\"<15\",soundLevel($T274, $AB274, BD274, $Y274, $W274,$AJ274,$AA274,\"NC\")+0.4),IF((soundLevel($T274, $AB274, BD274, $Y274, $W274,$AJ274,$AA274,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T274, $AB274, BD274, $Y274, $W274,$AJ274,$AA274,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T274, $AB274, BD274, $Y274, $W274,$AJ274,$AA274,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T274=\"Select Model\",\"\",IF($T274=\"LIU24_2W\",calcQwIP($Y274,$W274,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC274,$AI274,\"latent\",$U274&\"P\"&IF($V274=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T274,activeElevation),\"\"))","v":""},{"$f":"IF($T274=\"Select Model\",\"\",IF($T274=\"ACBC_1W\",calcQwIP($Y274,$W274,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC274,BD274,\"capacity\",$U274&\"P\"&IF($V274=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T274,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y274,$W274,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC274,BD274,\"capacity\",$U274&\"P\"&IF($V274=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T274,activeElevation)))","v":""},"",{"$f":"IF(T274=\"Select Model\", 0,waterPressureDrop(W274, U274 & \"P\" & IF(V274=\"Dual\",2,1) &\"C\", AC274, \"cooling\", T274))","v":0},{"$f":"IF(T274=\"Select Model\", \"\",getReturnWaterTemp(T274,AC274, activeEWTCooling, AS274, \"cooling\"))","v":""},"",{"$f":"IF($T274<>\"ACBC_1W\",\"\",IF($J274=\"\",\"\",FintubeCapacity($T274,$W274,$AE274,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T274=\"Select Model\",T274=\"PCBL\"),\"\",calcQwIP(Y274,W274,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD274,BD274,\"capacity\",U274&\"P\"&IF(V274=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T274,activeElevation))","v":""},"",{"$f":"IF(OR(T274=\"Select Model\",T274=\"PCBL\"), \"\",IF(AY274=0,\"N/A\",waterPressureDrop(W274, U274 & \"P\" & IF(V274=\"Dual\",2,1) &\"C\", AD274, \"heating\", T274)))","v":""},{"$f":"IF(OR(T274=\"Select Model\",T274=\"PCBL\"), \"\",IF(AY274=0,getReturnWaterTemp(T274,AE274, activeEWTHeating, AX274, \"heating\"),getReturnWaterTemp(T274,AD274, activeEWTHeating, AY274, \"heating\")))","v":""},"",{"$f":" getNozzle(T274, W274, Y274, Z274, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I275)),I275<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I275, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H275)),H275<0),\"\",intlEstQuantity(T275, W275*12, H275)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T275=\"Select Model\",\"\",coilCircuitChange(W275, U275, AC275, T275,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T275=\"Select Model\",\"\",beamWidth(T275))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T275=\"Select Model\",T275=\"PCBL\"), 0,getSPIP(T275, W275, Y275, BD275, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T275=\"Select Model\", \"\",IF(T275=\"PCBL\",0,primaryAirSensibleCapacityIP($T275,$W275,activeRoomTempCooling,activePriAirTempCooling,$Y275,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T275=\"Select Model\",\"\",IF($T275=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y275,activeElevation)))","v":""},{"$f":"IF(OR(T275=\"Select Model\",T275=\"PCBL\"), 0,IF(AD275=0,0,-primaryAirSensibleCapacityIP($T275,$W275,activeRoomTempHeating,activePriAirTempHeating,$Y275,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T275=\"Select Model\", \"\", InductionRatio($T275,BD275,$W275,$Y275)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T275=\"Select Model\", \"\",IF($T275=\"PCBL\",\"N/A\",minVAVSetBack(AA275, Y275))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T275=\"Select Model\", \"\",IF($T275= \"PCBL\",\"N/A\",getDischargeAirTemp($T275,$V275,$AC275,$W275,BD275,$AL275, $Y275, $AS275, \"cooling\",activeElevation,$AB275,$AJ275,$AV275,$BB275))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T275=\"Select Model\",$T275=\"PCBL\"), \"\",getDischargeAirTemp($T275,$V275,$AD275,$W275,BD275,$AL275, $Y275, $AY275, \"heating\",activeElevation,$AB275,$AJ275,$AV275,$BB275)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T275=\"Select Model\", \"\",IF(OR($T275=\"ACBC_1W\",$T275=\"ACBC_2W\",LEFT($T275,4)=\"ACBR\",$T275 = \"LIU24_2W\",LEFT($T275,3)=\"RIU\",LEFT($T275,6)=\"ACBL12\"), IF((soundLevel($T275, $AB275, BD275, $Y275, $W275,$AJ275,$AA275,\"dba\"))<15,\"<15\",soundLevel($T275, $AB275, BD275, $Y275, $W275,$AJ275,$AA275,\"dba\")+0.4),IF((soundLevel($T275, $AB275, BD275, $Y275, $W275,$AJ275,$AA275,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T275, $AB275, BD275, $Y275, $W275,$AJ275,$AA275,\"dba\")+5)<15, \"<15\", soundLevel($T275, $AB275, BD275,$Y275, $W275,$AJ275,$AA275,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T275=\"Select Model\", \"\",IF(OR($T275=\"ACBC_1W\",$T275=\"ACBC_2W\",LEFT($T275,4)=\"ACBR\",$T275=\"LIU24_2W\",LEFT($T275,3)=\"RIU\",LEFT($T275,6)=\"ACBL12\"), IF((soundLevel($T275, $AB275, BD275, $Y275, $W275,$AJ275,$AA275,\"NC\"))<15,\"<15\",soundLevel($T275, $AB275, BD275, $Y275, $W275,$AJ275,$AA275,\"NC\")+0.4),IF((soundLevel($T275, $AB275, BD275, $Y275, $W275,$AJ275,$AA275,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T275, $AB275, BD275, $Y275, $W275,$AJ275,$AA275,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T275, $AB275, BD275, $Y275, $W275,$AJ275,$AA275,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T275=\"Select Model\",\"\",IF($T275=\"LIU24_2W\",calcQwIP($Y275,$W275,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC275,$AI275,\"latent\",$U275&\"P\"&IF($V275=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T275,activeElevation),\"\"))","v":""},{"$f":"IF($T275=\"Select Model\",\"\",IF($T275=\"ACBC_1W\",calcQwIP($Y275,$W275,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC275,BD275,\"capacity\",$U275&\"P\"&IF($V275=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T275,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y275,$W275,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC275,BD275,\"capacity\",$U275&\"P\"&IF($V275=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T275,activeElevation)))","v":""},"",{"$f":"IF(T275=\"Select Model\", 0,waterPressureDrop(W275, U275 & \"P\" & IF(V275=\"Dual\",2,1) &\"C\", AC275, \"cooling\", T275))","v":0},{"$f":"IF(T275=\"Select Model\", \"\",getReturnWaterTemp(T275,AC275, activeEWTCooling, AS275, \"cooling\"))","v":""},"",{"$f":"IF($T275<>\"ACBC_1W\",\"\",IF($J275=\"\",\"\",FintubeCapacity($T275,$W275,$AE275,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T275=\"Select Model\",T275=\"PCBL\"),\"\",calcQwIP(Y275,W275,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD275,BD275,\"capacity\",U275&\"P\"&IF(V275=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T275,activeElevation))","v":""},"",{"$f":"IF(OR(T275=\"Select Model\",T275=\"PCBL\"), \"\",IF(AY275=0,\"N/A\",waterPressureDrop(W275, U275 & \"P\" & IF(V275=\"Dual\",2,1) &\"C\", AD275, \"heating\", T275)))","v":""},{"$f":"IF(OR(T275=\"Select Model\",T275=\"PCBL\"), \"\",IF(AY275=0,getReturnWaterTemp(T275,AE275, activeEWTHeating, AX275, \"heating\"),getReturnWaterTemp(T275,AD275, activeEWTHeating, AY275, \"heating\")))","v":""},"",{"$f":" getNozzle(T275, W275, Y275, Z275, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I276)),I276<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I276, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H276)),H276<0),\"\",intlEstQuantity(T276, W276*12, H276)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T276=\"Select Model\",\"\",coilCircuitChange(W276, U276, AC276, T276,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T276=\"Select Model\",\"\",beamWidth(T276))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T276=\"Select Model\",T276=\"PCBL\"), 0,getSPIP(T276, W276, Y276, BD276, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T276=\"Select Model\", \"\",IF(T276=\"PCBL\",0,primaryAirSensibleCapacityIP($T276,$W276,activeRoomTempCooling,activePriAirTempCooling,$Y276,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T276=\"Select Model\",\"\",IF($T276=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y276,activeElevation)))","v":""},{"$f":"IF(OR(T276=\"Select Model\",T276=\"PCBL\"), 0,IF(AD276=0,0,-primaryAirSensibleCapacityIP($T276,$W276,activeRoomTempHeating,activePriAirTempHeating,$Y276,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T276=\"Select Model\", \"\", InductionRatio($T276,BD276,$W276,$Y276)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T276=\"Select Model\", \"\",IF($T276=\"PCBL\",\"N/A\",minVAVSetBack(AA276, Y276))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T276=\"Select Model\", \"\",IF($T276= \"PCBL\",\"N/A\",getDischargeAirTemp($T276,$V276,$AC276,$W276,BD276,$AL276, $Y276, $AS276, \"cooling\",activeElevation,$AB276,$AJ276,$AV276,$BB276))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T276=\"Select Model\",$T276=\"PCBL\"), \"\",getDischargeAirTemp($T276,$V276,$AD276,$W276,BD276,$AL276, $Y276, $AY276, \"heating\",activeElevation,$AB276,$AJ276,$AV276,$BB276)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T276=\"Select Model\", \"\",IF(OR($T276=\"ACBC_1W\",$T276=\"ACBC_2W\",LEFT($T276,4)=\"ACBR\",$T276 = \"LIU24_2W\",LEFT($T276,3)=\"RIU\",LEFT($T276,6)=\"ACBL12\"), IF((soundLevel($T276, $AB276, BD276, $Y276, $W276,$AJ276,$AA276,\"dba\"))<15,\"<15\",soundLevel($T276, $AB276, BD276, $Y276, $W276,$AJ276,$AA276,\"dba\")+0.4),IF((soundLevel($T276, $AB276, BD276, $Y276, $W276,$AJ276,$AA276,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T276, $AB276, BD276, $Y276, $W276,$AJ276,$AA276,\"dba\")+5)<15, \"<15\", soundLevel($T276, $AB276, BD276,$Y276, $W276,$AJ276,$AA276,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T276=\"Select Model\", \"\",IF(OR($T276=\"ACBC_1W\",$T276=\"ACBC_2W\",LEFT($T276,4)=\"ACBR\",$T276=\"LIU24_2W\",LEFT($T276,3)=\"RIU\",LEFT($T276,6)=\"ACBL12\"), IF((soundLevel($T276, $AB276, BD276, $Y276, $W276,$AJ276,$AA276,\"NC\"))<15,\"<15\",soundLevel($T276, $AB276, BD276, $Y276, $W276,$AJ276,$AA276,\"NC\")+0.4),IF((soundLevel($T276, $AB276, BD276, $Y276, $W276,$AJ276,$AA276,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T276, $AB276, BD276, $Y276, $W276,$AJ276,$AA276,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T276, $AB276, BD276, $Y276, $W276,$AJ276,$AA276,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T276=\"Select Model\",\"\",IF($T276=\"LIU24_2W\",calcQwIP($Y276,$W276,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC276,$AI276,\"latent\",$U276&\"P\"&IF($V276=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T276,activeElevation),\"\"))","v":""},{"$f":"IF($T276=\"Select Model\",\"\",IF($T276=\"ACBC_1W\",calcQwIP($Y276,$W276,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC276,BD276,\"capacity\",$U276&\"P\"&IF($V276=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T276,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y276,$W276,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC276,BD276,\"capacity\",$U276&\"P\"&IF($V276=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T276,activeElevation)))","v":""},"",{"$f":"IF(T276=\"Select Model\", 0,waterPressureDrop(W276, U276 & \"P\" & IF(V276=\"Dual\",2,1) &\"C\", AC276, \"cooling\", T276))","v":0},{"$f":"IF(T276=\"Select Model\", \"\",getReturnWaterTemp(T276,AC276, activeEWTCooling, AS276, \"cooling\"))","v":""},"",{"$f":"IF($T276<>\"ACBC_1W\",\"\",IF($J276=\"\",\"\",FintubeCapacity($T276,$W276,$AE276,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T276=\"Select Model\",T276=\"PCBL\"),\"\",calcQwIP(Y276,W276,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD276,BD276,\"capacity\",U276&\"P\"&IF(V276=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T276,activeElevation))","v":""},"",{"$f":"IF(OR(T276=\"Select Model\",T276=\"PCBL\"), \"\",IF(AY276=0,\"N/A\",waterPressureDrop(W276, U276 & \"P\" & IF(V276=\"Dual\",2,1) &\"C\", AD276, \"heating\", T276)))","v":""},{"$f":"IF(OR(T276=\"Select Model\",T276=\"PCBL\"), \"\",IF(AY276=0,getReturnWaterTemp(T276,AE276, activeEWTHeating, AX276, \"heating\"),getReturnWaterTemp(T276,AD276, activeEWTHeating, AY276, \"heating\")))","v":""},"",{"$f":" getNozzle(T276, W276, Y276, Z276, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I277)),I277<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I277, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H277)),H277<0),\"\",intlEstQuantity(T277, W277*12, H277)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T277=\"Select Model\",\"\",coilCircuitChange(W277, U277, AC277, T277,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T277=\"Select Model\",\"\",beamWidth(T277))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T277=\"Select Model\",T277=\"PCBL\"), 0,getSPIP(T277, W277, Y277, BD277, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T277=\"Select Model\", \"\",IF(T277=\"PCBL\",0,primaryAirSensibleCapacityIP($T277,$W277,activeRoomTempCooling,activePriAirTempCooling,$Y277,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T277=\"Select Model\",\"\",IF($T277=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y277,activeElevation)))","v":""},{"$f":"IF(OR(T277=\"Select Model\",T277=\"PCBL\"), 0,IF(AD277=0,0,-primaryAirSensibleCapacityIP($T277,$W277,activeRoomTempHeating,activePriAirTempHeating,$Y277,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T277=\"Select Model\", \"\", InductionRatio($T277,BD277,$W277,$Y277)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T277=\"Select Model\", \"\",IF($T277=\"PCBL\",\"N/A\",minVAVSetBack(AA277, Y277))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T277=\"Select Model\", \"\",IF($T277= \"PCBL\",\"N/A\",getDischargeAirTemp($T277,$V277,$AC277,$W277,BD277,$AL277, $Y277, $AS277, \"cooling\",activeElevation,$AB277,$AJ277,$AV277,$BB277))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T277=\"Select Model\",$T277=\"PCBL\"), \"\",getDischargeAirTemp($T277,$V277,$AD277,$W277,BD277,$AL277, $Y277, $AY277, \"heating\",activeElevation,$AB277,$AJ277,$AV277,$BB277)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T277=\"Select Model\", \"\",IF(OR($T277=\"ACBC_1W\",$T277=\"ACBC_2W\",LEFT($T277,4)=\"ACBR\",$T277 = \"LIU24_2W\",LEFT($T277,3)=\"RIU\",LEFT($T277,6)=\"ACBL12\"), IF((soundLevel($T277, $AB277, BD277, $Y277, $W277,$AJ277,$AA277,\"dba\"))<15,\"<15\",soundLevel($T277, $AB277, BD277, $Y277, $W277,$AJ277,$AA277,\"dba\")+0.4),IF((soundLevel($T277, $AB277, BD277, $Y277, $W277,$AJ277,$AA277,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T277, $AB277, BD277, $Y277, $W277,$AJ277,$AA277,\"dba\")+5)<15, \"<15\", soundLevel($T277, $AB277, BD277,$Y277, $W277,$AJ277,$AA277,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T277=\"Select Model\", \"\",IF(OR($T277=\"ACBC_1W\",$T277=\"ACBC_2W\",LEFT($T277,4)=\"ACBR\",$T277=\"LIU24_2W\",LEFT($T277,3)=\"RIU\",LEFT($T277,6)=\"ACBL12\"), IF((soundLevel($T277, $AB277, BD277, $Y277, $W277,$AJ277,$AA277,\"NC\"))<15,\"<15\",soundLevel($T277, $AB277, BD277, $Y277, $W277,$AJ277,$AA277,\"NC\")+0.4),IF((soundLevel($T277, $AB277, BD277, $Y277, $W277,$AJ277,$AA277,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T277, $AB277, BD277, $Y277, $W277,$AJ277,$AA277,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T277, $AB277, BD277, $Y277, $W277,$AJ277,$AA277,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T277=\"Select Model\",\"\",IF($T277=\"LIU24_2W\",calcQwIP($Y277,$W277,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC277,$AI277,\"latent\",$U277&\"P\"&IF($V277=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T277,activeElevation),\"\"))","v":""},{"$f":"IF($T277=\"Select Model\",\"\",IF($T277=\"ACBC_1W\",calcQwIP($Y277,$W277,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC277,BD277,\"capacity\",$U277&\"P\"&IF($V277=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T277,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y277,$W277,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC277,BD277,\"capacity\",$U277&\"P\"&IF($V277=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T277,activeElevation)))","v":""},"",{"$f":"IF(T277=\"Select Model\", 0,waterPressureDrop(W277, U277 & \"P\" & IF(V277=\"Dual\",2,1) &\"C\", AC277, \"cooling\", T277))","v":0},{"$f":"IF(T277=\"Select Model\", \"\",getReturnWaterTemp(T277,AC277, activeEWTCooling, AS277, \"cooling\"))","v":""},"",{"$f":"IF($T277<>\"ACBC_1W\",\"\",IF($J277=\"\",\"\",FintubeCapacity($T277,$W277,$AE277,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T277=\"Select Model\",T277=\"PCBL\"),\"\",calcQwIP(Y277,W277,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD277,BD277,\"capacity\",U277&\"P\"&IF(V277=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T277,activeElevation))","v":""},"",{"$f":"IF(OR(T277=\"Select Model\",T277=\"PCBL\"), \"\",IF(AY277=0,\"N/A\",waterPressureDrop(W277, U277 & \"P\" & IF(V277=\"Dual\",2,1) &\"C\", AD277, \"heating\", T277)))","v":""},{"$f":"IF(OR(T277=\"Select Model\",T277=\"PCBL\"), \"\",IF(AY277=0,getReturnWaterTemp(T277,AE277, activeEWTHeating, AX277, \"heating\"),getReturnWaterTemp(T277,AD277, activeEWTHeating, AY277, \"heating\")))","v":""},"",{"$f":" getNozzle(T277, W277, Y277, Z277, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I278)),I278<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I278, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H278)),H278<0),\"\",intlEstQuantity(T278, W278*12, H278)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T278=\"Select Model\",\"\",coilCircuitChange(W278, U278, AC278, T278,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T278=\"Select Model\",\"\",beamWidth(T278))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T278=\"Select Model\",T278=\"PCBL\"), 0,getSPIP(T278, W278, Y278, BD278, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T278=\"Select Model\", \"\",IF(T278=\"PCBL\",0,primaryAirSensibleCapacityIP($T278,$W278,activeRoomTempCooling,activePriAirTempCooling,$Y278,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T278=\"Select Model\",\"\",IF($T278=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y278,activeElevation)))","v":""},{"$f":"IF(OR(T278=\"Select Model\",T278=\"PCBL\"), 0,IF(AD278=0,0,-primaryAirSensibleCapacityIP($T278,$W278,activeRoomTempHeating,activePriAirTempHeating,$Y278,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T278=\"Select Model\", \"\", InductionRatio($T278,BD278,$W278,$Y278)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T278=\"Select Model\", \"\",IF($T278=\"PCBL\",\"N/A\",minVAVSetBack(AA278, Y278))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T278=\"Select Model\", \"\",IF($T278= \"PCBL\",\"N/A\",getDischargeAirTemp($T278,$V278,$AC278,$W278,BD278,$AL278, $Y278, $AS278, \"cooling\",activeElevation,$AB278,$AJ278,$AV278,$BB278))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T278=\"Select Model\",$T278=\"PCBL\"), \"\",getDischargeAirTemp($T278,$V278,$AD278,$W278,BD278,$AL278, $Y278, $AY278, \"heating\",activeElevation,$AB278,$AJ278,$AV278,$BB278)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T278=\"Select Model\", \"\",IF(OR($T278=\"ACBC_1W\",$T278=\"ACBC_2W\",LEFT($T278,4)=\"ACBR\",$T278 = \"LIU24_2W\",LEFT($T278,3)=\"RIU\",LEFT($T278,6)=\"ACBL12\"), IF((soundLevel($T278, $AB278, BD278, $Y278, $W278,$AJ278,$AA278,\"dba\"))<15,\"<15\",soundLevel($T278, $AB278, BD278, $Y278, $W278,$AJ278,$AA278,\"dba\")+0.4),IF((soundLevel($T278, $AB278, BD278, $Y278, $W278,$AJ278,$AA278,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T278, $AB278, BD278, $Y278, $W278,$AJ278,$AA278,\"dba\")+5)<15, \"<15\", soundLevel($T278, $AB278, BD278,$Y278, $W278,$AJ278,$AA278,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T278=\"Select Model\", \"\",IF(OR($T278=\"ACBC_1W\",$T278=\"ACBC_2W\",LEFT($T278,4)=\"ACBR\",$T278=\"LIU24_2W\",LEFT($T278,3)=\"RIU\",LEFT($T278,6)=\"ACBL12\"), IF((soundLevel($T278, $AB278, BD278, $Y278, $W278,$AJ278,$AA278,\"NC\"))<15,\"<15\",soundLevel($T278, $AB278, BD278, $Y278, $W278,$AJ278,$AA278,\"NC\")+0.4),IF((soundLevel($T278, $AB278, BD278, $Y278, $W278,$AJ278,$AA278,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T278, $AB278, BD278, $Y278, $W278,$AJ278,$AA278,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T278, $AB278, BD278, $Y278, $W278,$AJ278,$AA278,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T278=\"Select Model\",\"\",IF($T278=\"LIU24_2W\",calcQwIP($Y278,$W278,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC278,$AI278,\"latent\",$U278&\"P\"&IF($V278=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T278,activeElevation),\"\"))","v":""},{"$f":"IF($T278=\"Select Model\",\"\",IF($T278=\"ACBC_1W\",calcQwIP($Y278,$W278,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC278,BD278,\"capacity\",$U278&\"P\"&IF($V278=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T278,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y278,$W278,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC278,BD278,\"capacity\",$U278&\"P\"&IF($V278=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T278,activeElevation)))","v":""},"",{"$f":"IF(T278=\"Select Model\", 0,waterPressureDrop(W278, U278 & \"P\" & IF(V278=\"Dual\",2,1) &\"C\", AC278, \"cooling\", T278))","v":0},{"$f":"IF(T278=\"Select Model\", \"\",getReturnWaterTemp(T278,AC278, activeEWTCooling, AS278, \"cooling\"))","v":""},"",{"$f":"IF($T278<>\"ACBC_1W\",\"\",IF($J278=\"\",\"\",FintubeCapacity($T278,$W278,$AE278,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T278=\"Select Model\",T278=\"PCBL\"),\"\",calcQwIP(Y278,W278,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD278,BD278,\"capacity\",U278&\"P\"&IF(V278=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T278,activeElevation))","v":""},"",{"$f":"IF(OR(T278=\"Select Model\",T278=\"PCBL\"), \"\",IF(AY278=0,\"N/A\",waterPressureDrop(W278, U278 & \"P\" & IF(V278=\"Dual\",2,1) &\"C\", AD278, \"heating\", T278)))","v":""},{"$f":"IF(OR(T278=\"Select Model\",T278=\"PCBL\"), \"\",IF(AY278=0,getReturnWaterTemp(T278,AE278, activeEWTHeating, AX278, \"heating\"),getReturnWaterTemp(T278,AD278, activeEWTHeating, AY278, \"heating\")))","v":""},"",{"$f":" getNozzle(T278, W278, Y278, Z278, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I279)),I279<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I279, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H279)),H279<0),\"\",intlEstQuantity(T279, W279*12, H279)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T279=\"Select Model\",\"\",coilCircuitChange(W279, U279, AC279, T279,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T279=\"Select Model\",\"\",beamWidth(T279))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T279=\"Select Model\",T279=\"PCBL\"), 0,getSPIP(T279, W279, Y279, BD279, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T279=\"Select Model\", \"\",IF(T279=\"PCBL\",0,primaryAirSensibleCapacityIP($T279,$W279,activeRoomTempCooling,activePriAirTempCooling,$Y279,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T279=\"Select Model\",\"\",IF($T279=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y279,activeElevation)))","v":""},{"$f":"IF(OR(T279=\"Select Model\",T279=\"PCBL\"), 0,IF(AD279=0,0,-primaryAirSensibleCapacityIP($T279,$W279,activeRoomTempHeating,activePriAirTempHeating,$Y279,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T279=\"Select Model\", \"\", InductionRatio($T279,BD279,$W279,$Y279)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T279=\"Select Model\", \"\",IF($T279=\"PCBL\",\"N/A\",minVAVSetBack(AA279, Y279))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T279=\"Select Model\", \"\",IF($T279= \"PCBL\",\"N/A\",getDischargeAirTemp($T279,$V279,$AC279,$W279,BD279,$AL279, $Y279, $AS279, \"cooling\",activeElevation,$AB279,$AJ279,$AV279,$BB279))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T279=\"Select Model\",$T279=\"PCBL\"), \"\",getDischargeAirTemp($T279,$V279,$AD279,$W279,BD279,$AL279, $Y279, $AY279, \"heating\",activeElevation,$AB279,$AJ279,$AV279,$BB279)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T279=\"Select Model\", \"\",IF(OR($T279=\"ACBC_1W\",$T279=\"ACBC_2W\",LEFT($T279,4)=\"ACBR\",$T279 = \"LIU24_2W\",LEFT($T279,3)=\"RIU\",LEFT($T279,6)=\"ACBL12\"), IF((soundLevel($T279, $AB279, BD279, $Y279, $W279,$AJ279,$AA279,\"dba\"))<15,\"<15\",soundLevel($T279, $AB279, BD279, $Y279, $W279,$AJ279,$AA279,\"dba\")+0.4),IF((soundLevel($T279, $AB279, BD279, $Y279, $W279,$AJ279,$AA279,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T279, $AB279, BD279, $Y279, $W279,$AJ279,$AA279,\"dba\")+5)<15, \"<15\", soundLevel($T279, $AB279, BD279,$Y279, $W279,$AJ279,$AA279,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T279=\"Select Model\", \"\",IF(OR($T279=\"ACBC_1W\",$T279=\"ACBC_2W\",LEFT($T279,4)=\"ACBR\",$T279=\"LIU24_2W\",LEFT($T279,3)=\"RIU\",LEFT($T279,6)=\"ACBL12\"), IF((soundLevel($T279, $AB279, BD279, $Y279, $W279,$AJ279,$AA279,\"NC\"))<15,\"<15\",soundLevel($T279, $AB279, BD279, $Y279, $W279,$AJ279,$AA279,\"NC\")+0.4),IF((soundLevel($T279, $AB279, BD279, $Y279, $W279,$AJ279,$AA279,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T279, $AB279, BD279, $Y279, $W279,$AJ279,$AA279,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T279, $AB279, BD279, $Y279, $W279,$AJ279,$AA279,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T279=\"Select Model\",\"\",IF($T279=\"LIU24_2W\",calcQwIP($Y279,$W279,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC279,$AI279,\"latent\",$U279&\"P\"&IF($V279=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T279,activeElevation),\"\"))","v":""},{"$f":"IF($T279=\"Select Model\",\"\",IF($T279=\"ACBC_1W\",calcQwIP($Y279,$W279,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC279,BD279,\"capacity\",$U279&\"P\"&IF($V279=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T279,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y279,$W279,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC279,BD279,\"capacity\",$U279&\"P\"&IF($V279=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T279,activeElevation)))","v":""},"",{"$f":"IF(T279=\"Select Model\", 0,waterPressureDrop(W279, U279 & \"P\" & IF(V279=\"Dual\",2,1) &\"C\", AC279, \"cooling\", T279))","v":0},{"$f":"IF(T279=\"Select Model\", \"\",getReturnWaterTemp(T279,AC279, activeEWTCooling, AS279, \"cooling\"))","v":""},"",{"$f":"IF($T279<>\"ACBC_1W\",\"\",IF($J279=\"\",\"\",FintubeCapacity($T279,$W279,$AE279,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T279=\"Select Model\",T279=\"PCBL\"),\"\",calcQwIP(Y279,W279,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD279,BD279,\"capacity\",U279&\"P\"&IF(V279=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T279,activeElevation))","v":""},"",{"$f":"IF(OR(T279=\"Select Model\",T279=\"PCBL\"), \"\",IF(AY279=0,\"N/A\",waterPressureDrop(W279, U279 & \"P\" & IF(V279=\"Dual\",2,1) &\"C\", AD279, \"heating\", T279)))","v":""},{"$f":"IF(OR(T279=\"Select Model\",T279=\"PCBL\"), \"\",IF(AY279=0,getReturnWaterTemp(T279,AE279, activeEWTHeating, AX279, \"heating\"),getReturnWaterTemp(T279,AD279, activeEWTHeating, AY279, \"heating\")))","v":""},"",{"$f":" getNozzle(T279, W279, Y279, Z279, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I280)),I280<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I280, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H280)),H280<0),\"\",intlEstQuantity(T280, W280*12, H280)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T280=\"Select Model\",\"\",coilCircuitChange(W280, U280, AC280, T280,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T280=\"Select Model\",\"\",beamWidth(T280))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T280=\"Select Model\",T280=\"PCBL\"), 0,getSPIP(T280, W280, Y280, BD280, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T280=\"Select Model\", \"\",IF(T280=\"PCBL\",0,primaryAirSensibleCapacityIP($T280,$W280,activeRoomTempCooling,activePriAirTempCooling,$Y280,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T280=\"Select Model\",\"\",IF($T280=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y280,activeElevation)))","v":""},{"$f":"IF(OR(T280=\"Select Model\",T280=\"PCBL\"), 0,IF(AD280=0,0,-primaryAirSensibleCapacityIP($T280,$W280,activeRoomTempHeating,activePriAirTempHeating,$Y280,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T280=\"Select Model\", \"\", InductionRatio($T280,BD280,$W280,$Y280)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T280=\"Select Model\", \"\",IF($T280=\"PCBL\",\"N/A\",minVAVSetBack(AA280, Y280))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T280=\"Select Model\", \"\",IF($T280= \"PCBL\",\"N/A\",getDischargeAirTemp($T280,$V280,$AC280,$W280,BD280,$AL280, $Y280, $AS280, \"cooling\",activeElevation,$AB280,$AJ280,$AV280,$BB280))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T280=\"Select Model\",$T280=\"PCBL\"), \"\",getDischargeAirTemp($T280,$V280,$AD280,$W280,BD280,$AL280, $Y280, $AY280, \"heating\",activeElevation,$AB280,$AJ280,$AV280,$BB280)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T280=\"Select Model\", \"\",IF(OR($T280=\"ACBC_1W\",$T280=\"ACBC_2W\",LEFT($T280,4)=\"ACBR\",$T280 = \"LIU24_2W\",LEFT($T280,3)=\"RIU\",LEFT($T280,6)=\"ACBL12\"), IF((soundLevel($T280, $AB280, BD280, $Y280, $W280,$AJ280,$AA280,\"dba\"))<15,\"<15\",soundLevel($T280, $AB280, BD280, $Y280, $W280,$AJ280,$AA280,\"dba\")+0.4),IF((soundLevel($T280, $AB280, BD280, $Y280, $W280,$AJ280,$AA280,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T280, $AB280, BD280, $Y280, $W280,$AJ280,$AA280,\"dba\")+5)<15, \"<15\", soundLevel($T280, $AB280, BD280,$Y280, $W280,$AJ280,$AA280,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T280=\"Select Model\", \"\",IF(OR($T280=\"ACBC_1W\",$T280=\"ACBC_2W\",LEFT($T280,4)=\"ACBR\",$T280=\"LIU24_2W\",LEFT($T280,3)=\"RIU\",LEFT($T280,6)=\"ACBL12\"), IF((soundLevel($T280, $AB280, BD280, $Y280, $W280,$AJ280,$AA280,\"NC\"))<15,\"<15\",soundLevel($T280, $AB280, BD280, $Y280, $W280,$AJ280,$AA280,\"NC\")+0.4),IF((soundLevel($T280, $AB280, BD280, $Y280, $W280,$AJ280,$AA280,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T280, $AB280, BD280, $Y280, $W280,$AJ280,$AA280,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T280, $AB280, BD280, $Y280, $W280,$AJ280,$AA280,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T280=\"Select Model\",\"\",IF($T280=\"LIU24_2W\",calcQwIP($Y280,$W280,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC280,$AI280,\"latent\",$U280&\"P\"&IF($V280=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T280,activeElevation),\"\"))","v":""},{"$f":"IF($T280=\"Select Model\",\"\",IF($T280=\"ACBC_1W\",calcQwIP($Y280,$W280,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC280,BD280,\"capacity\",$U280&\"P\"&IF($V280=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T280,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y280,$W280,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC280,BD280,\"capacity\",$U280&\"P\"&IF($V280=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T280,activeElevation)))","v":""},"",{"$f":"IF(T280=\"Select Model\", 0,waterPressureDrop(W280, U280 & \"P\" & IF(V280=\"Dual\",2,1) &\"C\", AC280, \"cooling\", T280))","v":0},{"$f":"IF(T280=\"Select Model\", \"\",getReturnWaterTemp(T280,AC280, activeEWTCooling, AS280, \"cooling\"))","v":""},"",{"$f":"IF($T280<>\"ACBC_1W\",\"\",IF($J280=\"\",\"\",FintubeCapacity($T280,$W280,$AE280,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T280=\"Select Model\",T280=\"PCBL\"),\"\",calcQwIP(Y280,W280,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD280,BD280,\"capacity\",U280&\"P\"&IF(V280=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T280,activeElevation))","v":""},"",{"$f":"IF(OR(T280=\"Select Model\",T280=\"PCBL\"), \"\",IF(AY280=0,\"N/A\",waterPressureDrop(W280, U280 & \"P\" & IF(V280=\"Dual\",2,1) &\"C\", AD280, \"heating\", T280)))","v":""},{"$f":"IF(OR(T280=\"Select Model\",T280=\"PCBL\"), \"\",IF(AY280=0,getReturnWaterTemp(T280,AE280, activeEWTHeating, AX280, \"heating\"),getReturnWaterTemp(T280,AD280, activeEWTHeating, AY280, \"heating\")))","v":""},"",{"$f":" getNozzle(T280, W280, Y280, Z280, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I281)),I281<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I281, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H281)),H281<0),\"\",intlEstQuantity(T281, W281*12, H281)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T281=\"Select Model\",\"\",coilCircuitChange(W281, U281, AC281, T281,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T281=\"Select Model\",\"\",beamWidth(T281))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T281=\"Select Model\",T281=\"PCBL\"), 0,getSPIP(T281, W281, Y281, BD281, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T281=\"Select Model\", \"\",IF(T281=\"PCBL\",0,primaryAirSensibleCapacityIP($T281,$W281,activeRoomTempCooling,activePriAirTempCooling,$Y281,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T281=\"Select Model\",\"\",IF($T281=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y281,activeElevation)))","v":""},{"$f":"IF(OR(T281=\"Select Model\",T281=\"PCBL\"), 0,IF(AD281=0,0,-primaryAirSensibleCapacityIP($T281,$W281,activeRoomTempHeating,activePriAirTempHeating,$Y281,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T281=\"Select Model\", \"\", InductionRatio($T281,BD281,$W281,$Y281)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T281=\"Select Model\", \"\",IF($T281=\"PCBL\",\"N/A\",minVAVSetBack(AA281, Y281))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T281=\"Select Model\", \"\",IF($T281= \"PCBL\",\"N/A\",getDischargeAirTemp($T281,$V281,$AC281,$W281,BD281,$AL281, $Y281, $AS281, \"cooling\",activeElevation,$AB281,$AJ281,$AV281,$BB281))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T281=\"Select Model\",$T281=\"PCBL\"), \"\",getDischargeAirTemp($T281,$V281,$AD281,$W281,BD281,$AL281, $Y281, $AY281, \"heating\",activeElevation,$AB281,$AJ281,$AV281,$BB281)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T281=\"Select Model\", \"\",IF(OR($T281=\"ACBC_1W\",$T281=\"ACBC_2W\",LEFT($T281,4)=\"ACBR\",$T281 = \"LIU24_2W\",LEFT($T281,3)=\"RIU\",LEFT($T281,6)=\"ACBL12\"), IF((soundLevel($T281, $AB281, BD281, $Y281, $W281,$AJ281,$AA281,\"dba\"))<15,\"<15\",soundLevel($T281, $AB281, BD281, $Y281, $W281,$AJ281,$AA281,\"dba\")+0.4),IF((soundLevel($T281, $AB281, BD281, $Y281, $W281,$AJ281,$AA281,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T281, $AB281, BD281, $Y281, $W281,$AJ281,$AA281,\"dba\")+5)<15, \"<15\", soundLevel($T281, $AB281, BD281,$Y281, $W281,$AJ281,$AA281,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T281=\"Select Model\", \"\",IF(OR($T281=\"ACBC_1W\",$T281=\"ACBC_2W\",LEFT($T281,4)=\"ACBR\",$T281=\"LIU24_2W\",LEFT($T281,3)=\"RIU\",LEFT($T281,6)=\"ACBL12\"), IF((soundLevel($T281, $AB281, BD281, $Y281, $W281,$AJ281,$AA281,\"NC\"))<15,\"<15\",soundLevel($T281, $AB281, BD281, $Y281, $W281,$AJ281,$AA281,\"NC\")+0.4),IF((soundLevel($T281, $AB281, BD281, $Y281, $W281,$AJ281,$AA281,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T281, $AB281, BD281, $Y281, $W281,$AJ281,$AA281,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T281, $AB281, BD281, $Y281, $W281,$AJ281,$AA281,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T281=\"Select Model\",\"\",IF($T281=\"LIU24_2W\",calcQwIP($Y281,$W281,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC281,$AI281,\"latent\",$U281&\"P\"&IF($V281=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T281,activeElevation),\"\"))","v":""},{"$f":"IF($T281=\"Select Model\",\"\",IF($T281=\"ACBC_1W\",calcQwIP($Y281,$W281,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC281,BD281,\"capacity\",$U281&\"P\"&IF($V281=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T281,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y281,$W281,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC281,BD281,\"capacity\",$U281&\"P\"&IF($V281=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T281,activeElevation)))","v":""},"",{"$f":"IF(T281=\"Select Model\", 0,waterPressureDrop(W281, U281 & \"P\" & IF(V281=\"Dual\",2,1) &\"C\", AC281, \"cooling\", T281))","v":0},{"$f":"IF(T281=\"Select Model\", \"\",getReturnWaterTemp(T281,AC281, activeEWTCooling, AS281, \"cooling\"))","v":""},"",{"$f":"IF($T281<>\"ACBC_1W\",\"\",IF($J281=\"\",\"\",FintubeCapacity($T281,$W281,$AE281,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T281=\"Select Model\",T281=\"PCBL\"),\"\",calcQwIP(Y281,W281,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD281,BD281,\"capacity\",U281&\"P\"&IF(V281=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T281,activeElevation))","v":""},"",{"$f":"IF(OR(T281=\"Select Model\",T281=\"PCBL\"), \"\",IF(AY281=0,\"N/A\",waterPressureDrop(W281, U281 & \"P\" & IF(V281=\"Dual\",2,1) &\"C\", AD281, \"heating\", T281)))","v":""},{"$f":"IF(OR(T281=\"Select Model\",T281=\"PCBL\"), \"\",IF(AY281=0,getReturnWaterTemp(T281,AE281, activeEWTHeating, AX281, \"heating\"),getReturnWaterTemp(T281,AD281, activeEWTHeating, AY281, \"heating\")))","v":""},"",{"$f":" getNozzle(T281, W281, Y281, Z281, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I282)),I282<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I282, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H282)),H282<0),\"\",intlEstQuantity(T282, W282*12, H282)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T282=\"Select Model\",\"\",coilCircuitChange(W282, U282, AC282, T282,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T282=\"Select Model\",\"\",beamWidth(T282))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T282=\"Select Model\",T282=\"PCBL\"), 0,getSPIP(T282, W282, Y282, BD282, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T282=\"Select Model\", \"\",IF(T282=\"PCBL\",0,primaryAirSensibleCapacityIP($T282,$W282,activeRoomTempCooling,activePriAirTempCooling,$Y282,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T282=\"Select Model\",\"\",IF($T282=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y282,activeElevation)))","v":""},{"$f":"IF(OR(T282=\"Select Model\",T282=\"PCBL\"), 0,IF(AD282=0,0,-primaryAirSensibleCapacityIP($T282,$W282,activeRoomTempHeating,activePriAirTempHeating,$Y282,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T282=\"Select Model\", \"\", InductionRatio($T282,BD282,$W282,$Y282)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T282=\"Select Model\", \"\",IF($T282=\"PCBL\",\"N/A\",minVAVSetBack(AA282, Y282))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T282=\"Select Model\", \"\",IF($T282= \"PCBL\",\"N/A\",getDischargeAirTemp($T282,$V282,$AC282,$W282,BD282,$AL282, $Y282, $AS282, \"cooling\",activeElevation,$AB282,$AJ282,$AV282,$BB282))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T282=\"Select Model\",$T282=\"PCBL\"), \"\",getDischargeAirTemp($T282,$V282,$AD282,$W282,BD282,$AL282, $Y282, $AY282, \"heating\",activeElevation,$AB282,$AJ282,$AV282,$BB282)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T282=\"Select Model\", \"\",IF(OR($T282=\"ACBC_1W\",$T282=\"ACBC_2W\",LEFT($T282,4)=\"ACBR\",$T282 = \"LIU24_2W\",LEFT($T282,3)=\"RIU\",LEFT($T282,6)=\"ACBL12\"), IF((soundLevel($T282, $AB282, BD282, $Y282, $W282,$AJ282,$AA282,\"dba\"))<15,\"<15\",soundLevel($T282, $AB282, BD282, $Y282, $W282,$AJ282,$AA282,\"dba\")+0.4),IF((soundLevel($T282, $AB282, BD282, $Y282, $W282,$AJ282,$AA282,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T282, $AB282, BD282, $Y282, $W282,$AJ282,$AA282,\"dba\")+5)<15, \"<15\", soundLevel($T282, $AB282, BD282,$Y282, $W282,$AJ282,$AA282,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T282=\"Select Model\", \"\",IF(OR($T282=\"ACBC_1W\",$T282=\"ACBC_2W\",LEFT($T282,4)=\"ACBR\",$T282=\"LIU24_2W\",LEFT($T282,3)=\"RIU\",LEFT($T282,6)=\"ACBL12\"), IF((soundLevel($T282, $AB282, BD282, $Y282, $W282,$AJ282,$AA282,\"NC\"))<15,\"<15\",soundLevel($T282, $AB282, BD282, $Y282, $W282,$AJ282,$AA282,\"NC\")+0.4),IF((soundLevel($T282, $AB282, BD282, $Y282, $W282,$AJ282,$AA282,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T282, $AB282, BD282, $Y282, $W282,$AJ282,$AA282,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T282, $AB282, BD282, $Y282, $W282,$AJ282,$AA282,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T282=\"Select Model\",\"\",IF($T282=\"LIU24_2W\",calcQwIP($Y282,$W282,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC282,$AI282,\"latent\",$U282&\"P\"&IF($V282=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T282,activeElevation),\"\"))","v":""},{"$f":"IF($T282=\"Select Model\",\"\",IF($T282=\"ACBC_1W\",calcQwIP($Y282,$W282,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC282,BD282,\"capacity\",$U282&\"P\"&IF($V282=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T282,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y282,$W282,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC282,BD282,\"capacity\",$U282&\"P\"&IF($V282=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T282,activeElevation)))","v":""},"",{"$f":"IF(T282=\"Select Model\", 0,waterPressureDrop(W282, U282 & \"P\" & IF(V282=\"Dual\",2,1) &\"C\", AC282, \"cooling\", T282))","v":0},{"$f":"IF(T282=\"Select Model\", \"\",getReturnWaterTemp(T282,AC282, activeEWTCooling, AS282, \"cooling\"))","v":""},"",{"$f":"IF($T282<>\"ACBC_1W\",\"\",IF($J282=\"\",\"\",FintubeCapacity($T282,$W282,$AE282,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T282=\"Select Model\",T282=\"PCBL\"),\"\",calcQwIP(Y282,W282,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD282,BD282,\"capacity\",U282&\"P\"&IF(V282=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T282,activeElevation))","v":""},"",{"$f":"IF(OR(T282=\"Select Model\",T282=\"PCBL\"), \"\",IF(AY282=0,\"N/A\",waterPressureDrop(W282, U282 & \"P\" & IF(V282=\"Dual\",2,1) &\"C\", AD282, \"heating\", T282)))","v":""},{"$f":"IF(OR(T282=\"Select Model\",T282=\"PCBL\"), \"\",IF(AY282=0,getReturnWaterTemp(T282,AE282, activeEWTHeating, AX282, \"heating\"),getReturnWaterTemp(T282,AD282, activeEWTHeating, AY282, \"heating\")))","v":""},"",{"$f":" getNozzle(T282, W282, Y282, Z282, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I283)),I283<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I283, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H283)),H283<0),\"\",intlEstQuantity(T283, W283*12, H283)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T283=\"Select Model\",\"\",coilCircuitChange(W283, U283, AC283, T283,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T283=\"Select Model\",\"\",beamWidth(T283))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T283=\"Select Model\",T283=\"PCBL\"), 0,getSPIP(T283, W283, Y283, BD283, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T283=\"Select Model\", \"\",IF(T283=\"PCBL\",0,primaryAirSensibleCapacityIP($T283,$W283,activeRoomTempCooling,activePriAirTempCooling,$Y283,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T283=\"Select Model\",\"\",IF($T283=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y283,activeElevation)))","v":""},{"$f":"IF(OR(T283=\"Select Model\",T283=\"PCBL\"), 0,IF(AD283=0,0,-primaryAirSensibleCapacityIP($T283,$W283,activeRoomTempHeating,activePriAirTempHeating,$Y283,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T283=\"Select Model\", \"\", InductionRatio($T283,BD283,$W283,$Y283)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T283=\"Select Model\", \"\",IF($T283=\"PCBL\",\"N/A\",minVAVSetBack(AA283, Y283))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T283=\"Select Model\", \"\",IF($T283= \"PCBL\",\"N/A\",getDischargeAirTemp($T283,$V283,$AC283,$W283,BD283,$AL283, $Y283, $AS283, \"cooling\",activeElevation,$AB283,$AJ283,$AV283,$BB283))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T283=\"Select Model\",$T283=\"PCBL\"), \"\",getDischargeAirTemp($T283,$V283,$AD283,$W283,BD283,$AL283, $Y283, $AY283, \"heating\",activeElevation,$AB283,$AJ283,$AV283,$BB283)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T283=\"Select Model\", \"\",IF(OR($T283=\"ACBC_1W\",$T283=\"ACBC_2W\",LEFT($T283,4)=\"ACBR\",$T283 = \"LIU24_2W\",LEFT($T283,3)=\"RIU\",LEFT($T283,6)=\"ACBL12\"), IF((soundLevel($T283, $AB283, BD283, $Y283, $W283,$AJ283,$AA283,\"dba\"))<15,\"<15\",soundLevel($T283, $AB283, BD283, $Y283, $W283,$AJ283,$AA283,\"dba\")+0.4),IF((soundLevel($T283, $AB283, BD283, $Y283, $W283,$AJ283,$AA283,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T283, $AB283, BD283, $Y283, $W283,$AJ283,$AA283,\"dba\")+5)<15, \"<15\", soundLevel($T283, $AB283, BD283,$Y283, $W283,$AJ283,$AA283,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T283=\"Select Model\", \"\",IF(OR($T283=\"ACBC_1W\",$T283=\"ACBC_2W\",LEFT($T283,4)=\"ACBR\",$T283=\"LIU24_2W\",LEFT($T283,3)=\"RIU\",LEFT($T283,6)=\"ACBL12\"), IF((soundLevel($T283, $AB283, BD283, $Y283, $W283,$AJ283,$AA283,\"NC\"))<15,\"<15\",soundLevel($T283, $AB283, BD283, $Y283, $W283,$AJ283,$AA283,\"NC\")+0.4),IF((soundLevel($T283, $AB283, BD283, $Y283, $W283,$AJ283,$AA283,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T283, $AB283, BD283, $Y283, $W283,$AJ283,$AA283,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T283, $AB283, BD283, $Y283, $W283,$AJ283,$AA283,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T283=\"Select Model\",\"\",IF($T283=\"LIU24_2W\",calcQwIP($Y283,$W283,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC283,$AI283,\"latent\",$U283&\"P\"&IF($V283=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T283,activeElevation),\"\"))","v":""},{"$f":"IF($T283=\"Select Model\",\"\",IF($T283=\"ACBC_1W\",calcQwIP($Y283,$W283,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC283,BD283,\"capacity\",$U283&\"P\"&IF($V283=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T283,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y283,$W283,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC283,BD283,\"capacity\",$U283&\"P\"&IF($V283=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T283,activeElevation)))","v":""},"",{"$f":"IF(T283=\"Select Model\", 0,waterPressureDrop(W283, U283 & \"P\" & IF(V283=\"Dual\",2,1) &\"C\", AC283, \"cooling\", T283))","v":0},{"$f":"IF(T283=\"Select Model\", \"\",getReturnWaterTemp(T283,AC283, activeEWTCooling, AS283, \"cooling\"))","v":""},"",{"$f":"IF($T283<>\"ACBC_1W\",\"\",IF($J283=\"\",\"\",FintubeCapacity($T283,$W283,$AE283,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T283=\"Select Model\",T283=\"PCBL\"),\"\",calcQwIP(Y283,W283,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD283,BD283,\"capacity\",U283&\"P\"&IF(V283=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T283,activeElevation))","v":""},"",{"$f":"IF(OR(T283=\"Select Model\",T283=\"PCBL\"), \"\",IF(AY283=0,\"N/A\",waterPressureDrop(W283, U283 & \"P\" & IF(V283=\"Dual\",2,1) &\"C\", AD283, \"heating\", T283)))","v":""},{"$f":"IF(OR(T283=\"Select Model\",T283=\"PCBL\"), \"\",IF(AY283=0,getReturnWaterTemp(T283,AE283, activeEWTHeating, AX283, \"heating\"),getReturnWaterTemp(T283,AD283, activeEWTHeating, AY283, \"heating\")))","v":""},"",{"$f":" getNozzle(T283, W283, Y283, Z283, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I284)),I284<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I284, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H284)),H284<0),\"\",intlEstQuantity(T284, W284*12, H284)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T284=\"Select Model\",\"\",coilCircuitChange(W284, U284, AC284, T284,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T284=\"Select Model\",\"\",beamWidth(T284))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T284=\"Select Model\",T284=\"PCBL\"), 0,getSPIP(T284, W284, Y284, BD284, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T284=\"Select Model\", \"\",IF(T284=\"PCBL\",0,primaryAirSensibleCapacityIP($T284,$W284,activeRoomTempCooling,activePriAirTempCooling,$Y284,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T284=\"Select Model\",\"\",IF($T284=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y284,activeElevation)))","v":""},{"$f":"IF(OR(T284=\"Select Model\",T284=\"PCBL\"), 0,IF(AD284=0,0,-primaryAirSensibleCapacityIP($T284,$W284,activeRoomTempHeating,activePriAirTempHeating,$Y284,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T284=\"Select Model\", \"\", InductionRatio($T284,BD284,$W284,$Y284)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T284=\"Select Model\", \"\",IF($T284=\"PCBL\",\"N/A\",minVAVSetBack(AA284, Y284))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T284=\"Select Model\", \"\",IF($T284= \"PCBL\",\"N/A\",getDischargeAirTemp($T284,$V284,$AC284,$W284,BD284,$AL284, $Y284, $AS284, \"cooling\",activeElevation,$AB284,$AJ284,$AV284,$BB284))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T284=\"Select Model\",$T284=\"PCBL\"), \"\",getDischargeAirTemp($T284,$V284,$AD284,$W284,BD284,$AL284, $Y284, $AY284, \"heating\",activeElevation,$AB284,$AJ284,$AV284,$BB284)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T284=\"Select Model\", \"\",IF(OR($T284=\"ACBC_1W\",$T284=\"ACBC_2W\",LEFT($T284,4)=\"ACBR\",$T284 = \"LIU24_2W\",LEFT($T284,3)=\"RIU\",LEFT($T284,6)=\"ACBL12\"), IF((soundLevel($T284, $AB284, BD284, $Y284, $W284,$AJ284,$AA284,\"dba\"))<15,\"<15\",soundLevel($T284, $AB284, BD284, $Y284, $W284,$AJ284,$AA284,\"dba\")+0.4),IF((soundLevel($T284, $AB284, BD284, $Y284, $W284,$AJ284,$AA284,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T284, $AB284, BD284, $Y284, $W284,$AJ284,$AA284,\"dba\")+5)<15, \"<15\", soundLevel($T284, $AB284, BD284,$Y284, $W284,$AJ284,$AA284,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T284=\"Select Model\", \"\",IF(OR($T284=\"ACBC_1W\",$T284=\"ACBC_2W\",LEFT($T284,4)=\"ACBR\",$T284=\"LIU24_2W\",LEFT($T284,3)=\"RIU\",LEFT($T284,6)=\"ACBL12\"), IF((soundLevel($T284, $AB284, BD284, $Y284, $W284,$AJ284,$AA284,\"NC\"))<15,\"<15\",soundLevel($T284, $AB284, BD284, $Y284, $W284,$AJ284,$AA284,\"NC\")+0.4),IF((soundLevel($T284, $AB284, BD284, $Y284, $W284,$AJ284,$AA284,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T284, $AB284, BD284, $Y284, $W284,$AJ284,$AA284,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T284, $AB284, BD284, $Y284, $W284,$AJ284,$AA284,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T284=\"Select Model\",\"\",IF($T284=\"LIU24_2W\",calcQwIP($Y284,$W284,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC284,$AI284,\"latent\",$U284&\"P\"&IF($V284=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T284,activeElevation),\"\"))","v":""},{"$f":"IF($T284=\"Select Model\",\"\",IF($T284=\"ACBC_1W\",calcQwIP($Y284,$W284,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC284,BD284,\"capacity\",$U284&\"P\"&IF($V284=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T284,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y284,$W284,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC284,BD284,\"capacity\",$U284&\"P\"&IF($V284=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T284,activeElevation)))","v":""},"",{"$f":"IF(T284=\"Select Model\", 0,waterPressureDrop(W284, U284 & \"P\" & IF(V284=\"Dual\",2,1) &\"C\", AC284, \"cooling\", T284))","v":0},{"$f":"IF(T284=\"Select Model\", \"\",getReturnWaterTemp(T284,AC284, activeEWTCooling, AS284, \"cooling\"))","v":""},"",{"$f":"IF($T284<>\"ACBC_1W\",\"\",IF($J284=\"\",\"\",FintubeCapacity($T284,$W284,$AE284,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T284=\"Select Model\",T284=\"PCBL\"),\"\",calcQwIP(Y284,W284,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD284,BD284,\"capacity\",U284&\"P\"&IF(V284=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T284,activeElevation))","v":""},"",{"$f":"IF(OR(T284=\"Select Model\",T284=\"PCBL\"), \"\",IF(AY284=0,\"N/A\",waterPressureDrop(W284, U284 & \"P\" & IF(V284=\"Dual\",2,1) &\"C\", AD284, \"heating\", T284)))","v":""},{"$f":"IF(OR(T284=\"Select Model\",T284=\"PCBL\"), \"\",IF(AY284=0,getReturnWaterTemp(T284,AE284, activeEWTHeating, AX284, \"heating\"),getReturnWaterTemp(T284,AD284, activeEWTHeating, AY284, \"heating\")))","v":""},"",{"$f":" getNozzle(T284, W284, Y284, Z284, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I285)),I285<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I285, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H285)),H285<0),\"\",intlEstQuantity(T285, W285*12, H285)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T285=\"Select Model\",\"\",coilCircuitChange(W285, U285, AC285, T285,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T285=\"Select Model\",\"\",beamWidth(T285))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T285=\"Select Model\",T285=\"PCBL\"), 0,getSPIP(T285, W285, Y285, BD285, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T285=\"Select Model\", \"\",IF(T285=\"PCBL\",0,primaryAirSensibleCapacityIP($T285,$W285,activeRoomTempCooling,activePriAirTempCooling,$Y285,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T285=\"Select Model\",\"\",IF($T285=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y285,activeElevation)))","v":""},{"$f":"IF(OR(T285=\"Select Model\",T285=\"PCBL\"), 0,IF(AD285=0,0,-primaryAirSensibleCapacityIP($T285,$W285,activeRoomTempHeating,activePriAirTempHeating,$Y285,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T285=\"Select Model\", \"\", InductionRatio($T285,BD285,$W285,$Y285)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T285=\"Select Model\", \"\",IF($T285=\"PCBL\",\"N/A\",minVAVSetBack(AA285, Y285))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T285=\"Select Model\", \"\",IF($T285= \"PCBL\",\"N/A\",getDischargeAirTemp($T285,$V285,$AC285,$W285,BD285,$AL285, $Y285, $AS285, \"cooling\",activeElevation,$AB285,$AJ285,$AV285,$BB285))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T285=\"Select Model\",$T285=\"PCBL\"), \"\",getDischargeAirTemp($T285,$V285,$AD285,$W285,BD285,$AL285, $Y285, $AY285, \"heating\",activeElevation,$AB285,$AJ285,$AV285,$BB285)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T285=\"Select Model\", \"\",IF(OR($T285=\"ACBC_1W\",$T285=\"ACBC_2W\",LEFT($T285,4)=\"ACBR\",$T285 = \"LIU24_2W\",LEFT($T285,3)=\"RIU\",LEFT($T285,6)=\"ACBL12\"), IF((soundLevel($T285, $AB285, BD285, $Y285, $W285,$AJ285,$AA285,\"dba\"))<15,\"<15\",soundLevel($T285, $AB285, BD285, $Y285, $W285,$AJ285,$AA285,\"dba\")+0.4),IF((soundLevel($T285, $AB285, BD285, $Y285, $W285,$AJ285,$AA285,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T285, $AB285, BD285, $Y285, $W285,$AJ285,$AA285,\"dba\")+5)<15, \"<15\", soundLevel($T285, $AB285, BD285,$Y285, $W285,$AJ285,$AA285,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T285=\"Select Model\", \"\",IF(OR($T285=\"ACBC_1W\",$T285=\"ACBC_2W\",LEFT($T285,4)=\"ACBR\",$T285=\"LIU24_2W\",LEFT($T285,3)=\"RIU\",LEFT($T285,6)=\"ACBL12\"), IF((soundLevel($T285, $AB285, BD285, $Y285, $W285,$AJ285,$AA285,\"NC\"))<15,\"<15\",soundLevel($T285, $AB285, BD285, $Y285, $W285,$AJ285,$AA285,\"NC\")+0.4),IF((soundLevel($T285, $AB285, BD285, $Y285, $W285,$AJ285,$AA285,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T285, $AB285, BD285, $Y285, $W285,$AJ285,$AA285,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T285, $AB285, BD285, $Y285, $W285,$AJ285,$AA285,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T285=\"Select Model\",\"\",IF($T285=\"LIU24_2W\",calcQwIP($Y285,$W285,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC285,$AI285,\"latent\",$U285&\"P\"&IF($V285=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T285,activeElevation),\"\"))","v":""},{"$f":"IF($T285=\"Select Model\",\"\",IF($T285=\"ACBC_1W\",calcQwIP($Y285,$W285,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC285,BD285,\"capacity\",$U285&\"P\"&IF($V285=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T285,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y285,$W285,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC285,BD285,\"capacity\",$U285&\"P\"&IF($V285=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T285,activeElevation)))","v":""},"",{"$f":"IF(T285=\"Select Model\", 0,waterPressureDrop(W285, U285 & \"P\" & IF(V285=\"Dual\",2,1) &\"C\", AC285, \"cooling\", T285))","v":0},{"$f":"IF(T285=\"Select Model\", \"\",getReturnWaterTemp(T285,AC285, activeEWTCooling, AS285, \"cooling\"))","v":""},"",{"$f":"IF($T285<>\"ACBC_1W\",\"\",IF($J285=\"\",\"\",FintubeCapacity($T285,$W285,$AE285,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T285=\"Select Model\",T285=\"PCBL\"),\"\",calcQwIP(Y285,W285,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD285,BD285,\"capacity\",U285&\"P\"&IF(V285=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T285,activeElevation))","v":""},"",{"$f":"IF(OR(T285=\"Select Model\",T285=\"PCBL\"), \"\",IF(AY285=0,\"N/A\",waterPressureDrop(W285, U285 & \"P\" & IF(V285=\"Dual\",2,1) &\"C\", AD285, \"heating\", T285)))","v":""},{"$f":"IF(OR(T285=\"Select Model\",T285=\"PCBL\"), \"\",IF(AY285=0,getReturnWaterTemp(T285,AE285, activeEWTHeating, AX285, \"heating\"),getReturnWaterTemp(T285,AD285, activeEWTHeating, AY285, \"heating\")))","v":""},"",{"$f":" getNozzle(T285, W285, Y285, Z285, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I286)),I286<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I286, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H286)),H286<0),\"\",intlEstQuantity(T286, W286*12, H286)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T286=\"Select Model\",\"\",coilCircuitChange(W286, U286, AC286, T286,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T286=\"Select Model\",\"\",beamWidth(T286))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T286=\"Select Model\",T286=\"PCBL\"), 0,getSPIP(T286, W286, Y286, BD286, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T286=\"Select Model\", \"\",IF(T286=\"PCBL\",0,primaryAirSensibleCapacityIP($T286,$W286,activeRoomTempCooling,activePriAirTempCooling,$Y286,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T286=\"Select Model\",\"\",IF($T286=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y286,activeElevation)))","v":""},{"$f":"IF(OR(T286=\"Select Model\",T286=\"PCBL\"), 0,IF(AD286=0,0,-primaryAirSensibleCapacityIP($T286,$W286,activeRoomTempHeating,activePriAirTempHeating,$Y286,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T286=\"Select Model\", \"\", InductionRatio($T286,BD286,$W286,$Y286)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T286=\"Select Model\", \"\",IF($T286=\"PCBL\",\"N/A\",minVAVSetBack(AA286, Y286))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T286=\"Select Model\", \"\",IF($T286= \"PCBL\",\"N/A\",getDischargeAirTemp($T286,$V286,$AC286,$W286,BD286,$AL286, $Y286, $AS286, \"cooling\",activeElevation,$AB286,$AJ286,$AV286,$BB286))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T286=\"Select Model\",$T286=\"PCBL\"), \"\",getDischargeAirTemp($T286,$V286,$AD286,$W286,BD286,$AL286, $Y286, $AY286, \"heating\",activeElevation,$AB286,$AJ286,$AV286,$BB286)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T286=\"Select Model\", \"\",IF(OR($T286=\"ACBC_1W\",$T286=\"ACBC_2W\",LEFT($T286,4)=\"ACBR\",$T286 = \"LIU24_2W\",LEFT($T286,3)=\"RIU\",LEFT($T286,6)=\"ACBL12\"), IF((soundLevel($T286, $AB286, BD286, $Y286, $W286,$AJ286,$AA286,\"dba\"))<15,\"<15\",soundLevel($T286, $AB286, BD286, $Y286, $W286,$AJ286,$AA286,\"dba\")+0.4),IF((soundLevel($T286, $AB286, BD286, $Y286, $W286,$AJ286,$AA286,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T286, $AB286, BD286, $Y286, $W286,$AJ286,$AA286,\"dba\")+5)<15, \"<15\", soundLevel($T286, $AB286, BD286,$Y286, $W286,$AJ286,$AA286,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T286=\"Select Model\", \"\",IF(OR($T286=\"ACBC_1W\",$T286=\"ACBC_2W\",LEFT($T286,4)=\"ACBR\",$T286=\"LIU24_2W\",LEFT($T286,3)=\"RIU\",LEFT($T286,6)=\"ACBL12\"), IF((soundLevel($T286, $AB286, BD286, $Y286, $W286,$AJ286,$AA286,\"NC\"))<15,\"<15\",soundLevel($T286, $AB286, BD286, $Y286, $W286,$AJ286,$AA286,\"NC\")+0.4),IF((soundLevel($T286, $AB286, BD286, $Y286, $W286,$AJ286,$AA286,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T286, $AB286, BD286, $Y286, $W286,$AJ286,$AA286,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T286, $AB286, BD286, $Y286, $W286,$AJ286,$AA286,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T286=\"Select Model\",\"\",IF($T286=\"LIU24_2W\",calcQwIP($Y286,$W286,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC286,$AI286,\"latent\",$U286&\"P\"&IF($V286=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T286,activeElevation),\"\"))","v":""},{"$f":"IF($T286=\"Select Model\",\"\",IF($T286=\"ACBC_1W\",calcQwIP($Y286,$W286,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC286,BD286,\"capacity\",$U286&\"P\"&IF($V286=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T286,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y286,$W286,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC286,BD286,\"capacity\",$U286&\"P\"&IF($V286=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T286,activeElevation)))","v":""},"",{"$f":"IF(T286=\"Select Model\", 0,waterPressureDrop(W286, U286 & \"P\" & IF(V286=\"Dual\",2,1) &\"C\", AC286, \"cooling\", T286))","v":0},{"$f":"IF(T286=\"Select Model\", \"\",getReturnWaterTemp(T286,AC286, activeEWTCooling, AS286, \"cooling\"))","v":""},"",{"$f":"IF($T286<>\"ACBC_1W\",\"\",IF($J286=\"\",\"\",FintubeCapacity($T286,$W286,$AE286,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T286=\"Select Model\",T286=\"PCBL\"),\"\",calcQwIP(Y286,W286,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD286,BD286,\"capacity\",U286&\"P\"&IF(V286=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T286,activeElevation))","v":""},"",{"$f":"IF(OR(T286=\"Select Model\",T286=\"PCBL\"), \"\",IF(AY286=0,\"N/A\",waterPressureDrop(W286, U286 & \"P\" & IF(V286=\"Dual\",2,1) &\"C\", AD286, \"heating\", T286)))","v":""},{"$f":"IF(OR(T286=\"Select Model\",T286=\"PCBL\"), \"\",IF(AY286=0,getReturnWaterTemp(T286,AE286, activeEWTHeating, AX286, \"heating\"),getReturnWaterTemp(T286,AD286, activeEWTHeating, AY286, \"heating\")))","v":""},"",{"$f":" getNozzle(T286, W286, Y286, Z286, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I287)),I287<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I287, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H287)),H287<0),\"\",intlEstQuantity(T287, W287*12, H287)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T287=\"Select Model\",\"\",coilCircuitChange(W287, U287, AC287, T287,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T287=\"Select Model\",\"\",beamWidth(T287))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T287=\"Select Model\",T287=\"PCBL\"), 0,getSPIP(T287, W287, Y287, BD287, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T287=\"Select Model\", \"\",IF(T287=\"PCBL\",0,primaryAirSensibleCapacityIP($T287,$W287,activeRoomTempCooling,activePriAirTempCooling,$Y287,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T287=\"Select Model\",\"\",IF($T287=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y287,activeElevation)))","v":""},{"$f":"IF(OR(T287=\"Select Model\",T287=\"PCBL\"), 0,IF(AD287=0,0,-primaryAirSensibleCapacityIP($T287,$W287,activeRoomTempHeating,activePriAirTempHeating,$Y287,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T287=\"Select Model\", \"\", InductionRatio($T287,BD287,$W287,$Y287)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T287=\"Select Model\", \"\",IF($T287=\"PCBL\",\"N/A\",minVAVSetBack(AA287, Y287))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T287=\"Select Model\", \"\",IF($T287= \"PCBL\",\"N/A\",getDischargeAirTemp($T287,$V287,$AC287,$W287,BD287,$AL287, $Y287, $AS287, \"cooling\",activeElevation,$AB287,$AJ287,$AV287,$BB287))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T287=\"Select Model\",$T287=\"PCBL\"), \"\",getDischargeAirTemp($T287,$V287,$AD287,$W287,BD287,$AL287, $Y287, $AY287, \"heating\",activeElevation,$AB287,$AJ287,$AV287,$BB287)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T287=\"Select Model\", \"\",IF(OR($T287=\"ACBC_1W\",$T287=\"ACBC_2W\",LEFT($T287,4)=\"ACBR\",$T287 = \"LIU24_2W\",LEFT($T287,3)=\"RIU\",LEFT($T287,6)=\"ACBL12\"), IF((soundLevel($T287, $AB287, BD287, $Y287, $W287,$AJ287,$AA287,\"dba\"))<15,\"<15\",soundLevel($T287, $AB287, BD287, $Y287, $W287,$AJ287,$AA287,\"dba\")+0.4),IF((soundLevel($T287, $AB287, BD287, $Y287, $W287,$AJ287,$AA287,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T287, $AB287, BD287, $Y287, $W287,$AJ287,$AA287,\"dba\")+5)<15, \"<15\", soundLevel($T287, $AB287, BD287,$Y287, $W287,$AJ287,$AA287,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T287=\"Select Model\", \"\",IF(OR($T287=\"ACBC_1W\",$T287=\"ACBC_2W\",LEFT($T287,4)=\"ACBR\",$T287=\"LIU24_2W\",LEFT($T287,3)=\"RIU\",LEFT($T287,6)=\"ACBL12\"), IF((soundLevel($T287, $AB287, BD287, $Y287, $W287,$AJ287,$AA287,\"NC\"))<15,\"<15\",soundLevel($T287, $AB287, BD287, $Y287, $W287,$AJ287,$AA287,\"NC\")+0.4),IF((soundLevel($T287, $AB287, BD287, $Y287, $W287,$AJ287,$AA287,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T287, $AB287, BD287, $Y287, $W287,$AJ287,$AA287,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T287, $AB287, BD287, $Y287, $W287,$AJ287,$AA287,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T287=\"Select Model\",\"\",IF($T287=\"LIU24_2W\",calcQwIP($Y287,$W287,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC287,$AI287,\"latent\",$U287&\"P\"&IF($V287=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T287,activeElevation),\"\"))","v":""},{"$f":"IF($T287=\"Select Model\",\"\",IF($T287=\"ACBC_1W\",calcQwIP($Y287,$W287,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC287,BD287,\"capacity\",$U287&\"P\"&IF($V287=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T287,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y287,$W287,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC287,BD287,\"capacity\",$U287&\"P\"&IF($V287=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T287,activeElevation)))","v":""},"",{"$f":"IF(T287=\"Select Model\", 0,waterPressureDrop(W287, U287 & \"P\" & IF(V287=\"Dual\",2,1) &\"C\", AC287, \"cooling\", T287))","v":0},{"$f":"IF(T287=\"Select Model\", \"\",getReturnWaterTemp(T287,AC287, activeEWTCooling, AS287, \"cooling\"))","v":""},"",{"$f":"IF($T287<>\"ACBC_1W\",\"\",IF($J287=\"\",\"\",FintubeCapacity($T287,$W287,$AE287,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T287=\"Select Model\",T287=\"PCBL\"),\"\",calcQwIP(Y287,W287,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD287,BD287,\"capacity\",U287&\"P\"&IF(V287=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T287,activeElevation))","v":""},"",{"$f":"IF(OR(T287=\"Select Model\",T287=\"PCBL\"), \"\",IF(AY287=0,\"N/A\",waterPressureDrop(W287, U287 & \"P\" & IF(V287=\"Dual\",2,1) &\"C\", AD287, \"heating\", T287)))","v":""},{"$f":"IF(OR(T287=\"Select Model\",T287=\"PCBL\"), \"\",IF(AY287=0,getReturnWaterTemp(T287,AE287, activeEWTHeating, AX287, \"heating\"),getReturnWaterTemp(T287,AD287, activeEWTHeating, AY287, \"heating\")))","v":""},"",{"$f":" getNozzle(T287, W287, Y287, Z287, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I288)),I288<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I288, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H288)),H288<0),\"\",intlEstQuantity(T288, W288*12, H288)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T288=\"Select Model\",\"\",coilCircuitChange(W288, U288, AC288, T288,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T288=\"Select Model\",\"\",beamWidth(T288))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T288=\"Select Model\",T288=\"PCBL\"), 0,getSPIP(T288, W288, Y288, BD288, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T288=\"Select Model\", \"\",IF(T288=\"PCBL\",0,primaryAirSensibleCapacityIP($T288,$W288,activeRoomTempCooling,activePriAirTempCooling,$Y288,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T288=\"Select Model\",\"\",IF($T288=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y288,activeElevation)))","v":""},{"$f":"IF(OR(T288=\"Select Model\",T288=\"PCBL\"), 0,IF(AD288=0,0,-primaryAirSensibleCapacityIP($T288,$W288,activeRoomTempHeating,activePriAirTempHeating,$Y288,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T288=\"Select Model\", \"\", InductionRatio($T288,BD288,$W288,$Y288)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T288=\"Select Model\", \"\",IF($T288=\"PCBL\",\"N/A\",minVAVSetBack(AA288, Y288))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T288=\"Select Model\", \"\",IF($T288= \"PCBL\",\"N/A\",getDischargeAirTemp($T288,$V288,$AC288,$W288,BD288,$AL288, $Y288, $AS288, \"cooling\",activeElevation,$AB288,$AJ288,$AV288,$BB288))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T288=\"Select Model\",$T288=\"PCBL\"), \"\",getDischargeAirTemp($T288,$V288,$AD288,$W288,BD288,$AL288, $Y288, $AY288, \"heating\",activeElevation,$AB288,$AJ288,$AV288,$BB288)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T288=\"Select Model\", \"\",IF(OR($T288=\"ACBC_1W\",$T288=\"ACBC_2W\",LEFT($T288,4)=\"ACBR\",$T288 = \"LIU24_2W\",LEFT($T288,3)=\"RIU\",LEFT($T288,6)=\"ACBL12\"), IF((soundLevel($T288, $AB288, BD288, $Y288, $W288,$AJ288,$AA288,\"dba\"))<15,\"<15\",soundLevel($T288, $AB288, BD288, $Y288, $W288,$AJ288,$AA288,\"dba\")+0.4),IF((soundLevel($T288, $AB288, BD288, $Y288, $W288,$AJ288,$AA288,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T288, $AB288, BD288, $Y288, $W288,$AJ288,$AA288,\"dba\")+5)<15, \"<15\", soundLevel($T288, $AB288, BD288,$Y288, $W288,$AJ288,$AA288,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T288=\"Select Model\", \"\",IF(OR($T288=\"ACBC_1W\",$T288=\"ACBC_2W\",LEFT($T288,4)=\"ACBR\",$T288=\"LIU24_2W\",LEFT($T288,3)=\"RIU\",LEFT($T288,6)=\"ACBL12\"), IF((soundLevel($T288, $AB288, BD288, $Y288, $W288,$AJ288,$AA288,\"NC\"))<15,\"<15\",soundLevel($T288, $AB288, BD288, $Y288, $W288,$AJ288,$AA288,\"NC\")+0.4),IF((soundLevel($T288, $AB288, BD288, $Y288, $W288,$AJ288,$AA288,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T288, $AB288, BD288, $Y288, $W288,$AJ288,$AA288,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T288, $AB288, BD288, $Y288, $W288,$AJ288,$AA288,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T288=\"Select Model\",\"\",IF($T288=\"LIU24_2W\",calcQwIP($Y288,$W288,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC288,$AI288,\"latent\",$U288&\"P\"&IF($V288=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T288,activeElevation),\"\"))","v":""},{"$f":"IF($T288=\"Select Model\",\"\",IF($T288=\"ACBC_1W\",calcQwIP($Y288,$W288,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC288,BD288,\"capacity\",$U288&\"P\"&IF($V288=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T288,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y288,$W288,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC288,BD288,\"capacity\",$U288&\"P\"&IF($V288=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T288,activeElevation)))","v":""},"",{"$f":"IF(T288=\"Select Model\", 0,waterPressureDrop(W288, U288 & \"P\" & IF(V288=\"Dual\",2,1) &\"C\", AC288, \"cooling\", T288))","v":0},{"$f":"IF(T288=\"Select Model\", \"\",getReturnWaterTemp(T288,AC288, activeEWTCooling, AS288, \"cooling\"))","v":""},"",{"$f":"IF($T288<>\"ACBC_1W\",\"\",IF($J288=\"\",\"\",FintubeCapacity($T288,$W288,$AE288,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T288=\"Select Model\",T288=\"PCBL\"),\"\",calcQwIP(Y288,W288,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD288,BD288,\"capacity\",U288&\"P\"&IF(V288=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T288,activeElevation))","v":""},"",{"$f":"IF(OR(T288=\"Select Model\",T288=\"PCBL\"), \"\",IF(AY288=0,\"N/A\",waterPressureDrop(W288, U288 & \"P\" & IF(V288=\"Dual\",2,1) &\"C\", AD288, \"heating\", T288)))","v":""},{"$f":"IF(OR(T288=\"Select Model\",T288=\"PCBL\"), \"\",IF(AY288=0,getReturnWaterTemp(T288,AE288, activeEWTHeating, AX288, \"heating\"),getReturnWaterTemp(T288,AD288, activeEWTHeating, AY288, \"heating\")))","v":""},"",{"$f":" getNozzle(T288, W288, Y288, Z288, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I289)),I289<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I289, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H289)),H289<0),\"\",intlEstQuantity(T289, W289*12, H289)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T289=\"Select Model\",\"\",coilCircuitChange(W289, U289, AC289, T289,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T289=\"Select Model\",\"\",beamWidth(T289))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T289=\"Select Model\",T289=\"PCBL\"), 0,getSPIP(T289, W289, Y289, BD289, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T289=\"Select Model\", \"\",IF(T289=\"PCBL\",0,primaryAirSensibleCapacityIP($T289,$W289,activeRoomTempCooling,activePriAirTempCooling,$Y289,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T289=\"Select Model\",\"\",IF($T289=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y289,activeElevation)))","v":""},{"$f":"IF(OR(T289=\"Select Model\",T289=\"PCBL\"), 0,IF(AD289=0,0,-primaryAirSensibleCapacityIP($T289,$W289,activeRoomTempHeating,activePriAirTempHeating,$Y289,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T289=\"Select Model\", \"\", InductionRatio($T289,BD289,$W289,$Y289)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T289=\"Select Model\", \"\",IF($T289=\"PCBL\",\"N/A\",minVAVSetBack(AA289, Y289))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T289=\"Select Model\", \"\",IF($T289= \"PCBL\",\"N/A\",getDischargeAirTemp($T289,$V289,$AC289,$W289,BD289,$AL289, $Y289, $AS289, \"cooling\",activeElevation,$AB289,$AJ289,$AV289,$BB289))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T289=\"Select Model\",$T289=\"PCBL\"), \"\",getDischargeAirTemp($T289,$V289,$AD289,$W289,BD289,$AL289, $Y289, $AY289, \"heating\",activeElevation,$AB289,$AJ289,$AV289,$BB289)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T289=\"Select Model\", \"\",IF(OR($T289=\"ACBC_1W\",$T289=\"ACBC_2W\",LEFT($T289,4)=\"ACBR\",$T289 = \"LIU24_2W\",LEFT($T289,3)=\"RIU\",LEFT($T289,6)=\"ACBL12\"), IF((soundLevel($T289, $AB289, BD289, $Y289, $W289,$AJ289,$AA289,\"dba\"))<15,\"<15\",soundLevel($T289, $AB289, BD289, $Y289, $W289,$AJ289,$AA289,\"dba\")+0.4),IF((soundLevel($T289, $AB289, BD289, $Y289, $W289,$AJ289,$AA289,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T289, $AB289, BD289, $Y289, $W289,$AJ289,$AA289,\"dba\")+5)<15, \"<15\", soundLevel($T289, $AB289, BD289,$Y289, $W289,$AJ289,$AA289,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T289=\"Select Model\", \"\",IF(OR($T289=\"ACBC_1W\",$T289=\"ACBC_2W\",LEFT($T289,4)=\"ACBR\",$T289=\"LIU24_2W\",LEFT($T289,3)=\"RIU\",LEFT($T289,6)=\"ACBL12\"), IF((soundLevel($T289, $AB289, BD289, $Y289, $W289,$AJ289,$AA289,\"NC\"))<15,\"<15\",soundLevel($T289, $AB289, BD289, $Y289, $W289,$AJ289,$AA289,\"NC\")+0.4),IF((soundLevel($T289, $AB289, BD289, $Y289, $W289,$AJ289,$AA289,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T289, $AB289, BD289, $Y289, $W289,$AJ289,$AA289,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T289, $AB289, BD289, $Y289, $W289,$AJ289,$AA289,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T289=\"Select Model\",\"\",IF($T289=\"LIU24_2W\",calcQwIP($Y289,$W289,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC289,$AI289,\"latent\",$U289&\"P\"&IF($V289=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T289,activeElevation),\"\"))","v":""},{"$f":"IF($T289=\"Select Model\",\"\",IF($T289=\"ACBC_1W\",calcQwIP($Y289,$W289,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC289,BD289,\"capacity\",$U289&\"P\"&IF($V289=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T289,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y289,$W289,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC289,BD289,\"capacity\",$U289&\"P\"&IF($V289=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T289,activeElevation)))","v":""},"",{"$f":"IF(T289=\"Select Model\", 0,waterPressureDrop(W289, U289 & \"P\" & IF(V289=\"Dual\",2,1) &\"C\", AC289, \"cooling\", T289))","v":0},{"$f":"IF(T289=\"Select Model\", \"\",getReturnWaterTemp(T289,AC289, activeEWTCooling, AS289, \"cooling\"))","v":""},"",{"$f":"IF($T289<>\"ACBC_1W\",\"\",IF($J289=\"\",\"\",FintubeCapacity($T289,$W289,$AE289,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T289=\"Select Model\",T289=\"PCBL\"),\"\",calcQwIP(Y289,W289,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD289,BD289,\"capacity\",U289&\"P\"&IF(V289=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T289,activeElevation))","v":""},"",{"$f":"IF(OR(T289=\"Select Model\",T289=\"PCBL\"), \"\",IF(AY289=0,\"N/A\",waterPressureDrop(W289, U289 & \"P\" & IF(V289=\"Dual\",2,1) &\"C\", AD289, \"heating\", T289)))","v":""},{"$f":"IF(OR(T289=\"Select Model\",T289=\"PCBL\"), \"\",IF(AY289=0,getReturnWaterTemp(T289,AE289, activeEWTHeating, AX289, \"heating\"),getReturnWaterTemp(T289,AD289, activeEWTHeating, AY289, \"heating\")))","v":""},"",{"$f":" getNozzle(T289, W289, Y289, Z289, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I290)),I290<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I290, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H290)),H290<0),\"\",intlEstQuantity(T290, W290*12, H290)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T290=\"Select Model\",\"\",coilCircuitChange(W290, U290, AC290, T290,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T290=\"Select Model\",\"\",beamWidth(T290))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T290=\"Select Model\",T290=\"PCBL\"), 0,getSPIP(T290, W290, Y290, BD290, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T290=\"Select Model\", \"\",IF(T290=\"PCBL\",0,primaryAirSensibleCapacityIP($T290,$W290,activeRoomTempCooling,activePriAirTempCooling,$Y290,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T290=\"Select Model\",\"\",IF($T290=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y290,activeElevation)))","v":""},{"$f":"IF(OR(T290=\"Select Model\",T290=\"PCBL\"), 0,IF(AD290=0,0,-primaryAirSensibleCapacityIP($T290,$W290,activeRoomTempHeating,activePriAirTempHeating,$Y290,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T290=\"Select Model\", \"\", InductionRatio($T290,BD290,$W290,$Y290)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T290=\"Select Model\", \"\",IF($T290=\"PCBL\",\"N/A\",minVAVSetBack(AA290, Y290))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T290=\"Select Model\", \"\",IF($T290= \"PCBL\",\"N/A\",getDischargeAirTemp($T290,$V290,$AC290,$W290,BD290,$AL290, $Y290, $AS290, \"cooling\",activeElevation,$AB290,$AJ290,$AV290,$BB290))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T290=\"Select Model\",$T290=\"PCBL\"), \"\",getDischargeAirTemp($T290,$V290,$AD290,$W290,BD290,$AL290, $Y290, $AY290, \"heating\",activeElevation,$AB290,$AJ290,$AV290,$BB290)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T290=\"Select Model\", \"\",IF(OR($T290=\"ACBC_1W\",$T290=\"ACBC_2W\",LEFT($T290,4)=\"ACBR\",$T290 = \"LIU24_2W\",LEFT($T290,3)=\"RIU\",LEFT($T290,6)=\"ACBL12\"), IF((soundLevel($T290, $AB290, BD290, $Y290, $W290,$AJ290,$AA290,\"dba\"))<15,\"<15\",soundLevel($T290, $AB290, BD290, $Y290, $W290,$AJ290,$AA290,\"dba\")+0.4),IF((soundLevel($T290, $AB290, BD290, $Y290, $W290,$AJ290,$AA290,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T290, $AB290, BD290, $Y290, $W290,$AJ290,$AA290,\"dba\")+5)<15, \"<15\", soundLevel($T290, $AB290, BD290,$Y290, $W290,$AJ290,$AA290,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T290=\"Select Model\", \"\",IF(OR($T290=\"ACBC_1W\",$T290=\"ACBC_2W\",LEFT($T290,4)=\"ACBR\",$T290=\"LIU24_2W\",LEFT($T290,3)=\"RIU\",LEFT($T290,6)=\"ACBL12\"), IF((soundLevel($T290, $AB290, BD290, $Y290, $W290,$AJ290,$AA290,\"NC\"))<15,\"<15\",soundLevel($T290, $AB290, BD290, $Y290, $W290,$AJ290,$AA290,\"NC\")+0.4),IF((soundLevel($T290, $AB290, BD290, $Y290, $W290,$AJ290,$AA290,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T290, $AB290, BD290, $Y290, $W290,$AJ290,$AA290,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T290, $AB290, BD290, $Y290, $W290,$AJ290,$AA290,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T290=\"Select Model\",\"\",IF($T290=\"LIU24_2W\",calcQwIP($Y290,$W290,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC290,$AI290,\"latent\",$U290&\"P\"&IF($V290=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T290,activeElevation),\"\"))","v":""},{"$f":"IF($T290=\"Select Model\",\"\",IF($T290=\"ACBC_1W\",calcQwIP($Y290,$W290,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC290,BD290,\"capacity\",$U290&\"P\"&IF($V290=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T290,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y290,$W290,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC290,BD290,\"capacity\",$U290&\"P\"&IF($V290=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T290,activeElevation)))","v":""},"",{"$f":"IF(T290=\"Select Model\", 0,waterPressureDrop(W290, U290 & \"P\" & IF(V290=\"Dual\",2,1) &\"C\", AC290, \"cooling\", T290))","v":0},{"$f":"IF(T290=\"Select Model\", \"\",getReturnWaterTemp(T290,AC290, activeEWTCooling, AS290, \"cooling\"))","v":""},"",{"$f":"IF($T290<>\"ACBC_1W\",\"\",IF($J290=\"\",\"\",FintubeCapacity($T290,$W290,$AE290,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T290=\"Select Model\",T290=\"PCBL\"),\"\",calcQwIP(Y290,W290,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD290,BD290,\"capacity\",U290&\"P\"&IF(V290=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T290,activeElevation))","v":""},"",{"$f":"IF(OR(T290=\"Select Model\",T290=\"PCBL\"), \"\",IF(AY290=0,\"N/A\",waterPressureDrop(W290, U290 & \"P\" & IF(V290=\"Dual\",2,1) &\"C\", AD290, \"heating\", T290)))","v":""},{"$f":"IF(OR(T290=\"Select Model\",T290=\"PCBL\"), \"\",IF(AY290=0,getReturnWaterTemp(T290,AE290, activeEWTHeating, AX290, \"heating\"),getReturnWaterTemp(T290,AD290, activeEWTHeating, AY290, \"heating\")))","v":""},"",{"$f":" getNozzle(T290, W290, Y290, Z290, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I291)),I291<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I291, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H291)),H291<0),\"\",intlEstQuantity(T291, W291*12, H291)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T291=\"Select Model\",\"\",coilCircuitChange(W291, U291, AC291, T291,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T291=\"Select Model\",\"\",beamWidth(T291))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T291=\"Select Model\",T291=\"PCBL\"), 0,getSPIP(T291, W291, Y291, BD291, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T291=\"Select Model\", \"\",IF(T291=\"PCBL\",0,primaryAirSensibleCapacityIP($T291,$W291,activeRoomTempCooling,activePriAirTempCooling,$Y291,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T291=\"Select Model\",\"\",IF($T291=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y291,activeElevation)))","v":""},{"$f":"IF(OR(T291=\"Select Model\",T291=\"PCBL\"), 0,IF(AD291=0,0,-primaryAirSensibleCapacityIP($T291,$W291,activeRoomTempHeating,activePriAirTempHeating,$Y291,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T291=\"Select Model\", \"\", InductionRatio($T291,BD291,$W291,$Y291)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T291=\"Select Model\", \"\",IF($T291=\"PCBL\",\"N/A\",minVAVSetBack(AA291, Y291))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T291=\"Select Model\", \"\",IF($T291= \"PCBL\",\"N/A\",getDischargeAirTemp($T291,$V291,$AC291,$W291,BD291,$AL291, $Y291, $AS291, \"cooling\",activeElevation,$AB291,$AJ291,$AV291,$BB291))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T291=\"Select Model\",$T291=\"PCBL\"), \"\",getDischargeAirTemp($T291,$V291,$AD291,$W291,BD291,$AL291, $Y291, $AY291, \"heating\",activeElevation,$AB291,$AJ291,$AV291,$BB291)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T291=\"Select Model\", \"\",IF(OR($T291=\"ACBC_1W\",$T291=\"ACBC_2W\",LEFT($T291,4)=\"ACBR\",$T291 = \"LIU24_2W\",LEFT($T291,3)=\"RIU\",LEFT($T291,6)=\"ACBL12\"), IF((soundLevel($T291, $AB291, BD291, $Y291, $W291,$AJ291,$AA291,\"dba\"))<15,\"<15\",soundLevel($T291, $AB291, BD291, $Y291, $W291,$AJ291,$AA291,\"dba\")+0.4),IF((soundLevel($T291, $AB291, BD291, $Y291, $W291,$AJ291,$AA291,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T291, $AB291, BD291, $Y291, $W291,$AJ291,$AA291,\"dba\")+5)<15, \"<15\", soundLevel($T291, $AB291, BD291,$Y291, $W291,$AJ291,$AA291,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T291=\"Select Model\", \"\",IF(OR($T291=\"ACBC_1W\",$T291=\"ACBC_2W\",LEFT($T291,4)=\"ACBR\",$T291=\"LIU24_2W\",LEFT($T291,3)=\"RIU\",LEFT($T291,6)=\"ACBL12\"), IF((soundLevel($T291, $AB291, BD291, $Y291, $W291,$AJ291,$AA291,\"NC\"))<15,\"<15\",soundLevel($T291, $AB291, BD291, $Y291, $W291,$AJ291,$AA291,\"NC\")+0.4),IF((soundLevel($T291, $AB291, BD291, $Y291, $W291,$AJ291,$AA291,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T291, $AB291, BD291, $Y291, $W291,$AJ291,$AA291,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T291, $AB291, BD291, $Y291, $W291,$AJ291,$AA291,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T291=\"Select Model\",\"\",IF($T291=\"LIU24_2W\",calcQwIP($Y291,$W291,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC291,$AI291,\"latent\",$U291&\"P\"&IF($V291=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T291,activeElevation),\"\"))","v":""},{"$f":"IF($T291=\"Select Model\",\"\",IF($T291=\"ACBC_1W\",calcQwIP($Y291,$W291,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC291,BD291,\"capacity\",$U291&\"P\"&IF($V291=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T291,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y291,$W291,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC291,BD291,\"capacity\",$U291&\"P\"&IF($V291=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T291,activeElevation)))","v":""},"",{"$f":"IF(T291=\"Select Model\", 0,waterPressureDrop(W291, U291 & \"P\" & IF(V291=\"Dual\",2,1) &\"C\", AC291, \"cooling\", T291))","v":0},{"$f":"IF(T291=\"Select Model\", \"\",getReturnWaterTemp(T291,AC291, activeEWTCooling, AS291, \"cooling\"))","v":""},"",{"$f":"IF($T291<>\"ACBC_1W\",\"\",IF($J291=\"\",\"\",FintubeCapacity($T291,$W291,$AE291,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T291=\"Select Model\",T291=\"PCBL\"),\"\",calcQwIP(Y291,W291,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD291,BD291,\"capacity\",U291&\"P\"&IF(V291=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T291,activeElevation))","v":""},"",{"$f":"IF(OR(T291=\"Select Model\",T291=\"PCBL\"), \"\",IF(AY291=0,\"N/A\",waterPressureDrop(W291, U291 & \"P\" & IF(V291=\"Dual\",2,1) &\"C\", AD291, \"heating\", T291)))","v":""},{"$f":"IF(OR(T291=\"Select Model\",T291=\"PCBL\"), \"\",IF(AY291=0,getReturnWaterTemp(T291,AE291, activeEWTHeating, AX291, \"heating\"),getReturnWaterTemp(T291,AD291, activeEWTHeating, AY291, \"heating\")))","v":""},"",{"$f":" getNozzle(T291, W291, Y291, Z291, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I292)),I292<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I292, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H292)),H292<0),\"\",intlEstQuantity(T292, W292*12, H292)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T292=\"Select Model\",\"\",coilCircuitChange(W292, U292, AC292, T292,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T292=\"Select Model\",\"\",beamWidth(T292))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T292=\"Select Model\",T292=\"PCBL\"), 0,getSPIP(T292, W292, Y292, BD292, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T292=\"Select Model\", \"\",IF(T292=\"PCBL\",0,primaryAirSensibleCapacityIP($T292,$W292,activeRoomTempCooling,activePriAirTempCooling,$Y292,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T292=\"Select Model\",\"\",IF($T292=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y292,activeElevation)))","v":""},{"$f":"IF(OR(T292=\"Select Model\",T292=\"PCBL\"), 0,IF(AD292=0,0,-primaryAirSensibleCapacityIP($T292,$W292,activeRoomTempHeating,activePriAirTempHeating,$Y292,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T292=\"Select Model\", \"\", InductionRatio($T292,BD292,$W292,$Y292)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T292=\"Select Model\", \"\",IF($T292=\"PCBL\",\"N/A\",minVAVSetBack(AA292, Y292))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T292=\"Select Model\", \"\",IF($T292= \"PCBL\",\"N/A\",getDischargeAirTemp($T292,$V292,$AC292,$W292,BD292,$AL292, $Y292, $AS292, \"cooling\",activeElevation,$AB292,$AJ292,$AV292,$BB292))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T292=\"Select Model\",$T292=\"PCBL\"), \"\",getDischargeAirTemp($T292,$V292,$AD292,$W292,BD292,$AL292, $Y292, $AY292, \"heating\",activeElevation,$AB292,$AJ292,$AV292,$BB292)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T292=\"Select Model\", \"\",IF(OR($T292=\"ACBC_1W\",$T292=\"ACBC_2W\",LEFT($T292,4)=\"ACBR\",$T292 = \"LIU24_2W\",LEFT($T292,3)=\"RIU\",LEFT($T292,6)=\"ACBL12\"), IF((soundLevel($T292, $AB292, BD292, $Y292, $W292,$AJ292,$AA292,\"dba\"))<15,\"<15\",soundLevel($T292, $AB292, BD292, $Y292, $W292,$AJ292,$AA292,\"dba\")+0.4),IF((soundLevel($T292, $AB292, BD292, $Y292, $W292,$AJ292,$AA292,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T292, $AB292, BD292, $Y292, $W292,$AJ292,$AA292,\"dba\")+5)<15, \"<15\", soundLevel($T292, $AB292, BD292,$Y292, $W292,$AJ292,$AA292,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T292=\"Select Model\", \"\",IF(OR($T292=\"ACBC_1W\",$T292=\"ACBC_2W\",LEFT($T292,4)=\"ACBR\",$T292=\"LIU24_2W\",LEFT($T292,3)=\"RIU\",LEFT($T292,6)=\"ACBL12\"), IF((soundLevel($T292, $AB292, BD292, $Y292, $W292,$AJ292,$AA292,\"NC\"))<15,\"<15\",soundLevel($T292, $AB292, BD292, $Y292, $W292,$AJ292,$AA292,\"NC\")+0.4),IF((soundLevel($T292, $AB292, BD292, $Y292, $W292,$AJ292,$AA292,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T292, $AB292, BD292, $Y292, $W292,$AJ292,$AA292,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T292, $AB292, BD292, $Y292, $W292,$AJ292,$AA292,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T292=\"Select Model\",\"\",IF($T292=\"LIU24_2W\",calcQwIP($Y292,$W292,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC292,$AI292,\"latent\",$U292&\"P\"&IF($V292=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T292,activeElevation),\"\"))","v":""},{"$f":"IF($T292=\"Select Model\",\"\",IF($T292=\"ACBC_1W\",calcQwIP($Y292,$W292,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC292,BD292,\"capacity\",$U292&\"P\"&IF($V292=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T292,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y292,$W292,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC292,BD292,\"capacity\",$U292&\"P\"&IF($V292=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T292,activeElevation)))","v":""},"",{"$f":"IF(T292=\"Select Model\", 0,waterPressureDrop(W292, U292 & \"P\" & IF(V292=\"Dual\",2,1) &\"C\", AC292, \"cooling\", T292))","v":0},{"$f":"IF(T292=\"Select Model\", \"\",getReturnWaterTemp(T292,AC292, activeEWTCooling, AS292, \"cooling\"))","v":""},"",{"$f":"IF($T292<>\"ACBC_1W\",\"\",IF($J292=\"\",\"\",FintubeCapacity($T292,$W292,$AE292,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T292=\"Select Model\",T292=\"PCBL\"),\"\",calcQwIP(Y292,W292,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD292,BD292,\"capacity\",U292&\"P\"&IF(V292=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T292,activeElevation))","v":""},"",{"$f":"IF(OR(T292=\"Select Model\",T292=\"PCBL\"), \"\",IF(AY292=0,\"N/A\",waterPressureDrop(W292, U292 & \"P\" & IF(V292=\"Dual\",2,1) &\"C\", AD292, \"heating\", T292)))","v":""},{"$f":"IF(OR(T292=\"Select Model\",T292=\"PCBL\"), \"\",IF(AY292=0,getReturnWaterTemp(T292,AE292, activeEWTHeating, AX292, \"heating\"),getReturnWaterTemp(T292,AD292, activeEWTHeating, AY292, \"heating\")))","v":""},"",{"$f":" getNozzle(T292, W292, Y292, Z292, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I293)),I293<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I293, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H293)),H293<0),\"\",intlEstQuantity(T293, W293*12, H293)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T293=\"Select Model\",\"\",coilCircuitChange(W293, U293, AC293, T293,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T293=\"Select Model\",\"\",beamWidth(T293))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T293=\"Select Model\",T293=\"PCBL\"), 0,getSPIP(T293, W293, Y293, BD293, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T293=\"Select Model\", \"\",IF(T293=\"PCBL\",0,primaryAirSensibleCapacityIP($T293,$W293,activeRoomTempCooling,activePriAirTempCooling,$Y293,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T293=\"Select Model\",\"\",IF($T293=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y293,activeElevation)))","v":""},{"$f":"IF(OR(T293=\"Select Model\",T293=\"PCBL\"), 0,IF(AD293=0,0,-primaryAirSensibleCapacityIP($T293,$W293,activeRoomTempHeating,activePriAirTempHeating,$Y293,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T293=\"Select Model\", \"\", InductionRatio($T293,BD293,$W293,$Y293)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T293=\"Select Model\", \"\",IF($T293=\"PCBL\",\"N/A\",minVAVSetBack(AA293, Y293))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T293=\"Select Model\", \"\",IF($T293= \"PCBL\",\"N/A\",getDischargeAirTemp($T293,$V293,$AC293,$W293,BD293,$AL293, $Y293, $AS293, \"cooling\",activeElevation,$AB293,$AJ293,$AV293,$BB293))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T293=\"Select Model\",$T293=\"PCBL\"), \"\",getDischargeAirTemp($T293,$V293,$AD293,$W293,BD293,$AL293, $Y293, $AY293, \"heating\",activeElevation,$AB293,$AJ293,$AV293,$BB293)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T293=\"Select Model\", \"\",IF(OR($T293=\"ACBC_1W\",$T293=\"ACBC_2W\",LEFT($T293,4)=\"ACBR\",$T293 = \"LIU24_2W\",LEFT($T293,3)=\"RIU\",LEFT($T293,6)=\"ACBL12\"), IF((soundLevel($T293, $AB293, BD293, $Y293, $W293,$AJ293,$AA293,\"dba\"))<15,\"<15\",soundLevel($T293, $AB293, BD293, $Y293, $W293,$AJ293,$AA293,\"dba\")+0.4),IF((soundLevel($T293, $AB293, BD293, $Y293, $W293,$AJ293,$AA293,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T293, $AB293, BD293, $Y293, $W293,$AJ293,$AA293,\"dba\")+5)<15, \"<15\", soundLevel($T293, $AB293, BD293,$Y293, $W293,$AJ293,$AA293,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T293=\"Select Model\", \"\",IF(OR($T293=\"ACBC_1W\",$T293=\"ACBC_2W\",LEFT($T293,4)=\"ACBR\",$T293=\"LIU24_2W\",LEFT($T293,3)=\"RIU\",LEFT($T293,6)=\"ACBL12\"), IF((soundLevel($T293, $AB293, BD293, $Y293, $W293,$AJ293,$AA293,\"NC\"))<15,\"<15\",soundLevel($T293, $AB293, BD293, $Y293, $W293,$AJ293,$AA293,\"NC\")+0.4),IF((soundLevel($T293, $AB293, BD293, $Y293, $W293,$AJ293,$AA293,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T293, $AB293, BD293, $Y293, $W293,$AJ293,$AA293,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T293, $AB293, BD293, $Y293, $W293,$AJ293,$AA293,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T293=\"Select Model\",\"\",IF($T293=\"LIU24_2W\",calcQwIP($Y293,$W293,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC293,$AI293,\"latent\",$U293&\"P\"&IF($V293=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T293,activeElevation),\"\"))","v":""},{"$f":"IF($T293=\"Select Model\",\"\",IF($T293=\"ACBC_1W\",calcQwIP($Y293,$W293,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC293,BD293,\"capacity\",$U293&\"P\"&IF($V293=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T293,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y293,$W293,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC293,BD293,\"capacity\",$U293&\"P\"&IF($V293=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T293,activeElevation)))","v":""},"",{"$f":"IF(T293=\"Select Model\", 0,waterPressureDrop(W293, U293 & \"P\" & IF(V293=\"Dual\",2,1) &\"C\", AC293, \"cooling\", T293))","v":0},{"$f":"IF(T293=\"Select Model\", \"\",getReturnWaterTemp(T293,AC293, activeEWTCooling, AS293, \"cooling\"))","v":""},"",{"$f":"IF($T293<>\"ACBC_1W\",\"\",IF($J293=\"\",\"\",FintubeCapacity($T293,$W293,$AE293,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T293=\"Select Model\",T293=\"PCBL\"),\"\",calcQwIP(Y293,W293,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD293,BD293,\"capacity\",U293&\"P\"&IF(V293=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T293,activeElevation))","v":""},"",{"$f":"IF(OR(T293=\"Select Model\",T293=\"PCBL\"), \"\",IF(AY293=0,\"N/A\",waterPressureDrop(W293, U293 & \"P\" & IF(V293=\"Dual\",2,1) &\"C\", AD293, \"heating\", T293)))","v":""},{"$f":"IF(OR(T293=\"Select Model\",T293=\"PCBL\"), \"\",IF(AY293=0,getReturnWaterTemp(T293,AE293, activeEWTHeating, AX293, \"heating\"),getReturnWaterTemp(T293,AD293, activeEWTHeating, AY293, \"heating\")))","v":""},"",{"$f":" getNozzle(T293, W293, Y293, Z293, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I294)),I294<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I294, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H294)),H294<0),\"\",intlEstQuantity(T294, W294*12, H294)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T294=\"Select Model\",\"\",coilCircuitChange(W294, U294, AC294, T294,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T294=\"Select Model\",\"\",beamWidth(T294))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T294=\"Select Model\",T294=\"PCBL\"), 0,getSPIP(T294, W294, Y294, BD294, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T294=\"Select Model\", \"\",IF(T294=\"PCBL\",0,primaryAirSensibleCapacityIP($T294,$W294,activeRoomTempCooling,activePriAirTempCooling,$Y294,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T294=\"Select Model\",\"\",IF($T294=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y294,activeElevation)))","v":""},{"$f":"IF(OR(T294=\"Select Model\",T294=\"PCBL\"), 0,IF(AD294=0,0,-primaryAirSensibleCapacityIP($T294,$W294,activeRoomTempHeating,activePriAirTempHeating,$Y294,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T294=\"Select Model\", \"\", InductionRatio($T294,BD294,$W294,$Y294)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T294=\"Select Model\", \"\",IF($T294=\"PCBL\",\"N/A\",minVAVSetBack(AA294, Y294))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T294=\"Select Model\", \"\",IF($T294= \"PCBL\",\"N/A\",getDischargeAirTemp($T294,$V294,$AC294,$W294,BD294,$AL294, $Y294, $AS294, \"cooling\",activeElevation,$AB294,$AJ294,$AV294,$BB294))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T294=\"Select Model\",$T294=\"PCBL\"), \"\",getDischargeAirTemp($T294,$V294,$AD294,$W294,BD294,$AL294, $Y294, $AY294, \"heating\",activeElevation,$AB294,$AJ294,$AV294,$BB294)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T294=\"Select Model\", \"\",IF(OR($T294=\"ACBC_1W\",$T294=\"ACBC_2W\",LEFT($T294,4)=\"ACBR\",$T294 = \"LIU24_2W\",LEFT($T294,3)=\"RIU\",LEFT($T294,6)=\"ACBL12\"), IF((soundLevel($T294, $AB294, BD294, $Y294, $W294,$AJ294,$AA294,\"dba\"))<15,\"<15\",soundLevel($T294, $AB294, BD294, $Y294, $W294,$AJ294,$AA294,\"dba\")+0.4),IF((soundLevel($T294, $AB294, BD294, $Y294, $W294,$AJ294,$AA294,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T294, $AB294, BD294, $Y294, $W294,$AJ294,$AA294,\"dba\")+5)<15, \"<15\", soundLevel($T294, $AB294, BD294,$Y294, $W294,$AJ294,$AA294,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T294=\"Select Model\", \"\",IF(OR($T294=\"ACBC_1W\",$T294=\"ACBC_2W\",LEFT($T294,4)=\"ACBR\",$T294=\"LIU24_2W\",LEFT($T294,3)=\"RIU\",LEFT($T294,6)=\"ACBL12\"), IF((soundLevel($T294, $AB294, BD294, $Y294, $W294,$AJ294,$AA294,\"NC\"))<15,\"<15\",soundLevel($T294, $AB294, BD294, $Y294, $W294,$AJ294,$AA294,\"NC\")+0.4),IF((soundLevel($T294, $AB294, BD294, $Y294, $W294,$AJ294,$AA294,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T294, $AB294, BD294, $Y294, $W294,$AJ294,$AA294,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T294, $AB294, BD294, $Y294, $W294,$AJ294,$AA294,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T294=\"Select Model\",\"\",IF($T294=\"LIU24_2W\",calcQwIP($Y294,$W294,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC294,$AI294,\"latent\",$U294&\"P\"&IF($V294=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T294,activeElevation),\"\"))","v":""},{"$f":"IF($T294=\"Select Model\",\"\",IF($T294=\"ACBC_1W\",calcQwIP($Y294,$W294,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC294,BD294,\"capacity\",$U294&\"P\"&IF($V294=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T294,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y294,$W294,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC294,BD294,\"capacity\",$U294&\"P\"&IF($V294=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T294,activeElevation)))","v":""},"",{"$f":"IF(T294=\"Select Model\", 0,waterPressureDrop(W294, U294 & \"P\" & IF(V294=\"Dual\",2,1) &\"C\", AC294, \"cooling\", T294))","v":0},{"$f":"IF(T294=\"Select Model\", \"\",getReturnWaterTemp(T294,AC294, activeEWTCooling, AS294, \"cooling\"))","v":""},"",{"$f":"IF($T294<>\"ACBC_1W\",\"\",IF($J294=\"\",\"\",FintubeCapacity($T294,$W294,$AE294,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T294=\"Select Model\",T294=\"PCBL\"),\"\",calcQwIP(Y294,W294,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD294,BD294,\"capacity\",U294&\"P\"&IF(V294=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T294,activeElevation))","v":""},"",{"$f":"IF(OR(T294=\"Select Model\",T294=\"PCBL\"), \"\",IF(AY294=0,\"N/A\",waterPressureDrop(W294, U294 & \"P\" & IF(V294=\"Dual\",2,1) &\"C\", AD294, \"heating\", T294)))","v":""},{"$f":"IF(OR(T294=\"Select Model\",T294=\"PCBL\"), \"\",IF(AY294=0,getReturnWaterTemp(T294,AE294, activeEWTHeating, AX294, \"heating\"),getReturnWaterTemp(T294,AD294, activeEWTHeating, AY294, \"heating\")))","v":""},"",{"$f":" getNozzle(T294, W294, Y294, Z294, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I295)),I295<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I295, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H295)),H295<0),\"\",intlEstQuantity(T295, W295*12, H295)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T295=\"Select Model\",\"\",coilCircuitChange(W295, U295, AC295, T295,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T295=\"Select Model\",\"\",beamWidth(T295))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T295=\"Select Model\",T295=\"PCBL\"), 0,getSPIP(T295, W295, Y295, BD295, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T295=\"Select Model\", \"\",IF(T295=\"PCBL\",0,primaryAirSensibleCapacityIP($T295,$W295,activeRoomTempCooling,activePriAirTempCooling,$Y295,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T295=\"Select Model\",\"\",IF($T295=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y295,activeElevation)))","v":""},{"$f":"IF(OR(T295=\"Select Model\",T295=\"PCBL\"), 0,IF(AD295=0,0,-primaryAirSensibleCapacityIP($T295,$W295,activeRoomTempHeating,activePriAirTempHeating,$Y295,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T295=\"Select Model\", \"\", InductionRatio($T295,BD295,$W295,$Y295)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T295=\"Select Model\", \"\",IF($T295=\"PCBL\",\"N/A\",minVAVSetBack(AA295, Y295))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T295=\"Select Model\", \"\",IF($T295= \"PCBL\",\"N/A\",getDischargeAirTemp($T295,$V295,$AC295,$W295,BD295,$AL295, $Y295, $AS295, \"cooling\",activeElevation,$AB295,$AJ295,$AV295,$BB295))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T295=\"Select Model\",$T295=\"PCBL\"), \"\",getDischargeAirTemp($T295,$V295,$AD295,$W295,BD295,$AL295, $Y295, $AY295, \"heating\",activeElevation,$AB295,$AJ295,$AV295,$BB295)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T295=\"Select Model\", \"\",IF(OR($T295=\"ACBC_1W\",$T295=\"ACBC_2W\",LEFT($T295,4)=\"ACBR\",$T295 = \"LIU24_2W\",LEFT($T295,3)=\"RIU\",LEFT($T295,6)=\"ACBL12\"), IF((soundLevel($T295, $AB295, BD295, $Y295, $W295,$AJ295,$AA295,\"dba\"))<15,\"<15\",soundLevel($T295, $AB295, BD295, $Y295, $W295,$AJ295,$AA295,\"dba\")+0.4),IF((soundLevel($T295, $AB295, BD295, $Y295, $W295,$AJ295,$AA295,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T295, $AB295, BD295, $Y295, $W295,$AJ295,$AA295,\"dba\")+5)<15, \"<15\", soundLevel($T295, $AB295, BD295,$Y295, $W295,$AJ295,$AA295,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T295=\"Select Model\", \"\",IF(OR($T295=\"ACBC_1W\",$T295=\"ACBC_2W\",LEFT($T295,4)=\"ACBR\",$T295=\"LIU24_2W\",LEFT($T295,3)=\"RIU\",LEFT($T295,6)=\"ACBL12\"), IF((soundLevel($T295, $AB295, BD295, $Y295, $W295,$AJ295,$AA295,\"NC\"))<15,\"<15\",soundLevel($T295, $AB295, BD295, $Y295, $W295,$AJ295,$AA295,\"NC\")+0.4),IF((soundLevel($T295, $AB295, BD295, $Y295, $W295,$AJ295,$AA295,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T295, $AB295, BD295, $Y295, $W295,$AJ295,$AA295,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T295, $AB295, BD295, $Y295, $W295,$AJ295,$AA295,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T295=\"Select Model\",\"\",IF($T295=\"LIU24_2W\",calcQwIP($Y295,$W295,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC295,$AI295,\"latent\",$U295&\"P\"&IF($V295=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T295,activeElevation),\"\"))","v":""},{"$f":"IF($T295=\"Select Model\",\"\",IF($T295=\"ACBC_1W\",calcQwIP($Y295,$W295,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC295,BD295,\"capacity\",$U295&\"P\"&IF($V295=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T295,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y295,$W295,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC295,BD295,\"capacity\",$U295&\"P\"&IF($V295=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T295,activeElevation)))","v":""},"",{"$f":"IF(T295=\"Select Model\", 0,waterPressureDrop(W295, U295 & \"P\" & IF(V295=\"Dual\",2,1) &\"C\", AC295, \"cooling\", T295))","v":0},{"$f":"IF(T295=\"Select Model\", \"\",getReturnWaterTemp(T295,AC295, activeEWTCooling, AS295, \"cooling\"))","v":""},"",{"$f":"IF($T295<>\"ACBC_1W\",\"\",IF($J295=\"\",\"\",FintubeCapacity($T295,$W295,$AE295,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T295=\"Select Model\",T295=\"PCBL\"),\"\",calcQwIP(Y295,W295,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD295,BD295,\"capacity\",U295&\"P\"&IF(V295=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T295,activeElevation))","v":""},"",{"$f":"IF(OR(T295=\"Select Model\",T295=\"PCBL\"), \"\",IF(AY295=0,\"N/A\",waterPressureDrop(W295, U295 & \"P\" & IF(V295=\"Dual\",2,1) &\"C\", AD295, \"heating\", T295)))","v":""},{"$f":"IF(OR(T295=\"Select Model\",T295=\"PCBL\"), \"\",IF(AY295=0,getReturnWaterTemp(T295,AE295, activeEWTHeating, AX295, \"heating\"),getReturnWaterTemp(T295,AD295, activeEWTHeating, AY295, \"heating\")))","v":""},"",{"$f":" getNozzle(T295, W295, Y295, Z295, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I296)),I296<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I296, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H296)),H296<0),\"\",intlEstQuantity(T296, W296*12, H296)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T296=\"Select Model\",\"\",coilCircuitChange(W296, U296, AC296, T296,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T296=\"Select Model\",\"\",beamWidth(T296))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T296=\"Select Model\",T296=\"PCBL\"), 0,getSPIP(T296, W296, Y296, BD296, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T296=\"Select Model\", \"\",IF(T296=\"PCBL\",0,primaryAirSensibleCapacityIP($T296,$W296,activeRoomTempCooling,activePriAirTempCooling,$Y296,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T296=\"Select Model\",\"\",IF($T296=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y296,activeElevation)))","v":""},{"$f":"IF(OR(T296=\"Select Model\",T296=\"PCBL\"), 0,IF(AD296=0,0,-primaryAirSensibleCapacityIP($T296,$W296,activeRoomTempHeating,activePriAirTempHeating,$Y296,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T296=\"Select Model\", \"\", InductionRatio($T296,BD296,$W296,$Y296)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T296=\"Select Model\", \"\",IF($T296=\"PCBL\",\"N/A\",minVAVSetBack(AA296, Y296))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T296=\"Select Model\", \"\",IF($T296= \"PCBL\",\"N/A\",getDischargeAirTemp($T296,$V296,$AC296,$W296,BD296,$AL296, $Y296, $AS296, \"cooling\",activeElevation,$AB296,$AJ296,$AV296,$BB296))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T296=\"Select Model\",$T296=\"PCBL\"), \"\",getDischargeAirTemp($T296,$V296,$AD296,$W296,BD296,$AL296, $Y296, $AY296, \"heating\",activeElevation,$AB296,$AJ296,$AV296,$BB296)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T296=\"Select Model\", \"\",IF(OR($T296=\"ACBC_1W\",$T296=\"ACBC_2W\",LEFT($T296,4)=\"ACBR\",$T296 = \"LIU24_2W\",LEFT($T296,3)=\"RIU\",LEFT($T296,6)=\"ACBL12\"), IF((soundLevel($T296, $AB296, BD296, $Y296, $W296,$AJ296,$AA296,\"dba\"))<15,\"<15\",soundLevel($T296, $AB296, BD296, $Y296, $W296,$AJ296,$AA296,\"dba\")+0.4),IF((soundLevel($T296, $AB296, BD296, $Y296, $W296,$AJ296,$AA296,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T296, $AB296, BD296, $Y296, $W296,$AJ296,$AA296,\"dba\")+5)<15, \"<15\", soundLevel($T296, $AB296, BD296,$Y296, $W296,$AJ296,$AA296,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T296=\"Select Model\", \"\",IF(OR($T296=\"ACBC_1W\",$T296=\"ACBC_2W\",LEFT($T296,4)=\"ACBR\",$T296=\"LIU24_2W\",LEFT($T296,3)=\"RIU\",LEFT($T296,6)=\"ACBL12\"), IF((soundLevel($T296, $AB296, BD296, $Y296, $W296,$AJ296,$AA296,\"NC\"))<15,\"<15\",soundLevel($T296, $AB296, BD296, $Y296, $W296,$AJ296,$AA296,\"NC\")+0.4),IF((soundLevel($T296, $AB296, BD296, $Y296, $W296,$AJ296,$AA296,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T296, $AB296, BD296, $Y296, $W296,$AJ296,$AA296,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T296, $AB296, BD296, $Y296, $W296,$AJ296,$AA296,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T296=\"Select Model\",\"\",IF($T296=\"LIU24_2W\",calcQwIP($Y296,$W296,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC296,$AI296,\"latent\",$U296&\"P\"&IF($V296=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T296,activeElevation),\"\"))","v":""},{"$f":"IF($T296=\"Select Model\",\"\",IF($T296=\"ACBC_1W\",calcQwIP($Y296,$W296,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC296,BD296,\"capacity\",$U296&\"P\"&IF($V296=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T296,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y296,$W296,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC296,BD296,\"capacity\",$U296&\"P\"&IF($V296=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T296,activeElevation)))","v":""},"",{"$f":"IF(T296=\"Select Model\", 0,waterPressureDrop(W296, U296 & \"P\" & IF(V296=\"Dual\",2,1) &\"C\", AC296, \"cooling\", T296))","v":0},{"$f":"IF(T296=\"Select Model\", \"\",getReturnWaterTemp(T296,AC296, activeEWTCooling, AS296, \"cooling\"))","v":""},"",{"$f":"IF($T296<>\"ACBC_1W\",\"\",IF($J296=\"\",\"\",FintubeCapacity($T296,$W296,$AE296,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T296=\"Select Model\",T296=\"PCBL\"),\"\",calcQwIP(Y296,W296,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD296,BD296,\"capacity\",U296&\"P\"&IF(V296=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T296,activeElevation))","v":""},"",{"$f":"IF(OR(T296=\"Select Model\",T296=\"PCBL\"), \"\",IF(AY296=0,\"N/A\",waterPressureDrop(W296, U296 & \"P\" & IF(V296=\"Dual\",2,1) &\"C\", AD296, \"heating\", T296)))","v":""},{"$f":"IF(OR(T296=\"Select Model\",T296=\"PCBL\"), \"\",IF(AY296=0,getReturnWaterTemp(T296,AE296, activeEWTHeating, AX296, \"heating\"),getReturnWaterTemp(T296,AD296, activeEWTHeating, AY296, \"heating\")))","v":""},"",{"$f":" getNozzle(T296, W296, Y296, Z296, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I297)),I297<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I297, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H297)),H297<0),\"\",intlEstQuantity(T297, W297*12, H297)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T297=\"Select Model\",\"\",coilCircuitChange(W297, U297, AC297, T297,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T297=\"Select Model\",\"\",beamWidth(T297))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T297=\"Select Model\",T297=\"PCBL\"), 0,getSPIP(T297, W297, Y297, BD297, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T297=\"Select Model\", \"\",IF(T297=\"PCBL\",0,primaryAirSensibleCapacityIP($T297,$W297,activeRoomTempCooling,activePriAirTempCooling,$Y297,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T297=\"Select Model\",\"\",IF($T297=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y297,activeElevation)))","v":""},{"$f":"IF(OR(T297=\"Select Model\",T297=\"PCBL\"), 0,IF(AD297=0,0,-primaryAirSensibleCapacityIP($T297,$W297,activeRoomTempHeating,activePriAirTempHeating,$Y297,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T297=\"Select Model\", \"\", InductionRatio($T297,BD297,$W297,$Y297)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T297=\"Select Model\", \"\",IF($T297=\"PCBL\",\"N/A\",minVAVSetBack(AA297, Y297))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T297=\"Select Model\", \"\",IF($T297= \"PCBL\",\"N/A\",getDischargeAirTemp($T297,$V297,$AC297,$W297,BD297,$AL297, $Y297, $AS297, \"cooling\",activeElevation,$AB297,$AJ297,$AV297,$BB297))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T297=\"Select Model\",$T297=\"PCBL\"), \"\",getDischargeAirTemp($T297,$V297,$AD297,$W297,BD297,$AL297, $Y297, $AY297, \"heating\",activeElevation,$AB297,$AJ297,$AV297,$BB297)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T297=\"Select Model\", \"\",IF(OR($T297=\"ACBC_1W\",$T297=\"ACBC_2W\",LEFT($T297,4)=\"ACBR\",$T297 = \"LIU24_2W\",LEFT($T297,3)=\"RIU\",LEFT($T297,6)=\"ACBL12\"), IF((soundLevel($T297, $AB297, BD297, $Y297, $W297,$AJ297,$AA297,\"dba\"))<15,\"<15\",soundLevel($T297, $AB297, BD297, $Y297, $W297,$AJ297,$AA297,\"dba\")+0.4),IF((soundLevel($T297, $AB297, BD297, $Y297, $W297,$AJ297,$AA297,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T297, $AB297, BD297, $Y297, $W297,$AJ297,$AA297,\"dba\")+5)<15, \"<15\", soundLevel($T297, $AB297, BD297,$Y297, $W297,$AJ297,$AA297,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T297=\"Select Model\", \"\",IF(OR($T297=\"ACBC_1W\",$T297=\"ACBC_2W\",LEFT($T297,4)=\"ACBR\",$T297=\"LIU24_2W\",LEFT($T297,3)=\"RIU\",LEFT($T297,6)=\"ACBL12\"), IF((soundLevel($T297, $AB297, BD297, $Y297, $W297,$AJ297,$AA297,\"NC\"))<15,\"<15\",soundLevel($T297, $AB297, BD297, $Y297, $W297,$AJ297,$AA297,\"NC\")+0.4),IF((soundLevel($T297, $AB297, BD297, $Y297, $W297,$AJ297,$AA297,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T297, $AB297, BD297, $Y297, $W297,$AJ297,$AA297,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T297, $AB297, BD297, $Y297, $W297,$AJ297,$AA297,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T297=\"Select Model\",\"\",IF($T297=\"LIU24_2W\",calcQwIP($Y297,$W297,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC297,$AI297,\"latent\",$U297&\"P\"&IF($V297=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T297,activeElevation),\"\"))","v":""},{"$f":"IF($T297=\"Select Model\",\"\",IF($T297=\"ACBC_1W\",calcQwIP($Y297,$W297,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC297,BD297,\"capacity\",$U297&\"P\"&IF($V297=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T297,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y297,$W297,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC297,BD297,\"capacity\",$U297&\"P\"&IF($V297=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T297,activeElevation)))","v":""},"",{"$f":"IF(T297=\"Select Model\", 0,waterPressureDrop(W297, U297 & \"P\" & IF(V297=\"Dual\",2,1) &\"C\", AC297, \"cooling\", T297))","v":0},{"$f":"IF(T297=\"Select Model\", \"\",getReturnWaterTemp(T297,AC297, activeEWTCooling, AS297, \"cooling\"))","v":""},"",{"$f":"IF($T297<>\"ACBC_1W\",\"\",IF($J297=\"\",\"\",FintubeCapacity($T297,$W297,$AE297,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T297=\"Select Model\",T297=\"PCBL\"),\"\",calcQwIP(Y297,W297,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD297,BD297,\"capacity\",U297&\"P\"&IF(V297=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T297,activeElevation))","v":""},"",{"$f":"IF(OR(T297=\"Select Model\",T297=\"PCBL\"), \"\",IF(AY297=0,\"N/A\",waterPressureDrop(W297, U297 & \"P\" & IF(V297=\"Dual\",2,1) &\"C\", AD297, \"heating\", T297)))","v":""},{"$f":"IF(OR(T297=\"Select Model\",T297=\"PCBL\"), \"\",IF(AY297=0,getReturnWaterTemp(T297,AE297, activeEWTHeating, AX297, \"heating\"),getReturnWaterTemp(T297,AD297, activeEWTHeating, AY297, \"heating\")))","v":""},"",{"$f":" getNozzle(T297, W297, Y297, Z297, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I298)),I298<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I298, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H298)),H298<0),\"\",intlEstQuantity(T298, W298*12, H298)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T298=\"Select Model\",\"\",coilCircuitChange(W298, U298, AC298, T298,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T298=\"Select Model\",\"\",beamWidth(T298))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T298=\"Select Model\",T298=\"PCBL\"), 0,getSPIP(T298, W298, Y298, BD298, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T298=\"Select Model\", \"\",IF(T298=\"PCBL\",0,primaryAirSensibleCapacityIP($T298,$W298,activeRoomTempCooling,activePriAirTempCooling,$Y298,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T298=\"Select Model\",\"\",IF($T298=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y298,activeElevation)))","v":""},{"$f":"IF(OR(T298=\"Select Model\",T298=\"PCBL\"), 0,IF(AD298=0,0,-primaryAirSensibleCapacityIP($T298,$W298,activeRoomTempHeating,activePriAirTempHeating,$Y298,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T298=\"Select Model\", \"\", InductionRatio($T298,BD298,$W298,$Y298)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T298=\"Select Model\", \"\",IF($T298=\"PCBL\",\"N/A\",minVAVSetBack(AA298, Y298))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T298=\"Select Model\", \"\",IF($T298= \"PCBL\",\"N/A\",getDischargeAirTemp($T298,$V298,$AC298,$W298,BD298,$AL298, $Y298, $AS298, \"cooling\",activeElevation,$AB298,$AJ298,$AV298,$BB298))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T298=\"Select Model\",$T298=\"PCBL\"), \"\",getDischargeAirTemp($T298,$V298,$AD298,$W298,BD298,$AL298, $Y298, $AY298, \"heating\",activeElevation,$AB298,$AJ298,$AV298,$BB298)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T298=\"Select Model\", \"\",IF(OR($T298=\"ACBC_1W\",$T298=\"ACBC_2W\",LEFT($T298,4)=\"ACBR\",$T298 = \"LIU24_2W\",LEFT($T298,3)=\"RIU\",LEFT($T298,6)=\"ACBL12\"), IF((soundLevel($T298, $AB298, BD298, $Y298, $W298,$AJ298,$AA298,\"dba\"))<15,\"<15\",soundLevel($T298, $AB298, BD298, $Y298, $W298,$AJ298,$AA298,\"dba\")+0.4),IF((soundLevel($T298, $AB298, BD298, $Y298, $W298,$AJ298,$AA298,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T298, $AB298, BD298, $Y298, $W298,$AJ298,$AA298,\"dba\")+5)<15, \"<15\", soundLevel($T298, $AB298, BD298,$Y298, $W298,$AJ298,$AA298,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T298=\"Select Model\", \"\",IF(OR($T298=\"ACBC_1W\",$T298=\"ACBC_2W\",LEFT($T298,4)=\"ACBR\",$T298=\"LIU24_2W\",LEFT($T298,3)=\"RIU\",LEFT($T298,6)=\"ACBL12\"), IF((soundLevel($T298, $AB298, BD298, $Y298, $W298,$AJ298,$AA298,\"NC\"))<15,\"<15\",soundLevel($T298, $AB298, BD298, $Y298, $W298,$AJ298,$AA298,\"NC\")+0.4),IF((soundLevel($T298, $AB298, BD298, $Y298, $W298,$AJ298,$AA298,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T298, $AB298, BD298, $Y298, $W298,$AJ298,$AA298,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T298, $AB298, BD298, $Y298, $W298,$AJ298,$AA298,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T298=\"Select Model\",\"\",IF($T298=\"LIU24_2W\",calcQwIP($Y298,$W298,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC298,$AI298,\"latent\",$U298&\"P\"&IF($V298=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T298,activeElevation),\"\"))","v":""},{"$f":"IF($T298=\"Select Model\",\"\",IF($T298=\"ACBC_1W\",calcQwIP($Y298,$W298,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC298,BD298,\"capacity\",$U298&\"P\"&IF($V298=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T298,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y298,$W298,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC298,BD298,\"capacity\",$U298&\"P\"&IF($V298=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T298,activeElevation)))","v":""},"",{"$f":"IF(T298=\"Select Model\", 0,waterPressureDrop(W298, U298 & \"P\" & IF(V298=\"Dual\",2,1) &\"C\", AC298, \"cooling\", T298))","v":0},{"$f":"IF(T298=\"Select Model\", \"\",getReturnWaterTemp(T298,AC298, activeEWTCooling, AS298, \"cooling\"))","v":""},"",{"$f":"IF($T298<>\"ACBC_1W\",\"\",IF($J298=\"\",\"\",FintubeCapacity($T298,$W298,$AE298,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T298=\"Select Model\",T298=\"PCBL\"),\"\",calcQwIP(Y298,W298,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD298,BD298,\"capacity\",U298&\"P\"&IF(V298=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T298,activeElevation))","v":""},"",{"$f":"IF(OR(T298=\"Select Model\",T298=\"PCBL\"), \"\",IF(AY298=0,\"N/A\",waterPressureDrop(W298, U298 & \"P\" & IF(V298=\"Dual\",2,1) &\"C\", AD298, \"heating\", T298)))","v":""},{"$f":"IF(OR(T298=\"Select Model\",T298=\"PCBL\"), \"\",IF(AY298=0,getReturnWaterTemp(T298,AE298, activeEWTHeating, AX298, \"heating\"),getReturnWaterTemp(T298,AD298, activeEWTHeating, AY298, \"heating\")))","v":""},"",{"$f":" getNozzle(T298, W298, Y298, Z298, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I299)),I299<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I299, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H299)),H299<0),\"\",intlEstQuantity(T299, W299*12, H299)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T299=\"Select Model\",\"\",coilCircuitChange(W299, U299, AC299, T299,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T299=\"Select Model\",\"\",beamWidth(T299))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T299=\"Select Model\",T299=\"PCBL\"), 0,getSPIP(T299, W299, Y299, BD299, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T299=\"Select Model\", \"\",IF(T299=\"PCBL\",0,primaryAirSensibleCapacityIP($T299,$W299,activeRoomTempCooling,activePriAirTempCooling,$Y299,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T299=\"Select Model\",\"\",IF($T299=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y299,activeElevation)))","v":""},{"$f":"IF(OR(T299=\"Select Model\",T299=\"PCBL\"), 0,IF(AD299=0,0,-primaryAirSensibleCapacityIP($T299,$W299,activeRoomTempHeating,activePriAirTempHeating,$Y299,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T299=\"Select Model\", \"\", InductionRatio($T299,BD299,$W299,$Y299)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T299=\"Select Model\", \"\",IF($T299=\"PCBL\",\"N/A\",minVAVSetBack(AA299, Y299))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T299=\"Select Model\", \"\",IF($T299= \"PCBL\",\"N/A\",getDischargeAirTemp($T299,$V299,$AC299,$W299,BD299,$AL299, $Y299, $AS299, \"cooling\",activeElevation,$AB299,$AJ299,$AV299,$BB299))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T299=\"Select Model\",$T299=\"PCBL\"), \"\",getDischargeAirTemp($T299,$V299,$AD299,$W299,BD299,$AL299, $Y299, $AY299, \"heating\",activeElevation,$AB299,$AJ299,$AV299,$BB299)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T299=\"Select Model\", \"\",IF(OR($T299=\"ACBC_1W\",$T299=\"ACBC_2W\",LEFT($T299,4)=\"ACBR\",$T299 = \"LIU24_2W\",LEFT($T299,3)=\"RIU\",LEFT($T299,6)=\"ACBL12\"), IF((soundLevel($T299, $AB299, BD299, $Y299, $W299,$AJ299,$AA299,\"dba\"))<15,\"<15\",soundLevel($T299, $AB299, BD299, $Y299, $W299,$AJ299,$AA299,\"dba\")+0.4),IF((soundLevel($T299, $AB299, BD299, $Y299, $W299,$AJ299,$AA299,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T299, $AB299, BD299, $Y299, $W299,$AJ299,$AA299,\"dba\")+5)<15, \"<15\", soundLevel($T299, $AB299, BD299,$Y299, $W299,$AJ299,$AA299,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T299=\"Select Model\", \"\",IF(OR($T299=\"ACBC_1W\",$T299=\"ACBC_2W\",LEFT($T299,4)=\"ACBR\",$T299=\"LIU24_2W\",LEFT($T299,3)=\"RIU\",LEFT($T299,6)=\"ACBL12\"), IF((soundLevel($T299, $AB299, BD299, $Y299, $W299,$AJ299,$AA299,\"NC\"))<15,\"<15\",soundLevel($T299, $AB299, BD299, $Y299, $W299,$AJ299,$AA299,\"NC\")+0.4),IF((soundLevel($T299, $AB299, BD299, $Y299, $W299,$AJ299,$AA299,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T299, $AB299, BD299, $Y299, $W299,$AJ299,$AA299,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T299, $AB299, BD299, $Y299, $W299,$AJ299,$AA299,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T299=\"Select Model\",\"\",IF($T299=\"LIU24_2W\",calcQwIP($Y299,$W299,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC299,$AI299,\"latent\",$U299&\"P\"&IF($V299=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T299,activeElevation),\"\"))","v":""},{"$f":"IF($T299=\"Select Model\",\"\",IF($T299=\"ACBC_1W\",calcQwIP($Y299,$W299,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC299,BD299,\"capacity\",$U299&\"P\"&IF($V299=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T299,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y299,$W299,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC299,BD299,\"capacity\",$U299&\"P\"&IF($V299=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T299,activeElevation)))","v":""},"",{"$f":"IF(T299=\"Select Model\", 0,waterPressureDrop(W299, U299 & \"P\" & IF(V299=\"Dual\",2,1) &\"C\", AC299, \"cooling\", T299))","v":0},{"$f":"IF(T299=\"Select Model\", \"\",getReturnWaterTemp(T299,AC299, activeEWTCooling, AS299, \"cooling\"))","v":""},"",{"$f":"IF($T299<>\"ACBC_1W\",\"\",IF($J299=\"\",\"\",FintubeCapacity($T299,$W299,$AE299,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T299=\"Select Model\",T299=\"PCBL\"),\"\",calcQwIP(Y299,W299,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD299,BD299,\"capacity\",U299&\"P\"&IF(V299=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T299,activeElevation))","v":""},"",{"$f":"IF(OR(T299=\"Select Model\",T299=\"PCBL\"), \"\",IF(AY299=0,\"N/A\",waterPressureDrop(W299, U299 & \"P\" & IF(V299=\"Dual\",2,1) &\"C\", AD299, \"heating\", T299)))","v":""},{"$f":"IF(OR(T299=\"Select Model\",T299=\"PCBL\"), \"\",IF(AY299=0,getReturnWaterTemp(T299,AE299, activeEWTHeating, AX299, \"heating\"),getReturnWaterTemp(T299,AD299, activeEWTHeating, AY299, \"heating\")))","v":""},"",{"$f":" getNozzle(T299, W299, Y299, Z299, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I300)),I300<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I300, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H300)),H300<0),\"\",intlEstQuantity(T300, W300*12, H300)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T300=\"Select Model\",\"\",coilCircuitChange(W300, U300, AC300, T300,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T300=\"Select Model\",\"\",beamWidth(T300))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T300=\"Select Model\",T300=\"PCBL\"), 0,getSPIP(T300, W300, Y300, BD300, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T300=\"Select Model\", \"\",IF(T300=\"PCBL\",0,primaryAirSensibleCapacityIP($T300,$W300,activeRoomTempCooling,activePriAirTempCooling,$Y300,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T300=\"Select Model\",\"\",IF($T300=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y300,activeElevation)))","v":""},{"$f":"IF(OR(T300=\"Select Model\",T300=\"PCBL\"), 0,IF(AD300=0,0,-primaryAirSensibleCapacityIP($T300,$W300,activeRoomTempHeating,activePriAirTempHeating,$Y300,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T300=\"Select Model\", \"\", InductionRatio($T300,BD300,$W300,$Y300)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T300=\"Select Model\", \"\",IF($T300=\"PCBL\",\"N/A\",minVAVSetBack(AA300, Y300))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T300=\"Select Model\", \"\",IF($T300= \"PCBL\",\"N/A\",getDischargeAirTemp($T300,$V300,$AC300,$W300,BD300,$AL300, $Y300, $AS300, \"cooling\",activeElevation,$AB300,$AJ300,$AV300,$BB300))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T300=\"Select Model\",$T300=\"PCBL\"), \"\",getDischargeAirTemp($T300,$V300,$AD300,$W300,BD300,$AL300, $Y300, $AY300, \"heating\",activeElevation,$AB300,$AJ300,$AV300,$BB300)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T300=\"Select Model\", \"\",IF(OR($T300=\"ACBC_1W\",$T300=\"ACBC_2W\",LEFT($T300,4)=\"ACBR\",$T300 = \"LIU24_2W\",LEFT($T300,3)=\"RIU\",LEFT($T300,6)=\"ACBL12\"), IF((soundLevel($T300, $AB300, BD300, $Y300, $W300,$AJ300,$AA300,\"dba\"))<15,\"<15\",soundLevel($T300, $AB300, BD300, $Y300, $W300,$AJ300,$AA300,\"dba\")+0.4),IF((soundLevel($T300, $AB300, BD300, $Y300, $W300,$AJ300,$AA300,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T300, $AB300, BD300, $Y300, $W300,$AJ300,$AA300,\"dba\")+5)<15, \"<15\", soundLevel($T300, $AB300, BD300,$Y300, $W300,$AJ300,$AA300,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T300=\"Select Model\", \"\",IF(OR($T300=\"ACBC_1W\",$T300=\"ACBC_2W\",LEFT($T300,4)=\"ACBR\",$T300=\"LIU24_2W\",LEFT($T300,3)=\"RIU\",LEFT($T300,6)=\"ACBL12\"), IF((soundLevel($T300, $AB300, BD300, $Y300, $W300,$AJ300,$AA300,\"NC\"))<15,\"<15\",soundLevel($T300, $AB300, BD300, $Y300, $W300,$AJ300,$AA300,\"NC\")+0.4),IF((soundLevel($T300, $AB300, BD300, $Y300, $W300,$AJ300,$AA300,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T300, $AB300, BD300, $Y300, $W300,$AJ300,$AA300,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T300, $AB300, BD300, $Y300, $W300,$AJ300,$AA300,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T300=\"Select Model\",\"\",IF($T300=\"LIU24_2W\",calcQwIP($Y300,$W300,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC300,$AI300,\"latent\",$U300&\"P\"&IF($V300=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T300,activeElevation),\"\"))","v":""},{"$f":"IF($T300=\"Select Model\",\"\",IF($T300=\"ACBC_1W\",calcQwIP($Y300,$W300,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC300,BD300,\"capacity\",$U300&\"P\"&IF($V300=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T300,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y300,$W300,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC300,BD300,\"capacity\",$U300&\"P\"&IF($V300=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T300,activeElevation)))","v":""},"",{"$f":"IF(T300=\"Select Model\", 0,waterPressureDrop(W300, U300 & \"P\" & IF(V300=\"Dual\",2,1) &\"C\", AC300, \"cooling\", T300))","v":0},{"$f":"IF(T300=\"Select Model\", \"\",getReturnWaterTemp(T300,AC300, activeEWTCooling, AS300, \"cooling\"))","v":""},"",{"$f":"IF($T300<>\"ACBC_1W\",\"\",IF($J300=\"\",\"\",FintubeCapacity($T300,$W300,$AE300,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T300=\"Select Model\",T300=\"PCBL\"),\"\",calcQwIP(Y300,W300,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD300,BD300,\"capacity\",U300&\"P\"&IF(V300=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T300,activeElevation))","v":""},"",{"$f":"IF(OR(T300=\"Select Model\",T300=\"PCBL\"), \"\",IF(AY300=0,\"N/A\",waterPressureDrop(W300, U300 & \"P\" & IF(V300=\"Dual\",2,1) &\"C\", AD300, \"heating\", T300)))","v":""},{"$f":"IF(OR(T300=\"Select Model\",T300=\"PCBL\"), \"\",IF(AY300=0,getReturnWaterTemp(T300,AE300, activeEWTHeating, AX300, \"heating\"),getReturnWaterTemp(T300,AD300, activeEWTHeating, AY300, \"heating\")))","v":""},"",{"$f":" getNozzle(T300, W300, Y300, Z300, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I301)),I301<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I301, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H301)),H301<0),\"\",intlEstQuantity(T301, W301*12, H301)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T301=\"Select Model\",\"\",coilCircuitChange(W301, U301, AC301, T301,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T301=\"Select Model\",\"\",beamWidth(T301))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T301=\"Select Model\",T301=\"PCBL\"), 0,getSPIP(T301, W301, Y301, BD301, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T301=\"Select Model\", \"\",IF(T301=\"PCBL\",0,primaryAirSensibleCapacityIP($T301,$W301,activeRoomTempCooling,activePriAirTempCooling,$Y301,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T301=\"Select Model\",\"\",IF($T301=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y301,activeElevation)))","v":""},{"$f":"IF(OR(T301=\"Select Model\",T301=\"PCBL\"), 0,IF(AD301=0,0,-primaryAirSensibleCapacityIP($T301,$W301,activeRoomTempHeating,activePriAirTempHeating,$Y301,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T301=\"Select Model\", \"\", InductionRatio($T301,BD301,$W301,$Y301)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T301=\"Select Model\", \"\",IF($T301=\"PCBL\",\"N/A\",minVAVSetBack(AA301, Y301))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T301=\"Select Model\", \"\",IF($T301= \"PCBL\",\"N/A\",getDischargeAirTemp($T301,$V301,$AC301,$W301,BD301,$AL301, $Y301, $AS301, \"cooling\",activeElevation,$AB301,$AJ301,$AV301,$BB301))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T301=\"Select Model\",$T301=\"PCBL\"), \"\",getDischargeAirTemp($T301,$V301,$AD301,$W301,BD301,$AL301, $Y301, $AY301, \"heating\",activeElevation,$AB301,$AJ301,$AV301,$BB301)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T301=\"Select Model\", \"\",IF(OR($T301=\"ACBC_1W\",$T301=\"ACBC_2W\",LEFT($T301,4)=\"ACBR\",$T301 = \"LIU24_2W\",LEFT($T301,3)=\"RIU\",LEFT($T301,6)=\"ACBL12\"), IF((soundLevel($T301, $AB301, BD301, $Y301, $W301,$AJ301,$AA301,\"dba\"))<15,\"<15\",soundLevel($T301, $AB301, BD301, $Y301, $W301,$AJ301,$AA301,\"dba\")+0.4),IF((soundLevel($T301, $AB301, BD301, $Y301, $W301,$AJ301,$AA301,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T301, $AB301, BD301, $Y301, $W301,$AJ301,$AA301,\"dba\")+5)<15, \"<15\", soundLevel($T301, $AB301, BD301,$Y301, $W301,$AJ301,$AA301,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T301=\"Select Model\", \"\",IF(OR($T301=\"ACBC_1W\",$T301=\"ACBC_2W\",LEFT($T301,4)=\"ACBR\",$T301=\"LIU24_2W\",LEFT($T301,3)=\"RIU\",LEFT($T301,6)=\"ACBL12\"), IF((soundLevel($T301, $AB301, BD301, $Y301, $W301,$AJ301,$AA301,\"NC\"))<15,\"<15\",soundLevel($T301, $AB301, BD301, $Y301, $W301,$AJ301,$AA301,\"NC\")+0.4),IF((soundLevel($T301, $AB301, BD301, $Y301, $W301,$AJ301,$AA301,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T301, $AB301, BD301, $Y301, $W301,$AJ301,$AA301,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T301, $AB301, BD301, $Y301, $W301,$AJ301,$AA301,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T301=\"Select Model\",\"\",IF($T301=\"LIU24_2W\",calcQwIP($Y301,$W301,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC301,$AI301,\"latent\",$U301&\"P\"&IF($V301=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T301,activeElevation),\"\"))","v":""},{"$f":"IF($T301=\"Select Model\",\"\",IF($T301=\"ACBC_1W\",calcQwIP($Y301,$W301,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC301,BD301,\"capacity\",$U301&\"P\"&IF($V301=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T301,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y301,$W301,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC301,BD301,\"capacity\",$U301&\"P\"&IF($V301=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T301,activeElevation)))","v":""},"",{"$f":"IF(T301=\"Select Model\", 0,waterPressureDrop(W301, U301 & \"P\" & IF(V301=\"Dual\",2,1) &\"C\", AC301, \"cooling\", T301))","v":0},{"$f":"IF(T301=\"Select Model\", \"\",getReturnWaterTemp(T301,AC301, activeEWTCooling, AS301, \"cooling\"))","v":""},"",{"$f":"IF($T301<>\"ACBC_1W\",\"\",IF($J301=\"\",\"\",FintubeCapacity($T301,$W301,$AE301,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T301=\"Select Model\",T301=\"PCBL\"),\"\",calcQwIP(Y301,W301,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD301,BD301,\"capacity\",U301&\"P\"&IF(V301=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T301,activeElevation))","v":""},"",{"$f":"IF(OR(T301=\"Select Model\",T301=\"PCBL\"), \"\",IF(AY301=0,\"N/A\",waterPressureDrop(W301, U301 & \"P\" & IF(V301=\"Dual\",2,1) &\"C\", AD301, \"heating\", T301)))","v":""},{"$f":"IF(OR(T301=\"Select Model\",T301=\"PCBL\"), \"\",IF(AY301=0,getReturnWaterTemp(T301,AE301, activeEWTHeating, AX301, \"heating\"),getReturnWaterTemp(T301,AD301, activeEWTHeating, AY301, \"heating\")))","v":""},"",{"$f":" getNozzle(T301, W301, Y301, Z301, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I302)),I302<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I302, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H302)),H302<0),\"\",intlEstQuantity(T302, W302*12, H302)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T302=\"Select Model\",\"\",coilCircuitChange(W302, U302, AC302, T302,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T302=\"Select Model\",\"\",beamWidth(T302))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T302=\"Select Model\",T302=\"PCBL\"), 0,getSPIP(T302, W302, Y302, BD302, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T302=\"Select Model\", \"\",IF(T302=\"PCBL\",0,primaryAirSensibleCapacityIP($T302,$W302,activeRoomTempCooling,activePriAirTempCooling,$Y302,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T302=\"Select Model\",\"\",IF($T302=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y302,activeElevation)))","v":""},{"$f":"IF(OR(T302=\"Select Model\",T302=\"PCBL\"), 0,IF(AD302=0,0,-primaryAirSensibleCapacityIP($T302,$W302,activeRoomTempHeating,activePriAirTempHeating,$Y302,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T302=\"Select Model\", \"\", InductionRatio($T302,BD302,$W302,$Y302)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T302=\"Select Model\", \"\",IF($T302=\"PCBL\",\"N/A\",minVAVSetBack(AA302, Y302))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T302=\"Select Model\", \"\",IF($T302= \"PCBL\",\"N/A\",getDischargeAirTemp($T302,$V302,$AC302,$W302,BD302,$AL302, $Y302, $AS302, \"cooling\",activeElevation,$AB302,$AJ302,$AV302,$BB302))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T302=\"Select Model\",$T302=\"PCBL\"), \"\",getDischargeAirTemp($T302,$V302,$AD302,$W302,BD302,$AL302, $Y302, $AY302, \"heating\",activeElevation,$AB302,$AJ302,$AV302,$BB302)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T302=\"Select Model\", \"\",IF(OR($T302=\"ACBC_1W\",$T302=\"ACBC_2W\",LEFT($T302,4)=\"ACBR\",$T302 = \"LIU24_2W\",LEFT($T302,3)=\"RIU\",LEFT($T302,6)=\"ACBL12\"), IF((soundLevel($T302, $AB302, BD302, $Y302, $W302,$AJ302,$AA302,\"dba\"))<15,\"<15\",soundLevel($T302, $AB302, BD302, $Y302, $W302,$AJ302,$AA302,\"dba\")+0.4),IF((soundLevel($T302, $AB302, BD302, $Y302, $W302,$AJ302,$AA302,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T302, $AB302, BD302, $Y302, $W302,$AJ302,$AA302,\"dba\")+5)<15, \"<15\", soundLevel($T302, $AB302, BD302,$Y302, $W302,$AJ302,$AA302,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T302=\"Select Model\", \"\",IF(OR($T302=\"ACBC_1W\",$T302=\"ACBC_2W\",LEFT($T302,4)=\"ACBR\",$T302=\"LIU24_2W\",LEFT($T302,3)=\"RIU\",LEFT($T302,6)=\"ACBL12\"), IF((soundLevel($T302, $AB302, BD302, $Y302, $W302,$AJ302,$AA302,\"NC\"))<15,\"<15\",soundLevel($T302, $AB302, BD302, $Y302, $W302,$AJ302,$AA302,\"NC\")+0.4),IF((soundLevel($T302, $AB302, BD302, $Y302, $W302,$AJ302,$AA302,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T302, $AB302, BD302, $Y302, $W302,$AJ302,$AA302,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T302, $AB302, BD302, $Y302, $W302,$AJ302,$AA302,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T302=\"Select Model\",\"\",IF($T302=\"LIU24_2W\",calcQwIP($Y302,$W302,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC302,$AI302,\"latent\",$U302&\"P\"&IF($V302=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T302,activeElevation),\"\"))","v":""},{"$f":"IF($T302=\"Select Model\",\"\",IF($T302=\"ACBC_1W\",calcQwIP($Y302,$W302,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC302,BD302,\"capacity\",$U302&\"P\"&IF($V302=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T302,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y302,$W302,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC302,BD302,\"capacity\",$U302&\"P\"&IF($V302=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T302,activeElevation)))","v":""},"",{"$f":"IF(T302=\"Select Model\", 0,waterPressureDrop(W302, U302 & \"P\" & IF(V302=\"Dual\",2,1) &\"C\", AC302, \"cooling\", T302))","v":0},{"$f":"IF(T302=\"Select Model\", \"\",getReturnWaterTemp(T302,AC302, activeEWTCooling, AS302, \"cooling\"))","v":""},"",{"$f":"IF($T302<>\"ACBC_1W\",\"\",IF($J302=\"\",\"\",FintubeCapacity($T302,$W302,$AE302,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T302=\"Select Model\",T302=\"PCBL\"),\"\",calcQwIP(Y302,W302,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD302,BD302,\"capacity\",U302&\"P\"&IF(V302=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T302,activeElevation))","v":""},"",{"$f":"IF(OR(T302=\"Select Model\",T302=\"PCBL\"), \"\",IF(AY302=0,\"N/A\",waterPressureDrop(W302, U302 & \"P\" & IF(V302=\"Dual\",2,1) &\"C\", AD302, \"heating\", T302)))","v":""},{"$f":"IF(OR(T302=\"Select Model\",T302=\"PCBL\"), \"\",IF(AY302=0,getReturnWaterTemp(T302,AE302, activeEWTHeating, AX302, \"heating\"),getReturnWaterTemp(T302,AD302, activeEWTHeating, AY302, \"heating\")))","v":""},"",{"$f":" getNozzle(T302, W302, Y302, Z302, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I303)),I303<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I303, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H303)),H303<0),\"\",intlEstQuantity(T303, W303*12, H303)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T303=\"Select Model\",\"\",coilCircuitChange(W303, U303, AC303, T303,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T303=\"Select Model\",\"\",beamWidth(T303))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T303=\"Select Model\",T303=\"PCBL\"), 0,getSPIP(T303, W303, Y303, BD303, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T303=\"Select Model\", \"\",IF(T303=\"PCBL\",0,primaryAirSensibleCapacityIP($T303,$W303,activeRoomTempCooling,activePriAirTempCooling,$Y303,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T303=\"Select Model\",\"\",IF($T303=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y303,activeElevation)))","v":""},{"$f":"IF(OR(T303=\"Select Model\",T303=\"PCBL\"), 0,IF(AD303=0,0,-primaryAirSensibleCapacityIP($T303,$W303,activeRoomTempHeating,activePriAirTempHeating,$Y303,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T303=\"Select Model\", \"\", InductionRatio($T303,BD303,$W303,$Y303)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T303=\"Select Model\", \"\",IF($T303=\"PCBL\",\"N/A\",minVAVSetBack(AA303, Y303))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T303=\"Select Model\", \"\",IF($T303= \"PCBL\",\"N/A\",getDischargeAirTemp($T303,$V303,$AC303,$W303,BD303,$AL303, $Y303, $AS303, \"cooling\",activeElevation,$AB303,$AJ303,$AV303,$BB303))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T303=\"Select Model\",$T303=\"PCBL\"), \"\",getDischargeAirTemp($T303,$V303,$AD303,$W303,BD303,$AL303, $Y303, $AY303, \"heating\",activeElevation,$AB303,$AJ303,$AV303,$BB303)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T303=\"Select Model\", \"\",IF(OR($T303=\"ACBC_1W\",$T303=\"ACBC_2W\",LEFT($T303,4)=\"ACBR\",$T303 = \"LIU24_2W\",LEFT($T303,3)=\"RIU\",LEFT($T303,6)=\"ACBL12\"), IF((soundLevel($T303, $AB303, BD303, $Y303, $W303,$AJ303,$AA303,\"dba\"))<15,\"<15\",soundLevel($T303, $AB303, BD303, $Y303, $W303,$AJ303,$AA303,\"dba\")+0.4),IF((soundLevel($T303, $AB303, BD303, $Y303, $W303,$AJ303,$AA303,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T303, $AB303, BD303, $Y303, $W303,$AJ303,$AA303,\"dba\")+5)<15, \"<15\", soundLevel($T303, $AB303, BD303,$Y303, $W303,$AJ303,$AA303,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T303=\"Select Model\", \"\",IF(OR($T303=\"ACBC_1W\",$T303=\"ACBC_2W\",LEFT($T303,4)=\"ACBR\",$T303=\"LIU24_2W\",LEFT($T303,3)=\"RIU\",LEFT($T303,6)=\"ACBL12\"), IF((soundLevel($T303, $AB303, BD303, $Y303, $W303,$AJ303,$AA303,\"NC\"))<15,\"<15\",soundLevel($T303, $AB303, BD303, $Y303, $W303,$AJ303,$AA303,\"NC\")+0.4),IF((soundLevel($T303, $AB303, BD303, $Y303, $W303,$AJ303,$AA303,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T303, $AB303, BD303, $Y303, $W303,$AJ303,$AA303,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T303, $AB303, BD303, $Y303, $W303,$AJ303,$AA303,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T303=\"Select Model\",\"\",IF($T303=\"LIU24_2W\",calcQwIP($Y303,$W303,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC303,$AI303,\"latent\",$U303&\"P\"&IF($V303=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T303,activeElevation),\"\"))","v":""},{"$f":"IF($T303=\"Select Model\",\"\",IF($T303=\"ACBC_1W\",calcQwIP($Y303,$W303,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC303,BD303,\"capacity\",$U303&\"P\"&IF($V303=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T303,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y303,$W303,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC303,BD303,\"capacity\",$U303&\"P\"&IF($V303=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T303,activeElevation)))","v":""},"",{"$f":"IF(T303=\"Select Model\", 0,waterPressureDrop(W303, U303 & \"P\" & IF(V303=\"Dual\",2,1) &\"C\", AC303, \"cooling\", T303))","v":0},{"$f":"IF(T303=\"Select Model\", \"\",getReturnWaterTemp(T303,AC303, activeEWTCooling, AS303, \"cooling\"))","v":""},"",{"$f":"IF($T303<>\"ACBC_1W\",\"\",IF($J303=\"\",\"\",FintubeCapacity($T303,$W303,$AE303,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T303=\"Select Model\",T303=\"PCBL\"),\"\",calcQwIP(Y303,W303,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD303,BD303,\"capacity\",U303&\"P\"&IF(V303=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T303,activeElevation))","v":""},"",{"$f":"IF(OR(T303=\"Select Model\",T303=\"PCBL\"), \"\",IF(AY303=0,\"N/A\",waterPressureDrop(W303, U303 & \"P\" & IF(V303=\"Dual\",2,1) &\"C\", AD303, \"heating\", T303)))","v":""},{"$f":"IF(OR(T303=\"Select Model\",T303=\"PCBL\"), \"\",IF(AY303=0,getReturnWaterTemp(T303,AE303, activeEWTHeating, AX303, \"heating\"),getReturnWaterTemp(T303,AD303, activeEWTHeating, AY303, \"heating\")))","v":""},"",{"$f":" getNozzle(T303, W303, Y303, Z303, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I304)),I304<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I304, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H304)),H304<0),\"\",intlEstQuantity(T304, W304*12, H304)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T304=\"Select Model\",\"\",coilCircuitChange(W304, U304, AC304, T304,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T304=\"Select Model\",\"\",beamWidth(T304))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T304=\"Select Model\",T304=\"PCBL\"), 0,getSPIP(T304, W304, Y304, BD304, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T304=\"Select Model\", \"\",IF(T304=\"PCBL\",0,primaryAirSensibleCapacityIP($T304,$W304,activeRoomTempCooling,activePriAirTempCooling,$Y304,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T304=\"Select Model\",\"\",IF($T304=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y304,activeElevation)))","v":""},{"$f":"IF(OR(T304=\"Select Model\",T304=\"PCBL\"), 0,IF(AD304=0,0,-primaryAirSensibleCapacityIP($T304,$W304,activeRoomTempHeating,activePriAirTempHeating,$Y304,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T304=\"Select Model\", \"\", InductionRatio($T304,BD304,$W304,$Y304)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T304=\"Select Model\", \"\",IF($T304=\"PCBL\",\"N/A\",minVAVSetBack(AA304, Y304))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T304=\"Select Model\", \"\",IF($T304= \"PCBL\",\"N/A\",getDischargeAirTemp($T304,$V304,$AC304,$W304,BD304,$AL304, $Y304, $AS304, \"cooling\",activeElevation,$AB304,$AJ304,$AV304,$BB304))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T304=\"Select Model\",$T304=\"PCBL\"), \"\",getDischargeAirTemp($T304,$V304,$AD304,$W304,BD304,$AL304, $Y304, $AY304, \"heating\",activeElevation,$AB304,$AJ304,$AV304,$BB304)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T304=\"Select Model\", \"\",IF(OR($T304=\"ACBC_1W\",$T304=\"ACBC_2W\",LEFT($T304,4)=\"ACBR\",$T304 = \"LIU24_2W\",LEFT($T304,3)=\"RIU\",LEFT($T304,6)=\"ACBL12\"), IF((soundLevel($T304, $AB304, BD304, $Y304, $W304,$AJ304,$AA304,\"dba\"))<15,\"<15\",soundLevel($T304, $AB304, BD304, $Y304, $W304,$AJ304,$AA304,\"dba\")+0.4),IF((soundLevel($T304, $AB304, BD304, $Y304, $W304,$AJ304,$AA304,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T304, $AB304, BD304, $Y304, $W304,$AJ304,$AA304,\"dba\")+5)<15, \"<15\", soundLevel($T304, $AB304, BD304,$Y304, $W304,$AJ304,$AA304,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T304=\"Select Model\", \"\",IF(OR($T304=\"ACBC_1W\",$T304=\"ACBC_2W\",LEFT($T304,4)=\"ACBR\",$T304=\"LIU24_2W\",LEFT($T304,3)=\"RIU\",LEFT($T304,6)=\"ACBL12\"), IF((soundLevel($T304, $AB304, BD304, $Y304, $W304,$AJ304,$AA304,\"NC\"))<15,\"<15\",soundLevel($T304, $AB304, BD304, $Y304, $W304,$AJ304,$AA304,\"NC\")+0.4),IF((soundLevel($T304, $AB304, BD304, $Y304, $W304,$AJ304,$AA304,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T304, $AB304, BD304, $Y304, $W304,$AJ304,$AA304,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T304, $AB304, BD304, $Y304, $W304,$AJ304,$AA304,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T304=\"Select Model\",\"\",IF($T304=\"LIU24_2W\",calcQwIP($Y304,$W304,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC304,$AI304,\"latent\",$U304&\"P\"&IF($V304=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T304,activeElevation),\"\"))","v":""},{"$f":"IF($T304=\"Select Model\",\"\",IF($T304=\"ACBC_1W\",calcQwIP($Y304,$W304,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC304,BD304,\"capacity\",$U304&\"P\"&IF($V304=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T304,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y304,$W304,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC304,BD304,\"capacity\",$U304&\"P\"&IF($V304=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T304,activeElevation)))","v":""},"",{"$f":"IF(T304=\"Select Model\", 0,waterPressureDrop(W304, U304 & \"P\" & IF(V304=\"Dual\",2,1) &\"C\", AC304, \"cooling\", T304))","v":0},{"$f":"IF(T304=\"Select Model\", \"\",getReturnWaterTemp(T304,AC304, activeEWTCooling, AS304, \"cooling\"))","v":""},"",{"$f":"IF($T304<>\"ACBC_1W\",\"\",IF($J304=\"\",\"\",FintubeCapacity($T304,$W304,$AE304,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T304=\"Select Model\",T304=\"PCBL\"),\"\",calcQwIP(Y304,W304,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD304,BD304,\"capacity\",U304&\"P\"&IF(V304=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T304,activeElevation))","v":""},"",{"$f":"IF(OR(T304=\"Select Model\",T304=\"PCBL\"), \"\",IF(AY304=0,\"N/A\",waterPressureDrop(W304, U304 & \"P\" & IF(V304=\"Dual\",2,1) &\"C\", AD304, \"heating\", T304)))","v":""},{"$f":"IF(OR(T304=\"Select Model\",T304=\"PCBL\"), \"\",IF(AY304=0,getReturnWaterTemp(T304,AE304, activeEWTHeating, AX304, \"heating\"),getReturnWaterTemp(T304,AD304, activeEWTHeating, AY304, \"heating\")))","v":""},"",{"$f":" getNozzle(T304, W304, Y304, Z304, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I305)),I305<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I305, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H305)),H305<0),\"\",intlEstQuantity(T305, W305*12, H305)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T305=\"Select Model\",\"\",coilCircuitChange(W305, U305, AC305, T305,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T305=\"Select Model\",\"\",beamWidth(T305))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T305=\"Select Model\",T305=\"PCBL\"), 0,getSPIP(T305, W305, Y305, BD305, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T305=\"Select Model\", \"\",IF(T305=\"PCBL\",0,primaryAirSensibleCapacityIP($T305,$W305,activeRoomTempCooling,activePriAirTempCooling,$Y305,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T305=\"Select Model\",\"\",IF($T305=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y305,activeElevation)))","v":""},{"$f":"IF(OR(T305=\"Select Model\",T305=\"PCBL\"), 0,IF(AD305=0,0,-primaryAirSensibleCapacityIP($T305,$W305,activeRoomTempHeating,activePriAirTempHeating,$Y305,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T305=\"Select Model\", \"\", InductionRatio($T305,BD305,$W305,$Y305)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T305=\"Select Model\", \"\",IF($T305=\"PCBL\",\"N/A\",minVAVSetBack(AA305, Y305))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T305=\"Select Model\", \"\",IF($T305= \"PCBL\",\"N/A\",getDischargeAirTemp($T305,$V305,$AC305,$W305,BD305,$AL305, $Y305, $AS305, \"cooling\",activeElevation,$AB305,$AJ305,$AV305,$BB305))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T305=\"Select Model\",$T305=\"PCBL\"), \"\",getDischargeAirTemp($T305,$V305,$AD305,$W305,BD305,$AL305, $Y305, $AY305, \"heating\",activeElevation,$AB305,$AJ305,$AV305,$BB305)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T305=\"Select Model\", \"\",IF(OR($T305=\"ACBC_1W\",$T305=\"ACBC_2W\",LEFT($T305,4)=\"ACBR\",$T305 = \"LIU24_2W\",LEFT($T305,3)=\"RIU\",LEFT($T305,6)=\"ACBL12\"), IF((soundLevel($T305, $AB305, BD305, $Y305, $W305,$AJ305,$AA305,\"dba\"))<15,\"<15\",soundLevel($T305, $AB305, BD305, $Y305, $W305,$AJ305,$AA305,\"dba\")+0.4),IF((soundLevel($T305, $AB305, BD305, $Y305, $W305,$AJ305,$AA305,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T305, $AB305, BD305, $Y305, $W305,$AJ305,$AA305,\"dba\")+5)<15, \"<15\", soundLevel($T305, $AB305, BD305,$Y305, $W305,$AJ305,$AA305,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T305=\"Select Model\", \"\",IF(OR($T305=\"ACBC_1W\",$T305=\"ACBC_2W\",LEFT($T305,4)=\"ACBR\",$T305=\"LIU24_2W\",LEFT($T305,3)=\"RIU\",LEFT($T305,6)=\"ACBL12\"), IF((soundLevel($T305, $AB305, BD305, $Y305, $W305,$AJ305,$AA305,\"NC\"))<15,\"<15\",soundLevel($T305, $AB305, BD305, $Y305, $W305,$AJ305,$AA305,\"NC\")+0.4),IF((soundLevel($T305, $AB305, BD305, $Y305, $W305,$AJ305,$AA305,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T305, $AB305, BD305, $Y305, $W305,$AJ305,$AA305,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T305, $AB305, BD305, $Y305, $W305,$AJ305,$AA305,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T305=\"Select Model\",\"\",IF($T305=\"LIU24_2W\",calcQwIP($Y305,$W305,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC305,$AI305,\"latent\",$U305&\"P\"&IF($V305=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T305,activeElevation),\"\"))","v":""},{"$f":"IF($T305=\"Select Model\",\"\",IF($T305=\"ACBC_1W\",calcQwIP($Y305,$W305,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC305,BD305,\"capacity\",$U305&\"P\"&IF($V305=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T305,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y305,$W305,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC305,BD305,\"capacity\",$U305&\"P\"&IF($V305=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T305,activeElevation)))","v":""},"",{"$f":"IF(T305=\"Select Model\", 0,waterPressureDrop(W305, U305 & \"P\" & IF(V305=\"Dual\",2,1) &\"C\", AC305, \"cooling\", T305))","v":0},{"$f":"IF(T305=\"Select Model\", \"\",getReturnWaterTemp(T305,AC305, activeEWTCooling, AS305, \"cooling\"))","v":""},"",{"$f":"IF($T305<>\"ACBC_1W\",\"\",IF($J305=\"\",\"\",FintubeCapacity($T305,$W305,$AE305,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T305=\"Select Model\",T305=\"PCBL\"),\"\",calcQwIP(Y305,W305,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD305,BD305,\"capacity\",U305&\"P\"&IF(V305=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T305,activeElevation))","v":""},"",{"$f":"IF(OR(T305=\"Select Model\",T305=\"PCBL\"), \"\",IF(AY305=0,\"N/A\",waterPressureDrop(W305, U305 & \"P\" & IF(V305=\"Dual\",2,1) &\"C\", AD305, \"heating\", T305)))","v":""},{"$f":"IF(OR(T305=\"Select Model\",T305=\"PCBL\"), \"\",IF(AY305=0,getReturnWaterTemp(T305,AE305, activeEWTHeating, AX305, \"heating\"),getReturnWaterTemp(T305,AD305, activeEWTHeating, AY305, \"heating\")))","v":""},"",{"$f":" getNozzle(T305, W305, Y305, Z305, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I306)),I306<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I306, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H306)),H306<0),\"\",intlEstQuantity(T306, W306*12, H306)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T306=\"Select Model\",\"\",coilCircuitChange(W306, U306, AC306, T306,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T306=\"Select Model\",\"\",beamWidth(T306))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T306=\"Select Model\",T306=\"PCBL\"), 0,getSPIP(T306, W306, Y306, BD306, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T306=\"Select Model\", \"\",IF(T306=\"PCBL\",0,primaryAirSensibleCapacityIP($T306,$W306,activeRoomTempCooling,activePriAirTempCooling,$Y306,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T306=\"Select Model\",\"\",IF($T306=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y306,activeElevation)))","v":""},{"$f":"IF(OR(T306=\"Select Model\",T306=\"PCBL\"), 0,IF(AD306=0,0,-primaryAirSensibleCapacityIP($T306,$W306,activeRoomTempHeating,activePriAirTempHeating,$Y306,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T306=\"Select Model\", \"\", InductionRatio($T306,BD306,$W306,$Y306)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T306=\"Select Model\", \"\",IF($T306=\"PCBL\",\"N/A\",minVAVSetBack(AA306, Y306))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T306=\"Select Model\", \"\",IF($T306= \"PCBL\",\"N/A\",getDischargeAirTemp($T306,$V306,$AC306,$W306,BD306,$AL306, $Y306, $AS306, \"cooling\",activeElevation,$AB306,$AJ306,$AV306,$BB306))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T306=\"Select Model\",$T306=\"PCBL\"), \"\",getDischargeAirTemp($T306,$V306,$AD306,$W306,BD306,$AL306, $Y306, $AY306, \"heating\",activeElevation,$AB306,$AJ306,$AV306,$BB306)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T306=\"Select Model\", \"\",IF(OR($T306=\"ACBC_1W\",$T306=\"ACBC_2W\",LEFT($T306,4)=\"ACBR\",$T306 = \"LIU24_2W\",LEFT($T306,3)=\"RIU\",LEFT($T306,6)=\"ACBL12\"), IF((soundLevel($T306, $AB306, BD306, $Y306, $W306,$AJ306,$AA306,\"dba\"))<15,\"<15\",soundLevel($T306, $AB306, BD306, $Y306, $W306,$AJ306,$AA306,\"dba\")+0.4),IF((soundLevel($T306, $AB306, BD306, $Y306, $W306,$AJ306,$AA306,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T306, $AB306, BD306, $Y306, $W306,$AJ306,$AA306,\"dba\")+5)<15, \"<15\", soundLevel($T306, $AB306, BD306,$Y306, $W306,$AJ306,$AA306,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T306=\"Select Model\", \"\",IF(OR($T306=\"ACBC_1W\",$T306=\"ACBC_2W\",LEFT($T306,4)=\"ACBR\",$T306=\"LIU24_2W\",LEFT($T306,3)=\"RIU\",LEFT($T306,6)=\"ACBL12\"), IF((soundLevel($T306, $AB306, BD306, $Y306, $W306,$AJ306,$AA306,\"NC\"))<15,\"<15\",soundLevel($T306, $AB306, BD306, $Y306, $W306,$AJ306,$AA306,\"NC\")+0.4),IF((soundLevel($T306, $AB306, BD306, $Y306, $W306,$AJ306,$AA306,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T306, $AB306, BD306, $Y306, $W306,$AJ306,$AA306,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T306, $AB306, BD306, $Y306, $W306,$AJ306,$AA306,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T306=\"Select Model\",\"\",IF($T306=\"LIU24_2W\",calcQwIP($Y306,$W306,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC306,$AI306,\"latent\",$U306&\"P\"&IF($V306=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T306,activeElevation),\"\"))","v":""},{"$f":"IF($T306=\"Select Model\",\"\",IF($T306=\"ACBC_1W\",calcQwIP($Y306,$W306,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC306,BD306,\"capacity\",$U306&\"P\"&IF($V306=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T306,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y306,$W306,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC306,BD306,\"capacity\",$U306&\"P\"&IF($V306=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T306,activeElevation)))","v":""},"",{"$f":"IF(T306=\"Select Model\", 0,waterPressureDrop(W306, U306 & \"P\" & IF(V306=\"Dual\",2,1) &\"C\", AC306, \"cooling\", T306))","v":0},{"$f":"IF(T306=\"Select Model\", \"\",getReturnWaterTemp(T306,AC306, activeEWTCooling, AS306, \"cooling\"))","v":""},"",{"$f":"IF($T306<>\"ACBC_1W\",\"\",IF($J306=\"\",\"\",FintubeCapacity($T306,$W306,$AE306,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T306=\"Select Model\",T306=\"PCBL\"),\"\",calcQwIP(Y306,W306,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD306,BD306,\"capacity\",U306&\"P\"&IF(V306=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T306,activeElevation))","v":""},"",{"$f":"IF(OR(T306=\"Select Model\",T306=\"PCBL\"), \"\",IF(AY306=0,\"N/A\",waterPressureDrop(W306, U306 & \"P\" & IF(V306=\"Dual\",2,1) &\"C\", AD306, \"heating\", T306)))","v":""},{"$f":"IF(OR(T306=\"Select Model\",T306=\"PCBL\"), \"\",IF(AY306=0,getReturnWaterTemp(T306,AE306, activeEWTHeating, AX306, \"heating\"),getReturnWaterTemp(T306,AD306, activeEWTHeating, AY306, \"heating\")))","v":""},"",{"$f":" getNozzle(T306, W306, Y306, Z306, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I307)),I307<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I307, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H307)),H307<0),\"\",intlEstQuantity(T307, W307*12, H307)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T307=\"Select Model\",\"\",coilCircuitChange(W307, U307, AC307, T307,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T307=\"Select Model\",\"\",beamWidth(T307))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T307=\"Select Model\",T307=\"PCBL\"), 0,getSPIP(T307, W307, Y307, BD307, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T307=\"Select Model\", \"\",IF(T307=\"PCBL\",0,primaryAirSensibleCapacityIP($T307,$W307,activeRoomTempCooling,activePriAirTempCooling,$Y307,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T307=\"Select Model\",\"\",IF($T307=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y307,activeElevation)))","v":""},{"$f":"IF(OR(T307=\"Select Model\",T307=\"PCBL\"), 0,IF(AD307=0,0,-primaryAirSensibleCapacityIP($T307,$W307,activeRoomTempHeating,activePriAirTempHeating,$Y307,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T307=\"Select Model\", \"\", InductionRatio($T307,BD307,$W307,$Y307)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T307=\"Select Model\", \"\",IF($T307=\"PCBL\",\"N/A\",minVAVSetBack(AA307, Y307))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T307=\"Select Model\", \"\",IF($T307= \"PCBL\",\"N/A\",getDischargeAirTemp($T307,$V307,$AC307,$W307,BD307,$AL307, $Y307, $AS307, \"cooling\",activeElevation,$AB307,$AJ307,$AV307,$BB307))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T307=\"Select Model\",$T307=\"PCBL\"), \"\",getDischargeAirTemp($T307,$V307,$AD307,$W307,BD307,$AL307, $Y307, $AY307, \"heating\",activeElevation,$AB307,$AJ307,$AV307,$BB307)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T307=\"Select Model\", \"\",IF(OR($T307=\"ACBC_1W\",$T307=\"ACBC_2W\",LEFT($T307,4)=\"ACBR\",$T307 = \"LIU24_2W\",LEFT($T307,3)=\"RIU\",LEFT($T307,6)=\"ACBL12\"), IF((soundLevel($T307, $AB307, BD307, $Y307, $W307,$AJ307,$AA307,\"dba\"))<15,\"<15\",soundLevel($T307, $AB307, BD307, $Y307, $W307,$AJ307,$AA307,\"dba\")+0.4),IF((soundLevel($T307, $AB307, BD307, $Y307, $W307,$AJ307,$AA307,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T307, $AB307, BD307, $Y307, $W307,$AJ307,$AA307,\"dba\")+5)<15, \"<15\", soundLevel($T307, $AB307, BD307,$Y307, $W307,$AJ307,$AA307,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T307=\"Select Model\", \"\",IF(OR($T307=\"ACBC_1W\",$T307=\"ACBC_2W\",LEFT($T307,4)=\"ACBR\",$T307=\"LIU24_2W\",LEFT($T307,3)=\"RIU\",LEFT($T307,6)=\"ACBL12\"), IF((soundLevel($T307, $AB307, BD307, $Y307, $W307,$AJ307,$AA307,\"NC\"))<15,\"<15\",soundLevel($T307, $AB307, BD307, $Y307, $W307,$AJ307,$AA307,\"NC\")+0.4),IF((soundLevel($T307, $AB307, BD307, $Y307, $W307,$AJ307,$AA307,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T307, $AB307, BD307, $Y307, $W307,$AJ307,$AA307,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T307, $AB307, BD307, $Y307, $W307,$AJ307,$AA307,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T307=\"Select Model\",\"\",IF($T307=\"LIU24_2W\",calcQwIP($Y307,$W307,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC307,$AI307,\"latent\",$U307&\"P\"&IF($V307=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T307,activeElevation),\"\"))","v":""},{"$f":"IF($T307=\"Select Model\",\"\",IF($T307=\"ACBC_1W\",calcQwIP($Y307,$W307,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC307,BD307,\"capacity\",$U307&\"P\"&IF($V307=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T307,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y307,$W307,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC307,BD307,\"capacity\",$U307&\"P\"&IF($V307=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T307,activeElevation)))","v":""},"",{"$f":"IF(T307=\"Select Model\", 0,waterPressureDrop(W307, U307 & \"P\" & IF(V307=\"Dual\",2,1) &\"C\", AC307, \"cooling\", T307))","v":0},{"$f":"IF(T307=\"Select Model\", \"\",getReturnWaterTemp(T307,AC307, activeEWTCooling, AS307, \"cooling\"))","v":""},"",{"$f":"IF($T307<>\"ACBC_1W\",\"\",IF($J307=\"\",\"\",FintubeCapacity($T307,$W307,$AE307,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T307=\"Select Model\",T307=\"PCBL\"),\"\",calcQwIP(Y307,W307,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD307,BD307,\"capacity\",U307&\"P\"&IF(V307=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T307,activeElevation))","v":""},"",{"$f":"IF(OR(T307=\"Select Model\",T307=\"PCBL\"), \"\",IF(AY307=0,\"N/A\",waterPressureDrop(W307, U307 & \"P\" & IF(V307=\"Dual\",2,1) &\"C\", AD307, \"heating\", T307)))","v":""},{"$f":"IF(OR(T307=\"Select Model\",T307=\"PCBL\"), \"\",IF(AY307=0,getReturnWaterTemp(T307,AE307, activeEWTHeating, AX307, \"heating\"),getReturnWaterTemp(T307,AD307, activeEWTHeating, AY307, \"heating\")))","v":""},"",{"$f":" getNozzle(T307, W307, Y307, Z307, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I308)),I308<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I308, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H308)),H308<0),\"\",intlEstQuantity(T308, W308*12, H308)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T308=\"Select Model\",\"\",coilCircuitChange(W308, U308, AC308, T308,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T308=\"Select Model\",\"\",beamWidth(T308))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T308=\"Select Model\",T308=\"PCBL\"), 0,getSPIP(T308, W308, Y308, BD308, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T308=\"Select Model\", \"\",IF(T308=\"PCBL\",0,primaryAirSensibleCapacityIP($T308,$W308,activeRoomTempCooling,activePriAirTempCooling,$Y308,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T308=\"Select Model\",\"\",IF($T308=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y308,activeElevation)))","v":""},{"$f":"IF(OR(T308=\"Select Model\",T308=\"PCBL\"), 0,IF(AD308=0,0,-primaryAirSensibleCapacityIP($T308,$W308,activeRoomTempHeating,activePriAirTempHeating,$Y308,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T308=\"Select Model\", \"\", InductionRatio($T308,BD308,$W308,$Y308)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T308=\"Select Model\", \"\",IF($T308=\"PCBL\",\"N/A\",minVAVSetBack(AA308, Y308))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T308=\"Select Model\", \"\",IF($T308= \"PCBL\",\"N/A\",getDischargeAirTemp($T308,$V308,$AC308,$W308,BD308,$AL308, $Y308, $AS308, \"cooling\",activeElevation,$AB308,$AJ308,$AV308,$BB308))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T308=\"Select Model\",$T308=\"PCBL\"), \"\",getDischargeAirTemp($T308,$V308,$AD308,$W308,BD308,$AL308, $Y308, $AY308, \"heating\",activeElevation,$AB308,$AJ308,$AV308,$BB308)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T308=\"Select Model\", \"\",IF(OR($T308=\"ACBC_1W\",$T308=\"ACBC_2W\",LEFT($T308,4)=\"ACBR\",$T308 = \"LIU24_2W\",LEFT($T308,3)=\"RIU\",LEFT($T308,6)=\"ACBL12\"), IF((soundLevel($T308, $AB308, BD308, $Y308, $W308,$AJ308,$AA308,\"dba\"))<15,\"<15\",soundLevel($T308, $AB308, BD308, $Y308, $W308,$AJ308,$AA308,\"dba\")+0.4),IF((soundLevel($T308, $AB308, BD308, $Y308, $W308,$AJ308,$AA308,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T308, $AB308, BD308, $Y308, $W308,$AJ308,$AA308,\"dba\")+5)<15, \"<15\", soundLevel($T308, $AB308, BD308,$Y308, $W308,$AJ308,$AA308,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T308=\"Select Model\", \"\",IF(OR($T308=\"ACBC_1W\",$T308=\"ACBC_2W\",LEFT($T308,4)=\"ACBR\",$T308=\"LIU24_2W\",LEFT($T308,3)=\"RIU\",LEFT($T308,6)=\"ACBL12\"), IF((soundLevel($T308, $AB308, BD308, $Y308, $W308,$AJ308,$AA308,\"NC\"))<15,\"<15\",soundLevel($T308, $AB308, BD308, $Y308, $W308,$AJ308,$AA308,\"NC\")+0.4),IF((soundLevel($T308, $AB308, BD308, $Y308, $W308,$AJ308,$AA308,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T308, $AB308, BD308, $Y308, $W308,$AJ308,$AA308,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T308, $AB308, BD308, $Y308, $W308,$AJ308,$AA308,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T308=\"Select Model\",\"\",IF($T308=\"LIU24_2W\",calcQwIP($Y308,$W308,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC308,$AI308,\"latent\",$U308&\"P\"&IF($V308=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T308,activeElevation),\"\"))","v":""},{"$f":"IF($T308=\"Select Model\",\"\",IF($T308=\"ACBC_1W\",calcQwIP($Y308,$W308,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC308,BD308,\"capacity\",$U308&\"P\"&IF($V308=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T308,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y308,$W308,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC308,BD308,\"capacity\",$U308&\"P\"&IF($V308=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T308,activeElevation)))","v":""},"",{"$f":"IF(T308=\"Select Model\", 0,waterPressureDrop(W308, U308 & \"P\" & IF(V308=\"Dual\",2,1) &\"C\", AC308, \"cooling\", T308))","v":0},{"$f":"IF(T308=\"Select Model\", \"\",getReturnWaterTemp(T308,AC308, activeEWTCooling, AS308, \"cooling\"))","v":""},"",{"$f":"IF($T308<>\"ACBC_1W\",\"\",IF($J308=\"\",\"\",FintubeCapacity($T308,$W308,$AE308,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T308=\"Select Model\",T308=\"PCBL\"),\"\",calcQwIP(Y308,W308,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD308,BD308,\"capacity\",U308&\"P\"&IF(V308=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T308,activeElevation))","v":""},"",{"$f":"IF(OR(T308=\"Select Model\",T308=\"PCBL\"), \"\",IF(AY308=0,\"N/A\",waterPressureDrop(W308, U308 & \"P\" & IF(V308=\"Dual\",2,1) &\"C\", AD308, \"heating\", T308)))","v":""},{"$f":"IF(OR(T308=\"Select Model\",T308=\"PCBL\"), \"\",IF(AY308=0,getReturnWaterTemp(T308,AE308, activeEWTHeating, AX308, \"heating\"),getReturnWaterTemp(T308,AD308, activeEWTHeating, AY308, \"heating\")))","v":""},"",{"$f":" getNozzle(T308, W308, Y308, Z308, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I309)),I309<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I309, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H309)),H309<0),\"\",intlEstQuantity(T309, W309*12, H309)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T309=\"Select Model\",\"\",coilCircuitChange(W309, U309, AC309, T309,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T309=\"Select Model\",\"\",beamWidth(T309))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T309=\"Select Model\",T309=\"PCBL\"), 0,getSPIP(T309, W309, Y309, BD309, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T309=\"Select Model\", \"\",IF(T309=\"PCBL\",0,primaryAirSensibleCapacityIP($T309,$W309,activeRoomTempCooling,activePriAirTempCooling,$Y309,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T309=\"Select Model\",\"\",IF($T309=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y309,activeElevation)))","v":""},{"$f":"IF(OR(T309=\"Select Model\",T309=\"PCBL\"), 0,IF(AD309=0,0,-primaryAirSensibleCapacityIP($T309,$W309,activeRoomTempHeating,activePriAirTempHeating,$Y309,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T309=\"Select Model\", \"\", InductionRatio($T309,BD309,$W309,$Y309)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T309=\"Select Model\", \"\",IF($T309=\"PCBL\",\"N/A\",minVAVSetBack(AA309, Y309))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T309=\"Select Model\", \"\",IF($T309= \"PCBL\",\"N/A\",getDischargeAirTemp($T309,$V309,$AC309,$W309,BD309,$AL309, $Y309, $AS309, \"cooling\",activeElevation,$AB309,$AJ309,$AV309,$BB309))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T309=\"Select Model\",$T309=\"PCBL\"), \"\",getDischargeAirTemp($T309,$V309,$AD309,$W309,BD309,$AL309, $Y309, $AY309, \"heating\",activeElevation,$AB309,$AJ309,$AV309,$BB309)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T309=\"Select Model\", \"\",IF(OR($T309=\"ACBC_1W\",$T309=\"ACBC_2W\",LEFT($T309,4)=\"ACBR\",$T309 = \"LIU24_2W\",LEFT($T309,3)=\"RIU\",LEFT($T309,6)=\"ACBL12\"), IF((soundLevel($T309, $AB309, BD309, $Y309, $W309,$AJ309,$AA309,\"dba\"))<15,\"<15\",soundLevel($T309, $AB309, BD309, $Y309, $W309,$AJ309,$AA309,\"dba\")+0.4),IF((soundLevel($T309, $AB309, BD309, $Y309, $W309,$AJ309,$AA309,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T309, $AB309, BD309, $Y309, $W309,$AJ309,$AA309,\"dba\")+5)<15, \"<15\", soundLevel($T309, $AB309, BD309,$Y309, $W309,$AJ309,$AA309,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T309=\"Select Model\", \"\",IF(OR($T309=\"ACBC_1W\",$T309=\"ACBC_2W\",LEFT($T309,4)=\"ACBR\",$T309=\"LIU24_2W\",LEFT($T309,3)=\"RIU\",LEFT($T309,6)=\"ACBL12\"), IF((soundLevel($T309, $AB309, BD309, $Y309, $W309,$AJ309,$AA309,\"NC\"))<15,\"<15\",soundLevel($T309, $AB309, BD309, $Y309, $W309,$AJ309,$AA309,\"NC\")+0.4),IF((soundLevel($T309, $AB309, BD309, $Y309, $W309,$AJ309,$AA309,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T309, $AB309, BD309, $Y309, $W309,$AJ309,$AA309,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T309, $AB309, BD309, $Y309, $W309,$AJ309,$AA309,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T309=\"Select Model\",\"\",IF($T309=\"LIU24_2W\",calcQwIP($Y309,$W309,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC309,$AI309,\"latent\",$U309&\"P\"&IF($V309=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T309,activeElevation),\"\"))","v":""},{"$f":"IF($T309=\"Select Model\",\"\",IF($T309=\"ACBC_1W\",calcQwIP($Y309,$W309,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC309,BD309,\"capacity\",$U309&\"P\"&IF($V309=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T309,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y309,$W309,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC309,BD309,\"capacity\",$U309&\"P\"&IF($V309=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T309,activeElevation)))","v":""},"",{"$f":"IF(T309=\"Select Model\", 0,waterPressureDrop(W309, U309 & \"P\" & IF(V309=\"Dual\",2,1) &\"C\", AC309, \"cooling\", T309))","v":0},{"$f":"IF(T309=\"Select Model\", \"\",getReturnWaterTemp(T309,AC309, activeEWTCooling, AS309, \"cooling\"))","v":""},"",{"$f":"IF($T309<>\"ACBC_1W\",\"\",IF($J309=\"\",\"\",FintubeCapacity($T309,$W309,$AE309,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T309=\"Select Model\",T309=\"PCBL\"),\"\",calcQwIP(Y309,W309,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD309,BD309,\"capacity\",U309&\"P\"&IF(V309=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T309,activeElevation))","v":""},"",{"$f":"IF(OR(T309=\"Select Model\",T309=\"PCBL\"), \"\",IF(AY309=0,\"N/A\",waterPressureDrop(W309, U309 & \"P\" & IF(V309=\"Dual\",2,1) &\"C\", AD309, \"heating\", T309)))","v":""},{"$f":"IF(OR(T309=\"Select Model\",T309=\"PCBL\"), \"\",IF(AY309=0,getReturnWaterTemp(T309,AE309, activeEWTHeating, AX309, \"heating\"),getReturnWaterTemp(T309,AD309, activeEWTHeating, AY309, \"heating\")))","v":""},"",{"$f":" getNozzle(T309, W309, Y309, Z309, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I310)),I310<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I310, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H310)),H310<0),\"\",intlEstQuantity(T310, W310*12, H310)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T310=\"Select Model\",\"\",coilCircuitChange(W310, U310, AC310, T310,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T310=\"Select Model\",\"\",beamWidth(T310))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T310=\"Select Model\",T310=\"PCBL\"), 0,getSPIP(T310, W310, Y310, BD310, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T310=\"Select Model\", \"\",IF(T310=\"PCBL\",0,primaryAirSensibleCapacityIP($T310,$W310,activeRoomTempCooling,activePriAirTempCooling,$Y310,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T310=\"Select Model\",\"\",IF($T310=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y310,activeElevation)))","v":""},{"$f":"IF(OR(T310=\"Select Model\",T310=\"PCBL\"), 0,IF(AD310=0,0,-primaryAirSensibleCapacityIP($T310,$W310,activeRoomTempHeating,activePriAirTempHeating,$Y310,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T310=\"Select Model\", \"\", InductionRatio($T310,BD310,$W310,$Y310)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T310=\"Select Model\", \"\",IF($T310=\"PCBL\",\"N/A\",minVAVSetBack(AA310, Y310))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T310=\"Select Model\", \"\",IF($T310= \"PCBL\",\"N/A\",getDischargeAirTemp($T310,$V310,$AC310,$W310,BD310,$AL310, $Y310, $AS310, \"cooling\",activeElevation,$AB310,$AJ310,$AV310,$BB310))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T310=\"Select Model\",$T310=\"PCBL\"), \"\",getDischargeAirTemp($T310,$V310,$AD310,$W310,BD310,$AL310, $Y310, $AY310, \"heating\",activeElevation,$AB310,$AJ310,$AV310,$BB310)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T310=\"Select Model\", \"\",IF(OR($T310=\"ACBC_1W\",$T310=\"ACBC_2W\",LEFT($T310,4)=\"ACBR\",$T310 = \"LIU24_2W\",LEFT($T310,3)=\"RIU\",LEFT($T310,6)=\"ACBL12\"), IF((soundLevel($T310, $AB310, BD310, $Y310, $W310,$AJ310,$AA310,\"dba\"))<15,\"<15\",soundLevel($T310, $AB310, BD310, $Y310, $W310,$AJ310,$AA310,\"dba\")+0.4),IF((soundLevel($T310, $AB310, BD310, $Y310, $W310,$AJ310,$AA310,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T310, $AB310, BD310, $Y310, $W310,$AJ310,$AA310,\"dba\")+5)<15, \"<15\", soundLevel($T310, $AB310, BD310,$Y310, $W310,$AJ310,$AA310,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T310=\"Select Model\", \"\",IF(OR($T310=\"ACBC_1W\",$T310=\"ACBC_2W\",LEFT($T310,4)=\"ACBR\",$T310=\"LIU24_2W\",LEFT($T310,3)=\"RIU\",LEFT($T310,6)=\"ACBL12\"), IF((soundLevel($T310, $AB310, BD310, $Y310, $W310,$AJ310,$AA310,\"NC\"))<15,\"<15\",soundLevel($T310, $AB310, BD310, $Y310, $W310,$AJ310,$AA310,\"NC\")+0.4),IF((soundLevel($T310, $AB310, BD310, $Y310, $W310,$AJ310,$AA310,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T310, $AB310, BD310, $Y310, $W310,$AJ310,$AA310,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T310, $AB310, BD310, $Y310, $W310,$AJ310,$AA310,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T310=\"Select Model\",\"\",IF($T310=\"LIU24_2W\",calcQwIP($Y310,$W310,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC310,$AI310,\"latent\",$U310&\"P\"&IF($V310=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T310,activeElevation),\"\"))","v":""},{"$f":"IF($T310=\"Select Model\",\"\",IF($T310=\"ACBC_1W\",calcQwIP($Y310,$W310,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC310,BD310,\"capacity\",$U310&\"P\"&IF($V310=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T310,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y310,$W310,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC310,BD310,\"capacity\",$U310&\"P\"&IF($V310=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T310,activeElevation)))","v":""},"",{"$f":"IF(T310=\"Select Model\", 0,waterPressureDrop(W310, U310 & \"P\" & IF(V310=\"Dual\",2,1) &\"C\", AC310, \"cooling\", T310))","v":0},{"$f":"IF(T310=\"Select Model\", \"\",getReturnWaterTemp(T310,AC310, activeEWTCooling, AS310, \"cooling\"))","v":""},"",{"$f":"IF($T310<>\"ACBC_1W\",\"\",IF($J310=\"\",\"\",FintubeCapacity($T310,$W310,$AE310,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T310=\"Select Model\",T310=\"PCBL\"),\"\",calcQwIP(Y310,W310,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD310,BD310,\"capacity\",U310&\"P\"&IF(V310=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T310,activeElevation))","v":""},"",{"$f":"IF(OR(T310=\"Select Model\",T310=\"PCBL\"), \"\",IF(AY310=0,\"N/A\",waterPressureDrop(W310, U310 & \"P\" & IF(V310=\"Dual\",2,1) &\"C\", AD310, \"heating\", T310)))","v":""},{"$f":"IF(OR(T310=\"Select Model\",T310=\"PCBL\"), \"\",IF(AY310=0,getReturnWaterTemp(T310,AE310, activeEWTHeating, AX310, \"heating\"),getReturnWaterTemp(T310,AD310, activeEWTHeating, AY310, \"heating\")))","v":""},"",{"$f":" getNozzle(T310, W310, Y310, Z310, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I311)),I311<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I311, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H311)),H311<0),\"\",intlEstQuantity(T311, W311*12, H311)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T311=\"Select Model\",\"\",coilCircuitChange(W311, U311, AC311, T311,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T311=\"Select Model\",\"\",beamWidth(T311))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T311=\"Select Model\",T311=\"PCBL\"), 0,getSPIP(T311, W311, Y311, BD311, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T311=\"Select Model\", \"\",IF(T311=\"PCBL\",0,primaryAirSensibleCapacityIP($T311,$W311,activeRoomTempCooling,activePriAirTempCooling,$Y311,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T311=\"Select Model\",\"\",IF($T311=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y311,activeElevation)))","v":""},{"$f":"IF(OR(T311=\"Select Model\",T311=\"PCBL\"), 0,IF(AD311=0,0,-primaryAirSensibleCapacityIP($T311,$W311,activeRoomTempHeating,activePriAirTempHeating,$Y311,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T311=\"Select Model\", \"\", InductionRatio($T311,BD311,$W311,$Y311)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T311=\"Select Model\", \"\",IF($T311=\"PCBL\",\"N/A\",minVAVSetBack(AA311, Y311))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T311=\"Select Model\", \"\",IF($T311= \"PCBL\",\"N/A\",getDischargeAirTemp($T311,$V311,$AC311,$W311,BD311,$AL311, $Y311, $AS311, \"cooling\",activeElevation,$AB311,$AJ311,$AV311,$BB311))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T311=\"Select Model\",$T311=\"PCBL\"), \"\",getDischargeAirTemp($T311,$V311,$AD311,$W311,BD311,$AL311, $Y311, $AY311, \"heating\",activeElevation,$AB311,$AJ311,$AV311,$BB311)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T311=\"Select Model\", \"\",IF(OR($T311=\"ACBC_1W\",$T311=\"ACBC_2W\",LEFT($T311,4)=\"ACBR\",$T311 = \"LIU24_2W\",LEFT($T311,3)=\"RIU\",LEFT($T311,6)=\"ACBL12\"), IF((soundLevel($T311, $AB311, BD311, $Y311, $W311,$AJ311,$AA311,\"dba\"))<15,\"<15\",soundLevel($T311, $AB311, BD311, $Y311, $W311,$AJ311,$AA311,\"dba\")+0.4),IF((soundLevel($T311, $AB311, BD311, $Y311, $W311,$AJ311,$AA311,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T311, $AB311, BD311, $Y311, $W311,$AJ311,$AA311,\"dba\")+5)<15, \"<15\", soundLevel($T311, $AB311, BD311,$Y311, $W311,$AJ311,$AA311,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T311=\"Select Model\", \"\",IF(OR($T311=\"ACBC_1W\",$T311=\"ACBC_2W\",LEFT($T311,4)=\"ACBR\",$T311=\"LIU24_2W\",LEFT($T311,3)=\"RIU\",LEFT($T311,6)=\"ACBL12\"), IF((soundLevel($T311, $AB311, BD311, $Y311, $W311,$AJ311,$AA311,\"NC\"))<15,\"<15\",soundLevel($T311, $AB311, BD311, $Y311, $W311,$AJ311,$AA311,\"NC\")+0.4),IF((soundLevel($T311, $AB311, BD311, $Y311, $W311,$AJ311,$AA311,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T311, $AB311, BD311, $Y311, $W311,$AJ311,$AA311,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T311, $AB311, BD311, $Y311, $W311,$AJ311,$AA311,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T311=\"Select Model\",\"\",IF($T311=\"LIU24_2W\",calcQwIP($Y311,$W311,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC311,$AI311,\"latent\",$U311&\"P\"&IF($V311=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T311,activeElevation),\"\"))","v":""},{"$f":"IF($T311=\"Select Model\",\"\",IF($T311=\"ACBC_1W\",calcQwIP($Y311,$W311,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC311,BD311,\"capacity\",$U311&\"P\"&IF($V311=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T311,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y311,$W311,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC311,BD311,\"capacity\",$U311&\"P\"&IF($V311=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T311,activeElevation)))","v":""},"",{"$f":"IF(T311=\"Select Model\", 0,waterPressureDrop(W311, U311 & \"P\" & IF(V311=\"Dual\",2,1) &\"C\", AC311, \"cooling\", T311))","v":0},{"$f":"IF(T311=\"Select Model\", \"\",getReturnWaterTemp(T311,AC311, activeEWTCooling, AS311, \"cooling\"))","v":""},"",{"$f":"IF($T311<>\"ACBC_1W\",\"\",IF($J311=\"\",\"\",FintubeCapacity($T311,$W311,$AE311,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T311=\"Select Model\",T311=\"PCBL\"),\"\",calcQwIP(Y311,W311,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD311,BD311,\"capacity\",U311&\"P\"&IF(V311=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T311,activeElevation))","v":""},"",{"$f":"IF(OR(T311=\"Select Model\",T311=\"PCBL\"), \"\",IF(AY311=0,\"N/A\",waterPressureDrop(W311, U311 & \"P\" & IF(V311=\"Dual\",2,1) &\"C\", AD311, \"heating\", T311)))","v":""},{"$f":"IF(OR(T311=\"Select Model\",T311=\"PCBL\"), \"\",IF(AY311=0,getReturnWaterTemp(T311,AE311, activeEWTHeating, AX311, \"heating\"),getReturnWaterTemp(T311,AD311, activeEWTHeating, AY311, \"heating\")))","v":""},"",{"$f":" getNozzle(T311, W311, Y311, Z311, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I312)),I312<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I312, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H312)),H312<0),\"\",intlEstQuantity(T312, W312*12, H312)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T312=\"Select Model\",\"\",coilCircuitChange(W312, U312, AC312, T312,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T312=\"Select Model\",\"\",beamWidth(T312))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T312=\"Select Model\",T312=\"PCBL\"), 0,getSPIP(T312, W312, Y312, BD312, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T312=\"Select Model\", \"\",IF(T312=\"PCBL\",0,primaryAirSensibleCapacityIP($T312,$W312,activeRoomTempCooling,activePriAirTempCooling,$Y312,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T312=\"Select Model\",\"\",IF($T312=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y312,activeElevation)))","v":""},{"$f":"IF(OR(T312=\"Select Model\",T312=\"PCBL\"), 0,IF(AD312=0,0,-primaryAirSensibleCapacityIP($T312,$W312,activeRoomTempHeating,activePriAirTempHeating,$Y312,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T312=\"Select Model\", \"\", InductionRatio($T312,BD312,$W312,$Y312)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T312=\"Select Model\", \"\",IF($T312=\"PCBL\",\"N/A\",minVAVSetBack(AA312, Y312))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T312=\"Select Model\", \"\",IF($T312= \"PCBL\",\"N/A\",getDischargeAirTemp($T312,$V312,$AC312,$W312,BD312,$AL312, $Y312, $AS312, \"cooling\",activeElevation,$AB312,$AJ312,$AV312,$BB312))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T312=\"Select Model\",$T312=\"PCBL\"), \"\",getDischargeAirTemp($T312,$V312,$AD312,$W312,BD312,$AL312, $Y312, $AY312, \"heating\",activeElevation,$AB312,$AJ312,$AV312,$BB312)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T312=\"Select Model\", \"\",IF(OR($T312=\"ACBC_1W\",$T312=\"ACBC_2W\",LEFT($T312,4)=\"ACBR\",$T312 = \"LIU24_2W\",LEFT($T312,3)=\"RIU\",LEFT($T312,6)=\"ACBL12\"), IF((soundLevel($T312, $AB312, BD312, $Y312, $W312,$AJ312,$AA312,\"dba\"))<15,\"<15\",soundLevel($T312, $AB312, BD312, $Y312, $W312,$AJ312,$AA312,\"dba\")+0.4),IF((soundLevel($T312, $AB312, BD312, $Y312, $W312,$AJ312,$AA312,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T312, $AB312, BD312, $Y312, $W312,$AJ312,$AA312,\"dba\")+5)<15, \"<15\", soundLevel($T312, $AB312, BD312,$Y312, $W312,$AJ312,$AA312,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T312=\"Select Model\", \"\",IF(OR($T312=\"ACBC_1W\",$T312=\"ACBC_2W\",LEFT($T312,4)=\"ACBR\",$T312=\"LIU24_2W\",LEFT($T312,3)=\"RIU\",LEFT($T312,6)=\"ACBL12\"), IF((soundLevel($T312, $AB312, BD312, $Y312, $W312,$AJ312,$AA312,\"NC\"))<15,\"<15\",soundLevel($T312, $AB312, BD312, $Y312, $W312,$AJ312,$AA312,\"NC\")+0.4),IF((soundLevel($T312, $AB312, BD312, $Y312, $W312,$AJ312,$AA312,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T312, $AB312, BD312, $Y312, $W312,$AJ312,$AA312,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T312, $AB312, BD312, $Y312, $W312,$AJ312,$AA312,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T312=\"Select Model\",\"\",IF($T312=\"LIU24_2W\",calcQwIP($Y312,$W312,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC312,$AI312,\"latent\",$U312&\"P\"&IF($V312=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T312,activeElevation),\"\"))","v":""},{"$f":"IF($T312=\"Select Model\",\"\",IF($T312=\"ACBC_1W\",calcQwIP($Y312,$W312,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC312,BD312,\"capacity\",$U312&\"P\"&IF($V312=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T312,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y312,$W312,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC312,BD312,\"capacity\",$U312&\"P\"&IF($V312=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T312,activeElevation)))","v":""},"",{"$f":"IF(T312=\"Select Model\", 0,waterPressureDrop(W312, U312 & \"P\" & IF(V312=\"Dual\",2,1) &\"C\", AC312, \"cooling\", T312))","v":0},{"$f":"IF(T312=\"Select Model\", \"\",getReturnWaterTemp(T312,AC312, activeEWTCooling, AS312, \"cooling\"))","v":""},"",{"$f":"IF($T312<>\"ACBC_1W\",\"\",IF($J312=\"\",\"\",FintubeCapacity($T312,$W312,$AE312,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T312=\"Select Model\",T312=\"PCBL\"),\"\",calcQwIP(Y312,W312,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD312,BD312,\"capacity\",U312&\"P\"&IF(V312=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T312,activeElevation))","v":""},"",{"$f":"IF(OR(T312=\"Select Model\",T312=\"PCBL\"), \"\",IF(AY312=0,\"N/A\",waterPressureDrop(W312, U312 & \"P\" & IF(V312=\"Dual\",2,1) &\"C\", AD312, \"heating\", T312)))","v":""},{"$f":"IF(OR(T312=\"Select Model\",T312=\"PCBL\"), \"\",IF(AY312=0,getReturnWaterTemp(T312,AE312, activeEWTHeating, AX312, \"heating\"),getReturnWaterTemp(T312,AD312, activeEWTHeating, AY312, \"heating\")))","v":""},"",{"$f":" getNozzle(T312, W312, Y312, Z312, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I313)),I313<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I313, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H313)),H313<0),\"\",intlEstQuantity(T313, W313*12, H313)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T313=\"Select Model\",\"\",coilCircuitChange(W313, U313, AC313, T313,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T313=\"Select Model\",\"\",beamWidth(T313))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T313=\"Select Model\",T313=\"PCBL\"), 0,getSPIP(T313, W313, Y313, BD313, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T313=\"Select Model\", \"\",IF(T313=\"PCBL\",0,primaryAirSensibleCapacityIP($T313,$W313,activeRoomTempCooling,activePriAirTempCooling,$Y313,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T313=\"Select Model\",\"\",IF($T313=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y313,activeElevation)))","v":""},{"$f":"IF(OR(T313=\"Select Model\",T313=\"PCBL\"), 0,IF(AD313=0,0,-primaryAirSensibleCapacityIP($T313,$W313,activeRoomTempHeating,activePriAirTempHeating,$Y313,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T313=\"Select Model\", \"\", InductionRatio($T313,BD313,$W313,$Y313)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T313=\"Select Model\", \"\",IF($T313=\"PCBL\",\"N/A\",minVAVSetBack(AA313, Y313))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T313=\"Select Model\", \"\",IF($T313= \"PCBL\",\"N/A\",getDischargeAirTemp($T313,$V313,$AC313,$W313,BD313,$AL313, $Y313, $AS313, \"cooling\",activeElevation,$AB313,$AJ313,$AV313,$BB313))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T313=\"Select Model\",$T313=\"PCBL\"), \"\",getDischargeAirTemp($T313,$V313,$AD313,$W313,BD313,$AL313, $Y313, $AY313, \"heating\",activeElevation,$AB313,$AJ313,$AV313,$BB313)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T313=\"Select Model\", \"\",IF(OR($T313=\"ACBC_1W\",$T313=\"ACBC_2W\",LEFT($T313,4)=\"ACBR\",$T313 = \"LIU24_2W\",LEFT($T313,3)=\"RIU\",LEFT($T313,6)=\"ACBL12\"), IF((soundLevel($T313, $AB313, BD313, $Y313, $W313,$AJ313,$AA313,\"dba\"))<15,\"<15\",soundLevel($T313, $AB313, BD313, $Y313, $W313,$AJ313,$AA313,\"dba\")+0.4),IF((soundLevel($T313, $AB313, BD313, $Y313, $W313,$AJ313,$AA313,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T313, $AB313, BD313, $Y313, $W313,$AJ313,$AA313,\"dba\")+5)<15, \"<15\", soundLevel($T313, $AB313, BD313,$Y313, $W313,$AJ313,$AA313,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T313=\"Select Model\", \"\",IF(OR($T313=\"ACBC_1W\",$T313=\"ACBC_2W\",LEFT($T313,4)=\"ACBR\",$T313=\"LIU24_2W\",LEFT($T313,3)=\"RIU\",LEFT($T313,6)=\"ACBL12\"), IF((soundLevel($T313, $AB313, BD313, $Y313, $W313,$AJ313,$AA313,\"NC\"))<15,\"<15\",soundLevel($T313, $AB313, BD313, $Y313, $W313,$AJ313,$AA313,\"NC\")+0.4),IF((soundLevel($T313, $AB313, BD313, $Y313, $W313,$AJ313,$AA313,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T313, $AB313, BD313, $Y313, $W313,$AJ313,$AA313,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T313, $AB313, BD313, $Y313, $W313,$AJ313,$AA313,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T313=\"Select Model\",\"\",IF($T313=\"LIU24_2W\",calcQwIP($Y313,$W313,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC313,$AI313,\"latent\",$U313&\"P\"&IF($V313=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T313,activeElevation),\"\"))","v":""},{"$f":"IF($T313=\"Select Model\",\"\",IF($T313=\"ACBC_1W\",calcQwIP($Y313,$W313,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC313,BD313,\"capacity\",$U313&\"P\"&IF($V313=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T313,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y313,$W313,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC313,BD313,\"capacity\",$U313&\"P\"&IF($V313=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T313,activeElevation)))","v":""},"",{"$f":"IF(T313=\"Select Model\", 0,waterPressureDrop(W313, U313 & \"P\" & IF(V313=\"Dual\",2,1) &\"C\", AC313, \"cooling\", T313))","v":0},{"$f":"IF(T313=\"Select Model\", \"\",getReturnWaterTemp(T313,AC313, activeEWTCooling, AS313, \"cooling\"))","v":""},"",{"$f":"IF($T313<>\"ACBC_1W\",\"\",IF($J313=\"\",\"\",FintubeCapacity($T313,$W313,$AE313,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T313=\"Select Model\",T313=\"PCBL\"),\"\",calcQwIP(Y313,W313,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD313,BD313,\"capacity\",U313&\"P\"&IF(V313=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T313,activeElevation))","v":""},"",{"$f":"IF(OR(T313=\"Select Model\",T313=\"PCBL\"), \"\",IF(AY313=0,\"N/A\",waterPressureDrop(W313, U313 & \"P\" & IF(V313=\"Dual\",2,1) &\"C\", AD313, \"heating\", T313)))","v":""},{"$f":"IF(OR(T313=\"Select Model\",T313=\"PCBL\"), \"\",IF(AY313=0,getReturnWaterTemp(T313,AE313, activeEWTHeating, AX313, \"heating\"),getReturnWaterTemp(T313,AD313, activeEWTHeating, AY313, \"heating\")))","v":""},"",{"$f":" getNozzle(T313, W313, Y313, Z313, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I314)),I314<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I314, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H314)),H314<0),\"\",intlEstQuantity(T314, W314*12, H314)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T314=\"Select Model\",\"\",coilCircuitChange(W314, U314, AC314, T314,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T314=\"Select Model\",\"\",beamWidth(T314))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T314=\"Select Model\",T314=\"PCBL\"), 0,getSPIP(T314, W314, Y314, BD314, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T314=\"Select Model\", \"\",IF(T314=\"PCBL\",0,primaryAirSensibleCapacityIP($T314,$W314,activeRoomTempCooling,activePriAirTempCooling,$Y314,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T314=\"Select Model\",\"\",IF($T314=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y314,activeElevation)))","v":""},{"$f":"IF(OR(T314=\"Select Model\",T314=\"PCBL\"), 0,IF(AD314=0,0,-primaryAirSensibleCapacityIP($T314,$W314,activeRoomTempHeating,activePriAirTempHeating,$Y314,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T314=\"Select Model\", \"\", InductionRatio($T314,BD314,$W314,$Y314)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T314=\"Select Model\", \"\",IF($T314=\"PCBL\",\"N/A\",minVAVSetBack(AA314, Y314))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T314=\"Select Model\", \"\",IF($T314= \"PCBL\",\"N/A\",getDischargeAirTemp($T314,$V314,$AC314,$W314,BD314,$AL314, $Y314, $AS314, \"cooling\",activeElevation,$AB314,$AJ314,$AV314,$BB314))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T314=\"Select Model\",$T314=\"PCBL\"), \"\",getDischargeAirTemp($T314,$V314,$AD314,$W314,BD314,$AL314, $Y314, $AY314, \"heating\",activeElevation,$AB314,$AJ314,$AV314,$BB314)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T314=\"Select Model\", \"\",IF(OR($T314=\"ACBC_1W\",$T314=\"ACBC_2W\",LEFT($T314,4)=\"ACBR\",$T314 = \"LIU24_2W\",LEFT($T314,3)=\"RIU\",LEFT($T314,6)=\"ACBL12\"), IF((soundLevel($T314, $AB314, BD314, $Y314, $W314,$AJ314,$AA314,\"dba\"))<15,\"<15\",soundLevel($T314, $AB314, BD314, $Y314, $W314,$AJ314,$AA314,\"dba\")+0.4),IF((soundLevel($T314, $AB314, BD314, $Y314, $W314,$AJ314,$AA314,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T314, $AB314, BD314, $Y314, $W314,$AJ314,$AA314,\"dba\")+5)<15, \"<15\", soundLevel($T314, $AB314, BD314,$Y314, $W314,$AJ314,$AA314,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T314=\"Select Model\", \"\",IF(OR($T314=\"ACBC_1W\",$T314=\"ACBC_2W\",LEFT($T314,4)=\"ACBR\",$T314=\"LIU24_2W\",LEFT($T314,3)=\"RIU\",LEFT($T314,6)=\"ACBL12\"), IF((soundLevel($T314, $AB314, BD314, $Y314, $W314,$AJ314,$AA314,\"NC\"))<15,\"<15\",soundLevel($T314, $AB314, BD314, $Y314, $W314,$AJ314,$AA314,\"NC\")+0.4),IF((soundLevel($T314, $AB314, BD314, $Y314, $W314,$AJ314,$AA314,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T314, $AB314, BD314, $Y314, $W314,$AJ314,$AA314,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T314, $AB314, BD314, $Y314, $W314,$AJ314,$AA314,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T314=\"Select Model\",\"\",IF($T314=\"LIU24_2W\",calcQwIP($Y314,$W314,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC314,$AI314,\"latent\",$U314&\"P\"&IF($V314=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T314,activeElevation),\"\"))","v":""},{"$f":"IF($T314=\"Select Model\",\"\",IF($T314=\"ACBC_1W\",calcQwIP($Y314,$W314,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC314,BD314,\"capacity\",$U314&\"P\"&IF($V314=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T314,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y314,$W314,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC314,BD314,\"capacity\",$U314&\"P\"&IF($V314=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T314,activeElevation)))","v":""},"",{"$f":"IF(T314=\"Select Model\", 0,waterPressureDrop(W314, U314 & \"P\" & IF(V314=\"Dual\",2,1) &\"C\", AC314, \"cooling\", T314))","v":0},{"$f":"IF(T314=\"Select Model\", \"\",getReturnWaterTemp(T314,AC314, activeEWTCooling, AS314, \"cooling\"))","v":""},"",{"$f":"IF($T314<>\"ACBC_1W\",\"\",IF($J314=\"\",\"\",FintubeCapacity($T314,$W314,$AE314,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T314=\"Select Model\",T314=\"PCBL\"),\"\",calcQwIP(Y314,W314,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD314,BD314,\"capacity\",U314&\"P\"&IF(V314=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T314,activeElevation))","v":""},"",{"$f":"IF(OR(T314=\"Select Model\",T314=\"PCBL\"), \"\",IF(AY314=0,\"N/A\",waterPressureDrop(W314, U314 & \"P\" & IF(V314=\"Dual\",2,1) &\"C\", AD314, \"heating\", T314)))","v":""},{"$f":"IF(OR(T314=\"Select Model\",T314=\"PCBL\"), \"\",IF(AY314=0,getReturnWaterTemp(T314,AE314, activeEWTHeating, AX314, \"heating\"),getReturnWaterTemp(T314,AD314, activeEWTHeating, AY314, \"heating\")))","v":""},"",{"$f":" getNozzle(T314, W314, Y314, Z314, activeElevation, TRUE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(NOT(ISNUMBER(I315)),I315<0),\"\",getMinAirFromLatentCapIP(activeRoomTempCooling, activeRHCooling, activePriAirTempCooling,activePriAirRHCooling, I315, activeElevation))","v":""},{"$f":"IFERROR(IF(OR(NOT(ISNUMBER(H315)),H315<0),\"\",intlEstQuantity(T315, W315*12, H315)),1)","v":""},"","","","","",false,"Default","Select Model",2,{"$f":"IF(T315=\"Select Model\",\"\",coilCircuitChange(W315, U315, AC315, T315,activeMaxWaterPressureDrop))","v":""},4,{"$f":"IF(T315=\"Select Model\",\"\",beamWidth(T315))","v":""},50,0.75,{"$f":"IFERROR(IF(OR(T315=\"Select Model\",T315=\"PCBL\"), 0,getSPIP(T315, W315, Y315, BD315, activeElevation)),-1)","v":0},5,0.5,0.5,0,{"$f":"IF(T315=\"Select Model\", \"\",IF(T315=\"PCBL\",0,primaryAirSensibleCapacityIP($T315,$W315,activeRoomTempCooling,activePriAirTempCooling,$Y315,activeElevation,\"cooling\")))","v":""},{"$f":"IF($T315=\"Select Model\",\"\",IF($T315=\"PCBL\",0,primaryAirLatentCapacityIP(activeRoomTempCooling,activeRHCooling,activePriAirTempCooling,activePriAirRHCooling,Y315,activeElevation)))","v":""},{"$f":"IF(OR(T315=\"Select Model\",T315=\"PCBL\"), 0,IF(AD315=0,0,-primaryAirSensibleCapacityIP($T315,$W315,activeRoomTempHeating,activePriAirTempHeating,$Y315,activeElevation,\"heating\")))","v":0},"",{"$f":"IFERROR(IF(T315=\"Select Model\", \"\", InductionRatio($T315,BD315,$W315,$Y315)),\"N/A\")","v":""},"","",{"$f":"IFERROR(IF(T315=\"Select Model\", \"\",IF($T315=\"PCBL\",\"N/A\",minVAVSetBack(AA315, Y315))),\"N/A\")","v":""},{"$f":"IFERROR(IF($T315=\"Select Model\", \"\",IF($T315= \"PCBL\",\"N/A\",getDischargeAirTemp($T315,$V315,$AC315,$W315,BD315,$AL315, $Y315, $AS315, \"cooling\",activeElevation,$AB315,$AJ315,$AV315,$BB315))),\"N/A\")","v":""},{"$f":"IFERROR(IF(OR($T315=\"Select Model\",$T315=\"PCBL\"), \"\",getDischargeAirTemp($T315,$V315,$AD315,$W315,BD315,$AL315, $Y315, $AY315, \"heating\",activeElevation,$AB315,$AJ315,$AV315,$BB315)),\"N/A\")","v":""},{"$f":"IFERROR(IF($T315=\"Select Model\", \"\",IF(OR($T315=\"ACBC_1W\",$T315=\"ACBC_2W\",LEFT($T315,4)=\"ACBR\",$T315 = \"LIU24_2W\",LEFT($T315,3)=\"RIU\",LEFT($T315,6)=\"ACBL12\"), IF((soundLevel($T315, $AB315, BD315, $Y315, $W315,$AJ315,$AA315,\"dba\"))<15,\"<15\",soundLevel($T315, $AB315, BD315, $Y315, $W315,$AJ315,$AA315,\"dba\")+0.4),IF((soundLevel($T315, $AB315, BD315, $Y315, $W315,$AJ315,$AA315,\"dba\")+5)<0, \"N/A\", IF((soundLevel($T315, $AB315, BD315, $Y315, $W315,$AJ315,$AA315,\"dba\")+5)<15, \"<15\", soundLevel($T315, $AB315, BD315,$Y315, $W315,$AJ315,$AA315,\"dba\")+5)))),\"<15\")","v":""},{"$f":"IFERROR(IF($T315=\"Select Model\", \"\",IF(OR($T315=\"ACBC_1W\",$T315=\"ACBC_2W\",LEFT($T315,4)=\"ACBR\",$T315=\"LIU24_2W\",LEFT($T315,3)=\"RIU\",LEFT($T315,6)=\"ACBL12\"), IF((soundLevel($T315, $AB315, BD315, $Y315, $W315,$AJ315,$AA315,\"NC\"))<15,\"<15\",soundLevel($T315, $AB315, BD315, $Y315, $W315,$AJ315,$AA315,\"NC\")+0.4),IF((soundLevel($T315, $AB315, BD315, $Y315, $W315,$AJ315,$AA315,\"NC\")+0.4)<0, \"N/A\", IF((soundLevel($T315, $AB315, BD315, $Y315, $W315,$AJ315,$AA315,\"NC\")-activeRoomAttenuation)<15, \"<15\", soundLevel($T315, $AB315, BD315, $Y315, $W315,$AJ315,$AA315,\"NC\")-activeRoomAttenuation)))),\"<15\")","v":""},{"$f":"IF($T315=\"Select Model\",\"\",IF($T315=\"LIU24_2W\",calcQwIP($Y315,$W315,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC315,$AI315,\"latent\",$U315&\"P\"&IF($V315=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T315,activeElevation),\"\"))","v":""},{"$f":"IF($T315=\"Select Model\",\"\",IF($T315=\"ACBC_1W\",calcQwIP($Y315,$W315,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC315,BD315,\"capacity\",$U315&\"P\"&IF($V315=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T315,activeElevation)*(1+activeStratificationCredit),calcQwIP($Y315,$W315,activeOnCoilTempCooling,activeRoomDewPointCooling,activeEWTCooling,$AC315,BD315,\"capacity\",$U315&\"P\"&IF($V315=\"Dual\",2,1)&\"C\",activeFluidTypeCooling,activeGlycolConCooling,\"cooling\",$T315,activeElevation)))","v":""},"",{"$f":"IF(T315=\"Select Model\", 0,waterPressureDrop(W315, U315 & \"P\" & IF(V315=\"Dual\",2,1) &\"C\", AC315, \"cooling\", T315))","v":0},{"$f":"IF(T315=\"Select Model\", \"\",getReturnWaterTemp(T315,AC315, activeEWTCooling, AS315, \"cooling\"))","v":""},"",{"$f":"IF($T315<>\"ACBC_1W\",\"\",IF($J315=\"\",\"\",FintubeCapacity($T315,$W315,$AE315,activeEWTHeating,activeOnCoilTempHeating)))","v":""},{"$f":"IF(OR(T315=\"Select Model\",T315=\"PCBL\"),\"\",calcQwIP(Y315,W315,activeOnCoilTempHeating,activeRoomDewPointCooling,activeEWTHeating,AD315,BD315,\"capacity\",U315&\"P\"&IF(V315=\"Dual\",2,1)&\"C\",activeFluidTypeHeating,activeGlycolConHeating,\"heating\",T315,activeElevation))","v":""},"",{"$f":"IF(OR(T315=\"Select Model\",T315=\"PCBL\"), \"\",IF(AY315=0,\"N/A\",waterPressureDrop(W315, U315 & \"P\" & IF(V315=\"Dual\",2,1) &\"C\", AD315, \"heating\", T315)))","v":""},{"$f":"IF(OR(T315=\"Select Model\",T315=\"PCBL\"), \"\",IF(AY315=0,getReturnWaterTemp(T315,AE315, activeEWTHeating, AX315, \"heating\"),getReturnWaterTemp(T315,AD315, activeEWTHeating, AY315, \"heating\")))","v":""},"",{"$f":" getNozzle(T315, W315, Y315, Z315, activeElevation, TRUE)","v":0}]

{"sheet":"Estimation Schedule","index":2,"n_rows":302,"n_cols":19,"rows_kept":302,"cut":false,"hidden":true,"merged":[]}
["Tags","QTY","Model","Piping","Circuitry","Length","Inlet Size",null,null,null,null,null,"Tag","Qty","Model","Piping","Circuitry","Length","Inlet Size"]
[1,1,"ACBL24_1W",2,"Single",6,5,null,null,null,null,null,{"$f":"IF('Run Selections'!T15=\"Select Model\", \"\", 'Run Selections'!F15)","v":""},{"$f":"IF('Run Selections'!T15=\"Select Model\", \"\", 'Run Selections'!L15)","v":""},{"$f":"IF('Run Selections'!T15=\"Select Model\", \"\", 'Run Selections'!T15)","v":""},{"$f":"IF('Run Selections'!T15=\"Select Model\", \"\", 'Run Selections'!U15)","v":""},{"$f":"IF('Run Selections'!T15=\"Select Model\", \"\", 'Run Selections'!V15)","v":""},{"$f":"IF('Run Selections'!T15=\"Select Model\", \"\", 'Run Selections'!W15)","v":""},{"$f":"IF('Run Selections'!T15=\"Select Model\", \"\", 'Run Selections'!AB15)","v":""}]
[2,1,"ACBL12_1W",2,"Single",6,5,null,null,null,null,null,{"$f":"IF('Run Selections'!T16=\"Select Model\", \"\", 'Run Selections'!F16)","v":""},{"$f":"IF('Run Selections'!T16=\"Select Model\", \"\", 'Run Selections'!L16)","v":""},{"$f":"IF('Run Selections'!T16=\"Select Model\", \"\", 'Run Selections'!T16)","v":""},{"$f":"IF('Run Selections'!T16=\"Select Model\", \"\", 'Run Selections'!U16)","v":""},{"$f":"IF('Run Selections'!T16=\"Select Model\", \"\", 'Run Selections'!V16)","v":""},{"$f":"IF('Run Selections'!T16=\"Select Model\", \"\", 'Run Selections'!W16)","v":""},{"$f":"IF('Run Selections'!T16=\"Select Model\", \"\", 'Run Selections'!AB16)","v":""}]
[3,1,"ACBL12_2W",2,"Single",4,5,null,null,null,null,null,{"$f":"IF('Run Selections'!T17=\"Select Model\", \"\", 'Run Selections'!F17)","v":""},{"$f":"IF('Run Selections'!T17=\"Select Model\", \"\", 'Run Selections'!L17)","v":""},{"$f":"IF('Run Selections'!T17=\"Select Model\", \"\", 'Run Selections'!T17)","v":""},{"$f":"IF('Run Selections'!T17=\"Select Model\", \"\", 'Run Selections'!U17)","v":""},{"$f":"IF('Run Selections'!T17=\"Select Model\", \"\", 'Run Selections'!V17)","v":""},{"$f":"IF('Run Selections'!T17=\"Select Model\", \"\", 'Run Selections'!W17)","v":""},{"$f":"IF('Run Selections'!T17=\"Select Model\", \"\", 'Run Selections'!AB17)","v":""}]
[4,1,"ACBL24_2W",2,"Single",4,5,null,null,null,null,null,{"$f":"IF('Run Selections'!T18=\"Select Model\", \"\", 'Run Selections'!F18)","v":""},{"$f":"IF('Run Selections'!T18=\"Select Model\", \"\", 'Run Selections'!L18)","v":""},{"$f":"IF('Run Selections'!T18=\"Select Model\", \"\", 'Run Selections'!T18)","v":""},{"$f":"IF('Run Selections'!T18=\"Select Model\", \"\", 'Run Selections'!U18)","v":""},{"$f":"IF('Run Selections'!T18=\"Select Model\", \"\", 'Run Selections'!V18)","v":""},{"$f":"IF('Run Selections'!T18=\"Select Model\", \"\", 'Run Selections'!W18)","v":""},{"$f":"IF('Run Selections'!T18=\"Select Model\", \"\", 'Run Selections'!AB18)","v":""}]
[5,1,"ACBC_1W",2,"Single",5,"6E",null,null,null,null,null,{"$f":"IF('Run Selections'!T19=\"Select Model\", \"\", 'Run Selections'!F19)","v":""},{"$f":"IF('Run Selections'!T19=\"Select Model\", \"\", 'Run Selections'!L19)","v":""},{"$f":"IF('Run Selections'!T19=\"Select Model\", \"\", 'Run Selections'!T19)","v":""},{"$f":"IF('Run Selections'!T19=\"Select Model\", \"\", 'Run Selections'!U19)","v":""},{"$f":"IF('Run Selections'!T19=\"Select Model\", \"\", 'Run Selections'!V19)","v":""},{"$f":"IF('Run Selections'!T19=\"Select Model\", \"\", 'Run Selections'!W19)","v":""},{"$f":"IF('Run Selections'!T19=\"Select Model\", \"\", 'Run Selections'!AB19)","v":""}]
[6,1,"ACBC_2W",4,"Single",4,"6E",null,null,null,null,null,{"$f":"IF('Run Selections'!T20=\"Select Model\", \"\", 'Run Selections'!F20)","v":""},{"$f":"IF('Run Selections'!T20=\"Select Model\", \"\", 'Run Selections'!L20)","v":""},{"$f":"IF('Run Selections'!T20=\"Select Model\", \"\", 'Run Selections'!T20)","v":""},{"$f":"IF('Run Selections'!T20=\"Select Model\", \"\", 'Run Selections'!U20)","v":""},{"$f":"IF('Run Selections'!T20=\"Select Model\", \"\", 'Run Selections'!V20)","v":""},{"$f":"IF('Run Selections'!T20=\"Select Model\", \"\", 'Run Selections'!W20)","v":""},{"$f":"IF('Run Selections'!T20=\"Select Model\", \"\", 'Run Selections'!AB20)","v":""}]
[7,1,"ACBR",2,"Single",8,"5eE",null,null,null,null,null,{"$f":"IF('Run Selections'!T21=\"Select Model\", \"\", 'Run Selections'!F21)","v":""},{"$f":"IF('Run Selections'!T21=\"Select Model\", \"\", 'Run Selections'!L21)","v":""},{"$f":"IF('Run Selections'!T21=\"Select Model\", \"\", 'Run Selections'!T21)","v":""},{"$f":"IF('Run Selections'!T21=\"Select Model\", \"\", 'Run Selections'!U21)","v":""},{"$f":"IF('Run Selections'!T21=\"Select Model\", \"\", 'Run Selections'!V21)","v":""},{"$f":"IF('Run Selections'!T21=\"Select Model\", \"\", 'Run Selections'!W21)","v":""},{"$f":"IF('Run Selections'!T21=\"Select Model\", \"\", 'Run Selections'!AB21)","v":""}]
[8,1,"LIU24_2W",2,"Dual",5,8,null,null,null,null,null,{"$f":"IF('Run Selections'!T22=\"Select Model\", \"\", 'Run Selections'!F22)","v":""},{"$f":"IF('Run Selections'!T22=\"Select Model\", \"\", 'Run Selections'!L22)","v":""},{"$f":"IF('Run Selections'!T22=\"Select Model\", \"\", 'Run Selections'!T22)","v":""},{"$f":"IF('Run Selections'!T22=\"Select Model\", \"\", 'Run Selections'!U22)","v":""},{"$f":"IF('Run Selections'!T22=\"Select Model\", \"\", 'Run Selections'!V22)","v":""},{"$f":"IF('Run Selections'!T22=\"Select Model\", \"\", 'Run Selections'!W22)","v":""},{"$f":"IF('Run Selections'!T22=\"Select Model\", \"\", 'Run Selections'!AB22)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T23=\"Select Model\", \"\", 'Run Selections'!F23)","v":""},{"$f":"IF('Run Selections'!T23=\"Select Model\", \"\", 'Run Selections'!L23)","v":""},{"$f":"IF('Run Selections'!T23=\"Select Model\", \"\", 'Run Selections'!T23)","v":""},{"$f":"IF('Run Selections'!T23=\"Select Model\", \"\", 'Run Selections'!U23)","v":""},{"$f":"IF('Run Selections'!T23=\"Select Model\", \"\", 'Run Selections'!V23)","v":""},{"$f":"IF('Run Selections'!T23=\"Select Model\", \"\", 'Run Selections'!W23)","v":""},{"$f":"IF('Run Selections'!T23=\"Select Model\", \"\", 'Run Selections'!AB23)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T24=\"Select Model\", \"\", 'Run Selections'!F24)","v":""},{"$f":"IF('Run Selections'!T24=\"Select Model\", \"\", 'Run Selections'!L24)","v":""},{"$f":"IF('Run Selections'!T24=\"Select Model\", \"\", 'Run Selections'!T24)","v":""},{"$f":"IF('Run Selections'!T24=\"Select Model\", \"\", 'Run Selections'!U24)","v":""},{"$f":"IF('Run Selections'!T24=\"Select Model\", \"\", 'Run Selections'!V24)","v":""},{"$f":"IF('Run Selections'!T24=\"Select Model\", \"\", 'Run Selections'!W24)","v":""},{"$f":"IF('Run Selections'!T24=\"Select Model\", \"\", 'Run Selections'!AB24)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T25=\"Select Model\", \"\", 'Run Selections'!F25)","v":""},{"$f":"IF('Run Selections'!T25=\"Select Model\", \"\", 'Run Selections'!L25)","v":""},{"$f":"IF('Run Selections'!T25=\"Select Model\", \"\", 'Run Selections'!T25)","v":""},{"$f":"IF('Run Selections'!T25=\"Select Model\", \"\", 'Run Selections'!U25)","v":""},{"$f":"IF('Run Selections'!T25=\"Select Model\", \"\", 'Run Selections'!V25)","v":""},{"$f":"IF('Run Selections'!T25=\"Select Model\", \"\", 'Run Selections'!W25)","v":""},{"$f":"IF('Run Selections'!T25=\"Select Model\", \"\", 'Run Selections'!AB25)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T26=\"Select Model\", \"\", 'Run Selections'!F26)","v":""},{"$f":"IF('Run Selections'!T26=\"Select Model\", \"\", 'Run Selections'!L26)","v":""},{"$f":"IF('Run Selections'!T26=\"Select Model\", \"\", 'Run Selections'!T26)","v":""},{"$f":"IF('Run Selections'!T26=\"Select Model\", \"\", 'Run Selections'!U26)","v":""},{"$f":"IF('Run Selections'!T26=\"Select Model\", \"\", 'Run Selections'!V26)","v":""},{"$f":"IF('Run Selections'!T26=\"Select Model\", \"\", 'Run Selections'!W26)","v":""},{"$f":"IF('Run Selections'!T26=\"Select Model\", \"\", 'Run Selections'!AB26)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T27=\"Select Model\", \"\", 'Run Selections'!F27)","v":""},{"$f":"IF('Run Selections'!T27=\"Select Model\", \"\", 'Run Selections'!L27)","v":""},{"$f":"IF('Run Selections'!T27=\"Select Model\", \"\", 'Run Selections'!T27)","v":""},{"$f":"IF('Run Selections'!T27=\"Select Model\", \"\", 'Run Selections'!U27)","v":""},{"$f":"IF('Run Selections'!T27=\"Select Model\", \"\", 'Run Selections'!V27)","v":""},{"$f":"IF('Run Selections'!T27=\"Select Model\", \"\", 'Run Selections'!W27)","v":""},{"$f":"IF('Run Selections'!T27=\"Select Model\", \"\", 'Run Selections'!AB27)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T28=\"Select Model\", \"\", 'Run Selections'!F28)","v":""},{"$f":"IF('Run Selections'!T28=\"Select Model\", \"\", 'Run Selections'!L28)","v":""},{"$f":"IF('Run Selections'!T28=\"Select Model\", \"\", 'Run Selections'!T28)","v":""},{"$f":"IF('Run Selections'!T28=\"Select Model\", \"\", 'Run Selections'!U28)","v":""},{"$f":"IF('Run Selections'!T28=\"Select Model\", \"\", 'Run Selections'!V28)","v":""},{"$f":"IF('Run Selections'!T28=\"Select Model\", \"\", 'Run Selections'!W28)","v":""},{"$f":"IF('Run Selections'!T28=\"Select Model\", \"\", 'Run Selections'!AB28)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T29=\"Select Model\", \"\", 'Run Selections'!F29)","v":""},{"$f":"IF('Run Selections'!T29=\"Select Model\", \"\", 'Run Selections'!L29)","v":""},{"$f":"IF('Run Selections'!T29=\"Select Model\", \"\", 'Run Selections'!T29)","v":""},{"$f":"IF('Run Selections'!T29=\"Select Model\", \"\", 'Run Selections'!U29)","v":""},{"$f":"IF('Run Selections'!T29=\"Select Model\", \"\", 'Run Selections'!V29)","v":""},{"$f":"IF('Run Selections'!T29=\"Select Model\", \"\", 'Run Selections'!W29)","v":""},{"$f":"IF('Run Selections'!T29=\"Select Model\", \"\", 'Run Selections'!AB29)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T30=\"Select Model\", \"\", 'Run Selections'!F30)","v":""},{"$f":"IF('Run Selections'!T30=\"Select Model\", \"\", 'Run Selections'!L30)","v":""},{"$f":"IF('Run Selections'!T30=\"Select Model\", \"\", 'Run Selections'!T30)","v":""},{"$f":"IF('Run Selections'!T30=\"Select Model\", \"\", 'Run Selections'!U30)","v":""},{"$f":"IF('Run Selections'!T30=\"Select Model\", \"\", 'Run Selections'!V30)","v":""},{"$f":"IF('Run Selections'!T30=\"Select Model\", \"\", 'Run Selections'!W30)","v":""},{"$f":"IF('Run Selections'!T30=\"Select Model\", \"\", 'Run Selections'!AB30)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T31=\"Select Model\", \"\", 'Run Selections'!F31)","v":""},{"$f":"IF('Run Selections'!T31=\"Select Model\", \"\", 'Run Selections'!L31)","v":""},{"$f":"IF('Run Selections'!T31=\"Select Model\", \"\", 'Run Selections'!T31)","v":""},{"$f":"IF('Run Selections'!T31=\"Select Model\", \"\", 'Run Selections'!U31)","v":""},{"$f":"IF('Run Selections'!T31=\"Select Model\", \"\", 'Run Selections'!V31)","v":""},{"$f":"IF('Run Selections'!T31=\"Select Model\", \"\", 'Run Selections'!W31)","v":""},{"$f":"IF('Run Selections'!T31=\"Select Model\", \"\", 'Run Selections'!AB31)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T32=\"Select Model\", \"\", 'Run Selections'!F32)","v":""},{"$f":"IF('Run Selections'!T32=\"Select Model\", \"\", 'Run Selections'!L32)","v":""},{"$f":"IF('Run Selections'!T32=\"Select Model\", \"\", 'Run Selections'!T32)","v":""},{"$f":"IF('Run Selections'!T32=\"Select Model\", \"\", 'Run Selections'!U32)","v":""},{"$f":"IF('Run Selections'!T32=\"Select Model\", \"\", 'Run Selections'!V32)","v":""},{"$f":"IF('Run Selections'!T32=\"Select Model\", \"\", 'Run Selections'!W32)","v":""},{"$f":"IF('Run Selections'!T32=\"Select Model\", \"\", 'Run Selections'!AB32)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T33=\"Select Model\", \"\", 'Run Selections'!F33)","v":""},{"$f":"IF('Run Selections'!T33=\"Select Model\", \"\", 'Run Selections'!L33)","v":""},{"$f":"IF('Run Selections'!T33=\"Select Model\", \"\", 'Run Selections'!T33)","v":""},{"$f":"IF('Run Selections'!T33=\"Select Model\", \"\", 'Run Selections'!U33)","v":""},{"$f":"IF('Run Selections'!T33=\"Select Model\", \"\", 'Run Selections'!V33)","v":""},{"$f":"IF('Run Selections'!T33=\"Select Model\", \"\", 'Run Selections'!W33)","v":""},{"$f":"IF('Run Selections'!T33=\"Select Model\", \"\", 'Run Selections'!AB33)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T34=\"Select Model\", \"\", 'Run Selections'!F34)","v":""},{"$f":"IF('Run Selections'!T34=\"Select Model\", \"\", 'Run Selections'!#REF!)","v":""},{"$f":"IF('Run Selections'!T34=\"Select Model\", \"\", 'Run Selections'!T34)","v":""},{"$f":"IF('Run Selections'!T34=\"Select Model\", \"\", 'Run Selections'!U34)","v":""},{"$f":"IF('Run Selections'!T34=\"Select Model\", \"\", 'Run Selections'!V34)","v":""},{"$f":"IF('Run Selections'!T34=\"Select Model\", \"\", 'Run Selections'!W34)","v":""},{"$f":"IF('Run Selections'!T34=\"Select Model\", \"\", 'Run Selections'!AB34)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T35=\"Select Model\", \"\", 'Run Selections'!F35)","v":""},{"$f":"IF('Run Selections'!T35=\"Select Model\", \"\", 'Run Selections'!L34)","v":""},{"$f":"IF('Run Selections'!T35=\"Select Model\", \"\", 'Run Selections'!T35)","v":""},{"$f":"IF('Run Selections'!T35=\"Select Model\", \"\", 'Run Selections'!U35)","v":""},{"$f":"IF('Run Selections'!T35=\"Select Model\", \"\", 'Run Selections'!V35)","v":""},{"$f":"IF('Run Selections'!T35=\"Select Model\", \"\", 'Run Selections'!W35)","v":""},{"$f":"IF('Run Selections'!T35=\"Select Model\", \"\", 'Run Selections'!AB35)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T36=\"Select Model\", \"\", 'Run Selections'!F36)","v":""},{"$f":"IF('Run Selections'!T36=\"Select Model\", \"\", 'Run Selections'!L36)","v":""},{"$f":"IF('Run Selections'!T36=\"Select Model\", \"\", 'Run Selections'!T36)","v":""},{"$f":"IF('Run Selections'!T36=\"Select Model\", \"\", 'Run Selections'!U36)","v":""},{"$f":"IF('Run Selections'!T36=\"Select Model\", \"\", 'Run Selections'!V36)","v":""},{"$f":"IF('Run Selections'!T36=\"Select Model\", \"\", 'Run Selections'!W36)","v":""},{"$f":"IF('Run Selections'!T36=\"Select Model\", \"\", 'Run Selections'!AB36)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T37=\"Select Model\", \"\", 'Run Selections'!F37)","v":""},{"$f":"IF('Run Selections'!T37=\"Select Model\", \"\", 'Run Selections'!L37)","v":""},{"$f":"IF('Run Selections'!T37=\"Select Model\", \"\", 'Run Selections'!T37)","v":""},{"$f":"IF('Run Selections'!T37=\"Select Model\", \"\", 'Run Selections'!U37)","v":""},{"$f":"IF('Run Selections'!T37=\"Select Model\", \"\", 'Run Selections'!V37)","v":""},{"$f":"IF('Run Selections'!T37=\"Select Model\", \"\", 'Run Selections'!W37)","v":""},{"$f":"IF('Run Selections'!T37=\"Select Model\", \"\", 'Run Selections'!AB37)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T38=\"Select Model\", \"\", 'Run Selections'!F38)","v":""},{"$f":"IF('Run Selections'!T38=\"Select Model\", \"\", 'Run Selections'!L38)","v":""},{"$f":"IF('Run Selections'!T38=\"Select Model\", \"\", 'Run Selections'!T38)","v":""},{"$f":"IF('Run Selections'!T38=\"Select Model\", \"\", 'Run Selections'!U38)","v":""},{"$f":"IF('Run Selections'!T38=\"Select Model\", \"\", 'Run Selections'!V38)","v":""},{"$f":"IF('Run Selections'!T38=\"Select Model\", \"\", 'Run Selections'!W38)","v":""},{"$f":"IF('Run Selections'!T38=\"Select Model\", \"\", 'Run Selections'!AB38)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T39=\"Select Model\", \"\", 'Run Selections'!F39)","v":""},{"$f":"IF('Run Selections'!T39=\"Select Model\", \"\", 'Run Selections'!L39)","v":""},{"$f":"IF('Run Selections'!T39=\"Select Model\", \"\", 'Run Selections'!T39)","v":""},{"$f":"IF('Run Selections'!T39=\"Select Model\", \"\", 'Run Selections'!U39)","v":""},{"$f":"IF('Run Selections'!T39=\"Select Model\", \"\", 'Run Selections'!V39)","v":""},{"$f":"IF('Run Selections'!T39=\"Select Model\", \"\", 'Run Selections'!W39)","v":""},{"$f":"IF('Run Selections'!T39=\"Select Model\", \"\", 'Run Selections'!AB39)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T40=\"Select Model\", \"\", 'Run Selections'!F40)","v":""},{"$f":"IF('Run Selections'!T40=\"Select Model\", \"\", 'Run Selections'!L40)","v":""},{"$f":"IF('Run Selections'!T40=\"Select Model\", \"\", 'Run Selections'!T40)","v":""},{"$f":"IF('Run Selections'!T40=\"Select Model\", \"\", 'Run Selections'!U40)","v":""},{"$f":"IF('Run Selections'!T40=\"Select Model\", \"\", 'Run Selections'!V40)","v":""},{"$f":"IF('Run Selections'!T40=\"Select Model\", \"\", 'Run Selections'!W40)","v":""},{"$f":"IF('Run Selections'!T40=\"Select Model\", \"\", 'Run Selections'!AB40)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T41=\"Select Model\", \"\", 'Run Selections'!F41)","v":""},{"$f":"IF('Run Selections'!T41=\"Select Model\", \"\", 'Run Selections'!L41)","v":""},{"$f":"IF('Run Selections'!T41=\"Select Model\", \"\", 'Run Selections'!T41)","v":""},{"$f":"IF('Run Selections'!T41=\"Select Model\", \"\", 'Run Selections'!U41)","v":""},{"$f":"IF('Run Selections'!T41=\"Select Model\", \"\", 'Run Selections'!V41)","v":""},{"$f":"IF('Run Selections'!T41=\"Select Model\", \"\", 'Run Selections'!W41)","v":""},{"$f":"IF('Run Selections'!T41=\"Select Model\", \"\", 'Run Selections'!AB41)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T42=\"Select Model\", \"\", 'Run Selections'!F42)","v":""},{"$f":"IF('Run Selections'!T42=\"Select Model\", \"\", 'Run Selections'!L42)","v":""},{"$f":"IF('Run Selections'!T42=\"Select Model\", \"\", 'Run Selections'!T42)","v":""},{"$f":"IF('Run Selections'!T42=\"Select Model\", \"\", 'Run Selections'!U42)","v":""},{"$f":"IF('Run Selections'!T42=\"Select Model\", \"\", 'Run Selections'!V42)","v":""},{"$f":"IF('Run Selections'!T42=\"Select Model\", \"\", 'Run Selections'!W42)","v":""},{"$f":"IF('Run Selections'!T42=\"Select Model\", \"\", 'Run Selections'!AB42)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T43=\"Select Model\", \"\", 'Run Selections'!F43)","v":""},{"$f":"IF('Run Selections'!T43=\"Select Model\", \"\", 'Run Selections'!L43)","v":""},{"$f":"IF('Run Selections'!T43=\"Select Model\", \"\", 'Run Selections'!T43)","v":""},{"$f":"IF('Run Selections'!T43=\"Select Model\", \"\", 'Run Selections'!U43)","v":""},{"$f":"IF('Run Selections'!T43=\"Select Model\", \"\", 'Run Selections'!V43)","v":""},{"$f":"IF('Run Selections'!T43=\"Select Model\", \"\", 'Run Selections'!W43)","v":""},{"$f":"IF('Run Selections'!T43=\"Select Model\", \"\", 'Run Selections'!AB43)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T44=\"Select Model\", \"\", 'Run Selections'!F44)","v":""},{"$f":"IF('Run Selections'!T44=\"Select Model\", \"\", 'Run Selections'!L44)","v":""},{"$f":"IF('Run Selections'!T44=\"Select Model\", \"\", 'Run Selections'!T44)","v":""},{"$f":"IF('Run Selections'!T44=\"Select Model\", \"\", 'Run Selections'!U44)","v":""},{"$f":"IF('Run Selections'!T44=\"Select Model\", \"\", 'Run Selections'!V44)","v":""},{"$f":"IF('Run Selections'!T44=\"Select Model\", \"\", 'Run Selections'!W44)","v":""},{"$f":"IF('Run Selections'!T44=\"Select Model\", \"\", 'Run Selections'!AB44)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T45=\"Select Model\", \"\", 'Run Selections'!F45)","v":""},{"$f":"IF('Run Selections'!T45=\"Select Model\", \"\", 'Run Selections'!L45)","v":""},{"$f":"IF('Run Selections'!T45=\"Select Model\", \"\", 'Run Selections'!T45)","v":""},{"$f":"IF('Run Selections'!T45=\"Select Model\", \"\", 'Run Selections'!U45)","v":""},{"$f":"IF('Run Selections'!T45=\"Select Model\", \"\", 'Run Selections'!V45)","v":""},{"$f":"IF('Run Selections'!T45=\"Select Model\", \"\", 'Run Selections'!W45)","v":""},{"$f":"IF('Run Selections'!T45=\"Select Model\", \"\", 'Run Selections'!AB45)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T46=\"Select Model\", \"\", 'Run Selections'!F46)","v":""},{"$f":"IF('Run Selections'!T46=\"Select Model\", \"\", 'Run Selections'!L46)","v":""},{"$f":"IF('Run Selections'!T46=\"Select Model\", \"\", 'Run Selections'!T46)","v":""},{"$f":"IF('Run Selections'!T46=\"Select Model\", \"\", 'Run Selections'!U46)","v":""},{"$f":"IF('Run Selections'!T46=\"Select Model\", \"\", 'Run Selections'!V46)","v":""},{"$f":"IF('Run Selections'!T46=\"Select Model\", \"\", 'Run Selections'!W46)","v":""},{"$f":"IF('Run Selections'!T46=\"Select Model\", \"\", 'Run Selections'!AB46)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T47=\"Select Model\", \"\", 'Run Selections'!F47)","v":""},{"$f":"IF('Run Selections'!T47=\"Select Model\", \"\", 'Run Selections'!L47)","v":""},{"$f":"IF('Run Selections'!T47=\"Select Model\", \"\", 'Run Selections'!T47)","v":""},{"$f":"IF('Run Selections'!T47=\"Select Model\", \"\", 'Run Selections'!U47)","v":""},{"$f":"IF('Run Selections'!T47=\"Select Model\", \"\", 'Run Selections'!V47)","v":""},{"$f":"IF('Run Selections'!T47=\"Select Model\", \"\", 'Run Selections'!W47)","v":""},{"$f":"IF('Run Selections'!T47=\"Select Model\", \"\", 'Run Selections'!AB47)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T48=\"Select Model\", \"\", 'Run Selections'!F48)","v":""},{"$f":"IF('Run Selections'!T48=\"Select Model\", \"\", 'Run Selections'!L48)","v":""},{"$f":"IF('Run Selections'!T48=\"Select Model\", \"\", 'Run Selections'!T48)","v":""},{"$f":"IF('Run Selections'!T48=\"Select Model\", \"\", 'Run Selections'!U48)","v":""},{"$f":"IF('Run Selections'!T48=\"Select Model\", \"\", 'Run Selections'!V48)","v":""},{"$f":"IF('Run Selections'!T48=\"Select Model\", \"\", 'Run Selections'!W48)","v":""},{"$f":"IF('Run Selections'!T48=\"Select Model\", \"\", 'Run Selections'!AB48)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T49=\"Select Model\", \"\", 'Run Selections'!F49)","v":""},{"$f":"IF('Run Selections'!T49=\"Select Model\", \"\", 'Run Selections'!L49)","v":""},{"$f":"IF('Run Selections'!T49=\"Select Model\", \"\", 'Run Selections'!T49)","v":""},{"$f":"IF('Run Selections'!T49=\"Select Model\", \"\", 'Run Selections'!U49)","v":""},{"$f":"IF('Run Selections'!T49=\"Select Model\", \"\", 'Run Selections'!V49)","v":""},{"$f":"IF('Run Selections'!T49=\"Select Model\", \"\", 'Run Selections'!W49)","v":""},{"$f":"IF('Run Selections'!T49=\"Select Model\", \"\", 'Run Selections'!AB49)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T50=\"Select Model\", \"\", 'Run Selections'!F50)","v":""},{"$f":"IF('Run Selections'!T50=\"Select Model\", \"\", 'Run Selections'!L50)","v":""},{"$f":"IF('Run Selections'!T50=\"Select Model\", \"\", 'Run Selections'!T50)","v":""},{"$f":"IF('Run Selections'!T50=\"Select Model\", \"\", 'Run Selections'!U50)","v":""},{"$f":"IF('Run Selections'!T50=\"Select Model\", \"\", 'Run Selections'!V50)","v":""},{"$f":"IF('Run Selections'!T50=\"Select Model\", \"\", 'Run Selections'!W50)","v":""},{"$f":"IF('Run Selections'!T50=\"Select Model\", \"\", 'Run Selections'!AB50)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T51=\"Select Model\", \"\", 'Run Selections'!F51)","v":""},{"$f":"IF('Run Selections'!T51=\"Select Model\", \"\", 'Run Selections'!L51)","v":""},{"$f":"IF('Run Selections'!T51=\"Select Model\", \"\", 'Run Selections'!T51)","v":""},{"$f":"IF('Run Selections'!T51=\"Select Model\", \"\", 'Run Selections'!U51)","v":""},{"$f":"IF('Run Selections'!T51=\"Select Model\", \"\", 'Run Selections'!V51)","v":""},{"$f":"IF('Run Selections'!T51=\"Select Model\", \"\", 'Run Selections'!W51)","v":""},{"$f":"IF('Run Selections'!T51=\"Select Model\", \"\", 'Run Selections'!AB51)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T52=\"Select Model\", \"\", 'Run Selections'!F52)","v":""},{"$f":"IF('Run Selections'!T52=\"Select Model\", \"\", 'Run Selections'!L52)","v":""},{"$f":"IF('Run Selections'!T52=\"Select Model\", \"\", 'Run Selections'!T52)","v":""},{"$f":"IF('Run Selections'!T52=\"Select Model\", \"\", 'Run Selections'!U52)","v":""},{"$f":"IF('Run Selections'!T52=\"Select Model\", \"\", 'Run Selections'!V52)","v":""},{"$f":"IF('Run Selections'!T52=\"Select Model\", \"\", 'Run Selections'!W52)","v":""},{"$f":"IF('Run Selections'!T52=\"Select Model\", \"\", 'Run Selections'!AB52)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T53=\"Select Model\", \"\", 'Run Selections'!F53)","v":""},{"$f":"IF('Run Selections'!T53=\"Select Model\", \"\", 'Run Selections'!L53)","v":""},{"$f":"IF('Run Selections'!T53=\"Select Model\", \"\", 'Run Selections'!T53)","v":""},{"$f":"IF('Run Selections'!T53=\"Select Model\", \"\", 'Run Selections'!U53)","v":""},{"$f":"IF('Run Selections'!T53=\"Select Model\", \"\", 'Run Selections'!V53)","v":""},{"$f":"IF('Run Selections'!T53=\"Select Model\", \"\", 'Run Selections'!W53)","v":""},{"$f":"IF('Run Selections'!T53=\"Select Model\", \"\", 'Run Selections'!AB53)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T54=\"Select Model\", \"\", 'Run Selections'!F54)","v":""},{"$f":"IF('Run Selections'!T54=\"Select Model\", \"\", 'Run Selections'!L54)","v":""},{"$f":"IF('Run Selections'!T54=\"Select Model\", \"\", 'Run Selections'!T54)","v":""},{"$f":"IF('Run Selections'!T54=\"Select Model\", \"\", 'Run Selections'!U54)","v":""},{"$f":"IF('Run Selections'!T54=\"Select Model\", \"\", 'Run Selections'!V54)","v":""},{"$f":"IF('Run Selections'!T54=\"Select Model\", \"\", 'Run Selections'!W54)","v":""},{"$f":"IF('Run Selections'!T54=\"Select Model\", \"\", 'Run Selections'!AB54)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T55=\"Select Model\", \"\", 'Run Selections'!F55)","v":""},{"$f":"IF('Run Selections'!T55=\"Select Model\", \"\", 'Run Selections'!L55)","v":""},{"$f":"IF('Run Selections'!T55=\"Select Model\", \"\", 'Run Selections'!T55)","v":""},{"$f":"IF('Run Selections'!T55=\"Select Model\", \"\", 'Run Selections'!U55)","v":""},{"$f":"IF('Run Selections'!T55=\"Select Model\", \"\", 'Run Selections'!V55)","v":""},{"$f":"IF('Run Selections'!T55=\"Select Model\", \"\", 'Run Selections'!W55)","v":""},{"$f":"IF('Run Selections'!T55=\"Select Model\", \"\", 'Run Selections'!AB55)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T56=\"Select Model\", \"\", 'Run Selections'!F56)","v":""},{"$f":"IF('Run Selections'!T56=\"Select Model\", \"\", 'Run Selections'!L56)","v":""},{"$f":"IF('Run Selections'!T56=\"Select Model\", \"\", 'Run Selections'!T56)","v":""},{"$f":"IF('Run Selections'!T56=\"Select Model\", \"\", 'Run Selections'!U56)","v":""},{"$f":"IF('Run Selections'!T56=\"Select Model\", \"\", 'Run Selections'!V56)","v":""},{"$f":"IF('Run Selections'!T56=\"Select Model\", \"\", 'Run Selections'!W56)","v":""},{"$f":"IF('Run Selections'!T56=\"Select Model\", \"\", 'Run Selections'!AB56)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T57=\"Select Model\", \"\", 'Run Selections'!F57)","v":""},{"$f":"IF('Run Selections'!T57=\"Select Model\", \"\", 'Run Selections'!L57)","v":""},{"$f":"IF('Run Selections'!T57=\"Select Model\", \"\", 'Run Selections'!T57)","v":""},{"$f":"IF('Run Selections'!T57=\"Select Model\", \"\", 'Run Selections'!U57)","v":""},{"$f":"IF('Run Selections'!T57=\"Select Model\", \"\", 'Run Selections'!V57)","v":""},{"$f":"IF('Run Selections'!T57=\"Select Model\", \"\", 'Run Selections'!W57)","v":""},{"$f":"IF('Run Selections'!T57=\"Select Model\", \"\", 'Run Selections'!AB57)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T58=\"Select Model\", \"\", 'Run Selections'!F58)","v":""},{"$f":"IF('Run Selections'!T58=\"Select Model\", \"\", 'Run Selections'!L58)","v":""},{"$f":"IF('Run Selections'!T58=\"Select Model\", \"\", 'Run Selections'!T58)","v":""},{"$f":"IF('Run Selections'!T58=\"Select Model\", \"\", 'Run Selections'!U58)","v":""},{"$f":"IF('Run Selections'!T58=\"Select Model\", \"\", 'Run Selections'!V58)","v":""},{"$f":"IF('Run Selections'!T58=\"Select Model\", \"\", 'Run Selections'!W58)","v":""},{"$f":"IF('Run Selections'!T58=\"Select Model\", \"\", 'Run Selections'!AB58)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T59=\"Select Model\", \"\", 'Run Selections'!F59)","v":""},{"$f":"IF('Run Selections'!T59=\"Select Model\", \"\", 'Run Selections'!L59)","v":""},{"$f":"IF('Run Selections'!T59=\"Select Model\", \"\", 'Run Selections'!T59)","v":""},{"$f":"IF('Run Selections'!T59=\"Select Model\", \"\", 'Run Selections'!U59)","v":""},{"$f":"IF('Run Selections'!T59=\"Select Model\", \"\", 'Run Selections'!V59)","v":""},{"$f":"IF('Run Selections'!T59=\"Select Model\", \"\", 'Run Selections'!W59)","v":""},{"$f":"IF('Run Selections'!T59=\"Select Model\", \"\", 'Run Selections'!AB59)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T60=\"Select Model\", \"\", 'Run Selections'!F60)","v":""},{"$f":"IF('Run Selections'!T60=\"Select Model\", \"\", 'Run Selections'!L60)","v":""},{"$f":"IF('Run Selections'!T60=\"Select Model\", \"\", 'Run Selections'!T60)","v":""},{"$f":"IF('Run Selections'!T60=\"Select Model\", \"\", 'Run Selections'!U60)","v":""},{"$f":"IF('Run Selections'!T60=\"Select Model\", \"\", 'Run Selections'!V60)","v":""},{"$f":"IF('Run Selections'!T60=\"Select Model\", \"\", 'Run Selections'!W60)","v":""},{"$f":"IF('Run Selections'!T60=\"Select Model\", \"\", 'Run Selections'!AB60)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T61=\"Select Model\", \"\", 'Run Selections'!F61)","v":""},{"$f":"IF('Run Selections'!T61=\"Select Model\", \"\", 'Run Selections'!L61)","v":""},{"$f":"IF('Run Selections'!T61=\"Select Model\", \"\", 'Run Selections'!T61)","v":""},{"$f":"IF('Run Selections'!T61=\"Select Model\", \"\", 'Run Selections'!U61)","v":""},{"$f":"IF('Run Selections'!T61=\"Select Model\", \"\", 'Run Selections'!V61)","v":""},{"$f":"IF('Run Selections'!T61=\"Select Model\", \"\", 'Run Selections'!W61)","v":""},{"$f":"IF('Run Selections'!T61=\"Select Model\", \"\", 'Run Selections'!AB61)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T62=\"Select Model\", \"\", 'Run Selections'!F62)","v":""},{"$f":"IF('Run Selections'!T62=\"Select Model\", \"\", 'Run Selections'!L62)","v":""},{"$f":"IF('Run Selections'!T62=\"Select Model\", \"\", 'Run Selections'!T62)","v":""},{"$f":"IF('Run Selections'!T62=\"Select Model\", \"\", 'Run Selections'!U62)","v":""},{"$f":"IF('Run Selections'!T62=\"Select Model\", \"\", 'Run Selections'!V62)","v":""},{"$f":"IF('Run Selections'!T62=\"Select Model\", \"\", 'Run Selections'!W62)","v":""},{"$f":"IF('Run Selections'!T62=\"Select Model\", \"\", 'Run Selections'!AB62)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T63=\"Select Model\", \"\", 'Run Selections'!F63)","v":""},{"$f":"IF('Run Selections'!T63=\"Select Model\", \"\", 'Run Selections'!L63)","v":""},{"$f":"IF('Run Selections'!T63=\"Select Model\", \"\", 'Run Selections'!T63)","v":""},{"$f":"IF('Run Selections'!T63=\"Select Model\", \"\", 'Run Selections'!U63)","v":""},{"$f":"IF('Run Selections'!T63=\"Select Model\", \"\", 'Run Selections'!V63)","v":""},{"$f":"IF('Run Selections'!T63=\"Select Model\", \"\", 'Run Selections'!W63)","v":""},{"$f":"IF('Run Selections'!T63=\"Select Model\", \"\", 'Run Selections'!AB63)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T64=\"Select Model\", \"\", 'Run Selections'!F64)","v":""},{"$f":"IF('Run Selections'!T64=\"Select Model\", \"\", 'Run Selections'!L64)","v":""},{"$f":"IF('Run Selections'!T64=\"Select Model\", \"\", 'Run Selections'!T64)","v":""},{"$f":"IF('Run Selections'!T64=\"Select Model\", \"\", 'Run Selections'!U64)","v":""},{"$f":"IF('Run Selections'!T64=\"Select Model\", \"\", 'Run Selections'!V64)","v":""},{"$f":"IF('Run Selections'!T64=\"Select Model\", \"\", 'Run Selections'!W64)","v":""},{"$f":"IF('Run Selections'!T64=\"Select Model\", \"\", 'Run Selections'!AB64)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T65=\"Select Model\", \"\", 'Run Selections'!F65)","v":""},{"$f":"IF('Run Selections'!T65=\"Select Model\", \"\", 'Run Selections'!L65)","v":""},{"$f":"IF('Run Selections'!T65=\"Select Model\", \"\", 'Run Selections'!T65)","v":""},{"$f":"IF('Run Selections'!T65=\"Select Model\", \"\", 'Run Selections'!U65)","v":""},{"$f":"IF('Run Selections'!T65=\"Select Model\", \"\", 'Run Selections'!V65)","v":""},{"$f":"IF('Run Selections'!T65=\"Select Model\", \"\", 'Run Selections'!W65)","v":""},{"$f":"IF('Run Selections'!T65=\"Select Model\", \"\", 'Run Selections'!AB65)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T66=\"Select Model\", \"\", 'Run Selections'!F66)","v":""},{"$f":"IF('Run Selections'!T66=\"Select Model\", \"\", 'Run Selections'!L66)","v":""},{"$f":"IF('Run Selections'!T66=\"Select Model\", \"\", 'Run Selections'!T66)","v":""},{"$f":"IF('Run Selections'!T66=\"Select Model\", \"\", 'Run Selections'!U66)","v":""},{"$f":"IF('Run Selections'!T66=\"Select Model\", \"\", 'Run Selections'!V66)","v":""},{"$f":"IF('Run Selections'!T66=\"Select Model\", \"\", 'Run Selections'!W66)","v":""},{"$f":"IF('Run Selections'!T66=\"Select Model\", \"\", 'Run Selections'!AB66)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T67=\"Select Model\", \"\", 'Run Selections'!F67)","v":""},{"$f":"IF('Run Selections'!T67=\"Select Model\", \"\", 'Run Selections'!L67)","v":""},{"$f":"IF('Run Selections'!T67=\"Select Model\", \"\", 'Run Selections'!T67)","v":""},{"$f":"IF('Run Selections'!T67=\"Select Model\", \"\", 'Run Selections'!U67)","v":""},{"$f":"IF('Run Selections'!T67=\"Select Model\", \"\", 'Run Selections'!V67)","v":""},{"$f":"IF('Run Selections'!T67=\"Select Model\", \"\", 'Run Selections'!W67)","v":""},{"$f":"IF('Run Selections'!T67=\"Select Model\", \"\", 'Run Selections'!AB67)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T68=\"Select Model\", \"\", 'Run Selections'!F68)","v":""},{"$f":"IF('Run Selections'!T68=\"Select Model\", \"\", 'Run Selections'!L68)","v":""},{"$f":"IF('Run Selections'!T68=\"Select Model\", \"\", 'Run Selections'!T68)","v":""},{"$f":"IF('Run Selections'!T68=\"Select Model\", \"\", 'Run Selections'!U68)","v":""},{"$f":"IF('Run Selections'!T68=\"Select Model\", \"\", 'Run Selections'!V68)","v":""},{"$f":"IF('Run Selections'!T68=\"Select Model\", \"\", 'Run Selections'!W68)","v":""},{"$f":"IF('Run Selections'!T68=\"Select Model\", \"\", 'Run Selections'!AB68)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T69=\"Select Model\", \"\", 'Run Selections'!F69)","v":""},{"$f":"IF('Run Selections'!T69=\"Select Model\", \"\", 'Run Selections'!L69)","v":""},{"$f":"IF('Run Selections'!T69=\"Select Model\", \"\", 'Run Selections'!T69)","v":""},{"$f":"IF('Run Selections'!T69=\"Select Model\", \"\", 'Run Selections'!U69)","v":""},{"$f":"IF('Run Selections'!T69=\"Select Model\", \"\", 'Run Selections'!V69)","v":""},{"$f":"IF('Run Selections'!T69=\"Select Model\", \"\", 'Run Selections'!W69)","v":""},{"$f":"IF('Run Selections'!T69=\"Select Model\", \"\", 'Run Selections'!AB69)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T70=\"Select Model\", \"\", 'Run Selections'!F70)","v":""},{"$f":"IF('Run Selections'!T70=\"Select Model\", \"\", 'Run Selections'!L70)","v":""},{"$f":"IF('Run Selections'!T70=\"Select Model\", \"\", 'Run Selections'!T70)","v":""},{"$f":"IF('Run Selections'!T70=\"Select Model\", \"\", 'Run Selections'!U70)","v":""},{"$f":"IF('Run Selections'!T70=\"Select Model\", \"\", 'Run Selections'!V70)","v":""},{"$f":"IF('Run Selections'!T70=\"Select Model\", \"\", 'Run Selections'!W70)","v":""},{"$f":"IF('Run Selections'!T70=\"Select Model\", \"\", 'Run Selections'!AB70)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T71=\"Select Model\", \"\", 'Run Selections'!F71)","v":""},{"$f":"IF('Run Selections'!T71=\"Select Model\", \"\", 'Run Selections'!L71)","v":""},{"$f":"IF('Run Selections'!T71=\"Select Model\", \"\", 'Run Selections'!T71)","v":""},{"$f":"IF('Run Selections'!T71=\"Select Model\", \"\", 'Run Selections'!U71)","v":""},{"$f":"IF('Run Selections'!T71=\"Select Model\", \"\", 'Run Selections'!V71)","v":""},{"$f":"IF('Run Selections'!T71=\"Select Model\", \"\", 'Run Selections'!W71)","v":""},{"$f":"IF('Run Selections'!T71=\"Select Model\", \"\", 'Run Selections'!AB71)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T72=\"Select Model\", \"\", 'Run Selections'!F72)","v":""},{"$f":"IF('Run Selections'!T72=\"Select Model\", \"\", 'Run Selections'!L72)","v":""},{"$f":"IF('Run Selections'!T72=\"Select Model\", \"\", 'Run Selections'!T72)","v":""},{"$f":"IF('Run Selections'!T72=\"Select Model\", \"\", 'Run Selections'!U72)","v":""},{"$f":"IF('Run Selections'!T72=\"Select Model\", \"\", 'Run Selections'!V72)","v":""},{"$f":"IF('Run Selections'!T72=\"Select Model\", \"\", 'Run Selections'!W72)","v":""},{"$f":"IF('Run Selections'!T72=\"Select Model\", \"\", 'Run Selections'!AB72)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T73=\"Select Model\", \"\", 'Run Selections'!F73)","v":""},{"$f":"IF('Run Selections'!T73=\"Select Model\", \"\", 'Run Selections'!L73)","v":""},{"$f":"IF('Run Selections'!T73=\"Select Model\", \"\", 'Run Selections'!T73)","v":""},{"$f":"IF('Run Selections'!T73=\"Select Model\", \"\", 'Run Selections'!U73)","v":""},{"$f":"IF('Run Selections'!T73=\"Select Model\", \"\", 'Run Selections'!V73)","v":""},{"$f":"IF('Run Selections'!T73=\"Select Model\", \"\", 'Run Selections'!W73)","v":""},{"$f":"IF('Run Selections'!T73=\"Select Model\", \"\", 'Run Selections'!AB73)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T74=\"Select Model\", \"\", 'Run Selections'!F74)","v":""},{"$f":"IF('Run Selections'!T74=\"Select Model\", \"\", 'Run Selections'!L74)","v":""},{"$f":"IF('Run Selections'!T74=\"Select Model\", \"\", 'Run Selections'!T74)","v":""},{"$f":"IF('Run Selections'!T74=\"Select Model\", \"\", 'Run Selections'!U74)","v":""},{"$f":"IF('Run Selections'!T74=\"Select Model\", \"\", 'Run Selections'!V74)","v":""},{"$f":"IF('Run Selections'!T74=\"Select Model\", \"\", 'Run Selections'!W74)","v":""},{"$f":"IF('Run Selections'!T74=\"Select Model\", \"\", 'Run Selections'!AB74)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T75=\"Select Model\", \"\", 'Run Selections'!F75)","v":""},{"$f":"IF('Run Selections'!T75=\"Select Model\", \"\", 'Run Selections'!L75)","v":""},{"$f":"IF('Run Selections'!T75=\"Select Model\", \"\", 'Run Selections'!T75)","v":""},{"$f":"IF('Run Selections'!T75=\"Select Model\", \"\", 'Run Selections'!U75)","v":""},{"$f":"IF('Run Selections'!T75=\"Select Model\", \"\", 'Run Selections'!V75)","v":""},{"$f":"IF('Run Selections'!T75=\"Select Model\", \"\", 'Run Selections'!W75)","v":""},{"$f":"IF('Run Selections'!T75=\"Select Model\", \"\", 'Run Selections'!AB75)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T76=\"Select Model\", \"\", 'Run Selections'!F76)","v":""},{"$f":"IF('Run Selections'!T76=\"Select Model\", \"\", 'Run Selections'!L76)","v":""},{"$f":"IF('Run Selections'!T76=\"Select Model\", \"\", 'Run Selections'!T76)","v":""},{"$f":"IF('Run Selections'!T76=\"Select Model\", \"\", 'Run Selections'!U76)","v":""},{"$f":"IF('Run Selections'!T76=\"Select Model\", \"\", 'Run Selections'!V76)","v":""},{"$f":"IF('Run Selections'!T76=\"Select Model\", \"\", 'Run Selections'!W76)","v":""},{"$f":"IF('Run Selections'!T76=\"Select Model\", \"\", 'Run Selections'!AB76)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T77=\"Select Model\", \"\", 'Run Selections'!F77)","v":""},{"$f":"IF('Run Selections'!T77=\"Select Model\", \"\", 'Run Selections'!L77)","v":""},{"$f":"IF('Run Selections'!T77=\"Select Model\", \"\", 'Run Selections'!T77)","v":""},{"$f":"IF('Run Selections'!T77=\"Select Model\", \"\", 'Run Selections'!U77)","v":""},{"$f":"IF('Run Selections'!T77=\"Select Model\", \"\", 'Run Selections'!V77)","v":""},{"$f":"IF('Run Selections'!T77=\"Select Model\", \"\", 'Run Selections'!W77)","v":""},{"$f":"IF('Run Selections'!T77=\"Select Model\", \"\", 'Run Selections'!AB77)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T78=\"Select Model\", \"\", 'Run Selections'!F78)","v":""},{"$f":"IF('Run Selections'!T78=\"Select Model\", \"\", 'Run Selections'!L78)","v":""},{"$f":"IF('Run Selections'!T78=\"Select Model\", \"\", 'Run Selections'!T78)","v":""},{"$f":"IF('Run Selections'!T78=\"Select Model\", \"\", 'Run Selections'!U78)","v":""},{"$f":"IF('Run Selections'!T78=\"Select Model\", \"\", 'Run Selections'!V78)","v":""},{"$f":"IF('Run Selections'!T78=\"Select Model\", \"\", 'Run Selections'!W78)","v":""},{"$f":"IF('Run Selections'!T78=\"Select Model\", \"\", 'Run Selections'!AB78)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T79=\"Select Model\", \"\", 'Run Selections'!F79)","v":""},{"$f":"IF('Run Selections'!T79=\"Select Model\", \"\", 'Run Selections'!L79)","v":""},{"$f":"IF('Run Selections'!T79=\"Select Model\", \"\", 'Run Selections'!T79)","v":""},{"$f":"IF('Run Selections'!T79=\"Select Model\", \"\", 'Run Selections'!U79)","v":""},{"$f":"IF('Run Selections'!T79=\"Select Model\", \"\", 'Run Selections'!V79)","v":""},{"$f":"IF('Run Selections'!T79=\"Select Model\", \"\", 'Run Selections'!W79)","v":""},{"$f":"IF('Run Selections'!T79=\"Select Model\", \"\", 'Run Selections'!AB79)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T80=\"Select Model\", \"\", 'Run Selections'!F80)","v":""},{"$f":"IF('Run Selections'!T80=\"Select Model\", \"\", 'Run Selections'!L80)","v":""},{"$f":"IF('Run Selections'!T80=\"Select Model\", \"\", 'Run Selections'!T80)","v":""},{"$f":"IF('Run Selections'!T80=\"Select Model\", \"\", 'Run Selections'!U80)","v":""},{"$f":"IF('Run Selections'!T80=\"Select Model\", \"\", 'Run Selections'!V80)","v":""},{"$f":"IF('Run Selections'!T80=\"Select Model\", \"\", 'Run Selections'!W80)","v":""},{"$f":"IF('Run Selections'!T80=\"Select Model\", \"\", 'Run Selections'!AB80)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T81=\"Select Model\", \"\", 'Run Selections'!F81)","v":""},{"$f":"IF('Run Selections'!T81=\"Select Model\", \"\", 'Run Selections'!L81)","v":""},{"$f":"IF('Run Selections'!T81=\"Select Model\", \"\", 'Run Selections'!T81)","v":""},{"$f":"IF('Run Selections'!T81=\"Select Model\", \"\", 'Run Selections'!U81)","v":""},{"$f":"IF('Run Selections'!T81=\"Select Model\", \"\", 'Run Selections'!V81)","v":""},{"$f":"IF('Run Selections'!T81=\"Select Model\", \"\", 'Run Selections'!W81)","v":""},{"$f":"IF('Run Selections'!T81=\"Select Model\", \"\", 'Run Selections'!AB81)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T82=\"Select Model\", \"\", 'Run Selections'!F82)","v":""},{"$f":"IF('Run Selections'!T82=\"Select Model\", \"\", 'Run Selections'!L82)","v":""},{"$f":"IF('Run Selections'!T82=\"Select Model\", \"\", 'Run Selections'!T82)","v":""},{"$f":"IF('Run Selections'!T82=\"Select Model\", \"\", 'Run Selections'!U82)","v":""},{"$f":"IF('Run Selections'!T82=\"Select Model\", \"\", 'Run Selections'!V82)","v":""},{"$f":"IF('Run Selections'!T82=\"Select Model\", \"\", 'Run Selections'!W82)","v":""},{"$f":"IF('Run Selections'!T82=\"Select Model\", \"\", 'Run Selections'!AB82)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T83=\"Select Model\", \"\", 'Run Selections'!F83)","v":""},{"$f":"IF('Run Selections'!T83=\"Select Model\", \"\", 'Run Selections'!L83)","v":""},{"$f":"IF('Run Selections'!T83=\"Select Model\", \"\", 'Run Selections'!T83)","v":""},{"$f":"IF('Run Selections'!T83=\"Select Model\", \"\", 'Run Selections'!U83)","v":""},{"$f":"IF('Run Selections'!T83=\"Select Model\", \"\", 'Run Selections'!V83)","v":""},{"$f":"IF('Run Selections'!T83=\"Select Model\", \"\", 'Run Selections'!W83)","v":""},{"$f":"IF('Run Selections'!T83=\"Select Model\", \"\", 'Run Selections'!AB83)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T84=\"Select Model\", \"\", 'Run Selections'!F84)","v":""},{"$f":"IF('Run Selections'!T84=\"Select Model\", \"\", 'Run Selections'!L84)","v":""},{"$f":"IF('Run Selections'!T84=\"Select Model\", \"\", 'Run Selections'!T84)","v":""},{"$f":"IF('Run Selections'!T84=\"Select Model\", \"\", 'Run Selections'!U84)","v":""},{"$f":"IF('Run Selections'!T84=\"Select Model\", \"\", 'Run Selections'!V84)","v":""},{"$f":"IF('Run Selections'!T84=\"Select Model\", \"\", 'Run Selections'!W84)","v":""},{"$f":"IF('Run Selections'!T84=\"Select Model\", \"\", 'Run Selections'!AB84)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T85=\"Select Model\", \"\", 'Run Selections'!F85)","v":""},{"$f":"IF('Run Selections'!T85=\"Select Model\", \"\", 'Run Selections'!L85)","v":""},{"$f":"IF('Run Selections'!T85=\"Select Model\", \"\", 'Run Selections'!T85)","v":""},{"$f":"IF('Run Selections'!T85=\"Select Model\", \"\", 'Run Selections'!U85)","v":""},{"$f":"IF('Run Selections'!T85=\"Select Model\", \"\", 'Run Selections'!V85)","v":""},{"$f":"IF('Run Selections'!T85=\"Select Model\", \"\", 'Run Selections'!W85)","v":""},{"$f":"IF('Run Selections'!T85=\"Select Model\", \"\", 'Run Selections'!AB85)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T86=\"Select Model\", \"\", 'Run Selections'!F86)","v":""},{"$f":"IF('Run Selections'!T86=\"Select Model\", \"\", 'Run Selections'!L86)","v":""},{"$f":"IF('Run Selections'!T86=\"Select Model\", \"\", 'Run Selections'!T86)","v":""},{"$f":"IF('Run Selections'!T86=\"Select Model\", \"\", 'Run Selections'!U86)","v":""},{"$f":"IF('Run Selections'!T86=\"Select Model\", \"\", 'Run Selections'!V86)","v":""},{"$f":"IF('Run Selections'!T86=\"Select Model\", \"\", 'Run Selections'!W86)","v":""},{"$f":"IF('Run Selections'!T86=\"Select Model\", \"\", 'Run Selections'!AB86)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T87=\"Select Model\", \"\", 'Run Selections'!F87)","v":""},{"$f":"IF('Run Selections'!T87=\"Select Model\", \"\", 'Run Selections'!L87)","v":""},{"$f":"IF('Run Selections'!T87=\"Select Model\", \"\", 'Run Selections'!T87)","v":""},{"$f":"IF('Run Selections'!T87=\"Select Model\", \"\", 'Run Selections'!U87)","v":""},{"$f":"IF('Run Selections'!T87=\"Select Model\", \"\", 'Run Selections'!V87)","v":""},{"$f":"IF('Run Selections'!T87=\"Select Model\", \"\", 'Run Selections'!W87)","v":""},{"$f":"IF('Run Selections'!T87=\"Select Model\", \"\", 'Run Selections'!AB87)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T88=\"Select Model\", \"\", 'Run Selections'!F88)","v":""},{"$f":"IF('Run Selections'!T88=\"Select Model\", \"\", 'Run Selections'!L88)","v":""},{"$f":"IF('Run Selections'!T88=\"Select Model\", \"\", 'Run Selections'!T88)","v":""},{"$f":"IF('Run Selections'!T88=\"Select Model\", \"\", 'Run Selections'!U88)","v":""},{"$f":"IF('Run Selections'!T88=\"Select Model\", \"\", 'Run Selections'!V88)","v":""},{"$f":"IF('Run Selections'!T88=\"Select Model\", \"\", 'Run Selections'!W88)","v":""},{"$f":"IF('Run Selections'!T88=\"Select Model\", \"\", 'Run Selections'!AB88)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T89=\"Select Model\", \"\", 'Run Selections'!F89)","v":""},{"$f":"IF('Run Selections'!T89=\"Select Model\", \"\", 'Run Selections'!L89)","v":""},{"$f":"IF('Run Selections'!T89=\"Select Model\", \"\", 'Run Selections'!T89)","v":""},{"$f":"IF('Run Selections'!T89=\"Select Model\", \"\", 'Run Selections'!U89)","v":""},{"$f":"IF('Run Selections'!T89=\"Select Model\", \"\", 'Run Selections'!V89)","v":""},{"$f":"IF('Run Selections'!T89=\"Select Model\", \"\", 'Run Selections'!W89)","v":""},{"$f":"IF('Run Selections'!T89=\"Select Model\", \"\", 'Run Selections'!AB89)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T90=\"Select Model\", \"\", 'Run Selections'!F90)","v":""},{"$f":"IF('Run Selections'!T90=\"Select Model\", \"\", 'Run Selections'!L90)","v":""},{"$f":"IF('Run Selections'!T90=\"Select Model\", \"\", 'Run Selections'!T90)","v":""},{"$f":"IF('Run Selections'!T90=\"Select Model\", \"\", 'Run Selections'!U90)","v":""},{"$f":"IF('Run Selections'!T90=\"Select Model\", \"\", 'Run Selections'!V90)","v":""},{"$f":"IF('Run Selections'!T90=\"Select Model\", \"\", 'Run Selections'!W90)","v":""},{"$f":"IF('Run Selections'!T90=\"Select Model\", \"\", 'Run Selections'!AB90)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T91=\"Select Model\", \"\", 'Run Selections'!F91)","v":""},{"$f":"IF('Run Selections'!T91=\"Select Model\", \"\", 'Run Selections'!L91)","v":""},{"$f":"IF('Run Selections'!T91=\"Select Model\", \"\", 'Run Selections'!T91)","v":""},{"$f":"IF('Run Selections'!T91=\"Select Model\", \"\", 'Run Selections'!U91)","v":""},{"$f":"IF('Run Selections'!T91=\"Select Model\", \"\", 'Run Selections'!V91)","v":""},{"$f":"IF('Run Selections'!T91=\"Select Model\", \"\", 'Run Selections'!W91)","v":""},{"$f":"IF('Run Selections'!T91=\"Select Model\", \"\", 'Run Selections'!AB91)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T92=\"Select Model\", \"\", 'Run Selections'!F92)","v":""},{"$f":"IF('Run Selections'!T92=\"Select Model\", \"\", 'Run Selections'!L92)","v":""},{"$f":"IF('Run Selections'!T92=\"Select Model\", \"\", 'Run Selections'!T92)","v":""},{"$f":"IF('Run Selections'!T92=\"Select Model\", \"\", 'Run Selections'!U92)","v":""},{"$f":"IF('Run Selections'!T92=\"Select Model\", \"\", 'Run Selections'!V92)","v":""},{"$f":"IF('Run Selections'!T92=\"Select Model\", \"\", 'Run Selections'!W92)","v":""},{"$f":"IF('Run Selections'!T92=\"Select Model\", \"\", 'Run Selections'!AB92)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T93=\"Select Model\", \"\", 'Run Selections'!F93)","v":""},{"$f":"IF('Run Selections'!T93=\"Select Model\", \"\", 'Run Selections'!L93)","v":""},{"$f":"IF('Run Selections'!T93=\"Select Model\", \"\", 'Run Selections'!T93)","v":""},{"$f":"IF('Run Selections'!T93=\"Select Model\", \"\", 'Run Selections'!U93)","v":""},{"$f":"IF('Run Selections'!T93=\"Select Model\", \"\", 'Run Selections'!V93)","v":""},{"$f":"IF('Run Selections'!T93=\"Select Model\", \"\", 'Run Selections'!W93)","v":""},{"$f":"IF('Run Selections'!T93=\"Select Model\", \"\", 'Run Selections'!AB93)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T94=\"Select Model\", \"\", 'Run Selections'!F94)","v":""},{"$f":"IF('Run Selections'!T94=\"Select Model\", \"\", 'Run Selections'!L94)","v":""},{"$f":"IF('Run Selections'!T94=\"Select Model\", \"\", 'Run Selections'!T94)","v":""},{"$f":"IF('Run Selections'!T94=\"Select Model\", \"\", 'Run Selections'!U94)","v":""},{"$f":"IF('Run Selections'!T94=\"Select Model\", \"\", 'Run Selections'!V94)","v":""},{"$f":"IF('Run Selections'!T94=\"Select Model\", \"\", 'Run Selections'!W94)","v":""},{"$f":"IF('Run Selections'!T94=\"Select Model\", \"\", 'Run Selections'!AB94)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T95=\"Select Model\", \"\", 'Run Selections'!F95)","v":""},{"$f":"IF('Run Selections'!T95=\"Select Model\", \"\", 'Run Selections'!L95)","v":""},{"$f":"IF('Run Selections'!T95=\"Select Model\", \"\", 'Run Selections'!T95)","v":""},{"$f":"IF('Run Selections'!T95=\"Select Model\", \"\", 'Run Selections'!U95)","v":""},{"$f":"IF('Run Selections'!T95=\"Select Model\", \"\", 'Run Selections'!V95)","v":""},{"$f":"IF('Run Selections'!T95=\"Select Model\", \"\", 'Run Selections'!W95)","v":""},{"$f":"IF('Run Selections'!T95=\"Select Model\", \"\", 'Run Selections'!AB95)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T96=\"Select Model\", \"\", 'Run Selections'!F96)","v":""},{"$f":"IF('Run Selections'!T96=\"Select Model\", \"\", 'Run Selections'!L96)","v":""},{"$f":"IF('Run Selections'!T96=\"Select Model\", \"\", 'Run Selections'!T96)","v":""},{"$f":"IF('Run Selections'!T96=\"Select Model\", \"\", 'Run Selections'!U96)","v":""},{"$f":"IF('Run Selections'!T96=\"Select Model\", \"\", 'Run Selections'!V96)","v":""},{"$f":"IF('Run Selections'!T96=\"Select Model\", \"\", 'Run Selections'!W96)","v":""},{"$f":"IF('Run Selections'!T96=\"Select Model\", \"\", 'Run Selections'!AB96)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T97=\"Select Model\", \"\", 'Run Selections'!F97)","v":""},{"$f":"IF('Run Selections'!T97=\"Select Model\", \"\", 'Run Selections'!L97)","v":""},{"$f":"IF('Run Selections'!T97=\"Select Model\", \"\", 'Run Selections'!T97)","v":""},{"$f":"IF('Run Selections'!T97=\"Select Model\", \"\", 'Run Selections'!U97)","v":""},{"$f":"IF('Run Selections'!T97=\"Select Model\", \"\", 'Run Selections'!V97)","v":""},{"$f":"IF('Run Selections'!T97=\"Select Model\", \"\", 'Run Selections'!W97)","v":""},{"$f":"IF('Run Selections'!T97=\"Select Model\", \"\", 'Run Selections'!AB97)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T98=\"Select Model\", \"\", 'Run Selections'!F98)","v":""},{"$f":"IF('Run Selections'!T98=\"Select Model\", \"\", 'Run Selections'!L98)","v":""},{"$f":"IF('Run Selections'!T98=\"Select Model\", \"\", 'Run Selections'!T98)","v":""},{"$f":"IF('Run Selections'!T98=\"Select Model\", \"\", 'Run Selections'!U98)","v":""},{"$f":"IF('Run Selections'!T98=\"Select Model\", \"\", 'Run Selections'!V98)","v":""},{"$f":"IF('Run Selections'!T98=\"Select Model\", \"\", 'Run Selections'!W98)","v":""},{"$f":"IF('Run Selections'!T98=\"Select Model\", \"\", 'Run Selections'!AB98)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T99=\"Select Model\", \"\", 'Run Selections'!F99)","v":""},{"$f":"IF('Run Selections'!T99=\"Select Model\", \"\", 'Run Selections'!L99)","v":""},{"$f":"IF('Run Selections'!T99=\"Select Model\", \"\", 'Run Selections'!T99)","v":""},{"$f":"IF('Run Selections'!T99=\"Select Model\", \"\", 'Run Selections'!U99)","v":""},{"$f":"IF('Run Selections'!T99=\"Select Model\", \"\", 'Run Selections'!V99)","v":""},{"$f":"IF('Run Selections'!T99=\"Select Model\", \"\", 'Run Selections'!W99)","v":""},{"$f":"IF('Run Selections'!T99=\"Select Model\", \"\", 'Run Selections'!AB99)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T100=\"Select Model\", \"\", 'Run Selections'!F100)","v":""},{"$f":"IF('Run Selections'!T100=\"Select Model\", \"\", 'Run Selections'!L100)","v":""},{"$f":"IF('Run Selections'!T100=\"Select Model\", \"\", 'Run Selections'!T100)","v":""},{"$f":"IF('Run Selections'!T100=\"Select Model\", \"\", 'Run Selections'!U100)","v":""},{"$f":"IF('Run Selections'!T100=\"Select Model\", \"\", 'Run Selections'!V100)","v":""},{"$f":"IF('Run Selections'!T100=\"Select Model\", \"\", 'Run Selections'!W100)","v":""},{"$f":"IF('Run Selections'!T100=\"Select Model\", \"\", 'Run Selections'!AB100)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T101=\"Select Model\", \"\", 'Run Selections'!F101)","v":""},{"$f":"IF('Run Selections'!T101=\"Select Model\", \"\", 'Run Selections'!L101)","v":""},{"$f":"IF('Run Selections'!T101=\"Select Model\", \"\", 'Run Selections'!T101)","v":""},{"$f":"IF('Run Selections'!T101=\"Select Model\", \"\", 'Run Selections'!U101)","v":""},{"$f":"IF('Run Selections'!T101=\"Select Model\", \"\", 'Run Selections'!V101)","v":""},{"$f":"IF('Run Selections'!T101=\"Select Model\", \"\", 'Run Selections'!W101)","v":""},{"$f":"IF('Run Selections'!T101=\"Select Model\", \"\", 'Run Selections'!AB101)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T102=\"Select Model\", \"\", 'Run Selections'!F102)","v":""},{"$f":"IF('Run Selections'!T102=\"Select Model\", \"\", 'Run Selections'!L102)","v":""},{"$f":"IF('Run Selections'!T102=\"Select Model\", \"\", 'Run Selections'!T102)","v":""},{"$f":"IF('Run Selections'!T102=\"Select Model\", \"\", 'Run Selections'!U102)","v":""},{"$f":"IF('Run Selections'!T102=\"Select Model\", \"\", 'Run Selections'!V102)","v":""},{"$f":"IF('Run Selections'!T102=\"Select Model\", \"\", 'Run Selections'!W102)","v":""},{"$f":"IF('Run Selections'!T102=\"Select Model\", \"\", 'Run Selections'!AB102)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T103=\"Select Model\", \"\", 'Run Selections'!F103)","v":""},{"$f":"IF('Run Selections'!T103=\"Select Model\", \"\", 'Run Selections'!L103)","v":""},{"$f":"IF('Run Selections'!T103=\"Select Model\", \"\", 'Run Selections'!T103)","v":""},{"$f":"IF('Run Selections'!T103=\"Select Model\", \"\", 'Run Selections'!U103)","v":""},{"$f":"IF('Run Selections'!T103=\"Select Model\", \"\", 'Run Selections'!V103)","v":""},{"$f":"IF('Run Selections'!T103=\"Select Model\", \"\", 'Run Selections'!W103)","v":""},{"$f":"IF('Run Selections'!T103=\"Select Model\", \"\", 'Run Selections'!AB103)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T104=\"Select Model\", \"\", 'Run Selections'!F104)","v":""},{"$f":"IF('Run Selections'!T104=\"Select Model\", \"\", 'Run Selections'!L104)","v":""},{"$f":"IF('Run Selections'!T104=\"Select Model\", \"\", 'Run Selections'!T104)","v":""},{"$f":"IF('Run Selections'!T104=\"Select Model\", \"\", 'Run Selections'!U104)","v":""},{"$f":"IF('Run Selections'!T104=\"Select Model\", \"\", 'Run Selections'!V104)","v":""},{"$f":"IF('Run Selections'!T104=\"Select Model\", \"\", 'Run Selections'!W104)","v":""},{"$f":"IF('Run Selections'!T104=\"Select Model\", \"\", 'Run Selections'!AB104)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T105=\"Select Model\", \"\", 'Run Selections'!F105)","v":""},{"$f":"IF('Run Selections'!T105=\"Select Model\", \"\", 'Run Selections'!L105)","v":""},{"$f":"IF('Run Selections'!T105=\"Select Model\", \"\", 'Run Selections'!T105)","v":""},{"$f":"IF('Run Selections'!T105=\"Select Model\", \"\", 'Run Selections'!U105)","v":""},{"$f":"IF('Run Selections'!T105=\"Select Model\", \"\", 'Run Selections'!V105)","v":""},{"$f":"IF('Run Selections'!T105=\"Select Model\", \"\", 'Run Selections'!W105)","v":""},{"$f":"IF('Run Selections'!T105=\"Select Model\", \"\", 'Run Selections'!AB105)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T106=\"Select Model\", \"\", 'Run Selections'!F106)","v":""},{"$f":"IF('Run Selections'!T106=\"Select Model\", \"\", 'Run Selections'!L106)","v":""},{"$f":"IF('Run Selections'!T106=\"Select Model\", \"\", 'Run Selections'!T106)","v":""},{"$f":"IF('Run Selections'!T106=\"Select Model\", \"\", 'Run Selections'!U106)","v":""},{"$f":"IF('Run Selections'!T106=\"Select Model\", \"\", 'Run Selections'!V106)","v":""},{"$f":"IF('Run Selections'!T106=\"Select Model\", \"\", 'Run Selections'!W106)","v":""},{"$f":"IF('Run Selections'!T106=\"Select Model\", \"\", 'Run Selections'!AB106)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T107=\"Select Model\", \"\", 'Run Selections'!F107)","v":""},{"$f":"IF('Run Selections'!T107=\"Select Model\", \"\", 'Run Selections'!L107)","v":""},{"$f":"IF('Run Selections'!T107=\"Select Model\", \"\", 'Run Selections'!T107)","v":""},{"$f":"IF('Run Selections'!T107=\"Select Model\", \"\", 'Run Selections'!U107)","v":""},{"$f":"IF('Run Selections'!T107=\"Select Model\", \"\", 'Run Selections'!V107)","v":""},{"$f":"IF('Run Selections'!T107=\"Select Model\", \"\", 'Run Selections'!W107)","v":""},{"$f":"IF('Run Selections'!T107=\"Select Model\", \"\", 'Run Selections'!AB107)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T108=\"Select Model\", \"\", 'Run Selections'!F108)","v":""},{"$f":"IF('Run Selections'!T108=\"Select Model\", \"\", 'Run Selections'!L108)","v":""},{"$f":"IF('Run Selections'!T108=\"Select Model\", \"\", 'Run Selections'!T108)","v":""},{"$f":"IF('Run Selections'!T108=\"Select Model\", \"\", 'Run Selections'!U108)","v":""},{"$f":"IF('Run Selections'!T108=\"Select Model\", \"\", 'Run Selections'!V108)","v":""},{"$f":"IF('Run Selections'!T108=\"Select Model\", \"\", 'Run Selections'!W108)","v":""},{"$f":"IF('Run Selections'!T108=\"Select Model\", \"\", 'Run Selections'!AB108)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T109=\"Select Model\", \"\", 'Run Selections'!F109)","v":""},{"$f":"IF('Run Selections'!T109=\"Select Model\", \"\", 'Run Selections'!L109)","v":""},{"$f":"IF('Run Selections'!T109=\"Select Model\", \"\", 'Run Selections'!T109)","v":""},{"$f":"IF('Run Selections'!T109=\"Select Model\", \"\", 'Run Selections'!U109)","v":""},{"$f":"IF('Run Selections'!T109=\"Select Model\", \"\", 'Run Selections'!V109)","v":""},{"$f":"IF('Run Selections'!T109=\"Select Model\", \"\", 'Run Selections'!W109)","v":""},{"$f":"IF('Run Selections'!T109=\"Select Model\", \"\", 'Run Selections'!AB109)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T110=\"Select Model\", \"\", 'Run Selections'!F110)","v":""},{"$f":"IF('Run Selections'!T110=\"Select Model\", \"\", 'Run Selections'!L110)","v":""},{"$f":"IF('Run Selections'!T110=\"Select Model\", \"\", 'Run Selections'!T110)","v":""},{"$f":"IF('Run Selections'!T110=\"Select Model\", \"\", 'Run Selections'!U110)","v":""},{"$f":"IF('Run Selections'!T110=\"Select Model\", \"\", 'Run Selections'!V110)","v":""},{"$f":"IF('Run Selections'!T110=\"Select Model\", \"\", 'Run Selections'!W110)","v":""},{"$f":"IF('Run Selections'!T110=\"Select Model\", \"\", 'Run Selections'!AB110)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T111=\"Select Model\", \"\", 'Run Selections'!F111)","v":""},{"$f":"IF('Run Selections'!T111=\"Select Model\", \"\", 'Run Selections'!L111)","v":""},{"$f":"IF('Run Selections'!T111=\"Select Model\", \"\", 'Run Selections'!T111)","v":""},{"$f":"IF('Run Selections'!T111=\"Select Model\", \"\", 'Run Selections'!U111)","v":""},{"$f":"IF('Run Selections'!T111=\"Select Model\", \"\", 'Run Selections'!V111)","v":""},{"$f":"IF('Run Selections'!T111=\"Select Model\", \"\", 'Run Selections'!W111)","v":""},{"$f":"IF('Run Selections'!T111=\"Select Model\", \"\", 'Run Selections'!AB111)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T112=\"Select Model\", \"\", 'Run Selections'!F112)","v":""},{"$f":"IF('Run Selections'!T112=\"Select Model\", \"\", 'Run Selections'!L112)","v":""},{"$f":"IF('Run Selections'!T112=\"Select Model\", \"\", 'Run Selections'!T112)","v":""},{"$f":"IF('Run Selections'!T112=\"Select Model\", \"\", 'Run Selections'!U112)","v":""},{"$f":"IF('Run Selections'!T112=\"Select Model\", \"\", 'Run Selections'!V112)","v":""},{"$f":"IF('Run Selections'!T112=\"Select Model\", \"\", 'Run Selections'!W112)","v":""},{"$f":"IF('Run Selections'!T112=\"Select Model\", \"\", 'Run Selections'!AB112)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T113=\"Select Model\", \"\", 'Run Selections'!F113)","v":""},{"$f":"IF('Run Selections'!T113=\"Select Model\", \"\", 'Run Selections'!L113)","v":""},{"$f":"IF('Run Selections'!T113=\"Select Model\", \"\", 'Run Selections'!T113)","v":""},{"$f":"IF('Run Selections'!T113=\"Select Model\", \"\", 'Run Selections'!U113)","v":""},{"$f":"IF('Run Selections'!T113=\"Select Model\", \"\", 'Run Selections'!V113)","v":""},{"$f":"IF('Run Selections'!T113=\"Select Model\", \"\", 'Run Selections'!W113)","v":""},{"$f":"IF('Run Selections'!T113=\"Select Model\", \"\", 'Run Selections'!AB113)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T114=\"Select Model\", \"\", 'Run Selections'!F114)","v":""},{"$f":"IF('Run Selections'!T114=\"Select Model\", \"\", 'Run Selections'!L114)","v":""},{"$f":"IF('Run Selections'!T114=\"Select Model\", \"\", 'Run Selections'!T114)","v":""},{"$f":"IF('Run Selections'!T114=\"Select Model\", \"\", 'Run Selections'!U114)","v":""},{"$f":"IF('Run Selections'!T114=\"Select Model\", \"\", 'Run Selections'!V114)","v":""},{"$f":"IF('Run Selections'!T114=\"Select Model\", \"\", 'Run Selections'!W114)","v":""},{"$f":"IF('Run Selections'!T114=\"Select Model\", \"\", 'Run Selections'!AB114)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T115=\"Select Model\", \"\", 'Run Selections'!F115)","v":""},{"$f":"IF('Run Selections'!T115=\"Select Model\", \"\", 'Run Selections'!L115)","v":""},{"$f":"IF('Run Selections'!T115=\"Select Model\", \"\", 'Run Selections'!T115)","v":""},{"$f":"IF('Run Selections'!T115=\"Select Model\", \"\", 'Run Selections'!U115)","v":""},{"$f":"IF('Run Selections'!T115=\"Select Model\", \"\", 'Run Selections'!V115)","v":""},{"$f":"IF('Run Selections'!T115=\"Select Model\", \"\", 'Run Selections'!W115)","v":""},{"$f":"IF('Run Selections'!T115=\"Select Model\", \"\", 'Run Selections'!AB115)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T116=\"Select Model\", \"\", 'Run Selections'!F116)","v":""},{"$f":"IF('Run Selections'!T116=\"Select Model\", \"\", 'Run Selections'!L116)","v":""},{"$f":"IF('Run Selections'!T116=\"Select Model\", \"\", 'Run Selections'!T116)","v":""},{"$f":"IF('Run Selections'!T116=\"Select Model\", \"\", 'Run Selections'!U116)","v":""},{"$f":"IF('Run Selections'!T116=\"Select Model\", \"\", 'Run Selections'!V116)","v":""},{"$f":"IF('Run Selections'!T116=\"Select Model\", \"\", 'Run Selections'!W116)","v":""},{"$f":"IF('Run Selections'!T116=\"Select Model\", \"\", 'Run Selections'!AB116)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T117=\"Select Model\", \"\", 'Run Selections'!F117)","v":""},{"$f":"IF('Run Selections'!T117=\"Select Model\", \"\", 'Run Selections'!L117)","v":""},{"$f":"IF('Run Selections'!T117=\"Select Model\", \"\", 'Run Selections'!T117)","v":""},{"$f":"IF('Run Selections'!T117=\"Select Model\", \"\", 'Run Selections'!U117)","v":""},{"$f":"IF('Run Selections'!T117=\"Select Model\", \"\", 'Run Selections'!V117)","v":""},{"$f":"IF('Run Selections'!T117=\"Select Model\", \"\", 'Run Selections'!W117)","v":""},{"$f":"IF('Run Selections'!T117=\"Select Model\", \"\", 'Run Selections'!AB117)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T118=\"Select Model\", \"\", 'Run Selections'!F118)","v":""},{"$f":"IF('Run Selections'!T118=\"Select Model\", \"\", 'Run Selections'!L118)","v":""},{"$f":"IF('Run Selections'!T118=\"Select Model\", \"\", 'Run Selections'!T118)","v":""},{"$f":"IF('Run Selections'!T118=\"Select Model\", \"\", 'Run Selections'!U118)","v":""},{"$f":"IF('Run Selections'!T118=\"Select Model\", \"\", 'Run Selections'!V118)","v":""},{"$f":"IF('Run Selections'!T118=\"Select Model\", \"\", 'Run Selections'!W118)","v":""},{"$f":"IF('Run Selections'!T118=\"Select Model\", \"\", 'Run Selections'!AB118)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T119=\"Select Model\", \"\", 'Run Selections'!F119)","v":""},{"$f":"IF('Run Selections'!T119=\"Select Model\", \"\", 'Run Selections'!L119)","v":""},{"$f":"IF('Run Selections'!T119=\"Select Model\", \"\", 'Run Selections'!T119)","v":""},{"$f":"IF('Run Selections'!T119=\"Select Model\", \"\", 'Run Selections'!U119)","v":""},{"$f":"IF('Run Selections'!T119=\"Select Model\", \"\", 'Run Selections'!V119)","v":""},{"$f":"IF('Run Selections'!T119=\"Select Model\", \"\", 'Run Selections'!W119)","v":""},{"$f":"IF('Run Selections'!T119=\"Select Model\", \"\", 'Run Selections'!AB119)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T120=\"Select Model\", \"\", 'Run Selections'!F120)","v":""},{"$f":"IF('Run Selections'!T120=\"Select Model\", \"\", 'Run Selections'!L120)","v":""},{"$f":"IF('Run Selections'!T120=\"Select Model\", \"\", 'Run Selections'!T120)","v":""},{"$f":"IF('Run Selections'!T120=\"Select Model\", \"\", 'Run Selections'!U120)","v":""},{"$f":"IF('Run Selections'!T120=\"Select Model\", \"\", 'Run Selections'!V120)","v":""},{"$f":"IF('Run Selections'!T120=\"Select Model\", \"\", 'Run Selections'!W120)","v":""},{"$f":"IF('Run Selections'!T120=\"Select Model\", \"\", 'Run Selections'!AB120)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T121=\"Select Model\", \"\", 'Run Selections'!F121)","v":""},{"$f":"IF('Run Selections'!T121=\"Select Model\", \"\", 'Run Selections'!L121)","v":""},{"$f":"IF('Run Selections'!T121=\"Select Model\", \"\", 'Run Selections'!T121)","v":""},{"$f":"IF('Run Selections'!T121=\"Select Model\", \"\", 'Run Selections'!U121)","v":""},{"$f":"IF('Run Selections'!T121=\"Select Model\", \"\", 'Run Selections'!V121)","v":""},{"$f":"IF('Run Selections'!T121=\"Select Model\", \"\", 'Run Selections'!W121)","v":""},{"$f":"IF('Run Selections'!T121=\"Select Model\", \"\", 'Run Selections'!AB121)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T122=\"Select Model\", \"\", 'Run Selections'!F122)","v":""},{"$f":"IF('Run Selections'!T122=\"Select Model\", \"\", 'Run Selections'!L122)","v":""},{"$f":"IF('Run Selections'!T122=\"Select Model\", \"\", 'Run Selections'!T122)","v":""},{"$f":"IF('Run Selections'!T122=\"Select Model\", \"\", 'Run Selections'!U122)","v":""},{"$f":"IF('Run Selections'!T122=\"Select Model\", \"\", 'Run Selections'!V122)","v":""},{"$f":"IF('Run Selections'!T122=\"Select Model\", \"\", 'Run Selections'!W122)","v":""},{"$f":"IF('Run Selections'!T122=\"Select Model\", \"\", 'Run Selections'!AB122)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T123=\"Select Model\", \"\", 'Run Selections'!F123)","v":""},{"$f":"IF('Run Selections'!T123=\"Select Model\", \"\", 'Run Selections'!L123)","v":""},{"$f":"IF('Run Selections'!T123=\"Select Model\", \"\", 'Run Selections'!T123)","v":""},{"$f":"IF('Run Selections'!T123=\"Select Model\", \"\", 'Run Selections'!U123)","v":""},{"$f":"IF('Run Selections'!T123=\"Select Model\", \"\", 'Run Selections'!V123)","v":""},{"$f":"IF('Run Selections'!T123=\"Select Model\", \"\", 'Run Selections'!W123)","v":""},{"$f":"IF('Run Selections'!T123=\"Select Model\", \"\", 'Run Selections'!AB123)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T124=\"Select Model\", \"\", 'Run Selections'!F124)","v":""},{"$f":"IF('Run Selections'!T124=\"Select Model\", \"\", 'Run Selections'!L124)","v":""},{"$f":"IF('Run Selections'!T124=\"Select Model\", \"\", 'Run Selections'!T124)","v":""},{"$f":"IF('Run Selections'!T124=\"Select Model\", \"\", 'Run Selections'!U124)","v":""},{"$f":"IF('Run Selections'!T124=\"Select Model\", \"\", 'Run Selections'!V124)","v":""},{"$f":"IF('Run Selections'!T124=\"Select Model\", \"\", 'Run Selections'!W124)","v":""},{"$f":"IF('Run Selections'!T124=\"Select Model\", \"\", 'Run Selections'!AB124)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T125=\"Select Model\", \"\", 'Run Selections'!F125)","v":""},{"$f":"IF('Run Selections'!T125=\"Select Model\", \"\", 'Run Selections'!L125)","v":""},{"$f":"IF('Run Selections'!T125=\"Select Model\", \"\", 'Run Selections'!T125)","v":""},{"$f":"IF('Run Selections'!T125=\"Select Model\", \"\", 'Run Selections'!U125)","v":""},{"$f":"IF('Run Selections'!T125=\"Select Model\", \"\", 'Run Selections'!V125)","v":""},{"$f":"IF('Run Selections'!T125=\"Select Model\", \"\", 'Run Selections'!W125)","v":""},{"$f":"IF('Run Selections'!T125=\"Select Model\", \"\", 'Run Selections'!AB125)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T126=\"Select Model\", \"\", 'Run Selections'!F126)","v":""},{"$f":"IF('Run Selections'!T126=\"Select Model\", \"\", 'Run Selections'!L126)","v":""},{"$f":"IF('Run Selections'!T126=\"Select Model\", \"\", 'Run Selections'!T126)","v":""},{"$f":"IF('Run Selections'!T126=\"Select Model\", \"\", 'Run Selections'!U126)","v":""},{"$f":"IF('Run Selections'!T126=\"Select Model\", \"\", 'Run Selections'!V126)","v":""},{"$f":"IF('Run Selections'!T126=\"Select Model\", \"\", 'Run Selections'!W126)","v":""},{"$f":"IF('Run Selections'!T126=\"Select Model\", \"\", 'Run Selections'!AB126)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T127=\"Select Model\", \"\", 'Run Selections'!F127)","v":""},{"$f":"IF('Run Selections'!T127=\"Select Model\", \"\", 'Run Selections'!L127)","v":""},{"$f":"IF('Run Selections'!T127=\"Select Model\", \"\", 'Run Selections'!T127)","v":""},{"$f":"IF('Run Selections'!T127=\"Select Model\", \"\", 'Run Selections'!U127)","v":""},{"$f":"IF('Run Selections'!T127=\"Select Model\", \"\", 'Run Selections'!V127)","v":""},{"$f":"IF('Run Selections'!T127=\"Select Model\", \"\", 'Run Selections'!W127)","v":""},{"$f":"IF('Run Selections'!T127=\"Select Model\", \"\", 'Run Selections'!AB127)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T128=\"Select Model\", \"\", 'Run Selections'!F128)","v":""},{"$f":"IF('Run Selections'!T128=\"Select Model\", \"\", 'Run Selections'!L128)","v":""},{"$f":"IF('Run Selections'!T128=\"Select Model\", \"\", 'Run Selections'!T128)","v":""},{"$f":"IF('Run Selections'!T128=\"Select Model\", \"\", 'Run Selections'!U128)","v":""},{"$f":"IF('Run Selections'!T128=\"Select Model\", \"\", 'Run Selections'!V128)","v":""},{"$f":"IF('Run Selections'!T128=\"Select Model\", \"\", 'Run Selections'!W128)","v":""},{"$f":"IF('Run Selections'!T128=\"Select Model\", \"\", 'Run Selections'!AB128)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T129=\"Select Model\", \"\", 'Run Selections'!F129)","v":""},{"$f":"IF('Run Selections'!T129=\"Select Model\", \"\", 'Run Selections'!L129)","v":""},{"$f":"IF('Run Selections'!T129=\"Select Model\", \"\", 'Run Selections'!T129)","v":""},{"$f":"IF('Run Selections'!T129=\"Select Model\", \"\", 'Run Selections'!U129)","v":""},{"$f":"IF('Run Selections'!T129=\"Select Model\", \"\", 'Run Selections'!V129)","v":""},{"$f":"IF('Run Selections'!T129=\"Select Model\", \"\", 'Run Selections'!W129)","v":""},{"$f":"IF('Run Selections'!T129=\"Select Model\", \"\", 'Run Selections'!AB129)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T130=\"Select Model\", \"\", 'Run Selections'!F130)","v":""},{"$f":"IF('Run Selections'!T130=\"Select Model\", \"\", 'Run Selections'!L130)","v":""},{"$f":"IF('Run Selections'!T130=\"Select Model\", \"\", 'Run Selections'!T130)","v":""},{"$f":"IF('Run Selections'!T130=\"Select Model\", \"\", 'Run Selections'!U130)","v":""},{"$f":"IF('Run Selections'!T130=\"Select Model\", \"\", 'Run Selections'!V130)","v":""},{"$f":"IF('Run Selections'!T130=\"Select Model\", \"\", 'Run Selections'!W130)","v":""},{"$f":"IF('Run Selections'!T130=\"Select Model\", \"\", 'Run Selections'!AB130)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T131=\"Select Model\", \"\", 'Run Selections'!F131)","v":""},{"$f":"IF('Run Selections'!T131=\"Select Model\", \"\", 'Run Selections'!L131)","v":""},{"$f":"IF('Run Selections'!T131=\"Select Model\", \"\", 'Run Selections'!T131)","v":""},{"$f":"IF('Run Selections'!T131=\"Select Model\", \"\", 'Run Selections'!U131)","v":""},{"$f":"IF('Run Selections'!T131=\"Select Model\", \"\", 'Run Selections'!V131)","v":""},{"$f":"IF('Run Selections'!T131=\"Select Model\", \"\", 'Run Selections'!W131)","v":""},{"$f":"IF('Run Selections'!T131=\"Select Model\", \"\", 'Run Selections'!AB131)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T132=\"Select Model\", \"\", 'Run Selections'!F132)","v":""},{"$f":"IF('Run Selections'!T132=\"Select Model\", \"\", 'Run Selections'!L132)","v":""},{"$f":"IF('Run Selections'!T132=\"Select Model\", \"\", 'Run Selections'!T132)","v":""},{"$f":"IF('Run Selections'!T132=\"Select Model\", \"\", 'Run Selections'!U132)","v":""},{"$f":"IF('Run Selections'!T132=\"Select Model\", \"\", 'Run Selections'!V132)","v":""},{"$f":"IF('Run Selections'!T132=\"Select Model\", \"\", 'Run Selections'!W132)","v":""},{"$f":"IF('Run Selections'!T132=\"Select Model\", \"\", 'Run Selections'!AB132)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T133=\"Select Model\", \"\", 'Run Selections'!F133)","v":""},{"$f":"IF('Run Selections'!T133=\"Select Model\", \"\", 'Run Selections'!L133)","v":""},{"$f":"IF('Run Selections'!T133=\"Select Model\", \"\", 'Run Selections'!T133)","v":""},{"$f":"IF('Run Selections'!T133=\"Select Model\", \"\", 'Run Selections'!U133)","v":""},{"$f":"IF('Run Selections'!T133=\"Select Model\", \"\", 'Run Selections'!V133)","v":""},{"$f":"IF('Run Selections'!T133=\"Select Model\", \"\", 'Run Selections'!W133)","v":""},{"$f":"IF('Run Selections'!T133=\"Select Model\", \"\", 'Run Selections'!AB133)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T134=\"Select Model\", \"\", 'Run Selections'!F134)","v":""},{"$f":"IF('Run Selections'!T134=\"Select Model\", \"\", 'Run Selections'!L134)","v":""},{"$f":"IF('Run Selections'!T134=\"Select Model\", \"\", 'Run Selections'!T134)","v":""},{"$f":"IF('Run Selections'!T134=\"Select Model\", \"\", 'Run Selections'!U134)","v":""},{"$f":"IF('Run Selections'!T134=\"Select Model\", \"\", 'Run Selections'!V134)","v":""},{"$f":"IF('Run Selections'!T134=\"Select Model\", \"\", 'Run Selections'!W134)","v":""},{"$f":"IF('Run Selections'!T134=\"Select Model\", \"\", 'Run Selections'!AB134)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T135=\"Select Model\", \"\", 'Run Selections'!F135)","v":""},{"$f":"IF('Run Selections'!T135=\"Select Model\", \"\", 'Run Selections'!L135)","v":""},{"$f":"IF('Run Selections'!T135=\"Select Model\", \"\", 'Run Selections'!T135)","v":""},{"$f":"IF('Run Selections'!T135=\"Select Model\", \"\", 'Run Selections'!U135)","v":""},{"$f":"IF('Run Selections'!T135=\"Select Model\", \"\", 'Run Selections'!V135)","v":""},{"$f":"IF('Run Selections'!T135=\"Select Model\", \"\", 'Run Selections'!W135)","v":""},{"$f":"IF('Run Selections'!T135=\"Select Model\", \"\", 'Run Selections'!AB135)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T136=\"Select Model\", \"\", 'Run Selections'!F136)","v":""},{"$f":"IF('Run Selections'!T136=\"Select Model\", \"\", 'Run Selections'!L136)","v":""},{"$f":"IF('Run Selections'!T136=\"Select Model\", \"\", 'Run Selections'!T136)","v":""},{"$f":"IF('Run Selections'!T136=\"Select Model\", \"\", 'Run Selections'!U136)","v":""},{"$f":"IF('Run Selections'!T136=\"Select Model\", \"\", 'Run Selections'!V136)","v":""},{"$f":"IF('Run Selections'!T136=\"Select Model\", \"\", 'Run Selections'!W136)","v":""},{"$f":"IF('Run Selections'!T136=\"Select Model\", \"\", 'Run Selections'!AB136)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T137=\"Select Model\", \"\", 'Run Selections'!F137)","v":""},{"$f":"IF('Run Selections'!T137=\"Select Model\", \"\", 'Run Selections'!L137)","v":""},{"$f":"IF('Run Selections'!T137=\"Select Model\", \"\", 'Run Selections'!T137)","v":""},{"$f":"IF('Run Selections'!T137=\"Select Model\", \"\", 'Run Selections'!U137)","v":""},{"$f":"IF('Run Selections'!T137=\"Select Model\", \"\", 'Run Selections'!V137)","v":""},{"$f":"IF('Run Selections'!T137=\"Select Model\", \"\", 'Run Selections'!W137)","v":""},{"$f":"IF('Run Selections'!T137=\"Select Model\", \"\", 'Run Selections'!AB137)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T138=\"Select Model\", \"\", 'Run Selections'!F138)","v":""},{"$f":"IF('Run Selections'!T138=\"Select Model\", \"\", 'Run Selections'!L138)","v":""},{"$f":"IF('Run Selections'!T138=\"Select Model\", \"\", 'Run Selections'!T138)","v":""},{"$f":"IF('Run Selections'!T138=\"Select Model\", \"\", 'Run Selections'!U138)","v":""},{"$f":"IF('Run Selections'!T138=\"Select Model\", \"\", 'Run Selections'!V138)","v":""},{"$f":"IF('Run Selections'!T138=\"Select Model\", \"\", 'Run Selections'!W138)","v":""},{"$f":"IF('Run Selections'!T138=\"Select Model\", \"\", 'Run Selections'!AB138)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T139=\"Select Model\", \"\", 'Run Selections'!F139)","v":""},{"$f":"IF('Run Selections'!T139=\"Select Model\", \"\", 'Run Selections'!L139)","v":""},{"$f":"IF('Run Selections'!T139=\"Select Model\", \"\", 'Run Selections'!T139)","v":""},{"$f":"IF('Run Selections'!T139=\"Select Model\", \"\", 'Run Selections'!U139)","v":""},{"$f":"IF('Run Selections'!T139=\"Select Model\", \"\", 'Run Selections'!V139)","v":""},{"$f":"IF('Run Selections'!T139=\"Select Model\", \"\", 'Run Selections'!W139)","v":""},{"$f":"IF('Run Selections'!T139=\"Select Model\", \"\", 'Run Selections'!AB139)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T140=\"Select Model\", \"\", 'Run Selections'!F140)","v":""},{"$f":"IF('Run Selections'!T140=\"Select Model\", \"\", 'Run Selections'!L140)","v":""},{"$f":"IF('Run Selections'!T140=\"Select Model\", \"\", 'Run Selections'!T140)","v":""},{"$f":"IF('Run Selections'!T140=\"Select Model\", \"\", 'Run Selections'!U140)","v":""},{"$f":"IF('Run Selections'!T140=\"Select Model\", \"\", 'Run Selections'!V140)","v":""},{"$f":"IF('Run Selections'!T140=\"Select Model\", \"\", 'Run Selections'!W140)","v":""},{"$f":"IF('Run Selections'!T140=\"Select Model\", \"\", 'Run Selections'!AB140)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T141=\"Select Model\", \"\", 'Run Selections'!F141)","v":""},{"$f":"IF('Run Selections'!T141=\"Select Model\", \"\", 'Run Selections'!L141)","v":""},{"$f":"IF('Run Selections'!T141=\"Select Model\", \"\", 'Run Selections'!T141)","v":""},{"$f":"IF('Run Selections'!T141=\"Select Model\", \"\", 'Run Selections'!U141)","v":""},{"$f":"IF('Run Selections'!T141=\"Select Model\", \"\", 'Run Selections'!V141)","v":""},{"$f":"IF('Run Selections'!T141=\"Select Model\", \"\", 'Run Selections'!W141)","v":""},{"$f":"IF('Run Selections'!T141=\"Select Model\", \"\", 'Run Selections'!AB141)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T142=\"Select Model\", \"\", 'Run Selections'!F142)","v":""},{"$f":"IF('Run Selections'!T142=\"Select Model\", \"\", 'Run Selections'!L142)","v":""},{"$f":"IF('Run Selections'!T142=\"Select Model\", \"\", 'Run Selections'!T142)","v":""},{"$f":"IF('Run Selections'!T142=\"Select Model\", \"\", 'Run Selections'!U142)","v":""},{"$f":"IF('Run Selections'!T142=\"Select Model\", \"\", 'Run Selections'!V142)","v":""},{"$f":"IF('Run Selections'!T142=\"Select Model\", \"\", 'Run Selections'!W142)","v":""},{"$f":"IF('Run Selections'!T142=\"Select Model\", \"\", 'Run Selections'!AB142)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T143=\"Select Model\", \"\", 'Run Selections'!F143)","v":""},{"$f":"IF('Run Selections'!T143=\"Select Model\", \"\", 'Run Selections'!L143)","v":""},{"$f":"IF('Run Selections'!T143=\"Select Model\", \"\", 'Run Selections'!T143)","v":""},{"$f":"IF('Run Selections'!T143=\"Select Model\", \"\", 'Run Selections'!U143)","v":""},{"$f":"IF('Run Selections'!T143=\"Select Model\", \"\", 'Run Selections'!V143)","v":""},{"$f":"IF('Run Selections'!T143=\"Select Model\", \"\", 'Run Selections'!W143)","v":""},{"$f":"IF('Run Selections'!T143=\"Select Model\", \"\", 'Run Selections'!AB143)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T144=\"Select Model\", \"\", 'Run Selections'!F144)","v":""},{"$f":"IF('Run Selections'!T144=\"Select Model\", \"\", 'Run Selections'!L144)","v":""},{"$f":"IF('Run Selections'!T144=\"Select Model\", \"\", 'Run Selections'!T144)","v":""},{"$f":"IF('Run Selections'!T144=\"Select Model\", \"\", 'Run Selections'!U144)","v":""},{"$f":"IF('Run Selections'!T144=\"Select Model\", \"\", 'Run Selections'!V144)","v":""},{"$f":"IF('Run Selections'!T144=\"Select Model\", \"\", 'Run Selections'!W144)","v":""},{"$f":"IF('Run Selections'!T144=\"Select Model\", \"\", 'Run Selections'!AB144)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T145=\"Select Model\", \"\", 'Run Selections'!F145)","v":""},{"$f":"IF('Run Selections'!T145=\"Select Model\", \"\", 'Run Selections'!L145)","v":""},{"$f":"IF('Run Selections'!T145=\"Select Model\", \"\", 'Run Selections'!T145)","v":""},{"$f":"IF('Run Selections'!T145=\"Select Model\", \"\", 'Run Selections'!U145)","v":""},{"$f":"IF('Run Selections'!T145=\"Select Model\", \"\", 'Run Selections'!V145)","v":""},{"$f":"IF('Run Selections'!T145=\"Select Model\", \"\", 'Run Selections'!W145)","v":""},{"$f":"IF('Run Selections'!T145=\"Select Model\", \"\", 'Run Selections'!AB145)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T146=\"Select Model\", \"\", 'Run Selections'!F146)","v":""},{"$f":"IF('Run Selections'!T146=\"Select Model\", \"\", 'Run Selections'!L146)","v":""},{"$f":"IF('Run Selections'!T146=\"Select Model\", \"\", 'Run Selections'!T146)","v":""},{"$f":"IF('Run Selections'!T146=\"Select Model\", \"\", 'Run Selections'!U146)","v":""},{"$f":"IF('Run Selections'!T146=\"Select Model\", \"\", 'Run Selections'!V146)","v":""},{"$f":"IF('Run Selections'!T146=\"Select Model\", \"\", 'Run Selections'!W146)","v":""},{"$f":"IF('Run Selections'!T146=\"Select Model\", \"\", 'Run Selections'!AB146)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T147=\"Select Model\", \"\", 'Run Selections'!F147)","v":""},{"$f":"IF('Run Selections'!T147=\"Select Model\", \"\", 'Run Selections'!L147)","v":""},{"$f":"IF('Run Selections'!T147=\"Select Model\", \"\", 'Run Selections'!T147)","v":""},{"$f":"IF('Run Selections'!T147=\"Select Model\", \"\", 'Run Selections'!U147)","v":""},{"$f":"IF('Run Selections'!T147=\"Select Model\", \"\", 'Run Selections'!V147)","v":""},{"$f":"IF('Run Selections'!T147=\"Select Model\", \"\", 'Run Selections'!W147)","v":""},{"$f":"IF('Run Selections'!T147=\"Select Model\", \"\", 'Run Selections'!AB147)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T148=\"Select Model\", \"\", 'Run Selections'!F148)","v":""},{"$f":"IF('Run Selections'!T148=\"Select Model\", \"\", 'Run Selections'!L148)","v":""},{"$f":"IF('Run Selections'!T148=\"Select Model\", \"\", 'Run Selections'!T148)","v":""},{"$f":"IF('Run Selections'!T148=\"Select Model\", \"\", 'Run Selections'!U148)","v":""},{"$f":"IF('Run Selections'!T148=\"Select Model\", \"\", 'Run Selections'!V148)","v":""},{"$f":"IF('Run Selections'!T148=\"Select Model\", \"\", 'Run Selections'!W148)","v":""},{"$f":"IF('Run Selections'!T148=\"Select Model\", \"\", 'Run Selections'!AB148)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T149=\"Select Model\", \"\", 'Run Selections'!F149)","v":""},{"$f":"IF('Run Selections'!T149=\"Select Model\", \"\", 'Run Selections'!L149)","v":""},{"$f":"IF('Run Selections'!T149=\"Select Model\", \"\", 'Run Selections'!T149)","v":""},{"$f":"IF('Run Selections'!T149=\"Select Model\", \"\", 'Run Selections'!U149)","v":""},{"$f":"IF('Run Selections'!T149=\"Select Model\", \"\", 'Run Selections'!V149)","v":""},{"$f":"IF('Run Selections'!T149=\"Select Model\", \"\", 'Run Selections'!W149)","v":""},{"$f":"IF('Run Selections'!T149=\"Select Model\", \"\", 'Run Selections'!AB149)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T150=\"Select Model\", \"\", 'Run Selections'!F150)","v":""},{"$f":"IF('Run Selections'!T150=\"Select Model\", \"\", 'Run Selections'!L150)","v":""},{"$f":"IF('Run Selections'!T150=\"Select Model\", \"\", 'Run Selections'!T150)","v":""},{"$f":"IF('Run Selections'!T150=\"Select Model\", \"\", 'Run Selections'!U150)","v":""},{"$f":"IF('Run Selections'!T150=\"Select Model\", \"\", 'Run Selections'!V150)","v":""},{"$f":"IF('Run Selections'!T150=\"Select Model\", \"\", 'Run Selections'!W150)","v":""},{"$f":"IF('Run Selections'!T150=\"Select Model\", \"\", 'Run Selections'!AB150)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T151=\"Select Model\", \"\", 'Run Selections'!F151)","v":""},{"$f":"IF('Run Selections'!T151=\"Select Model\", \"\", 'Run Selections'!L151)","v":""},{"$f":"IF('Run Selections'!T151=\"Select Model\", \"\", 'Run Selections'!T151)","v":""},{"$f":"IF('Run Selections'!T151=\"Select Model\", \"\", 'Run Selections'!U151)","v":""},{"$f":"IF('Run Selections'!T151=\"Select Model\", \"\", 'Run Selections'!V151)","v":""},{"$f":"IF('Run Selections'!T151=\"Select Model\", \"\", 'Run Selections'!W151)","v":""},{"$f":"IF('Run Selections'!T151=\"Select Model\", \"\", 'Run Selections'!AB151)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T152=\"Select Model\", \"\", 'Run Selections'!F152)","v":""},{"$f":"IF('Run Selections'!T152=\"Select Model\", \"\", 'Run Selections'!L152)","v":""},{"$f":"IF('Run Selections'!T152=\"Select Model\", \"\", 'Run Selections'!T152)","v":""},{"$f":"IF('Run Selections'!T152=\"Select Model\", \"\", 'Run Selections'!U152)","v":""},{"$f":"IF('Run Selections'!T152=\"Select Model\", \"\", 'Run Selections'!V152)","v":""},{"$f":"IF('Run Selections'!T152=\"Select Model\", \"\", 'Run Selections'!W152)","v":""},{"$f":"IF('Run Selections'!T152=\"Select Model\", \"\", 'Run Selections'!AB152)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T153=\"Select Model\", \"\", 'Run Selections'!F153)","v":""},{"$f":"IF('Run Selections'!T153=\"Select Model\", \"\", 'Run Selections'!L153)","v":""},{"$f":"IF('Run Selections'!T153=\"Select Model\", \"\", 'Run Selections'!T153)","v":""},{"$f":"IF('Run Selections'!T153=\"Select Model\", \"\", 'Run Selections'!U153)","v":""},{"$f":"IF('Run Selections'!T153=\"Select Model\", \"\", 'Run Selections'!V153)","v":""},{"$f":"IF('Run Selections'!T153=\"Select Model\", \"\", 'Run Selections'!W153)","v":""},{"$f":"IF('Run Selections'!T153=\"Select Model\", \"\", 'Run Selections'!AB153)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T154=\"Select Model\", \"\", 'Run Selections'!F154)","v":""},{"$f":"IF('Run Selections'!T154=\"Select Model\", \"\", 'Run Selections'!L154)","v":""},{"$f":"IF('Run Selections'!T154=\"Select Model\", \"\", 'Run Selections'!T154)","v":""},{"$f":"IF('Run Selections'!T154=\"Select Model\", \"\", 'Run Selections'!U154)","v":""},{"$f":"IF('Run Selections'!T154=\"Select Model\", \"\", 'Run Selections'!V154)","v":""},{"$f":"IF('Run Selections'!T154=\"Select Model\", \"\", 'Run Selections'!W154)","v":""},{"$f":"IF('Run Selections'!T154=\"Select Model\", \"\", 'Run Selections'!AB154)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T155=\"Select Model\", \"\", 'Run Selections'!F155)","v":""},{"$f":"IF('Run Selections'!T155=\"Select Model\", \"\", 'Run Selections'!L155)","v":""},{"$f":"IF('Run Selections'!T155=\"Select Model\", \"\", 'Run Selections'!T155)","v":""},{"$f":"IF('Run Selections'!T155=\"Select Model\", \"\", 'Run Selections'!U155)","v":""},{"$f":"IF('Run Selections'!T155=\"Select Model\", \"\", 'Run Selections'!V155)","v":""},{"$f":"IF('Run Selections'!T155=\"Select Model\", \"\", 'Run Selections'!W155)","v":""},{"$f":"IF('Run Selections'!T155=\"Select Model\", \"\", 'Run Selections'!AB155)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T156=\"Select Model\", \"\", 'Run Selections'!F156)","v":""},{"$f":"IF('Run Selections'!T156=\"Select Model\", \"\", 'Run Selections'!L156)","v":""},{"$f":"IF('Run Selections'!T156=\"Select Model\", \"\", 'Run Selections'!T156)","v":""},{"$f":"IF('Run Selections'!T156=\"Select Model\", \"\", 'Run Selections'!U156)","v":""},{"$f":"IF('Run Selections'!T156=\"Select Model\", \"\", 'Run Selections'!V156)","v":""},{"$f":"IF('Run Selections'!T156=\"Select Model\", \"\", 'Run Selections'!W156)","v":""},{"$f":"IF('Run Selections'!T156=\"Select Model\", \"\", 'Run Selections'!AB156)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T157=\"Select Model\", \"\", 'Run Selections'!F157)","v":""},{"$f":"IF('Run Selections'!T157=\"Select Model\", \"\", 'Run Selections'!L157)","v":""},{"$f":"IF('Run Selections'!T157=\"Select Model\", \"\", 'Run Selections'!T157)","v":""},{"$f":"IF('Run Selections'!T157=\"Select Model\", \"\", 'Run Selections'!U157)","v":""},{"$f":"IF('Run Selections'!T157=\"Select Model\", \"\", 'Run Selections'!V157)","v":""},{"$f":"IF('Run Selections'!T157=\"Select Model\", \"\", 'Run Selections'!W157)","v":""},{"$f":"IF('Run Selections'!T157=\"Select Model\", \"\", 'Run Selections'!AB157)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T158=\"Select Model\", \"\", 'Run Selections'!F158)","v":""},{"$f":"IF('Run Selections'!T158=\"Select Model\", \"\", 'Run Selections'!L158)","v":""},{"$f":"IF('Run Selections'!T158=\"Select Model\", \"\", 'Run Selections'!T158)","v":""},{"$f":"IF('Run Selections'!T158=\"Select Model\", \"\", 'Run Selections'!U158)","v":""},{"$f":"IF('Run Selections'!T158=\"Select Model\", \"\", 'Run Selections'!V158)","v":""},{"$f":"IF('Run Selections'!T158=\"Select Model\", \"\", 'Run Selections'!W158)","v":""},{"$f":"IF('Run Selections'!T158=\"Select Model\", \"\", 'Run Selections'!AB158)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T159=\"Select Model\", \"\", 'Run Selections'!F159)","v":""},{"$f":"IF('Run Selections'!T159=\"Select Model\", \"\", 'Run Selections'!L159)","v":""},{"$f":"IF('Run Selections'!T159=\"Select Model\", \"\", 'Run Selections'!T159)","v":""},{"$f":"IF('Run Selections'!T159=\"Select Model\", \"\", 'Run Selections'!U159)","v":""},{"$f":"IF('Run Selections'!T159=\"Select Model\", \"\", 'Run Selections'!V159)","v":""},{"$f":"IF('Run Selections'!T159=\"Select Model\", \"\", 'Run Selections'!W159)","v":""},{"$f":"IF('Run Selections'!T159=\"Select Model\", \"\", 'Run Selections'!AB159)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T160=\"Select Model\", \"\", 'Run Selections'!F160)","v":""},{"$f":"IF('Run Selections'!T160=\"Select Model\", \"\", 'Run Selections'!L160)","v":""},{"$f":"IF('Run Selections'!T160=\"Select Model\", \"\", 'Run Selections'!T160)","v":""},{"$f":"IF('Run Selections'!T160=\"Select Model\", \"\", 'Run Selections'!U160)","v":""},{"$f":"IF('Run Selections'!T160=\"Select Model\", \"\", 'Run Selections'!V160)","v":""},{"$f":"IF('Run Selections'!T160=\"Select Model\", \"\", 'Run Selections'!W160)","v":""},{"$f":"IF('Run Selections'!T160=\"Select Model\", \"\", 'Run Selections'!AB160)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T161=\"Select Model\", \"\", 'Run Selections'!F161)","v":""},{"$f":"IF('Run Selections'!T161=\"Select Model\", \"\", 'Run Selections'!L161)","v":""},{"$f":"IF('Run Selections'!T161=\"Select Model\", \"\", 'Run Selections'!T161)","v":""},{"$f":"IF('Run Selections'!T161=\"Select Model\", \"\", 'Run Selections'!U161)","v":""},{"$f":"IF('Run Selections'!T161=\"Select Model\", \"\", 'Run Selections'!V161)","v":""},{"$f":"IF('Run Selections'!T161=\"Select Model\", \"\", 'Run Selections'!W161)","v":""},{"$f":"IF('Run Selections'!T161=\"Select Model\", \"\", 'Run Selections'!AB161)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T162=\"Select Model\", \"\", 'Run Selections'!F162)","v":""},{"$f":"IF('Run Selections'!T162=\"Select Model\", \"\", 'Run Selections'!L162)","v":""},{"$f":"IF('Run Selections'!T162=\"Select Model\", \"\", 'Run Selections'!T162)","v":""},{"$f":"IF('Run Selections'!T162=\"Select Model\", \"\", 'Run Selections'!U162)","v":""},{"$f":"IF('Run Selections'!T162=\"Select Model\", \"\", 'Run Selections'!V162)","v":""},{"$f":"IF('Run Selections'!T162=\"Select Model\", \"\", 'Run Selections'!W162)","v":""},{"$f":"IF('Run Selections'!T162=\"Select Model\", \"\", 'Run Selections'!AB162)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T163=\"Select Model\", \"\", 'Run Selections'!F163)","v":""},{"$f":"IF('Run Selections'!T163=\"Select Model\", \"\", 'Run Selections'!L163)","v":""},{"$f":"IF('Run Selections'!T163=\"Select Model\", \"\", 'Run Selections'!T163)","v":""},{"$f":"IF('Run Selections'!T163=\"Select Model\", \"\", 'Run Selections'!U163)","v":""},{"$f":"IF('Run Selections'!T163=\"Select Model\", \"\", 'Run Selections'!V163)","v":""},{"$f":"IF('Run Selections'!T163=\"Select Model\", \"\", 'Run Selections'!W163)","v":""},{"$f":"IF('Run Selections'!T163=\"Select Model\", \"\", 'Run Selections'!AB163)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T164=\"Select Model\", \"\", 'Run Selections'!F164)","v":""},{"$f":"IF('Run Selections'!T164=\"Select Model\", \"\", 'Run Selections'!L164)","v":""},{"$f":"IF('Run Selections'!T164=\"Select Model\", \"\", 'Run Selections'!T164)","v":""},{"$f":"IF('Run Selections'!T164=\"Select Model\", \"\", 'Run Selections'!U164)","v":""},{"$f":"IF('Run Selections'!T164=\"Select Model\", \"\", 'Run Selections'!V164)","v":""},{"$f":"IF('Run Selections'!T164=\"Select Model\", \"\", 'Run Selections'!W164)","v":""},{"$f":"IF('Run Selections'!T164=\"Select Model\", \"\", 'Run Selections'!AB164)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T165=\"Select Model\", \"\", 'Run Selections'!F165)","v":""},{"$f":"IF('Run Selections'!T165=\"Select Model\", \"\", 'Run Selections'!L165)","v":""},{"$f":"IF('Run Selections'!T165=\"Select Model\", \"\", 'Run Selections'!T165)","v":""},{"$f":"IF('Run Selections'!T165=\"Select Model\", \"\", 'Run Selections'!U165)","v":""},{"$f":"IF('Run Selections'!T165=\"Select Model\", \"\", 'Run Selections'!V165)","v":""},{"$f":"IF('Run Selections'!T165=\"Select Model\", \"\", 'Run Selections'!W165)","v":""},{"$f":"IF('Run Selections'!T165=\"Select Model\", \"\", 'Run Selections'!AB165)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T166=\"Select Model\", \"\", 'Run Selections'!F166)","v":""},{"$f":"IF('Run Selections'!T166=\"Select Model\", \"\", 'Run Selections'!L166)","v":""},{"$f":"IF('Run Selections'!T166=\"Select Model\", \"\", 'Run Selections'!T166)","v":""},{"$f":"IF('Run Selections'!T166=\"Select Model\", \"\", 'Run Selections'!U166)","v":""},{"$f":"IF('Run Selections'!T166=\"Select Model\", \"\", 'Run Selections'!V166)","v":""},{"$f":"IF('Run Selections'!T166=\"Select Model\", \"\", 'Run Selections'!W166)","v":""},{"$f":"IF('Run Selections'!T166=\"Select Model\", \"\", 'Run Selections'!AB166)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T167=\"Select Model\", \"\", 'Run Selections'!F167)","v":""},{"$f":"IF('Run Selections'!T167=\"Select Model\", \"\", 'Run Selections'!L167)","v":""},{"$f":"IF('Run Selections'!T167=\"Select Model\", \"\", 'Run Selections'!T167)","v":""},{"$f":"IF('Run Selections'!T167=\"Select Model\", \"\", 'Run Selections'!U167)","v":""},{"$f":"IF('Run Selections'!T167=\"Select Model\", \"\", 'Run Selections'!V167)","v":""},{"$f":"IF('Run Selections'!T167=\"Select Model\", \"\", 'Run Selections'!W167)","v":""},{"$f":"IF('Run Selections'!T167=\"Select Model\", \"\", 'Run Selections'!AB167)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T168=\"Select Model\", \"\", 'Run Selections'!F168)","v":""},{"$f":"IF('Run Selections'!T168=\"Select Model\", \"\", 'Run Selections'!L168)","v":""},{"$f":"IF('Run Selections'!T168=\"Select Model\", \"\", 'Run Selections'!T168)","v":""},{"$f":"IF('Run Selections'!T168=\"Select Model\", \"\", 'Run Selections'!U168)","v":""},{"$f":"IF('Run Selections'!T168=\"Select Model\", \"\", 'Run Selections'!V168)","v":""},{"$f":"IF('Run Selections'!T168=\"Select Model\", \"\", 'Run Selections'!W168)","v":""},{"$f":"IF('Run Selections'!T168=\"Select Model\", \"\", 'Run Selections'!AB168)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T169=\"Select Model\", \"\", 'Run Selections'!F169)","v":""},{"$f":"IF('Run Selections'!T169=\"Select Model\", \"\", 'Run Selections'!L169)","v":""},{"$f":"IF('Run Selections'!T169=\"Select Model\", \"\", 'Run Selections'!T169)","v":""},{"$f":"IF('Run Selections'!T169=\"Select Model\", \"\", 'Run Selections'!U169)","v":""},{"$f":"IF('Run Selections'!T169=\"Select Model\", \"\", 'Run Selections'!V169)","v":""},{"$f":"IF('Run Selections'!T169=\"Select Model\", \"\", 'Run Selections'!W169)","v":""},{"$f":"IF('Run Selections'!T169=\"Select Model\", \"\", 'Run Selections'!AB169)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T170=\"Select Model\", \"\", 'Run Selections'!F170)","v":""},{"$f":"IF('Run Selections'!T170=\"Select Model\", \"\", 'Run Selections'!L170)","v":""},{"$f":"IF('Run Selections'!T170=\"Select Model\", \"\", 'Run Selections'!T170)","v":""},{"$f":"IF('Run Selections'!T170=\"Select Model\", \"\", 'Run Selections'!U170)","v":""},{"$f":"IF('Run Selections'!T170=\"Select Model\", \"\", 'Run Selections'!V170)","v":""},{"$f":"IF('Run Selections'!T170=\"Select Model\", \"\", 'Run Selections'!W170)","v":""},{"$f":"IF('Run Selections'!T170=\"Select Model\", \"\", 'Run Selections'!AB170)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T171=\"Select Model\", \"\", 'Run Selections'!F171)","v":""},{"$f":"IF('Run Selections'!T171=\"Select Model\", \"\", 'Run Selections'!L171)","v":""},{"$f":"IF('Run Selections'!T171=\"Select Model\", \"\", 'Run Selections'!T171)","v":""},{"$f":"IF('Run Selections'!T171=\"Select Model\", \"\", 'Run Selections'!U171)","v":""},{"$f":"IF('Run Selections'!T171=\"Select Model\", \"\", 'Run Selections'!V171)","v":""},{"$f":"IF('Run Selections'!T171=\"Select Model\", \"\", 'Run Selections'!W171)","v":""},{"$f":"IF('Run Selections'!T171=\"Select Model\", \"\", 'Run Selections'!AB171)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T172=\"Select Model\", \"\", 'Run Selections'!F172)","v":""},{"$f":"IF('Run Selections'!T172=\"Select Model\", \"\", 'Run Selections'!L172)","v":""},{"$f":"IF('Run Selections'!T172=\"Select Model\", \"\", 'Run Selections'!T172)","v":""},{"$f":"IF('Run Selections'!T172=\"Select Model\", \"\", 'Run Selections'!U172)","v":""},{"$f":"IF('Run Selections'!T172=\"Select Model\", \"\", 'Run Selections'!V172)","v":""},{"$f":"IF('Run Selections'!T172=\"Select Model\", \"\", 'Run Selections'!W172)","v":""},{"$f":"IF('Run Selections'!T172=\"Select Model\", \"\", 'Run Selections'!AB172)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T173=\"Select Model\", \"\", 'Run Selections'!F173)","v":""},{"$f":"IF('Run Selections'!T173=\"Select Model\", \"\", 'Run Selections'!L173)","v":""},{"$f":"IF('Run Selections'!T173=\"Select Model\", \"\", 'Run Selections'!T173)","v":""},{"$f":"IF('Run Selections'!T173=\"Select Model\", \"\", 'Run Selections'!U173)","v":""},{"$f":"IF('Run Selections'!T173=\"Select Model\", \"\", 'Run Selections'!V173)","v":""},{"$f":"IF('Run Selections'!T173=\"Select Model\", \"\", 'Run Selections'!W173)","v":""},{"$f":"IF('Run Selections'!T173=\"Select Model\", \"\", 'Run Selections'!AB173)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T174=\"Select Model\", \"\", 'Run Selections'!F174)","v":""},{"$f":"IF('Run Selections'!T174=\"Select Model\", \"\", 'Run Selections'!L174)","v":""},{"$f":"IF('Run Selections'!T174=\"Select Model\", \"\", 'Run Selections'!T174)","v":""},{"$f":"IF('Run Selections'!T174=\"Select Model\", \"\", 'Run Selections'!U174)","v":""},{"$f":"IF('Run Selections'!T174=\"Select Model\", \"\", 'Run Selections'!V174)","v":""},{"$f":"IF('Run Selections'!T174=\"Select Model\", \"\", 'Run Selections'!W174)","v":""},{"$f":"IF('Run Selections'!T174=\"Select Model\", \"\", 'Run Selections'!AB174)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T175=\"Select Model\", \"\", 'Run Selections'!F175)","v":""},{"$f":"IF('Run Selections'!T175=\"Select Model\", \"\", 'Run Selections'!L175)","v":""},{"$f":"IF('Run Selections'!T175=\"Select Model\", \"\", 'Run Selections'!T175)","v":""},{"$f":"IF('Run Selections'!T175=\"Select Model\", \"\", 'Run Selections'!U175)","v":""},{"$f":"IF('Run Selections'!T175=\"Select Model\", \"\", 'Run Selections'!V175)","v":""},{"$f":"IF('Run Selections'!T175=\"Select Model\", \"\", 'Run Selections'!W175)","v":""},{"$f":"IF('Run Selections'!T175=\"Select Model\", \"\", 'Run Selections'!AB175)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T176=\"Select Model\", \"\", 'Run Selections'!F176)","v":""},{"$f":"IF('Run Selections'!T176=\"Select Model\", \"\", 'Run Selections'!L176)","v":""},{"$f":"IF('Run Selections'!T176=\"Select Model\", \"\", 'Run Selections'!T176)","v":""},{"$f":"IF('Run Selections'!T176=\"Select Model\", \"\", 'Run Selections'!U176)","v":""},{"$f":"IF('Run Selections'!T176=\"Select Model\", \"\", 'Run Selections'!V176)","v":""},{"$f":"IF('Run Selections'!T176=\"Select Model\", \"\", 'Run Selections'!W176)","v":""},{"$f":"IF('Run Selections'!T176=\"Select Model\", \"\", 'Run Selections'!AB176)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T177=\"Select Model\", \"\", 'Run Selections'!F177)","v":""},{"$f":"IF('Run Selections'!T177=\"Select Model\", \"\", 'Run Selections'!L177)","v":""},{"$f":"IF('Run Selections'!T177=\"Select Model\", \"\", 'Run Selections'!T177)","v":""},{"$f":"IF('Run Selections'!T177=\"Select Model\", \"\", 'Run Selections'!U177)","v":""},{"$f":"IF('Run Selections'!T177=\"Select Model\", \"\", 'Run Selections'!V177)","v":""},{"$f":"IF('Run Selections'!T177=\"Select Model\", \"\", 'Run Selections'!W177)","v":""},{"$f":"IF('Run Selections'!T177=\"Select Model\", \"\", 'Run Selections'!AB177)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T178=\"Select Model\", \"\", 'Run Selections'!F178)","v":""},{"$f":"IF('Run Selections'!T178=\"Select Model\", \"\", 'Run Selections'!L178)","v":""},{"$f":"IF('Run Selections'!T178=\"Select Model\", \"\", 'Run Selections'!T178)","v":""},{"$f":"IF('Run Selections'!T178=\"Select Model\", \"\", 'Run Selections'!U178)","v":""},{"$f":"IF('Run Selections'!T178=\"Select Model\", \"\", 'Run Selections'!V178)","v":""},{"$f":"IF('Run Selections'!T178=\"Select Model\", \"\", 'Run Selections'!W178)","v":""},{"$f":"IF('Run Selections'!T178=\"Select Model\", \"\", 'Run Selections'!AB178)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T179=\"Select Model\", \"\", 'Run Selections'!F179)","v":""},{"$f":"IF('Run Selections'!T179=\"Select Model\", \"\", 'Run Selections'!L179)","v":""},{"$f":"IF('Run Selections'!T179=\"Select Model\", \"\", 'Run Selections'!T179)","v":""},{"$f":"IF('Run Selections'!T179=\"Select Model\", \"\", 'Run Selections'!U179)","v":""},{"$f":"IF('Run Selections'!T179=\"Select Model\", \"\", 'Run Selections'!V179)","v":""},{"$f":"IF('Run Selections'!T179=\"Select Model\", \"\", 'Run Selections'!W179)","v":""},{"$f":"IF('Run Selections'!T179=\"Select Model\", \"\", 'Run Selections'!AB179)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T180=\"Select Model\", \"\", 'Run Selections'!F180)","v":""},{"$f":"IF('Run Selections'!T180=\"Select Model\", \"\", 'Run Selections'!L180)","v":""},{"$f":"IF('Run Selections'!T180=\"Select Model\", \"\", 'Run Selections'!T180)","v":""},{"$f":"IF('Run Selections'!T180=\"Select Model\", \"\", 'Run Selections'!U180)","v":""},{"$f":"IF('Run Selections'!T180=\"Select Model\", \"\", 'Run Selections'!V180)","v":""},{"$f":"IF('Run Selections'!T180=\"Select Model\", \"\", 'Run Selections'!W180)","v":""},{"$f":"IF('Run Selections'!T180=\"Select Model\", \"\", 'Run Selections'!AB180)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T181=\"Select Model\", \"\", 'Run Selections'!F181)","v":""},{"$f":"IF('Run Selections'!T181=\"Select Model\", \"\", 'Run Selections'!L181)","v":""},{"$f":"IF('Run Selections'!T181=\"Select Model\", \"\", 'Run Selections'!T181)","v":""},{"$f":"IF('Run Selections'!T181=\"Select Model\", \"\", 'Run Selections'!U181)","v":""},{"$f":"IF('Run Selections'!T181=\"Select Model\", \"\", 'Run Selections'!V181)","v":""},{"$f":"IF('Run Selections'!T181=\"Select Model\", \"\", 'Run Selections'!W181)","v":""},{"$f":"IF('Run Selections'!T181=\"Select Model\", \"\", 'Run Selections'!AB181)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T182=\"Select Model\", \"\", 'Run Selections'!F182)","v":""},{"$f":"IF('Run Selections'!T182=\"Select Model\", \"\", 'Run Selections'!L182)","v":""},{"$f":"IF('Run Selections'!T182=\"Select Model\", \"\", 'Run Selections'!T182)","v":""},{"$f":"IF('Run Selections'!T182=\"Select Model\", \"\", 'Run Selections'!U182)","v":""},{"$f":"IF('Run Selections'!T182=\"Select Model\", \"\", 'Run Selections'!V182)","v":""},{"$f":"IF('Run Selections'!T182=\"Select Model\", \"\", 'Run Selections'!W182)","v":""},{"$f":"IF('Run Selections'!T182=\"Select Model\", \"\", 'Run Selections'!AB182)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T183=\"Select Model\", \"\", 'Run Selections'!F183)","v":""},{"$f":"IF('Run Selections'!T183=\"Select Model\", \"\", 'Run Selections'!L183)","v":""},{"$f":"IF('Run Selections'!T183=\"Select Model\", \"\", 'Run Selections'!T183)","v":""},{"$f":"IF('Run Selections'!T183=\"Select Model\", \"\", 'Run Selections'!U183)","v":""},{"$f":"IF('Run Selections'!T183=\"Select Model\", \"\", 'Run Selections'!V183)","v":""},{"$f":"IF('Run Selections'!T183=\"Select Model\", \"\", 'Run Selections'!W183)","v":""},{"$f":"IF('Run Selections'!T183=\"Select Model\", \"\", 'Run Selections'!AB183)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T184=\"Select Model\", \"\", 'Run Selections'!F184)","v":""},{"$f":"IF('Run Selections'!T184=\"Select Model\", \"\", 'Run Selections'!L184)","v":""},{"$f":"IF('Run Selections'!T184=\"Select Model\", \"\", 'Run Selections'!T184)","v":""},{"$f":"IF('Run Selections'!T184=\"Select Model\", \"\", 'Run Selections'!U184)","v":""},{"$f":"IF('Run Selections'!T184=\"Select Model\", \"\", 'Run Selections'!V184)","v":""},{"$f":"IF('Run Selections'!T184=\"Select Model\", \"\", 'Run Selections'!W184)","v":""},{"$f":"IF('Run Selections'!T184=\"Select Model\", \"\", 'Run Selections'!AB184)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T185=\"Select Model\", \"\", 'Run Selections'!F185)","v":""},{"$f":"IF('Run Selections'!T185=\"Select Model\", \"\", 'Run Selections'!L185)","v":""},{"$f":"IF('Run Selections'!T185=\"Select Model\", \"\", 'Run Selections'!T185)","v":""},{"$f":"IF('Run Selections'!T185=\"Select Model\", \"\", 'Run Selections'!U185)","v":""},{"$f":"IF('Run Selections'!T185=\"Select Model\", \"\", 'Run Selections'!V185)","v":""},{"$f":"IF('Run Selections'!T185=\"Select Model\", \"\", 'Run Selections'!W185)","v":""},{"$f":"IF('Run Selections'!T185=\"Select Model\", \"\", 'Run Selections'!AB185)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T186=\"Select Model\", \"\", 'Run Selections'!F186)","v":""},{"$f":"IF('Run Selections'!T186=\"Select Model\", \"\", 'Run Selections'!L186)","v":""},{"$f":"IF('Run Selections'!T186=\"Select Model\", \"\", 'Run Selections'!T186)","v":""},{"$f":"IF('Run Selections'!T186=\"Select Model\", \"\", 'Run Selections'!U186)","v":""},{"$f":"IF('Run Selections'!T186=\"Select Model\", \"\", 'Run Selections'!V186)","v":""},{"$f":"IF('Run Selections'!T186=\"Select Model\", \"\", 'Run Selections'!W186)","v":""},{"$f":"IF('Run Selections'!T186=\"Select Model\", \"\", 'Run Selections'!AB186)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T187=\"Select Model\", \"\", 'Run Selections'!F187)","v":""},{"$f":"IF('Run Selections'!T187=\"Select Model\", \"\", 'Run Selections'!L187)","v":""},{"$f":"IF('Run Selections'!T187=\"Select Model\", \"\", 'Run Selections'!T187)","v":""},{"$f":"IF('Run Selections'!T187=\"Select Model\", \"\", 'Run Selections'!U187)","v":""},{"$f":"IF('Run Selections'!T187=\"Select Model\", \"\", 'Run Selections'!V187)","v":""},{"$f":"IF('Run Selections'!T187=\"Select Model\", \"\", 'Run Selections'!W187)","v":""},{"$f":"IF('Run Selections'!T187=\"Select Model\", \"\", 'Run Selections'!AB187)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T188=\"Select Model\", \"\", 'Run Selections'!F188)","v":""},{"$f":"IF('Run Selections'!T188=\"Select Model\", \"\", 'Run Selections'!L188)","v":""},{"$f":"IF('Run Selections'!T188=\"Select Model\", \"\", 'Run Selections'!T188)","v":""},{"$f":"IF('Run Selections'!T188=\"Select Model\", \"\", 'Run Selections'!U188)","v":""},{"$f":"IF('Run Selections'!T188=\"Select Model\", \"\", 'Run Selections'!V188)","v":""},{"$f":"IF('Run Selections'!T188=\"Select Model\", \"\", 'Run Selections'!W188)","v":""},{"$f":"IF('Run Selections'!T188=\"Select Model\", \"\", 'Run Selections'!AB188)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T189=\"Select Model\", \"\", 'Run Selections'!F189)","v":""},{"$f":"IF('Run Selections'!T189=\"Select Model\", \"\", 'Run Selections'!L189)","v":""},{"$f":"IF('Run Selections'!T189=\"Select Model\", \"\", 'Run Selections'!T189)","v":""},{"$f":"IF('Run Selections'!T189=\"Select Model\", \"\", 'Run Selections'!U189)","v":""},{"$f":"IF('Run Selections'!T189=\"Select Model\", \"\", 'Run Selections'!V189)","v":""},{"$f":"IF('Run Selections'!T189=\"Select Model\", \"\", 'Run Selections'!W189)","v":""},{"$f":"IF('Run Selections'!T189=\"Select Model\", \"\", 'Run Selections'!AB189)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T190=\"Select Model\", \"\", 'Run Selections'!F190)","v":""},{"$f":"IF('Run Selections'!T190=\"Select Model\", \"\", 'Run Selections'!L190)","v":""},{"$f":"IF('Run Selections'!T190=\"Select Model\", \"\", 'Run Selections'!T190)","v":""},{"$f":"IF('Run Selections'!T190=\"Select Model\", \"\", 'Run Selections'!U190)","v":""},{"$f":"IF('Run Selections'!T190=\"Select Model\", \"\", 'Run Selections'!V190)","v":""},{"$f":"IF('Run Selections'!T190=\"Select Model\", \"\", 'Run Selections'!W190)","v":""},{"$f":"IF('Run Selections'!T190=\"Select Model\", \"\", 'Run Selections'!AB190)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T191=\"Select Model\", \"\", 'Run Selections'!F191)","v":""},{"$f":"IF('Run Selections'!T191=\"Select Model\", \"\", 'Run Selections'!L191)","v":""},{"$f":"IF('Run Selections'!T191=\"Select Model\", \"\", 'Run Selections'!T191)","v":""},{"$f":"IF('Run Selections'!T191=\"Select Model\", \"\", 'Run Selections'!U191)","v":""},{"$f":"IF('Run Selections'!T191=\"Select Model\", \"\", 'Run Selections'!V191)","v":""},{"$f":"IF('Run Selections'!T191=\"Select Model\", \"\", 'Run Selections'!W191)","v":""},{"$f":"IF('Run Selections'!T191=\"Select Model\", \"\", 'Run Selections'!AB191)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T192=\"Select Model\", \"\", 'Run Selections'!F192)","v":""},{"$f":"IF('Run Selections'!T192=\"Select Model\", \"\", 'Run Selections'!L192)","v":""},{"$f":"IF('Run Selections'!T192=\"Select Model\", \"\", 'Run Selections'!T192)","v":""},{"$f":"IF('Run Selections'!T192=\"Select Model\", \"\", 'Run Selections'!U192)","v":""},{"$f":"IF('Run Selections'!T192=\"Select Model\", \"\", 'Run Selections'!V192)","v":""},{"$f":"IF('Run Selections'!T192=\"Select Model\", \"\", 'Run Selections'!W192)","v":""},{"$f":"IF('Run Selections'!T192=\"Select Model\", \"\", 'Run Selections'!AB192)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T193=\"Select Model\", \"\", 'Run Selections'!F193)","v":""},{"$f":"IF('Run Selections'!T193=\"Select Model\", \"\", 'Run Selections'!L193)","v":""},{"$f":"IF('Run Selections'!T193=\"Select Model\", \"\", 'Run Selections'!T193)","v":""},{"$f":"IF('Run Selections'!T193=\"Select Model\", \"\", 'Run Selections'!U193)","v":""},{"$f":"IF('Run Selections'!T193=\"Select Model\", \"\", 'Run Selections'!V193)","v":""},{"$f":"IF('Run Selections'!T193=\"Select Model\", \"\", 'Run Selections'!W193)","v":""},{"$f":"IF('Run Selections'!T193=\"Select Model\", \"\", 'Run Selections'!AB193)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T194=\"Select Model\", \"\", 'Run Selections'!F194)","v":""},{"$f":"IF('Run Selections'!T194=\"Select Model\", \"\", 'Run Selections'!L194)","v":""},{"$f":"IF('Run Selections'!T194=\"Select Model\", \"\", 'Run Selections'!T194)","v":""},{"$f":"IF('Run Selections'!T194=\"Select Model\", \"\", 'Run Selections'!U194)","v":""},{"$f":"IF('Run Selections'!T194=\"Select Model\", \"\", 'Run Selections'!V194)","v":""},{"$f":"IF('Run Selections'!T194=\"Select Model\", \"\", 'Run Selections'!W194)","v":""},{"$f":"IF('Run Selections'!T194=\"Select Model\", \"\", 'Run Selections'!AB194)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T195=\"Select Model\", \"\", 'Run Selections'!F195)","v":""},{"$f":"IF('Run Selections'!T195=\"Select Model\", \"\", 'Run Selections'!L195)","v":""},{"$f":"IF('Run Selections'!T195=\"Select Model\", \"\", 'Run Selections'!T195)","v":""},{"$f":"IF('Run Selections'!T195=\"Select Model\", \"\", 'Run Selections'!U195)","v":""},{"$f":"IF('Run Selections'!T195=\"Select Model\", \"\", 'Run Selections'!V195)","v":""},{"$f":"IF('Run Selections'!T195=\"Select Model\", \"\", 'Run Selections'!W195)","v":""},{"$f":"IF('Run Selections'!T195=\"Select Model\", \"\", 'Run Selections'!AB195)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T196=\"Select Model\", \"\", 'Run Selections'!F196)","v":""},{"$f":"IF('Run Selections'!T196=\"Select Model\", \"\", 'Run Selections'!L196)","v":""},{"$f":"IF('Run Selections'!T196=\"Select Model\", \"\", 'Run Selections'!T196)","v":""},{"$f":"IF('Run Selections'!T196=\"Select Model\", \"\", 'Run Selections'!U196)","v":""},{"$f":"IF('Run Selections'!T196=\"Select Model\", \"\", 'Run Selections'!V196)","v":""},{"$f":"IF('Run Selections'!T196=\"Select Model\", \"\", 'Run Selections'!W196)","v":""},{"$f":"IF('Run Selections'!T196=\"Select Model\", \"\", 'Run Selections'!AB196)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T197=\"Select Model\", \"\", 'Run Selections'!F197)","v":""},{"$f":"IF('Run Selections'!T197=\"Select Model\", \"\", 'Run Selections'!L197)","v":""},{"$f":"IF('Run Selections'!T197=\"Select Model\", \"\", 'Run Selections'!T197)","v":""},{"$f":"IF('Run Selections'!T197=\"Select Model\", \"\", 'Run Selections'!U197)","v":""},{"$f":"IF('Run Selections'!T197=\"Select Model\", \"\", 'Run Selections'!V197)","v":""},{"$f":"IF('Run Selections'!T197=\"Select Model\", \"\", 'Run Selections'!W197)","v":""},{"$f":"IF('Run Selections'!T197=\"Select Model\", \"\", 'Run Selections'!AB197)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T198=\"Select Model\", \"\", 'Run Selections'!F198)","v":""},{"$f":"IF('Run Selections'!T198=\"Select Model\", \"\", 'Run Selections'!L198)","v":""},{"$f":"IF('Run Selections'!T198=\"Select Model\", \"\", 'Run Selections'!T198)","v":""},{"$f":"IF('Run Selections'!T198=\"Select Model\", \"\", 'Run Selections'!U198)","v":""},{"$f":"IF('Run Selections'!T198=\"Select Model\", \"\", 'Run Selections'!V198)","v":""},{"$f":"IF('Run Selections'!T198=\"Select Model\", \"\", 'Run Selections'!W198)","v":""},{"$f":"IF('Run Selections'!T198=\"Select Model\", \"\", 'Run Selections'!AB198)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T199=\"Select Model\", \"\", 'Run Selections'!F199)","v":""},{"$f":"IF('Run Selections'!T199=\"Select Model\", \"\", 'Run Selections'!L199)","v":""},{"$f":"IF('Run Selections'!T199=\"Select Model\", \"\", 'Run Selections'!T199)","v":""},{"$f":"IF('Run Selections'!T199=\"Select Model\", \"\", 'Run Selections'!U199)","v":""},{"$f":"IF('Run Selections'!T199=\"Select Model\", \"\", 'Run Selections'!V199)","v":""},{"$f":"IF('Run Selections'!T199=\"Select Model\", \"\", 'Run Selections'!W199)","v":""},{"$f":"IF('Run Selections'!T199=\"Select Model\", \"\", 'Run Selections'!AB199)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T200=\"Select Model\", \"\", 'Run Selections'!F200)","v":""},{"$f":"IF('Run Selections'!T200=\"Select Model\", \"\", 'Run Selections'!L200)","v":""},{"$f":"IF('Run Selections'!T200=\"Select Model\", \"\", 'Run Selections'!T200)","v":""},{"$f":"IF('Run Selections'!T200=\"Select Model\", \"\", 'Run Selections'!U200)","v":""},{"$f":"IF('Run Selections'!T200=\"Select Model\", \"\", 'Run Selections'!V200)","v":""},{"$f":"IF('Run Selections'!T200=\"Select Model\", \"\", 'Run Selections'!W200)","v":""},{"$f":"IF('Run Selections'!T200=\"Select Model\", \"\", 'Run Selections'!AB200)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T201=\"Select Model\", \"\", 'Run Selections'!F201)","v":""},{"$f":"IF('Run Selections'!T201=\"Select Model\", \"\", 'Run Selections'!L201)","v":""},{"$f":"IF('Run Selections'!T201=\"Select Model\", \"\", 'Run Selections'!T201)","v":""},{"$f":"IF('Run Selections'!T201=\"Select Model\", \"\", 'Run Selections'!U201)","v":""},{"$f":"IF('Run Selections'!T201=\"Select Model\", \"\", 'Run Selections'!V201)","v":""},{"$f":"IF('Run Selections'!T201=\"Select Model\", \"\", 'Run Selections'!W201)","v":""},{"$f":"IF('Run Selections'!T201=\"Select Model\", \"\", 'Run Selections'!AB201)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T202=\"Select Model\", \"\", 'Run Selections'!F202)","v":""},{"$f":"IF('Run Selections'!T202=\"Select Model\", \"\", 'Run Selections'!L202)","v":""},{"$f":"IF('Run Selections'!T202=\"Select Model\", \"\", 'Run Selections'!T202)","v":""},{"$f":"IF('Run Selections'!T202=\"Select Model\", \"\", 'Run Selections'!U202)","v":""},{"$f":"IF('Run Selections'!T202=\"Select Model\", \"\", 'Run Selections'!V202)","v":""},{"$f":"IF('Run Selections'!T202=\"Select Model\", \"\", 'Run Selections'!W202)","v":""},{"$f":"IF('Run Selections'!T202=\"Select Model\", \"\", 'Run Selections'!AB202)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T203=\"Select Model\", \"\", 'Run Selections'!F203)","v":""},{"$f":"IF('Run Selections'!T203=\"Select Model\", \"\", 'Run Selections'!L203)","v":""},{"$f":"IF('Run Selections'!T203=\"Select Model\", \"\", 'Run Selections'!T203)","v":""},{"$f":"IF('Run Selections'!T203=\"Select Model\", \"\", 'Run Selections'!U203)","v":""},{"$f":"IF('Run Selections'!T203=\"Select Model\", \"\", 'Run Selections'!V203)","v":""},{"$f":"IF('Run Selections'!T203=\"Select Model\", \"\", 'Run Selections'!W203)","v":""},{"$f":"IF('Run Selections'!T203=\"Select Model\", \"\", 'Run Selections'!AB203)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T204=\"Select Model\", \"\", 'Run Selections'!F204)","v":""},{"$f":"IF('Run Selections'!T204=\"Select Model\", \"\", 'Run Selections'!L204)","v":""},{"$f":"IF('Run Selections'!T204=\"Select Model\", \"\", 'Run Selections'!T204)","v":""},{"$f":"IF('Run Selections'!T204=\"Select Model\", \"\", 'Run Selections'!U204)","v":""},{"$f":"IF('Run Selections'!T204=\"Select Model\", \"\", 'Run Selections'!V204)","v":""},{"$f":"IF('Run Selections'!T204=\"Select Model\", \"\", 'Run Selections'!W204)","v":""},{"$f":"IF('Run Selections'!T204=\"Select Model\", \"\", 'Run Selections'!AB204)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T205=\"Select Model\", \"\", 'Run Selections'!F205)","v":""},{"$f":"IF('Run Selections'!T205=\"Select Model\", \"\", 'Run Selections'!L205)","v":""},{"$f":"IF('Run Selections'!T205=\"Select Model\", \"\", 'Run Selections'!T205)","v":""},{"$f":"IF('Run Selections'!T205=\"Select Model\", \"\", 'Run Selections'!U205)","v":""},{"$f":"IF('Run Selections'!T205=\"Select Model\", \"\", 'Run Selections'!V205)","v":""},{"$f":"IF('Run Selections'!T205=\"Select Model\", \"\", 'Run Selections'!W205)","v":""},{"$f":"IF('Run Selections'!T205=\"Select Model\", \"\", 'Run Selections'!AB205)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T206=\"Select Model\", \"\", 'Run Selections'!F206)","v":""},{"$f":"IF('Run Selections'!T206=\"Select Model\", \"\", 'Run Selections'!L206)","v":""},{"$f":"IF('Run Selections'!T206=\"Select Model\", \"\", 'Run Selections'!T206)","v":""},{"$f":"IF('Run Selections'!T206=\"Select Model\", \"\", 'Run Selections'!U206)","v":""},{"$f":"IF('Run Selections'!T206=\"Select Model\", \"\", 'Run Selections'!V206)","v":""},{"$f":"IF('Run Selections'!T206=\"Select Model\", \"\", 'Run Selections'!W206)","v":""},{"$f":"IF('Run Selections'!T206=\"Select Model\", \"\", 'Run Selections'!AB206)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T207=\"Select Model\", \"\", 'Run Selections'!F207)","v":""},{"$f":"IF('Run Selections'!T207=\"Select Model\", \"\", 'Run Selections'!L207)","v":""},{"$f":"IF('Run Selections'!T207=\"Select Model\", \"\", 'Run Selections'!T207)","v":""},{"$f":"IF('Run Selections'!T207=\"Select Model\", \"\", 'Run Selections'!U207)","v":""},{"$f":"IF('Run Selections'!T207=\"Select Model\", \"\", 'Run Selections'!V207)","v":""},{"$f":"IF('Run Selections'!T207=\"Select Model\", \"\", 'Run Selections'!W207)","v":""},{"$f":"IF('Run Selections'!T207=\"Select Model\", \"\", 'Run Selections'!AB207)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T208=\"Select Model\", \"\", 'Run Selections'!F208)","v":""},{"$f":"IF('Run Selections'!T208=\"Select Model\", \"\", 'Run Selections'!L208)","v":""},{"$f":"IF('Run Selections'!T208=\"Select Model\", \"\", 'Run Selections'!T208)","v":""},{"$f":"IF('Run Selections'!T208=\"Select Model\", \"\", 'Run Selections'!U208)","v":""},{"$f":"IF('Run Selections'!T208=\"Select Model\", \"\", 'Run Selections'!V208)","v":""},{"$f":"IF('Run Selections'!T208=\"Select Model\", \"\", 'Run Selections'!W208)","v":""},{"$f":"IF('Run Selections'!T208=\"Select Model\", \"\", 'Run Selections'!AB208)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T209=\"Select Model\", \"\", 'Run Selections'!F209)","v":""},{"$f":"IF('Run Selections'!T209=\"Select Model\", \"\", 'Run Selections'!L209)","v":""},{"$f":"IF('Run Selections'!T209=\"Select Model\", \"\", 'Run Selections'!T209)","v":""},{"$f":"IF('Run Selections'!T209=\"Select Model\", \"\", 'Run Selections'!U209)","v":""},{"$f":"IF('Run Selections'!T209=\"Select Model\", \"\", 'Run Selections'!V209)","v":""},{"$f":"IF('Run Selections'!T209=\"Select Model\", \"\", 'Run Selections'!W209)","v":""},{"$f":"IF('Run Selections'!T209=\"Select Model\", \"\", 'Run Selections'!AB209)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T210=\"Select Model\", \"\", 'Run Selections'!F210)","v":""},{"$f":"IF('Run Selections'!T210=\"Select Model\", \"\", 'Run Selections'!L210)","v":""},{"$f":"IF('Run Selections'!T210=\"Select Model\", \"\", 'Run Selections'!T210)","v":""},{"$f":"IF('Run Selections'!T210=\"Select Model\", \"\", 'Run Selections'!U210)","v":""},{"$f":"IF('Run Selections'!T210=\"Select Model\", \"\", 'Run Selections'!V210)","v":""},{"$f":"IF('Run Selections'!T210=\"Select Model\", \"\", 'Run Selections'!W210)","v":""},{"$f":"IF('Run Selections'!T210=\"Select Model\", \"\", 'Run Selections'!AB210)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T211=\"Select Model\", \"\", 'Run Selections'!F211)","v":""},{"$f":"IF('Run Selections'!T211=\"Select Model\", \"\", 'Run Selections'!L211)","v":""},{"$f":"IF('Run Selections'!T211=\"Select Model\", \"\", 'Run Selections'!T211)","v":""},{"$f":"IF('Run Selections'!T211=\"Select Model\", \"\", 'Run Selections'!U211)","v":""},{"$f":"IF('Run Selections'!T211=\"Select Model\", \"\", 'Run Selections'!V211)","v":""},{"$f":"IF('Run Selections'!T211=\"Select Model\", \"\", 'Run Selections'!W211)","v":""},{"$f":"IF('Run Selections'!T211=\"Select Model\", \"\", 'Run Selections'!AB211)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T212=\"Select Model\", \"\", 'Run Selections'!F212)","v":""},{"$f":"IF('Run Selections'!T212=\"Select Model\", \"\", 'Run Selections'!L212)","v":""},{"$f":"IF('Run Selections'!T212=\"Select Model\", \"\", 'Run Selections'!T212)","v":""},{"$f":"IF('Run Selections'!T212=\"Select Model\", \"\", 'Run Selections'!U212)","v":""},{"$f":"IF('Run Selections'!T212=\"Select Model\", \"\", 'Run Selections'!V212)","v":""},{"$f":"IF('Run Selections'!T212=\"Select Model\", \"\", 'Run Selections'!W212)","v":""},{"$f":"IF('Run Selections'!T212=\"Select Model\", \"\", 'Run Selections'!AB212)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T213=\"Select Model\", \"\", 'Run Selections'!F213)","v":""},{"$f":"IF('Run Selections'!T213=\"Select Model\", \"\", 'Run Selections'!L213)","v":""},{"$f":"IF('Run Selections'!T213=\"Select Model\", \"\", 'Run Selections'!T213)","v":""},{"$f":"IF('Run Selections'!T213=\"Select Model\", \"\", 'Run Selections'!U213)","v":""},{"$f":"IF('Run Selections'!T213=\"Select Model\", \"\", 'Run Selections'!V213)","v":""},{"$f":"IF('Run Selections'!T213=\"Select Model\", \"\", 'Run Selections'!W213)","v":""},{"$f":"IF('Run Selections'!T213=\"Select Model\", \"\", 'Run Selections'!AB213)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T214=\"Select Model\", \"\", 'Run Selections'!F214)","v":""},{"$f":"IF('Run Selections'!T214=\"Select Model\", \"\", 'Run Selections'!L214)","v":""},{"$f":"IF('Run Selections'!T214=\"Select Model\", \"\", 'Run Selections'!T214)","v":""},{"$f":"IF('Run Selections'!T214=\"Select Model\", \"\", 'Run Selections'!U214)","v":""},{"$f":"IF('Run Selections'!T214=\"Select Model\", \"\", 'Run Selections'!V214)","v":""},{"$f":"IF('Run Selections'!T214=\"Select Model\", \"\", 'Run Selections'!W214)","v":""},{"$f":"IF('Run Selections'!T214=\"Select Model\", \"\", 'Run Selections'!AB214)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T215=\"Select Model\", \"\", 'Run Selections'!F215)","v":""},{"$f":"IF('Run Selections'!T215=\"Select Model\", \"\", 'Run Selections'!L215)","v":""},{"$f":"IF('Run Selections'!T215=\"Select Model\", \"\", 'Run Selections'!T215)","v":""},{"$f":"IF('Run Selections'!T215=\"Select Model\", \"\", 'Run Selections'!U215)","v":""},{"$f":"IF('Run Selections'!T215=\"Select Model\", \"\", 'Run Selections'!V215)","v":""},{"$f":"IF('Run Selections'!T215=\"Select Model\", \"\", 'Run Selections'!W215)","v":""},{"$f":"IF('Run Selections'!T215=\"Select Model\", \"\", 'Run Selections'!AB215)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T216=\"Select Model\", \"\", 'Run Selections'!F216)","v":""},{"$f":"IF('Run Selections'!T216=\"Select Model\", \"\", 'Run Selections'!L216)","v":""},{"$f":"IF('Run Selections'!T216=\"Select Model\", \"\", 'Run Selections'!T216)","v":""},{"$f":"IF('Run Selections'!T216=\"Select Model\", \"\", 'Run Selections'!U216)","v":""},{"$f":"IF('Run Selections'!T216=\"Select Model\", \"\", 'Run Selections'!V216)","v":""},{"$f":"IF('Run Selections'!T216=\"Select Model\", \"\", 'Run Selections'!W216)","v":""},{"$f":"IF('Run Selections'!T216=\"Select Model\", \"\", 'Run Selections'!AB216)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T217=\"Select Model\", \"\", 'Run Selections'!F217)","v":""},{"$f":"IF('Run Selections'!T217=\"Select Model\", \"\", 'Run Selections'!L217)","v":""},{"$f":"IF('Run Selections'!T217=\"Select Model\", \"\", 'Run Selections'!T217)","v":""},{"$f":"IF('Run Selections'!T217=\"Select Model\", \"\", 'Run Selections'!U217)","v":""},{"$f":"IF('Run Selections'!T217=\"Select Model\", \"\", 'Run Selections'!V217)","v":""},{"$f":"IF('Run Selections'!T217=\"Select Model\", \"\", 'Run Selections'!W217)","v":""},{"$f":"IF('Run Selections'!T217=\"Select Model\", \"\", 'Run Selections'!AB217)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T218=\"Select Model\", \"\", 'Run Selections'!F218)","v":""},{"$f":"IF('Run Selections'!T218=\"Select Model\", \"\", 'Run Selections'!L218)","v":""},{"$f":"IF('Run Selections'!T218=\"Select Model\", \"\", 'Run Selections'!T218)","v":""},{"$f":"IF('Run Selections'!T218=\"Select Model\", \"\", 'Run Selections'!U218)","v":""},{"$f":"IF('Run Selections'!T218=\"Select Model\", \"\", 'Run Selections'!V218)","v":""},{"$f":"IF('Run Selections'!T218=\"Select Model\", \"\", 'Run Selections'!W218)","v":""},{"$f":"IF('Run Selections'!T218=\"Select Model\", \"\", 'Run Selections'!AB218)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T219=\"Select Model\", \"\", 'Run Selections'!F219)","v":""},{"$f":"IF('Run Selections'!T219=\"Select Model\", \"\", 'Run Selections'!L219)","v":""},{"$f":"IF('Run Selections'!T219=\"Select Model\", \"\", 'Run Selections'!T219)","v":""},{"$f":"IF('Run Selections'!T219=\"Select Model\", \"\", 'Run Selections'!U219)","v":""},{"$f":"IF('Run Selections'!T219=\"Select Model\", \"\", 'Run Selections'!V219)","v":""},{"$f":"IF('Run Selections'!T219=\"Select Model\", \"\", 'Run Selections'!W219)","v":""},{"$f":"IF('Run Selections'!T219=\"Select Model\", \"\", 'Run Selections'!AB219)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T220=\"Select Model\", \"\", 'Run Selections'!F220)","v":""},{"$f":"IF('Run Selections'!T220=\"Select Model\", \"\", 'Run Selections'!L220)","v":""},{"$f":"IF('Run Selections'!T220=\"Select Model\", \"\", 'Run Selections'!T220)","v":""},{"$f":"IF('Run Selections'!T220=\"Select Model\", \"\", 'Run Selections'!U220)","v":""},{"$f":"IF('Run Selections'!T220=\"Select Model\", \"\", 'Run Selections'!V220)","v":""},{"$f":"IF('Run Selections'!T220=\"Select Model\", \"\", 'Run Selections'!W220)","v":""},{"$f":"IF('Run Selections'!T220=\"Select Model\", \"\", 'Run Selections'!AB220)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T221=\"Select Model\", \"\", 'Run Selections'!F221)","v":""},{"$f":"IF('Run Selections'!T221=\"Select Model\", \"\", 'Run Selections'!L221)","v":""},{"$f":"IF('Run Selections'!T221=\"Select Model\", \"\", 'Run Selections'!T221)","v":""},{"$f":"IF('Run Selections'!T221=\"Select Model\", \"\", 'Run Selections'!U221)","v":""},{"$f":"IF('Run Selections'!T221=\"Select Model\", \"\", 'Run Selections'!V221)","v":""},{"$f":"IF('Run Selections'!T221=\"Select Model\", \"\", 'Run Selections'!W221)","v":""},{"$f":"IF('Run Selections'!T221=\"Select Model\", \"\", 'Run Selections'!AB221)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T222=\"Select Model\", \"\", 'Run Selections'!F222)","v":""},{"$f":"IF('Run Selections'!T222=\"Select Model\", \"\", 'Run Selections'!L222)","v":""},{"$f":"IF('Run Selections'!T222=\"Select Model\", \"\", 'Run Selections'!T222)","v":""},{"$f":"IF('Run Selections'!T222=\"Select Model\", \"\", 'Run Selections'!U222)","v":""},{"$f":"IF('Run Selections'!T222=\"Select Model\", \"\", 'Run Selections'!V222)","v":""},{"$f":"IF('Run Selections'!T222=\"Select Model\", \"\", 'Run Selections'!W222)","v":""},{"$f":"IF('Run Selections'!T222=\"Select Model\", \"\", 'Run Selections'!AB222)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T223=\"Select Model\", \"\", 'Run Selections'!F223)","v":""},{"$f":"IF('Run Selections'!T223=\"Select Model\", \"\", 'Run Selections'!L223)","v":""},{"$f":"IF('Run Selections'!T223=\"Select Model\", \"\", 'Run Selections'!T223)","v":""},{"$f":"IF('Run Selections'!T223=\"Select Model\", \"\", 'Run Selections'!U223)","v":""},{"$f":"IF('Run Selections'!T223=\"Select Model\", \"\", 'Run Selections'!V223)","v":""},{"$f":"IF('Run Selections'!T223=\"Select Model\", \"\", 'Run Selections'!W223)","v":""},{"$f":"IF('Run Selections'!T223=\"Select Model\", \"\", 'Run Selections'!AB223)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T224=\"Select Model\", \"\", 'Run Selections'!F224)","v":""},{"$f":"IF('Run Selections'!T224=\"Select Model\", \"\", 'Run Selections'!L224)","v":""},{"$f":"IF('Run Selections'!T224=\"Select Model\", \"\", 'Run Selections'!T224)","v":""},{"$f":"IF('Run Selections'!T224=\"Select Model\", \"\", 'Run Selections'!U224)","v":""},{"$f":"IF('Run Selections'!T224=\"Select Model\", \"\", 'Run Selections'!V224)","v":""},{"$f":"IF('Run Selections'!T224=\"Select Model\", \"\", 'Run Selections'!W224)","v":""},{"$f":"IF('Run Selections'!T224=\"Select Model\", \"\", 'Run Selections'!AB224)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T225=\"Select Model\", \"\", 'Run Selections'!F225)","v":""},{"$f":"IF('Run Selections'!T225=\"Select Model\", \"\", 'Run Selections'!L225)","v":""},{"$f":"IF('Run Selections'!T225=\"Select Model\", \"\", 'Run Selections'!T225)","v":""},{"$f":"IF('Run Selections'!T225=\"Select Model\", \"\", 'Run Selections'!U225)","v":""},{"$f":"IF('Run Selections'!T225=\"Select Model\", \"\", 'Run Selections'!V225)","v":""},{"$f":"IF('Run Selections'!T225=\"Select Model\", \"\", 'Run Selections'!W225)","v":""},{"$f":"IF('Run Selections'!T225=\"Select Model\", \"\", 'Run Selections'!AB225)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T226=\"Select Model\", \"\", 'Run Selections'!F226)","v":""},{"$f":"IF('Run Selections'!T226=\"Select Model\", \"\", 'Run Selections'!L226)","v":""},{"$f":"IF('Run Selections'!T226=\"Select Model\", \"\", 'Run Selections'!T226)","v":""},{"$f":"IF('Run Selections'!T226=\"Select Model\", \"\", 'Run Selections'!U226)","v":""},{"$f":"IF('Run Selections'!T226=\"Select Model\", \"\", 'Run Selections'!V226)","v":""},{"$f":"IF('Run Selections'!T226=\"Select Model\", \"\", 'Run Selections'!W226)","v":""},{"$f":"IF('Run Selections'!T226=\"Select Model\", \"\", 'Run Selections'!AB226)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T227=\"Select Model\", \"\", 'Run Selections'!F227)","v":""},{"$f":"IF('Run Selections'!T227=\"Select Model\", \"\", 'Run Selections'!L227)","v":""},{"$f":"IF('Run Selections'!T227=\"Select Model\", \"\", 'Run Selections'!T227)","v":""},{"$f":"IF('Run Selections'!T227=\"Select Model\", \"\", 'Run Selections'!U227)","v":""},{"$f":"IF('Run Selections'!T227=\"Select Model\", \"\", 'Run Selections'!V227)","v":""},{"$f":"IF('Run Selections'!T227=\"Select Model\", \"\", 'Run Selections'!W227)","v":""},{"$f":"IF('Run Selections'!T227=\"Select Model\", \"\", 'Run Selections'!AB227)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T228=\"Select Model\", \"\", 'Run Selections'!F228)","v":""},{"$f":"IF('Run Selections'!T228=\"Select Model\", \"\", 'Run Selections'!L228)","v":""},{"$f":"IF('Run Selections'!T228=\"Select Model\", \"\", 'Run Selections'!T228)","v":""},{"$f":"IF('Run Selections'!T228=\"Select Model\", \"\", 'Run Selections'!U228)","v":""},{"$f":"IF('Run Selections'!T228=\"Select Model\", \"\", 'Run Selections'!V228)","v":""},{"$f":"IF('Run Selections'!T228=\"Select Model\", \"\", 'Run Selections'!W228)","v":""},{"$f":"IF('Run Selections'!T228=\"Select Model\", \"\", 'Run Selections'!AB228)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T229=\"Select Model\", \"\", 'Run Selections'!F229)","v":""},{"$f":"IF('Run Selections'!T229=\"Select Model\", \"\", 'Run Selections'!L229)","v":""},{"$f":"IF('Run Selections'!T229=\"Select Model\", \"\", 'Run Selections'!T229)","v":""},{"$f":"IF('Run Selections'!T229=\"Select Model\", \"\", 'Run Selections'!U229)","v":""},{"$f":"IF('Run Selections'!T229=\"Select Model\", \"\", 'Run Selections'!V229)","v":""},{"$f":"IF('Run Selections'!T229=\"Select Model\", \"\", 'Run Selections'!W229)","v":""},{"$f":"IF('Run Selections'!T229=\"Select Model\", \"\", 'Run Selections'!AB229)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T230=\"Select Model\", \"\", 'Run Selections'!F230)","v":""},{"$f":"IF('Run Selections'!T230=\"Select Model\", \"\", 'Run Selections'!L230)","v":""},{"$f":"IF('Run Selections'!T230=\"Select Model\", \"\", 'Run Selections'!T230)","v":""},{"$f":"IF('Run Selections'!T230=\"Select Model\", \"\", 'Run Selections'!U230)","v":""},{"$f":"IF('Run Selections'!T230=\"Select Model\", \"\", 'Run Selections'!V230)","v":""},{"$f":"IF('Run Selections'!T230=\"Select Model\", \"\", 'Run Selections'!W230)","v":""},{"$f":"IF('Run Selections'!T230=\"Select Model\", \"\", 'Run Selections'!AB230)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T231=\"Select Model\", \"\", 'Run Selections'!F231)","v":""},{"$f":"IF('Run Selections'!T231=\"Select Model\", \"\", 'Run Selections'!L231)","v":""},{"$f":"IF('Run Selections'!T231=\"Select Model\", \"\", 'Run Selections'!T231)","v":""},{"$f":"IF('Run Selections'!T231=\"Select Model\", \"\", 'Run Selections'!U231)","v":""},{"$f":"IF('Run Selections'!T231=\"Select Model\", \"\", 'Run Selections'!V231)","v":""},{"$f":"IF('Run Selections'!T231=\"Select Model\", \"\", 'Run Selections'!W231)","v":""},{"$f":"IF('Run Selections'!T231=\"Select Model\", \"\", 'Run Selections'!AB231)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T232=\"Select Model\", \"\", 'Run Selections'!F232)","v":""},{"$f":"IF('Run Selections'!T232=\"Select Model\", \"\", 'Run Selections'!L232)","v":""},{"$f":"IF('Run Selections'!T232=\"Select Model\", \"\", 'Run Selections'!T232)","v":""},{"$f":"IF('Run Selections'!T232=\"Select Model\", \"\", 'Run Selections'!U232)","v":""},{"$f":"IF('Run Selections'!T232=\"Select Model\", \"\", 'Run Selections'!V232)","v":""},{"$f":"IF('Run Selections'!T232=\"Select Model\", \"\", 'Run Selections'!W232)","v":""},{"$f":"IF('Run Selections'!T232=\"Select Model\", \"\", 'Run Selections'!AB232)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T233=\"Select Model\", \"\", 'Run Selections'!F233)","v":""},{"$f":"IF('Run Selections'!T233=\"Select Model\", \"\", 'Run Selections'!L233)","v":""},{"$f":"IF('Run Selections'!T233=\"Select Model\", \"\", 'Run Selections'!T233)","v":""},{"$f":"IF('Run Selections'!T233=\"Select Model\", \"\", 'Run Selections'!U233)","v":""},{"$f":"IF('Run Selections'!T233=\"Select Model\", \"\", 'Run Selections'!V233)","v":""},{"$f":"IF('Run Selections'!T233=\"Select Model\", \"\", 'Run Selections'!W233)","v":""},{"$f":"IF('Run Selections'!T233=\"Select Model\", \"\", 'Run Selections'!AB233)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T234=\"Select Model\", \"\", 'Run Selections'!F234)","v":""},{"$f":"IF('Run Selections'!T234=\"Select Model\", \"\", 'Run Selections'!L234)","v":""},{"$f":"IF('Run Selections'!T234=\"Select Model\", \"\", 'Run Selections'!T234)","v":""},{"$f":"IF('Run Selections'!T234=\"Select Model\", \"\", 'Run Selections'!U234)","v":""},{"$f":"IF('Run Selections'!T234=\"Select Model\", \"\", 'Run Selections'!V234)","v":""},{"$f":"IF('Run Selections'!T234=\"Select Model\", \"\", 'Run Selections'!W234)","v":""},{"$f":"IF('Run Selections'!T234=\"Select Model\", \"\", 'Run Selections'!AB234)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T235=\"Select Model\", \"\", 'Run Selections'!F235)","v":""},{"$f":"IF('Run Selections'!T235=\"Select Model\", \"\", 'Run Selections'!L235)","v":""},{"$f":"IF('Run Selections'!T235=\"Select Model\", \"\", 'Run Selections'!T235)","v":""},{"$f":"IF('Run Selections'!T235=\"Select Model\", \"\", 'Run Selections'!U235)","v":""},{"$f":"IF('Run Selections'!T235=\"Select Model\", \"\", 'Run Selections'!V235)","v":""},{"$f":"IF('Run Selections'!T235=\"Select Model\", \"\", 'Run Selections'!W235)","v":""},{"$f":"IF('Run Selections'!T235=\"Select Model\", \"\", 'Run Selections'!AB235)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T236=\"Select Model\", \"\", 'Run Selections'!F236)","v":""},{"$f":"IF('Run Selections'!T236=\"Select Model\", \"\", 'Run Selections'!L236)","v":""},{"$f":"IF('Run Selections'!T236=\"Select Model\", \"\", 'Run Selections'!T236)","v":""},{"$f":"IF('Run Selections'!T236=\"Select Model\", \"\", 'Run Selections'!U236)","v":""},{"$f":"IF('Run Selections'!T236=\"Select Model\", \"\", 'Run Selections'!V236)","v":""},{"$f":"IF('Run Selections'!T236=\"Select Model\", \"\", 'Run Selections'!W236)","v":""},{"$f":"IF('Run Selections'!T236=\"Select Model\", \"\", 'Run Selections'!AB236)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T237=\"Select Model\", \"\", 'Run Selections'!F237)","v":""},{"$f":"IF('Run Selections'!T237=\"Select Model\", \"\", 'Run Selections'!L237)","v":""},{"$f":"IF('Run Selections'!T237=\"Select Model\", \"\", 'Run Selections'!T237)","v":""},{"$f":"IF('Run Selections'!T237=\"Select Model\", \"\", 'Run Selections'!U237)","v":""},{"$f":"IF('Run Selections'!T237=\"Select Model\", \"\", 'Run Selections'!V237)","v":""},{"$f":"IF('Run Selections'!T237=\"Select Model\", \"\", 'Run Selections'!W237)","v":""},{"$f":"IF('Run Selections'!T237=\"Select Model\", \"\", 'Run Selections'!AB237)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T238=\"Select Model\", \"\", 'Run Selections'!F238)","v":""},{"$f":"IF('Run Selections'!T238=\"Select Model\", \"\", 'Run Selections'!L238)","v":""},{"$f":"IF('Run Selections'!T238=\"Select Model\", \"\", 'Run Selections'!T238)","v":""},{"$f":"IF('Run Selections'!T238=\"Select Model\", \"\", 'Run Selections'!U238)","v":""},{"$f":"IF('Run Selections'!T238=\"Select Model\", \"\", 'Run Selections'!V238)","v":""},{"$f":"IF('Run Selections'!T238=\"Select Model\", \"\", 'Run Selections'!W238)","v":""},{"$f":"IF('Run Selections'!T238=\"Select Model\", \"\", 'Run Selections'!AB238)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T239=\"Select Model\", \"\", 'Run Selections'!F239)","v":""},{"$f":"IF('Run Selections'!T239=\"Select Model\", \"\", 'Run Selections'!L239)","v":""},{"$f":"IF('Run Selections'!T239=\"Select Model\", \"\", 'Run Selections'!T239)","v":""},{"$f":"IF('Run Selections'!T239=\"Select Model\", \"\", 'Run Selections'!U239)","v":""},{"$f":"IF('Run Selections'!T239=\"Select Model\", \"\", 'Run Selections'!V239)","v":""},{"$f":"IF('Run Selections'!T239=\"Select Model\", \"\", 'Run Selections'!W239)","v":""},{"$f":"IF('Run Selections'!T239=\"Select Model\", \"\", 'Run Selections'!AB239)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T240=\"Select Model\", \"\", 'Run Selections'!F240)","v":""},{"$f":"IF('Run Selections'!T240=\"Select Model\", \"\", 'Run Selections'!L240)","v":""},{"$f":"IF('Run Selections'!T240=\"Select Model\", \"\", 'Run Selections'!T240)","v":""},{"$f":"IF('Run Selections'!T240=\"Select Model\", \"\", 'Run Selections'!U240)","v":""},{"$f":"IF('Run Selections'!T240=\"Select Model\", \"\", 'Run Selections'!V240)","v":""},{"$f":"IF('Run Selections'!T240=\"Select Model\", \"\", 'Run Selections'!W240)","v":""},{"$f":"IF('Run Selections'!T240=\"Select Model\", \"\", 'Run Selections'!AB240)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T241=\"Select Model\", \"\", 'Run Selections'!F241)","v":""},{"$f":"IF('Run Selections'!T241=\"Select Model\", \"\", 'Run Selections'!L241)","v":""},{"$f":"IF('Run Selections'!T241=\"Select Model\", \"\", 'Run Selections'!T241)","v":""},{"$f":"IF('Run Selections'!T241=\"Select Model\", \"\", 'Run Selections'!U241)","v":""},{"$f":"IF('Run Selections'!T241=\"Select Model\", \"\", 'Run Selections'!V241)","v":""},{"$f":"IF('Run Selections'!T241=\"Select Model\", \"\", 'Run Selections'!W241)","v":""},{"$f":"IF('Run Selections'!T241=\"Select Model\", \"\", 'Run Selections'!AB241)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T242=\"Select Model\", \"\", 'Run Selections'!F242)","v":""},{"$f":"IF('Run Selections'!T242=\"Select Model\", \"\", 'Run Selections'!L242)","v":""},{"$f":"IF('Run Selections'!T242=\"Select Model\", \"\", 'Run Selections'!T242)","v":""},{"$f":"IF('Run Selections'!T242=\"Select Model\", \"\", 'Run Selections'!U242)","v":""},{"$f":"IF('Run Selections'!T242=\"Select Model\", \"\", 'Run Selections'!V242)","v":""},{"$f":"IF('Run Selections'!T242=\"Select Model\", \"\", 'Run Selections'!W242)","v":""},{"$f":"IF('Run Selections'!T242=\"Select Model\", \"\", 'Run Selections'!AB242)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T243=\"Select Model\", \"\", 'Run Selections'!F243)","v":""},{"$f":"IF('Run Selections'!T243=\"Select Model\", \"\", 'Run Selections'!L243)","v":""},{"$f":"IF('Run Selections'!T243=\"Select Model\", \"\", 'Run Selections'!T243)","v":""},{"$f":"IF('Run Selections'!T243=\"Select Model\", \"\", 'Run Selections'!U243)","v":""},{"$f":"IF('Run Selections'!T243=\"Select Model\", \"\", 'Run Selections'!V243)","v":""},{"$f":"IF('Run Selections'!T243=\"Select Model\", \"\", 'Run Selections'!W243)","v":""},{"$f":"IF('Run Selections'!T243=\"Select Model\", \"\", 'Run Selections'!AB243)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T244=\"Select Model\", \"\", 'Run Selections'!F244)","v":""},{"$f":"IF('Run Selections'!T244=\"Select Model\", \"\", 'Run Selections'!L244)","v":""},{"$f":"IF('Run Selections'!T244=\"Select Model\", \"\", 'Run Selections'!T244)","v":""},{"$f":"IF('Run Selections'!T244=\"Select Model\", \"\", 'Run Selections'!U244)","v":""},{"$f":"IF('Run Selections'!T244=\"Select Model\", \"\", 'Run Selections'!V244)","v":""},{"$f":"IF('Run Selections'!T244=\"Select Model\", \"\", 'Run Selections'!W244)","v":""},{"$f":"IF('Run Selections'!T244=\"Select Model\", \"\", 'Run Selections'!AB244)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T245=\"Select Model\", \"\", 'Run Selections'!F245)","v":""},{"$f":"IF('Run Selections'!T245=\"Select Model\", \"\", 'Run Selections'!L245)","v":""},{"$f":"IF('Run Selections'!T245=\"Select Model\", \"\", 'Run Selections'!T245)","v":""},{"$f":"IF('Run Selections'!T245=\"Select Model\", \"\", 'Run Selections'!U245)","v":""},{"$f":"IF('Run Selections'!T245=\"Select Model\", \"\", 'Run Selections'!V245)","v":""},{"$f":"IF('Run Selections'!T245=\"Select Model\", \"\", 'Run Selections'!W245)","v":""},{"$f":"IF('Run Selections'!T245=\"Select Model\", \"\", 'Run Selections'!AB245)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T246=\"Select Model\", \"\", 'Run Selections'!F246)","v":""},{"$f":"IF('Run Selections'!T246=\"Select Model\", \"\", 'Run Selections'!L246)","v":""},{"$f":"IF('Run Selections'!T246=\"Select Model\", \"\", 'Run Selections'!T246)","v":""},{"$f":"IF('Run Selections'!T246=\"Select Model\", \"\", 'Run Selections'!U246)","v":""},{"$f":"IF('Run Selections'!T246=\"Select Model\", \"\", 'Run Selections'!V246)","v":""},{"$f":"IF('Run Selections'!T246=\"Select Model\", \"\", 'Run Selections'!W246)","v":""},{"$f":"IF('Run Selections'!T246=\"Select Model\", \"\", 'Run Selections'!AB246)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T247=\"Select Model\", \"\", 'Run Selections'!F247)","v":""},{"$f":"IF('Run Selections'!T247=\"Select Model\", \"\", 'Run Selections'!L247)","v":""},{"$f":"IF('Run Selections'!T247=\"Select Model\", \"\", 'Run Selections'!T247)","v":""},{"$f":"IF('Run Selections'!T247=\"Select Model\", \"\", 'Run Selections'!U247)","v":""},{"$f":"IF('Run Selections'!T247=\"Select Model\", \"\", 'Run Selections'!V247)","v":""},{"$f":"IF('Run Selections'!T247=\"Select Model\", \"\", 'Run Selections'!W247)","v":""},{"$f":"IF('Run Selections'!T247=\"Select Model\", \"\", 'Run Selections'!AB247)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T248=\"Select Model\", \"\", 'Run Selections'!F248)","v":""},{"$f":"IF('Run Selections'!T248=\"Select Model\", \"\", 'Run Selections'!L248)","v":""},{"$f":"IF('Run Selections'!T248=\"Select Model\", \"\", 'Run Selections'!T248)","v":""},{"$f":"IF('Run Selections'!T248=\"Select Model\", \"\", 'Run Selections'!U248)","v":""},{"$f":"IF('Run Selections'!T248=\"Select Model\", \"\", 'Run Selections'!V248)","v":""},{"$f":"IF('Run Selections'!T248=\"Select Model\", \"\", 'Run Selections'!W248)","v":""},{"$f":"IF('Run Selections'!T248=\"Select Model\", \"\", 'Run Selections'!AB248)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T249=\"Select Model\", \"\", 'Run Selections'!F249)","v":""},{"$f":"IF('Run Selections'!T249=\"Select Model\", \"\", 'Run Selections'!L249)","v":""},{"$f":"IF('Run Selections'!T249=\"Select Model\", \"\", 'Run Selections'!T249)","v":""},{"$f":"IF('Run Selections'!T249=\"Select Model\", \"\", 'Run Selections'!U249)","v":""},{"$f":"IF('Run Selections'!T249=\"Select Model\", \"\", 'Run Selections'!V249)","v":""},{"$f":"IF('Run Selections'!T249=\"Select Model\", \"\", 'Run Selections'!W249)","v":""},{"$f":"IF('Run Selections'!T249=\"Select Model\", \"\", 'Run Selections'!AB249)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T250=\"Select Model\", \"\", 'Run Selections'!F250)","v":""},{"$f":"IF('Run Selections'!T250=\"Select Model\", \"\", 'Run Selections'!L250)","v":""},{"$f":"IF('Run Selections'!T250=\"Select Model\", \"\", 'Run Selections'!T250)","v":""},{"$f":"IF('Run Selections'!T250=\"Select Model\", \"\", 'Run Selections'!U250)","v":""},{"$f":"IF('Run Selections'!T250=\"Select Model\", \"\", 'Run Selections'!V250)","v":""},{"$f":"IF('Run Selections'!T250=\"Select Model\", \"\", 'Run Selections'!W250)","v":""},{"$f":"IF('Run Selections'!T250=\"Select Model\", \"\", 'Run Selections'!AB250)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T251=\"Select Model\", \"\", 'Run Selections'!F251)","v":""},{"$f":"IF('Run Selections'!T251=\"Select Model\", \"\", 'Run Selections'!L251)","v":""},{"$f":"IF('Run Selections'!T251=\"Select Model\", \"\", 'Run Selections'!T251)","v":""},{"$f":"IF('Run Selections'!T251=\"Select Model\", \"\", 'Run Selections'!U251)","v":""},{"$f":"IF('Run Selections'!T251=\"Select Model\", \"\", 'Run Selections'!V251)","v":""},{"$f":"IF('Run Selections'!T251=\"Select Model\", \"\", 'Run Selections'!W251)","v":""},{"$f":"IF('Run Selections'!T251=\"Select Model\", \"\", 'Run Selections'!AB251)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T252=\"Select Model\", \"\", 'Run Selections'!F252)","v":""},{"$f":"IF('Run Selections'!T252=\"Select Model\", \"\", 'Run Selections'!L252)","v":""},{"$f":"IF('Run Selections'!T252=\"Select Model\", \"\", 'Run Selections'!T252)","v":""},{"$f":"IF('Run Selections'!T252=\"Select Model\", \"\", 'Run Selections'!U252)","v":""},{"$f":"IF('Run Selections'!T252=\"Select Model\", \"\", 'Run Selections'!V252)","v":""},{"$f":"IF('Run Selections'!T252=\"Select Model\", \"\", 'Run Selections'!W252)","v":""},{"$f":"IF('Run Selections'!T252=\"Select Model\", \"\", 'Run Selections'!AB252)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T253=\"Select Model\", \"\", 'Run Selections'!F253)","v":""},{"$f":"IF('Run Selections'!T253=\"Select Model\", \"\", 'Run Selections'!L253)","v":""},{"$f":"IF('Run Selections'!T253=\"Select Model\", \"\", 'Run Selections'!T253)","v":""},{"$f":"IF('Run Selections'!T253=\"Select Model\", \"\", 'Run Selections'!U253)","v":""},{"$f":"IF('Run Selections'!T253=\"Select Model\", \"\", 'Run Selections'!V253)","v":""},{"$f":"IF('Run Selections'!T253=\"Select Model\", \"\", 'Run Selections'!W253)","v":""},{"$f":"IF('Run Selections'!T253=\"Select Model\", \"\", 'Run Selections'!AB253)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T254=\"Select Model\", \"\", 'Run Selections'!F254)","v":""},{"$f":"IF('Run Selections'!T254=\"Select Model\", \"\", 'Run Selections'!L254)","v":""},{"$f":"IF('Run Selections'!T254=\"Select Model\", \"\", 'Run Selections'!T254)","v":""},{"$f":"IF('Run Selections'!T254=\"Select Model\", \"\", 'Run Selections'!U254)","v":""},{"$f":"IF('Run Selections'!T254=\"Select Model\", \"\", 'Run Selections'!V254)","v":""},{"$f":"IF('Run Selections'!T254=\"Select Model\", \"\", 'Run Selections'!W254)","v":""},{"$f":"IF('Run Selections'!T254=\"Select Model\", \"\", 'Run Selections'!AB254)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T255=\"Select Model\", \"\", 'Run Selections'!F255)","v":""},{"$f":"IF('Run Selections'!T255=\"Select Model\", \"\", 'Run Selections'!L255)","v":""},{"$f":"IF('Run Selections'!T255=\"Select Model\", \"\", 'Run Selections'!T255)","v":""},{"$f":"IF('Run Selections'!T255=\"Select Model\", \"\", 'Run Selections'!U255)","v":""},{"$f":"IF('Run Selections'!T255=\"Select Model\", \"\", 'Run Selections'!V255)","v":""},{"$f":"IF('Run Selections'!T255=\"Select Model\", \"\", 'Run Selections'!W255)","v":""},{"$f":"IF('Run Selections'!T255=\"Select Model\", \"\", 'Run Selections'!AB255)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T256=\"Select Model\", \"\", 'Run Selections'!F256)","v":""},{"$f":"IF('Run Selections'!T256=\"Select Model\", \"\", 'Run Selections'!L256)","v":""},{"$f":"IF('Run Selections'!T256=\"Select Model\", \"\", 'Run Selections'!T256)","v":""},{"$f":"IF('Run Selections'!T256=\"Select Model\", \"\", 'Run Selections'!U256)","v":""},{"$f":"IF('Run Selections'!T256=\"Select Model\", \"\", 'Run Selections'!V256)","v":""},{"$f":"IF('Run Selections'!T256=\"Select Model\", \"\", 'Run Selections'!W256)","v":""},{"$f":"IF('Run Selections'!T256=\"Select Model\", \"\", 'Run Selections'!AB256)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T257=\"Select Model\", \"\", 'Run Selections'!F257)","v":""},{"$f":"IF('Run Selections'!T257=\"Select Model\", \"\", 'Run Selections'!L257)","v":""},{"$f":"IF('Run Selections'!T257=\"Select Model\", \"\", 'Run Selections'!T257)","v":""},{"$f":"IF('Run Selections'!T257=\"Select Model\", \"\", 'Run Selections'!U257)","v":""},{"$f":"IF('Run Selections'!T257=\"Select Model\", \"\", 'Run Selections'!V257)","v":""},{"$f":"IF('Run Selections'!T257=\"Select Model\", \"\", 'Run Selections'!W257)","v":""},{"$f":"IF('Run Selections'!T257=\"Select Model\", \"\", 'Run Selections'!AB257)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T258=\"Select Model\", \"\", 'Run Selections'!F258)","v":""},{"$f":"IF('Run Selections'!T258=\"Select Model\", \"\", 'Run Selections'!L258)","v":""},{"$f":"IF('Run Selections'!T258=\"Select Model\", \"\", 'Run Selections'!T258)","v":""},{"$f":"IF('Run Selections'!T258=\"Select Model\", \"\", 'Run Selections'!U258)","v":""},{"$f":"IF('Run Selections'!T258=\"Select Model\", \"\", 'Run Selections'!V258)","v":""},{"$f":"IF('Run Selections'!T258=\"Select Model\", \"\", 'Run Selections'!W258)","v":""},{"$f":"IF('Run Selections'!T258=\"Select Model\", \"\", 'Run Selections'!AB258)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T259=\"Select Model\", \"\", 'Run Selections'!F259)","v":""},{"$f":"IF('Run Selections'!T259=\"Select Model\", \"\", 'Run Selections'!L259)","v":""},{"$f":"IF('Run Selections'!T259=\"Select Model\", \"\", 'Run Selections'!T259)","v":""},{"$f":"IF('Run Selections'!T259=\"Select Model\", \"\", 'Run Selections'!U259)","v":""},{"$f":"IF('Run Selections'!T259=\"Select Model\", \"\", 'Run Selections'!V259)","v":""},{"$f":"IF('Run Selections'!T259=\"Select Model\", \"\", 'Run Selections'!W259)","v":""},{"$f":"IF('Run Selections'!T259=\"Select Model\", \"\", 'Run Selections'!AB259)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T260=\"Select Model\", \"\", 'Run Selections'!F260)","v":""},{"$f":"IF('Run Selections'!T260=\"Select Model\", \"\", 'Run Selections'!L260)","v":""},{"$f":"IF('Run Selections'!T260=\"Select Model\", \"\", 'Run Selections'!T260)","v":""},{"$f":"IF('Run Selections'!T260=\"Select Model\", \"\", 'Run Selections'!U260)","v":""},{"$f":"IF('Run Selections'!T260=\"Select Model\", \"\", 'Run Selections'!V260)","v":""},{"$f":"IF('Run Selections'!T260=\"Select Model\", \"\", 'Run Selections'!W260)","v":""},{"$f":"IF('Run Selections'!T260=\"Select Model\", \"\", 'Run Selections'!AB260)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T261=\"Select Model\", \"\", 'Run Selections'!F261)","v":""},{"$f":"IF('Run Selections'!T261=\"Select Model\", \"\", 'Run Selections'!L261)","v":""},{"$f":"IF('Run Selections'!T261=\"Select Model\", \"\", 'Run Selections'!T261)","v":""},{"$f":"IF('Run Selections'!T261=\"Select Model\", \"\", 'Run Selections'!U261)","v":""},{"$f":"IF('Run Selections'!T261=\"Select Model\", \"\", 'Run Selections'!V261)","v":""},{"$f":"IF('Run Selections'!T261=\"Select Model\", \"\", 'Run Selections'!W261)","v":""},{"$f":"IF('Run Selections'!T261=\"Select Model\", \"\", 'Run Selections'!AB261)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T262=\"Select Model\", \"\", 'Run Selections'!F262)","v":""},{"$f":"IF('Run Selections'!T262=\"Select Model\", \"\", 'Run Selections'!L262)","v":""},{"$f":"IF('Run Selections'!T262=\"Select Model\", \"\", 'Run Selections'!T262)","v":""},{"$f":"IF('Run Selections'!T262=\"Select Model\", \"\", 'Run Selections'!U262)","v":""},{"$f":"IF('Run Selections'!T262=\"Select Model\", \"\", 'Run Selections'!V262)","v":""},{"$f":"IF('Run Selections'!T262=\"Select Model\", \"\", 'Run Selections'!W262)","v":""},{"$f":"IF('Run Selections'!T262=\"Select Model\", \"\", 'Run Selections'!AB262)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T263=\"Select Model\", \"\", 'Run Selections'!F263)","v":""},{"$f":"IF('Run Selections'!T263=\"Select Model\", \"\", 'Run Selections'!L263)","v":""},{"$f":"IF('Run Selections'!T263=\"Select Model\", \"\", 'Run Selections'!T263)","v":""},{"$f":"IF('Run Selections'!T263=\"Select Model\", \"\", 'Run Selections'!U263)","v":""},{"$f":"IF('Run Selections'!T263=\"Select Model\", \"\", 'Run Selections'!V263)","v":""},{"$f":"IF('Run Selections'!T263=\"Select Model\", \"\", 'Run Selections'!W263)","v":""},{"$f":"IF('Run Selections'!T263=\"Select Model\", \"\", 'Run Selections'!AB263)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T264=\"Select Model\", \"\", 'Run Selections'!F264)","v":""},{"$f":"IF('Run Selections'!T264=\"Select Model\", \"\", 'Run Selections'!L264)","v":""},{"$f":"IF('Run Selections'!T264=\"Select Model\", \"\", 'Run Selections'!T264)","v":""},{"$f":"IF('Run Selections'!T264=\"Select Model\", \"\", 'Run Selections'!U264)","v":""},{"$f":"IF('Run Selections'!T264=\"Select Model\", \"\", 'Run Selections'!V264)","v":""},{"$f":"IF('Run Selections'!T264=\"Select Model\", \"\", 'Run Selections'!W264)","v":""},{"$f":"IF('Run Selections'!T264=\"Select Model\", \"\", 'Run Selections'!AB264)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T265=\"Select Model\", \"\", 'Run Selections'!F265)","v":""},{"$f":"IF('Run Selections'!T265=\"Select Model\", \"\", 'Run Selections'!L265)","v":""},{"$f":"IF('Run Selections'!T265=\"Select Model\", \"\", 'Run Selections'!T265)","v":""},{"$f":"IF('Run Selections'!T265=\"Select Model\", \"\", 'Run Selections'!U265)","v":""},{"$f":"IF('Run Selections'!T265=\"Select Model\", \"\", 'Run Selections'!V265)","v":""},{"$f":"IF('Run Selections'!T265=\"Select Model\", \"\", 'Run Selections'!W265)","v":""},{"$f":"IF('Run Selections'!T265=\"Select Model\", \"\", 'Run Selections'!AB265)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T266=\"Select Model\", \"\", 'Run Selections'!F266)","v":""},{"$f":"IF('Run Selections'!T266=\"Select Model\", \"\", 'Run Selections'!L266)","v":""},{"$f":"IF('Run Selections'!T266=\"Select Model\", \"\", 'Run Selections'!T266)","v":""},{"$f":"IF('Run Selections'!T266=\"Select Model\", \"\", 'Run Selections'!U266)","v":""},{"$f":"IF('Run Selections'!T266=\"Select Model\", \"\", 'Run Selections'!V266)","v":""},{"$f":"IF('Run Selections'!T266=\"Select Model\", \"\", 'Run Selections'!W266)","v":""},{"$f":"IF('Run Selections'!T266=\"Select Model\", \"\", 'Run Selections'!AB266)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T267=\"Select Model\", \"\", 'Run Selections'!F267)","v":""},{"$f":"IF('Run Selections'!T267=\"Select Model\", \"\", 'Run Selections'!L267)","v":""},{"$f":"IF('Run Selections'!T267=\"Select Model\", \"\", 'Run Selections'!T267)","v":""},{"$f":"IF('Run Selections'!T267=\"Select Model\", \"\", 'Run Selections'!U267)","v":""},{"$f":"IF('Run Selections'!T267=\"Select Model\", \"\", 'Run Selections'!V267)","v":""},{"$f":"IF('Run Selections'!T267=\"Select Model\", \"\", 'Run Selections'!W267)","v":""},{"$f":"IF('Run Selections'!T267=\"Select Model\", \"\", 'Run Selections'!AB267)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T268=\"Select Model\", \"\", 'Run Selections'!F268)","v":""},{"$f":"IF('Run Selections'!T268=\"Select Model\", \"\", 'Run Selections'!L268)","v":""},{"$f":"IF('Run Selections'!T268=\"Select Model\", \"\", 'Run Selections'!T268)","v":""},{"$f":"IF('Run Selections'!T268=\"Select Model\", \"\", 'Run Selections'!U268)","v":""},{"$f":"IF('Run Selections'!T268=\"Select Model\", \"\", 'Run Selections'!V268)","v":""},{"$f":"IF('Run Selections'!T268=\"Select Model\", \"\", 'Run Selections'!W268)","v":""},{"$f":"IF('Run Selections'!T268=\"Select Model\", \"\", 'Run Selections'!AB268)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T269=\"Select Model\", \"\", 'Run Selections'!F269)","v":""},{"$f":"IF('Run Selections'!T269=\"Select Model\", \"\", 'Run Selections'!L269)","v":""},{"$f":"IF('Run Selections'!T269=\"Select Model\", \"\", 'Run Selections'!T269)","v":""},{"$f":"IF('Run Selections'!T269=\"Select Model\", \"\", 'Run Selections'!U269)","v":""},{"$f":"IF('Run Selections'!T269=\"Select Model\", \"\", 'Run Selections'!V269)","v":""},{"$f":"IF('Run Selections'!T269=\"Select Model\", \"\", 'Run Selections'!W269)","v":""},{"$f":"IF('Run Selections'!T269=\"Select Model\", \"\", 'Run Selections'!AB269)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T270=\"Select Model\", \"\", 'Run Selections'!F270)","v":""},{"$f":"IF('Run Selections'!T270=\"Select Model\", \"\", 'Run Selections'!L270)","v":""},{"$f":"IF('Run Selections'!T270=\"Select Model\", \"\", 'Run Selections'!T270)","v":""},{"$f":"IF('Run Selections'!T270=\"Select Model\", \"\", 'Run Selections'!U270)","v":""},{"$f":"IF('Run Selections'!T270=\"Select Model\", \"\", 'Run Selections'!V270)","v":""},{"$f":"IF('Run Selections'!T270=\"Select Model\", \"\", 'Run Selections'!W270)","v":""},{"$f":"IF('Run Selections'!T270=\"Select Model\", \"\", 'Run Selections'!AB270)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T271=\"Select Model\", \"\", 'Run Selections'!F271)","v":""},{"$f":"IF('Run Selections'!T271=\"Select Model\", \"\", 'Run Selections'!L271)","v":""},{"$f":"IF('Run Selections'!T271=\"Select Model\", \"\", 'Run Selections'!T271)","v":""},{"$f":"IF('Run Selections'!T271=\"Select Model\", \"\", 'Run Selections'!U271)","v":""},{"$f":"IF('Run Selections'!T271=\"Select Model\", \"\", 'Run Selections'!V271)","v":""},{"$f":"IF('Run Selections'!T271=\"Select Model\", \"\", 'Run Selections'!W271)","v":""},{"$f":"IF('Run Selections'!T271=\"Select Model\", \"\", 'Run Selections'!AB271)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T272=\"Select Model\", \"\", 'Run Selections'!F272)","v":""},{"$f":"IF('Run Selections'!T272=\"Select Model\", \"\", 'Run Selections'!L272)","v":""},{"$f":"IF('Run Selections'!T272=\"Select Model\", \"\", 'Run Selections'!T272)","v":""},{"$f":"IF('Run Selections'!T272=\"Select Model\", \"\", 'Run Selections'!U272)","v":""},{"$f":"IF('Run Selections'!T272=\"Select Model\", \"\", 'Run Selections'!V272)","v":""},{"$f":"IF('Run Selections'!T272=\"Select Model\", \"\", 'Run Selections'!W272)","v":""},{"$f":"IF('Run Selections'!T272=\"Select Model\", \"\", 'Run Selections'!AB272)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T273=\"Select Model\", \"\", 'Run Selections'!F273)","v":""},{"$f":"IF('Run Selections'!T273=\"Select Model\", \"\", 'Run Selections'!L273)","v":""},{"$f":"IF('Run Selections'!T273=\"Select Model\", \"\", 'Run Selections'!T273)","v":""},{"$f":"IF('Run Selections'!T273=\"Select Model\", \"\", 'Run Selections'!U273)","v":""},{"$f":"IF('Run Selections'!T273=\"Select Model\", \"\", 'Run Selections'!V273)","v":""},{"$f":"IF('Run Selections'!T273=\"Select Model\", \"\", 'Run Selections'!W273)","v":""},{"$f":"IF('Run Selections'!T273=\"Select Model\", \"\", 'Run Selections'!AB273)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T274=\"Select Model\", \"\", 'Run Selections'!F274)","v":""},{"$f":"IF('Run Selections'!T274=\"Select Model\", \"\", 'Run Selections'!L274)","v":""},{"$f":"IF('Run Selections'!T274=\"Select Model\", \"\", 'Run Selections'!T274)","v":""},{"$f":"IF('Run Selections'!T274=\"Select Model\", \"\", 'Run Selections'!U274)","v":""},{"$f":"IF('Run Selections'!T274=\"Select Model\", \"\", 'Run Selections'!V274)","v":""},{"$f":"IF('Run Selections'!T274=\"Select Model\", \"\", 'Run Selections'!W274)","v":""},{"$f":"IF('Run Selections'!T274=\"Select Model\", \"\", 'Run Selections'!AB274)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T275=\"Select Model\", \"\", 'Run Selections'!F275)","v":""},{"$f":"IF('Run Selections'!T275=\"Select Model\", \"\", 'Run Selections'!L275)","v":""},{"$f":"IF('Run Selections'!T275=\"Select Model\", \"\", 'Run Selections'!T275)","v":""},{"$f":"IF('Run Selections'!T275=\"Select Model\", \"\", 'Run Selections'!U275)","v":""},{"$f":"IF('Run Selections'!T275=\"Select Model\", \"\", 'Run Selections'!V275)","v":""},{"$f":"IF('Run Selections'!T275=\"Select Model\", \"\", 'Run Selections'!W275)","v":""},{"$f":"IF('Run Selections'!T275=\"Select Model\", \"\", 'Run Selections'!AB275)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T276=\"Select Model\", \"\", 'Run Selections'!F276)","v":""},{"$f":"IF('Run Selections'!T276=\"Select Model\", \"\", 'Run Selections'!L276)","v":""},{"$f":"IF('Run Selections'!T276=\"Select Model\", \"\", 'Run Selections'!T276)","v":""},{"$f":"IF('Run Selections'!T276=\"Select Model\", \"\", 'Run Selections'!U276)","v":""},{"$f":"IF('Run Selections'!T276=\"Select Model\", \"\", 'Run Selections'!V276)","v":""},{"$f":"IF('Run Selections'!T276=\"Select Model\", \"\", 'Run Selections'!W276)","v":""},{"$f":"IF('Run Selections'!T276=\"Select Model\", \"\", 'Run Selections'!AB276)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T277=\"Select Model\", \"\", 'Run Selections'!F277)","v":""},{"$f":"IF('Run Selections'!T277=\"Select Model\", \"\", 'Run Selections'!L277)","v":""},{"$f":"IF('Run Selections'!T277=\"Select Model\", \"\", 'Run Selections'!T277)","v":""},{"$f":"IF('Run Selections'!T277=\"Select Model\", \"\", 'Run Selections'!U277)","v":""},{"$f":"IF('Run Selections'!T277=\"Select Model\", \"\", 'Run Selections'!V277)","v":""},{"$f":"IF('Run Selections'!T277=\"Select Model\", \"\", 'Run Selections'!W277)","v":""},{"$f":"IF('Run Selections'!T277=\"Select Model\", \"\", 'Run Selections'!AB277)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T278=\"Select Model\", \"\", 'Run Selections'!F278)","v":""},{"$f":"IF('Run Selections'!T278=\"Select Model\", \"\", 'Run Selections'!L278)","v":""},{"$f":"IF('Run Selections'!T278=\"Select Model\", \"\", 'Run Selections'!T278)","v":""},{"$f":"IF('Run Selections'!T278=\"Select Model\", \"\", 'Run Selections'!U278)","v":""},{"$f":"IF('Run Selections'!T278=\"Select Model\", \"\", 'Run Selections'!V278)","v":""},{"$f":"IF('Run Selections'!T278=\"Select Model\", \"\", 'Run Selections'!W278)","v":""},{"$f":"IF('Run Selections'!T278=\"Select Model\", \"\", 'Run Selections'!AB278)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T279=\"Select Model\", \"\", 'Run Selections'!F279)","v":""},{"$f":"IF('Run Selections'!T279=\"Select Model\", \"\", 'Run Selections'!L279)","v":""},{"$f":"IF('Run Selections'!T279=\"Select Model\", \"\", 'Run Selections'!T279)","v":""},{"$f":"IF('Run Selections'!T279=\"Select Model\", \"\", 'Run Selections'!U279)","v":""},{"$f":"IF('Run Selections'!T279=\"Select Model\", \"\", 'Run Selections'!V279)","v":""},{"$f":"IF('Run Selections'!T279=\"Select Model\", \"\", 'Run Selections'!W279)","v":""},{"$f":"IF('Run Selections'!T279=\"Select Model\", \"\", 'Run Selections'!AB279)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T280=\"Select Model\", \"\", 'Run Selections'!F280)","v":""},{"$f":"IF('Run Selections'!T280=\"Select Model\", \"\", 'Run Selections'!L280)","v":""},{"$f":"IF('Run Selections'!T280=\"Select Model\", \"\", 'Run Selections'!T280)","v":""},{"$f":"IF('Run Selections'!T280=\"Select Model\", \"\", 'Run Selections'!U280)","v":""},{"$f":"IF('Run Selections'!T280=\"Select Model\", \"\", 'Run Selections'!V280)","v":""},{"$f":"IF('Run Selections'!T280=\"Select Model\", \"\", 'Run Selections'!W280)","v":""},{"$f":"IF('Run Selections'!T280=\"Select Model\", \"\", 'Run Selections'!AB280)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T281=\"Select Model\", \"\", 'Run Selections'!F281)","v":""},{"$f":"IF('Run Selections'!T281=\"Select Model\", \"\", 'Run Selections'!L281)","v":""},{"$f":"IF('Run Selections'!T281=\"Select Model\", \"\", 'Run Selections'!T281)","v":""},{"$f":"IF('Run Selections'!T281=\"Select Model\", \"\", 'Run Selections'!U281)","v":""},{"$f":"IF('Run Selections'!T281=\"Select Model\", \"\", 'Run Selections'!V281)","v":""},{"$f":"IF('Run Selections'!T281=\"Select Model\", \"\", 'Run Selections'!W281)","v":""},{"$f":"IF('Run Selections'!T281=\"Select Model\", \"\", 'Run Selections'!AB281)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T282=\"Select Model\", \"\", 'Run Selections'!F282)","v":""},{"$f":"IF('Run Selections'!T282=\"Select Model\", \"\", 'Run Selections'!L282)","v":""},{"$f":"IF('Run Selections'!T282=\"Select Model\", \"\", 'Run Selections'!T282)","v":""},{"$f":"IF('Run Selections'!T282=\"Select Model\", \"\", 'Run Selections'!U282)","v":""},{"$f":"IF('Run Selections'!T282=\"Select Model\", \"\", 'Run Selections'!V282)","v":""},{"$f":"IF('Run Selections'!T282=\"Select Model\", \"\", 'Run Selections'!W282)","v":""},{"$f":"IF('Run Selections'!T282=\"Select Model\", \"\", 'Run Selections'!AB282)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T283=\"Select Model\", \"\", 'Run Selections'!F283)","v":""},{"$f":"IF('Run Selections'!T283=\"Select Model\", \"\", 'Run Selections'!L283)","v":""},{"$f":"IF('Run Selections'!T283=\"Select Model\", \"\", 'Run Selections'!T283)","v":""},{"$f":"IF('Run Selections'!T283=\"Select Model\", \"\", 'Run Selections'!U283)","v":""},{"$f":"IF('Run Selections'!T283=\"Select Model\", \"\", 'Run Selections'!V283)","v":""},{"$f":"IF('Run Selections'!T283=\"Select Model\", \"\", 'Run Selections'!W283)","v":""},{"$f":"IF('Run Selections'!T283=\"Select Model\", \"\", 'Run Selections'!AB283)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T284=\"Select Model\", \"\", 'Run Selections'!F284)","v":""},{"$f":"IF('Run Selections'!T284=\"Select Model\", \"\", 'Run Selections'!L284)","v":""},{"$f":"IF('Run Selections'!T284=\"Select Model\", \"\", 'Run Selections'!T284)","v":""},{"$f":"IF('Run Selections'!T284=\"Select Model\", \"\", 'Run Selections'!U284)","v":""},{"$f":"IF('Run Selections'!T284=\"Select Model\", \"\", 'Run Selections'!V284)","v":""},{"$f":"IF('Run Selections'!T284=\"Select Model\", \"\", 'Run Selections'!W284)","v":""},{"$f":"IF('Run Selections'!T284=\"Select Model\", \"\", 'Run Selections'!AB284)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T285=\"Select Model\", \"\", 'Run Selections'!F285)","v":""},{"$f":"IF('Run Selections'!T285=\"Select Model\", \"\", 'Run Selections'!L285)","v":""},{"$f":"IF('Run Selections'!T285=\"Select Model\", \"\", 'Run Selections'!T285)","v":""},{"$f":"IF('Run Selections'!T285=\"Select Model\", \"\", 'Run Selections'!U285)","v":""},{"$f":"IF('Run Selections'!T285=\"Select Model\", \"\", 'Run Selections'!V285)","v":""},{"$f":"IF('Run Selections'!T285=\"Select Model\", \"\", 'Run Selections'!W285)","v":""},{"$f":"IF('Run Selections'!T285=\"Select Model\", \"\", 'Run Selections'!AB285)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T286=\"Select Model\", \"\", 'Run Selections'!F286)","v":""},{"$f":"IF('Run Selections'!T286=\"Select Model\", \"\", 'Run Selections'!L286)","v":""},{"$f":"IF('Run Selections'!T286=\"Select Model\", \"\", 'Run Selections'!T286)","v":""},{"$f":"IF('Run Selections'!T286=\"Select Model\", \"\", 'Run Selections'!U286)","v":""},{"$f":"IF('Run Selections'!T286=\"Select Model\", \"\", 'Run Selections'!V286)","v":""},{"$f":"IF('Run Selections'!T286=\"Select Model\", \"\", 'Run Selections'!W286)","v":""},{"$f":"IF('Run Selections'!T286=\"Select Model\", \"\", 'Run Selections'!AB286)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T287=\"Select Model\", \"\", 'Run Selections'!F287)","v":""},{"$f":"IF('Run Selections'!T287=\"Select Model\", \"\", 'Run Selections'!L287)","v":""},{"$f":"IF('Run Selections'!T287=\"Select Model\", \"\", 'Run Selections'!T287)","v":""},{"$f":"IF('Run Selections'!T287=\"Select Model\", \"\", 'Run Selections'!U287)","v":""},{"$f":"IF('Run Selections'!T287=\"Select Model\", \"\", 'Run Selections'!V287)","v":""},{"$f":"IF('Run Selections'!T287=\"Select Model\", \"\", 'Run Selections'!W287)","v":""},{"$f":"IF('Run Selections'!T287=\"Select Model\", \"\", 'Run Selections'!AB287)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T288=\"Select Model\", \"\", 'Run Selections'!F288)","v":""},{"$f":"IF('Run Selections'!T288=\"Select Model\", \"\", 'Run Selections'!L288)","v":""},{"$f":"IF('Run Selections'!T288=\"Select Model\", \"\", 'Run Selections'!T288)","v":""},{"$f":"IF('Run Selections'!T288=\"Select Model\", \"\", 'Run Selections'!U288)","v":""},{"$f":"IF('Run Selections'!T288=\"Select Model\", \"\", 'Run Selections'!V288)","v":""},{"$f":"IF('Run Selections'!T288=\"Select Model\", \"\", 'Run Selections'!W288)","v":""},{"$f":"IF('Run Selections'!T288=\"Select Model\", \"\", 'Run Selections'!AB288)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T289=\"Select Model\", \"\", 'Run Selections'!F289)","v":""},{"$f":"IF('Run Selections'!T289=\"Select Model\", \"\", 'Run Selections'!L289)","v":""},{"$f":"IF('Run Selections'!T289=\"Select Model\", \"\", 'Run Selections'!T289)","v":""},{"$f":"IF('Run Selections'!T289=\"Select Model\", \"\", 'Run Selections'!U289)","v":""},{"$f":"IF('Run Selections'!T289=\"Select Model\", \"\", 'Run Selections'!V289)","v":""},{"$f":"IF('Run Selections'!T289=\"Select Model\", \"\", 'Run Selections'!W289)","v":""},{"$f":"IF('Run Selections'!T289=\"Select Model\", \"\", 'Run Selections'!AB289)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T290=\"Select Model\", \"\", 'Run Selections'!F290)","v":""},{"$f":"IF('Run Selections'!T290=\"Select Model\", \"\", 'Run Selections'!L290)","v":""},{"$f":"IF('Run Selections'!T290=\"Select Model\", \"\", 'Run Selections'!T290)","v":""},{"$f":"IF('Run Selections'!T290=\"Select Model\", \"\", 'Run Selections'!U290)","v":""},{"$f":"IF('Run Selections'!T290=\"Select Model\", \"\", 'Run Selections'!V290)","v":""},{"$f":"IF('Run Selections'!T290=\"Select Model\", \"\", 'Run Selections'!W290)","v":""},{"$f":"IF('Run Selections'!T290=\"Select Model\", \"\", 'Run Selections'!AB290)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T291=\"Select Model\", \"\", 'Run Selections'!F291)","v":""},{"$f":"IF('Run Selections'!T291=\"Select Model\", \"\", 'Run Selections'!L291)","v":""},{"$f":"IF('Run Selections'!T291=\"Select Model\", \"\", 'Run Selections'!T291)","v":""},{"$f":"IF('Run Selections'!T291=\"Select Model\", \"\", 'Run Selections'!U291)","v":""},{"$f":"IF('Run Selections'!T291=\"Select Model\", \"\", 'Run Selections'!V291)","v":""},{"$f":"IF('Run Selections'!T291=\"Select Model\", \"\", 'Run Selections'!W291)","v":""},{"$f":"IF('Run Selections'!T291=\"Select Model\", \"\", 'Run Selections'!AB291)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T292=\"Select Model\", \"\", 'Run Selections'!F292)","v":""},{"$f":"IF('Run Selections'!T292=\"Select Model\", \"\", 'Run Selections'!L292)","v":""},{"$f":"IF('Run Selections'!T292=\"Select Model\", \"\", 'Run Selections'!T292)","v":""},{"$f":"IF('Run Selections'!T292=\"Select Model\", \"\", 'Run Selections'!U292)","v":""},{"$f":"IF('Run Selections'!T292=\"Select Model\", \"\", 'Run Selections'!V292)","v":""},{"$f":"IF('Run Selections'!T292=\"Select Model\", \"\", 'Run Selections'!W292)","v":""},{"$f":"IF('Run Selections'!T292=\"Select Model\", \"\", 'Run Selections'!AB292)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T293=\"Select Model\", \"\", 'Run Selections'!F293)","v":""},{"$f":"IF('Run Selections'!T293=\"Select Model\", \"\", 'Run Selections'!L293)","v":""},{"$f":"IF('Run Selections'!T293=\"Select Model\", \"\", 'Run Selections'!T293)","v":""},{"$f":"IF('Run Selections'!T293=\"Select Model\", \"\", 'Run Selections'!U293)","v":""},{"$f":"IF('Run Selections'!T293=\"Select Model\", \"\", 'Run Selections'!V293)","v":""},{"$f":"IF('Run Selections'!T293=\"Select Model\", \"\", 'Run Selections'!W293)","v":""},{"$f":"IF('Run Selections'!T293=\"Select Model\", \"\", 'Run Selections'!AB293)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T294=\"Select Model\", \"\", 'Run Selections'!F294)","v":""},{"$f":"IF('Run Selections'!T294=\"Select Model\", \"\", 'Run Selections'!L294)","v":""},{"$f":"IF('Run Selections'!T294=\"Select Model\", \"\", 'Run Selections'!T294)","v":""},{"$f":"IF('Run Selections'!T294=\"Select Model\", \"\", 'Run Selections'!U294)","v":""},{"$f":"IF('Run Selections'!T294=\"Select Model\", \"\", 'Run Selections'!V294)","v":""},{"$f":"IF('Run Selections'!T294=\"Select Model\", \"\", 'Run Selections'!W294)","v":""},{"$f":"IF('Run Selections'!T294=\"Select Model\", \"\", 'Run Selections'!AB294)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T295=\"Select Model\", \"\", 'Run Selections'!F295)","v":""},{"$f":"IF('Run Selections'!T295=\"Select Model\", \"\", 'Run Selections'!L295)","v":""},{"$f":"IF('Run Selections'!T295=\"Select Model\", \"\", 'Run Selections'!T295)","v":""},{"$f":"IF('Run Selections'!T295=\"Select Model\", \"\", 'Run Selections'!U295)","v":""},{"$f":"IF('Run Selections'!T295=\"Select Model\", \"\", 'Run Selections'!V295)","v":""},{"$f":"IF('Run Selections'!T295=\"Select Model\", \"\", 'Run Selections'!W295)","v":""},{"$f":"IF('Run Selections'!T295=\"Select Model\", \"\", 'Run Selections'!AB295)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T296=\"Select Model\", \"\", 'Run Selections'!F296)","v":""},{"$f":"IF('Run Selections'!T296=\"Select Model\", \"\", 'Run Selections'!L296)","v":""},{"$f":"IF('Run Selections'!T296=\"Select Model\", \"\", 'Run Selections'!T296)","v":""},{"$f":"IF('Run Selections'!T296=\"Select Model\", \"\", 'Run Selections'!U296)","v":""},{"$f":"IF('Run Selections'!T296=\"Select Model\", \"\", 'Run Selections'!V296)","v":""},{"$f":"IF('Run Selections'!T296=\"Select Model\", \"\", 'Run Selections'!W296)","v":""},{"$f":"IF('Run Selections'!T296=\"Select Model\", \"\", 'Run Selections'!AB296)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T297=\"Select Model\", \"\", 'Run Selections'!F297)","v":""},{"$f":"IF('Run Selections'!T297=\"Select Model\", \"\", 'Run Selections'!L297)","v":""},{"$f":"IF('Run Selections'!T297=\"Select Model\", \"\", 'Run Selections'!T297)","v":""},{"$f":"IF('Run Selections'!T297=\"Select Model\", \"\", 'Run Selections'!U297)","v":""},{"$f":"IF('Run Selections'!T297=\"Select Model\", \"\", 'Run Selections'!V297)","v":""},{"$f":"IF('Run Selections'!T297=\"Select Model\", \"\", 'Run Selections'!W297)","v":""},{"$f":"IF('Run Selections'!T297=\"Select Model\", \"\", 'Run Selections'!AB297)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T298=\"Select Model\", \"\", 'Run Selections'!F298)","v":""},{"$f":"IF('Run Selections'!T298=\"Select Model\", \"\", 'Run Selections'!L298)","v":""},{"$f":"IF('Run Selections'!T298=\"Select Model\", \"\", 'Run Selections'!T298)","v":""},{"$f":"IF('Run Selections'!T298=\"Select Model\", \"\", 'Run Selections'!U298)","v":""},{"$f":"IF('Run Selections'!T298=\"Select Model\", \"\", 'Run Selections'!V298)","v":""},{"$f":"IF('Run Selections'!T298=\"Select Model\", \"\", 'Run Selections'!W298)","v":""},{"$f":"IF('Run Selections'!T298=\"Select Model\", \"\", 'Run Selections'!AB298)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T299=\"Select Model\", \"\", 'Run Selections'!F299)","v":""},{"$f":"IF('Run Selections'!T299=\"Select Model\", \"\", 'Run Selections'!L299)","v":""},{"$f":"IF('Run Selections'!T299=\"Select Model\", \"\", 'Run Selections'!T299)","v":""},{"$f":"IF('Run Selections'!T299=\"Select Model\", \"\", 'Run Selections'!U299)","v":""},{"$f":"IF('Run Selections'!T299=\"Select Model\", \"\", 'Run Selections'!V299)","v":""},{"$f":"IF('Run Selections'!T299=\"Select Model\", \"\", 'Run Selections'!W299)","v":""},{"$f":"IF('Run Selections'!T299=\"Select Model\", \"\", 'Run Selections'!AB299)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T300=\"Select Model\", \"\", 'Run Selections'!F300)","v":""},{"$f":"IF('Run Selections'!T300=\"Select Model\", \"\", 'Run Selections'!L300)","v":""},{"$f":"IF('Run Selections'!T300=\"Select Model\", \"\", 'Run Selections'!T300)","v":""},{"$f":"IF('Run Selections'!T300=\"Select Model\", \"\", 'Run Selections'!U300)","v":""},{"$f":"IF('Run Selections'!T300=\"Select Model\", \"\", 'Run Selections'!V300)","v":""},{"$f":"IF('Run Selections'!T300=\"Select Model\", \"\", 'Run Selections'!W300)","v":""},{"$f":"IF('Run Selections'!T300=\"Select Model\", \"\", 'Run Selections'!AB300)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T301=\"Select Model\", \"\", 'Run Selections'!F301)","v":""},{"$f":"IF('Run Selections'!T301=\"Select Model\", \"\", 'Run Selections'!L301)","v":""},{"$f":"IF('Run Selections'!T301=\"Select Model\", \"\", 'Run Selections'!T301)","v":""},{"$f":"IF('Run Selections'!T301=\"Select Model\", \"\", 'Run Selections'!U301)","v":""},{"$f":"IF('Run Selections'!T301=\"Select Model\", \"\", 'Run Selections'!V301)","v":""},{"$f":"IF('Run Selections'!T301=\"Select Model\", \"\", 'Run Selections'!W301)","v":""},{"$f":"IF('Run Selections'!T301=\"Select Model\", \"\", 'Run Selections'!AB301)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T302=\"Select Model\", \"\", 'Run Selections'!F302)","v":""},{"$f":"IF('Run Selections'!T302=\"Select Model\", \"\", 'Run Selections'!L302)","v":""},{"$f":"IF('Run Selections'!T302=\"Select Model\", \"\", 'Run Selections'!T302)","v":""},{"$f":"IF('Run Selections'!T302=\"Select Model\", \"\", 'Run Selections'!U302)","v":""},{"$f":"IF('Run Selections'!T302=\"Select Model\", \"\", 'Run Selections'!V302)","v":""},{"$f":"IF('Run Selections'!T302=\"Select Model\", \"\", 'Run Selections'!W302)","v":""},{"$f":"IF('Run Selections'!T302=\"Select Model\", \"\", 'Run Selections'!AB302)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T303=\"Select Model\", \"\", 'Run Selections'!F303)","v":""},{"$f":"IF('Run Selections'!T303=\"Select Model\", \"\", 'Run Selections'!L303)","v":""},{"$f":"IF('Run Selections'!T303=\"Select Model\", \"\", 'Run Selections'!T303)","v":""},{"$f":"IF('Run Selections'!T303=\"Select Model\", \"\", 'Run Selections'!U303)","v":""},{"$f":"IF('Run Selections'!T303=\"Select Model\", \"\", 'Run Selections'!V303)","v":""},{"$f":"IF('Run Selections'!T303=\"Select Model\", \"\", 'Run Selections'!W303)","v":""},{"$f":"IF('Run Selections'!T303=\"Select Model\", \"\", 'Run Selections'!AB303)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T304=\"Select Model\", \"\", 'Run Selections'!F304)","v":""},{"$f":"IF('Run Selections'!T304=\"Select Model\", \"\", 'Run Selections'!L304)","v":""},{"$f":"IF('Run Selections'!T304=\"Select Model\", \"\", 'Run Selections'!T304)","v":""},{"$f":"IF('Run Selections'!T304=\"Select Model\", \"\", 'Run Selections'!U304)","v":""},{"$f":"IF('Run Selections'!T304=\"Select Model\", \"\", 'Run Selections'!V304)","v":""},{"$f":"IF('Run Selections'!T304=\"Select Model\", \"\", 'Run Selections'!W304)","v":""},{"$f":"IF('Run Selections'!T304=\"Select Model\", \"\", 'Run Selections'!AB304)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T305=\"Select Model\", \"\", 'Run Selections'!F305)","v":""},{"$f":"IF('Run Selections'!T305=\"Select Model\", \"\", 'Run Selections'!L305)","v":""},{"$f":"IF('Run Selections'!T305=\"Select Model\", \"\", 'Run Selections'!T305)","v":""},{"$f":"IF('Run Selections'!T305=\"Select Model\", \"\", 'Run Selections'!U305)","v":""},{"$f":"IF('Run Selections'!T305=\"Select Model\", \"\", 'Run Selections'!V305)","v":""},{"$f":"IF('Run Selections'!T305=\"Select Model\", \"\", 'Run Selections'!W305)","v":""},{"$f":"IF('Run Selections'!T305=\"Select Model\", \"\", 'Run Selections'!AB305)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T306=\"Select Model\", \"\", 'Run Selections'!F306)","v":""},{"$f":"IF('Run Selections'!T306=\"Select Model\", \"\", 'Run Selections'!L306)","v":""},{"$f":"IF('Run Selections'!T306=\"Select Model\", \"\", 'Run Selections'!T306)","v":""},{"$f":"IF('Run Selections'!T306=\"Select Model\", \"\", 'Run Selections'!U306)","v":""},{"$f":"IF('Run Selections'!T306=\"Select Model\", \"\", 'Run Selections'!V306)","v":""},{"$f":"IF('Run Selections'!T306=\"Select Model\", \"\", 'Run Selections'!W306)","v":""},{"$f":"IF('Run Selections'!T306=\"Select Model\", \"\", 'Run Selections'!AB306)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T307=\"Select Model\", \"\", 'Run Selections'!F307)","v":""},{"$f":"IF('Run Selections'!T307=\"Select Model\", \"\", 'Run Selections'!L307)","v":""},{"$f":"IF('Run Selections'!T307=\"Select Model\", \"\", 'Run Selections'!T307)","v":""},{"$f":"IF('Run Selections'!T307=\"Select Model\", \"\", 'Run Selections'!U307)","v":""},{"$f":"IF('Run Selections'!T307=\"Select Model\", \"\", 'Run Selections'!V307)","v":""},{"$f":"IF('Run Selections'!T307=\"Select Model\", \"\", 'Run Selections'!W307)","v":""},{"$f":"IF('Run Selections'!T307=\"Select Model\", \"\", 'Run Selections'!AB307)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T308=\"Select Model\", \"\", 'Run Selections'!F308)","v":""},{"$f":"IF('Run Selections'!T308=\"Select Model\", \"\", 'Run Selections'!L308)","v":""},{"$f":"IF('Run Selections'!T308=\"Select Model\", \"\", 'Run Selections'!T308)","v":""},{"$f":"IF('Run Selections'!T308=\"Select Model\", \"\", 'Run Selections'!U308)","v":""},{"$f":"IF('Run Selections'!T308=\"Select Model\", \"\", 'Run Selections'!V308)","v":""},{"$f":"IF('Run Selections'!T308=\"Select Model\", \"\", 'Run Selections'!W308)","v":""},{"$f":"IF('Run Selections'!T308=\"Select Model\", \"\", 'Run Selections'!AB308)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T309=\"Select Model\", \"\", 'Run Selections'!F309)","v":""},{"$f":"IF('Run Selections'!T309=\"Select Model\", \"\", 'Run Selections'!L309)","v":""},{"$f":"IF('Run Selections'!T309=\"Select Model\", \"\", 'Run Selections'!T309)","v":""},{"$f":"IF('Run Selections'!T309=\"Select Model\", \"\", 'Run Selections'!U309)","v":""},{"$f":"IF('Run Selections'!T309=\"Select Model\", \"\", 'Run Selections'!V309)","v":""},{"$f":"IF('Run Selections'!T309=\"Select Model\", \"\", 'Run Selections'!W309)","v":""},{"$f":"IF('Run Selections'!T309=\"Select Model\", \"\", 'Run Selections'!AB309)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T310=\"Select Model\", \"\", 'Run Selections'!F310)","v":""},{"$f":"IF('Run Selections'!T310=\"Select Model\", \"\", 'Run Selections'!L310)","v":""},{"$f":"IF('Run Selections'!T310=\"Select Model\", \"\", 'Run Selections'!T310)","v":""},{"$f":"IF('Run Selections'!T310=\"Select Model\", \"\", 'Run Selections'!U310)","v":""},{"$f":"IF('Run Selections'!T310=\"Select Model\", \"\", 'Run Selections'!V310)","v":""},{"$f":"IF('Run Selections'!T310=\"Select Model\", \"\", 'Run Selections'!W310)","v":""},{"$f":"IF('Run Selections'!T310=\"Select Model\", \"\", 'Run Selections'!AB310)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T311=\"Select Model\", \"\", 'Run Selections'!F311)","v":""},{"$f":"IF('Run Selections'!T311=\"Select Model\", \"\", 'Run Selections'!L311)","v":""},{"$f":"IF('Run Selections'!T311=\"Select Model\", \"\", 'Run Selections'!T311)","v":""},{"$f":"IF('Run Selections'!T311=\"Select Model\", \"\", 'Run Selections'!U311)","v":""},{"$f":"IF('Run Selections'!T311=\"Select Model\", \"\", 'Run Selections'!V311)","v":""},{"$f":"IF('Run Selections'!T311=\"Select Model\", \"\", 'Run Selections'!W311)","v":""},{"$f":"IF('Run Selections'!T311=\"Select Model\", \"\", 'Run Selections'!AB311)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T312=\"Select Model\", \"\", 'Run Selections'!F312)","v":""},{"$f":"IF('Run Selections'!T312=\"Select Model\", \"\", 'Run Selections'!L312)","v":""},{"$f":"IF('Run Selections'!T312=\"Select Model\", \"\", 'Run Selections'!T312)","v":""},{"$f":"IF('Run Selections'!T312=\"Select Model\", \"\", 'Run Selections'!U312)","v":""},{"$f":"IF('Run Selections'!T312=\"Select Model\", \"\", 'Run Selections'!V312)","v":""},{"$f":"IF('Run Selections'!T312=\"Select Model\", \"\", 'Run Selections'!W312)","v":""},{"$f":"IF('Run Selections'!T312=\"Select Model\", \"\", 'Run Selections'!AB312)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T313=\"Select Model\", \"\", 'Run Selections'!F313)","v":""},{"$f":"IF('Run Selections'!T313=\"Select Model\", \"\", 'Run Selections'!L313)","v":""},{"$f":"IF('Run Selections'!T313=\"Select Model\", \"\", 'Run Selections'!T313)","v":""},{"$f":"IF('Run Selections'!T313=\"Select Model\", \"\", 'Run Selections'!U313)","v":""},{"$f":"IF('Run Selections'!T313=\"Select Model\", \"\", 'Run Selections'!V313)","v":""},{"$f":"IF('Run Selections'!T313=\"Select Model\", \"\", 'Run Selections'!W313)","v":""},{"$f":"IF('Run Selections'!T313=\"Select Model\", \"\", 'Run Selections'!AB313)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T314=\"Select Model\", \"\", 'Run Selections'!F314)","v":""},{"$f":"IF('Run Selections'!T314=\"Select Model\", \"\", 'Run Selections'!L314)","v":""},{"$f":"IF('Run Selections'!T314=\"Select Model\", \"\", 'Run Selections'!T314)","v":""},{"$f":"IF('Run Selections'!T314=\"Select Model\", \"\", 'Run Selections'!U314)","v":""},{"$f":"IF('Run Selections'!T314=\"Select Model\", \"\", 'Run Selections'!V314)","v":""},{"$f":"IF('Run Selections'!T314=\"Select Model\", \"\", 'Run Selections'!W314)","v":""},{"$f":"IF('Run Selections'!T314=\"Select Model\", \"\", 'Run Selections'!AB314)","v":""}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF('Run Selections'!T315=\"Select Model\", \"\", 'Run Selections'!T315)","v":""},{"$f":"IF('Run Selections'!T315=\"Select Model\", \"\", 'Run Selections'!U315)","v":""},{"$f":"IF('Run Selections'!T315=\"Select Model\", \"\", 'Run Selections'!V315)","v":""},{"$f":"IF('Run Selections'!T315=\"Select Model\", \"\", 'Run Selections'!W315)","v":""},{"$f":"IF('Run Selections'!T315=\"Select Model\", \"\", 'Run Selections'!AB315)","v":""}]

{"sheet":"Building Summary","index":3,"n_rows":18,"n_cols":12,"rows_kept":18,"cut":false,"hidden":false,"merged":[[17,0,17,1],[21,0,21,1],[18,0,18,1],[20,0,20,1],[19,0,19,1],[0,4,1,7],[3,0,3,1],[3,3,3,4],[2,0,2,2],[2,3,2,5],[2,6,2,9]]}
[null,null,null,null,"Chilled Beam System Design Summary"]
[]
["Room Setpoints",null,null,"Primary Air Conditions",null,null,"Water Conditions",null,null,null,"Altitude"]
["Cooling",null,"Heating","Cooling",null,"Heating","Cooling Temp.","Additive","Heating Temp.","Additive",{"$f":"activeElevation","v":0}]
[{"$f":"activeRoomTempCooling","v":75},{"$f":"activeRHCooling/100","v":0.5},{"$f":"activeRoomTempHeating","v":72},{"$f":"activePriAirTempCooling","v":55},{"$f":"activePriAirRHCooling/100","v":0.8},{"$f":"activePriAirTempHeating","v":55},{"$f":"activeEWTCooling","v":57},{"$f":"activeFluidTypeCooling","v":"Water"},{"$f":"activeEWTHeating","v":120},{"$f":"activeFluidTypeHeating","v":"Water"},"ft"]
[]
["Motor Efficiency",0.8,null,null,null,null,null,null,null,"Primary Air",{"$f":"'Run Selections'!L3","v":0}]
["Pump Efficiency ",0.9,null,null,null,"Invalid Series ID",null,null,null,"Primay per sq footage",{"$f":"IFERROR(K7/B15,\"-\")","v":"-"}]
["Fan Efficiency",0.65,null,null,null,null,null,null,null,"Total Space Air Movement",{"$f":"SUMPRODUCT('Run Selections'!AL15:AL315,'Run Selections'!L15:L315)","v":0}]
["Upstream Water Pressure Drop \n(ft W.G.)",100,null,null,null,null,null,null,null,"Chilled Water",{"$f":"'Run Selections'!L4","v":0}]
["Upstream Air Pressure Drop\n(in W.G.)",0.46,null,null,null,null,null,null,null,"Hot Water",{"$f":"'Run Selections'!L5","v":0}]
["Peak Pump Power",{"$f":"((SUM('Run Selections'!$H$15:$H$315)/(500)/(activeMaxWaterPressureDrop)*(B10*1.3*(4/100)))/(3960)/($B$8)/($B$7))","v":0},null,null,null,null,null,null,null,"Airside Cooling",0]
["Peak Fan Power",{"$f":"(SUM('Run Selections'!$H$15:$H$315)/(1.085)/(25))*($B$11)/(6346)/($B$9)/($B$7)","v":0},null,null,null,null,null,null,null,"Waterside Cooling",0,"Airside Cooling"]
["Number of Zones",{"$f":"IF(COUNTA('Run Selections'!$F15:$F315)=0,\"-\",COUNTA('Run Selections'!$F15:$F315))","v":"-"},null,null,null,null,null,null,null,"Total Sensible Cooling",{"$f":"K12+K13","v":0},"Waterside Cooling"]
["Total Area",{"$f":"IFERROR(SUM('Run Selections'!$G$15:$G$315),\"\")","v":0},null,null,null,null,null,null,null,"Total Sensible Cooling per square foot",{"$f":"IFERROR(K14/B15,\"-\")","v":"-"}]
["Beam Quantity",{"$f":"IF('Run Selections'!$O$3=0,\"-\",'Run Selections'!$O$3)","v":"-"},null,null,null,null,null,null,null,"Total Heating",{"$f":"ABS(SUM('Run Selections'!O15:O315))","v":0}]
["Total Beam Length",{"$f":"'Run Selections'!$O$4","v":0},null,null,null,null,null,null,null,"Total Sensible Heating per square foot",{"$f":"IFERROR(K16/B15,\"-\")","v":"-"}]
[null,null,null,null,null,null,null,null,null,"Total Latent Cooling",{"$f":"ABS(SUM('Run Selections'!N15:N315))","v":0}]

{"sheet":"Notes","index":4,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[]}
["Chilled Beam Selection Software Notes",null,null,"Nozzle Size Order"]
["NOTE: Refer to online application and selection guides before making and finalizing selections. Contact Sustainable@priceindustries.com with any questions."]
[null,null,null,"ACBL24 / LIU"]
["General:",null,null,10,"309"]
["1. Make sure to \"Enable Macros\" or Click \"Yes\" when Asked to \"Enable Content\"",null,null,20,"416"]
["2. Green cells are inputs",null,null,30,"412"]
["3. White cells are outputs. White cells cannot be changed.",null,null,35,"406"]
["4. Values that turn blue are manual inputs",null,null,40,"510"]
["5. Cells that turn Red or Orange should be taken as warnings per notes below.",null,null,50,"506"]
["6. Generally, input Page and Green Input cells do not provide any selections. Only the main performance page and white cells  provides selection feedback.",null,null,60,"607"]
[null,null,null,70,"604"]
["Global Conditions:",null,null,80,"601"]
["1. Adjust Space Dew Point / Wet Bulb by changing the RH%"]
["2. If certain white cells are Orange in the Room / Primary conditions, space may not be receiving dehumidification or the supply air is more humid than space set point.",null,null,"ACBL12"]
["3. If Entering Water Temp for cooling is RED, the water temperature is below the Room Dew Point. This means condensation may form at the water coil during operation.",null,null,20,"101"]
["4. Primary Air temperature will not turn red, but it should be noted that supplying air colder than the space dew point may cause condensation to form on the chilled beam's sheet metal plenum. This is true for other HVAC products as well.",null,null,30,"201"]
["5. Stratification credit may be applied to ACBC_1W only",null,null,40,"301"]
[null,null,null,50,"405"]
["Selections:",null,null,60,"401"]
["1. Typical recommended Chilled Beam Static Pressure operating Ranges = 0.2 - 0.8 in. wg",null,null,70,"501"]
["2. Primary Airflow (CFM) for linear beams (per beam) - Typically up to 25 CFM / ft for 2 Way Discharge and 15 CFM for 1 Way Discharge",null,null,80,"601"]
["3. Water Flow Rate (GPM) (per beam) - select between 0.5 to 2.5 GPM with pressure drops in the 0-10 ft wg range.",null,"50Rmoo"]
["4. PCBL Selections need to be done manually. Autoselect will not work with this model.",null,null,"ACBR"]
["5. If Sound Level, Air Static Pressure, and Water Pressure Drop cells are Red or Orange, check the Global Condition max inputs.",null,null,10,"406"]
["6. Nozzles are selected automatically based on \"target pressure\". If necessary, Nozzles can be changed by adjusting the \"Target Pressure\" column before \"Exact Pressure\". Nozzle size order starting from smallest to largest noted on the right.",null,null,20,"506"]
["7. To check VAV operation of a chilled beam, select \"VAV\" in the Zone / Room Selection Options to the left of Model Select. This will lock the nozzle size. VAV should be changed back to Default if the nozzle needs to be changed.",null,null,30,"608"]
["8. Standard Inlet velocity / duct sizing practices should be kept in mind when selecting Airflows through inlet sizes of the chilled beams (recommended limit approx. 750 FPM, 1000 FPM max). ",null,null,40,"605"]
["9. Model ACBR capacity is based on NO DERATE. Certain Grille / Diffuser selections (by others) may cause a derate.",null,null,50,"603"]
["10. Discharge Air Temps for Heating recommended to be within 20F dT of Room Set point in heating to mitigate stratification.",null,null,60,"601"]
["11. In \"Throw Data\", 50 FPM terminal velocity is generally the the recommended limit for throw selections in a zone."]
["12. Total Sensible Capacity is the combined capacity of Air and Water Coil capacities. Latent Capacity is not included.",null,null,"ACBM"]
["13. Typical selections should be selected below 35 NC per beam.",null,null,20,"101"]
[null,null,null,30,"201"]
[null,null,null,40,"301"]
[null,null,null,50,"401"]
[null,null,null,60,"501"]
[null,null,null,70,"601"]
[]
[null,null,null,"ACBC"]
[null,null,null,50,405]
[null,null,null,70,504]

{"sheet":"Active Throw","index":5,"n_rows":315,"n_cols":21,"rows_kept":315,"cut":false,"hidden":true,"merged":[[9,19,9,20],[10,19,11,19],[10,20,11,20],[10,15,11,15],[10,16,11,16],[10,17,11,17],[9,16,9,17],[9,12,9,15],[10,14,11,14],[10,12,11,12],[10,13,11,13],[9,10,10,10],[9,1,12,1],[2,1,3,1],[9,3,12,3],[9,4,11,4],[10,7,11,7],[9,5,9,7],[10,5,11,5],[10,6,12,6],[9,9,11,9]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Room or Zone Number/Name",null,"Beam Model","Length","Primary Air",null,null,null,"Total Discharge","Throw",null,"Room Dimensions",null,null,null,"Terminal Velocities",null,"Nozzle Size","Adjacent Zone"]
[null,null,null,null,null,"Flow","Nozzle Code","Exact Pressure",null,null,null,null,"Room Height","Occupied Zone Height","Dist To Wall","Dist Between Beams","Velocity At Wall","Velocity Between Beams",null,"Zone for 60 FPM","Zone for 40 FPM"]
[null,null,null,null,null,null,null,null,null,null,"150-100-50"]
[null,null,null,null,"ft (nom)","CFM",null,"in WG",null,"CFM","ft",null,"H (ft)","HC (ft)","CW (ft)","CB (ft)","FPM","FPM",null,"ft","ft"]
[]
[null,{"$f":"IF(TRIM('Run Selections'!F15)=\"\",\"\",'Run Selections'!F15)","v":""},null,{"$f":"'Run Selections'!T15","v":"Select Model"},{"$f":"'Run Selections'!W15","v":4},{"$f":"'Run Selections'!Y15","v":50},{"$f":"'Run Selections'!AI15","v":""},{"$f":"'Run Selections'!AA15","v":0},null,{"$f":"'Run Selections'!AL15","v":""},{"$f":"IF(D15=\"Select Model\",\"N/A\",throwCombined(F15, D15, S15, E15,J15))","v":"N/A"},null,10,3.5,5,8,{"$f":"IF(D15=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K15, M15, N15, O15),0))","v":"N/A"},{"$f":"IF(D15=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K15,M15,N15,P15)),0))","v":"N/A"},{"$f":"'Run Selections'!BD15","v":0},{"$f":"IF(LEFT($D15,4)<>\"ACBC\",\"N/A\",AdjacentZone($D15,$E15,$S15,$F15,60))","v":"N/A"},{"$f":"IF(LEFT($D15,4)<>\"ACBC\",\"N/A\",AdjacentZone($D15,$E15,$S15,$F15,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F16)=\"\",\"\",'Run Selections'!F16)","v":""},null,{"$f":"'Run Selections'!T16","v":"Select Model"},{"$f":"'Run Selections'!W16","v":4},{"$f":"'Run Selections'!Y16","v":50},{"$f":"'Run Selections'!AI16","v":""},{"$f":"'Run Selections'!AA16","v":0},null,{"$f":"'Run Selections'!AL16","v":""},{"$f":"IF(D16=\"Select Model\",\"N/A\",throwCombined(F16, D16, S16, E16,J16))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D16=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K16, M16, N16, O16),0))","v":"N/A"},{"$f":"IF(D16=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K16,M16,N16,P16)),0))","v":"N/A"},{"$f":"'Run Selections'!BD16","v":0},{"$f":"IF(LEFT($D16,4)<>\"ACBC\",\"N/A\",AdjacentZone($D16,$E16,$S16,$F16,60))","v":"N/A"},{"$f":"IF(LEFT($D16,4)<>\"ACBC\",\"N/A\",AdjacentZone($D16,$E16,$S16,$F16,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F17)=\"\",\"\",'Run Selections'!F17)","v":""},null,{"$f":"'Run Selections'!T17","v":"Select Model"},{"$f":"'Run Selections'!W17","v":4},{"$f":"'Run Selections'!Y17","v":50},{"$f":"'Run Selections'!AI17","v":""},{"$f":"'Run Selections'!AA17","v":0},null,{"$f":"'Run Selections'!AL17","v":""},{"$f":"IF(D17=\"Select Model\",\"N/A\",throwCombined(F17, D17, S17, E17,J17))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D17=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K17, M17, N17, O17),0))","v":"N/A"},{"$f":"IF(D17=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K17,M17,N17,P17)),0))","v":"N/A"},{"$f":"'Run Selections'!BD17","v":0},{"$f":"IF(LEFT($D17,4)<>\"ACBC\",\"N/A\",AdjacentZone($D17,$E17,$S17,$F17,60))","v":"N/A"},{"$f":"IF(LEFT($D17,4)<>\"ACBC\",\"N/A\",AdjacentZone($D17,$E17,$S17,$F17,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F18)=\"\",\"\",'Run Selections'!F18)","v":""},null,{"$f":"'Run Selections'!T18","v":"Select Model"},{"$f":"'Run Selections'!W18","v":4},{"$f":"'Run Selections'!Y18","v":50},{"$f":"'Run Selections'!AI18","v":""},{"$f":"'Run Selections'!AA18","v":0},null,{"$f":"'Run Selections'!AL18","v":""},{"$f":"IF(D18=\"Select Model\",\"N/A\",throwCombined(F18, D18, S18, E18,J18))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D18=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K18, M18, N18, O18),0))","v":"N/A"},{"$f":"IF(D18=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K18,M18,N18,P18)),0))","v":"N/A"},{"$f":"'Run Selections'!BD18","v":0},{"$f":"IF(LEFT($D18,4)<>\"ACBC\",\"N/A\",AdjacentZone($D18,$E18,$S18,$F18,60))","v":"N/A"},{"$f":"IF(LEFT($D18,4)<>\"ACBC\",\"N/A\",AdjacentZone($D18,$E18,$S18,$F18,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F19)=\"\",\"\",'Run Selections'!F19)","v":""},null,{"$f":"'Run Selections'!T19","v":"Select Model"},{"$f":"'Run Selections'!W19","v":4},{"$f":"'Run Selections'!Y19","v":50},{"$f":"'Run Selections'!AI19","v":""},{"$f":"'Run Selections'!AA19","v":0},null,{"$f":"'Run Selections'!AL19","v":""},{"$f":"IF(D19=\"Select Model\",\"N/A\",throwCombined(F19, D19, S19, E19,J19))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D19=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K19, M19, N19, O19),0))","v":"N/A"},{"$f":"IF(D19=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K19,M19,N19,P19)),0))","v":"N/A"},{"$f":"'Run Selections'!BD19","v":0},{"$f":"IF(LEFT($D19,4)<>\"ACBC\",\"N/A\",AdjacentZone($D19,$E19,$S19,$F19,60))","v":"N/A"},{"$f":"IF(LEFT($D19,4)<>\"ACBC\",\"N/A\",AdjacentZone($D19,$E19,$S19,$F19,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F20)=\"\",\"\",'Run Selections'!F20)","v":""},null,{"$f":"'Run Selections'!T20","v":"Select Model"},{"$f":"'Run Selections'!W20","v":4},{"$f":"'Run Selections'!Y20","v":50},{"$f":"'Run Selections'!AI20","v":""},{"$f":"'Run Selections'!AA20","v":0},null,{"$f":"'Run Selections'!AL20","v":""},{"$f":"IF(D20=\"Select Model\",\"N/A\",throwCombined(F20, D20, S20, E20,J20))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D20=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K20, M20, N20, O20),0))","v":"N/A"},{"$f":"IF(D20=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K20,M20,N20,P20)),0))","v":"N/A"},{"$f":"'Run Selections'!BD20","v":0},{"$f":"IF(LEFT($D20,4)<>\"ACBC\",\"N/A\",AdjacentZone($D20,$E20,$S20,$F20,60))","v":"N/A"},{"$f":"IF(LEFT($D20,4)<>\"ACBC\",\"N/A\",AdjacentZone($D20,$E20,$S20,$F20,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F21)=\"\",\"\",'Run Selections'!F21)","v":""},null,{"$f":"'Run Selections'!T21","v":"Select Model"},{"$f":"'Run Selections'!W21","v":4},{"$f":"'Run Selections'!Y21","v":50},{"$f":"'Run Selections'!AI21","v":""},{"$f":"'Run Selections'!AA21","v":0},null,{"$f":"'Run Selections'!AL21","v":""},{"$f":"IF(D21=\"Select Model\",\"N/A\",throwCombined(F21, D21, S21, E21,J21))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D21=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K21, M21, N21, O21),0))","v":"N/A"},{"$f":"IF(D21=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K21,M21,N21,P21)),0))","v":"N/A"},{"$f":"'Run Selections'!BD21","v":0},{"$f":"IF(LEFT($D21,4)<>\"ACBC\",\"N/A\",AdjacentZone($D21,$E21,$S21,$F21,60))","v":"N/A"},{"$f":"IF(LEFT($D21,4)<>\"ACBC\",\"N/A\",AdjacentZone($D21,$E21,$S21,$F21,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F22)=\"\",\"\",'Run Selections'!F22)","v":""},null,{"$f":"'Run Selections'!T22","v":"Select Model"},{"$f":"'Run Selections'!W22","v":4},{"$f":"'Run Selections'!Y22","v":50},{"$f":"'Run Selections'!AI22","v":""},{"$f":"'Run Selections'!AA22","v":0},null,{"$f":"'Run Selections'!AL22","v":""},{"$f":"IF(D22=\"Select Model\",\"N/A\",throwCombined(F22, D22, S22, E22,J22))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D22=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K22, M22, N22, O22),0))","v":"N/A"},{"$f":"IF(D22=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K22,M22,N22,P22)),0))","v":"N/A"},{"$f":"'Run Selections'!BD22","v":0},{"$f":"IF(LEFT($D22,4)<>\"ACBC\",\"N/A\",AdjacentZone($D22,$E22,$S22,$F22,60))","v":"N/A"},{"$f":"IF(LEFT($D22,4)<>\"ACBC\",\"N/A\",AdjacentZone($D22,$E22,$S22,$F22,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F23)=\"\",\"\",'Run Selections'!F23)","v":""},null,{"$f":"'Run Selections'!T23","v":"Select Model"},{"$f":"'Run Selections'!W23","v":4},{"$f":"'Run Selections'!Y23","v":50},{"$f":"'Run Selections'!AI23","v":""},{"$f":"'Run Selections'!AA23","v":0},null,{"$f":"'Run Selections'!AL23","v":""},{"$f":"IF(D23=\"Select Model\",\"N/A\",throwCombined(F23, D23, S23, E23,J23))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D23=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K23, M23, N23, O23),0))","v":"N/A"},{"$f":"IF(D23=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K23,M23,N23,P23)),0))","v":"N/A"},{"$f":"'Run Selections'!BD23","v":0},{"$f":"IF(LEFT($D23,4)<>\"ACBC\",\"N/A\",AdjacentZone($D23,$E23,$S23,$F23,60))","v":"N/A"},{"$f":"IF(LEFT($D23,4)<>\"ACBC\",\"N/A\",AdjacentZone($D23,$E23,$S23,$F23,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F24)=\"\",\"\",'Run Selections'!F24)","v":""},null,{"$f":"'Run Selections'!T24","v":"Select Model"},{"$f":"'Run Selections'!W24","v":4},{"$f":"'Run Selections'!Y24","v":50},{"$f":"'Run Selections'!AI24","v":""},{"$f":"'Run Selections'!AA24","v":0},null,{"$f":"'Run Selections'!AL24","v":""},{"$f":"IF(D24=\"Select Model\",\"N/A\",throwCombined(F24, D24, S24, E24,J24))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D24=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K24, M24, N24, O24),0))","v":"N/A"},{"$f":"IF(D24=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K24,M24,N24,P24)),0))","v":"N/A"},{"$f":"'Run Selections'!BD24","v":0},{"$f":"IF(LEFT($D24,4)<>\"ACBC\",\"N/A\",AdjacentZone($D24,$E24,$S24,$F24,60))","v":"N/A"},{"$f":"IF(LEFT($D24,4)<>\"ACBC\",\"N/A\",AdjacentZone($D24,$E24,$S24,$F24,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F25)=\"\",\"\",'Run Selections'!F25)","v":""},null,{"$f":"'Run Selections'!T25","v":"Select Model"},{"$f":"'Run Selections'!W25","v":4},{"$f":"'Run Selections'!Y25","v":50},{"$f":"'Run Selections'!AI25","v":""},{"$f":"'Run Selections'!AA25","v":0},null,{"$f":"'Run Selections'!AL25","v":""},{"$f":"IF(D25=\"Select Model\",\"N/A\",throwCombined(F25, D25, S25, E25,J25))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D25=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K25, M25, N25, O25),0))","v":"N/A"},{"$f":"IF(D25=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K25,M25,N25,P25)),0))","v":"N/A"},{"$f":"'Run Selections'!BD25","v":0},{"$f":"IF(LEFT($D25,4)<>\"ACBC\",\"N/A\",AdjacentZone($D25,$E25,$S25,$F25,60))","v":"N/A"},{"$f":"IF(LEFT($D25,4)<>\"ACBC\",\"N/A\",AdjacentZone($D25,$E25,$S25,$F25,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F26)=\"\",\"\",'Run Selections'!F26)","v":""},null,{"$f":"'Run Selections'!T26","v":"Select Model"},{"$f":"'Run Selections'!W26","v":4.33},{"$f":"'Run Selections'!Y26","v":50},{"$f":"'Run Selections'!AI26","v":""},{"$f":"'Run Selections'!AA26","v":0},null,{"$f":"'Run Selections'!AL26","v":""},{"$f":"IF(D26=\"Select Model\",\"N/A\",throwCombined(F26, D26, S26, E26,J26))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D26=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K26, M26, N26, O26),0))","v":"N/A"},{"$f":"IF(D26=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K26,M26,N26,P26)),0))","v":"N/A"},{"$f":"'Run Selections'!BD26","v":0},{"$f":"IF(LEFT($D26,4)<>\"ACBC\",\"N/A\",AdjacentZone($D26,$E26,$S26,$F26,60))","v":"N/A"},{"$f":"IF(LEFT($D26,4)<>\"ACBC\",\"N/A\",AdjacentZone($D26,$E26,$S26,$F26,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F27)=\"\",\"\",'Run Selections'!F27)","v":""},null,{"$f":"'Run Selections'!T27","v":"Select Model"},{"$f":"'Run Selections'!W27","v":4},{"$f":"'Run Selections'!Y27","v":50},{"$f":"'Run Selections'!AI27","v":""},{"$f":"'Run Selections'!AA27","v":0},null,{"$f":"'Run Selections'!AL27","v":""},{"$f":"IF(D27=\"Select Model\",\"N/A\",throwCombined(F27, D27, S27, E27,J27))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D27=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K27, M27, N27, O27),0))","v":"N/A"},{"$f":"IF(D27=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K27,M27,N27,P27)),0))","v":"N/A"},{"$f":"'Run Selections'!BD27","v":0},{"$f":"IF(LEFT($D27,4)<>\"ACBC\",\"N/A\",AdjacentZone($D27,$E27,$S27,$F27,60))","v":"N/A"},{"$f":"IF(LEFT($D27,4)<>\"ACBC\",\"N/A\",AdjacentZone($D27,$E27,$S27,$F27,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F28)=\"\",\"\",'Run Selections'!F28)","v":""},null,{"$f":"'Run Selections'!T28","v":"Select Model"},{"$f":"'Run Selections'!W28","v":4},{"$f":"'Run Selections'!Y28","v":50},{"$f":"'Run Selections'!AI28","v":""},{"$f":"'Run Selections'!AA28","v":0},null,{"$f":"'Run Selections'!AL28","v":""},{"$f":"IF(D28=\"Select Model\",\"N/A\",throwCombined(F28, D28, S28, E28,J28))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D28=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K28, M28, N28, O28),0))","v":"N/A"},{"$f":"IF(D28=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K28,M28,N28,P28)),0))","v":"N/A"},{"$f":"'Run Selections'!BD28","v":0},{"$f":"IF(LEFT($D28,4)<>\"ACBC\",\"N/A\",AdjacentZone($D28,$E28,$S28,$F28,60))","v":"N/A"},{"$f":"IF(LEFT($D28,4)<>\"ACBC\",\"N/A\",AdjacentZone($D28,$E28,$S28,$F28,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F29)=\"\",\"\",'Run Selections'!F29)","v":""},null,{"$f":"'Run Selections'!T29","v":"Select Model"},{"$f":"'Run Selections'!W29","v":4},{"$f":"'Run Selections'!Y29","v":50},{"$f":"'Run Selections'!AI29","v":""},{"$f":"'Run Selections'!AA29","v":0},null,{"$f":"'Run Selections'!AL29","v":""},{"$f":"IF(D29=\"Select Model\",\"N/A\",throwCombined(F29, D29, S29, E29,J29))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D29=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K29, M29, N29, O29),0))","v":"N/A"},{"$f":"IF(D29=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K29,M29,N29,P29)),0))","v":"N/A"},{"$f":"'Run Selections'!BD29","v":0},{"$f":"IF(LEFT($D29,4)<>\"ACBC\",\"N/A\",AdjacentZone($D29,$E29,$S29,$F29,60))","v":"N/A"},{"$f":"IF(LEFT($D29,4)<>\"ACBC\",\"N/A\",AdjacentZone($D29,$E29,$S29,$F29,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F30)=\"\",\"\",'Run Selections'!F30)","v":""},null,{"$f":"'Run Selections'!T30","v":"Select Model"},{"$f":"'Run Selections'!W30","v":4},{"$f":"'Run Selections'!Y30","v":50},{"$f":"'Run Selections'!AI30","v":""},{"$f":"'Run Selections'!AA30","v":0},null,{"$f":"'Run Selections'!AL30","v":""},{"$f":"IF(D30=\"Select Model\",\"N/A\",throwCombined(F30, D30, S30, E30,J30))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D30=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K30, M30, N30, O30),0))","v":"N/A"},{"$f":"IF(D30=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K30,M30,N30,P30)),0))","v":"N/A"},{"$f":"'Run Selections'!BD30","v":0},{"$f":"IF(LEFT($D30,4)<>\"ACBC\",\"N/A\",AdjacentZone($D30,$E30,$S30,$F30,60))","v":"N/A"},{"$f":"IF(LEFT($D30,4)<>\"ACBC\",\"N/A\",AdjacentZone($D30,$E30,$S30,$F30,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F31)=\"\",\"\",'Run Selections'!F31)","v":""},null,{"$f":"'Run Selections'!T31","v":"Select Model"},{"$f":"'Run Selections'!W31","v":4},{"$f":"'Run Selections'!Y31","v":50},{"$f":"'Run Selections'!AI31","v":""},{"$f":"'Run Selections'!AA31","v":0},null,{"$f":"'Run Selections'!AL31","v":""},{"$f":"IF(D31=\"Select Model\",\"N/A\",throwCombined(F31, D31, S31, E31,J31))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D31=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K31, M31, N31, O31),0))","v":"N/A"},{"$f":"IF(D31=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K31,M31,N31,P31)),0))","v":"N/A"},{"$f":"'Run Selections'!BD31","v":0},{"$f":"IF(LEFT($D31,4)<>\"ACBC\",\"N/A\",AdjacentZone($D31,$E31,$S31,$F31,60))","v":"N/A"},{"$f":"IF(LEFT($D31,4)<>\"ACBC\",\"N/A\",AdjacentZone($D31,$E31,$S31,$F31,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F32)=\"\",\"\",'Run Selections'!F32)","v":""},null,{"$f":"'Run Selections'!T32","v":"Select Model"},{"$f":"'Run Selections'!W32","v":4},{"$f":"'Run Selections'!Y32","v":50},{"$f":"'Run Selections'!AI32","v":""},{"$f":"'Run Selections'!AA32","v":0},null,{"$f":"'Run Selections'!AL32","v":""},{"$f":"IF(D32=\"Select Model\",\"N/A\",throwCombined(F32, D32, S32, E32,J32))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D32=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K32, M32, N32, O32),0))","v":"N/A"},{"$f":"IF(D32=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K32,M32,N32,P32)),0))","v":"N/A"},{"$f":"'Run Selections'!BD32","v":0},{"$f":"IF(LEFT($D32,4)<>\"ACBC\",\"N/A\",AdjacentZone($D32,$E32,$S32,$F32,60))","v":"N/A"},{"$f":"IF(LEFT($D32,4)<>\"ACBC\",\"N/A\",AdjacentZone($D32,$E32,$S32,$F32,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F33)=\"\",\"\",'Run Selections'!F33)","v":""},null,{"$f":"'Run Selections'!T33","v":"Select Model"},{"$f":"'Run Selections'!W33","v":4},{"$f":"'Run Selections'!Y33","v":50},{"$f":"'Run Selections'!AI33","v":""},{"$f":"'Run Selections'!AA33","v":0},null,{"$f":"'Run Selections'!AL33","v":""},{"$f":"IF(D33=\"Select Model\",\"N/A\",throwCombined(F33, D33, S33, E33,J33))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D33=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K33, M33, N33, O33),0))","v":"N/A"},{"$f":"IF(D33=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K33,M33,N33,P33)),0))","v":"N/A"},{"$f":"'Run Selections'!BD33","v":0},{"$f":"IF(LEFT($D33,4)<>\"ACBC\",\"N/A\",AdjacentZone($D33,$E33,$S33,$F33,60))","v":"N/A"},{"$f":"IF(LEFT($D33,4)<>\"ACBC\",\"N/A\",AdjacentZone($D33,$E33,$S33,$F33,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F34)=\"\",\"\",'Run Selections'!F34)","v":""},null,{"$f":"'Run Selections'!T34","v":"Select Model"},{"$f":"'Run Selections'!W34","v":4},{"$f":"'Run Selections'!Y34","v":50},{"$f":"'Run Selections'!AI34","v":""},{"$f":"'Run Selections'!AA34","v":0},null,{"$f":"'Run Selections'!AL34","v":""},{"$f":"IF(D34=\"Select Model\",\"N/A\",throwCombined(F34, D34, S34, E34,J34))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D34=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K34, M34, N34, O34),0))","v":"N/A"},{"$f":"IF(D34=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K34,M34,N34,P34)),0))","v":"N/A"},{"$f":"'Run Selections'!BD34","v":0},{"$f":"IF(LEFT($D34,4)<>\"ACBC\",\"N/A\",AdjacentZone($D34,$E34,$S34,$F34,60))","v":"N/A"},{"$f":"IF(LEFT($D34,4)<>\"ACBC\",\"N/A\",AdjacentZone($D34,$E34,$S34,$F34,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F35)=\"\",\"\",'Run Selections'!F35)","v":""},null,{"$f":"'Run Selections'!T35","v":"Select Model"},{"$f":"'Run Selections'!W35","v":4},{"$f":"'Run Selections'!Y35","v":50},{"$f":"'Run Selections'!AI35","v":""},{"$f":"'Run Selections'!AA35","v":0},null,{"$f":"'Run Selections'!AL35","v":""},{"$f":"IF(D35=\"Select Model\",\"N/A\",throwCombined(F35, D35, S35, E35,J35))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D35=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K35, M35, N35, O35),0))","v":"N/A"},{"$f":"IF(D35=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K35,M35,N35,P35)),0))","v":"N/A"},{"$f":"'Run Selections'!BD35","v":0},{"$f":"IF(LEFT($D35,4)<>\"ACBC\",\"N/A\",AdjacentZone($D35,$E35,$S35,$F35,60))","v":"N/A"},{"$f":"IF(LEFT($D35,4)<>\"ACBC\",\"N/A\",AdjacentZone($D35,$E35,$S35,$F35,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F36)=\"\",\"\",'Run Selections'!F36)","v":""},null,{"$f":"'Run Selections'!T36","v":"Select Model"},{"$f":"'Run Selections'!W36","v":4},{"$f":"'Run Selections'!Y36","v":50},{"$f":"'Run Selections'!AI36","v":""},{"$f":"'Run Selections'!AA36","v":0},null,{"$f":"'Run Selections'!AL36","v":""},{"$f":"IF(D36=\"Select Model\",\"N/A\",throwCombined(F36, D36, S36, E36,J36))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D36=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K36, M36, N36, O36),0))","v":"N/A"},{"$f":"IF(D36=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K36,M36,N36,P36)),0))","v":"N/A"},{"$f":"'Run Selections'!BD36","v":0},{"$f":"IF(LEFT($D36,4)<>\"ACBC\",\"N/A\",AdjacentZone($D36,$E36,$S36,$F36,60))","v":"N/A"},{"$f":"IF(LEFT($D36,4)<>\"ACBC\",\"N/A\",AdjacentZone($D36,$E36,$S36,$F36,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F37)=\"\",\"\",'Run Selections'!F37)","v":""},null,{"$f":"'Run Selections'!T37","v":"Select Model"},{"$f":"'Run Selections'!W37","v":4},{"$f":"'Run Selections'!Y37","v":50},{"$f":"'Run Selections'!AI37","v":""},{"$f":"'Run Selections'!AA37","v":0},null,{"$f":"'Run Selections'!AL37","v":""},{"$f":"IF(D37=\"Select Model\",\"N/A\",throwCombined(F37, D37, S37, E37,J37))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D37=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K37, M37, N37, O37),0))","v":"N/A"},{"$f":"IF(D37=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K37,M37,N37,P37)),0))","v":"N/A"},{"$f":"'Run Selections'!BD37","v":0},{"$f":"IF(LEFT($D37,4)<>\"ACBC\",\"N/A\",AdjacentZone($D37,$E37,$S37,$F37,60))","v":"N/A"},{"$f":"IF(LEFT($D37,4)<>\"ACBC\",\"N/A\",AdjacentZone($D37,$E37,$S37,$F37,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F38)=\"\",\"\",'Run Selections'!F38)","v":""},null,{"$f":"'Run Selections'!T38","v":"Select Model"},{"$f":"'Run Selections'!W38","v":4},{"$f":"'Run Selections'!Y38","v":50},{"$f":"'Run Selections'!AI38","v":""},{"$f":"'Run Selections'!AA38","v":0},null,{"$f":"'Run Selections'!AL38","v":""},{"$f":"IF(D38=\"Select Model\",\"N/A\",throwCombined(F38, D38, S38, E38,J38))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D38=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K38, M38, N38, O38),0))","v":"N/A"},{"$f":"IF(D38=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K38,M38,N38,P38)),0))","v":"N/A"},{"$f":"'Run Selections'!BD38","v":0},{"$f":"IF(LEFT($D38,4)<>\"ACBC\",\"N/A\",AdjacentZone($D38,$E38,$S38,$F38,60))","v":"N/A"},{"$f":"IF(LEFT($D38,4)<>\"ACBC\",\"N/A\",AdjacentZone($D38,$E38,$S38,$F38,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F39)=\"\",\"\",'Run Selections'!F39)","v":""},null,{"$f":"'Run Selections'!T39","v":"Select Model"},{"$f":"'Run Selections'!W39","v":4},{"$f":"'Run Selections'!Y39","v":50},{"$f":"'Run Selections'!AI39","v":""},{"$f":"'Run Selections'!AA39","v":0},null,{"$f":"'Run Selections'!AL39","v":""},{"$f":"IF(D39=\"Select Model\",\"N/A\",throwCombined(F39, D39, S39, E39,J39))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D39=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K39, M39, N39, O39),0))","v":"N/A"},{"$f":"IF(D39=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K39,M39,N39,P39)),0))","v":"N/A"},{"$f":"'Run Selections'!BD39","v":0},{"$f":"IF(LEFT($D39,4)<>\"ACBC\",\"N/A\",AdjacentZone($D39,$E39,$S39,$F39,60))","v":"N/A"},{"$f":"IF(LEFT($D39,4)<>\"ACBC\",\"N/A\",AdjacentZone($D39,$E39,$S39,$F39,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F40)=\"\",\"\",'Run Selections'!F40)","v":""},null,{"$f":"'Run Selections'!T40","v":"Select Model"},{"$f":"'Run Selections'!W40","v":4},{"$f":"'Run Selections'!Y40","v":50},{"$f":"'Run Selections'!AI40","v":""},{"$f":"'Run Selections'!AA40","v":0},null,{"$f":"'Run Selections'!AL40","v":""},{"$f":"IF(D40=\"Select Model\",\"N/A\",throwCombined(F40, D40, S40, E40,J40))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D40=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K40, M40, N40, O40),0))","v":"N/A"},{"$f":"IF(D40=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K40,M40,N40,P40)),0))","v":"N/A"},{"$f":"'Run Selections'!BD40","v":0},{"$f":"IF(LEFT($D40,4)<>\"ACBC\",\"N/A\",AdjacentZone($D40,$E40,$S40,$F40,60))","v":"N/A"},{"$f":"IF(LEFT($D40,4)<>\"ACBC\",\"N/A\",AdjacentZone($D40,$E40,$S40,$F40,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F41)=\"\",\"\",'Run Selections'!F41)","v":""},null,{"$f":"'Run Selections'!T41","v":"Select Model"},{"$f":"'Run Selections'!W41","v":4},{"$f":"'Run Selections'!Y41","v":50},{"$f":"'Run Selections'!AI41","v":""},{"$f":"'Run Selections'!AA41","v":0},null,{"$f":"'Run Selections'!AL41","v":""},{"$f":"IF(D41=\"Select Model\",\"N/A\",throwCombined(F41, D41, S41, E41,J41))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D41=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K41, M41, N41, O41),0))","v":"N/A"},{"$f":"IF(D41=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K41,M41,N41,P41)),0))","v":"N/A"},{"$f":"'Run Selections'!BD41","v":0},{"$f":"IF(LEFT($D41,4)<>\"ACBC\",\"N/A\",AdjacentZone($D41,$E41,$S41,$F41,60))","v":"N/A"},{"$f":"IF(LEFT($D41,4)<>\"ACBC\",\"N/A\",AdjacentZone($D41,$E41,$S41,$F41,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F42)=\"\",\"\",'Run Selections'!F42)","v":""},null,{"$f":"'Run Selections'!T42","v":"Select Model"},{"$f":"'Run Selections'!W42","v":4},{"$f":"'Run Selections'!Y42","v":50},{"$f":"'Run Selections'!AI42","v":""},{"$f":"'Run Selections'!AA42","v":0},null,{"$f":"'Run Selections'!AL42","v":""},{"$f":"IF(D42=\"Select Model\",\"N/A\",throwCombined(F42, D42, S42, E42,J42))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D42=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K42, M42, N42, O42),0))","v":"N/A"},{"$f":"IF(D42=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K42,M42,N42,P42)),0))","v":"N/A"},{"$f":"'Run Selections'!BD42","v":0},{"$f":"IF(LEFT($D42,4)<>\"ACBC\",\"N/A\",AdjacentZone($D42,$E42,$S42,$F42,60))","v":"N/A"},{"$f":"IF(LEFT($D42,4)<>\"ACBC\",\"N/A\",AdjacentZone($D42,$E42,$S42,$F42,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F43)=\"\",\"\",'Run Selections'!F43)","v":""},null,{"$f":"'Run Selections'!T43","v":"Select Model"},{"$f":"'Run Selections'!W43","v":4},{"$f":"'Run Selections'!Y43","v":50},{"$f":"'Run Selections'!AI43","v":""},{"$f":"'Run Selections'!AA43","v":0},null,{"$f":"'Run Selections'!AL43","v":""},{"$f":"IF(D43=\"Select Model\",\"N/A\",throwCombined(F43, D43, S43, E43,J43))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D43=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K43, M43, N43, O43),0))","v":"N/A"},{"$f":"IF(D43=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K43,M43,N43,P43)),0))","v":"N/A"},{"$f":"'Run Selections'!BD43","v":0},{"$f":"IF(LEFT($D43,4)<>\"ACBC\",\"N/A\",AdjacentZone($D43,$E43,$S43,$F43,60))","v":"N/A"},{"$f":"IF(LEFT($D43,4)<>\"ACBC\",\"N/A\",AdjacentZone($D43,$E43,$S43,$F43,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F44)=\"\",\"\",'Run Selections'!F44)","v":""},null,{"$f":"'Run Selections'!T44","v":"Select Model"},{"$f":"'Run Selections'!W44","v":4},{"$f":"'Run Selections'!Y44","v":50},{"$f":"'Run Selections'!AI44","v":""},{"$f":"'Run Selections'!AA44","v":0},null,{"$f":"'Run Selections'!AL44","v":""},{"$f":"IF(D44=\"Select Model\",\"N/A\",throwCombined(F44, D44, S44, E44,J44))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D44=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K44, M44, N44, O44),0))","v":"N/A"},{"$f":"IF(D44=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K44,M44,N44,P44)),0))","v":"N/A"},{"$f":"'Run Selections'!BD44","v":0},{"$f":"IF(LEFT($D44,4)<>\"ACBC\",\"N/A\",AdjacentZone($D44,$E44,$S44,$F44,60))","v":"N/A"},{"$f":"IF(LEFT($D44,4)<>\"ACBC\",\"N/A\",AdjacentZone($D44,$E44,$S44,$F44,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F45)=\"\",\"\",'Run Selections'!F45)","v":""},null,{"$f":"'Run Selections'!T45","v":"Select Model"},{"$f":"'Run Selections'!W45","v":4},{"$f":"'Run Selections'!Y45","v":50},{"$f":"'Run Selections'!AI45","v":""},{"$f":"'Run Selections'!AA45","v":0},null,{"$f":"'Run Selections'!AL45","v":""},{"$f":"IF(D45=\"Select Model\",\"N/A\",throwCombined(F45, D45, S45, E45,J45))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D45=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K45, M45, N45, O45),0))","v":"N/A"},{"$f":"IF(D45=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K45,M45,N45,P45)),0))","v":"N/A"},{"$f":"'Run Selections'!BD45","v":0},{"$f":"IF(LEFT($D45,4)<>\"ACBC\",\"N/A\",AdjacentZone($D45,$E45,$S45,$F45,60))","v":"N/A"},{"$f":"IF(LEFT($D45,4)<>\"ACBC\",\"N/A\",AdjacentZone($D45,$E45,$S45,$F45,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F46)=\"\",\"\",'Run Selections'!F46)","v":""},null,{"$f":"'Run Selections'!T46","v":"Select Model"},{"$f":"'Run Selections'!W46","v":4},{"$f":"'Run Selections'!Y46","v":50},{"$f":"'Run Selections'!AI46","v":""},{"$f":"'Run Selections'!AA46","v":0},null,{"$f":"'Run Selections'!AL46","v":""},{"$f":"IF(D46=\"Select Model\",\"N/A\",throwCombined(F46, D46, S46, E46,J46))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D46=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K46, M46, N46, O46),0))","v":"N/A"},{"$f":"IF(D46=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K46,M46,N46,P46)),0))","v":"N/A"},{"$f":"'Run Selections'!BD46","v":0},{"$f":"IF(LEFT($D46,4)<>\"ACBC\",\"N/A\",AdjacentZone($D46,$E46,$S46,$F46,60))","v":"N/A"},{"$f":"IF(LEFT($D46,4)<>\"ACBC\",\"N/A\",AdjacentZone($D46,$E46,$S46,$F46,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F47)=\"\",\"\",'Run Selections'!F47)","v":""},null,{"$f":"'Run Selections'!T47","v":"Select Model"},{"$f":"'Run Selections'!W47","v":4},{"$f":"'Run Selections'!Y47","v":50},{"$f":"'Run Selections'!AI47","v":""},{"$f":"'Run Selections'!AA47","v":0},null,{"$f":"'Run Selections'!AL47","v":""},{"$f":"IF(D47=\"Select Model\",\"N/A\",throwCombined(F47, D47, S47, E47,J47))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D47=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K47, M47, N47, O47),0))","v":"N/A"},{"$f":"IF(D47=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K47,M47,N47,P47)),0))","v":"N/A"},{"$f":"'Run Selections'!BD47","v":0},{"$f":"IF(LEFT($D47,4)<>\"ACBC\",\"N/A\",AdjacentZone($D47,$E47,$S47,$F47,60))","v":"N/A"},{"$f":"IF(LEFT($D47,4)<>\"ACBC\",\"N/A\",AdjacentZone($D47,$E47,$S47,$F47,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F48)=\"\",\"\",'Run Selections'!F48)","v":""},null,{"$f":"'Run Selections'!T48","v":"Select Model"},{"$f":"'Run Selections'!W48","v":4},{"$f":"'Run Selections'!Y48","v":50},{"$f":"'Run Selections'!AI48","v":""},{"$f":"'Run Selections'!AA48","v":0},null,{"$f":"'Run Selections'!AL48","v":""},{"$f":"IF(D48=\"Select Model\",\"N/A\",throwCombined(F48, D48, S48, E48,J48))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D48=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K48, M48, N48, O48),0))","v":"N/A"},{"$f":"IF(D48=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K48,M48,N48,P48)),0))","v":"N/A"},{"$f":"'Run Selections'!BD48","v":0},{"$f":"IF(LEFT($D48,4)<>\"ACBC\",\"N/A\",AdjacentZone($D48,$E48,$S48,$F48,60))","v":"N/A"},{"$f":"IF(LEFT($D48,4)<>\"ACBC\",\"N/A\",AdjacentZone($D48,$E48,$S48,$F48,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F49)=\"\",\"\",'Run Selections'!F49)","v":""},null,{"$f":"'Run Selections'!T49","v":"Select Model"},{"$f":"'Run Selections'!W49","v":4},{"$f":"'Run Selections'!Y49","v":50},{"$f":"'Run Selections'!AI49","v":""},{"$f":"'Run Selections'!AA49","v":0},null,{"$f":"'Run Selections'!AL49","v":""},{"$f":"IF(D49=\"Select Model\",\"N/A\",throwCombined(F49, D49, S49, E49,J49))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D49=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K49, M49, N49, O49),0))","v":"N/A"},{"$f":"IF(D49=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K49,M49,N49,P49)),0))","v":"N/A"},{"$f":"'Run Selections'!BD49","v":0},{"$f":"IF(LEFT($D49,4)<>\"ACBC\",\"N/A\",AdjacentZone($D49,$E49,$S49,$F49,60))","v":"N/A"},{"$f":"IF(LEFT($D49,4)<>\"ACBC\",\"N/A\",AdjacentZone($D49,$E49,$S49,$F49,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F50)=\"\",\"\",'Run Selections'!F50)","v":""},null,{"$f":"'Run Selections'!T50","v":"Select Model"},{"$f":"'Run Selections'!W50","v":4},{"$f":"'Run Selections'!Y50","v":50},{"$f":"'Run Selections'!AI50","v":""},{"$f":"'Run Selections'!AA50","v":0},null,{"$f":"'Run Selections'!AL50","v":""},{"$f":"IF(D50=\"Select Model\",\"N/A\",throwCombined(F50, D50, S50, E50,J50))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D50=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K50, M50, N50, O50),0))","v":"N/A"},{"$f":"IF(D50=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K50,M50,N50,P50)),0))","v":"N/A"},{"$f":"'Run Selections'!BD50","v":0},{"$f":"IF(LEFT($D50,4)<>\"ACBC\",\"N/A\",AdjacentZone($D50,$E50,$S50,$F50,60))","v":"N/A"},{"$f":"IF(LEFT($D50,4)<>\"ACBC\",\"N/A\",AdjacentZone($D50,$E50,$S50,$F50,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F51)=\"\",\"\",'Run Selections'!F51)","v":""},null,{"$f":"'Run Selections'!T51","v":"Select Model"},{"$f":"'Run Selections'!W51","v":4},{"$f":"'Run Selections'!Y51","v":50},{"$f":"'Run Selections'!AI51","v":""},{"$f":"'Run Selections'!AA51","v":0},null,{"$f":"'Run Selections'!AL51","v":""},{"$f":"IF(D51=\"Select Model\",\"N/A\",throwCombined(F51, D51, S51, E51,J51))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D51=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K51, M51, N51, O51),0))","v":"N/A"},{"$f":"IF(D51=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K51,M51,N51,P51)),0))","v":"N/A"},{"$f":"'Run Selections'!BD51","v":0},{"$f":"IF(LEFT($D51,4)<>\"ACBC\",\"N/A\",AdjacentZone($D51,$E51,$S51,$F51,60))","v":"N/A"},{"$f":"IF(LEFT($D51,4)<>\"ACBC\",\"N/A\",AdjacentZone($D51,$E51,$S51,$F51,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F52)=\"\",\"\",'Run Selections'!F52)","v":""},null,{"$f":"'Run Selections'!T52","v":"Select Model"},{"$f":"'Run Selections'!W52","v":4},{"$f":"'Run Selections'!Y52","v":50},{"$f":"'Run Selections'!AI52","v":""},{"$f":"'Run Selections'!AA52","v":0},null,{"$f":"'Run Selections'!AL52","v":""},{"$f":"IF(D52=\"Select Model\",\"N/A\",throwCombined(F52, D52, S52, E52,J52))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D52=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K52, M52, N52, O52),0))","v":"N/A"},{"$f":"IF(D52=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K52,M52,N52,P52)),0))","v":"N/A"},{"$f":"'Run Selections'!BD52","v":0},{"$f":"IF(LEFT($D52,4)<>\"ACBC\",\"N/A\",AdjacentZone($D52,$E52,$S52,$F52,60))","v":"N/A"},{"$f":"IF(LEFT($D52,4)<>\"ACBC\",\"N/A\",AdjacentZone($D52,$E52,$S52,$F52,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F53)=\"\",\"\",'Run Selections'!F53)","v":""},null,{"$f":"'Run Selections'!T53","v":"Select Model"},{"$f":"'Run Selections'!W53","v":4},{"$f":"'Run Selections'!Y53","v":50},{"$f":"'Run Selections'!AI53","v":""},{"$f":"'Run Selections'!AA53","v":0},null,{"$f":"'Run Selections'!AL53","v":""},{"$f":"IF(D53=\"Select Model\",\"N/A\",throwCombined(F53, D53, S53, E53,J53))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D53=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K53, M53, N53, O53),0))","v":"N/A"},{"$f":"IF(D53=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K53,M53,N53,P53)),0))","v":"N/A"},{"$f":"'Run Selections'!BD53","v":0},{"$f":"IF(LEFT($D53,4)<>\"ACBC\",\"N/A\",AdjacentZone($D53,$E53,$S53,$F53,60))","v":"N/A"},{"$f":"IF(LEFT($D53,4)<>\"ACBC\",\"N/A\",AdjacentZone($D53,$E53,$S53,$F53,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F54)=\"\",\"\",'Run Selections'!F54)","v":""},null,{"$f":"'Run Selections'!T54","v":"Select Model"},{"$f":"'Run Selections'!W54","v":4},{"$f":"'Run Selections'!Y54","v":50},{"$f":"'Run Selections'!AI54","v":""},{"$f":"'Run Selections'!AA54","v":0},null,{"$f":"'Run Selections'!AL54","v":""},{"$f":"IF(D54=\"Select Model\",\"N/A\",throwCombined(F54, D54, S54, E54,J54))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D54=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K54, M54, N54, O54),0))","v":"N/A"},{"$f":"IF(D54=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K54,M54,N54,P54)),0))","v":"N/A"},{"$f":"'Run Selections'!BD54","v":0},{"$f":"IF(LEFT($D54,4)<>\"ACBC\",\"N/A\",AdjacentZone($D54,$E54,$S54,$F54,60))","v":"N/A"},{"$f":"IF(LEFT($D54,4)<>\"ACBC\",\"N/A\",AdjacentZone($D54,$E54,$S54,$F54,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F55)=\"\",\"\",'Run Selections'!F55)","v":""},null,{"$f":"'Run Selections'!T55","v":"Select Model"},{"$f":"'Run Selections'!W55","v":4},{"$f":"'Run Selections'!Y55","v":50},{"$f":"'Run Selections'!AI55","v":""},{"$f":"'Run Selections'!AA55","v":0},null,{"$f":"'Run Selections'!AL55","v":""},{"$f":"IF(D55=\"Select Model\",\"N/A\",throwCombined(F55, D55, S55, E55,J55))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D55=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K55, M55, N55, O55),0))","v":"N/A"},{"$f":"IF(D55=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K55,M55,N55,P55)),0))","v":"N/A"},{"$f":"'Run Selections'!BD55","v":0},{"$f":"IF(LEFT($D55,4)<>\"ACBC\",\"N/A\",AdjacentZone($D55,$E55,$S55,$F55,60))","v":"N/A"},{"$f":"IF(LEFT($D55,4)<>\"ACBC\",\"N/A\",AdjacentZone($D55,$E55,$S55,$F55,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F56)=\"\",\"\",'Run Selections'!F56)","v":""},null,{"$f":"'Run Selections'!T56","v":"Select Model"},{"$f":"'Run Selections'!W56","v":4},{"$f":"'Run Selections'!Y56","v":50},{"$f":"'Run Selections'!AI56","v":""},{"$f":"'Run Selections'!AA56","v":0},null,{"$f":"'Run Selections'!AL56","v":""},{"$f":"IF(D56=\"Select Model\",\"N/A\",throwCombined(F56, D56, S56, E56,J56))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D56=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K56, M56, N56, O56),0))","v":"N/A"},{"$f":"IF(D56=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K56,M56,N56,P56)),0))","v":"N/A"},{"$f":"'Run Selections'!BD56","v":0},{"$f":"IF(LEFT($D56,4)<>\"ACBC\",\"N/A\",AdjacentZone($D56,$E56,$S56,$F56,60))","v":"N/A"},{"$f":"IF(LEFT($D56,4)<>\"ACBC\",\"N/A\",AdjacentZone($D56,$E56,$S56,$F56,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F57)=\"\",\"\",'Run Selections'!F57)","v":""},null,{"$f":"'Run Selections'!T57","v":"Select Model"},{"$f":"'Run Selections'!W57","v":4},{"$f":"'Run Selections'!Y57","v":50},{"$f":"'Run Selections'!AI57","v":""},{"$f":"'Run Selections'!AA57","v":0},null,{"$f":"'Run Selections'!AL57","v":""},{"$f":"IF(D57=\"Select Model\",\"N/A\",throwCombined(F57, D57, S57, E57,J57))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D57=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K57, M57, N57, O57),0))","v":"N/A"},{"$f":"IF(D57=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K57,M57,N57,P57)),0))","v":"N/A"},{"$f":"'Run Selections'!BD57","v":0},{"$f":"IF(LEFT($D57,4)<>\"ACBC\",\"N/A\",AdjacentZone($D57,$E57,$S57,$F57,60))","v":"N/A"},{"$f":"IF(LEFT($D57,4)<>\"ACBC\",\"N/A\",AdjacentZone($D57,$E57,$S57,$F57,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F58)=\"\",\"\",'Run Selections'!F58)","v":""},null,{"$f":"'Run Selections'!T58","v":"Select Model"},{"$f":"'Run Selections'!W58","v":4},{"$f":"'Run Selections'!Y58","v":50},{"$f":"'Run Selections'!AI58","v":""},{"$f":"'Run Selections'!AA58","v":0},null,{"$f":"'Run Selections'!AL58","v":""},{"$f":"IF(D58=\"Select Model\",\"N/A\",throwCombined(F58, D58, S58, E58,J58))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D58=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K58, M58, N58, O58),0))","v":"N/A"},{"$f":"IF(D58=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K58,M58,N58,P58)),0))","v":"N/A"},{"$f":"'Run Selections'!BD58","v":0},{"$f":"IF(LEFT($D58,4)<>\"ACBC\",\"N/A\",AdjacentZone($D58,$E58,$S58,$F58,60))","v":"N/A"},{"$f":"IF(LEFT($D58,4)<>\"ACBC\",\"N/A\",AdjacentZone($D58,$E58,$S58,$F58,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F59)=\"\",\"\",'Run Selections'!F59)","v":""},null,{"$f":"'Run Selections'!T59","v":"Select Model"},{"$f":"'Run Selections'!W59","v":4},{"$f":"'Run Selections'!Y59","v":50},{"$f":"'Run Selections'!AI59","v":""},{"$f":"'Run Selections'!AA59","v":0},null,{"$f":"'Run Selections'!AL59","v":""},{"$f":"IF(D59=\"Select Model\",\"N/A\",throwCombined(F59, D59, S59, E59,J59))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D59=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K59, M59, N59, O59),0))","v":"N/A"},{"$f":"IF(D59=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K59,M59,N59,P59)),0))","v":"N/A"},{"$f":"'Run Selections'!BD59","v":0},{"$f":"IF(LEFT($D59,4)<>\"ACBC\",\"N/A\",AdjacentZone($D59,$E59,$S59,$F59,60))","v":"N/A"},{"$f":"IF(LEFT($D59,4)<>\"ACBC\",\"N/A\",AdjacentZone($D59,$E59,$S59,$F59,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F60)=\"\",\"\",'Run Selections'!F60)","v":""},null,{"$f":"'Run Selections'!T60","v":"Select Model"},{"$f":"'Run Selections'!W60","v":4},{"$f":"'Run Selections'!Y60","v":50},{"$f":"'Run Selections'!AI60","v":""},{"$f":"'Run Selections'!AA60","v":0},null,{"$f":"'Run Selections'!AL60","v":""},{"$f":"IF(D60=\"Select Model\",\"N/A\",throwCombined(F60, D60, S60, E60,J60))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D60=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K60, M60, N60, O60),0))","v":"N/A"},{"$f":"IF(D60=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K60,M60,N60,P60)),0))","v":"N/A"},{"$f":"'Run Selections'!BD60","v":0},{"$f":"IF(LEFT($D60,4)<>\"ACBC\",\"N/A\",AdjacentZone($D60,$E60,$S60,$F60,60))","v":"N/A"},{"$f":"IF(LEFT($D60,4)<>\"ACBC\",\"N/A\",AdjacentZone($D60,$E60,$S60,$F60,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F61)=\"\",\"\",'Run Selections'!F61)","v":""},null,{"$f":"'Run Selections'!T61","v":"Select Model"},{"$f":"'Run Selections'!W61","v":4},{"$f":"'Run Selections'!Y61","v":50},{"$f":"'Run Selections'!AI61","v":""},{"$f":"'Run Selections'!AA61","v":0},null,{"$f":"'Run Selections'!AL61","v":""},{"$f":"IF(D61=\"Select Model\",\"N/A\",throwCombined(F61, D61, S61, E61,J61))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D61=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K61, M61, N61, O61),0))","v":"N/A"},{"$f":"IF(D61=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K61,M61,N61,P61)),0))","v":"N/A"},{"$f":"'Run Selections'!BD61","v":0},{"$f":"IF(LEFT($D61,4)<>\"ACBC\",\"N/A\",AdjacentZone($D61,$E61,$S61,$F61,60))","v":"N/A"},{"$f":"IF(LEFT($D61,4)<>\"ACBC\",\"N/A\",AdjacentZone($D61,$E61,$S61,$F61,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F62)=\"\",\"\",'Run Selections'!F62)","v":""},null,{"$f":"'Run Selections'!T62","v":"Select Model"},{"$f":"'Run Selections'!W62","v":4},{"$f":"'Run Selections'!Y62","v":50},{"$f":"'Run Selections'!AI62","v":""},{"$f":"'Run Selections'!AA62","v":0},null,{"$f":"'Run Selections'!AL62","v":""},{"$f":"IF(D62=\"Select Model\",\"N/A\",throwCombined(F62, D62, S62, E62,J62))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D62=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K62, M62, N62, O62),0))","v":"N/A"},{"$f":"IF(D62=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K62,M62,N62,P62)),0))","v":"N/A"},{"$f":"'Run Selections'!BD62","v":0},{"$f":"IF(LEFT($D62,4)<>\"ACBC\",\"N/A\",AdjacentZone($D62,$E62,$S62,$F62,60))","v":"N/A"},{"$f":"IF(LEFT($D62,4)<>\"ACBC\",\"N/A\",AdjacentZone($D62,$E62,$S62,$F62,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F63)=\"\",\"\",'Run Selections'!F63)","v":""},null,{"$f":"'Run Selections'!T63","v":"Select Model"},{"$f":"'Run Selections'!W63","v":4},{"$f":"'Run Selections'!Y63","v":50},{"$f":"'Run Selections'!AI63","v":""},{"$f":"'Run Selections'!AA63","v":0},null,{"$f":"'Run Selections'!AL63","v":""},{"$f":"IF(D63=\"Select Model\",\"N/A\",throwCombined(F63, D63, S63, E63,J63))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D63=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K63, M63, N63, O63),0))","v":"N/A"},{"$f":"IF(D63=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K63,M63,N63,P63)),0))","v":"N/A"},{"$f":"'Run Selections'!BD63","v":0},{"$f":"IF(LEFT($D63,4)<>\"ACBC\",\"N/A\",AdjacentZone($D63,$E63,$S63,$F63,60))","v":"N/A"},{"$f":"IF(LEFT($D63,4)<>\"ACBC\",\"N/A\",AdjacentZone($D63,$E63,$S63,$F63,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F64)=\"\",\"\",'Run Selections'!F64)","v":""},null,{"$f":"'Run Selections'!T64","v":"Select Model"},{"$f":"'Run Selections'!W64","v":4},{"$f":"'Run Selections'!Y64","v":50},{"$f":"'Run Selections'!AI64","v":""},{"$f":"'Run Selections'!AA64","v":0},null,{"$f":"'Run Selections'!AL64","v":""},{"$f":"IF(D64=\"Select Model\",\"N/A\",throwCombined(F64, D64, S64, E64,J64))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D64=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K64, M64, N64, O64),0))","v":"N/A"},{"$f":"IF(D64=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K64,M64,N64,P64)),0))","v":"N/A"},{"$f":"'Run Selections'!BD64","v":0},{"$f":"IF(LEFT($D64,4)<>\"ACBC\",\"N/A\",AdjacentZone($D64,$E64,$S64,$F64,60))","v":"N/A"},{"$f":"IF(LEFT($D64,4)<>\"ACBC\",\"N/A\",AdjacentZone($D64,$E64,$S64,$F64,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F65)=\"\",\"\",'Run Selections'!F65)","v":""},null,{"$f":"'Run Selections'!T65","v":"Select Model"},{"$f":"'Run Selections'!W65","v":4},{"$f":"'Run Selections'!Y65","v":50},{"$f":"'Run Selections'!AI65","v":""},{"$f":"'Run Selections'!AA65","v":0},null,{"$f":"'Run Selections'!AL65","v":""},{"$f":"IF(D65=\"Select Model\",\"N/A\",throwCombined(F65, D65, S65, E65,J65))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D65=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K65, M65, N65, O65),0))","v":"N/A"},{"$f":"IF(D65=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K65,M65,N65,P65)),0))","v":"N/A"},{"$f":"'Run Selections'!BD65","v":0},{"$f":"IF(LEFT($D65,4)<>\"ACBC\",\"N/A\",AdjacentZone($D65,$E65,$S65,$F65,60))","v":"N/A"},{"$f":"IF(LEFT($D65,4)<>\"ACBC\",\"N/A\",AdjacentZone($D65,$E65,$S65,$F65,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F66)=\"\",\"\",'Run Selections'!F66)","v":""},null,{"$f":"'Run Selections'!T66","v":"Select Model"},{"$f":"'Run Selections'!W66","v":4},{"$f":"'Run Selections'!Y66","v":50},{"$f":"'Run Selections'!AI66","v":""},{"$f":"'Run Selections'!AA66","v":0},null,{"$f":"'Run Selections'!AL66","v":""},{"$f":"IF(D66=\"Select Model\",\"N/A\",throwCombined(F66, D66, S66, E66,J66))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D66=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K66, M66, N66, O66),0))","v":"N/A"},{"$f":"IF(D66=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K66,M66,N66,P66)),0))","v":"N/A"},{"$f":"'Run Selections'!BD66","v":0},{"$f":"IF(LEFT($D66,4)<>\"ACBC\",\"N/A\",AdjacentZone($D66,$E66,$S66,$F66,60))","v":"N/A"},{"$f":"IF(LEFT($D66,4)<>\"ACBC\",\"N/A\",AdjacentZone($D66,$E66,$S66,$F66,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F67)=\"\",\"\",'Run Selections'!F67)","v":""},null,{"$f":"'Run Selections'!T67","v":"Select Model"},{"$f":"'Run Selections'!W67","v":4},{"$f":"'Run Selections'!Y67","v":50},{"$f":"'Run Selections'!AI67","v":""},{"$f":"'Run Selections'!AA67","v":0},null,{"$f":"'Run Selections'!AL67","v":""},{"$f":"IF(D67=\"Select Model\",\"N/A\",throwCombined(F67, D67, S67, E67,J67))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D67=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K67, M67, N67, O67),0))","v":"N/A"},{"$f":"IF(D67=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K67,M67,N67,P67)),0))","v":"N/A"},{"$f":"'Run Selections'!BD67","v":0},{"$f":"IF(LEFT($D67,4)<>\"ACBC\",\"N/A\",AdjacentZone($D67,$E67,$S67,$F67,60))","v":"N/A"},{"$f":"IF(LEFT($D67,4)<>\"ACBC\",\"N/A\",AdjacentZone($D67,$E67,$S67,$F67,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F68)=\"\",\"\",'Run Selections'!F68)","v":""},null,{"$f":"'Run Selections'!T68","v":"Select Model"},{"$f":"'Run Selections'!W68","v":4},{"$f":"'Run Selections'!Y68","v":50},{"$f":"'Run Selections'!AI68","v":""},{"$f":"'Run Selections'!AA68","v":0},null,{"$f":"'Run Selections'!AL68","v":""},{"$f":"IF(D68=\"Select Model\",\"N/A\",throwCombined(F68, D68, S68, E68,J68))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D68=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K68, M68, N68, O68),0))","v":"N/A"},{"$f":"IF(D68=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K68,M68,N68,P68)),0))","v":"N/A"},{"$f":"'Run Selections'!BD68","v":0},{"$f":"IF(LEFT($D68,4)<>\"ACBC\",\"N/A\",AdjacentZone($D68,$E68,$S68,$F68,60))","v":"N/A"},{"$f":"IF(LEFT($D68,4)<>\"ACBC\",\"N/A\",AdjacentZone($D68,$E68,$S68,$F68,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F69)=\"\",\"\",'Run Selections'!F69)","v":""},null,{"$f":"'Run Selections'!T69","v":"Select Model"},{"$f":"'Run Selections'!W69","v":4},{"$f":"'Run Selections'!Y69","v":50},{"$f":"'Run Selections'!AI69","v":""},{"$f":"'Run Selections'!AA69","v":0},null,{"$f":"'Run Selections'!AL69","v":""},{"$f":"IF(D69=\"Select Model\",\"N/A\",throwCombined(F69, D69, S69, E69,J69))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D69=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K69, M69, N69, O69),0))","v":"N/A"},{"$f":"IF(D69=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K69,M69,N69,P69)),0))","v":"N/A"},{"$f":"'Run Selections'!BD69","v":0},{"$f":"IF(LEFT($D69,4)<>\"ACBC\",\"N/A\",AdjacentZone($D69,$E69,$S69,$F69,60))","v":"N/A"},{"$f":"IF(LEFT($D69,4)<>\"ACBC\",\"N/A\",AdjacentZone($D69,$E69,$S69,$F69,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F70)=\"\",\"\",'Run Selections'!F70)","v":""},null,{"$f":"'Run Selections'!T70","v":"Select Model"},{"$f":"'Run Selections'!W70","v":4},{"$f":"'Run Selections'!Y70","v":50},{"$f":"'Run Selections'!AI70","v":""},{"$f":"'Run Selections'!AA70","v":0},null,{"$f":"'Run Selections'!AL70","v":""},{"$f":"IF(D70=\"Select Model\",\"N/A\",throwCombined(F70, D70, S70, E70,J70))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D70=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K70, M70, N70, O70),0))","v":"N/A"},{"$f":"IF(D70=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K70,M70,N70,P70)),0))","v":"N/A"},{"$f":"'Run Selections'!BD70","v":0},{"$f":"IF(LEFT($D70,4)<>\"ACBC\",\"N/A\",AdjacentZone($D70,$E70,$S70,$F70,60))","v":"N/A"},{"$f":"IF(LEFT($D70,4)<>\"ACBC\",\"N/A\",AdjacentZone($D70,$E70,$S70,$F70,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F71)=\"\",\"\",'Run Selections'!F71)","v":""},null,{"$f":"'Run Selections'!T71","v":"Select Model"},{"$f":"'Run Selections'!W71","v":4},{"$f":"'Run Selections'!Y71","v":50},{"$f":"'Run Selections'!AI71","v":""},{"$f":"'Run Selections'!AA71","v":0},null,{"$f":"'Run Selections'!AL71","v":""},{"$f":"IF(D71=\"Select Model\",\"N/A\",throwCombined(F71, D71, S71, E71,J71))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D71=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K71, M71, N71, O71),0))","v":"N/A"},{"$f":"IF(D71=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K71,M71,N71,P71)),0))","v":"N/A"},{"$f":"'Run Selections'!BD71","v":0},{"$f":"IF(LEFT($D71,4)<>\"ACBC\",\"N/A\",AdjacentZone($D71,$E71,$S71,$F71,60))","v":"N/A"},{"$f":"IF(LEFT($D71,4)<>\"ACBC\",\"N/A\",AdjacentZone($D71,$E71,$S71,$F71,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F72)=\"\",\"\",'Run Selections'!F72)","v":""},null,{"$f":"'Run Selections'!T72","v":"Select Model"},{"$f":"'Run Selections'!W72","v":4},{"$f":"'Run Selections'!Y72","v":50},{"$f":"'Run Selections'!AI72","v":""},{"$f":"'Run Selections'!AA72","v":0},null,{"$f":"'Run Selections'!AL72","v":""},{"$f":"IF(D72=\"Select Model\",\"N/A\",throwCombined(F72, D72, S72, E72,J72))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D72=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K72, M72, N72, O72),0))","v":"N/A"},{"$f":"IF(D72=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K72,M72,N72,P72)),0))","v":"N/A"},{"$f":"'Run Selections'!BD72","v":0},{"$f":"IF(LEFT($D72,4)<>\"ACBC\",\"N/A\",AdjacentZone($D72,$E72,$S72,$F72,60))","v":"N/A"},{"$f":"IF(LEFT($D72,4)<>\"ACBC\",\"N/A\",AdjacentZone($D72,$E72,$S72,$F72,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F73)=\"\",\"\",'Run Selections'!F73)","v":""},null,{"$f":"'Run Selections'!T73","v":"Select Model"},{"$f":"'Run Selections'!W73","v":4},{"$f":"'Run Selections'!Y73","v":50},{"$f":"'Run Selections'!AI73","v":""},{"$f":"'Run Selections'!AA73","v":0},null,{"$f":"'Run Selections'!AL73","v":""},{"$f":"IF(D73=\"Select Model\",\"N/A\",throwCombined(F73, D73, S73, E73,J73))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D73=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K73, M73, N73, O73),0))","v":"N/A"},{"$f":"IF(D73=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K73,M73,N73,P73)),0))","v":"N/A"},{"$f":"'Run Selections'!BD73","v":0},{"$f":"IF(LEFT($D73,4)<>\"ACBC\",\"N/A\",AdjacentZone($D73,$E73,$S73,$F73,60))","v":"N/A"},{"$f":"IF(LEFT($D73,4)<>\"ACBC\",\"N/A\",AdjacentZone($D73,$E73,$S73,$F73,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F74)=\"\",\"\",'Run Selections'!F74)","v":""},null,{"$f":"'Run Selections'!T74","v":"Select Model"},{"$f":"'Run Selections'!W74","v":4},{"$f":"'Run Selections'!Y74","v":50},{"$f":"'Run Selections'!AI74","v":""},{"$f":"'Run Selections'!AA74","v":0},null,{"$f":"'Run Selections'!AL74","v":""},{"$f":"IF(D74=\"Select Model\",\"N/A\",throwCombined(F74, D74, S74, E74,J74))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D74=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K74, M74, N74, O74),0))","v":"N/A"},{"$f":"IF(D74=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K74,M74,N74,P74)),0))","v":"N/A"},{"$f":"'Run Selections'!BD74","v":0},{"$f":"IF(LEFT($D74,4)<>\"ACBC\",\"N/A\",AdjacentZone($D74,$E74,$S74,$F74,60))","v":"N/A"},{"$f":"IF(LEFT($D74,4)<>\"ACBC\",\"N/A\",AdjacentZone($D74,$E74,$S74,$F74,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F75)=\"\",\"\",'Run Selections'!F75)","v":""},null,{"$f":"'Run Selections'!T75","v":"Select Model"},{"$f":"'Run Selections'!W75","v":4},{"$f":"'Run Selections'!Y75","v":50},{"$f":"'Run Selections'!AI75","v":""},{"$f":"'Run Selections'!AA75","v":0},null,{"$f":"'Run Selections'!AL75","v":""},{"$f":"IF(D75=\"Select Model\",\"N/A\",throwCombined(F75, D75, S75, E75,J75))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D75=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K75, M75, N75, O75),0))","v":"N/A"},{"$f":"IF(D75=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K75,M75,N75,P75)),0))","v":"N/A"},{"$f":"'Run Selections'!BD75","v":0},{"$f":"IF(LEFT($D75,4)<>\"ACBC\",\"N/A\",AdjacentZone($D75,$E75,$S75,$F75,60))","v":"N/A"},{"$f":"IF(LEFT($D75,4)<>\"ACBC\",\"N/A\",AdjacentZone($D75,$E75,$S75,$F75,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F76)=\"\",\"\",'Run Selections'!F76)","v":""},null,{"$f":"'Run Selections'!T76","v":"Select Model"},{"$f":"'Run Selections'!W76","v":4},{"$f":"'Run Selections'!Y76","v":50},{"$f":"'Run Selections'!AI76","v":""},{"$f":"'Run Selections'!AA76","v":0},null,{"$f":"'Run Selections'!AL76","v":""},{"$f":"IF(D76=\"Select Model\",\"N/A\",throwCombined(F76, D76, S76, E76,J76))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D76=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K76, M76, N76, O76),0))","v":"N/A"},{"$f":"IF(D76=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K76,M76,N76,P76)),0))","v":"N/A"},{"$f":"'Run Selections'!BD76","v":0},{"$f":"IF(LEFT($D76,4)<>\"ACBC\",\"N/A\",AdjacentZone($D76,$E76,$S76,$F76,60))","v":"N/A"},{"$f":"IF(LEFT($D76,4)<>\"ACBC\",\"N/A\",AdjacentZone($D76,$E76,$S76,$F76,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F77)=\"\",\"\",'Run Selections'!F77)","v":""},null,{"$f":"'Run Selections'!T77","v":"Select Model"},{"$f":"'Run Selections'!W77","v":4},{"$f":"'Run Selections'!Y77","v":50},{"$f":"'Run Selections'!AI77","v":""},{"$f":"'Run Selections'!AA77","v":0},null,{"$f":"'Run Selections'!AL77","v":""},{"$f":"IF(D77=\"Select Model\",\"N/A\",throwCombined(F77, D77, S77, E77,J77))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D77=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K77, M77, N77, O77),0))","v":"N/A"},{"$f":"IF(D77=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K77,M77,N77,P77)),0))","v":"N/A"},{"$f":"'Run Selections'!BD77","v":0},{"$f":"IF(LEFT($D77,4)<>\"ACBC\",\"N/A\",AdjacentZone($D77,$E77,$S77,$F77,60))","v":"N/A"},{"$f":"IF(LEFT($D77,4)<>\"ACBC\",\"N/A\",AdjacentZone($D77,$E77,$S77,$F77,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F78)=\"\",\"\",'Run Selections'!F78)","v":""},null,{"$f":"'Run Selections'!T78","v":"Select Model"},{"$f":"'Run Selections'!W78","v":4},{"$f":"'Run Selections'!Y78","v":50},{"$f":"'Run Selections'!AI78","v":""},{"$f":"'Run Selections'!AA78","v":0},null,{"$f":"'Run Selections'!AL78","v":""},{"$f":"IF(D78=\"Select Model\",\"N/A\",throwCombined(F78, D78, S78, E78,J78))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D78=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K78, M78, N78, O78),0))","v":"N/A"},{"$f":"IF(D78=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K78,M78,N78,P78)),0))","v":"N/A"},{"$f":"'Run Selections'!BD78","v":0},{"$f":"IF(LEFT($D78,4)<>\"ACBC\",\"N/A\",AdjacentZone($D78,$E78,$S78,$F78,60))","v":"N/A"},{"$f":"IF(LEFT($D78,4)<>\"ACBC\",\"N/A\",AdjacentZone($D78,$E78,$S78,$F78,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F79)=\"\",\"\",'Run Selections'!F79)","v":""},null,{"$f":"'Run Selections'!T79","v":"Select Model"},{"$f":"'Run Selections'!W79","v":4},{"$f":"'Run Selections'!Y79","v":50},{"$f":"'Run Selections'!AI79","v":""},{"$f":"'Run Selections'!AA79","v":0},null,{"$f":"'Run Selections'!AL79","v":""},{"$f":"IF(D79=\"Select Model\",\"N/A\",throwCombined(F79, D79, S79, E79,J79))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D79=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K79, M79, N79, O79),0))","v":"N/A"},{"$f":"IF(D79=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K79,M79,N79,P79)),0))","v":"N/A"},{"$f":"'Run Selections'!BD79","v":0},{"$f":"IF(LEFT($D79,4)<>\"ACBC\",\"N/A\",AdjacentZone($D79,$E79,$S79,$F79,60))","v":"N/A"},{"$f":"IF(LEFT($D79,4)<>\"ACBC\",\"N/A\",AdjacentZone($D79,$E79,$S79,$F79,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F80)=\"\",\"\",'Run Selections'!F80)","v":""},null,{"$f":"'Run Selections'!T80","v":"Select Model"},{"$f":"'Run Selections'!W80","v":4},{"$f":"'Run Selections'!Y80","v":50},{"$f":"'Run Selections'!AI80","v":""},{"$f":"'Run Selections'!AA80","v":0},null,{"$f":"'Run Selections'!AL80","v":""},{"$f":"IF(D80=\"Select Model\",\"N/A\",throwCombined(F80, D80, S80, E80,J80))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D80=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K80, M80, N80, O80),0))","v":"N/A"},{"$f":"IF(D80=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K80,M80,N80,P80)),0))","v":"N/A"},{"$f":"'Run Selections'!BD80","v":0},{"$f":"IF(LEFT($D80,4)<>\"ACBC\",\"N/A\",AdjacentZone($D80,$E80,$S80,$F80,60))","v":"N/A"},{"$f":"IF(LEFT($D80,4)<>\"ACBC\",\"N/A\",AdjacentZone($D80,$E80,$S80,$F80,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F81)=\"\",\"\",'Run Selections'!F81)","v":""},null,{"$f":"'Run Selections'!T81","v":"Select Model"},{"$f":"'Run Selections'!W81","v":4},{"$f":"'Run Selections'!Y81","v":50},{"$f":"'Run Selections'!AI81","v":""},{"$f":"'Run Selections'!AA81","v":0},null,{"$f":"'Run Selections'!AL81","v":""},{"$f":"IF(D81=\"Select Model\",\"N/A\",throwCombined(F81, D81, S81, E81,J81))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D81=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K81, M81, N81, O81),0))","v":"N/A"},{"$f":"IF(D81=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K81,M81,N81,P81)),0))","v":"N/A"},{"$f":"'Run Selections'!BD81","v":0},{"$f":"IF(LEFT($D81,4)<>\"ACBC\",\"N/A\",AdjacentZone($D81,$E81,$S81,$F81,60))","v":"N/A"},{"$f":"IF(LEFT($D81,4)<>\"ACBC\",\"N/A\",AdjacentZone($D81,$E81,$S81,$F81,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F82)=\"\",\"\",'Run Selections'!F82)","v":""},null,{"$f":"'Run Selections'!T82","v":"Select Model"},{"$f":"'Run Selections'!W82","v":4},{"$f":"'Run Selections'!Y82","v":50},{"$f":"'Run Selections'!AI82","v":""},{"$f":"'Run Selections'!AA82","v":0},null,{"$f":"'Run Selections'!AL82","v":""},{"$f":"IF(D82=\"Select Model\",\"N/A\",throwCombined(F82, D82, S82, E82,J82))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D82=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K82, M82, N82, O82),0))","v":"N/A"},{"$f":"IF(D82=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K82,M82,N82,P82)),0))","v":"N/A"},{"$f":"'Run Selections'!BD82","v":0},{"$f":"IF(LEFT($D82,4)<>\"ACBC\",\"N/A\",AdjacentZone($D82,$E82,$S82,$F82,60))","v":"N/A"},{"$f":"IF(LEFT($D82,4)<>\"ACBC\",\"N/A\",AdjacentZone($D82,$E82,$S82,$F82,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F83)=\"\",\"\",'Run Selections'!F83)","v":""},null,{"$f":"'Run Selections'!T83","v":"Select Model"},{"$f":"'Run Selections'!W83","v":4},{"$f":"'Run Selections'!Y83","v":50},{"$f":"'Run Selections'!AI83","v":""},{"$f":"'Run Selections'!AA83","v":0},null,{"$f":"'Run Selections'!AL83","v":""},{"$f":"IF(D83=\"Select Model\",\"N/A\",throwCombined(F83, D83, S83, E83,J83))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D83=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K83, M83, N83, O83),0))","v":"N/A"},{"$f":"IF(D83=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K83,M83,N83,P83)),0))","v":"N/A"},{"$f":"'Run Selections'!BD83","v":0},{"$f":"IF(LEFT($D83,4)<>\"ACBC\",\"N/A\",AdjacentZone($D83,$E83,$S83,$F83,60))","v":"N/A"},{"$f":"IF(LEFT($D83,4)<>\"ACBC\",\"N/A\",AdjacentZone($D83,$E83,$S83,$F83,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F84)=\"\",\"\",'Run Selections'!F84)","v":""},null,{"$f":"'Run Selections'!T84","v":"Select Model"},{"$f":"'Run Selections'!W84","v":4},{"$f":"'Run Selections'!Y84","v":50},{"$f":"'Run Selections'!AI84","v":""},{"$f":"'Run Selections'!AA84","v":0},null,{"$f":"'Run Selections'!AL84","v":""},{"$f":"IF(D84=\"Select Model\",\"N/A\",throwCombined(F84, D84, S84, E84,J84))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D84=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K84, M84, N84, O84),0))","v":"N/A"},{"$f":"IF(D84=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K84,M84,N84,P84)),0))","v":"N/A"},{"$f":"'Run Selections'!BD84","v":0},{"$f":"IF(LEFT($D84,4)<>\"ACBC\",\"N/A\",AdjacentZone($D84,$E84,$S84,$F84,60))","v":"N/A"},{"$f":"IF(LEFT($D84,4)<>\"ACBC\",\"N/A\",AdjacentZone($D84,$E84,$S84,$F84,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F85)=\"\",\"\",'Run Selections'!F85)","v":""},null,{"$f":"'Run Selections'!T85","v":"Select Model"},{"$f":"'Run Selections'!W85","v":4},{"$f":"'Run Selections'!Y85","v":50},{"$f":"'Run Selections'!AI85","v":""},{"$f":"'Run Selections'!AA85","v":0},null,{"$f":"'Run Selections'!AL85","v":""},{"$f":"IF(D85=\"Select Model\",\"N/A\",throwCombined(F85, D85, S85, E85,J85))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D85=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K85, M85, N85, O85),0))","v":"N/A"},{"$f":"IF(D85=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K85,M85,N85,P85)),0))","v":"N/A"},{"$f":"'Run Selections'!BD85","v":0},{"$f":"IF(LEFT($D85,4)<>\"ACBC\",\"N/A\",AdjacentZone($D85,$E85,$S85,$F85,60))","v":"N/A"},{"$f":"IF(LEFT($D85,4)<>\"ACBC\",\"N/A\",AdjacentZone($D85,$E85,$S85,$F85,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F86)=\"\",\"\",'Run Selections'!F86)","v":""},null,{"$f":"'Run Selections'!T86","v":"Select Model"},{"$f":"'Run Selections'!W86","v":4},{"$f":"'Run Selections'!Y86","v":50},{"$f":"'Run Selections'!AI86","v":""},{"$f":"'Run Selections'!AA86","v":0},null,{"$f":"'Run Selections'!AL86","v":""},{"$f":"IF(D86=\"Select Model\",\"N/A\",throwCombined(F86, D86, S86, E86,J86))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D86=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K86, M86, N86, O86),0))","v":"N/A"},{"$f":"IF(D86=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K86,M86,N86,P86)),0))","v":"N/A"},{"$f":"'Run Selections'!BD86","v":0},{"$f":"IF(LEFT($D86,4)<>\"ACBC\",\"N/A\",AdjacentZone($D86,$E86,$S86,$F86,60))","v":"N/A"},{"$f":"IF(LEFT($D86,4)<>\"ACBC\",\"N/A\",AdjacentZone($D86,$E86,$S86,$F86,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F87)=\"\",\"\",'Run Selections'!F87)","v":""},null,{"$f":"'Run Selections'!T87","v":"Select Model"},{"$f":"'Run Selections'!W87","v":4},{"$f":"'Run Selections'!Y87","v":50},{"$f":"'Run Selections'!AI87","v":""},{"$f":"'Run Selections'!AA87","v":0},null,{"$f":"'Run Selections'!AL87","v":""},{"$f":"IF(D87=\"Select Model\",\"N/A\",throwCombined(F87, D87, S87, E87,J87))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D87=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K87, M87, N87, O87),0))","v":"N/A"},{"$f":"IF(D87=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K87,M87,N87,P87)),0))","v":"N/A"},{"$f":"'Run Selections'!BD87","v":0},{"$f":"IF(LEFT($D87,4)<>\"ACBC\",\"N/A\",AdjacentZone($D87,$E87,$S87,$F87,60))","v":"N/A"},{"$f":"IF(LEFT($D87,4)<>\"ACBC\",\"N/A\",AdjacentZone($D87,$E87,$S87,$F87,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F88)=\"\",\"\",'Run Selections'!F88)","v":""},null,{"$f":"'Run Selections'!T88","v":"Select Model"},{"$f":"'Run Selections'!W88","v":4},{"$f":"'Run Selections'!Y88","v":50},{"$f":"'Run Selections'!AI88","v":""},{"$f":"'Run Selections'!AA88","v":0},null,{"$f":"'Run Selections'!AL88","v":""},{"$f":"IF(D88=\"Select Model\",\"N/A\",throwCombined(F88, D88, S88, E88,J88))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D88=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K88, M88, N88, O88),0))","v":"N/A"},{"$f":"IF(D88=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K88,M88,N88,P88)),0))","v":"N/A"},{"$f":"'Run Selections'!BD88","v":0},{"$f":"IF(LEFT($D88,4)<>\"ACBC\",\"N/A\",AdjacentZone($D88,$E88,$S88,$F88,60))","v":"N/A"},{"$f":"IF(LEFT($D88,4)<>\"ACBC\",\"N/A\",AdjacentZone($D88,$E88,$S88,$F88,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F89)=\"\",\"\",'Run Selections'!F89)","v":""},null,{"$f":"'Run Selections'!T89","v":"Select Model"},{"$f":"'Run Selections'!W89","v":4},{"$f":"'Run Selections'!Y89","v":50},{"$f":"'Run Selections'!AI89","v":""},{"$f":"'Run Selections'!AA89","v":0},null,{"$f":"'Run Selections'!AL89","v":""},{"$f":"IF(D89=\"Select Model\",\"N/A\",throwCombined(F89, D89, S89, E89,J89))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D89=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K89, M89, N89, O89),0))","v":"N/A"},{"$f":"IF(D89=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K89,M89,N89,P89)),0))","v":"N/A"},{"$f":"'Run Selections'!BD89","v":0},{"$f":"IF(LEFT($D89,4)<>\"ACBC\",\"N/A\",AdjacentZone($D89,$E89,$S89,$F89,60))","v":"N/A"},{"$f":"IF(LEFT($D89,4)<>\"ACBC\",\"N/A\",AdjacentZone($D89,$E89,$S89,$F89,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F90)=\"\",\"\",'Run Selections'!F90)","v":""},null,{"$f":"'Run Selections'!T90","v":"Select Model"},{"$f":"'Run Selections'!W90","v":4},{"$f":"'Run Selections'!Y90","v":50},{"$f":"'Run Selections'!AI90","v":""},{"$f":"'Run Selections'!AA90","v":0},null,{"$f":"'Run Selections'!AL90","v":""},{"$f":"IF(D90=\"Select Model\",\"N/A\",throwCombined(F90, D90, S90, E90,J90))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D90=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K90, M90, N90, O90),0))","v":"N/A"},{"$f":"IF(D90=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K90,M90,N90,P90)),0))","v":"N/A"},{"$f":"'Run Selections'!BD90","v":0},{"$f":"IF(LEFT($D90,4)<>\"ACBC\",\"N/A\",AdjacentZone($D90,$E90,$S90,$F90,60))","v":"N/A"},{"$f":"IF(LEFT($D90,4)<>\"ACBC\",\"N/A\",AdjacentZone($D90,$E90,$S90,$F90,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F91)=\"\",\"\",'Run Selections'!F91)","v":""},null,{"$f":"'Run Selections'!T91","v":"Select Model"},{"$f":"'Run Selections'!W91","v":4},{"$f":"'Run Selections'!Y91","v":50},{"$f":"'Run Selections'!AI91","v":""},{"$f":"'Run Selections'!AA91","v":0},null,{"$f":"'Run Selections'!AL91","v":""},{"$f":"IF(D91=\"Select Model\",\"N/A\",throwCombined(F91, D91, S91, E91,J91))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D91=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K91, M91, N91, O91),0))","v":"N/A"},{"$f":"IF(D91=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K91,M91,N91,P91)),0))","v":"N/A"},{"$f":"'Run Selections'!BD91","v":0},{"$f":"IF(LEFT($D91,4)<>\"ACBC\",\"N/A\",AdjacentZone($D91,$E91,$S91,$F91,60))","v":"N/A"},{"$f":"IF(LEFT($D91,4)<>\"ACBC\",\"N/A\",AdjacentZone($D91,$E91,$S91,$F91,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F92)=\"\",\"\",'Run Selections'!F92)","v":""},null,{"$f":"'Run Selections'!T92","v":"Select Model"},{"$f":"'Run Selections'!W92","v":4},{"$f":"'Run Selections'!Y92","v":50},{"$f":"'Run Selections'!AI92","v":""},{"$f":"'Run Selections'!AA92","v":0},null,{"$f":"'Run Selections'!AL92","v":""},{"$f":"IF(D92=\"Select Model\",\"N/A\",throwCombined(F92, D92, S92, E92,J92))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D92=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K92, M92, N92, O92),0))","v":"N/A"},{"$f":"IF(D92=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K92,M92,N92,P92)),0))","v":"N/A"},{"$f":"'Run Selections'!BD92","v":0},{"$f":"IF(LEFT($D92,4)<>\"ACBC\",\"N/A\",AdjacentZone($D92,$E92,$S92,$F92,60))","v":"N/A"},{"$f":"IF(LEFT($D92,4)<>\"ACBC\",\"N/A\",AdjacentZone($D92,$E92,$S92,$F92,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F93)=\"\",\"\",'Run Selections'!F93)","v":""},null,{"$f":"'Run Selections'!T93","v":"Select Model"},{"$f":"'Run Selections'!W93","v":4},{"$f":"'Run Selections'!Y93","v":50},{"$f":"'Run Selections'!AI93","v":""},{"$f":"'Run Selections'!AA93","v":0},null,{"$f":"'Run Selections'!AL93","v":""},{"$f":"IF(D93=\"Select Model\",\"N/A\",throwCombined(F93, D93, S93, E93,J93))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D93=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K93, M93, N93, O93),0))","v":"N/A"},{"$f":"IF(D93=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K93,M93,N93,P93)),0))","v":"N/A"},{"$f":"'Run Selections'!BD93","v":0},{"$f":"IF(LEFT($D93,4)<>\"ACBC\",\"N/A\",AdjacentZone($D93,$E93,$S93,$F93,60))","v":"N/A"},{"$f":"IF(LEFT($D93,4)<>\"ACBC\",\"N/A\",AdjacentZone($D93,$E93,$S93,$F93,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F94)=\"\",\"\",'Run Selections'!F94)","v":""},null,{"$f":"'Run Selections'!T94","v":"Select Model"},{"$f":"'Run Selections'!W94","v":4},{"$f":"'Run Selections'!Y94","v":50},{"$f":"'Run Selections'!AI94","v":""},{"$f":"'Run Selections'!AA94","v":0},null,{"$f":"'Run Selections'!AL94","v":""},{"$f":"IF(D94=\"Select Model\",\"N/A\",throwCombined(F94, D94, S94, E94,J94))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D94=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K94, M94, N94, O94),0))","v":"N/A"},{"$f":"IF(D94=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K94,M94,N94,P94)),0))","v":"N/A"},{"$f":"'Run Selections'!BD94","v":0},{"$f":"IF(LEFT($D94,4)<>\"ACBC\",\"N/A\",AdjacentZone($D94,$E94,$S94,$F94,60))","v":"N/A"},{"$f":"IF(LEFT($D94,4)<>\"ACBC\",\"N/A\",AdjacentZone($D94,$E94,$S94,$F94,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F95)=\"\",\"\",'Run Selections'!F95)","v":""},null,{"$f":"'Run Selections'!T95","v":"Select Model"},{"$f":"'Run Selections'!W95","v":4},{"$f":"'Run Selections'!Y95","v":50},{"$f":"'Run Selections'!AI95","v":""},{"$f":"'Run Selections'!AA95","v":0},null,{"$f":"'Run Selections'!AL95","v":""},{"$f":"IF(D95=\"Select Model\",\"N/A\",throwCombined(F95, D95, S95, E95,J95))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D95=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K95, M95, N95, O95),0))","v":"N/A"},{"$f":"IF(D95=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K95,M95,N95,P95)),0))","v":"N/A"},{"$f":"'Run Selections'!BD95","v":0},{"$f":"IF(LEFT($D95,4)<>\"ACBC\",\"N/A\",AdjacentZone($D95,$E95,$S95,$F95,60))","v":"N/A"},{"$f":"IF(LEFT($D95,4)<>\"ACBC\",\"N/A\",AdjacentZone($D95,$E95,$S95,$F95,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F96)=\"\",\"\",'Run Selections'!F96)","v":""},null,{"$f":"'Run Selections'!T96","v":"Select Model"},{"$f":"'Run Selections'!W96","v":4},{"$f":"'Run Selections'!Y96","v":50},{"$f":"'Run Selections'!AI96","v":""},{"$f":"'Run Selections'!AA96","v":0},null,{"$f":"'Run Selections'!AL96","v":""},{"$f":"IF(D96=\"Select Model\",\"N/A\",throwCombined(F96, D96, S96, E96,J96))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D96=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K96, M96, N96, O96),0))","v":"N/A"},{"$f":"IF(D96=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K96,M96,N96,P96)),0))","v":"N/A"},{"$f":"'Run Selections'!BD96","v":0},{"$f":"IF(LEFT($D96,4)<>\"ACBC\",\"N/A\",AdjacentZone($D96,$E96,$S96,$F96,60))","v":"N/A"},{"$f":"IF(LEFT($D96,4)<>\"ACBC\",\"N/A\",AdjacentZone($D96,$E96,$S96,$F96,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F97)=\"\",\"\",'Run Selections'!F97)","v":""},null,{"$f":"'Run Selections'!T97","v":"Select Model"},{"$f":"'Run Selections'!W97","v":4},{"$f":"'Run Selections'!Y97","v":50},{"$f":"'Run Selections'!AI97","v":""},{"$f":"'Run Selections'!AA97","v":0},null,{"$f":"'Run Selections'!AL97","v":""},{"$f":"IF(D97=\"Select Model\",\"N/A\",throwCombined(F97, D97, S97, E97,J97))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D97=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K97, M97, N97, O97),0))","v":"N/A"},{"$f":"IF(D97=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K97,M97,N97,P97)),0))","v":"N/A"},{"$f":"'Run Selections'!BD97","v":0},{"$f":"IF(LEFT($D97,4)<>\"ACBC\",\"N/A\",AdjacentZone($D97,$E97,$S97,$F97,60))","v":"N/A"},{"$f":"IF(LEFT($D97,4)<>\"ACBC\",\"N/A\",AdjacentZone($D97,$E97,$S97,$F97,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F98)=\"\",\"\",'Run Selections'!F98)","v":""},null,{"$f":"'Run Selections'!T98","v":"Select Model"},{"$f":"'Run Selections'!W98","v":4},{"$f":"'Run Selections'!Y98","v":50},{"$f":"'Run Selections'!AI98","v":""},{"$f":"'Run Selections'!AA98","v":0},null,{"$f":"'Run Selections'!AL98","v":""},{"$f":"IF(D98=\"Select Model\",\"N/A\",throwCombined(F98, D98, S98, E98,J98))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D98=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K98, M98, N98, O98),0))","v":"N/A"},{"$f":"IF(D98=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K98,M98,N98,P98)),0))","v":"N/A"},{"$f":"'Run Selections'!BD98","v":0},{"$f":"IF(LEFT($D98,4)<>\"ACBC\",\"N/A\",AdjacentZone($D98,$E98,$S98,$F98,60))","v":"N/A"},{"$f":"IF(LEFT($D98,4)<>\"ACBC\",\"N/A\",AdjacentZone($D98,$E98,$S98,$F98,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F99)=\"\",\"\",'Run Selections'!F99)","v":""},null,{"$f":"'Run Selections'!T99","v":"Select Model"},{"$f":"'Run Selections'!W99","v":4},{"$f":"'Run Selections'!Y99","v":50},{"$f":"'Run Selections'!AI99","v":""},{"$f":"'Run Selections'!AA99","v":0},null,{"$f":"'Run Selections'!AL99","v":""},{"$f":"IF(D99=\"Select Model\",\"N/A\",throwCombined(F99, D99, S99, E99,J99))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D99=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K99, M99, N99, O99),0))","v":"N/A"},{"$f":"IF(D99=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K99,M99,N99,P99)),0))","v":"N/A"},{"$f":"'Run Selections'!BD99","v":0},{"$f":"IF(LEFT($D99,4)<>\"ACBC\",\"N/A\",AdjacentZone($D99,$E99,$S99,$F99,60))","v":"N/A"},{"$f":"IF(LEFT($D99,4)<>\"ACBC\",\"N/A\",AdjacentZone($D99,$E99,$S99,$F99,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F100)=\"\",\"\",'Run Selections'!F100)","v":""},null,{"$f":"'Run Selections'!T100","v":"Select Model"},{"$f":"'Run Selections'!W100","v":4},{"$f":"'Run Selections'!Y100","v":50},{"$f":"'Run Selections'!AI100","v":""},{"$f":"'Run Selections'!AA100","v":0},null,{"$f":"'Run Selections'!AL100","v":""},{"$f":"IF(D100=\"Select Model\",\"N/A\",throwCombined(F100, D100, S100, E100,J100))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D100=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K100, M100, N100, O100),0))","v":"N/A"},{"$f":"IF(D100=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K100,M100,N100,P100)),0))","v":"N/A"},{"$f":"'Run Selections'!BD100","v":0},{"$f":"IF(LEFT($D100,4)<>\"ACBC\",\"N/A\",AdjacentZone($D100,$E100,$S100,$F100,60))","v":"N/A"},{"$f":"IF(LEFT($D100,4)<>\"ACBC\",\"N/A\",AdjacentZone($D100,$E100,$S100,$F100,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F101)=\"\",\"\",'Run Selections'!F101)","v":""},null,{"$f":"'Run Selections'!T101","v":"Select Model"},{"$f":"'Run Selections'!W101","v":4},{"$f":"'Run Selections'!Y101","v":50},{"$f":"'Run Selections'!AI101","v":""},{"$f":"'Run Selections'!AA101","v":0},null,{"$f":"'Run Selections'!AL101","v":""},{"$f":"IF(D101=\"Select Model\",\"N/A\",throwCombined(F101, D101, S101, E101,J101))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D101=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K101, M101, N101, O101),0))","v":"N/A"},{"$f":"IF(D101=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K101,M101,N101,P101)),0))","v":"N/A"},{"$f":"'Run Selections'!BD101","v":0},{"$f":"IF(LEFT($D101,4)<>\"ACBC\",\"N/A\",AdjacentZone($D101,$E101,$S101,$F101,60))","v":"N/A"},{"$f":"IF(LEFT($D101,4)<>\"ACBC\",\"N/A\",AdjacentZone($D101,$E101,$S101,$F101,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F102)=\"\",\"\",'Run Selections'!F102)","v":""},null,{"$f":"'Run Selections'!T102","v":"Select Model"},{"$f":"'Run Selections'!W102","v":4},{"$f":"'Run Selections'!Y102","v":50},{"$f":"'Run Selections'!AI102","v":""},{"$f":"'Run Selections'!AA102","v":0},null,{"$f":"'Run Selections'!AL102","v":""},{"$f":"IF(D102=\"Select Model\",\"N/A\",throwCombined(F102, D102, S102, E102,J102))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D102=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K102, M102, N102, O102),0))","v":"N/A"},{"$f":"IF(D102=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K102,M102,N102,P102)),0))","v":"N/A"},{"$f":"'Run Selections'!BD102","v":0},{"$f":"IF(LEFT($D102,4)<>\"ACBC\",\"N/A\",AdjacentZone($D102,$E102,$S102,$F102,60))","v":"N/A"},{"$f":"IF(LEFT($D102,4)<>\"ACBC\",\"N/A\",AdjacentZone($D102,$E102,$S102,$F102,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F103)=\"\",\"\",'Run Selections'!F103)","v":""},null,{"$f":"'Run Selections'!T103","v":"Select Model"},{"$f":"'Run Selections'!W103","v":4},{"$f":"'Run Selections'!Y103","v":50},{"$f":"'Run Selections'!AI103","v":""},{"$f":"'Run Selections'!AA103","v":0},null,{"$f":"'Run Selections'!AL103","v":""},{"$f":"IF(D103=\"Select Model\",\"N/A\",throwCombined(F103, D103, S103, E103,J103))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D103=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K103, M103, N103, O103),0))","v":"N/A"},{"$f":"IF(D103=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K103,M103,N103,P103)),0))","v":"N/A"},{"$f":"'Run Selections'!BD103","v":0},{"$f":"IF(LEFT($D103,4)<>\"ACBC\",\"N/A\",AdjacentZone($D103,$E103,$S103,$F103,60))","v":"N/A"},{"$f":"IF(LEFT($D103,4)<>\"ACBC\",\"N/A\",AdjacentZone($D103,$E103,$S103,$F103,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F104)=\"\",\"\",'Run Selections'!F104)","v":""},null,{"$f":"'Run Selections'!T104","v":"Select Model"},{"$f":"'Run Selections'!W104","v":4},{"$f":"'Run Selections'!Y104","v":50},{"$f":"'Run Selections'!AI104","v":""},{"$f":"'Run Selections'!AA104","v":0},null,{"$f":"'Run Selections'!AL104","v":""},{"$f":"IF(D104=\"Select Model\",\"N/A\",throwCombined(F104, D104, S104, E104,J104))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D104=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K104, M104, N104, O104),0))","v":"N/A"},{"$f":"IF(D104=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K104,M104,N104,P104)),0))","v":"N/A"},{"$f":"'Run Selections'!BD104","v":0},{"$f":"IF(LEFT($D104,4)<>\"ACBC\",\"N/A\",AdjacentZone($D104,$E104,$S104,$F104,60))","v":"N/A"},{"$f":"IF(LEFT($D104,4)<>\"ACBC\",\"N/A\",AdjacentZone($D104,$E104,$S104,$F104,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F105)=\"\",\"\",'Run Selections'!F105)","v":""},null,{"$f":"'Run Selections'!T105","v":"Select Model"},{"$f":"'Run Selections'!W105","v":4},{"$f":"'Run Selections'!Y105","v":50},{"$f":"'Run Selections'!AI105","v":""},{"$f":"'Run Selections'!AA105","v":0},null,{"$f":"'Run Selections'!AL105","v":""},{"$f":"IF(D105=\"Select Model\",\"N/A\",throwCombined(F105, D105, S105, E105,J105))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D105=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K105, M105, N105, O105),0))","v":"N/A"},{"$f":"IF(D105=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K105,M105,N105,P105)),0))","v":"N/A"},{"$f":"'Run Selections'!BD105","v":0},{"$f":"IF(LEFT($D105,4)<>\"ACBC\",\"N/A\",AdjacentZone($D105,$E105,$S105,$F105,60))","v":"N/A"},{"$f":"IF(LEFT($D105,4)<>\"ACBC\",\"N/A\",AdjacentZone($D105,$E105,$S105,$F105,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F106)=\"\",\"\",'Run Selections'!F106)","v":""},null,{"$f":"'Run Selections'!T106","v":"Select Model"},{"$f":"'Run Selections'!W106","v":4},{"$f":"'Run Selections'!Y106","v":50},{"$f":"'Run Selections'!AI106","v":""},{"$f":"'Run Selections'!AA106","v":0},null,{"$f":"'Run Selections'!AL106","v":""},{"$f":"IF(D106=\"Select Model\",\"N/A\",throwCombined(F106, D106, S106, E106,J106))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D106=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K106, M106, N106, O106),0))","v":"N/A"},{"$f":"IF(D106=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K106,M106,N106,P106)),0))","v":"N/A"},{"$f":"'Run Selections'!BD106","v":0},{"$f":"IF(LEFT($D106,4)<>\"ACBC\",\"N/A\",AdjacentZone($D106,$E106,$S106,$F106,60))","v":"N/A"},{"$f":"IF(LEFT($D106,4)<>\"ACBC\",\"N/A\",AdjacentZone($D106,$E106,$S106,$F106,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F107)=\"\",\"\",'Run Selections'!F107)","v":""},null,{"$f":"'Run Selections'!T107","v":"Select Model"},{"$f":"'Run Selections'!W107","v":4},{"$f":"'Run Selections'!Y107","v":50},{"$f":"'Run Selections'!AI107","v":""},{"$f":"'Run Selections'!AA107","v":0},null,{"$f":"'Run Selections'!AL107","v":""},{"$f":"IF(D107=\"Select Model\",\"N/A\",throwCombined(F107, D107, S107, E107,J107))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D107=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K107, M107, N107, O107),0))","v":"N/A"},{"$f":"IF(D107=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K107,M107,N107,P107)),0))","v":"N/A"},{"$f":"'Run Selections'!BD107","v":0},{"$f":"IF(LEFT($D107,4)<>\"ACBC\",\"N/A\",AdjacentZone($D107,$E107,$S107,$F107,60))","v":"N/A"},{"$f":"IF(LEFT($D107,4)<>\"ACBC\",\"N/A\",AdjacentZone($D107,$E107,$S107,$F107,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F108)=\"\",\"\",'Run Selections'!F108)","v":""},null,{"$f":"'Run Selections'!T108","v":"Select Model"},{"$f":"'Run Selections'!W108","v":4},{"$f":"'Run Selections'!Y108","v":50},{"$f":"'Run Selections'!AI108","v":""},{"$f":"'Run Selections'!AA108","v":0},null,{"$f":"'Run Selections'!AL108","v":""},{"$f":"IF(D108=\"Select Model\",\"N/A\",throwCombined(F108, D108, S108, E108,J108))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D108=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K108, M108, N108, O108),0))","v":"N/A"},{"$f":"IF(D108=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K108,M108,N108,P108)),0))","v":"N/A"},{"$f":"'Run Selections'!BD108","v":0},{"$f":"IF(LEFT($D108,4)<>\"ACBC\",\"N/A\",AdjacentZone($D108,$E108,$S108,$F108,60))","v":"N/A"},{"$f":"IF(LEFT($D108,4)<>\"ACBC\",\"N/A\",AdjacentZone($D108,$E108,$S108,$F108,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F109)=\"\",\"\",'Run Selections'!F109)","v":""},null,{"$f":"'Run Selections'!T109","v":"Select Model"},{"$f":"'Run Selections'!W109","v":4},{"$f":"'Run Selections'!Y109","v":50},{"$f":"'Run Selections'!AI109","v":""},{"$f":"'Run Selections'!AA109","v":0},null,{"$f":"'Run Selections'!AL109","v":""},{"$f":"IF(D109=\"Select Model\",\"N/A\",throwCombined(F109, D109, S109, E109,J109))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D109=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K109, M109, N109, O109),0))","v":"N/A"},{"$f":"IF(D109=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K109,M109,N109,P109)),0))","v":"N/A"},{"$f":"'Run Selections'!BD109","v":0},{"$f":"IF(LEFT($D109,4)<>\"ACBC\",\"N/A\",AdjacentZone($D109,$E109,$S109,$F109,60))","v":"N/A"},{"$f":"IF(LEFT($D109,4)<>\"ACBC\",\"N/A\",AdjacentZone($D109,$E109,$S109,$F109,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F110)=\"\",\"\",'Run Selections'!F110)","v":""},null,{"$f":"'Run Selections'!T110","v":"Select Model"},{"$f":"'Run Selections'!W110","v":4},{"$f":"'Run Selections'!Y110","v":50},{"$f":"'Run Selections'!AI110","v":""},{"$f":"'Run Selections'!AA110","v":0},null,{"$f":"'Run Selections'!AL110","v":""},{"$f":"IF(D110=\"Select Model\",\"N/A\",throwCombined(F110, D110, S110, E110,J110))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D110=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K110, M110, N110, O110),0))","v":"N/A"},{"$f":"IF(D110=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K110,M110,N110,P110)),0))","v":"N/A"},{"$f":"'Run Selections'!BD110","v":0},{"$f":"IF(LEFT($D110,4)<>\"ACBC\",\"N/A\",AdjacentZone($D110,$E110,$S110,$F110,60))","v":"N/A"},{"$f":"IF(LEFT($D110,4)<>\"ACBC\",\"N/A\",AdjacentZone($D110,$E110,$S110,$F110,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F111)=\"\",\"\",'Run Selections'!F111)","v":""},null,{"$f":"'Run Selections'!T111","v":"Select Model"},{"$f":"'Run Selections'!W111","v":4},{"$f":"'Run Selections'!Y111","v":50},{"$f":"'Run Selections'!AI111","v":""},{"$f":"'Run Selections'!AA111","v":0},null,{"$f":"'Run Selections'!AL111","v":""},{"$f":"IF(D111=\"Select Model\",\"N/A\",throwCombined(F111, D111, S111, E111,J111))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D111=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K111, M111, N111, O111),0))","v":"N/A"},{"$f":"IF(D111=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K111,M111,N111,P111)),0))","v":"N/A"},{"$f":"'Run Selections'!BD111","v":0},{"$f":"IF(LEFT($D111,4)<>\"ACBC\",\"N/A\",AdjacentZone($D111,$E111,$S111,$F111,60))","v":"N/A"},{"$f":"IF(LEFT($D111,4)<>\"ACBC\",\"N/A\",AdjacentZone($D111,$E111,$S111,$F111,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F112)=\"\",\"\",'Run Selections'!F112)","v":""},null,{"$f":"'Run Selections'!T112","v":"Select Model"},{"$f":"'Run Selections'!W112","v":4},{"$f":"'Run Selections'!Y112","v":50},{"$f":"'Run Selections'!AI112","v":""},{"$f":"'Run Selections'!AA112","v":0},null,{"$f":"'Run Selections'!AL112","v":""},{"$f":"IF(D112=\"Select Model\",\"N/A\",throwCombined(F112, D112, S112, E112,J112))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D112=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K112, M112, N112, O112),0))","v":"N/A"},{"$f":"IF(D112=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K112,M112,N112,P112)),0))","v":"N/A"},{"$f":"'Run Selections'!BD112","v":0},{"$f":"IF(LEFT($D112,4)<>\"ACBC\",\"N/A\",AdjacentZone($D112,$E112,$S112,$F112,60))","v":"N/A"},{"$f":"IF(LEFT($D112,4)<>\"ACBC\",\"N/A\",AdjacentZone($D112,$E112,$S112,$F112,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F113)=\"\",\"\",'Run Selections'!F113)","v":""},null,{"$f":"'Run Selections'!T113","v":"Select Model"},{"$f":"'Run Selections'!W113","v":4},{"$f":"'Run Selections'!Y113","v":50},{"$f":"'Run Selections'!AI113","v":""},{"$f":"'Run Selections'!AA113","v":0},null,{"$f":"'Run Selections'!AL113","v":""},{"$f":"IF(D113=\"Select Model\",\"N/A\",throwCombined(F113, D113, S113, E113,J113))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D113=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K113, M113, N113, O113),0))","v":"N/A"},{"$f":"IF(D113=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K113,M113,N113,P113)),0))","v":"N/A"},{"$f":"'Run Selections'!BD113","v":0},{"$f":"IF(LEFT($D113,4)<>\"ACBC\",\"N/A\",AdjacentZone($D113,$E113,$S113,$F113,60))","v":"N/A"},{"$f":"IF(LEFT($D113,4)<>\"ACBC\",\"N/A\",AdjacentZone($D113,$E113,$S113,$F113,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F114)=\"\",\"\",'Run Selections'!F114)","v":""},null,{"$f":"'Run Selections'!T114","v":"Select Model"},{"$f":"'Run Selections'!W114","v":4},{"$f":"'Run Selections'!Y114","v":50},{"$f":"'Run Selections'!AI114","v":""},{"$f":"'Run Selections'!AA114","v":0},null,{"$f":"'Run Selections'!AL114","v":""},{"$f":"IF(D114=\"Select Model\",\"N/A\",throwCombined(F114, D114, S114, E114,J114))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D114=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K114, M114, N114, O114),0))","v":"N/A"},{"$f":"IF(D114=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K114,M114,N114,P114)),0))","v":"N/A"},{"$f":"'Run Selections'!BD114","v":0},{"$f":"IF(LEFT($D114,4)<>\"ACBC\",\"N/A\",AdjacentZone($D114,$E114,$S114,$F114,60))","v":"N/A"},{"$f":"IF(LEFT($D114,4)<>\"ACBC\",\"N/A\",AdjacentZone($D114,$E114,$S114,$F114,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F115)=\"\",\"\",'Run Selections'!F115)","v":""},null,{"$f":"'Run Selections'!T115","v":"Select Model"},{"$f":"'Run Selections'!W115","v":4},{"$f":"'Run Selections'!Y115","v":50},{"$f":"'Run Selections'!AI115","v":""},{"$f":"'Run Selections'!AA115","v":0},null,{"$f":"'Run Selections'!AL115","v":""},{"$f":"IF(D115=\"Select Model\",\"N/A\",throwCombined(F115, D115, S115, E115,J115))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D115=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K115, M115, N115, O115),0))","v":"N/A"},{"$f":"IF(D115=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K115,M115,N115,P115)),0))","v":"N/A"},{"$f":"'Run Selections'!BD115","v":0},{"$f":"IF(LEFT($D115,4)<>\"ACBC\",\"N/A\",AdjacentZone($D115,$E115,$S115,$F115,60))","v":"N/A"},{"$f":"IF(LEFT($D115,4)<>\"ACBC\",\"N/A\",AdjacentZone($D115,$E115,$S115,$F115,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F116)=\"\",\"\",'Run Selections'!F116)","v":""},null,{"$f":"'Run Selections'!T116","v":"Select Model"},{"$f":"'Run Selections'!W116","v":4},{"$f":"'Run Selections'!Y116","v":50},{"$f":"'Run Selections'!AI116","v":""},{"$f":"'Run Selections'!AA116","v":0},null,{"$f":"'Run Selections'!AL116","v":""},{"$f":"IF(D116=\"Select Model\",\"N/A\",throwCombined(F116, D116, S116, E116,J116))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D116=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K116, M116, N116, O116),0))","v":"N/A"},{"$f":"IF(D116=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K116,M116,N116,P116)),0))","v":"N/A"},{"$f":"'Run Selections'!BD116","v":0},{"$f":"IF(LEFT($D116,4)<>\"ACBC\",\"N/A\",AdjacentZone($D116,$E116,$S116,$F116,60))","v":"N/A"},{"$f":"IF(LEFT($D116,4)<>\"ACBC\",\"N/A\",AdjacentZone($D116,$E116,$S116,$F116,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F117)=\"\",\"\",'Run Selections'!F117)","v":""},null,{"$f":"'Run Selections'!T117","v":"Select Model"},{"$f":"'Run Selections'!W117","v":4},{"$f":"'Run Selections'!Y117","v":50},{"$f":"'Run Selections'!AI117","v":""},{"$f":"'Run Selections'!AA117","v":0},null,{"$f":"'Run Selections'!AL117","v":""},{"$f":"IF(D117=\"Select Model\",\"N/A\",throwCombined(F117, D117, S117, E117,J117))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D117=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K117, M117, N117, O117),0))","v":"N/A"},{"$f":"IF(D117=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K117,M117,N117,P117)),0))","v":"N/A"},{"$f":"'Run Selections'!BD117","v":0},{"$f":"IF(LEFT($D117,4)<>\"ACBC\",\"N/A\",AdjacentZone($D117,$E117,$S117,$F117,60))","v":"N/A"},{"$f":"IF(LEFT($D117,4)<>\"ACBC\",\"N/A\",AdjacentZone($D117,$E117,$S117,$F117,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F118)=\"\",\"\",'Run Selections'!F118)","v":""},null,{"$f":"'Run Selections'!T118","v":"Select Model"},{"$f":"'Run Selections'!W118","v":4},{"$f":"'Run Selections'!Y118","v":50},{"$f":"'Run Selections'!AI118","v":""},{"$f":"'Run Selections'!AA118","v":0},null,{"$f":"'Run Selections'!AL118","v":""},{"$f":"IF(D118=\"Select Model\",\"N/A\",throwCombined(F118, D118, S118, E118,J118))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D118=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K118, M118, N118, O118),0))","v":"N/A"},{"$f":"IF(D118=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K118,M118,N118,P118)),0))","v":"N/A"},{"$f":"'Run Selections'!BD118","v":0},{"$f":"IF(LEFT($D118,4)<>\"ACBC\",\"N/A\",AdjacentZone($D118,$E118,$S118,$F118,60))","v":"N/A"},{"$f":"IF(LEFT($D118,4)<>\"ACBC\",\"N/A\",AdjacentZone($D118,$E118,$S118,$F118,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F119)=\"\",\"\",'Run Selections'!F119)","v":""},null,{"$f":"'Run Selections'!T119","v":"Select Model"},{"$f":"'Run Selections'!W119","v":4},{"$f":"'Run Selections'!Y119","v":50},{"$f":"'Run Selections'!AI119","v":""},{"$f":"'Run Selections'!AA119","v":0},null,{"$f":"'Run Selections'!AL119","v":""},{"$f":"IF(D119=\"Select Model\",\"N/A\",throwCombined(F119, D119, S119, E119,J119))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D119=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K119, M119, N119, O119),0))","v":"N/A"},{"$f":"IF(D119=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K119,M119,N119,P119)),0))","v":"N/A"},{"$f":"'Run Selections'!BD119","v":0},{"$f":"IF(LEFT($D119,4)<>\"ACBC\",\"N/A\",AdjacentZone($D119,$E119,$S119,$F119,60))","v":"N/A"},{"$f":"IF(LEFT($D119,4)<>\"ACBC\",\"N/A\",AdjacentZone($D119,$E119,$S119,$F119,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F120)=\"\",\"\",'Run Selections'!F120)","v":""},null,{"$f":"'Run Selections'!T120","v":"Select Model"},{"$f":"'Run Selections'!W120","v":4},{"$f":"'Run Selections'!Y120","v":50},{"$f":"'Run Selections'!AI120","v":""},{"$f":"'Run Selections'!AA120","v":0},null,{"$f":"'Run Selections'!AL120","v":""},{"$f":"IF(D120=\"Select Model\",\"N/A\",throwCombined(F120, D120, S120, E120,J120))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D120=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K120, M120, N120, O120),0))","v":"N/A"},{"$f":"IF(D120=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K120,M120,N120,P120)),0))","v":"N/A"},{"$f":"'Run Selections'!BD120","v":0},{"$f":"IF(LEFT($D120,4)<>\"ACBC\",\"N/A\",AdjacentZone($D120,$E120,$S120,$F120,60))","v":"N/A"},{"$f":"IF(LEFT($D120,4)<>\"ACBC\",\"N/A\",AdjacentZone($D120,$E120,$S120,$F120,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F121)=\"\",\"\",'Run Selections'!F121)","v":""},null,{"$f":"'Run Selections'!T121","v":"Select Model"},{"$f":"'Run Selections'!W121","v":4},{"$f":"'Run Selections'!Y121","v":50},{"$f":"'Run Selections'!AI121","v":""},{"$f":"'Run Selections'!AA121","v":0},null,{"$f":"'Run Selections'!AL121","v":""},{"$f":"IF(D121=\"Select Model\",\"N/A\",throwCombined(F121, D121, S121, E121,J121))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D121=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K121, M121, N121, O121),0))","v":"N/A"},{"$f":"IF(D121=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K121,M121,N121,P121)),0))","v":"N/A"},{"$f":"'Run Selections'!BD121","v":0},{"$f":"IF(LEFT($D121,4)<>\"ACBC\",\"N/A\",AdjacentZone($D121,$E121,$S121,$F121,60))","v":"N/A"},{"$f":"IF(LEFT($D121,4)<>\"ACBC\",\"N/A\",AdjacentZone($D121,$E121,$S121,$F121,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F122)=\"\",\"\",'Run Selections'!F122)","v":""},null,{"$f":"'Run Selections'!T122","v":"Select Model"},{"$f":"'Run Selections'!W122","v":4},{"$f":"'Run Selections'!Y122","v":50},{"$f":"'Run Selections'!AI122","v":""},{"$f":"'Run Selections'!AA122","v":0},null,{"$f":"'Run Selections'!AL122","v":""},{"$f":"IF(D122=\"Select Model\",\"N/A\",throwCombined(F122, D122, S122, E122,J122))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D122=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K122, M122, N122, O122),0))","v":"N/A"},{"$f":"IF(D122=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K122,M122,N122,P122)),0))","v":"N/A"},{"$f":"'Run Selections'!BD122","v":0},{"$f":"IF(LEFT($D122,4)<>\"ACBC\",\"N/A\",AdjacentZone($D122,$E122,$S122,$F122,60))","v":"N/A"},{"$f":"IF(LEFT($D122,4)<>\"ACBC\",\"N/A\",AdjacentZone($D122,$E122,$S122,$F122,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F123)=\"\",\"\",'Run Selections'!F123)","v":""},null,{"$f":"'Run Selections'!T123","v":"Select Model"},{"$f":"'Run Selections'!W123","v":4},{"$f":"'Run Selections'!Y123","v":50},{"$f":"'Run Selections'!AI123","v":""},{"$f":"'Run Selections'!AA123","v":0},null,{"$f":"'Run Selections'!AL123","v":""},{"$f":"IF(D123=\"Select Model\",\"N/A\",throwCombined(F123, D123, S123, E123,J123))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D123=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K123, M123, N123, O123),0))","v":"N/A"},{"$f":"IF(D123=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K123,M123,N123,P123)),0))","v":"N/A"},{"$f":"'Run Selections'!BD123","v":0},{"$f":"IF(LEFT($D123,4)<>\"ACBC\",\"N/A\",AdjacentZone($D123,$E123,$S123,$F123,60))","v":"N/A"},{"$f":"IF(LEFT($D123,4)<>\"ACBC\",\"N/A\",AdjacentZone($D123,$E123,$S123,$F123,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F124)=\"\",\"\",'Run Selections'!F124)","v":""},null,{"$f":"'Run Selections'!T124","v":"Select Model"},{"$f":"'Run Selections'!W124","v":4},{"$f":"'Run Selections'!Y124","v":50},{"$f":"'Run Selections'!AI124","v":""},{"$f":"'Run Selections'!AA124","v":0},null,{"$f":"'Run Selections'!AL124","v":""},{"$f":"IF(D124=\"Select Model\",\"N/A\",throwCombined(F124, D124, S124, E124,J124))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D124=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K124, M124, N124, O124),0))","v":"N/A"},{"$f":"IF(D124=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K124,M124,N124,P124)),0))","v":"N/A"},{"$f":"'Run Selections'!BD124","v":0},{"$f":"IF(LEFT($D124,4)<>\"ACBC\",\"N/A\",AdjacentZone($D124,$E124,$S124,$F124,60))","v":"N/A"},{"$f":"IF(LEFT($D124,4)<>\"ACBC\",\"N/A\",AdjacentZone($D124,$E124,$S124,$F124,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F125)=\"\",\"\",'Run Selections'!F125)","v":""},null,{"$f":"'Run Selections'!T125","v":"Select Model"},{"$f":"'Run Selections'!W125","v":4},{"$f":"'Run Selections'!Y125","v":50},{"$f":"'Run Selections'!AI125","v":""},{"$f":"'Run Selections'!AA125","v":0},null,{"$f":"'Run Selections'!AL125","v":""},{"$f":"IF(D125=\"Select Model\",\"N/A\",throwCombined(F125, D125, S125, E125,J125))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D125=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K125, M125, N125, O125),0))","v":"N/A"},{"$f":"IF(D125=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K125,M125,N125,P125)),0))","v":"N/A"},{"$f":"'Run Selections'!BD125","v":0},{"$f":"IF(LEFT($D125,4)<>\"ACBC\",\"N/A\",AdjacentZone($D125,$E125,$S125,$F125,60))","v":"N/A"},{"$f":"IF(LEFT($D125,4)<>\"ACBC\",\"N/A\",AdjacentZone($D125,$E125,$S125,$F125,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F126)=\"\",\"\",'Run Selections'!F126)","v":""},null,{"$f":"'Run Selections'!T126","v":"Select Model"},{"$f":"'Run Selections'!W126","v":4},{"$f":"'Run Selections'!Y126","v":50},{"$f":"'Run Selections'!AI126","v":""},{"$f":"'Run Selections'!AA126","v":0},null,{"$f":"'Run Selections'!AL126","v":""},{"$f":"IF(D126=\"Select Model\",\"N/A\",throwCombined(F126, D126, S126, E126,J126))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D126=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K126, M126, N126, O126),0))","v":"N/A"},{"$f":"IF(D126=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K126,M126,N126,P126)),0))","v":"N/A"},{"$f":"'Run Selections'!BD126","v":0},{"$f":"IF(LEFT($D126,4)<>\"ACBC\",\"N/A\",AdjacentZone($D126,$E126,$S126,$F126,60))","v":"N/A"},{"$f":"IF(LEFT($D126,4)<>\"ACBC\",\"N/A\",AdjacentZone($D126,$E126,$S126,$F126,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F127)=\"\",\"\",'Run Selections'!F127)","v":""},null,{"$f":"'Run Selections'!T127","v":"Select Model"},{"$f":"'Run Selections'!W127","v":4},{"$f":"'Run Selections'!Y127","v":50},{"$f":"'Run Selections'!AI127","v":""},{"$f":"'Run Selections'!AA127","v":0},null,{"$f":"'Run Selections'!AL127","v":""},{"$f":"IF(D127=\"Select Model\",\"N/A\",throwCombined(F127, D127, S127, E127,J127))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D127=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K127, M127, N127, O127),0))","v":"N/A"},{"$f":"IF(D127=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K127,M127,N127,P127)),0))","v":"N/A"},{"$f":"'Run Selections'!BD127","v":0},{"$f":"IF(LEFT($D127,4)<>\"ACBC\",\"N/A\",AdjacentZone($D127,$E127,$S127,$F127,60))","v":"N/A"},{"$f":"IF(LEFT($D127,4)<>\"ACBC\",\"N/A\",AdjacentZone($D127,$E127,$S127,$F127,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F128)=\"\",\"\",'Run Selections'!F128)","v":""},null,{"$f":"'Run Selections'!T128","v":"Select Model"},{"$f":"'Run Selections'!W128","v":4},{"$f":"'Run Selections'!Y128","v":50},{"$f":"'Run Selections'!AI128","v":""},{"$f":"'Run Selections'!AA128","v":0},null,{"$f":"'Run Selections'!AL128","v":""},{"$f":"IF(D128=\"Select Model\",\"N/A\",throwCombined(F128, D128, S128, E128,J128))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D128=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K128, M128, N128, O128),0))","v":"N/A"},{"$f":"IF(D128=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K128,M128,N128,P128)),0))","v":"N/A"},{"$f":"'Run Selections'!BD128","v":0},{"$f":"IF(LEFT($D128,4)<>\"ACBC\",\"N/A\",AdjacentZone($D128,$E128,$S128,$F128,60))","v":"N/A"},{"$f":"IF(LEFT($D128,4)<>\"ACBC\",\"N/A\",AdjacentZone($D128,$E128,$S128,$F128,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F129)=\"\",\"\",'Run Selections'!F129)","v":""},null,{"$f":"'Run Selections'!T129","v":"Select Model"},{"$f":"'Run Selections'!W129","v":4},{"$f":"'Run Selections'!Y129","v":50},{"$f":"'Run Selections'!AI129","v":""},{"$f":"'Run Selections'!AA129","v":0},null,{"$f":"'Run Selections'!AL129","v":""},{"$f":"IF(D129=\"Select Model\",\"N/A\",throwCombined(F129, D129, S129, E129,J129))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D129=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K129, M129, N129, O129),0))","v":"N/A"},{"$f":"IF(D129=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K129,M129,N129,P129)),0))","v":"N/A"},{"$f":"'Run Selections'!BD129","v":0},{"$f":"IF(LEFT($D129,4)<>\"ACBC\",\"N/A\",AdjacentZone($D129,$E129,$S129,$F129,60))","v":"N/A"},{"$f":"IF(LEFT($D129,4)<>\"ACBC\",\"N/A\",AdjacentZone($D129,$E129,$S129,$F129,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F130)=\"\",\"\",'Run Selections'!F130)","v":""},null,{"$f":"'Run Selections'!T130","v":"Select Model"},{"$f":"'Run Selections'!W130","v":4},{"$f":"'Run Selections'!Y130","v":50},{"$f":"'Run Selections'!AI130","v":""},{"$f":"'Run Selections'!AA130","v":0},null,{"$f":"'Run Selections'!AL130","v":""},{"$f":"IF(D130=\"Select Model\",\"N/A\",throwCombined(F130, D130, S130, E130,J130))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D130=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K130, M130, N130, O130),0))","v":"N/A"},{"$f":"IF(D130=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K130,M130,N130,P130)),0))","v":"N/A"},{"$f":"'Run Selections'!BD130","v":0},{"$f":"IF(LEFT($D130,4)<>\"ACBC\",\"N/A\",AdjacentZone($D130,$E130,$S130,$F130,60))","v":"N/A"},{"$f":"IF(LEFT($D130,4)<>\"ACBC\",\"N/A\",AdjacentZone($D130,$E130,$S130,$F130,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F131)=\"\",\"\",'Run Selections'!F131)","v":""},null,{"$f":"'Run Selections'!T131","v":"Select Model"},{"$f":"'Run Selections'!W131","v":4},{"$f":"'Run Selections'!Y131","v":50},{"$f":"'Run Selections'!AI131","v":""},{"$f":"'Run Selections'!AA131","v":0},null,{"$f":"'Run Selections'!AL131","v":""},{"$f":"IF(D131=\"Select Model\",\"N/A\",throwCombined(F131, D131, S131, E131,J131))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D131=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K131, M131, N131, O131),0))","v":"N/A"},{"$f":"IF(D131=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K131,M131,N131,P131)),0))","v":"N/A"},{"$f":"'Run Selections'!BD131","v":0},{"$f":"IF(LEFT($D131,4)<>\"ACBC\",\"N/A\",AdjacentZone($D131,$E131,$S131,$F131,60))","v":"N/A"},{"$f":"IF(LEFT($D131,4)<>\"ACBC\",\"N/A\",AdjacentZone($D131,$E131,$S131,$F131,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F132)=\"\",\"\",'Run Selections'!F132)","v":""},null,{"$f":"'Run Selections'!T132","v":"Select Model"},{"$f":"'Run Selections'!W132","v":4},{"$f":"'Run Selections'!Y132","v":50},{"$f":"'Run Selections'!AI132","v":""},{"$f":"'Run Selections'!AA132","v":0},null,{"$f":"'Run Selections'!AL132","v":""},{"$f":"IF(D132=\"Select Model\",\"N/A\",throwCombined(F132, D132, S132, E132,J132))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D132=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K132, M132, N132, O132),0))","v":"N/A"},{"$f":"IF(D132=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K132,M132,N132,P132)),0))","v":"N/A"},{"$f":"'Run Selections'!BD132","v":0},{"$f":"IF(LEFT($D132,4)<>\"ACBC\",\"N/A\",AdjacentZone($D132,$E132,$S132,$F132,60))","v":"N/A"},{"$f":"IF(LEFT($D132,4)<>\"ACBC\",\"N/A\",AdjacentZone($D132,$E132,$S132,$F132,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F133)=\"\",\"\",'Run Selections'!F133)","v":""},null,{"$f":"'Run Selections'!T133","v":"Select Model"},{"$f":"'Run Selections'!W133","v":4},{"$f":"'Run Selections'!Y133","v":50},{"$f":"'Run Selections'!AI133","v":""},{"$f":"'Run Selections'!AA133","v":0},null,{"$f":"'Run Selections'!AL133","v":""},{"$f":"IF(D133=\"Select Model\",\"N/A\",throwCombined(F133, D133, S133, E133,J133))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D133=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K133, M133, N133, O133),0))","v":"N/A"},{"$f":"IF(D133=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K133,M133,N133,P133)),0))","v":"N/A"},{"$f":"'Run Selections'!BD133","v":0},{"$f":"IF(LEFT($D133,4)<>\"ACBC\",\"N/A\",AdjacentZone($D133,$E133,$S133,$F133,60))","v":"N/A"},{"$f":"IF(LEFT($D133,4)<>\"ACBC\",\"N/A\",AdjacentZone($D133,$E133,$S133,$F133,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F134)=\"\",\"\",'Run Selections'!F134)","v":""},null,{"$f":"'Run Selections'!T134","v":"Select Model"},{"$f":"'Run Selections'!W134","v":4},{"$f":"'Run Selections'!Y134","v":50},{"$f":"'Run Selections'!AI134","v":""},{"$f":"'Run Selections'!AA134","v":0},null,{"$f":"'Run Selections'!AL134","v":""},{"$f":"IF(D134=\"Select Model\",\"N/A\",throwCombined(F134, D134, S134, E134,J134))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D134=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K134, M134, N134, O134),0))","v":"N/A"},{"$f":"IF(D134=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K134,M134,N134,P134)),0))","v":"N/A"},{"$f":"'Run Selections'!BD134","v":0},{"$f":"IF(LEFT($D134,4)<>\"ACBC\",\"N/A\",AdjacentZone($D134,$E134,$S134,$F134,60))","v":"N/A"},{"$f":"IF(LEFT($D134,4)<>\"ACBC\",\"N/A\",AdjacentZone($D134,$E134,$S134,$F134,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F135)=\"\",\"\",'Run Selections'!F135)","v":""},null,{"$f":"'Run Selections'!T135","v":"Select Model"},{"$f":"'Run Selections'!W135","v":4},{"$f":"'Run Selections'!Y135","v":50},{"$f":"'Run Selections'!AI135","v":""},{"$f":"'Run Selections'!AA135","v":0},null,{"$f":"'Run Selections'!AL135","v":""},{"$f":"IF(D135=\"Select Model\",\"N/A\",throwCombined(F135, D135, S135, E135,J135))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D135=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K135, M135, N135, O135),0))","v":"N/A"},{"$f":"IF(D135=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K135,M135,N135,P135)),0))","v":"N/A"},{"$f":"'Run Selections'!BD135","v":0},{"$f":"IF(LEFT($D135,4)<>\"ACBC\",\"N/A\",AdjacentZone($D135,$E135,$S135,$F135,60))","v":"N/A"},{"$f":"IF(LEFT($D135,4)<>\"ACBC\",\"N/A\",AdjacentZone($D135,$E135,$S135,$F135,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F136)=\"\",\"\",'Run Selections'!F136)","v":""},null,{"$f":"'Run Selections'!T136","v":"Select Model"},{"$f":"'Run Selections'!W136","v":4},{"$f":"'Run Selections'!Y136","v":50},{"$f":"'Run Selections'!AI136","v":""},{"$f":"'Run Selections'!AA136","v":0},null,{"$f":"'Run Selections'!AL136","v":""},{"$f":"IF(D136=\"Select Model\",\"N/A\",throwCombined(F136, D136, S136, E136,J136))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D136=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K136, M136, N136, O136),0))","v":"N/A"},{"$f":"IF(D136=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K136,M136,N136,P136)),0))","v":"N/A"},{"$f":"'Run Selections'!BD136","v":0},{"$f":"IF(LEFT($D136,4)<>\"ACBC\",\"N/A\",AdjacentZone($D136,$E136,$S136,$F136,60))","v":"N/A"},{"$f":"IF(LEFT($D136,4)<>\"ACBC\",\"N/A\",AdjacentZone($D136,$E136,$S136,$F136,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F137)=\"\",\"\",'Run Selections'!F137)","v":""},null,{"$f":"'Run Selections'!T137","v":"Select Model"},{"$f":"'Run Selections'!W137","v":4},{"$f":"'Run Selections'!Y137","v":50},{"$f":"'Run Selections'!AI137","v":""},{"$f":"'Run Selections'!AA137","v":0},null,{"$f":"'Run Selections'!AL137","v":""},{"$f":"IF(D137=\"Select Model\",\"N/A\",throwCombined(F137, D137, S137, E137,J137))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D137=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K137, M137, N137, O137),0))","v":"N/A"},{"$f":"IF(D137=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K137,M137,N137,P137)),0))","v":"N/A"},{"$f":"'Run Selections'!BD137","v":0},{"$f":"IF(LEFT($D137,4)<>\"ACBC\",\"N/A\",AdjacentZone($D137,$E137,$S137,$F137,60))","v":"N/A"},{"$f":"IF(LEFT($D137,4)<>\"ACBC\",\"N/A\",AdjacentZone($D137,$E137,$S137,$F137,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F138)=\"\",\"\",'Run Selections'!F138)","v":""},null,{"$f":"'Run Selections'!T138","v":"Select Model"},{"$f":"'Run Selections'!W138","v":4},{"$f":"'Run Selections'!Y138","v":50},{"$f":"'Run Selections'!AI138","v":""},{"$f":"'Run Selections'!AA138","v":0},null,{"$f":"'Run Selections'!AL138","v":""},{"$f":"IF(D138=\"Select Model\",\"N/A\",throwCombined(F138, D138, S138, E138,J138))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D138=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K138, M138, N138, O138),0))","v":"N/A"},{"$f":"IF(D138=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K138,M138,N138,P138)),0))","v":"N/A"},{"$f":"'Run Selections'!BD138","v":0},{"$f":"IF(LEFT($D138,4)<>\"ACBC\",\"N/A\",AdjacentZone($D138,$E138,$S138,$F138,60))","v":"N/A"},{"$f":"IF(LEFT($D138,4)<>\"ACBC\",\"N/A\",AdjacentZone($D138,$E138,$S138,$F138,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F139)=\"\",\"\",'Run Selections'!F139)","v":""},null,{"$f":"'Run Selections'!T139","v":"Select Model"},{"$f":"'Run Selections'!W139","v":4},{"$f":"'Run Selections'!Y139","v":50},{"$f":"'Run Selections'!AI139","v":""},{"$f":"'Run Selections'!AA139","v":0},null,{"$f":"'Run Selections'!AL139","v":""},{"$f":"IF(D139=\"Select Model\",\"N/A\",throwCombined(F139, D139, S139, E139,J139))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D139=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K139, M139, N139, O139),0))","v":"N/A"},{"$f":"IF(D139=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K139,M139,N139,P139)),0))","v":"N/A"},{"$f":"'Run Selections'!BD139","v":0},{"$f":"IF(LEFT($D139,4)<>\"ACBC\",\"N/A\",AdjacentZone($D139,$E139,$S139,$F139,60))","v":"N/A"},{"$f":"IF(LEFT($D139,4)<>\"ACBC\",\"N/A\",AdjacentZone($D139,$E139,$S139,$F139,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F140)=\"\",\"\",'Run Selections'!F140)","v":""},null,{"$f":"'Run Selections'!T140","v":"Select Model"},{"$f":"'Run Selections'!W140","v":4},{"$f":"'Run Selections'!Y140","v":50},{"$f":"'Run Selections'!AI140","v":""},{"$f":"'Run Selections'!AA140","v":0},null,{"$f":"'Run Selections'!AL140","v":""},{"$f":"IF(D140=\"Select Model\",\"N/A\",throwCombined(F140, D140, S140, E140,J140))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D140=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K140, M140, N140, O140),0))","v":"N/A"},{"$f":"IF(D140=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K140,M140,N140,P140)),0))","v":"N/A"},{"$f":"'Run Selections'!BD140","v":0},{"$f":"IF(LEFT($D140,4)<>\"ACBC\",\"N/A\",AdjacentZone($D140,$E140,$S140,$F140,60))","v":"N/A"},{"$f":"IF(LEFT($D140,4)<>\"ACBC\",\"N/A\",AdjacentZone($D140,$E140,$S140,$F140,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F141)=\"\",\"\",'Run Selections'!F141)","v":""},null,{"$f":"'Run Selections'!T141","v":"Select Model"},{"$f":"'Run Selections'!W141","v":4},{"$f":"'Run Selections'!Y141","v":50},{"$f":"'Run Selections'!AI141","v":""},{"$f":"'Run Selections'!AA141","v":0},null,{"$f":"'Run Selections'!AL141","v":""},{"$f":"IF(D141=\"Select Model\",\"N/A\",throwCombined(F141, D141, S141, E141,J141))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D141=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K141, M141, N141, O141),0))","v":"N/A"},{"$f":"IF(D141=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K141,M141,N141,P141)),0))","v":"N/A"},{"$f":"'Run Selections'!BD141","v":0},{"$f":"IF(LEFT($D141,4)<>\"ACBC\",\"N/A\",AdjacentZone($D141,$E141,$S141,$F141,60))","v":"N/A"},{"$f":"IF(LEFT($D141,4)<>\"ACBC\",\"N/A\",AdjacentZone($D141,$E141,$S141,$F141,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F142)=\"\",\"\",'Run Selections'!F142)","v":""},null,{"$f":"'Run Selections'!T142","v":"Select Model"},{"$f":"'Run Selections'!W142","v":4},{"$f":"'Run Selections'!Y142","v":50},{"$f":"'Run Selections'!AI142","v":""},{"$f":"'Run Selections'!AA142","v":0},null,{"$f":"'Run Selections'!AL142","v":""},{"$f":"IF(D142=\"Select Model\",\"N/A\",throwCombined(F142, D142, S142, E142,J142))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D142=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K142, M142, N142, O142),0))","v":"N/A"},{"$f":"IF(D142=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K142,M142,N142,P142)),0))","v":"N/A"},{"$f":"'Run Selections'!BD142","v":0},{"$f":"IF(LEFT($D142,4)<>\"ACBC\",\"N/A\",AdjacentZone($D142,$E142,$S142,$F142,60))","v":"N/A"},{"$f":"IF(LEFT($D142,4)<>\"ACBC\",\"N/A\",AdjacentZone($D142,$E142,$S142,$F142,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F143)=\"\",\"\",'Run Selections'!F143)","v":""},null,{"$f":"'Run Selections'!T143","v":"Select Model"},{"$f":"'Run Selections'!W143","v":4},{"$f":"'Run Selections'!Y143","v":50},{"$f":"'Run Selections'!AI143","v":""},{"$f":"'Run Selections'!AA143","v":0},null,{"$f":"'Run Selections'!AL143","v":""},{"$f":"IF(D143=\"Select Model\",\"N/A\",throwCombined(F143, D143, S143, E143,J143))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D143=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K143, M143, N143, O143),0))","v":"N/A"},{"$f":"IF(D143=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K143,M143,N143,P143)),0))","v":"N/A"},{"$f":"'Run Selections'!BD143","v":0},{"$f":"IF(LEFT($D143,4)<>\"ACBC\",\"N/A\",AdjacentZone($D143,$E143,$S143,$F143,60))","v":"N/A"},{"$f":"IF(LEFT($D143,4)<>\"ACBC\",\"N/A\",AdjacentZone($D143,$E143,$S143,$F143,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F144)=\"\",\"\",'Run Selections'!F144)","v":""},null,{"$f":"'Run Selections'!T144","v":"Select Model"},{"$f":"'Run Selections'!W144","v":4},{"$f":"'Run Selections'!Y144","v":50},{"$f":"'Run Selections'!AI144","v":""},{"$f":"'Run Selections'!AA144","v":0},null,{"$f":"'Run Selections'!AL144","v":""},{"$f":"IF(D144=\"Select Model\",\"N/A\",throwCombined(F144, D144, S144, E144,J144))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D144=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K144, M144, N144, O144),0))","v":"N/A"},{"$f":"IF(D144=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K144,M144,N144,P144)),0))","v":"N/A"},{"$f":"'Run Selections'!BD144","v":0},{"$f":"IF(LEFT($D144,4)<>\"ACBC\",\"N/A\",AdjacentZone($D144,$E144,$S144,$F144,60))","v":"N/A"},{"$f":"IF(LEFT($D144,4)<>\"ACBC\",\"N/A\",AdjacentZone($D144,$E144,$S144,$F144,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F145)=\"\",\"\",'Run Selections'!F145)","v":""},null,{"$f":"'Run Selections'!T145","v":"Select Model"},{"$f":"'Run Selections'!W145","v":4},{"$f":"'Run Selections'!Y145","v":50},{"$f":"'Run Selections'!AI145","v":""},{"$f":"'Run Selections'!AA145","v":0},null,{"$f":"'Run Selections'!AL145","v":""},{"$f":"IF(D145=\"Select Model\",\"N/A\",throwCombined(F145, D145, S145, E145,J145))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D145=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K145, M145, N145, O145),0))","v":"N/A"},{"$f":"IF(D145=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K145,M145,N145,P145)),0))","v":"N/A"},{"$f":"'Run Selections'!BD145","v":0},{"$f":"IF(LEFT($D145,4)<>\"ACBC\",\"N/A\",AdjacentZone($D145,$E145,$S145,$F145,60))","v":"N/A"},{"$f":"IF(LEFT($D145,4)<>\"ACBC\",\"N/A\",AdjacentZone($D145,$E145,$S145,$F145,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F146)=\"\",\"\",'Run Selections'!F146)","v":""},null,{"$f":"'Run Selections'!T146","v":"Select Model"},{"$f":"'Run Selections'!W146","v":4},{"$f":"'Run Selections'!Y146","v":50},{"$f":"'Run Selections'!AI146","v":""},{"$f":"'Run Selections'!AA146","v":0},null,{"$f":"'Run Selections'!AL146","v":""},{"$f":"IF(D146=\"Select Model\",\"N/A\",throwCombined(F146, D146, S146, E146,J146))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D146=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K146, M146, N146, O146),0))","v":"N/A"},{"$f":"IF(D146=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K146,M146,N146,P146)),0))","v":"N/A"},{"$f":"'Run Selections'!BD146","v":0},{"$f":"IF(LEFT($D146,4)<>\"ACBC\",\"N/A\",AdjacentZone($D146,$E146,$S146,$F146,60))","v":"N/A"},{"$f":"IF(LEFT($D146,4)<>\"ACBC\",\"N/A\",AdjacentZone($D146,$E146,$S146,$F146,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F147)=\"\",\"\",'Run Selections'!F147)","v":""},null,{"$f":"'Run Selections'!T147","v":"Select Model"},{"$f":"'Run Selections'!W147","v":4},{"$f":"'Run Selections'!Y147","v":50},{"$f":"'Run Selections'!AI147","v":""},{"$f":"'Run Selections'!AA147","v":0},null,{"$f":"'Run Selections'!AL147","v":""},{"$f":"IF(D147=\"Select Model\",\"N/A\",throwCombined(F147, D147, S147, E147,J147))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D147=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K147, M147, N147, O147),0))","v":"N/A"},{"$f":"IF(D147=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K147,M147,N147,P147)),0))","v":"N/A"},{"$f":"'Run Selections'!BD147","v":0},{"$f":"IF(LEFT($D147,4)<>\"ACBC\",\"N/A\",AdjacentZone($D147,$E147,$S147,$F147,60))","v":"N/A"},{"$f":"IF(LEFT($D147,4)<>\"ACBC\",\"N/A\",AdjacentZone($D147,$E147,$S147,$F147,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F148)=\"\",\"\",'Run Selections'!F148)","v":""},null,{"$f":"'Run Selections'!T148","v":"Select Model"},{"$f":"'Run Selections'!W148","v":4},{"$f":"'Run Selections'!Y148","v":50},{"$f":"'Run Selections'!AI148","v":""},{"$f":"'Run Selections'!AA148","v":0},null,{"$f":"'Run Selections'!AL148","v":""},{"$f":"IF(D148=\"Select Model\",\"N/A\",throwCombined(F148, D148, S148, E148,J148))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D148=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K148, M148, N148, O148),0))","v":"N/A"},{"$f":"IF(D148=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K148,M148,N148,P148)),0))","v":"N/A"},{"$f":"'Run Selections'!BD148","v":0},{"$f":"IF(LEFT($D148,4)<>\"ACBC\",\"N/A\",AdjacentZone($D148,$E148,$S148,$F148,60))","v":"N/A"},{"$f":"IF(LEFT($D148,4)<>\"ACBC\",\"N/A\",AdjacentZone($D148,$E148,$S148,$F148,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F149)=\"\",\"\",'Run Selections'!F149)","v":""},null,{"$f":"'Run Selections'!T149","v":"Select Model"},{"$f":"'Run Selections'!W149","v":4},{"$f":"'Run Selections'!Y149","v":50},{"$f":"'Run Selections'!AI149","v":""},{"$f":"'Run Selections'!AA149","v":0},null,{"$f":"'Run Selections'!AL149","v":""},{"$f":"IF(D149=\"Select Model\",\"N/A\",throwCombined(F149, D149, S149, E149,J149))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D149=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K149, M149, N149, O149),0))","v":"N/A"},{"$f":"IF(D149=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K149,M149,N149,P149)),0))","v":"N/A"},{"$f":"'Run Selections'!BD149","v":0},{"$f":"IF(LEFT($D149,4)<>\"ACBC\",\"N/A\",AdjacentZone($D149,$E149,$S149,$F149,60))","v":"N/A"},{"$f":"IF(LEFT($D149,4)<>\"ACBC\",\"N/A\",AdjacentZone($D149,$E149,$S149,$F149,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F150)=\"\",\"\",'Run Selections'!F150)","v":""},null,{"$f":"'Run Selections'!T150","v":"Select Model"},{"$f":"'Run Selections'!W150","v":4},{"$f":"'Run Selections'!Y150","v":50},{"$f":"'Run Selections'!AI150","v":""},{"$f":"'Run Selections'!AA150","v":0},null,{"$f":"'Run Selections'!AL150","v":""},{"$f":"IF(D150=\"Select Model\",\"N/A\",throwCombined(F150, D150, S150, E150,J150))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D150=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K150, M150, N150, O150),0))","v":"N/A"},{"$f":"IF(D150=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K150,M150,N150,P150)),0))","v":"N/A"},{"$f":"'Run Selections'!BD150","v":0},{"$f":"IF(LEFT($D150,4)<>\"ACBC\",\"N/A\",AdjacentZone($D150,$E150,$S150,$F150,60))","v":"N/A"},{"$f":"IF(LEFT($D150,4)<>\"ACBC\",\"N/A\",AdjacentZone($D150,$E150,$S150,$F150,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F151)=\"\",\"\",'Run Selections'!F151)","v":""},null,{"$f":"'Run Selections'!T151","v":"Select Model"},{"$f":"'Run Selections'!W151","v":4},{"$f":"'Run Selections'!Y151","v":50},{"$f":"'Run Selections'!AI151","v":""},{"$f":"'Run Selections'!AA151","v":0},null,{"$f":"'Run Selections'!AL151","v":""},{"$f":"IF(D151=\"Select Model\",\"N/A\",throwCombined(F151, D151, S151, E151,J151))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D151=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K151, M151, N151, O151),0))","v":"N/A"},{"$f":"IF(D151=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K151,M151,N151,P151)),0))","v":"N/A"},{"$f":"'Run Selections'!BD151","v":0},{"$f":"IF(LEFT($D151,4)<>\"ACBC\",\"N/A\",AdjacentZone($D151,$E151,$S151,$F151,60))","v":"N/A"},{"$f":"IF(LEFT($D151,4)<>\"ACBC\",\"N/A\",AdjacentZone($D151,$E151,$S151,$F151,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F152)=\"\",\"\",'Run Selections'!F152)","v":""},null,{"$f":"'Run Selections'!T152","v":"Select Model"},{"$f":"'Run Selections'!W152","v":4},{"$f":"'Run Selections'!Y152","v":50},{"$f":"'Run Selections'!AI152","v":""},{"$f":"'Run Selections'!AA152","v":0},null,{"$f":"'Run Selections'!AL152","v":""},{"$f":"IF(D152=\"Select Model\",\"N/A\",throwCombined(F152, D152, S152, E152,J152))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D152=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K152, M152, N152, O152),0))","v":"N/A"},{"$f":"IF(D152=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K152,M152,N152,P152)),0))","v":"N/A"},{"$f":"'Run Selections'!BD152","v":0},{"$f":"IF(LEFT($D152,4)<>\"ACBC\",\"N/A\",AdjacentZone($D152,$E152,$S152,$F152,60))","v":"N/A"},{"$f":"IF(LEFT($D152,4)<>\"ACBC\",\"N/A\",AdjacentZone($D152,$E152,$S152,$F152,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F153)=\"\",\"\",'Run Selections'!F153)","v":""},null,{"$f":"'Run Selections'!T153","v":"Select Model"},{"$f":"'Run Selections'!W153","v":4},{"$f":"'Run Selections'!Y153","v":50},{"$f":"'Run Selections'!AI153","v":""},{"$f":"'Run Selections'!AA153","v":0},null,{"$f":"'Run Selections'!AL153","v":""},{"$f":"IF(D153=\"Select Model\",\"N/A\",throwCombined(F153, D153, S153, E153,J153))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D153=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K153, M153, N153, O153),0))","v":"N/A"},{"$f":"IF(D153=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K153,M153,N153,P153)),0))","v":"N/A"},{"$f":"'Run Selections'!BD153","v":0},{"$f":"IF(LEFT($D153,4)<>\"ACBC\",\"N/A\",AdjacentZone($D153,$E153,$S153,$F153,60))","v":"N/A"},{"$f":"IF(LEFT($D153,4)<>\"ACBC\",\"N/A\",AdjacentZone($D153,$E153,$S153,$F153,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F154)=\"\",\"\",'Run Selections'!F154)","v":""},null,{"$f":"'Run Selections'!T154","v":"Select Model"},{"$f":"'Run Selections'!W154","v":4},{"$f":"'Run Selections'!Y154","v":50},{"$f":"'Run Selections'!AI154","v":""},{"$f":"'Run Selections'!AA154","v":0},null,{"$f":"'Run Selections'!AL154","v":""},{"$f":"IF(D154=\"Select Model\",\"N/A\",throwCombined(F154, D154, S154, E154,J154))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D154=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K154, M154, N154, O154),0))","v":"N/A"},{"$f":"IF(D154=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K154,M154,N154,P154)),0))","v":"N/A"},{"$f":"'Run Selections'!BD154","v":0},{"$f":"IF(LEFT($D154,4)<>\"ACBC\",\"N/A\",AdjacentZone($D154,$E154,$S154,$F154,60))","v":"N/A"},{"$f":"IF(LEFT($D154,4)<>\"ACBC\",\"N/A\",AdjacentZone($D154,$E154,$S154,$F154,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F155)=\"\",\"\",'Run Selections'!F155)","v":""},null,{"$f":"'Run Selections'!T155","v":"Select Model"},{"$f":"'Run Selections'!W155","v":4},{"$f":"'Run Selections'!Y155","v":50},{"$f":"'Run Selections'!AI155","v":""},{"$f":"'Run Selections'!AA155","v":0},null,{"$f":"'Run Selections'!AL155","v":""},{"$f":"IF(D155=\"Select Model\",\"N/A\",throwCombined(F155, D155, S155, E155,J155))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D155=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K155, M155, N155, O155),0))","v":"N/A"},{"$f":"IF(D155=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K155,M155,N155,P155)),0))","v":"N/A"},{"$f":"'Run Selections'!BD155","v":0},{"$f":"IF(LEFT($D155,4)<>\"ACBC\",\"N/A\",AdjacentZone($D155,$E155,$S155,$F155,60))","v":"N/A"},{"$f":"IF(LEFT($D155,4)<>\"ACBC\",\"N/A\",AdjacentZone($D155,$E155,$S155,$F155,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F156)=\"\",\"\",'Run Selections'!F156)","v":""},null,{"$f":"'Run Selections'!T156","v":"Select Model"},{"$f":"'Run Selections'!W156","v":4},{"$f":"'Run Selections'!Y156","v":50},{"$f":"'Run Selections'!AI156","v":""},{"$f":"'Run Selections'!AA156","v":0},null,{"$f":"'Run Selections'!AL156","v":""},{"$f":"IF(D156=\"Select Model\",\"N/A\",throwCombined(F156, D156, S156, E156,J156))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D156=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K156, M156, N156, O156),0))","v":"N/A"},{"$f":"IF(D156=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K156,M156,N156,P156)),0))","v":"N/A"},{"$f":"'Run Selections'!BD156","v":0},{"$f":"IF(LEFT($D156,4)<>\"ACBC\",\"N/A\",AdjacentZone($D156,$E156,$S156,$F156,60))","v":"N/A"},{"$f":"IF(LEFT($D156,4)<>\"ACBC\",\"N/A\",AdjacentZone($D156,$E156,$S156,$F156,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F157)=\"\",\"\",'Run Selections'!F157)","v":""},null,{"$f":"'Run Selections'!T157","v":"Select Model"},{"$f":"'Run Selections'!W157","v":4},{"$f":"'Run Selections'!Y157","v":50},{"$f":"'Run Selections'!AI157","v":""},{"$f":"'Run Selections'!AA157","v":0},null,{"$f":"'Run Selections'!AL157","v":""},{"$f":"IF(D157=\"Select Model\",\"N/A\",throwCombined(F157, D157, S157, E157,J157))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D157=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K157, M157, N157, O157),0))","v":"N/A"},{"$f":"IF(D157=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K157,M157,N157,P157)),0))","v":"N/A"},{"$f":"'Run Selections'!BD157","v":0},{"$f":"IF(LEFT($D157,4)<>\"ACBC\",\"N/A\",AdjacentZone($D157,$E157,$S157,$F157,60))","v":"N/A"},{"$f":"IF(LEFT($D157,4)<>\"ACBC\",\"N/A\",AdjacentZone($D157,$E157,$S157,$F157,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F158)=\"\",\"\",'Run Selections'!F158)","v":""},null,{"$f":"'Run Selections'!T158","v":"Select Model"},{"$f":"'Run Selections'!W158","v":4},{"$f":"'Run Selections'!Y158","v":50},{"$f":"'Run Selections'!AI158","v":""},{"$f":"'Run Selections'!AA158","v":0},null,{"$f":"'Run Selections'!AL158","v":""},{"$f":"IF(D158=\"Select Model\",\"N/A\",throwCombined(F158, D158, S158, E158,J158))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D158=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K158, M158, N158, O158),0))","v":"N/A"},{"$f":"IF(D158=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K158,M158,N158,P158)),0))","v":"N/A"},{"$f":"'Run Selections'!BD158","v":0},{"$f":"IF(LEFT($D158,4)<>\"ACBC\",\"N/A\",AdjacentZone($D158,$E158,$S158,$F158,60))","v":"N/A"},{"$f":"IF(LEFT($D158,4)<>\"ACBC\",\"N/A\",AdjacentZone($D158,$E158,$S158,$F158,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F159)=\"\",\"\",'Run Selections'!F159)","v":""},null,{"$f":"'Run Selections'!T159","v":"Select Model"},{"$f":"'Run Selections'!W159","v":4},{"$f":"'Run Selections'!Y159","v":50},{"$f":"'Run Selections'!AI159","v":""},{"$f":"'Run Selections'!AA159","v":0},null,{"$f":"'Run Selections'!AL159","v":""},{"$f":"IF(D159=\"Select Model\",\"N/A\",throwCombined(F159, D159, S159, E159,J159))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D159=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K159, M159, N159, O159),0))","v":"N/A"},{"$f":"IF(D159=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K159,M159,N159,P159)),0))","v":"N/A"},{"$f":"'Run Selections'!BD159","v":0},{"$f":"IF(LEFT($D159,4)<>\"ACBC\",\"N/A\",AdjacentZone($D159,$E159,$S159,$F159,60))","v":"N/A"},{"$f":"IF(LEFT($D159,4)<>\"ACBC\",\"N/A\",AdjacentZone($D159,$E159,$S159,$F159,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F160)=\"\",\"\",'Run Selections'!F160)","v":""},null,{"$f":"'Run Selections'!T160","v":"Select Model"},{"$f":"'Run Selections'!W160","v":4},{"$f":"'Run Selections'!Y160","v":50},{"$f":"'Run Selections'!AI160","v":""},{"$f":"'Run Selections'!AA160","v":0},null,{"$f":"'Run Selections'!AL160","v":""},{"$f":"IF(D160=\"Select Model\",\"N/A\",throwCombined(F160, D160, S160, E160,J160))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D160=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K160, M160, N160, O160),0))","v":"N/A"},{"$f":"IF(D160=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K160,M160,N160,P160)),0))","v":"N/A"},{"$f":"'Run Selections'!BD160","v":0},{"$f":"IF(LEFT($D160,4)<>\"ACBC\",\"N/A\",AdjacentZone($D160,$E160,$S160,$F160,60))","v":"N/A"},{"$f":"IF(LEFT($D160,4)<>\"ACBC\",\"N/A\",AdjacentZone($D160,$E160,$S160,$F160,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F161)=\"\",\"\",'Run Selections'!F161)","v":""},null,{"$f":"'Run Selections'!T161","v":"Select Model"},{"$f":"'Run Selections'!W161","v":4},{"$f":"'Run Selections'!Y161","v":50},{"$f":"'Run Selections'!AI161","v":""},{"$f":"'Run Selections'!AA161","v":0},null,{"$f":"'Run Selections'!AL161","v":""},{"$f":"IF(D161=\"Select Model\",\"N/A\",throwCombined(F161, D161, S161, E161,J161))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D161=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K161, M161, N161, O161),0))","v":"N/A"},{"$f":"IF(D161=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K161,M161,N161,P161)),0))","v":"N/A"},{"$f":"'Run Selections'!BD161","v":0},{"$f":"IF(LEFT($D161,4)<>\"ACBC\",\"N/A\",AdjacentZone($D161,$E161,$S161,$F161,60))","v":"N/A"},{"$f":"IF(LEFT($D161,4)<>\"ACBC\",\"N/A\",AdjacentZone($D161,$E161,$S161,$F161,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F162)=\"\",\"\",'Run Selections'!F162)","v":""},null,{"$f":"'Run Selections'!T162","v":"Select Model"},{"$f":"'Run Selections'!W162","v":4},{"$f":"'Run Selections'!Y162","v":50},{"$f":"'Run Selections'!AI162","v":""},{"$f":"'Run Selections'!AA162","v":0},null,{"$f":"'Run Selections'!AL162","v":""},{"$f":"IF(D162=\"Select Model\",\"N/A\",throwCombined(F162, D162, S162, E162,J162))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D162=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K162, M162, N162, O162),0))","v":"N/A"},{"$f":"IF(D162=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K162,M162,N162,P162)),0))","v":"N/A"},{"$f":"'Run Selections'!BD162","v":0},{"$f":"IF(LEFT($D162,4)<>\"ACBC\",\"N/A\",AdjacentZone($D162,$E162,$S162,$F162,60))","v":"N/A"},{"$f":"IF(LEFT($D162,4)<>\"ACBC\",\"N/A\",AdjacentZone($D162,$E162,$S162,$F162,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F163)=\"\",\"\",'Run Selections'!F163)","v":""},null,{"$f":"'Run Selections'!T163","v":"Select Model"},{"$f":"'Run Selections'!W163","v":4},{"$f":"'Run Selections'!Y163","v":50},{"$f":"'Run Selections'!AI163","v":""},{"$f":"'Run Selections'!AA163","v":0},null,{"$f":"'Run Selections'!AL163","v":""},{"$f":"IF(D163=\"Select Model\",\"N/A\",throwCombined(F163, D163, S163, E163,J163))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D163=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K163, M163, N163, O163),0))","v":"N/A"},{"$f":"IF(D163=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K163,M163,N163,P163)),0))","v":"N/A"},{"$f":"'Run Selections'!BD163","v":0},{"$f":"IF(LEFT($D163,4)<>\"ACBC\",\"N/A\",AdjacentZone($D163,$E163,$S163,$F163,60))","v":"N/A"},{"$f":"IF(LEFT($D163,4)<>\"ACBC\",\"N/A\",AdjacentZone($D163,$E163,$S163,$F163,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F164)=\"\",\"\",'Run Selections'!F164)","v":""},null,{"$f":"'Run Selections'!T164","v":"Select Model"},{"$f":"'Run Selections'!W164","v":4},{"$f":"'Run Selections'!Y164","v":50},{"$f":"'Run Selections'!AI164","v":""},{"$f":"'Run Selections'!AA164","v":0},null,{"$f":"'Run Selections'!AL164","v":""},{"$f":"IF(D164=\"Select Model\",\"N/A\",throwCombined(F164, D164, S164, E164,J164))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D164=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K164, M164, N164, O164),0))","v":"N/A"},{"$f":"IF(D164=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K164,M164,N164,P164)),0))","v":"N/A"},{"$f":"'Run Selections'!BD164","v":0},{"$f":"IF(LEFT($D164,4)<>\"ACBC\",\"N/A\",AdjacentZone($D164,$E164,$S164,$F164,60))","v":"N/A"},{"$f":"IF(LEFT($D164,4)<>\"ACBC\",\"N/A\",AdjacentZone($D164,$E164,$S164,$F164,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F165)=\"\",\"\",'Run Selections'!F165)","v":""},null,{"$f":"'Run Selections'!T165","v":"Select Model"},{"$f":"'Run Selections'!W165","v":4},{"$f":"'Run Selections'!Y165","v":50},{"$f":"'Run Selections'!AI165","v":""},{"$f":"'Run Selections'!AA165","v":0},null,{"$f":"'Run Selections'!AL165","v":""},{"$f":"IF(D165=\"Select Model\",\"N/A\",throwCombined(F165, D165, S165, E165,J165))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D165=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K165, M165, N165, O165),0))","v":"N/A"},{"$f":"IF(D165=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K165,M165,N165,P165)),0))","v":"N/A"},{"$f":"'Run Selections'!BD165","v":0},{"$f":"IF(LEFT($D165,4)<>\"ACBC\",\"N/A\",AdjacentZone($D165,$E165,$S165,$F165,60))","v":"N/A"},{"$f":"IF(LEFT($D165,4)<>\"ACBC\",\"N/A\",AdjacentZone($D165,$E165,$S165,$F165,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F166)=\"\",\"\",'Run Selections'!F166)","v":""},null,{"$f":"'Run Selections'!T166","v":"Select Model"},{"$f":"'Run Selections'!W166","v":4},{"$f":"'Run Selections'!Y166","v":50},{"$f":"'Run Selections'!AI166","v":""},{"$f":"'Run Selections'!AA166","v":0},null,{"$f":"'Run Selections'!AL166","v":""},{"$f":"IF(D166=\"Select Model\",\"N/A\",throwCombined(F166, D166, S166, E166,J166))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D166=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K166, M166, N166, O166),0))","v":"N/A"},{"$f":"IF(D166=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K166,M166,N166,P166)),0))","v":"N/A"},{"$f":"'Run Selections'!BD166","v":0},{"$f":"IF(LEFT($D166,4)<>\"ACBC\",\"N/A\",AdjacentZone($D166,$E166,$S166,$F166,60))","v":"N/A"},{"$f":"IF(LEFT($D166,4)<>\"ACBC\",\"N/A\",AdjacentZone($D166,$E166,$S166,$F166,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F167)=\"\",\"\",'Run Selections'!F167)","v":""},null,{"$f":"'Run Selections'!T167","v":"Select Model"},{"$f":"'Run Selections'!W167","v":4},{"$f":"'Run Selections'!Y167","v":50},{"$f":"'Run Selections'!AI167","v":""},{"$f":"'Run Selections'!AA167","v":0},null,{"$f":"'Run Selections'!AL167","v":""},{"$f":"IF(D167=\"Select Model\",\"N/A\",throwCombined(F167, D167, S167, E167,J167))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D167=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K167, M167, N167, O167),0))","v":"N/A"},{"$f":"IF(D167=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K167,M167,N167,P167)),0))","v":"N/A"},{"$f":"'Run Selections'!BD167","v":0},{"$f":"IF(LEFT($D167,4)<>\"ACBC\",\"N/A\",AdjacentZone($D167,$E167,$S167,$F167,60))","v":"N/A"},{"$f":"IF(LEFT($D167,4)<>\"ACBC\",\"N/A\",AdjacentZone($D167,$E167,$S167,$F167,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F168)=\"\",\"\",'Run Selections'!F168)","v":""},null,{"$f":"'Run Selections'!T168","v":"Select Model"},{"$f":"'Run Selections'!W168","v":4},{"$f":"'Run Selections'!Y168","v":50},{"$f":"'Run Selections'!AI168","v":""},{"$f":"'Run Selections'!AA168","v":0},null,{"$f":"'Run Selections'!AL168","v":""},{"$f":"IF(D168=\"Select Model\",\"N/A\",throwCombined(F168, D168, S168, E168,J168))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D168=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K168, M168, N168, O168),0))","v":"N/A"},{"$f":"IF(D168=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K168,M168,N168,P168)),0))","v":"N/A"},{"$f":"'Run Selections'!BD168","v":0},{"$f":"IF(LEFT($D168,4)<>\"ACBC\",\"N/A\",AdjacentZone($D168,$E168,$S168,$F168,60))","v":"N/A"},{"$f":"IF(LEFT($D168,4)<>\"ACBC\",\"N/A\",AdjacentZone($D168,$E168,$S168,$F168,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F169)=\"\",\"\",'Run Selections'!F169)","v":""},null,{"$f":"'Run Selections'!T169","v":"Select Model"},{"$f":"'Run Selections'!W169","v":4},{"$f":"'Run Selections'!Y169","v":50},{"$f":"'Run Selections'!AI169","v":""},{"$f":"'Run Selections'!AA169","v":0},null,{"$f":"'Run Selections'!AL169","v":""},{"$f":"IF(D169=\"Select Model\",\"N/A\",throwCombined(F169, D169, S169, E169,J169))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D169=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K169, M169, N169, O169),0))","v":"N/A"},{"$f":"IF(D169=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K169,M169,N169,P169)),0))","v":"N/A"},{"$f":"'Run Selections'!BD169","v":0},{"$f":"IF(LEFT($D169,4)<>\"ACBC\",\"N/A\",AdjacentZone($D169,$E169,$S169,$F169,60))","v":"N/A"},{"$f":"IF(LEFT($D169,4)<>\"ACBC\",\"N/A\",AdjacentZone($D169,$E169,$S169,$F169,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F170)=\"\",\"\",'Run Selections'!F170)","v":""},null,{"$f":"'Run Selections'!T170","v":"Select Model"},{"$f":"'Run Selections'!W170","v":4},{"$f":"'Run Selections'!Y170","v":50},{"$f":"'Run Selections'!AI170","v":""},{"$f":"'Run Selections'!AA170","v":0},null,{"$f":"'Run Selections'!AL170","v":""},{"$f":"IF(D170=\"Select Model\",\"N/A\",throwCombined(F170, D170, S170, E170,J170))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D170=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K170, M170, N170, O170),0))","v":"N/A"},{"$f":"IF(D170=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K170,M170,N170,P170)),0))","v":"N/A"},{"$f":"'Run Selections'!BD170","v":0},{"$f":"IF(LEFT($D170,4)<>\"ACBC\",\"N/A\",AdjacentZone($D170,$E170,$S170,$F170,60))","v":"N/A"},{"$f":"IF(LEFT($D170,4)<>\"ACBC\",\"N/A\",AdjacentZone($D170,$E170,$S170,$F170,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F171)=\"\",\"\",'Run Selections'!F171)","v":""},null,{"$f":"'Run Selections'!T171","v":"Select Model"},{"$f":"'Run Selections'!W171","v":4},{"$f":"'Run Selections'!Y171","v":50},{"$f":"'Run Selections'!AI171","v":""},{"$f":"'Run Selections'!AA171","v":0},null,{"$f":"'Run Selections'!AL171","v":""},{"$f":"IF(D171=\"Select Model\",\"N/A\",throwCombined(F171, D171, S171, E171,J171))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D171=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K171, M171, N171, O171),0))","v":"N/A"},{"$f":"IF(D171=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K171,M171,N171,P171)),0))","v":"N/A"},{"$f":"'Run Selections'!BD171","v":0},{"$f":"IF(LEFT($D171,4)<>\"ACBC\",\"N/A\",AdjacentZone($D171,$E171,$S171,$F171,60))","v":"N/A"},{"$f":"IF(LEFT($D171,4)<>\"ACBC\",\"N/A\",AdjacentZone($D171,$E171,$S171,$F171,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F172)=\"\",\"\",'Run Selections'!F172)","v":""},null,{"$f":"'Run Selections'!T172","v":"Select Model"},{"$f":"'Run Selections'!W172","v":4},{"$f":"'Run Selections'!Y172","v":50},{"$f":"'Run Selections'!AI172","v":""},{"$f":"'Run Selections'!AA172","v":0},null,{"$f":"'Run Selections'!AL172","v":""},{"$f":"IF(D172=\"Select Model\",\"N/A\",throwCombined(F172, D172, S172, E172,J172))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D172=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K172, M172, N172, O172),0))","v":"N/A"},{"$f":"IF(D172=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K172,M172,N172,P172)),0))","v":"N/A"},{"$f":"'Run Selections'!BD172","v":0},{"$f":"IF(LEFT($D172,4)<>\"ACBC\",\"N/A\",AdjacentZone($D172,$E172,$S172,$F172,60))","v":"N/A"},{"$f":"IF(LEFT($D172,4)<>\"ACBC\",\"N/A\",AdjacentZone($D172,$E172,$S172,$F172,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F173)=\"\",\"\",'Run Selections'!F173)","v":""},null,{"$f":"'Run Selections'!T173","v":"Select Model"},{"$f":"'Run Selections'!W173","v":4},{"$f":"'Run Selections'!Y173","v":50},{"$f":"'Run Selections'!AI173","v":""},{"$f":"'Run Selections'!AA173","v":0},null,{"$f":"'Run Selections'!AL173","v":""},{"$f":"IF(D173=\"Select Model\",\"N/A\",throwCombined(F173, D173, S173, E173,J173))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D173=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K173, M173, N173, O173),0))","v":"N/A"},{"$f":"IF(D173=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K173,M173,N173,P173)),0))","v":"N/A"},{"$f":"'Run Selections'!BD173","v":0},{"$f":"IF(LEFT($D173,4)<>\"ACBC\",\"N/A\",AdjacentZone($D173,$E173,$S173,$F173,60))","v":"N/A"},{"$f":"IF(LEFT($D173,4)<>\"ACBC\",\"N/A\",AdjacentZone($D173,$E173,$S173,$F173,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F174)=\"\",\"\",'Run Selections'!F174)","v":""},null,{"$f":"'Run Selections'!T174","v":"Select Model"},{"$f":"'Run Selections'!W174","v":4},{"$f":"'Run Selections'!Y174","v":50},{"$f":"'Run Selections'!AI174","v":""},{"$f":"'Run Selections'!AA174","v":0},null,{"$f":"'Run Selections'!AL174","v":""},{"$f":"IF(D174=\"Select Model\",\"N/A\",throwCombined(F174, D174, S174, E174,J174))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D174=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K174, M174, N174, O174),0))","v":"N/A"},{"$f":"IF(D174=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K174,M174,N174,P174)),0))","v":"N/A"},{"$f":"'Run Selections'!BD174","v":0},{"$f":"IF(LEFT($D174,4)<>\"ACBC\",\"N/A\",AdjacentZone($D174,$E174,$S174,$F174,60))","v":"N/A"},{"$f":"IF(LEFT($D174,4)<>\"ACBC\",\"N/A\",AdjacentZone($D174,$E174,$S174,$F174,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F175)=\"\",\"\",'Run Selections'!F175)","v":""},null,{"$f":"'Run Selections'!T175","v":"Select Model"},{"$f":"'Run Selections'!W175","v":4},{"$f":"'Run Selections'!Y175","v":50},{"$f":"'Run Selections'!AI175","v":""},{"$f":"'Run Selections'!AA175","v":0},null,{"$f":"'Run Selections'!AL175","v":""},{"$f":"IF(D175=\"Select Model\",\"N/A\",throwCombined(F175, D175, S175, E175,J175))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D175=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K175, M175, N175, O175),0))","v":"N/A"},{"$f":"IF(D175=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K175,M175,N175,P175)),0))","v":"N/A"},{"$f":"'Run Selections'!BD175","v":0},{"$f":"IF(LEFT($D175,4)<>\"ACBC\",\"N/A\",AdjacentZone($D175,$E175,$S175,$F175,60))","v":"N/A"},{"$f":"IF(LEFT($D175,4)<>\"ACBC\",\"N/A\",AdjacentZone($D175,$E175,$S175,$F175,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F176)=\"\",\"\",'Run Selections'!F176)","v":""},null,{"$f":"'Run Selections'!T176","v":"Select Model"},{"$f":"'Run Selections'!W176","v":4},{"$f":"'Run Selections'!Y176","v":50},{"$f":"'Run Selections'!AI176","v":""},{"$f":"'Run Selections'!AA176","v":0},null,{"$f":"'Run Selections'!AL176","v":""},{"$f":"IF(D176=\"Select Model\",\"N/A\",throwCombined(F176, D176, S176, E176,J176))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D176=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K176, M176, N176, O176),0))","v":"N/A"},{"$f":"IF(D176=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K176,M176,N176,P176)),0))","v":"N/A"},{"$f":"'Run Selections'!BD176","v":0},{"$f":"IF(LEFT($D176,4)<>\"ACBC\",\"N/A\",AdjacentZone($D176,$E176,$S176,$F176,60))","v":"N/A"},{"$f":"IF(LEFT($D176,4)<>\"ACBC\",\"N/A\",AdjacentZone($D176,$E176,$S176,$F176,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F177)=\"\",\"\",'Run Selections'!F177)","v":""},null,{"$f":"'Run Selections'!T177","v":"Select Model"},{"$f":"'Run Selections'!W177","v":4},{"$f":"'Run Selections'!Y177","v":50},{"$f":"'Run Selections'!AI177","v":""},{"$f":"'Run Selections'!AA177","v":0},null,{"$f":"'Run Selections'!AL177","v":""},{"$f":"IF(D177=\"Select Model\",\"N/A\",throwCombined(F177, D177, S177, E177,J177))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D177=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K177, M177, N177, O177),0))","v":"N/A"},{"$f":"IF(D177=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K177,M177,N177,P177)),0))","v":"N/A"},{"$f":"'Run Selections'!BD177","v":0},{"$f":"IF(LEFT($D177,4)<>\"ACBC\",\"N/A\",AdjacentZone($D177,$E177,$S177,$F177,60))","v":"N/A"},{"$f":"IF(LEFT($D177,4)<>\"ACBC\",\"N/A\",AdjacentZone($D177,$E177,$S177,$F177,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F178)=\"\",\"\",'Run Selections'!F178)","v":""},null,{"$f":"'Run Selections'!T178","v":"Select Model"},{"$f":"'Run Selections'!W178","v":4},{"$f":"'Run Selections'!Y178","v":50},{"$f":"'Run Selections'!AI178","v":""},{"$f":"'Run Selections'!AA178","v":0},null,{"$f":"'Run Selections'!AL178","v":""},{"$f":"IF(D178=\"Select Model\",\"N/A\",throwCombined(F178, D178, S178, E178,J178))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D178=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K178, M178, N178, O178),0))","v":"N/A"},{"$f":"IF(D178=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K178,M178,N178,P178)),0))","v":"N/A"},{"$f":"'Run Selections'!BD178","v":0},{"$f":"IF(LEFT($D178,4)<>\"ACBC\",\"N/A\",AdjacentZone($D178,$E178,$S178,$F178,60))","v":"N/A"},{"$f":"IF(LEFT($D178,4)<>\"ACBC\",\"N/A\",AdjacentZone($D178,$E178,$S178,$F178,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F179)=\"\",\"\",'Run Selections'!F179)","v":""},null,{"$f":"'Run Selections'!T179","v":"Select Model"},{"$f":"'Run Selections'!W179","v":4},{"$f":"'Run Selections'!Y179","v":50},{"$f":"'Run Selections'!AI179","v":""},{"$f":"'Run Selections'!AA179","v":0},null,{"$f":"'Run Selections'!AL179","v":""},{"$f":"IF(D179=\"Select Model\",\"N/A\",throwCombined(F179, D179, S179, E179,J179))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D179=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K179, M179, N179, O179),0))","v":"N/A"},{"$f":"IF(D179=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K179,M179,N179,P179)),0))","v":"N/A"},{"$f":"'Run Selections'!BD179","v":0},{"$f":"IF(LEFT($D179,4)<>\"ACBC\",\"N/A\",AdjacentZone($D179,$E179,$S179,$F179,60))","v":"N/A"},{"$f":"IF(LEFT($D179,4)<>\"ACBC\",\"N/A\",AdjacentZone($D179,$E179,$S179,$F179,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F180)=\"\",\"\",'Run Selections'!F180)","v":""},null,{"$f":"'Run Selections'!T180","v":"Select Model"},{"$f":"'Run Selections'!W180","v":4},{"$f":"'Run Selections'!Y180","v":50},{"$f":"'Run Selections'!AI180","v":""},{"$f":"'Run Selections'!AA180","v":0},null,{"$f":"'Run Selections'!AL180","v":""},{"$f":"IF(D180=\"Select Model\",\"N/A\",throwCombined(F180, D180, S180, E180,J180))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D180=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K180, M180, N180, O180),0))","v":"N/A"},{"$f":"IF(D180=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K180,M180,N180,P180)),0))","v":"N/A"},{"$f":"'Run Selections'!BD180","v":0},{"$f":"IF(LEFT($D180,4)<>\"ACBC\",\"N/A\",AdjacentZone($D180,$E180,$S180,$F180,60))","v":"N/A"},{"$f":"IF(LEFT($D180,4)<>\"ACBC\",\"N/A\",AdjacentZone($D180,$E180,$S180,$F180,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F181)=\"\",\"\",'Run Selections'!F181)","v":""},null,{"$f":"'Run Selections'!T181","v":"Select Model"},{"$f":"'Run Selections'!W181","v":4},{"$f":"'Run Selections'!Y181","v":50},{"$f":"'Run Selections'!AI181","v":""},{"$f":"'Run Selections'!AA181","v":0},null,{"$f":"'Run Selections'!AL181","v":""},{"$f":"IF(D181=\"Select Model\",\"N/A\",throwCombined(F181, D181, S181, E181,J181))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D181=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K181, M181, N181, O181),0))","v":"N/A"},{"$f":"IF(D181=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K181,M181,N181,P181)),0))","v":"N/A"},{"$f":"'Run Selections'!BD181","v":0},{"$f":"IF(LEFT($D181,4)<>\"ACBC\",\"N/A\",AdjacentZone($D181,$E181,$S181,$F181,60))","v":"N/A"},{"$f":"IF(LEFT($D181,4)<>\"ACBC\",\"N/A\",AdjacentZone($D181,$E181,$S181,$F181,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F182)=\"\",\"\",'Run Selections'!F182)","v":""},null,{"$f":"'Run Selections'!T182","v":"Select Model"},{"$f":"'Run Selections'!W182","v":4},{"$f":"'Run Selections'!Y182","v":50},{"$f":"'Run Selections'!AI182","v":""},{"$f":"'Run Selections'!AA182","v":0},null,{"$f":"'Run Selections'!AL182","v":""},{"$f":"IF(D182=\"Select Model\",\"N/A\",throwCombined(F182, D182, S182, E182,J182))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D182=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K182, M182, N182, O182),0))","v":"N/A"},{"$f":"IF(D182=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K182,M182,N182,P182)),0))","v":"N/A"},{"$f":"'Run Selections'!BD182","v":0},{"$f":"IF(LEFT($D182,4)<>\"ACBC\",\"N/A\",AdjacentZone($D182,$E182,$S182,$F182,60))","v":"N/A"},{"$f":"IF(LEFT($D182,4)<>\"ACBC\",\"N/A\",AdjacentZone($D182,$E182,$S182,$F182,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F183)=\"\",\"\",'Run Selections'!F183)","v":""},null,{"$f":"'Run Selections'!T183","v":"Select Model"},{"$f":"'Run Selections'!W183","v":4},{"$f":"'Run Selections'!Y183","v":50},{"$f":"'Run Selections'!AI183","v":""},{"$f":"'Run Selections'!AA183","v":0},null,{"$f":"'Run Selections'!AL183","v":""},{"$f":"IF(D183=\"Select Model\",\"N/A\",throwCombined(F183, D183, S183, E183,J183))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D183=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K183, M183, N183, O183),0))","v":"N/A"},{"$f":"IF(D183=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K183,M183,N183,P183)),0))","v":"N/A"},{"$f":"'Run Selections'!BD183","v":0},{"$f":"IF(LEFT($D183,4)<>\"ACBC\",\"N/A\",AdjacentZone($D183,$E183,$S183,$F183,60))","v":"N/A"},{"$f":"IF(LEFT($D183,4)<>\"ACBC\",\"N/A\",AdjacentZone($D183,$E183,$S183,$F183,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F184)=\"\",\"\",'Run Selections'!F184)","v":""},null,{"$f":"'Run Selections'!T184","v":"Select Model"},{"$f":"'Run Selections'!W184","v":4},{"$f":"'Run Selections'!Y184","v":50},{"$f":"'Run Selections'!AI184","v":""},{"$f":"'Run Selections'!AA184","v":0},null,{"$f":"'Run Selections'!AL184","v":""},{"$f":"IF(D184=\"Select Model\",\"N/A\",throwCombined(F184, D184, S184, E184,J184))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D184=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K184, M184, N184, O184),0))","v":"N/A"},{"$f":"IF(D184=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K184,M184,N184,P184)),0))","v":"N/A"},{"$f":"'Run Selections'!BD184","v":0},{"$f":"IF(LEFT($D184,4)<>\"ACBC\",\"N/A\",AdjacentZone($D184,$E184,$S184,$F184,60))","v":"N/A"},{"$f":"IF(LEFT($D184,4)<>\"ACBC\",\"N/A\",AdjacentZone($D184,$E184,$S184,$F184,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F185)=\"\",\"\",'Run Selections'!F185)","v":""},null,{"$f":"'Run Selections'!T185","v":"Select Model"},{"$f":"'Run Selections'!W185","v":4},{"$f":"'Run Selections'!Y185","v":50},{"$f":"'Run Selections'!AI185","v":""},{"$f":"'Run Selections'!AA185","v":0},null,{"$f":"'Run Selections'!AL185","v":""},{"$f":"IF(D185=\"Select Model\",\"N/A\",throwCombined(F185, D185, S185, E185,J185))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D185=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K185, M185, N185, O185),0))","v":"N/A"},{"$f":"IF(D185=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K185,M185,N185,P185)),0))","v":"N/A"},{"$f":"'Run Selections'!BD185","v":0},{"$f":"IF(LEFT($D185,4)<>\"ACBC\",\"N/A\",AdjacentZone($D185,$E185,$S185,$F185,60))","v":"N/A"},{"$f":"IF(LEFT($D185,4)<>\"ACBC\",\"N/A\",AdjacentZone($D185,$E185,$S185,$F185,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F186)=\"\",\"\",'Run Selections'!F186)","v":""},null,{"$f":"'Run Selections'!T186","v":"Select Model"},{"$f":"'Run Selections'!W186","v":4},{"$f":"'Run Selections'!Y186","v":50},{"$f":"'Run Selections'!AI186","v":""},{"$f":"'Run Selections'!AA186","v":0},null,{"$f":"'Run Selections'!AL186","v":""},{"$f":"IF(D186=\"Select Model\",\"N/A\",throwCombined(F186, D186, S186, E186,J186))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D186=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K186, M186, N186, O186),0))","v":"N/A"},{"$f":"IF(D186=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K186,M186,N186,P186)),0))","v":"N/A"},{"$f":"'Run Selections'!BD186","v":0},{"$f":"IF(LEFT($D186,4)<>\"ACBC\",\"N/A\",AdjacentZone($D186,$E186,$S186,$F186,60))","v":"N/A"},{"$f":"IF(LEFT($D186,4)<>\"ACBC\",\"N/A\",AdjacentZone($D186,$E186,$S186,$F186,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F187)=\"\",\"\",'Run Selections'!F187)","v":""},null,{"$f":"'Run Selections'!T187","v":"Select Model"},{"$f":"'Run Selections'!W187","v":4},{"$f":"'Run Selections'!Y187","v":50},{"$f":"'Run Selections'!AI187","v":""},{"$f":"'Run Selections'!AA187","v":0},null,{"$f":"'Run Selections'!AL187","v":""},{"$f":"IF(D187=\"Select Model\",\"N/A\",throwCombined(F187, D187, S187, E187,J187))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D187=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K187, M187, N187, O187),0))","v":"N/A"},{"$f":"IF(D187=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K187,M187,N187,P187)),0))","v":"N/A"},{"$f":"'Run Selections'!BD187","v":0},{"$f":"IF(LEFT($D187,4)<>\"ACBC\",\"N/A\",AdjacentZone($D187,$E187,$S187,$F187,60))","v":"N/A"},{"$f":"IF(LEFT($D187,4)<>\"ACBC\",\"N/A\",AdjacentZone($D187,$E187,$S187,$F187,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F188)=\"\",\"\",'Run Selections'!F188)","v":""},null,{"$f":"'Run Selections'!T188","v":"Select Model"},{"$f":"'Run Selections'!W188","v":4},{"$f":"'Run Selections'!Y188","v":50},{"$f":"'Run Selections'!AI188","v":""},{"$f":"'Run Selections'!AA188","v":0},null,{"$f":"'Run Selections'!AL188","v":""},{"$f":"IF(D188=\"Select Model\",\"N/A\",throwCombined(F188, D188, S188, E188,J188))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D188=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K188, M188, N188, O188),0))","v":"N/A"},{"$f":"IF(D188=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K188,M188,N188,P188)),0))","v":"N/A"},{"$f":"'Run Selections'!BD188","v":0},{"$f":"IF(LEFT($D188,4)<>\"ACBC\",\"N/A\",AdjacentZone($D188,$E188,$S188,$F188,60))","v":"N/A"},{"$f":"IF(LEFT($D188,4)<>\"ACBC\",\"N/A\",AdjacentZone($D188,$E188,$S188,$F188,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F189)=\"\",\"\",'Run Selections'!F189)","v":""},null,{"$f":"'Run Selections'!T189","v":"Select Model"},{"$f":"'Run Selections'!W189","v":4},{"$f":"'Run Selections'!Y189","v":50},{"$f":"'Run Selections'!AI189","v":""},{"$f":"'Run Selections'!AA189","v":0},null,{"$f":"'Run Selections'!AL189","v":""},{"$f":"IF(D189=\"Select Model\",\"N/A\",throwCombined(F189, D189, S189, E189,J189))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D189=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K189, M189, N189, O189),0))","v":"N/A"},{"$f":"IF(D189=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K189,M189,N189,P189)),0))","v":"N/A"},{"$f":"'Run Selections'!BD189","v":0},{"$f":"IF(LEFT($D189,4)<>\"ACBC\",\"N/A\",AdjacentZone($D189,$E189,$S189,$F189,60))","v":"N/A"},{"$f":"IF(LEFT($D189,4)<>\"ACBC\",\"N/A\",AdjacentZone($D189,$E189,$S189,$F189,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F190)=\"\",\"\",'Run Selections'!F190)","v":""},null,{"$f":"'Run Selections'!T190","v":"Select Model"},{"$f":"'Run Selections'!W190","v":4},{"$f":"'Run Selections'!Y190","v":50},{"$f":"'Run Selections'!AI190","v":""},{"$f":"'Run Selections'!AA190","v":0},null,{"$f":"'Run Selections'!AL190","v":""},{"$f":"IF(D190=\"Select Model\",\"N/A\",throwCombined(F190, D190, S190, E190,J190))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D190=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K190, M190, N190, O190),0))","v":"N/A"},{"$f":"IF(D190=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K190,M190,N190,P190)),0))","v":"N/A"},{"$f":"'Run Selections'!BD190","v":0},{"$f":"IF(LEFT($D190,4)<>\"ACBC\",\"N/A\",AdjacentZone($D190,$E190,$S190,$F190,60))","v":"N/A"},{"$f":"IF(LEFT($D190,4)<>\"ACBC\",\"N/A\",AdjacentZone($D190,$E190,$S190,$F190,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F191)=\"\",\"\",'Run Selections'!F191)","v":""},null,{"$f":"'Run Selections'!T191","v":"Select Model"},{"$f":"'Run Selections'!W191","v":4},{"$f":"'Run Selections'!Y191","v":50},{"$f":"'Run Selections'!AI191","v":""},{"$f":"'Run Selections'!AA191","v":0},null,{"$f":"'Run Selections'!AL191","v":""},{"$f":"IF(D191=\"Select Model\",\"N/A\",throwCombined(F191, D191, S191, E191,J191))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D191=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K191, M191, N191, O191),0))","v":"N/A"},{"$f":"IF(D191=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K191,M191,N191,P191)),0))","v":"N/A"},{"$f":"'Run Selections'!BD191","v":0},{"$f":"IF(LEFT($D191,4)<>\"ACBC\",\"N/A\",AdjacentZone($D191,$E191,$S191,$F191,60))","v":"N/A"},{"$f":"IF(LEFT($D191,4)<>\"ACBC\",\"N/A\",AdjacentZone($D191,$E191,$S191,$F191,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F192)=\"\",\"\",'Run Selections'!F192)","v":""},null,{"$f":"'Run Selections'!T192","v":"Select Model"},{"$f":"'Run Selections'!W192","v":4},{"$f":"'Run Selections'!Y192","v":50},{"$f":"'Run Selections'!AI192","v":""},{"$f":"'Run Selections'!AA192","v":0},null,{"$f":"'Run Selections'!AL192","v":""},{"$f":"IF(D192=\"Select Model\",\"N/A\",throwCombined(F192, D192, S192, E192,J192))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D192=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K192, M192, N192, O192),0))","v":"N/A"},{"$f":"IF(D192=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K192,M192,N192,P192)),0))","v":"N/A"},{"$f":"'Run Selections'!BD192","v":0},{"$f":"IF(LEFT($D192,4)<>\"ACBC\",\"N/A\",AdjacentZone($D192,$E192,$S192,$F192,60))","v":"N/A"},{"$f":"IF(LEFT($D192,4)<>\"ACBC\",\"N/A\",AdjacentZone($D192,$E192,$S192,$F192,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F193)=\"\",\"\",'Run Selections'!F193)","v":""},null,{"$f":"'Run Selections'!T193","v":"Select Model"},{"$f":"'Run Selections'!W193","v":4},{"$f":"'Run Selections'!Y193","v":50},{"$f":"'Run Selections'!AI193","v":""},{"$f":"'Run Selections'!AA193","v":0},null,{"$f":"'Run Selections'!AL193","v":""},{"$f":"IF(D193=\"Select Model\",\"N/A\",throwCombined(F193, D193, S193, E193,J193))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D193=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K193, M193, N193, O193),0))","v":"N/A"},{"$f":"IF(D193=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K193,M193,N193,P193)),0))","v":"N/A"},{"$f":"'Run Selections'!BD193","v":0},{"$f":"IF(LEFT($D193,4)<>\"ACBC\",\"N/A\",AdjacentZone($D193,$E193,$S193,$F193,60))","v":"N/A"},{"$f":"IF(LEFT($D193,4)<>\"ACBC\",\"N/A\",AdjacentZone($D193,$E193,$S193,$F193,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F194)=\"\",\"\",'Run Selections'!F194)","v":""},null,{"$f":"'Run Selections'!T194","v":"Select Model"},{"$f":"'Run Selections'!W194","v":4},{"$f":"'Run Selections'!Y194","v":50},{"$f":"'Run Selections'!AI194","v":""},{"$f":"'Run Selections'!AA194","v":0},null,{"$f":"'Run Selections'!AL194","v":""},{"$f":"IF(D194=\"Select Model\",\"N/A\",throwCombined(F194, D194, S194, E194,J194))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D194=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K194, M194, N194, O194),0))","v":"N/A"},{"$f":"IF(D194=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K194,M194,N194,P194)),0))","v":"N/A"},{"$f":"'Run Selections'!BD194","v":0},{"$f":"IF(LEFT($D194,4)<>\"ACBC\",\"N/A\",AdjacentZone($D194,$E194,$S194,$F194,60))","v":"N/A"},{"$f":"IF(LEFT($D194,4)<>\"ACBC\",\"N/A\",AdjacentZone($D194,$E194,$S194,$F194,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F195)=\"\",\"\",'Run Selections'!F195)","v":""},null,{"$f":"'Run Selections'!T195","v":"Select Model"},{"$f":"'Run Selections'!W195","v":4},{"$f":"'Run Selections'!Y195","v":50},{"$f":"'Run Selections'!AI195","v":""},{"$f":"'Run Selections'!AA195","v":0},null,{"$f":"'Run Selections'!AL195","v":""},{"$f":"IF(D195=\"Select Model\",\"N/A\",throwCombined(F195, D195, S195, E195,J195))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D195=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K195, M195, N195, O195),0))","v":"N/A"},{"$f":"IF(D195=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K195,M195,N195,P195)),0))","v":"N/A"},{"$f":"'Run Selections'!BD195","v":0},{"$f":"IF(LEFT($D195,4)<>\"ACBC\",\"N/A\",AdjacentZone($D195,$E195,$S195,$F195,60))","v":"N/A"},{"$f":"IF(LEFT($D195,4)<>\"ACBC\",\"N/A\",AdjacentZone($D195,$E195,$S195,$F195,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F196)=\"\",\"\",'Run Selections'!F196)","v":""},null,{"$f":"'Run Selections'!T196","v":"Select Model"},{"$f":"'Run Selections'!W196","v":4},{"$f":"'Run Selections'!Y196","v":50},{"$f":"'Run Selections'!AI196","v":""},{"$f":"'Run Selections'!AA196","v":0},null,{"$f":"'Run Selections'!AL196","v":""},{"$f":"IF(D196=\"Select Model\",\"N/A\",throwCombined(F196, D196, S196, E196,J196))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D196=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K196, M196, N196, O196),0))","v":"N/A"},{"$f":"IF(D196=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K196,M196,N196,P196)),0))","v":"N/A"},{"$f":"'Run Selections'!BD196","v":0},{"$f":"IF(LEFT($D196,4)<>\"ACBC\",\"N/A\",AdjacentZone($D196,$E196,$S196,$F196,60))","v":"N/A"},{"$f":"IF(LEFT($D196,4)<>\"ACBC\",\"N/A\",AdjacentZone($D196,$E196,$S196,$F196,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F197)=\"\",\"\",'Run Selections'!F197)","v":""},null,{"$f":"'Run Selections'!T197","v":"Select Model"},{"$f":"'Run Selections'!W197","v":4},{"$f":"'Run Selections'!Y197","v":50},{"$f":"'Run Selections'!AI197","v":""},{"$f":"'Run Selections'!AA197","v":0},null,{"$f":"'Run Selections'!AL197","v":""},{"$f":"IF(D197=\"Select Model\",\"N/A\",throwCombined(F197, D197, S197, E197,J197))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D197=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K197, M197, N197, O197),0))","v":"N/A"},{"$f":"IF(D197=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K197,M197,N197,P197)),0))","v":"N/A"},{"$f":"'Run Selections'!BD197","v":0},{"$f":"IF(LEFT($D197,4)<>\"ACBC\",\"N/A\",AdjacentZone($D197,$E197,$S197,$F197,60))","v":"N/A"},{"$f":"IF(LEFT($D197,4)<>\"ACBC\",\"N/A\",AdjacentZone($D197,$E197,$S197,$F197,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F198)=\"\",\"\",'Run Selections'!F198)","v":""},null,{"$f":"'Run Selections'!T198","v":"Select Model"},{"$f":"'Run Selections'!W198","v":4},{"$f":"'Run Selections'!Y198","v":50},{"$f":"'Run Selections'!AI198","v":""},{"$f":"'Run Selections'!AA198","v":0},null,{"$f":"'Run Selections'!AL198","v":""},{"$f":"IF(D198=\"Select Model\",\"N/A\",throwCombined(F198, D198, S198, E198,J198))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D198=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K198, M198, N198, O198),0))","v":"N/A"},{"$f":"IF(D198=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K198,M198,N198,P198)),0))","v":"N/A"},{"$f":"'Run Selections'!BD198","v":0},{"$f":"IF(LEFT($D198,4)<>\"ACBC\",\"N/A\",AdjacentZone($D198,$E198,$S198,$F198,60))","v":"N/A"},{"$f":"IF(LEFT($D198,4)<>\"ACBC\",\"N/A\",AdjacentZone($D198,$E198,$S198,$F198,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F199)=\"\",\"\",'Run Selections'!F199)","v":""},null,{"$f":"'Run Selections'!T199","v":"Select Model"},{"$f":"'Run Selections'!W199","v":4},{"$f":"'Run Selections'!Y199","v":50},{"$f":"'Run Selections'!AI199","v":""},{"$f":"'Run Selections'!AA199","v":0},null,{"$f":"'Run Selections'!AL199","v":""},{"$f":"IF(D199=\"Select Model\",\"N/A\",throwCombined(F199, D199, S199, E199,J199))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D199=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K199, M199, N199, O199),0))","v":"N/A"},{"$f":"IF(D199=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K199,M199,N199,P199)),0))","v":"N/A"},{"$f":"'Run Selections'!BD199","v":0},{"$f":"IF(LEFT($D199,4)<>\"ACBC\",\"N/A\",AdjacentZone($D199,$E199,$S199,$F199,60))","v":"N/A"},{"$f":"IF(LEFT($D199,4)<>\"ACBC\",\"N/A\",AdjacentZone($D199,$E199,$S199,$F199,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F200)=\"\",\"\",'Run Selections'!F200)","v":""},null,{"$f":"'Run Selections'!T200","v":"Select Model"},{"$f":"'Run Selections'!W200","v":4},{"$f":"'Run Selections'!Y200","v":50},{"$f":"'Run Selections'!AI200","v":""},{"$f":"'Run Selections'!AA200","v":0},null,{"$f":"'Run Selections'!AL200","v":""},{"$f":"IF(D200=\"Select Model\",\"N/A\",throwCombined(F200, D200, S200, E200,J200))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D200=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K200, M200, N200, O200),0))","v":"N/A"},{"$f":"IF(D200=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K200,M200,N200,P200)),0))","v":"N/A"},{"$f":"'Run Selections'!BD200","v":0},{"$f":"IF(LEFT($D200,4)<>\"ACBC\",\"N/A\",AdjacentZone($D200,$E200,$S200,$F200,60))","v":"N/A"},{"$f":"IF(LEFT($D200,4)<>\"ACBC\",\"N/A\",AdjacentZone($D200,$E200,$S200,$F200,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F201)=\"\",\"\",'Run Selections'!F201)","v":""},null,{"$f":"'Run Selections'!T201","v":"Select Model"},{"$f":"'Run Selections'!W201","v":4},{"$f":"'Run Selections'!Y201","v":50},{"$f":"'Run Selections'!AI201","v":""},{"$f":"'Run Selections'!AA201","v":0},null,{"$f":"'Run Selections'!AL201","v":""},{"$f":"IF(D201=\"Select Model\",\"N/A\",throwCombined(F201, D201, S201, E201,J201))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D201=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K201, M201, N201, O201),0))","v":"N/A"},{"$f":"IF(D201=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K201,M201,N201,P201)),0))","v":"N/A"},{"$f":"'Run Selections'!BD201","v":0},{"$f":"IF(LEFT($D201,4)<>\"ACBC\",\"N/A\",AdjacentZone($D201,$E201,$S201,$F201,60))","v":"N/A"},{"$f":"IF(LEFT($D201,4)<>\"ACBC\",\"N/A\",AdjacentZone($D201,$E201,$S201,$F201,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F202)=\"\",\"\",'Run Selections'!F202)","v":""},null,{"$f":"'Run Selections'!T202","v":"Select Model"},{"$f":"'Run Selections'!W202","v":4},{"$f":"'Run Selections'!Y202","v":50},{"$f":"'Run Selections'!AI202","v":""},{"$f":"'Run Selections'!AA202","v":0},null,{"$f":"'Run Selections'!AL202","v":""},{"$f":"IF(D202=\"Select Model\",\"N/A\",throwCombined(F202, D202, S202, E202,J202))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D202=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K202, M202, N202, O202),0))","v":"N/A"},{"$f":"IF(D202=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K202,M202,N202,P202)),0))","v":"N/A"},{"$f":"'Run Selections'!BD202","v":0},{"$f":"IF(LEFT($D202,4)<>\"ACBC\",\"N/A\",AdjacentZone($D202,$E202,$S202,$F202,60))","v":"N/A"},{"$f":"IF(LEFT($D202,4)<>\"ACBC\",\"N/A\",AdjacentZone($D202,$E202,$S202,$F202,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F203)=\"\",\"\",'Run Selections'!F203)","v":""},null,{"$f":"'Run Selections'!T203","v":"Select Model"},{"$f":"'Run Selections'!W203","v":4},{"$f":"'Run Selections'!Y203","v":50},{"$f":"'Run Selections'!AI203","v":""},{"$f":"'Run Selections'!AA203","v":0},null,{"$f":"'Run Selections'!AL203","v":""},{"$f":"IF(D203=\"Select Model\",\"N/A\",throwCombined(F203, D203, S203, E203,J203))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D203=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K203, M203, N203, O203),0))","v":"N/A"},{"$f":"IF(D203=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K203,M203,N203,P203)),0))","v":"N/A"},{"$f":"'Run Selections'!BD203","v":0},{"$f":"IF(LEFT($D203,4)<>\"ACBC\",\"N/A\",AdjacentZone($D203,$E203,$S203,$F203,60))","v":"N/A"},{"$f":"IF(LEFT($D203,4)<>\"ACBC\",\"N/A\",AdjacentZone($D203,$E203,$S203,$F203,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F204)=\"\",\"\",'Run Selections'!F204)","v":""},null,{"$f":"'Run Selections'!T204","v":"Select Model"},{"$f":"'Run Selections'!W204","v":4},{"$f":"'Run Selections'!Y204","v":50},{"$f":"'Run Selections'!AI204","v":""},{"$f":"'Run Selections'!AA204","v":0},null,{"$f":"'Run Selections'!AL204","v":""},{"$f":"IF(D204=\"Select Model\",\"N/A\",throwCombined(F204, D204, S204, E204,J204))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D204=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K204, M204, N204, O204),0))","v":"N/A"},{"$f":"IF(D204=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K204,M204,N204,P204)),0))","v":"N/A"},{"$f":"'Run Selections'!BD204","v":0},{"$f":"IF(LEFT($D204,4)<>\"ACBC\",\"N/A\",AdjacentZone($D204,$E204,$S204,$F204,60))","v":"N/A"},{"$f":"IF(LEFT($D204,4)<>\"ACBC\",\"N/A\",AdjacentZone($D204,$E204,$S204,$F204,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F205)=\"\",\"\",'Run Selections'!F205)","v":""},null,{"$f":"'Run Selections'!T205","v":"Select Model"},{"$f":"'Run Selections'!W205","v":4},{"$f":"'Run Selections'!Y205","v":50},{"$f":"'Run Selections'!AI205","v":""},{"$f":"'Run Selections'!AA205","v":0},null,{"$f":"'Run Selections'!AL205","v":""},{"$f":"IF(D205=\"Select Model\",\"N/A\",throwCombined(F205, D205, S205, E205,J205))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D205=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K205, M205, N205, O205),0))","v":"N/A"},{"$f":"IF(D205=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K205,M205,N205,P205)),0))","v":"N/A"},{"$f":"'Run Selections'!BD205","v":0},{"$f":"IF(LEFT($D205,4)<>\"ACBC\",\"N/A\",AdjacentZone($D205,$E205,$S205,$F205,60))","v":"N/A"},{"$f":"IF(LEFT($D205,4)<>\"ACBC\",\"N/A\",AdjacentZone($D205,$E205,$S205,$F205,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F206)=\"\",\"\",'Run Selections'!F206)","v":""},null,{"$f":"'Run Selections'!T206","v":"Select Model"},{"$f":"'Run Selections'!W206","v":4},{"$f":"'Run Selections'!Y206","v":50},{"$f":"'Run Selections'!AI206","v":""},{"$f":"'Run Selections'!AA206","v":0},null,{"$f":"'Run Selections'!AL206","v":""},{"$f":"IF(D206=\"Select Model\",\"N/A\",throwCombined(F206, D206, S206, E206,J206))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D206=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K206, M206, N206, O206),0))","v":"N/A"},{"$f":"IF(D206=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K206,M206,N206,P206)),0))","v":"N/A"},{"$f":"'Run Selections'!BD206","v":0},{"$f":"IF(LEFT($D206,4)<>\"ACBC\",\"N/A\",AdjacentZone($D206,$E206,$S206,$F206,60))","v":"N/A"},{"$f":"IF(LEFT($D206,4)<>\"ACBC\",\"N/A\",AdjacentZone($D206,$E206,$S206,$F206,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F207)=\"\",\"\",'Run Selections'!F207)","v":""},null,{"$f":"'Run Selections'!T207","v":"Select Model"},{"$f":"'Run Selections'!W207","v":4},{"$f":"'Run Selections'!Y207","v":50},{"$f":"'Run Selections'!AI207","v":""},{"$f":"'Run Selections'!AA207","v":0},null,{"$f":"'Run Selections'!AL207","v":""},{"$f":"IF(D207=\"Select Model\",\"N/A\",throwCombined(F207, D207, S207, E207,J207))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D207=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K207, M207, N207, O207),0))","v":"N/A"},{"$f":"IF(D207=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K207,M207,N207,P207)),0))","v":"N/A"},{"$f":"'Run Selections'!BD207","v":0},{"$f":"IF(LEFT($D207,4)<>\"ACBC\",\"N/A\",AdjacentZone($D207,$E207,$S207,$F207,60))","v":"N/A"},{"$f":"IF(LEFT($D207,4)<>\"ACBC\",\"N/A\",AdjacentZone($D207,$E207,$S207,$F207,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F208)=\"\",\"\",'Run Selections'!F208)","v":""},null,{"$f":"'Run Selections'!T208","v":"Select Model"},{"$f":"'Run Selections'!W208","v":4},{"$f":"'Run Selections'!Y208","v":50},{"$f":"'Run Selections'!AI208","v":""},{"$f":"'Run Selections'!AA208","v":0},null,{"$f":"'Run Selections'!AL208","v":""},{"$f":"IF(D208=\"Select Model\",\"N/A\",throwCombined(F208, D208, S208, E208,J208))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D208=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K208, M208, N208, O208),0))","v":"N/A"},{"$f":"IF(D208=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K208,M208,N208,P208)),0))","v":"N/A"},{"$f":"'Run Selections'!BD208","v":0},{"$f":"IF(LEFT($D208,4)<>\"ACBC\",\"N/A\",AdjacentZone($D208,$E208,$S208,$F208,60))","v":"N/A"},{"$f":"IF(LEFT($D208,4)<>\"ACBC\",\"N/A\",AdjacentZone($D208,$E208,$S208,$F208,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F209)=\"\",\"\",'Run Selections'!F209)","v":""},null,{"$f":"'Run Selections'!T209","v":"Select Model"},{"$f":"'Run Selections'!W209","v":4},{"$f":"'Run Selections'!Y209","v":50},{"$f":"'Run Selections'!AI209","v":""},{"$f":"'Run Selections'!AA209","v":0},null,{"$f":"'Run Selections'!AL209","v":""},{"$f":"IF(D209=\"Select Model\",\"N/A\",throwCombined(F209, D209, S209, E209,J209))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D209=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K209, M209, N209, O209),0))","v":"N/A"},{"$f":"IF(D209=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K209,M209,N209,P209)),0))","v":"N/A"},{"$f":"'Run Selections'!BD209","v":0},{"$f":"IF(LEFT($D209,4)<>\"ACBC\",\"N/A\",AdjacentZone($D209,$E209,$S209,$F209,60))","v":"N/A"},{"$f":"IF(LEFT($D209,4)<>\"ACBC\",\"N/A\",AdjacentZone($D209,$E209,$S209,$F209,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F210)=\"\",\"\",'Run Selections'!F210)","v":""},null,{"$f":"'Run Selections'!T210","v":"Select Model"},{"$f":"'Run Selections'!W210","v":4},{"$f":"'Run Selections'!Y210","v":50},{"$f":"'Run Selections'!AI210","v":""},{"$f":"'Run Selections'!AA210","v":0},null,{"$f":"'Run Selections'!AL210","v":""},{"$f":"IF(D210=\"Select Model\",\"N/A\",throwCombined(F210, D210, S210, E210,J210))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D210=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K210, M210, N210, O210),0))","v":"N/A"},{"$f":"IF(D210=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K210,M210,N210,P210)),0))","v":"N/A"},{"$f":"'Run Selections'!BD210","v":0},{"$f":"IF(LEFT($D210,4)<>\"ACBC\",\"N/A\",AdjacentZone($D210,$E210,$S210,$F210,60))","v":"N/A"},{"$f":"IF(LEFT($D210,4)<>\"ACBC\",\"N/A\",AdjacentZone($D210,$E210,$S210,$F210,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F211)=\"\",\"\",'Run Selections'!F211)","v":""},null,{"$f":"'Run Selections'!T211","v":"Select Model"},{"$f":"'Run Selections'!W211","v":4},{"$f":"'Run Selections'!Y211","v":50},{"$f":"'Run Selections'!AI211","v":""},{"$f":"'Run Selections'!AA211","v":0},null,{"$f":"'Run Selections'!AL211","v":""},{"$f":"IF(D211=\"Select Model\",\"N/A\",throwCombined(F211, D211, S211, E211,J211))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D211=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K211, M211, N211, O211),0))","v":"N/A"},{"$f":"IF(D211=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K211,M211,N211,P211)),0))","v":"N/A"},{"$f":"'Run Selections'!BD211","v":0},{"$f":"IF(LEFT($D211,4)<>\"ACBC\",\"N/A\",AdjacentZone($D211,$E211,$S211,$F211,60))","v":"N/A"},{"$f":"IF(LEFT($D211,4)<>\"ACBC\",\"N/A\",AdjacentZone($D211,$E211,$S211,$F211,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F212)=\"\",\"\",'Run Selections'!F212)","v":""},null,{"$f":"'Run Selections'!T212","v":"Select Model"},{"$f":"'Run Selections'!W212","v":4},{"$f":"'Run Selections'!Y212","v":50},{"$f":"'Run Selections'!AI212","v":""},{"$f":"'Run Selections'!AA212","v":0},null,{"$f":"'Run Selections'!AL212","v":""},{"$f":"IF(D212=\"Select Model\",\"N/A\",throwCombined(F212, D212, S212, E212,J212))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D212=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K212, M212, N212, O212),0))","v":"N/A"},{"$f":"IF(D212=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K212,M212,N212,P212)),0))","v":"N/A"},{"$f":"'Run Selections'!BD212","v":0},{"$f":"IF(LEFT($D212,4)<>\"ACBC\",\"N/A\",AdjacentZone($D212,$E212,$S212,$F212,60))","v":"N/A"},{"$f":"IF(LEFT($D212,4)<>\"ACBC\",\"N/A\",AdjacentZone($D212,$E212,$S212,$F212,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F213)=\"\",\"\",'Run Selections'!F213)","v":""},null,{"$f":"'Run Selections'!T213","v":"Select Model"},{"$f":"'Run Selections'!W213","v":4},{"$f":"'Run Selections'!Y213","v":50},{"$f":"'Run Selections'!AI213","v":""},{"$f":"'Run Selections'!AA213","v":0},null,{"$f":"'Run Selections'!AL213","v":""},{"$f":"IF(D213=\"Select Model\",\"N/A\",throwCombined(F213, D213, S213, E213,J213))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D213=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K213, M213, N213, O213),0))","v":"N/A"},{"$f":"IF(D213=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K213,M213,N213,P213)),0))","v":"N/A"},{"$f":"'Run Selections'!BD213","v":0},{"$f":"IF(LEFT($D213,4)<>\"ACBC\",\"N/A\",AdjacentZone($D213,$E213,$S213,$F213,60))","v":"N/A"},{"$f":"IF(LEFT($D213,4)<>\"ACBC\",\"N/A\",AdjacentZone($D213,$E213,$S213,$F213,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F214)=\"\",\"\",'Run Selections'!F214)","v":""},null,{"$f":"'Run Selections'!T214","v":"Select Model"},{"$f":"'Run Selections'!W214","v":4},{"$f":"'Run Selections'!Y214","v":50},{"$f":"'Run Selections'!AI214","v":""},{"$f":"'Run Selections'!AA214","v":0},null,{"$f":"'Run Selections'!AL214","v":""},{"$f":"IF(D214=\"Select Model\",\"N/A\",throwCombined(F214, D214, S214, E214,J214))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D214=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K214, M214, N214, O214),0))","v":"N/A"},{"$f":"IF(D214=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K214,M214,N214,P214)),0))","v":"N/A"},{"$f":"'Run Selections'!BD214","v":0},{"$f":"IF(LEFT($D214,4)<>\"ACBC\",\"N/A\",AdjacentZone($D214,$E214,$S214,$F214,60))","v":"N/A"},{"$f":"IF(LEFT($D214,4)<>\"ACBC\",\"N/A\",AdjacentZone($D214,$E214,$S214,$F214,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F215)=\"\",\"\",'Run Selections'!F215)","v":""},null,{"$f":"'Run Selections'!T215","v":"Select Model"},{"$f":"'Run Selections'!W215","v":4},{"$f":"'Run Selections'!Y215","v":50},{"$f":"'Run Selections'!AI215","v":""},{"$f":"'Run Selections'!AA215","v":0},null,{"$f":"'Run Selections'!AL215","v":""},{"$f":"IF(D215=\"Select Model\",\"N/A\",throwCombined(F215, D215, S215, E215,J215))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D215=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K215, M215, N215, O215),0))","v":"N/A"},{"$f":"IF(D215=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K215,M215,N215,P215)),0))","v":"N/A"},{"$f":"'Run Selections'!BD215","v":0},{"$f":"IF(LEFT($D215,4)<>\"ACBC\",\"N/A\",AdjacentZone($D215,$E215,$S215,$F215,60))","v":"N/A"},{"$f":"IF(LEFT($D215,4)<>\"ACBC\",\"N/A\",AdjacentZone($D215,$E215,$S215,$F215,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F216)=\"\",\"\",'Run Selections'!F216)","v":""},null,{"$f":"'Run Selections'!T216","v":"Select Model"},{"$f":"'Run Selections'!W216","v":4},{"$f":"'Run Selections'!Y216","v":50},{"$f":"'Run Selections'!AI216","v":""},{"$f":"'Run Selections'!AA216","v":0},null,{"$f":"'Run Selections'!AL216","v":""},{"$f":"IF(D216=\"Select Model\",\"N/A\",throwCombined(F216, D216, S216, E216,J216))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D216=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K216, M216, N216, O216),0))","v":"N/A"},{"$f":"IF(D216=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K216,M216,N216,P216)),0))","v":"N/A"},{"$f":"'Run Selections'!BD216","v":0},{"$f":"IF(LEFT($D216,4)<>\"ACBC\",\"N/A\",AdjacentZone($D216,$E216,$S216,$F216,60))","v":"N/A"},{"$f":"IF(LEFT($D216,4)<>\"ACBC\",\"N/A\",AdjacentZone($D216,$E216,$S216,$F216,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F217)=\"\",\"\",'Run Selections'!F217)","v":""},null,{"$f":"'Run Selections'!T217","v":"Select Model"},{"$f":"'Run Selections'!W217","v":4},{"$f":"'Run Selections'!Y217","v":50},{"$f":"'Run Selections'!AI217","v":""},{"$f":"'Run Selections'!AA217","v":0},null,{"$f":"'Run Selections'!AL217","v":""},{"$f":"IF(D217=\"Select Model\",\"N/A\",throwCombined(F217, D217, S217, E217,J217))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D217=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K217, M217, N217, O217),0))","v":"N/A"},{"$f":"IF(D217=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K217,M217,N217,P217)),0))","v":"N/A"},{"$f":"'Run Selections'!BD217","v":0},{"$f":"IF(LEFT($D217,4)<>\"ACBC\",\"N/A\",AdjacentZone($D217,$E217,$S217,$F217,60))","v":"N/A"},{"$f":"IF(LEFT($D217,4)<>\"ACBC\",\"N/A\",AdjacentZone($D217,$E217,$S217,$F217,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F218)=\"\",\"\",'Run Selections'!F218)","v":""},null,{"$f":"'Run Selections'!T218","v":"Select Model"},{"$f":"'Run Selections'!W218","v":4},{"$f":"'Run Selections'!Y218","v":50},{"$f":"'Run Selections'!AI218","v":""},{"$f":"'Run Selections'!AA218","v":0},null,{"$f":"'Run Selections'!AL218","v":""},{"$f":"IF(D218=\"Select Model\",\"N/A\",throwCombined(F218, D218, S218, E218,J218))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D218=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K218, M218, N218, O218),0))","v":"N/A"},{"$f":"IF(D218=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K218,M218,N218,P218)),0))","v":"N/A"},{"$f":"'Run Selections'!BD218","v":0},{"$f":"IF(LEFT($D218,4)<>\"ACBC\",\"N/A\",AdjacentZone($D218,$E218,$S218,$F218,60))","v":"N/A"},{"$f":"IF(LEFT($D218,4)<>\"ACBC\",\"N/A\",AdjacentZone($D218,$E218,$S218,$F218,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F219)=\"\",\"\",'Run Selections'!F219)","v":""},null,{"$f":"'Run Selections'!T219","v":"Select Model"},{"$f":"'Run Selections'!W219","v":4},{"$f":"'Run Selections'!Y219","v":50},{"$f":"'Run Selections'!AI219","v":""},{"$f":"'Run Selections'!AA219","v":0},null,{"$f":"'Run Selections'!AL219","v":""},{"$f":"IF(D219=\"Select Model\",\"N/A\",throwCombined(F219, D219, S219, E219,J219))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D219=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K219, M219, N219, O219),0))","v":"N/A"},{"$f":"IF(D219=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K219,M219,N219,P219)),0))","v":"N/A"},{"$f":"'Run Selections'!BD219","v":0},{"$f":"IF(LEFT($D219,4)<>\"ACBC\",\"N/A\",AdjacentZone($D219,$E219,$S219,$F219,60))","v":"N/A"},{"$f":"IF(LEFT($D219,4)<>\"ACBC\",\"N/A\",AdjacentZone($D219,$E219,$S219,$F219,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F220)=\"\",\"\",'Run Selections'!F220)","v":""},null,{"$f":"'Run Selections'!T220","v":"Select Model"},{"$f":"'Run Selections'!W220","v":4},{"$f":"'Run Selections'!Y220","v":50},{"$f":"'Run Selections'!AI220","v":""},{"$f":"'Run Selections'!AA220","v":0},null,{"$f":"'Run Selections'!AL220","v":""},{"$f":"IF(D220=\"Select Model\",\"N/A\",throwCombined(F220, D220, S220, E220,J220))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D220=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K220, M220, N220, O220),0))","v":"N/A"},{"$f":"IF(D220=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K220,M220,N220,P220)),0))","v":"N/A"},{"$f":"'Run Selections'!BD220","v":0},{"$f":"IF(LEFT($D220,4)<>\"ACBC\",\"N/A\",AdjacentZone($D220,$E220,$S220,$F220,60))","v":"N/A"},{"$f":"IF(LEFT($D220,4)<>\"ACBC\",\"N/A\",AdjacentZone($D220,$E220,$S220,$F220,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F221)=\"\",\"\",'Run Selections'!F221)","v":""},null,{"$f":"'Run Selections'!T221","v":"Select Model"},{"$f":"'Run Selections'!W221","v":4},{"$f":"'Run Selections'!Y221","v":50},{"$f":"'Run Selections'!AI221","v":""},{"$f":"'Run Selections'!AA221","v":0},null,{"$f":"'Run Selections'!AL221","v":""},{"$f":"IF(D221=\"Select Model\",\"N/A\",throwCombined(F221, D221, S221, E221,J221))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D221=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K221, M221, N221, O221),0))","v":"N/A"},{"$f":"IF(D221=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K221,M221,N221,P221)),0))","v":"N/A"},{"$f":"'Run Selections'!BD221","v":0},{"$f":"IF(LEFT($D221,4)<>\"ACBC\",\"N/A\",AdjacentZone($D221,$E221,$S221,$F221,60))","v":"N/A"},{"$f":"IF(LEFT($D221,4)<>\"ACBC\",\"N/A\",AdjacentZone($D221,$E221,$S221,$F221,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F222)=\"\",\"\",'Run Selections'!F222)","v":""},null,{"$f":"'Run Selections'!T222","v":"Select Model"},{"$f":"'Run Selections'!W222","v":4},{"$f":"'Run Selections'!Y222","v":50},{"$f":"'Run Selections'!AI222","v":""},{"$f":"'Run Selections'!AA222","v":0},null,{"$f":"'Run Selections'!AL222","v":""},{"$f":"IF(D222=\"Select Model\",\"N/A\",throwCombined(F222, D222, S222, E222,J222))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D222=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K222, M222, N222, O222),0))","v":"N/A"},{"$f":"IF(D222=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K222,M222,N222,P222)),0))","v":"N/A"},{"$f":"'Run Selections'!BD222","v":0},{"$f":"IF(LEFT($D222,4)<>\"ACBC\",\"N/A\",AdjacentZone($D222,$E222,$S222,$F222,60))","v":"N/A"},{"$f":"IF(LEFT($D222,4)<>\"ACBC\",\"N/A\",AdjacentZone($D222,$E222,$S222,$F222,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F223)=\"\",\"\",'Run Selections'!F223)","v":""},null,{"$f":"'Run Selections'!T223","v":"Select Model"},{"$f":"'Run Selections'!W223","v":4},{"$f":"'Run Selections'!Y223","v":50},{"$f":"'Run Selections'!AI223","v":""},{"$f":"'Run Selections'!AA223","v":0},null,{"$f":"'Run Selections'!AL223","v":""},{"$f":"IF(D223=\"Select Model\",\"N/A\",throwCombined(F223, D223, S223, E223,J223))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D223=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K223, M223, N223, O223),0))","v":"N/A"},{"$f":"IF(D223=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K223,M223,N223,P223)),0))","v":"N/A"},{"$f":"'Run Selections'!BD223","v":0},{"$f":"IF(LEFT($D223,4)<>\"ACBC\",\"N/A\",AdjacentZone($D223,$E223,$S223,$F223,60))","v":"N/A"},{"$f":"IF(LEFT($D223,4)<>\"ACBC\",\"N/A\",AdjacentZone($D223,$E223,$S223,$F223,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F224)=\"\",\"\",'Run Selections'!F224)","v":""},null,{"$f":"'Run Selections'!T224","v":"Select Model"},{"$f":"'Run Selections'!W224","v":4},{"$f":"'Run Selections'!Y224","v":50},{"$f":"'Run Selections'!AI224","v":""},{"$f":"'Run Selections'!AA224","v":0},null,{"$f":"'Run Selections'!AL224","v":""},{"$f":"IF(D224=\"Select Model\",\"N/A\",throwCombined(F224, D224, S224, E224,J224))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D224=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K224, M224, N224, O224),0))","v":"N/A"},{"$f":"IF(D224=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K224,M224,N224,P224)),0))","v":"N/A"},{"$f":"'Run Selections'!BD224","v":0},{"$f":"IF(LEFT($D224,4)<>\"ACBC\",\"N/A\",AdjacentZone($D224,$E224,$S224,$F224,60))","v":"N/A"},{"$f":"IF(LEFT($D224,4)<>\"ACBC\",\"N/A\",AdjacentZone($D224,$E224,$S224,$F224,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F225)=\"\",\"\",'Run Selections'!F225)","v":""},null,{"$f":"'Run Selections'!T225","v":"Select Model"},{"$f":"'Run Selections'!W225","v":4},{"$f":"'Run Selections'!Y225","v":50},{"$f":"'Run Selections'!AI225","v":""},{"$f":"'Run Selections'!AA225","v":0},null,{"$f":"'Run Selections'!AL225","v":""},{"$f":"IF(D225=\"Select Model\",\"N/A\",throwCombined(F225, D225, S225, E225,J225))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D225=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K225, M225, N225, O225),0))","v":"N/A"},{"$f":"IF(D225=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K225,M225,N225,P225)),0))","v":"N/A"},{"$f":"'Run Selections'!BD225","v":0},{"$f":"IF(LEFT($D225,4)<>\"ACBC\",\"N/A\",AdjacentZone($D225,$E225,$S225,$F225,60))","v":"N/A"},{"$f":"IF(LEFT($D225,4)<>\"ACBC\",\"N/A\",AdjacentZone($D225,$E225,$S225,$F225,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F226)=\"\",\"\",'Run Selections'!F226)","v":""},null,{"$f":"'Run Selections'!T226","v":"Select Model"},{"$f":"'Run Selections'!W226","v":4},{"$f":"'Run Selections'!Y226","v":50},{"$f":"'Run Selections'!AI226","v":""},{"$f":"'Run Selections'!AA226","v":0},null,{"$f":"'Run Selections'!AL226","v":""},{"$f":"IF(D226=\"Select Model\",\"N/A\",throwCombined(F226, D226, S226, E226,J226))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D226=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K226, M226, N226, O226),0))","v":"N/A"},{"$f":"IF(D226=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K226,M226,N226,P226)),0))","v":"N/A"},{"$f":"'Run Selections'!BD226","v":0},{"$f":"IF(LEFT($D226,4)<>\"ACBC\",\"N/A\",AdjacentZone($D226,$E226,$S226,$F226,60))","v":"N/A"},{"$f":"IF(LEFT($D226,4)<>\"ACBC\",\"N/A\",AdjacentZone($D226,$E226,$S226,$F226,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F227)=\"\",\"\",'Run Selections'!F227)","v":""},null,{"$f":"'Run Selections'!T227","v":"Select Model"},{"$f":"'Run Selections'!W227","v":4},{"$f":"'Run Selections'!Y227","v":50},{"$f":"'Run Selections'!AI227","v":""},{"$f":"'Run Selections'!AA227","v":0},null,{"$f":"'Run Selections'!AL227","v":""},{"$f":"IF(D227=\"Select Model\",\"N/A\",throwCombined(F227, D227, S227, E227,J227))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D227=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K227, M227, N227, O227),0))","v":"N/A"},{"$f":"IF(D227=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K227,M227,N227,P227)),0))","v":"N/A"},{"$f":"'Run Selections'!BD227","v":0},{"$f":"IF(LEFT($D227,4)<>\"ACBC\",\"N/A\",AdjacentZone($D227,$E227,$S227,$F227,60))","v":"N/A"},{"$f":"IF(LEFT($D227,4)<>\"ACBC\",\"N/A\",AdjacentZone($D227,$E227,$S227,$F227,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F228)=\"\",\"\",'Run Selections'!F228)","v":""},null,{"$f":"'Run Selections'!T228","v":"Select Model"},{"$f":"'Run Selections'!W228","v":4},{"$f":"'Run Selections'!Y228","v":50},{"$f":"'Run Selections'!AI228","v":""},{"$f":"'Run Selections'!AA228","v":0},null,{"$f":"'Run Selections'!AL228","v":""},{"$f":"IF(D228=\"Select Model\",\"N/A\",throwCombined(F228, D228, S228, E228,J228))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D228=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K228, M228, N228, O228),0))","v":"N/A"},{"$f":"IF(D228=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K228,M228,N228,P228)),0))","v":"N/A"},{"$f":"'Run Selections'!BD228","v":0},{"$f":"IF(LEFT($D228,4)<>\"ACBC\",\"N/A\",AdjacentZone($D228,$E228,$S228,$F228,60))","v":"N/A"},{"$f":"IF(LEFT($D228,4)<>\"ACBC\",\"N/A\",AdjacentZone($D228,$E228,$S228,$F228,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F229)=\"\",\"\",'Run Selections'!F229)","v":""},null,{"$f":"'Run Selections'!T229","v":"Select Model"},{"$f":"'Run Selections'!W229","v":4},{"$f":"'Run Selections'!Y229","v":50},{"$f":"'Run Selections'!AI229","v":""},{"$f":"'Run Selections'!AA229","v":0},null,{"$f":"'Run Selections'!AL229","v":""},{"$f":"IF(D229=\"Select Model\",\"N/A\",throwCombined(F229, D229, S229, E229,J229))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D229=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K229, M229, N229, O229),0))","v":"N/A"},{"$f":"IF(D229=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K229,M229,N229,P229)),0))","v":"N/A"},{"$f":"'Run Selections'!BD229","v":0},{"$f":"IF(LEFT($D229,4)<>\"ACBC\",\"N/A\",AdjacentZone($D229,$E229,$S229,$F229,60))","v":"N/A"},{"$f":"IF(LEFT($D229,4)<>\"ACBC\",\"N/A\",AdjacentZone($D229,$E229,$S229,$F229,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F230)=\"\",\"\",'Run Selections'!F230)","v":""},null,{"$f":"'Run Selections'!T230","v":"Select Model"},{"$f":"'Run Selections'!W230","v":4},{"$f":"'Run Selections'!Y230","v":50},{"$f":"'Run Selections'!AI230","v":""},{"$f":"'Run Selections'!AA230","v":0},null,{"$f":"'Run Selections'!AL230","v":""},{"$f":"IF(D230=\"Select Model\",\"N/A\",throwCombined(F230, D230, S230, E230,J230))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D230=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K230, M230, N230, O230),0))","v":"N/A"},{"$f":"IF(D230=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K230,M230,N230,P230)),0))","v":"N/A"},{"$f":"'Run Selections'!BD230","v":0},{"$f":"IF(LEFT($D230,4)<>\"ACBC\",\"N/A\",AdjacentZone($D230,$E230,$S230,$F230,60))","v":"N/A"},{"$f":"IF(LEFT($D230,4)<>\"ACBC\",\"N/A\",AdjacentZone($D230,$E230,$S230,$F230,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F231)=\"\",\"\",'Run Selections'!F231)","v":""},null,{"$f":"'Run Selections'!T231","v":"Select Model"},{"$f":"'Run Selections'!W231","v":4},{"$f":"'Run Selections'!Y231","v":50},{"$f":"'Run Selections'!AI231","v":""},{"$f":"'Run Selections'!AA231","v":0},null,{"$f":"'Run Selections'!AL231","v":""},{"$f":"IF(D231=\"Select Model\",\"N/A\",throwCombined(F231, D231, S231, E231,J231))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D231=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K231, M231, N231, O231),0))","v":"N/A"},{"$f":"IF(D231=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K231,M231,N231,P231)),0))","v":"N/A"},{"$f":"'Run Selections'!BD231","v":0},{"$f":"IF(LEFT($D231,4)<>\"ACBC\",\"N/A\",AdjacentZone($D231,$E231,$S231,$F231,60))","v":"N/A"},{"$f":"IF(LEFT($D231,4)<>\"ACBC\",\"N/A\",AdjacentZone($D231,$E231,$S231,$F231,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F232)=\"\",\"\",'Run Selections'!F232)","v":""},null,{"$f":"'Run Selections'!T232","v":"Select Model"},{"$f":"'Run Selections'!W232","v":4},{"$f":"'Run Selections'!Y232","v":50},{"$f":"'Run Selections'!AI232","v":""},{"$f":"'Run Selections'!AA232","v":0},null,{"$f":"'Run Selections'!AL232","v":""},{"$f":"IF(D232=\"Select Model\",\"N/A\",throwCombined(F232, D232, S232, E232,J232))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D232=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K232, M232, N232, O232),0))","v":"N/A"},{"$f":"IF(D232=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K232,M232,N232,P232)),0))","v":"N/A"},{"$f":"'Run Selections'!BD232","v":0},{"$f":"IF(LEFT($D232,4)<>\"ACBC\",\"N/A\",AdjacentZone($D232,$E232,$S232,$F232,60))","v":"N/A"},{"$f":"IF(LEFT($D232,4)<>\"ACBC\",\"N/A\",AdjacentZone($D232,$E232,$S232,$F232,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F233)=\"\",\"\",'Run Selections'!F233)","v":""},null,{"$f":"'Run Selections'!T233","v":"Select Model"},{"$f":"'Run Selections'!W233","v":4},{"$f":"'Run Selections'!Y233","v":50},{"$f":"'Run Selections'!AI233","v":""},{"$f":"'Run Selections'!AA233","v":0},null,{"$f":"'Run Selections'!AL233","v":""},{"$f":"IF(D233=\"Select Model\",\"N/A\",throwCombined(F233, D233, S233, E233,J233))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D233=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K233, M233, N233, O233),0))","v":"N/A"},{"$f":"IF(D233=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K233,M233,N233,P233)),0))","v":"N/A"},{"$f":"'Run Selections'!BD233","v":0},{"$f":"IF(LEFT($D233,4)<>\"ACBC\",\"N/A\",AdjacentZone($D233,$E233,$S233,$F233,60))","v":"N/A"},{"$f":"IF(LEFT($D233,4)<>\"ACBC\",\"N/A\",AdjacentZone($D233,$E233,$S233,$F233,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F234)=\"\",\"\",'Run Selections'!F234)","v":""},null,{"$f":"'Run Selections'!T234","v":"Select Model"},{"$f":"'Run Selections'!W234","v":4},{"$f":"'Run Selections'!Y234","v":50},{"$f":"'Run Selections'!AI234","v":""},{"$f":"'Run Selections'!AA234","v":0},null,{"$f":"'Run Selections'!AL234","v":""},{"$f":"IF(D234=\"Select Model\",\"N/A\",throwCombined(F234, D234, S234, E234,J234))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D234=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K234, M234, N234, O234),0))","v":"N/A"},{"$f":"IF(D234=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K234,M234,N234,P234)),0))","v":"N/A"},{"$f":"'Run Selections'!BD234","v":0},{"$f":"IF(LEFT($D234,4)<>\"ACBC\",\"N/A\",AdjacentZone($D234,$E234,$S234,$F234,60))","v":"N/A"},{"$f":"IF(LEFT($D234,4)<>\"ACBC\",\"N/A\",AdjacentZone($D234,$E234,$S234,$F234,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F235)=\"\",\"\",'Run Selections'!F235)","v":""},null,{"$f":"'Run Selections'!T235","v":"Select Model"},{"$f":"'Run Selections'!W235","v":4},{"$f":"'Run Selections'!Y235","v":50},{"$f":"'Run Selections'!AI235","v":""},{"$f":"'Run Selections'!AA235","v":0},null,{"$f":"'Run Selections'!AL235","v":""},{"$f":"IF(D235=\"Select Model\",\"N/A\",throwCombined(F235, D235, S235, E235,J235))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D235=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K235, M235, N235, O235),0))","v":"N/A"},{"$f":"IF(D235=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K235,M235,N235,P235)),0))","v":"N/A"},{"$f":"'Run Selections'!BD235","v":0},{"$f":"IF(LEFT($D235,4)<>\"ACBC\",\"N/A\",AdjacentZone($D235,$E235,$S235,$F235,60))","v":"N/A"},{"$f":"IF(LEFT($D235,4)<>\"ACBC\",\"N/A\",AdjacentZone($D235,$E235,$S235,$F235,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F236)=\"\",\"\",'Run Selections'!F236)","v":""},null,{"$f":"'Run Selections'!T236","v":"Select Model"},{"$f":"'Run Selections'!W236","v":4},{"$f":"'Run Selections'!Y236","v":50},{"$f":"'Run Selections'!AI236","v":""},{"$f":"'Run Selections'!AA236","v":0},null,{"$f":"'Run Selections'!AL236","v":""},{"$f":"IF(D236=\"Select Model\",\"N/A\",throwCombined(F236, D236, S236, E236,J236))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D236=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K236, M236, N236, O236),0))","v":"N/A"},{"$f":"IF(D236=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K236,M236,N236,P236)),0))","v":"N/A"},{"$f":"'Run Selections'!BD236","v":0},{"$f":"IF(LEFT($D236,4)<>\"ACBC\",\"N/A\",AdjacentZone($D236,$E236,$S236,$F236,60))","v":"N/A"},{"$f":"IF(LEFT($D236,4)<>\"ACBC\",\"N/A\",AdjacentZone($D236,$E236,$S236,$F236,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F237)=\"\",\"\",'Run Selections'!F237)","v":""},null,{"$f":"'Run Selections'!T237","v":"Select Model"},{"$f":"'Run Selections'!W237","v":4},{"$f":"'Run Selections'!Y237","v":50},{"$f":"'Run Selections'!AI237","v":""},{"$f":"'Run Selections'!AA237","v":0},null,{"$f":"'Run Selections'!AL237","v":""},{"$f":"IF(D237=\"Select Model\",\"N/A\",throwCombined(F237, D237, S237, E237,J237))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D237=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K237, M237, N237, O237),0))","v":"N/A"},{"$f":"IF(D237=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K237,M237,N237,P237)),0))","v":"N/A"},{"$f":"'Run Selections'!BD237","v":0},{"$f":"IF(LEFT($D237,4)<>\"ACBC\",\"N/A\",AdjacentZone($D237,$E237,$S237,$F237,60))","v":"N/A"},{"$f":"IF(LEFT($D237,4)<>\"ACBC\",\"N/A\",AdjacentZone($D237,$E237,$S237,$F237,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F238)=\"\",\"\",'Run Selections'!F238)","v":""},null,{"$f":"'Run Selections'!T238","v":"Select Model"},{"$f":"'Run Selections'!W238","v":4},{"$f":"'Run Selections'!Y238","v":50},{"$f":"'Run Selections'!AI238","v":""},{"$f":"'Run Selections'!AA238","v":0},null,{"$f":"'Run Selections'!AL238","v":""},{"$f":"IF(D238=\"Select Model\",\"N/A\",throwCombined(F238, D238, S238, E238,J238))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D238=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K238, M238, N238, O238),0))","v":"N/A"},{"$f":"IF(D238=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K238,M238,N238,P238)),0))","v":"N/A"},{"$f":"'Run Selections'!BD238","v":0},{"$f":"IF(LEFT($D238,4)<>\"ACBC\",\"N/A\",AdjacentZone($D238,$E238,$S238,$F238,60))","v":"N/A"},{"$f":"IF(LEFT($D238,4)<>\"ACBC\",\"N/A\",AdjacentZone($D238,$E238,$S238,$F238,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F239)=\"\",\"\",'Run Selections'!F239)","v":""},null,{"$f":"'Run Selections'!T239","v":"Select Model"},{"$f":"'Run Selections'!W239","v":4},{"$f":"'Run Selections'!Y239","v":50},{"$f":"'Run Selections'!AI239","v":""},{"$f":"'Run Selections'!AA239","v":0},null,{"$f":"'Run Selections'!AL239","v":""},{"$f":"IF(D239=\"Select Model\",\"N/A\",throwCombined(F239, D239, S239, E239,J239))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D239=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K239, M239, N239, O239),0))","v":"N/A"},{"$f":"IF(D239=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K239,M239,N239,P239)),0))","v":"N/A"},{"$f":"'Run Selections'!BD239","v":0},{"$f":"IF(LEFT($D239,4)<>\"ACBC\",\"N/A\",AdjacentZone($D239,$E239,$S239,$F239,60))","v":"N/A"},{"$f":"IF(LEFT($D239,4)<>\"ACBC\",\"N/A\",AdjacentZone($D239,$E239,$S239,$F239,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F240)=\"\",\"\",'Run Selections'!F240)","v":""},null,{"$f":"'Run Selections'!T240","v":"Select Model"},{"$f":"'Run Selections'!W240","v":4},{"$f":"'Run Selections'!Y240","v":50},{"$f":"'Run Selections'!AI240","v":""},{"$f":"'Run Selections'!AA240","v":0},null,{"$f":"'Run Selections'!AL240","v":""},{"$f":"IF(D240=\"Select Model\",\"N/A\",throwCombined(F240, D240, S240, E240,J240))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D240=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K240, M240, N240, O240),0))","v":"N/A"},{"$f":"IF(D240=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K240,M240,N240,P240)),0))","v":"N/A"},{"$f":"'Run Selections'!BD240","v":0},{"$f":"IF(LEFT($D240,4)<>\"ACBC\",\"N/A\",AdjacentZone($D240,$E240,$S240,$F240,60))","v":"N/A"},{"$f":"IF(LEFT($D240,4)<>\"ACBC\",\"N/A\",AdjacentZone($D240,$E240,$S240,$F240,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F241)=\"\",\"\",'Run Selections'!F241)","v":""},null,{"$f":"'Run Selections'!T241","v":"Select Model"},{"$f":"'Run Selections'!W241","v":4},{"$f":"'Run Selections'!Y241","v":50},{"$f":"'Run Selections'!AI241","v":""},{"$f":"'Run Selections'!AA241","v":0},null,{"$f":"'Run Selections'!AL241","v":""},{"$f":"IF(D241=\"Select Model\",\"N/A\",throwCombined(F241, D241, S241, E241,J241))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D241=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K241, M241, N241, O241),0))","v":"N/A"},{"$f":"IF(D241=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K241,M241,N241,P241)),0))","v":"N/A"},{"$f":"'Run Selections'!BD241","v":0},{"$f":"IF(LEFT($D241,4)<>\"ACBC\",\"N/A\",AdjacentZone($D241,$E241,$S241,$F241,60))","v":"N/A"},{"$f":"IF(LEFT($D241,4)<>\"ACBC\",\"N/A\",AdjacentZone($D241,$E241,$S241,$F241,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F242)=\"\",\"\",'Run Selections'!F242)","v":""},null,{"$f":"'Run Selections'!T242","v":"Select Model"},{"$f":"'Run Selections'!W242","v":4},{"$f":"'Run Selections'!Y242","v":50},{"$f":"'Run Selections'!AI242","v":""},{"$f":"'Run Selections'!AA242","v":0},null,{"$f":"'Run Selections'!AL242","v":""},{"$f":"IF(D242=\"Select Model\",\"N/A\",throwCombined(F242, D242, S242, E242,J242))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D242=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K242, M242, N242, O242),0))","v":"N/A"},{"$f":"IF(D242=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K242,M242,N242,P242)),0))","v":"N/A"},{"$f":"'Run Selections'!BD242","v":0},{"$f":"IF(LEFT($D242,4)<>\"ACBC\",\"N/A\",AdjacentZone($D242,$E242,$S242,$F242,60))","v":"N/A"},{"$f":"IF(LEFT($D242,4)<>\"ACBC\",\"N/A\",AdjacentZone($D242,$E242,$S242,$F242,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F243)=\"\",\"\",'Run Selections'!F243)","v":""},null,{"$f":"'Run Selections'!T243","v":"Select Model"},{"$f":"'Run Selections'!W243","v":4},{"$f":"'Run Selections'!Y243","v":50},{"$f":"'Run Selections'!AI243","v":""},{"$f":"'Run Selections'!AA243","v":0},null,{"$f":"'Run Selections'!AL243","v":""},{"$f":"IF(D243=\"Select Model\",\"N/A\",throwCombined(F243, D243, S243, E243,J243))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D243=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K243, M243, N243, O243),0))","v":"N/A"},{"$f":"IF(D243=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K243,M243,N243,P243)),0))","v":"N/A"},{"$f":"'Run Selections'!BD243","v":0},{"$f":"IF(LEFT($D243,4)<>\"ACBC\",\"N/A\",AdjacentZone($D243,$E243,$S243,$F243,60))","v":"N/A"},{"$f":"IF(LEFT($D243,4)<>\"ACBC\",\"N/A\",AdjacentZone($D243,$E243,$S243,$F243,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F244)=\"\",\"\",'Run Selections'!F244)","v":""},null,{"$f":"'Run Selections'!T244","v":"Select Model"},{"$f":"'Run Selections'!W244","v":4},{"$f":"'Run Selections'!Y244","v":50},{"$f":"'Run Selections'!AI244","v":""},{"$f":"'Run Selections'!AA244","v":0},null,{"$f":"'Run Selections'!AL244","v":""},{"$f":"IF(D244=\"Select Model\",\"N/A\",throwCombined(F244, D244, S244, E244,J244))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D244=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K244, M244, N244, O244),0))","v":"N/A"},{"$f":"IF(D244=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K244,M244,N244,P244)),0))","v":"N/A"},{"$f":"'Run Selections'!BD244","v":0},{"$f":"IF(LEFT($D244,4)<>\"ACBC\",\"N/A\",AdjacentZone($D244,$E244,$S244,$F244,60))","v":"N/A"},{"$f":"IF(LEFT($D244,4)<>\"ACBC\",\"N/A\",AdjacentZone($D244,$E244,$S244,$F244,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F245)=\"\",\"\",'Run Selections'!F245)","v":""},null,{"$f":"'Run Selections'!T245","v":"Select Model"},{"$f":"'Run Selections'!W245","v":4},{"$f":"'Run Selections'!Y245","v":50},{"$f":"'Run Selections'!AI245","v":""},{"$f":"'Run Selections'!AA245","v":0},null,{"$f":"'Run Selections'!AL245","v":""},{"$f":"IF(D245=\"Select Model\",\"N/A\",throwCombined(F245, D245, S245, E245,J245))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D245=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K245, M245, N245, O245),0))","v":"N/A"},{"$f":"IF(D245=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K245,M245,N245,P245)),0))","v":"N/A"},{"$f":"'Run Selections'!BD245","v":0},{"$f":"IF(LEFT($D245,4)<>\"ACBC\",\"N/A\",AdjacentZone($D245,$E245,$S245,$F245,60))","v":"N/A"},{"$f":"IF(LEFT($D245,4)<>\"ACBC\",\"N/A\",AdjacentZone($D245,$E245,$S245,$F245,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F246)=\"\",\"\",'Run Selections'!F246)","v":""},null,{"$f":"'Run Selections'!T246","v":"Select Model"},{"$f":"'Run Selections'!W246","v":4},{"$f":"'Run Selections'!Y246","v":50},{"$f":"'Run Selections'!AI246","v":""},{"$f":"'Run Selections'!AA246","v":0},null,{"$f":"'Run Selections'!AL246","v":""},{"$f":"IF(D246=\"Select Model\",\"N/A\",throwCombined(F246, D246, S246, E246,J246))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D246=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K246, M246, N246, O246),0))","v":"N/A"},{"$f":"IF(D246=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K246,M246,N246,P246)),0))","v":"N/A"},{"$f":"'Run Selections'!BD246","v":0},{"$f":"IF(LEFT($D246,4)<>\"ACBC\",\"N/A\",AdjacentZone($D246,$E246,$S246,$F246,60))","v":"N/A"},{"$f":"IF(LEFT($D246,4)<>\"ACBC\",\"N/A\",AdjacentZone($D246,$E246,$S246,$F246,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F247)=\"\",\"\",'Run Selections'!F247)","v":""},null,{"$f":"'Run Selections'!T247","v":"Select Model"},{"$f":"'Run Selections'!W247","v":4},{"$f":"'Run Selections'!Y247","v":50},{"$f":"'Run Selections'!AI247","v":""},{"$f":"'Run Selections'!AA247","v":0},null,{"$f":"'Run Selections'!AL247","v":""},{"$f":"IF(D247=\"Select Model\",\"N/A\",throwCombined(F247, D247, S247, E247,J247))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D247=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K247, M247, N247, O247),0))","v":"N/A"},{"$f":"IF(D247=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K247,M247,N247,P247)),0))","v":"N/A"},{"$f":"'Run Selections'!BD247","v":0},{"$f":"IF(LEFT($D247,4)<>\"ACBC\",\"N/A\",AdjacentZone($D247,$E247,$S247,$F247,60))","v":"N/A"},{"$f":"IF(LEFT($D247,4)<>\"ACBC\",\"N/A\",AdjacentZone($D247,$E247,$S247,$F247,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F248)=\"\",\"\",'Run Selections'!F248)","v":""},null,{"$f":"'Run Selections'!T248","v":"Select Model"},{"$f":"'Run Selections'!W248","v":4},{"$f":"'Run Selections'!Y248","v":50},{"$f":"'Run Selections'!AI248","v":""},{"$f":"'Run Selections'!AA248","v":0},null,{"$f":"'Run Selections'!AL248","v":""},{"$f":"IF(D248=\"Select Model\",\"N/A\",throwCombined(F248, D248, S248, E248,J248))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D248=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K248, M248, N248, O248),0))","v":"N/A"},{"$f":"IF(D248=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K248,M248,N248,P248)),0))","v":"N/A"},{"$f":"'Run Selections'!BD248","v":0},{"$f":"IF(LEFT($D248,4)<>\"ACBC\",\"N/A\",AdjacentZone($D248,$E248,$S248,$F248,60))","v":"N/A"},{"$f":"IF(LEFT($D248,4)<>\"ACBC\",\"N/A\",AdjacentZone($D248,$E248,$S248,$F248,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F249)=\"\",\"\",'Run Selections'!F249)","v":""},null,{"$f":"'Run Selections'!T249","v":"Select Model"},{"$f":"'Run Selections'!W249","v":4},{"$f":"'Run Selections'!Y249","v":50},{"$f":"'Run Selections'!AI249","v":""},{"$f":"'Run Selections'!AA249","v":0},null,{"$f":"'Run Selections'!AL249","v":""},{"$f":"IF(D249=\"Select Model\",\"N/A\",throwCombined(F249, D249, S249, E249,J249))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D249=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K249, M249, N249, O249),0))","v":"N/A"},{"$f":"IF(D249=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K249,M249,N249,P249)),0))","v":"N/A"},{"$f":"'Run Selections'!BD249","v":0},{"$f":"IF(LEFT($D249,4)<>\"ACBC\",\"N/A\",AdjacentZone($D249,$E249,$S249,$F249,60))","v":"N/A"},{"$f":"IF(LEFT($D249,4)<>\"ACBC\",\"N/A\",AdjacentZone($D249,$E249,$S249,$F249,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F250)=\"\",\"\",'Run Selections'!F250)","v":""},null,{"$f":"'Run Selections'!T250","v":"Select Model"},{"$f":"'Run Selections'!W250","v":4},{"$f":"'Run Selections'!Y250","v":50},{"$f":"'Run Selections'!AI250","v":""},{"$f":"'Run Selections'!AA250","v":0},null,{"$f":"'Run Selections'!AL250","v":""},{"$f":"IF(D250=\"Select Model\",\"N/A\",throwCombined(F250, D250, S250, E250,J250))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D250=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K250, M250, N250, O250),0))","v":"N/A"},{"$f":"IF(D250=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K250,M250,N250,P250)),0))","v":"N/A"},{"$f":"'Run Selections'!BD250","v":0},{"$f":"IF(LEFT($D250,4)<>\"ACBC\",\"N/A\",AdjacentZone($D250,$E250,$S250,$F250,60))","v":"N/A"},{"$f":"IF(LEFT($D250,4)<>\"ACBC\",\"N/A\",AdjacentZone($D250,$E250,$S250,$F250,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F251)=\"\",\"\",'Run Selections'!F251)","v":""},null,{"$f":"'Run Selections'!T251","v":"Select Model"},{"$f":"'Run Selections'!W251","v":4},{"$f":"'Run Selections'!Y251","v":50},{"$f":"'Run Selections'!AI251","v":""},{"$f":"'Run Selections'!AA251","v":0},null,{"$f":"'Run Selections'!AL251","v":""},{"$f":"IF(D251=\"Select Model\",\"N/A\",throwCombined(F251, D251, S251, E251,J251))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D251=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K251, M251, N251, O251),0))","v":"N/A"},{"$f":"IF(D251=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K251,M251,N251,P251)),0))","v":"N/A"},{"$f":"'Run Selections'!BD251","v":0},{"$f":"IF(LEFT($D251,4)<>\"ACBC\",\"N/A\",AdjacentZone($D251,$E251,$S251,$F251,60))","v":"N/A"},{"$f":"IF(LEFT($D251,4)<>\"ACBC\",\"N/A\",AdjacentZone($D251,$E251,$S251,$F251,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F252)=\"\",\"\",'Run Selections'!F252)","v":""},null,{"$f":"'Run Selections'!T252","v":"Select Model"},{"$f":"'Run Selections'!W252","v":4},{"$f":"'Run Selections'!Y252","v":50},{"$f":"'Run Selections'!AI252","v":""},{"$f":"'Run Selections'!AA252","v":0},null,{"$f":"'Run Selections'!AL252","v":""},{"$f":"IF(D252=\"Select Model\",\"N/A\",throwCombined(F252, D252, S252, E252,J252))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D252=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K252, M252, N252, O252),0))","v":"N/A"},{"$f":"IF(D252=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K252,M252,N252,P252)),0))","v":"N/A"},{"$f":"'Run Selections'!BD252","v":0},{"$f":"IF(LEFT($D252,4)<>\"ACBC\",\"N/A\",AdjacentZone($D252,$E252,$S252,$F252,60))","v":"N/A"},{"$f":"IF(LEFT($D252,4)<>\"ACBC\",\"N/A\",AdjacentZone($D252,$E252,$S252,$F252,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F253)=\"\",\"\",'Run Selections'!F253)","v":""},null,{"$f":"'Run Selections'!T253","v":"Select Model"},{"$f":"'Run Selections'!W253","v":4},{"$f":"'Run Selections'!Y253","v":50},{"$f":"'Run Selections'!AI253","v":""},{"$f":"'Run Selections'!AA253","v":0},null,{"$f":"'Run Selections'!AL253","v":""},{"$f":"IF(D253=\"Select Model\",\"N/A\",throwCombined(F253, D253, S253, E253,J253))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D253=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K253, M253, N253, O253),0))","v":"N/A"},{"$f":"IF(D253=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K253,M253,N253,P253)),0))","v":"N/A"},{"$f":"'Run Selections'!BD253","v":0},{"$f":"IF(LEFT($D253,4)<>\"ACBC\",\"N/A\",AdjacentZone($D253,$E253,$S253,$F253,60))","v":"N/A"},{"$f":"IF(LEFT($D253,4)<>\"ACBC\",\"N/A\",AdjacentZone($D253,$E253,$S253,$F253,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F254)=\"\",\"\",'Run Selections'!F254)","v":""},null,{"$f":"'Run Selections'!T254","v":"Select Model"},{"$f":"'Run Selections'!W254","v":4},{"$f":"'Run Selections'!Y254","v":50},{"$f":"'Run Selections'!AI254","v":""},{"$f":"'Run Selections'!AA254","v":0},null,{"$f":"'Run Selections'!AL254","v":""},{"$f":"IF(D254=\"Select Model\",\"N/A\",throwCombined(F254, D254, S254, E254,J254))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D254=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K254, M254, N254, O254),0))","v":"N/A"},{"$f":"IF(D254=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K254,M254,N254,P254)),0))","v":"N/A"},{"$f":"'Run Selections'!BD254","v":0},{"$f":"IF(LEFT($D254,4)<>\"ACBC\",\"N/A\",AdjacentZone($D254,$E254,$S254,$F254,60))","v":"N/A"},{"$f":"IF(LEFT($D254,4)<>\"ACBC\",\"N/A\",AdjacentZone($D254,$E254,$S254,$F254,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F255)=\"\",\"\",'Run Selections'!F255)","v":""},null,{"$f":"'Run Selections'!T255","v":"Select Model"},{"$f":"'Run Selections'!W255","v":4},{"$f":"'Run Selections'!Y255","v":50},{"$f":"'Run Selections'!AI255","v":""},{"$f":"'Run Selections'!AA255","v":0},null,{"$f":"'Run Selections'!AL255","v":""},{"$f":"IF(D255=\"Select Model\",\"N/A\",throwCombined(F255, D255, S255, E255,J255))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D255=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K255, M255, N255, O255),0))","v":"N/A"},{"$f":"IF(D255=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K255,M255,N255,P255)),0))","v":"N/A"},{"$f":"'Run Selections'!BD255","v":0},{"$f":"IF(LEFT($D255,4)<>\"ACBC\",\"N/A\",AdjacentZone($D255,$E255,$S255,$F255,60))","v":"N/A"},{"$f":"IF(LEFT($D255,4)<>\"ACBC\",\"N/A\",AdjacentZone($D255,$E255,$S255,$F255,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F256)=\"\",\"\",'Run Selections'!F256)","v":""},null,{"$f":"'Run Selections'!T256","v":"Select Model"},{"$f":"'Run Selections'!W256","v":4},{"$f":"'Run Selections'!Y256","v":50},{"$f":"'Run Selections'!AI256","v":""},{"$f":"'Run Selections'!AA256","v":0},null,{"$f":"'Run Selections'!AL256","v":""},{"$f":"IF(D256=\"Select Model\",\"N/A\",throwCombined(F256, D256, S256, E256,J256))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D256=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K256, M256, N256, O256),0))","v":"N/A"},{"$f":"IF(D256=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K256,M256,N256,P256)),0))","v":"N/A"},{"$f":"'Run Selections'!BD256","v":0},{"$f":"IF(LEFT($D256,4)<>\"ACBC\",\"N/A\",AdjacentZone($D256,$E256,$S256,$F256,60))","v":"N/A"},{"$f":"IF(LEFT($D256,4)<>\"ACBC\",\"N/A\",AdjacentZone($D256,$E256,$S256,$F256,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F257)=\"\",\"\",'Run Selections'!F257)","v":""},null,{"$f":"'Run Selections'!T257","v":"Select Model"},{"$f":"'Run Selections'!W257","v":4},{"$f":"'Run Selections'!Y257","v":50},{"$f":"'Run Selections'!AI257","v":""},{"$f":"'Run Selections'!AA257","v":0},null,{"$f":"'Run Selections'!AL257","v":""},{"$f":"IF(D257=\"Select Model\",\"N/A\",throwCombined(F257, D257, S257, E257,J257))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D257=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K257, M257, N257, O257),0))","v":"N/A"},{"$f":"IF(D257=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K257,M257,N257,P257)),0))","v":"N/A"},{"$f":"'Run Selections'!BD257","v":0},{"$f":"IF(LEFT($D257,4)<>\"ACBC\",\"N/A\",AdjacentZone($D257,$E257,$S257,$F257,60))","v":"N/A"},{"$f":"IF(LEFT($D257,4)<>\"ACBC\",\"N/A\",AdjacentZone($D257,$E257,$S257,$F257,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F258)=\"\",\"\",'Run Selections'!F258)","v":""},null,{"$f":"'Run Selections'!T258","v":"Select Model"},{"$f":"'Run Selections'!W258","v":4},{"$f":"'Run Selections'!Y258","v":50},{"$f":"'Run Selections'!AI258","v":""},{"$f":"'Run Selections'!AA258","v":0},null,{"$f":"'Run Selections'!AL258","v":""},{"$f":"IF(D258=\"Select Model\",\"N/A\",throwCombined(F258, D258, S258, E258,J258))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D258=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K258, M258, N258, O258),0))","v":"N/A"},{"$f":"IF(D258=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K258,M258,N258,P258)),0))","v":"N/A"},{"$f":"'Run Selections'!BD258","v":0},{"$f":"IF(LEFT($D258,4)<>\"ACBC\",\"N/A\",AdjacentZone($D258,$E258,$S258,$F258,60))","v":"N/A"},{"$f":"IF(LEFT($D258,4)<>\"ACBC\",\"N/A\",AdjacentZone($D258,$E258,$S258,$F258,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F259)=\"\",\"\",'Run Selections'!F259)","v":""},null,{"$f":"'Run Selections'!T259","v":"Select Model"},{"$f":"'Run Selections'!W259","v":4},{"$f":"'Run Selections'!Y259","v":50},{"$f":"'Run Selections'!AI259","v":""},{"$f":"'Run Selections'!AA259","v":0},null,{"$f":"'Run Selections'!AL259","v":""},{"$f":"IF(D259=\"Select Model\",\"N/A\",throwCombined(F259, D259, S259, E259,J259))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D259=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K259, M259, N259, O259),0))","v":"N/A"},{"$f":"IF(D259=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K259,M259,N259,P259)),0))","v":"N/A"},{"$f":"'Run Selections'!BD259","v":0},{"$f":"IF(LEFT($D259,4)<>\"ACBC\",\"N/A\",AdjacentZone($D259,$E259,$S259,$F259,60))","v":"N/A"},{"$f":"IF(LEFT($D259,4)<>\"ACBC\",\"N/A\",AdjacentZone($D259,$E259,$S259,$F259,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F260)=\"\",\"\",'Run Selections'!F260)","v":""},null,{"$f":"'Run Selections'!T260","v":"Select Model"},{"$f":"'Run Selections'!W260","v":4},{"$f":"'Run Selections'!Y260","v":50},{"$f":"'Run Selections'!AI260","v":""},{"$f":"'Run Selections'!AA260","v":0},null,{"$f":"'Run Selections'!AL260","v":""},{"$f":"IF(D260=\"Select Model\",\"N/A\",throwCombined(F260, D260, S260, E260,J260))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D260=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K260, M260, N260, O260),0))","v":"N/A"},{"$f":"IF(D260=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K260,M260,N260,P260)),0))","v":"N/A"},{"$f":"'Run Selections'!BD260","v":0},{"$f":"IF(LEFT($D260,4)<>\"ACBC\",\"N/A\",AdjacentZone($D260,$E260,$S260,$F260,60))","v":"N/A"},{"$f":"IF(LEFT($D260,4)<>\"ACBC\",\"N/A\",AdjacentZone($D260,$E260,$S260,$F260,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F261)=\"\",\"\",'Run Selections'!F261)","v":""},null,{"$f":"'Run Selections'!T261","v":"Select Model"},{"$f":"'Run Selections'!W261","v":4},{"$f":"'Run Selections'!Y261","v":50},{"$f":"'Run Selections'!AI261","v":""},{"$f":"'Run Selections'!AA261","v":0},null,{"$f":"'Run Selections'!AL261","v":""},{"$f":"IF(D261=\"Select Model\",\"N/A\",throwCombined(F261, D261, S261, E261,J261))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D261=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K261, M261, N261, O261),0))","v":"N/A"},{"$f":"IF(D261=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K261,M261,N261,P261)),0))","v":"N/A"},{"$f":"'Run Selections'!BD261","v":0},{"$f":"IF(LEFT($D261,4)<>\"ACBC\",\"N/A\",AdjacentZone($D261,$E261,$S261,$F261,60))","v":"N/A"},{"$f":"IF(LEFT($D261,4)<>\"ACBC\",\"N/A\",AdjacentZone($D261,$E261,$S261,$F261,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F262)=\"\",\"\",'Run Selections'!F262)","v":""},null,{"$f":"'Run Selections'!T262","v":"Select Model"},{"$f":"'Run Selections'!W262","v":4},{"$f":"'Run Selections'!Y262","v":50},{"$f":"'Run Selections'!AI262","v":""},{"$f":"'Run Selections'!AA262","v":0},null,{"$f":"'Run Selections'!AL262","v":""},{"$f":"IF(D262=\"Select Model\",\"N/A\",throwCombined(F262, D262, S262, E262,J262))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D262=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K262, M262, N262, O262),0))","v":"N/A"},{"$f":"IF(D262=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K262,M262,N262,P262)),0))","v":"N/A"},{"$f":"'Run Selections'!BD262","v":0},{"$f":"IF(LEFT($D262,4)<>\"ACBC\",\"N/A\",AdjacentZone($D262,$E262,$S262,$F262,60))","v":"N/A"},{"$f":"IF(LEFT($D262,4)<>\"ACBC\",\"N/A\",AdjacentZone($D262,$E262,$S262,$F262,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F263)=\"\",\"\",'Run Selections'!F263)","v":""},null,{"$f":"'Run Selections'!T263","v":"Select Model"},{"$f":"'Run Selections'!W263","v":4},{"$f":"'Run Selections'!Y263","v":50},{"$f":"'Run Selections'!AI263","v":""},{"$f":"'Run Selections'!AA263","v":0},null,{"$f":"'Run Selections'!AL263","v":""},{"$f":"IF(D263=\"Select Model\",\"N/A\",throwCombined(F263, D263, S263, E263,J263))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D263=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K263, M263, N263, O263),0))","v":"N/A"},{"$f":"IF(D263=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K263,M263,N263,P263)),0))","v":"N/A"},{"$f":"'Run Selections'!BD263","v":0},{"$f":"IF(LEFT($D263,4)<>\"ACBC\",\"N/A\",AdjacentZone($D263,$E263,$S263,$F263,60))","v":"N/A"},{"$f":"IF(LEFT($D263,4)<>\"ACBC\",\"N/A\",AdjacentZone($D263,$E263,$S263,$F263,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F264)=\"\",\"\",'Run Selections'!F264)","v":""},null,{"$f":"'Run Selections'!T264","v":"Select Model"},{"$f":"'Run Selections'!W264","v":4},{"$f":"'Run Selections'!Y264","v":50},{"$f":"'Run Selections'!AI264","v":""},{"$f":"'Run Selections'!AA264","v":0},null,{"$f":"'Run Selections'!AL264","v":""},{"$f":"IF(D264=\"Select Model\",\"N/A\",throwCombined(F264, D264, S264, E264,J264))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D264=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K264, M264, N264, O264),0))","v":"N/A"},{"$f":"IF(D264=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K264,M264,N264,P264)),0))","v":"N/A"},{"$f":"'Run Selections'!BD264","v":0},{"$f":"IF(LEFT($D264,4)<>\"ACBC\",\"N/A\",AdjacentZone($D264,$E264,$S264,$F264,60))","v":"N/A"},{"$f":"IF(LEFT($D264,4)<>\"ACBC\",\"N/A\",AdjacentZone($D264,$E264,$S264,$F264,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F265)=\"\",\"\",'Run Selections'!F265)","v":""},null,{"$f":"'Run Selections'!T265","v":"Select Model"},{"$f":"'Run Selections'!W265","v":4},{"$f":"'Run Selections'!Y265","v":50},{"$f":"'Run Selections'!AI265","v":""},{"$f":"'Run Selections'!AA265","v":0},null,{"$f":"'Run Selections'!AL265","v":""},{"$f":"IF(D265=\"Select Model\",\"N/A\",throwCombined(F265, D265, S265, E265,J265))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D265=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K265, M265, N265, O265),0))","v":"N/A"},{"$f":"IF(D265=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K265,M265,N265,P265)),0))","v":"N/A"},{"$f":"'Run Selections'!BD265","v":0},{"$f":"IF(LEFT($D265,4)<>\"ACBC\",\"N/A\",AdjacentZone($D265,$E265,$S265,$F265,60))","v":"N/A"},{"$f":"IF(LEFT($D265,4)<>\"ACBC\",\"N/A\",AdjacentZone($D265,$E265,$S265,$F265,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F266)=\"\",\"\",'Run Selections'!F266)","v":""},null,{"$f":"'Run Selections'!T266","v":"Select Model"},{"$f":"'Run Selections'!W266","v":4},{"$f":"'Run Selections'!Y266","v":50},{"$f":"'Run Selections'!AI266","v":""},{"$f":"'Run Selections'!AA266","v":0},null,{"$f":"'Run Selections'!AL266","v":""},{"$f":"IF(D266=\"Select Model\",\"N/A\",throwCombined(F266, D266, S266, E266,J266))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D266=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K266, M266, N266, O266),0))","v":"N/A"},{"$f":"IF(D266=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K266,M266,N266,P266)),0))","v":"N/A"},{"$f":"'Run Selections'!BD266","v":0},{"$f":"IF(LEFT($D266,4)<>\"ACBC\",\"N/A\",AdjacentZone($D266,$E266,$S266,$F266,60))","v":"N/A"},{"$f":"IF(LEFT($D266,4)<>\"ACBC\",\"N/A\",AdjacentZone($D266,$E266,$S266,$F266,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F267)=\"\",\"\",'Run Selections'!F267)","v":""},null,{"$f":"'Run Selections'!T267","v":"Select Model"},{"$f":"'Run Selections'!W267","v":4},{"$f":"'Run Selections'!Y267","v":50},{"$f":"'Run Selections'!AI267","v":""},{"$f":"'Run Selections'!AA267","v":0},null,{"$f":"'Run Selections'!AL267","v":""},{"$f":"IF(D267=\"Select Model\",\"N/A\",throwCombined(F267, D267, S267, E267,J267))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D267=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K267, M267, N267, O267),0))","v":"N/A"},{"$f":"IF(D267=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K267,M267,N267,P267)),0))","v":"N/A"},{"$f":"'Run Selections'!BD267","v":0},{"$f":"IF(LEFT($D267,4)<>\"ACBC\",\"N/A\",AdjacentZone($D267,$E267,$S267,$F267,60))","v":"N/A"},{"$f":"IF(LEFT($D267,4)<>\"ACBC\",\"N/A\",AdjacentZone($D267,$E267,$S267,$F267,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F268)=\"\",\"\",'Run Selections'!F268)","v":""},null,{"$f":"'Run Selections'!T268","v":"Select Model"},{"$f":"'Run Selections'!W268","v":4},{"$f":"'Run Selections'!Y268","v":50},{"$f":"'Run Selections'!AI268","v":""},{"$f":"'Run Selections'!AA268","v":0},null,{"$f":"'Run Selections'!AL268","v":""},{"$f":"IF(D268=\"Select Model\",\"N/A\",throwCombined(F268, D268, S268, E268,J268))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D268=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K268, M268, N268, O268),0))","v":"N/A"},{"$f":"IF(D268=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K268,M268,N268,P268)),0))","v":"N/A"},{"$f":"'Run Selections'!BD268","v":0},{"$f":"IF(LEFT($D268,4)<>\"ACBC\",\"N/A\",AdjacentZone($D268,$E268,$S268,$F268,60))","v":"N/A"},{"$f":"IF(LEFT($D268,4)<>\"ACBC\",\"N/A\",AdjacentZone($D268,$E268,$S268,$F268,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F269)=\"\",\"\",'Run Selections'!F269)","v":""},null,{"$f":"'Run Selections'!T269","v":"Select Model"},{"$f":"'Run Selections'!W269","v":4},{"$f":"'Run Selections'!Y269","v":50},{"$f":"'Run Selections'!AI269","v":""},{"$f":"'Run Selections'!AA269","v":0},null,{"$f":"'Run Selections'!AL269","v":""},{"$f":"IF(D269=\"Select Model\",\"N/A\",throwCombined(F269, D269, S269, E269,J269))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D269=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K269, M269, N269, O269),0))","v":"N/A"},{"$f":"IF(D269=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K269,M269,N269,P269)),0))","v":"N/A"},{"$f":"'Run Selections'!BD269","v":0},{"$f":"IF(LEFT($D269,4)<>\"ACBC\",\"N/A\",AdjacentZone($D269,$E269,$S269,$F269,60))","v":"N/A"},{"$f":"IF(LEFT($D269,4)<>\"ACBC\",\"N/A\",AdjacentZone($D269,$E269,$S269,$F269,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F270)=\"\",\"\",'Run Selections'!F270)","v":""},null,{"$f":"'Run Selections'!T270","v":"Select Model"},{"$f":"'Run Selections'!W270","v":4},{"$f":"'Run Selections'!Y270","v":50},{"$f":"'Run Selections'!AI270","v":""},{"$f":"'Run Selections'!AA270","v":0},null,{"$f":"'Run Selections'!AL270","v":""},{"$f":"IF(D270=\"Select Model\",\"N/A\",throwCombined(F270, D270, S270, E270,J270))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D270=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K270, M270, N270, O270),0))","v":"N/A"},{"$f":"IF(D270=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K270,M270,N270,P270)),0))","v":"N/A"},{"$f":"'Run Selections'!BD270","v":0},{"$f":"IF(LEFT($D270,4)<>\"ACBC\",\"N/A\",AdjacentZone($D270,$E270,$S270,$F270,60))","v":"N/A"},{"$f":"IF(LEFT($D270,4)<>\"ACBC\",\"N/A\",AdjacentZone($D270,$E270,$S270,$F270,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F271)=\"\",\"\",'Run Selections'!F271)","v":""},null,{"$f":"'Run Selections'!T271","v":"Select Model"},{"$f":"'Run Selections'!W271","v":4},{"$f":"'Run Selections'!Y271","v":50},{"$f":"'Run Selections'!AI271","v":""},{"$f":"'Run Selections'!AA271","v":0},null,{"$f":"'Run Selections'!AL271","v":""},{"$f":"IF(D271=\"Select Model\",\"N/A\",throwCombined(F271, D271, S271, E271,J271))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D271=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K271, M271, N271, O271),0))","v":"N/A"},{"$f":"IF(D271=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K271,M271,N271,P271)),0))","v":"N/A"},{"$f":"'Run Selections'!BD271","v":0},{"$f":"IF(LEFT($D271,4)<>\"ACBC\",\"N/A\",AdjacentZone($D271,$E271,$S271,$F271,60))","v":"N/A"},{"$f":"IF(LEFT($D271,4)<>\"ACBC\",\"N/A\",AdjacentZone($D271,$E271,$S271,$F271,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F272)=\"\",\"\",'Run Selections'!F272)","v":""},null,{"$f":"'Run Selections'!T272","v":"Select Model"},{"$f":"'Run Selections'!W272","v":4},{"$f":"'Run Selections'!Y272","v":50},{"$f":"'Run Selections'!AI272","v":""},{"$f":"'Run Selections'!AA272","v":0},null,{"$f":"'Run Selections'!AL272","v":""},{"$f":"IF(D272=\"Select Model\",\"N/A\",throwCombined(F272, D272, S272, E272,J272))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D272=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K272, M272, N272, O272),0))","v":"N/A"},{"$f":"IF(D272=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K272,M272,N272,P272)),0))","v":"N/A"},{"$f":"'Run Selections'!BD272","v":0},{"$f":"IF(LEFT($D272,4)<>\"ACBC\",\"N/A\",AdjacentZone($D272,$E272,$S272,$F272,60))","v":"N/A"},{"$f":"IF(LEFT($D272,4)<>\"ACBC\",\"N/A\",AdjacentZone($D272,$E272,$S272,$F272,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F273)=\"\",\"\",'Run Selections'!F273)","v":""},null,{"$f":"'Run Selections'!T273","v":"Select Model"},{"$f":"'Run Selections'!W273","v":4},{"$f":"'Run Selections'!Y273","v":50},{"$f":"'Run Selections'!AI273","v":""},{"$f":"'Run Selections'!AA273","v":0},null,{"$f":"'Run Selections'!AL273","v":""},{"$f":"IF(D273=\"Select Model\",\"N/A\",throwCombined(F273, D273, S273, E273,J273))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D273=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K273, M273, N273, O273),0))","v":"N/A"},{"$f":"IF(D273=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K273,M273,N273,P273)),0))","v":"N/A"},{"$f":"'Run Selections'!BD273","v":0},{"$f":"IF(LEFT($D273,4)<>\"ACBC\",\"N/A\",AdjacentZone($D273,$E273,$S273,$F273,60))","v":"N/A"},{"$f":"IF(LEFT($D273,4)<>\"ACBC\",\"N/A\",AdjacentZone($D273,$E273,$S273,$F273,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F274)=\"\",\"\",'Run Selections'!F274)","v":""},null,{"$f":"'Run Selections'!T274","v":"Select Model"},{"$f":"'Run Selections'!W274","v":4},{"$f":"'Run Selections'!Y274","v":50},{"$f":"'Run Selections'!AI274","v":""},{"$f":"'Run Selections'!AA274","v":0},null,{"$f":"'Run Selections'!AL274","v":""},{"$f":"IF(D274=\"Select Model\",\"N/A\",throwCombined(F274, D274, S274, E274,J274))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D274=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K274, M274, N274, O274),0))","v":"N/A"},{"$f":"IF(D274=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K274,M274,N274,P274)),0))","v":"N/A"},{"$f":"'Run Selections'!BD274","v":0},{"$f":"IF(LEFT($D274,4)<>\"ACBC\",\"N/A\",AdjacentZone($D274,$E274,$S274,$F274,60))","v":"N/A"},{"$f":"IF(LEFT($D274,4)<>\"ACBC\",\"N/A\",AdjacentZone($D274,$E274,$S274,$F274,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F275)=\"\",\"\",'Run Selections'!F275)","v":""},null,{"$f":"'Run Selections'!T275","v":"Select Model"},{"$f":"'Run Selections'!W275","v":4},{"$f":"'Run Selections'!Y275","v":50},{"$f":"'Run Selections'!AI275","v":""},{"$f":"'Run Selections'!AA275","v":0},null,{"$f":"'Run Selections'!AL275","v":""},{"$f":"IF(D275=\"Select Model\",\"N/A\",throwCombined(F275, D275, S275, E275,J275))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D275=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K275, M275, N275, O275),0))","v":"N/A"},{"$f":"IF(D275=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K275,M275,N275,P275)),0))","v":"N/A"},{"$f":"'Run Selections'!BD275","v":0},{"$f":"IF(LEFT($D275,4)<>\"ACBC\",\"N/A\",AdjacentZone($D275,$E275,$S275,$F275,60))","v":"N/A"},{"$f":"IF(LEFT($D275,4)<>\"ACBC\",\"N/A\",AdjacentZone($D275,$E275,$S275,$F275,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F276)=\"\",\"\",'Run Selections'!F276)","v":""},null,{"$f":"'Run Selections'!T276","v":"Select Model"},{"$f":"'Run Selections'!W276","v":4},{"$f":"'Run Selections'!Y276","v":50},{"$f":"'Run Selections'!AI276","v":""},{"$f":"'Run Selections'!AA276","v":0},null,{"$f":"'Run Selections'!AL276","v":""},{"$f":"IF(D276=\"Select Model\",\"N/A\",throwCombined(F276, D276, S276, E276,J276))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D276=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K276, M276, N276, O276),0))","v":"N/A"},{"$f":"IF(D276=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K276,M276,N276,P276)),0))","v":"N/A"},{"$f":"'Run Selections'!BD276","v":0},{"$f":"IF(LEFT($D276,4)<>\"ACBC\",\"N/A\",AdjacentZone($D276,$E276,$S276,$F276,60))","v":"N/A"},{"$f":"IF(LEFT($D276,4)<>\"ACBC\",\"N/A\",AdjacentZone($D276,$E276,$S276,$F276,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F277)=\"\",\"\",'Run Selections'!F277)","v":""},null,{"$f":"'Run Selections'!T277","v":"Select Model"},{"$f":"'Run Selections'!W277","v":4},{"$f":"'Run Selections'!Y277","v":50},{"$f":"'Run Selections'!AI277","v":""},{"$f":"'Run Selections'!AA277","v":0},null,{"$f":"'Run Selections'!AL277","v":""},{"$f":"IF(D277=\"Select Model\",\"N/A\",throwCombined(F277, D277, S277, E277,J277))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D277=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K277, M277, N277, O277),0))","v":"N/A"},{"$f":"IF(D277=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K277,M277,N277,P277)),0))","v":"N/A"},{"$f":"'Run Selections'!BD277","v":0},{"$f":"IF(LEFT($D277,4)<>\"ACBC\",\"N/A\",AdjacentZone($D277,$E277,$S277,$F277,60))","v":"N/A"},{"$f":"IF(LEFT($D277,4)<>\"ACBC\",\"N/A\",AdjacentZone($D277,$E277,$S277,$F277,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F278)=\"\",\"\",'Run Selections'!F278)","v":""},null,{"$f":"'Run Selections'!T278","v":"Select Model"},{"$f":"'Run Selections'!W278","v":4},{"$f":"'Run Selections'!Y278","v":50},{"$f":"'Run Selections'!AI278","v":""},{"$f":"'Run Selections'!AA278","v":0},null,{"$f":"'Run Selections'!AL278","v":""},{"$f":"IF(D278=\"Select Model\",\"N/A\",throwCombined(F278, D278, S278, E278,J278))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D278=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K278, M278, N278, O278),0))","v":"N/A"},{"$f":"IF(D278=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K278,M278,N278,P278)),0))","v":"N/A"},{"$f":"'Run Selections'!BD278","v":0},{"$f":"IF(LEFT($D278,4)<>\"ACBC\",\"N/A\",AdjacentZone($D278,$E278,$S278,$F278,60))","v":"N/A"},{"$f":"IF(LEFT($D278,4)<>\"ACBC\",\"N/A\",AdjacentZone($D278,$E278,$S278,$F278,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F279)=\"\",\"\",'Run Selections'!F279)","v":""},null,{"$f":"'Run Selections'!T279","v":"Select Model"},{"$f":"'Run Selections'!W279","v":4},{"$f":"'Run Selections'!Y279","v":50},{"$f":"'Run Selections'!AI279","v":""},{"$f":"'Run Selections'!AA279","v":0},null,{"$f":"'Run Selections'!AL279","v":""},{"$f":"IF(D279=\"Select Model\",\"N/A\",throwCombined(F279, D279, S279, E279,J279))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D279=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K279, M279, N279, O279),0))","v":"N/A"},{"$f":"IF(D279=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K279,M279,N279,P279)),0))","v":"N/A"},{"$f":"'Run Selections'!BD279","v":0},{"$f":"IF(LEFT($D279,4)<>\"ACBC\",\"N/A\",AdjacentZone($D279,$E279,$S279,$F279,60))","v":"N/A"},{"$f":"IF(LEFT($D279,4)<>\"ACBC\",\"N/A\",AdjacentZone($D279,$E279,$S279,$F279,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F280)=\"\",\"\",'Run Selections'!F280)","v":""},null,{"$f":"'Run Selections'!T280","v":"Select Model"},{"$f":"'Run Selections'!W280","v":4},{"$f":"'Run Selections'!Y280","v":50},{"$f":"'Run Selections'!AI280","v":""},{"$f":"'Run Selections'!AA280","v":0},null,{"$f":"'Run Selections'!AL280","v":""},{"$f":"IF(D280=\"Select Model\",\"N/A\",throwCombined(F280, D280, S280, E280,J280))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D280=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K280, M280, N280, O280),0))","v":"N/A"},{"$f":"IF(D280=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K280,M280,N280,P280)),0))","v":"N/A"},{"$f":"'Run Selections'!BD280","v":0},{"$f":"IF(LEFT($D280,4)<>\"ACBC\",\"N/A\",AdjacentZone($D280,$E280,$S280,$F280,60))","v":"N/A"},{"$f":"IF(LEFT($D280,4)<>\"ACBC\",\"N/A\",AdjacentZone($D280,$E280,$S280,$F280,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F281)=\"\",\"\",'Run Selections'!F281)","v":""},null,{"$f":"'Run Selections'!T281","v":"Select Model"},{"$f":"'Run Selections'!W281","v":4},{"$f":"'Run Selections'!Y281","v":50},{"$f":"'Run Selections'!AI281","v":""},{"$f":"'Run Selections'!AA281","v":0},null,{"$f":"'Run Selections'!AL281","v":""},{"$f":"IF(D281=\"Select Model\",\"N/A\",throwCombined(F281, D281, S281, E281,J281))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D281=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K281, M281, N281, O281),0))","v":"N/A"},{"$f":"IF(D281=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K281,M281,N281,P281)),0))","v":"N/A"},{"$f":"'Run Selections'!BD281","v":0},{"$f":"IF(LEFT($D281,4)<>\"ACBC\",\"N/A\",AdjacentZone($D281,$E281,$S281,$F281,60))","v":"N/A"},{"$f":"IF(LEFT($D281,4)<>\"ACBC\",\"N/A\",AdjacentZone($D281,$E281,$S281,$F281,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F282)=\"\",\"\",'Run Selections'!F282)","v":""},null,{"$f":"'Run Selections'!T282","v":"Select Model"},{"$f":"'Run Selections'!W282","v":4},{"$f":"'Run Selections'!Y282","v":50},{"$f":"'Run Selections'!AI282","v":""},{"$f":"'Run Selections'!AA282","v":0},null,{"$f":"'Run Selections'!AL282","v":""},{"$f":"IF(D282=\"Select Model\",\"N/A\",throwCombined(F282, D282, S282, E282,J282))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D282=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K282, M282, N282, O282),0))","v":"N/A"},{"$f":"IF(D282=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K282,M282,N282,P282)),0))","v":"N/A"},{"$f":"'Run Selections'!BD282","v":0},{"$f":"IF(LEFT($D282,4)<>\"ACBC\",\"N/A\",AdjacentZone($D282,$E282,$S282,$F282,60))","v":"N/A"},{"$f":"IF(LEFT($D282,4)<>\"ACBC\",\"N/A\",AdjacentZone($D282,$E282,$S282,$F282,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F283)=\"\",\"\",'Run Selections'!F283)","v":""},null,{"$f":"'Run Selections'!T283","v":"Select Model"},{"$f":"'Run Selections'!W283","v":4},{"$f":"'Run Selections'!Y283","v":50},{"$f":"'Run Selections'!AI283","v":""},{"$f":"'Run Selections'!AA283","v":0},null,{"$f":"'Run Selections'!AL283","v":""},{"$f":"IF(D283=\"Select Model\",\"N/A\",throwCombined(F283, D283, S283, E283,J283))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D283=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K283, M283, N283, O283),0))","v":"N/A"},{"$f":"IF(D283=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K283,M283,N283,P283)),0))","v":"N/A"},{"$f":"'Run Selections'!BD283","v":0},{"$f":"IF(LEFT($D283,4)<>\"ACBC\",\"N/A\",AdjacentZone($D283,$E283,$S283,$F283,60))","v":"N/A"},{"$f":"IF(LEFT($D283,4)<>\"ACBC\",\"N/A\",AdjacentZone($D283,$E283,$S283,$F283,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F284)=\"\",\"\",'Run Selections'!F284)","v":""},null,{"$f":"'Run Selections'!T284","v":"Select Model"},{"$f":"'Run Selections'!W284","v":4},{"$f":"'Run Selections'!Y284","v":50},{"$f":"'Run Selections'!AI284","v":""},{"$f":"'Run Selections'!AA284","v":0},null,{"$f":"'Run Selections'!AL284","v":""},{"$f":"IF(D284=\"Select Model\",\"N/A\",throwCombined(F284, D284, S284, E284,J284))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D284=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K284, M284, N284, O284),0))","v":"N/A"},{"$f":"IF(D284=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K284,M284,N284,P284)),0))","v":"N/A"},{"$f":"'Run Selections'!BD284","v":0},{"$f":"IF(LEFT($D284,4)<>\"ACBC\",\"N/A\",AdjacentZone($D284,$E284,$S284,$F284,60))","v":"N/A"},{"$f":"IF(LEFT($D284,4)<>\"ACBC\",\"N/A\",AdjacentZone($D284,$E284,$S284,$F284,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F285)=\"\",\"\",'Run Selections'!F285)","v":""},null,{"$f":"'Run Selections'!T285","v":"Select Model"},{"$f":"'Run Selections'!W285","v":4},{"$f":"'Run Selections'!Y285","v":50},{"$f":"'Run Selections'!AI285","v":""},{"$f":"'Run Selections'!AA285","v":0},null,{"$f":"'Run Selections'!AL285","v":""},{"$f":"IF(D285=\"Select Model\",\"N/A\",throwCombined(F285, D285, S285, E285,J285))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D285=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K285, M285, N285, O285),0))","v":"N/A"},{"$f":"IF(D285=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K285,M285,N285,P285)),0))","v":"N/A"},{"$f":"'Run Selections'!BD285","v":0},{"$f":"IF(LEFT($D285,4)<>\"ACBC\",\"N/A\",AdjacentZone($D285,$E285,$S285,$F285,60))","v":"N/A"},{"$f":"IF(LEFT($D285,4)<>\"ACBC\",\"N/A\",AdjacentZone($D285,$E285,$S285,$F285,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F286)=\"\",\"\",'Run Selections'!F286)","v":""},null,{"$f":"'Run Selections'!T286","v":"Select Model"},{"$f":"'Run Selections'!W286","v":4},{"$f":"'Run Selections'!Y286","v":50},{"$f":"'Run Selections'!AI286","v":""},{"$f":"'Run Selections'!AA286","v":0},null,{"$f":"'Run Selections'!AL286","v":""},{"$f":"IF(D286=\"Select Model\",\"N/A\",throwCombined(F286, D286, S286, E286,J286))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D286=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K286, M286, N286, O286),0))","v":"N/A"},{"$f":"IF(D286=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K286,M286,N286,P286)),0))","v":"N/A"},{"$f":"'Run Selections'!BD286","v":0},{"$f":"IF(LEFT($D286,4)<>\"ACBC\",\"N/A\",AdjacentZone($D286,$E286,$S286,$F286,60))","v":"N/A"},{"$f":"IF(LEFT($D286,4)<>\"ACBC\",\"N/A\",AdjacentZone($D286,$E286,$S286,$F286,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F287)=\"\",\"\",'Run Selections'!F287)","v":""},null,{"$f":"'Run Selections'!T287","v":"Select Model"},{"$f":"'Run Selections'!W287","v":4},{"$f":"'Run Selections'!Y287","v":50},{"$f":"'Run Selections'!AI287","v":""},{"$f":"'Run Selections'!AA287","v":0},null,{"$f":"'Run Selections'!AL287","v":""},{"$f":"IF(D287=\"Select Model\",\"N/A\",throwCombined(F287, D287, S287, E287,J287))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D287=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K287, M287, N287, O287),0))","v":"N/A"},{"$f":"IF(D287=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K287,M287,N287,P287)),0))","v":"N/A"},{"$f":"'Run Selections'!BD287","v":0},{"$f":"IF(LEFT($D287,4)<>\"ACBC\",\"N/A\",AdjacentZone($D287,$E287,$S287,$F287,60))","v":"N/A"},{"$f":"IF(LEFT($D287,4)<>\"ACBC\",\"N/A\",AdjacentZone($D287,$E287,$S287,$F287,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F288)=\"\",\"\",'Run Selections'!F288)","v":""},null,{"$f":"'Run Selections'!T288","v":"Select Model"},{"$f":"'Run Selections'!W288","v":4},{"$f":"'Run Selections'!Y288","v":50},{"$f":"'Run Selections'!AI288","v":""},{"$f":"'Run Selections'!AA288","v":0},null,{"$f":"'Run Selections'!AL288","v":""},{"$f":"IF(D288=\"Select Model\",\"N/A\",throwCombined(F288, D288, S288, E288,J288))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D288=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K288, M288, N288, O288),0))","v":"N/A"},{"$f":"IF(D288=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K288,M288,N288,P288)),0))","v":"N/A"},{"$f":"'Run Selections'!BD288","v":0},{"$f":"IF(LEFT($D288,4)<>\"ACBC\",\"N/A\",AdjacentZone($D288,$E288,$S288,$F288,60))","v":"N/A"},{"$f":"IF(LEFT($D288,4)<>\"ACBC\",\"N/A\",AdjacentZone($D288,$E288,$S288,$F288,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F289)=\"\",\"\",'Run Selections'!F289)","v":""},null,{"$f":"'Run Selections'!T289","v":"Select Model"},{"$f":"'Run Selections'!W289","v":4},{"$f":"'Run Selections'!Y289","v":50},{"$f":"'Run Selections'!AI289","v":""},{"$f":"'Run Selections'!AA289","v":0},null,{"$f":"'Run Selections'!AL289","v":""},{"$f":"IF(D289=\"Select Model\",\"N/A\",throwCombined(F289, D289, S289, E289,J289))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D289=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K289, M289, N289, O289),0))","v":"N/A"},{"$f":"IF(D289=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K289,M289,N289,P289)),0))","v":"N/A"},{"$f":"'Run Selections'!BD289","v":0},{"$f":"IF(LEFT($D289,4)<>\"ACBC\",\"N/A\",AdjacentZone($D289,$E289,$S289,$F289,60))","v":"N/A"},{"$f":"IF(LEFT($D289,4)<>\"ACBC\",\"N/A\",AdjacentZone($D289,$E289,$S289,$F289,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F290)=\"\",\"\",'Run Selections'!F290)","v":""},null,{"$f":"'Run Selections'!T290","v":"Select Model"},{"$f":"'Run Selections'!W290","v":4},{"$f":"'Run Selections'!Y290","v":50},{"$f":"'Run Selections'!AI290","v":""},{"$f":"'Run Selections'!AA290","v":0},null,{"$f":"'Run Selections'!AL290","v":""},{"$f":"IF(D290=\"Select Model\",\"N/A\",throwCombined(F290, D290, S290, E290,J290))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D290=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K290, M290, N290, O290),0))","v":"N/A"},{"$f":"IF(D290=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K290,M290,N290,P290)),0))","v":"N/A"},{"$f":"'Run Selections'!BD290","v":0},{"$f":"IF(LEFT($D290,4)<>\"ACBC\",\"N/A\",AdjacentZone($D290,$E290,$S290,$F290,60))","v":"N/A"},{"$f":"IF(LEFT($D290,4)<>\"ACBC\",\"N/A\",AdjacentZone($D290,$E290,$S290,$F290,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F291)=\"\",\"\",'Run Selections'!F291)","v":""},null,{"$f":"'Run Selections'!T291","v":"Select Model"},{"$f":"'Run Selections'!W291","v":4},{"$f":"'Run Selections'!Y291","v":50},{"$f":"'Run Selections'!AI291","v":""},{"$f":"'Run Selections'!AA291","v":0},null,{"$f":"'Run Selections'!AL291","v":""},{"$f":"IF(D291=\"Select Model\",\"N/A\",throwCombined(F291, D291, S291, E291,J291))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D291=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K291, M291, N291, O291),0))","v":"N/A"},{"$f":"IF(D291=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K291,M291,N291,P291)),0))","v":"N/A"},{"$f":"'Run Selections'!BD291","v":0},{"$f":"IF(LEFT($D291,4)<>\"ACBC\",\"N/A\",AdjacentZone($D291,$E291,$S291,$F291,60))","v":"N/A"},{"$f":"IF(LEFT($D291,4)<>\"ACBC\",\"N/A\",AdjacentZone($D291,$E291,$S291,$F291,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F292)=\"\",\"\",'Run Selections'!F292)","v":""},null,{"$f":"'Run Selections'!T292","v":"Select Model"},{"$f":"'Run Selections'!W292","v":4},{"$f":"'Run Selections'!Y292","v":50},{"$f":"'Run Selections'!AI292","v":""},{"$f":"'Run Selections'!AA292","v":0},null,{"$f":"'Run Selections'!AL292","v":""},{"$f":"IF(D292=\"Select Model\",\"N/A\",throwCombined(F292, D292, S292, E292,J292))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D292=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K292, M292, N292, O292),0))","v":"N/A"},{"$f":"IF(D292=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K292,M292,N292,P292)),0))","v":"N/A"},{"$f":"'Run Selections'!BD292","v":0},{"$f":"IF(LEFT($D292,4)<>\"ACBC\",\"N/A\",AdjacentZone($D292,$E292,$S292,$F292,60))","v":"N/A"},{"$f":"IF(LEFT($D292,4)<>\"ACBC\",\"N/A\",AdjacentZone($D292,$E292,$S292,$F292,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F293)=\"\",\"\",'Run Selections'!F293)","v":""},null,{"$f":"'Run Selections'!T293","v":"Select Model"},{"$f":"'Run Selections'!W293","v":4},{"$f":"'Run Selections'!Y293","v":50},{"$f":"'Run Selections'!AI293","v":""},{"$f":"'Run Selections'!AA293","v":0},null,{"$f":"'Run Selections'!AL293","v":""},{"$f":"IF(D293=\"Select Model\",\"N/A\",throwCombined(F293, D293, S293, E293,J293))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D293=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K293, M293, N293, O293),0))","v":"N/A"},{"$f":"IF(D293=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K293,M293,N293,P293)),0))","v":"N/A"},{"$f":"'Run Selections'!BD293","v":0},{"$f":"IF(LEFT($D293,4)<>\"ACBC\",\"N/A\",AdjacentZone($D293,$E293,$S293,$F293,60))","v":"N/A"},{"$f":"IF(LEFT($D293,4)<>\"ACBC\",\"N/A\",AdjacentZone($D293,$E293,$S293,$F293,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F294)=\"\",\"\",'Run Selections'!F294)","v":""},null,{"$f":"'Run Selections'!T294","v":"Select Model"},{"$f":"'Run Selections'!W294","v":4},{"$f":"'Run Selections'!Y294","v":50},{"$f":"'Run Selections'!AI294","v":""},{"$f":"'Run Selections'!AA294","v":0},null,{"$f":"'Run Selections'!AL294","v":""},{"$f":"IF(D294=\"Select Model\",\"N/A\",throwCombined(F294, D294, S294, E294,J294))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D294=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K294, M294, N294, O294),0))","v":"N/A"},{"$f":"IF(D294=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K294,M294,N294,P294)),0))","v":"N/A"},{"$f":"'Run Selections'!BD294","v":0},{"$f":"IF(LEFT($D294,4)<>\"ACBC\",\"N/A\",AdjacentZone($D294,$E294,$S294,$F294,60))","v":"N/A"},{"$f":"IF(LEFT($D294,4)<>\"ACBC\",\"N/A\",AdjacentZone($D294,$E294,$S294,$F294,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F295)=\"\",\"\",'Run Selections'!F295)","v":""},null,{"$f":"'Run Selections'!T295","v":"Select Model"},{"$f":"'Run Selections'!W295","v":4},{"$f":"'Run Selections'!Y295","v":50},{"$f":"'Run Selections'!AI295","v":""},{"$f":"'Run Selections'!AA295","v":0},null,{"$f":"'Run Selections'!AL295","v":""},{"$f":"IF(D295=\"Select Model\",\"N/A\",throwCombined(F295, D295, S295, E295,J295))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D295=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K295, M295, N295, O295),0))","v":"N/A"},{"$f":"IF(D295=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K295,M295,N295,P295)),0))","v":"N/A"},{"$f":"'Run Selections'!BD295","v":0},{"$f":"IF(LEFT($D295,4)<>\"ACBC\",\"N/A\",AdjacentZone($D295,$E295,$S295,$F295,60))","v":"N/A"},{"$f":"IF(LEFT($D295,4)<>\"ACBC\",\"N/A\",AdjacentZone($D295,$E295,$S295,$F295,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F296)=\"\",\"\",'Run Selections'!F296)","v":""},null,{"$f":"'Run Selections'!T296","v":"Select Model"},{"$f":"'Run Selections'!W296","v":4},{"$f":"'Run Selections'!Y296","v":50},{"$f":"'Run Selections'!AI296","v":""},{"$f":"'Run Selections'!AA296","v":0},null,{"$f":"'Run Selections'!AL296","v":""},{"$f":"IF(D296=\"Select Model\",\"N/A\",throwCombined(F296, D296, S296, E296,J296))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D296=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K296, M296, N296, O296),0))","v":"N/A"},{"$f":"IF(D296=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K296,M296,N296,P296)),0))","v":"N/A"},{"$f":"'Run Selections'!BD296","v":0},{"$f":"IF(LEFT($D296,4)<>\"ACBC\",\"N/A\",AdjacentZone($D296,$E296,$S296,$F296,60))","v":"N/A"},{"$f":"IF(LEFT($D296,4)<>\"ACBC\",\"N/A\",AdjacentZone($D296,$E296,$S296,$F296,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F297)=\"\",\"\",'Run Selections'!F297)","v":""},null,{"$f":"'Run Selections'!T297","v":"Select Model"},{"$f":"'Run Selections'!W297","v":4},{"$f":"'Run Selections'!Y297","v":50},{"$f":"'Run Selections'!AI297","v":""},{"$f":"'Run Selections'!AA297","v":0},null,{"$f":"'Run Selections'!AL297","v":""},{"$f":"IF(D297=\"Select Model\",\"N/A\",throwCombined(F297, D297, S297, E297,J297))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D297=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K297, M297, N297, O297),0))","v":"N/A"},{"$f":"IF(D297=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K297,M297,N297,P297)),0))","v":"N/A"},{"$f":"'Run Selections'!BD297","v":0},{"$f":"IF(LEFT($D297,4)<>\"ACBC\",\"N/A\",AdjacentZone($D297,$E297,$S297,$F297,60))","v":"N/A"},{"$f":"IF(LEFT($D297,4)<>\"ACBC\",\"N/A\",AdjacentZone($D297,$E297,$S297,$F297,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F298)=\"\",\"\",'Run Selections'!F298)","v":""},null,{"$f":"'Run Selections'!T298","v":"Select Model"},{"$f":"'Run Selections'!W298","v":4},{"$f":"'Run Selections'!Y298","v":50},{"$f":"'Run Selections'!AI298","v":""},{"$f":"'Run Selections'!AA298","v":0},null,{"$f":"'Run Selections'!AL298","v":""},{"$f":"IF(D298=\"Select Model\",\"N/A\",throwCombined(F298, D298, S298, E298,J298))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D298=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K298, M298, N298, O298),0))","v":"N/A"},{"$f":"IF(D298=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K298,M298,N298,P298)),0))","v":"N/A"},{"$f":"'Run Selections'!BD298","v":0},{"$f":"IF(LEFT($D298,4)<>\"ACBC\",\"N/A\",AdjacentZone($D298,$E298,$S298,$F298,60))","v":"N/A"},{"$f":"IF(LEFT($D298,4)<>\"ACBC\",\"N/A\",AdjacentZone($D298,$E298,$S298,$F298,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F299)=\"\",\"\",'Run Selections'!F299)","v":""},null,{"$f":"'Run Selections'!T299","v":"Select Model"},{"$f":"'Run Selections'!W299","v":4},{"$f":"'Run Selections'!Y299","v":50},{"$f":"'Run Selections'!AI299","v":""},{"$f":"'Run Selections'!AA299","v":0},null,{"$f":"'Run Selections'!AL299","v":""},{"$f":"IF(D299=\"Select Model\",\"N/A\",throwCombined(F299, D299, S299, E299,J299))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D299=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K299, M299, N299, O299),0))","v":"N/A"},{"$f":"IF(D299=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K299,M299,N299,P299)),0))","v":"N/A"},{"$f":"'Run Selections'!BD299","v":0},{"$f":"IF(LEFT($D299,4)<>\"ACBC\",\"N/A\",AdjacentZone($D299,$E299,$S299,$F299,60))","v":"N/A"},{"$f":"IF(LEFT($D299,4)<>\"ACBC\",\"N/A\",AdjacentZone($D299,$E299,$S299,$F299,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F300)=\"\",\"\",'Run Selections'!F300)","v":""},null,{"$f":"'Run Selections'!T300","v":"Select Model"},{"$f":"'Run Selections'!W300","v":4},{"$f":"'Run Selections'!Y300","v":50},{"$f":"'Run Selections'!AI300","v":""},{"$f":"'Run Selections'!AA300","v":0},null,{"$f":"'Run Selections'!AL300","v":""},{"$f":"IF(D300=\"Select Model\",\"N/A\",throwCombined(F300, D300, S300, E300,J300))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D300=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K300, M300, N300, O300),0))","v":"N/A"},{"$f":"IF(D300=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K300,M300,N300,P300)),0))","v":"N/A"},{"$f":"'Run Selections'!BD300","v":0},{"$f":"IF(LEFT($D300,4)<>\"ACBC\",\"N/A\",AdjacentZone($D300,$E300,$S300,$F300,60))","v":"N/A"},{"$f":"IF(LEFT($D300,4)<>\"ACBC\",\"N/A\",AdjacentZone($D300,$E300,$S300,$F300,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F301)=\"\",\"\",'Run Selections'!F301)","v":""},null,{"$f":"'Run Selections'!T301","v":"Select Model"},{"$f":"'Run Selections'!W301","v":4},{"$f":"'Run Selections'!Y301","v":50},{"$f":"'Run Selections'!AI301","v":""},{"$f":"'Run Selections'!AA301","v":0},null,{"$f":"'Run Selections'!AL301","v":""},{"$f":"IF(D301=\"Select Model\",\"N/A\",throwCombined(F301, D301, S301, E301,J301))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D301=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K301, M301, N301, O301),0))","v":"N/A"},{"$f":"IF(D301=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K301,M301,N301,P301)),0))","v":"N/A"},{"$f":"'Run Selections'!BD301","v":0},{"$f":"IF(LEFT($D301,4)<>\"ACBC\",\"N/A\",AdjacentZone($D301,$E301,$S301,$F301,60))","v":"N/A"},{"$f":"IF(LEFT($D301,4)<>\"ACBC\",\"N/A\",AdjacentZone($D301,$E301,$S301,$F301,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F302)=\"\",\"\",'Run Selections'!F302)","v":""},null,{"$f":"'Run Selections'!T302","v":"Select Model"},{"$f":"'Run Selections'!W302","v":4},{"$f":"'Run Selections'!Y302","v":50},{"$f":"'Run Selections'!AI302","v":""},{"$f":"'Run Selections'!AA302","v":0},null,{"$f":"'Run Selections'!AL302","v":""},{"$f":"IF(D302=\"Select Model\",\"N/A\",throwCombined(F302, D302, S302, E302,J302))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D302=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K302, M302, N302, O302),0))","v":"N/A"},{"$f":"IF(D302=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K302,M302,N302,P302)),0))","v":"N/A"},{"$f":"'Run Selections'!BD302","v":0},{"$f":"IF(LEFT($D302,4)<>\"ACBC\",\"N/A\",AdjacentZone($D302,$E302,$S302,$F302,60))","v":"N/A"},{"$f":"IF(LEFT($D302,4)<>\"ACBC\",\"N/A\",AdjacentZone($D302,$E302,$S302,$F302,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F303)=\"\",\"\",'Run Selections'!F303)","v":""},null,{"$f":"'Run Selections'!T303","v":"Select Model"},{"$f":"'Run Selections'!W303","v":4},{"$f":"'Run Selections'!Y303","v":50},{"$f":"'Run Selections'!AI303","v":""},{"$f":"'Run Selections'!AA303","v":0},null,{"$f":"'Run Selections'!AL303","v":""},{"$f":"IF(D303=\"Select Model\",\"N/A\",throwCombined(F303, D303, S303, E303,J303))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D303=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K303, M303, N303, O303),0))","v":"N/A"},{"$f":"IF(D303=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K303,M303,N303,P303)),0))","v":"N/A"},{"$f":"'Run Selections'!BD303","v":0},{"$f":"IF(LEFT($D303,4)<>\"ACBC\",\"N/A\",AdjacentZone($D303,$E303,$S303,$F303,60))","v":"N/A"},{"$f":"IF(LEFT($D303,4)<>\"ACBC\",\"N/A\",AdjacentZone($D303,$E303,$S303,$F303,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F304)=\"\",\"\",'Run Selections'!F304)","v":""},null,{"$f":"'Run Selections'!T304","v":"Select Model"},{"$f":"'Run Selections'!W304","v":4},{"$f":"'Run Selections'!Y304","v":50},{"$f":"'Run Selections'!AI304","v":""},{"$f":"'Run Selections'!AA304","v":0},null,{"$f":"'Run Selections'!AL304","v":""},{"$f":"IF(D304=\"Select Model\",\"N/A\",throwCombined(F304, D304, S304, E304,J304))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D304=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K304, M304, N304, O304),0))","v":"N/A"},{"$f":"IF(D304=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K304,M304,N304,P304)),0))","v":"N/A"},{"$f":"'Run Selections'!BD304","v":0},{"$f":"IF(LEFT($D304,4)<>\"ACBC\",\"N/A\",AdjacentZone($D304,$E304,$S304,$F304,60))","v":"N/A"},{"$f":"IF(LEFT($D304,4)<>\"ACBC\",\"N/A\",AdjacentZone($D304,$E304,$S304,$F304,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F305)=\"\",\"\",'Run Selections'!F305)","v":""},null,{"$f":"'Run Selections'!T305","v":"Select Model"},{"$f":"'Run Selections'!W305","v":4},{"$f":"'Run Selections'!Y305","v":50},{"$f":"'Run Selections'!AI305","v":""},{"$f":"'Run Selections'!AA305","v":0},null,{"$f":"'Run Selections'!AL305","v":""},{"$f":"IF(D305=\"Select Model\",\"N/A\",throwCombined(F305, D305, S305, E305,J305))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D305=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K305, M305, N305, O305),0))","v":"N/A"},{"$f":"IF(D305=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K305,M305,N305,P305)),0))","v":"N/A"},{"$f":"'Run Selections'!BD305","v":0},{"$f":"IF(LEFT($D305,4)<>\"ACBC\",\"N/A\",AdjacentZone($D305,$E305,$S305,$F305,60))","v":"N/A"},{"$f":"IF(LEFT($D305,4)<>\"ACBC\",\"N/A\",AdjacentZone($D305,$E305,$S305,$F305,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F306)=\"\",\"\",'Run Selections'!F306)","v":""},null,{"$f":"'Run Selections'!T306","v":"Select Model"},{"$f":"'Run Selections'!W306","v":4},{"$f":"'Run Selections'!Y306","v":50},{"$f":"'Run Selections'!AI306","v":""},{"$f":"'Run Selections'!AA306","v":0},null,{"$f":"'Run Selections'!AL306","v":""},{"$f":"IF(D306=\"Select Model\",\"N/A\",throwCombined(F306, D306, S306, E306,J306))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D306=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K306, M306, N306, O306),0))","v":"N/A"},{"$f":"IF(D306=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K306,M306,N306,P306)),0))","v":"N/A"},{"$f":"'Run Selections'!BD306","v":0},{"$f":"IF(LEFT($D306,4)<>\"ACBC\",\"N/A\",AdjacentZone($D306,$E306,$S306,$F306,60))","v":"N/A"},{"$f":"IF(LEFT($D306,4)<>\"ACBC\",\"N/A\",AdjacentZone($D306,$E306,$S306,$F306,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F307)=\"\",\"\",'Run Selections'!F307)","v":""},null,{"$f":"'Run Selections'!T307","v":"Select Model"},{"$f":"'Run Selections'!W307","v":4},{"$f":"'Run Selections'!Y307","v":50},{"$f":"'Run Selections'!AI307","v":""},{"$f":"'Run Selections'!AA307","v":0},null,{"$f":"'Run Selections'!AL307","v":""},{"$f":"IF(D307=\"Select Model\",\"N/A\",throwCombined(F307, D307, S307, E307,J307))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D307=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K307, M307, N307, O307),0))","v":"N/A"},{"$f":"IF(D307=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K307,M307,N307,P307)),0))","v":"N/A"},{"$f":"'Run Selections'!BD307","v":0},{"$f":"IF(LEFT($D307,4)<>\"ACBC\",\"N/A\",AdjacentZone($D307,$E307,$S307,$F307,60))","v":"N/A"},{"$f":"IF(LEFT($D307,4)<>\"ACBC\",\"N/A\",AdjacentZone($D307,$E307,$S307,$F307,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F308)=\"\",\"\",'Run Selections'!F308)","v":""},null,{"$f":"'Run Selections'!T308","v":"Select Model"},{"$f":"'Run Selections'!W308","v":4},{"$f":"'Run Selections'!Y308","v":50},{"$f":"'Run Selections'!AI308","v":""},{"$f":"'Run Selections'!AA308","v":0},null,{"$f":"'Run Selections'!AL308","v":""},{"$f":"IF(D308=\"Select Model\",\"N/A\",throwCombined(F308, D308, S308, E308,J308))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D308=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K308, M308, N308, O308),0))","v":"N/A"},{"$f":"IF(D308=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K308,M308,N308,P308)),0))","v":"N/A"},{"$f":"'Run Selections'!BD308","v":0},{"$f":"IF(LEFT($D308,4)<>\"ACBC\",\"N/A\",AdjacentZone($D308,$E308,$S308,$F308,60))","v":"N/A"},{"$f":"IF(LEFT($D308,4)<>\"ACBC\",\"N/A\",AdjacentZone($D308,$E308,$S308,$F308,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F309)=\"\",\"\",'Run Selections'!F309)","v":""},null,{"$f":"'Run Selections'!T309","v":"Select Model"},{"$f":"'Run Selections'!W309","v":4},{"$f":"'Run Selections'!Y309","v":50},{"$f":"'Run Selections'!AI309","v":""},{"$f":"'Run Selections'!AA309","v":0},null,{"$f":"'Run Selections'!AL309","v":""},{"$f":"IF(D309=\"Select Model\",\"N/A\",throwCombined(F309, D309, S309, E309,J309))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D309=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K309, M309, N309, O309),0))","v":"N/A"},{"$f":"IF(D309=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K309,M309,N309,P309)),0))","v":"N/A"},{"$f":"'Run Selections'!BD309","v":0},{"$f":"IF(LEFT($D309,4)<>\"ACBC\",\"N/A\",AdjacentZone($D309,$E309,$S309,$F309,60))","v":"N/A"},{"$f":"IF(LEFT($D309,4)<>\"ACBC\",\"N/A\",AdjacentZone($D309,$E309,$S309,$F309,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F310)=\"\",\"\",'Run Selections'!F310)","v":""},null,{"$f":"'Run Selections'!T310","v":"Select Model"},{"$f":"'Run Selections'!W310","v":4},{"$f":"'Run Selections'!Y310","v":50},{"$f":"'Run Selections'!AI310","v":""},{"$f":"'Run Selections'!AA310","v":0},null,{"$f":"'Run Selections'!AL310","v":""},{"$f":"IF(D310=\"Select Model\",\"N/A\",throwCombined(F310, D310, S310, E310,J310))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D310=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K310, M310, N310, O310),0))","v":"N/A"},{"$f":"IF(D310=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K310,M310,N310,P310)),0))","v":"N/A"},{"$f":"'Run Selections'!BD310","v":0},{"$f":"IF(LEFT($D310,4)<>\"ACBC\",\"N/A\",AdjacentZone($D310,$E310,$S310,$F310,60))","v":"N/A"},{"$f":"IF(LEFT($D310,4)<>\"ACBC\",\"N/A\",AdjacentZone($D310,$E310,$S310,$F310,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F311)=\"\",\"\",'Run Selections'!F311)","v":""},null,{"$f":"'Run Selections'!T311","v":"Select Model"},{"$f":"'Run Selections'!W311","v":4},{"$f":"'Run Selections'!Y311","v":50},{"$f":"'Run Selections'!AI311","v":""},{"$f":"'Run Selections'!AA311","v":0},null,{"$f":"'Run Selections'!AL311","v":""},{"$f":"IF(D311=\"Select Model\",\"N/A\",throwCombined(F311, D311, S311, E311,J311))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D311=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K311, M311, N311, O311),0))","v":"N/A"},{"$f":"IF(D311=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K311,M311,N311,P311)),0))","v":"N/A"},{"$f":"'Run Selections'!BD311","v":0},{"$f":"IF(LEFT($D311,4)<>\"ACBC\",\"N/A\",AdjacentZone($D311,$E311,$S311,$F311,60))","v":"N/A"},{"$f":"IF(LEFT($D311,4)<>\"ACBC\",\"N/A\",AdjacentZone($D311,$E311,$S311,$F311,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F312)=\"\",\"\",'Run Selections'!F312)","v":""},null,{"$f":"'Run Selections'!T312","v":"Select Model"},{"$f":"'Run Selections'!W312","v":4},{"$f":"'Run Selections'!Y312","v":50},{"$f":"'Run Selections'!AI312","v":""},{"$f":"'Run Selections'!AA312","v":0},null,{"$f":"'Run Selections'!AL312","v":""},{"$f":"IF(D312=\"Select Model\",\"N/A\",throwCombined(F312, D312, S312, E312,J312))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D312=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K312, M312, N312, O312),0))","v":"N/A"},{"$f":"IF(D312=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K312,M312,N312,P312)),0))","v":"N/A"},{"$f":"'Run Selections'!BD312","v":0},{"$f":"IF(LEFT($D312,4)<>\"ACBC\",\"N/A\",AdjacentZone($D312,$E312,$S312,$F312,60))","v":"N/A"},{"$f":"IF(LEFT($D312,4)<>\"ACBC\",\"N/A\",AdjacentZone($D312,$E312,$S312,$F312,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F313)=\"\",\"\",'Run Selections'!F313)","v":""},null,{"$f":"'Run Selections'!T313","v":"Select Model"},{"$f":"'Run Selections'!W313","v":4},{"$f":"'Run Selections'!Y313","v":50},{"$f":"'Run Selections'!AI313","v":""},{"$f":"'Run Selections'!AA313","v":0},null,{"$f":"'Run Selections'!AL313","v":""},{"$f":"IF(D313=\"Select Model\",\"N/A\",throwCombined(F313, D313, S313, E313,J313))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D313=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K313, M313, N313, O313),0))","v":"N/A"},{"$f":"IF(D313=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K313,M313,N313,P313)),0))","v":"N/A"},{"$f":"'Run Selections'!BD313","v":0},{"$f":"IF(LEFT($D313,4)<>\"ACBC\",\"N/A\",AdjacentZone($D313,$E313,$S313,$F313,60))","v":"N/A"},{"$f":"IF(LEFT($D313,4)<>\"ACBC\",\"N/A\",AdjacentZone($D313,$E313,$S313,$F313,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F314)=\"\",\"\",'Run Selections'!F314)","v":""},null,{"$f":"'Run Selections'!T314","v":"Select Model"},{"$f":"'Run Selections'!W314","v":4},{"$f":"'Run Selections'!Y314","v":50},{"$f":"'Run Selections'!AI314","v":""},{"$f":"'Run Selections'!AA314","v":0},null,{"$f":"'Run Selections'!AL314","v":""},{"$f":"IF(D314=\"Select Model\",\"N/A\",throwCombined(F314, D314, S314, E314,J314))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D314=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K314, M314, N314, O314),0))","v":"N/A"},{"$f":"IF(D314=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K314,M314,N314,P314)),0))","v":"N/A"},{"$f":"'Run Selections'!BD314","v":0},{"$f":"IF(LEFT($D314,4)<>\"ACBC\",\"N/A\",AdjacentZone($D314,$E314,$S314,$F314,60))","v":"N/A"},{"$f":"IF(LEFT($D314,4)<>\"ACBC\",\"N/A\",AdjacentZone($D314,$E314,$S314,$F314,40))","v":"N/A"}]
[null,{"$f":"IF(TRIM('Run Selections'!F315)=\"\",\"\",'Run Selections'!F315)","v":""},null,{"$f":"'Run Selections'!T315","v":"Select Model"},{"$f":"'Run Selections'!W315","v":4},{"$f":"'Run Selections'!Y315","v":50},{"$f":"'Run Selections'!AI315","v":""},{"$f":"'Run Selections'!AA315","v":0},null,{"$f":"'Run Selections'!AL315","v":""},{"$f":"IF(D315=\"Select Model\",\"N/A\",throwCombined(F315, D315, S315, E315,J315))","v":"N/A"},null,10,3.5,7,12,{"$f":"IF(D315=\"Select Model\",\"N/A\",FormatThrowVelocity(CalculateVelocityAtPerimeter(K315, M315, N315, O315),0))","v":"N/A"},{"$f":"IF(D315=\"Select Model\",\"N/A\",FormatThrowVelocity((CalculateVelocityAtCenterAirstream(K315,M315,N315,P315)),0))","v":"N/A"},{"$f":"'Run Selections'!BD315","v":0},{"$f":"IF(LEFT($D315,4)<>\"ACBC\",\"N/A\",AdjacentZone($D315,$E315,$S315,$F315,60))","v":"N/A"},{"$f":"IF(LEFT($D315,4)<>\"ACBC\",\"N/A\",AdjacentZone($D315,$E315,$S315,$F315,40))","v":"N/A"}]

{"sheet":"Performance Schedule","index":6,"n_rows":31,"n_cols":43,"rows_kept":31,"cut":false,"hidden":true,"merged":[[19,41,19,42],[16,41,17,42],[14,41,15,42],[14,26,15,38],[14,17,15,17],[14,24,15,24],[14,23,15,23],[14,22,15,22],[14,21,15,21],[14,20,15,20],[14,19,15,19],[14,18,15,18],[16,37,19,37],[16,26,17,26],[16,39,19,39],[16,40,19,40],[18,26,19,29],[16,21,18,21],[16,22,18,22],[16,23,18,23],[16,24,18,24],[7,0,7,2],[8,0,10,2],[11,0,11,2],[16,38,19,38],[16,33,19,33],[16,34,18,34],[16,29,17,29],[16,30,19,30],[16,31,16,32],[17,31,18,31],[17,32,18,32],[16,35,19,35],[16,27,17,27],[16,28,17,28],[16,5,18,5],[16,9,18,9],[7,12,7,13],[7,14,7,15],[7,5,7,7],[8,5,8,7],[16,6,18,6],[16,7,19,7],[17,13,18,13],[17,14,18,14],[17,15,18,15],[16,10,16,12],[17,10,18,10],[17,11,18,11],[17,12,18,12],[16,13,16,15],[7,9,7,10],[8,9,8,10],[6,5,6,8],[4,5,4,7],[1,5,1,15],[2,5,2,8],[2,12,2,15],[3,14,3,15],[3,5,3,7],[6,9,6,11],[2,9,2,11],[3,9,3,10],[4,9,4,10],[6,12,6,15],[14,39,15,39],[14,40,15,40],[12,4,12,15],[16,18,18,18],[16,19,18,19],[16,20,18,20],[16,17,18,17],[14,1,15,15],[16,1,19,1],[17,8,18,8],[12,0,12,2],[14,0,19,0],[16,2,19,2],[16,36,19,36],[16,3,19,3],[16,4,18,4]]}
[null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,null,0]
[null,null,null,null,null,"Building Conditions"]
[null,null,null,null,null,"Room Conditions Cooling",null,null,null,"Primary Air Conditions Cooling",null,null,"Entering Water Cooling"]
[null,null,null,null,null,"Dry Bulb ⁰F",null,null,{"$f":"activeRoomTempCooling","v":75},"Dry Bulb ⁰F",null,{"$f":"activePriAirTempCooling","v":55},"Temperature ⁰F",null,{"$f":"'Run Selections'!$C$36","v":57}]
[null,null,null,null,null,"Relative Humidity % RH",null,null,{"$f":"activeRHCooling","v":50},"Wet Bulb ⁰F",null,{"$f":"'Run Selections'!$C$30","v":51.64519999999996},"Fluid Type",{"$f":"activeFluidTypeCooling","v":"Water"},"Percent",{"$f":"IF(N5=\"Water\",\"N/A\",activeGlycolConCooling)","v":"N/A"}]
[]
[null,null,null,null,null,"Room Conditions Heating",null,null,null,"Primary Air Conditions Heating",null,null,"Entering Water Heating"]
["Project Name",null,null,"Owner",null,"Dry Bulb ⁰F",null,null,{"$f":"activeRoomTempHeating","v":72},"Dry Bulb ⁰F",null,{"$f":"activePriAirTempHeating","v":55},"Temperature ⁰F",null,{"$f":"'Run Selections'!$D$36","v":120}]
[{"$f":"'Run Selections'!A9","v":"Project Name"},null,null,{"$f":"IF(ISBLANK(ProjectOwner),\"\",ProjectOwner)","v":"Name"},null,"Relative Humidity % RH",null,null,{"$f":"activeRHHeating","v":50},"Wet Bulb ⁰F",null,{"$f":"'Run Selections'!$D$30","v":51.64519999999996},"Fluid Type",{"$f":"activeFluidTypeHeating","v":"Water"},"Percent",{"$f":"IF(N9=\"Water\",\"N/A\",activeGlycolConHeating)","v":"N/A"}]
[null,null,null,"Revision"]
[null,null,null,{"$f":"'Run Selections'!D11","v":"001"}]
["Project Elevation (ft)",null,null,"Date"]
[{"$f":"'Run Selections'!A13","v":0},null,null,{"$f":"'Run Selections'!D13","v":"2023-09-06"},"Additional Schedule Parameters"]
[]
["Room or Zone Number/Name","Beam Performance Parameters",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Beam Configuration Parameters"]
[]
[null,"Qty","Model","Coil Type","Coil Length","Primary Air Flow","Primary Air Pressure","Nozzle\nCode","Air Inlet","Sound Level","Cooling",null,null,"Heating",null,null,null,"Latent\n(in Cooling)","Airside Capacity\n(in Cooling)","Coil Capacity","Leaving Water Temp","Airside Capacity\n(in Heating)","Coil Capacity","Leaving Water Temp","Throw \n150-100-50 \nAZ-60 : AZ-40 \n(ACBC Only)",null,"Access Blank","Return Exhaust","Air Diffuser","Slimline Coupling","Border Style Tegular/Flush or Exposed","Beam",null,"Discharge Grille or Diffuser","Intake Grille","Inlet Dampers \n(shipped loose)","Condensate Sensor (fitted)","Lint Screen","Additional Notes","Induction\nRatio","Total Discharge Air","Discharge Air Temp"]
[null,null,null,null,null,null,null,null,"Size",null,"Chilled Water","Cooling Water Pressure","Total Sensible","Hot Water","Heating Water Pressure","Total Sensible",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Total Length","Total Width"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL Series Only",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cooling","Heating"]
[null,null,null,null,"ft (nom)","CFM","in WG",null,"in","NC","GPM","ft W.G.","BTUH","GPM","ft W.G.","BTUH",null,"BTUH","BTUH","BTUH","⁰F","BTUH","BTUH","⁰F","ft",null,null,null,null,null,null,"ft (nom)","in (nom)",null,"ACBL/H",null,null,null,null,null,null,"⁰F"]
[]
[]
[]
[]
[]
[]
[]
[]
["Notes:"]
[" - Beams to have room exposed surfaces finished in standard B12 White."]
[" - Air plenums to be standard galvanized steel."]

{"sheet":"Active Configure & Quote","index":7,"n_rows":315,"n_cols":28,"rows_kept":315,"cut":false,"hidden":true,"merged":[[26,3,29,3],[23,3,24,3],[30,0,31,3],[10,27,12,27],[10,14,12,14],[10,23,12,23],[10,26,12,26],[10,25,12,25],[11,10,11,12],[10,9,11,9],[10,20,12,20],[11,0,12,3],[10,17,10,18],[11,17,12,17],[11,18,12,18],[10,8,12,8],[26,0,29,2],[32,0,32,2],[25,0,25,2],[21,0,21,2],[22,0,22,2],[23,0,24,2],[14,0,14,2],[13,0,13,2],[18,0,18,2],[19,0,20,3],[10,24,12,24],[10,13,11,13],[10,7,12,7],[9,5,12,5],[10,21,11,21],[10,15,10,16],[17,0,17,2],[10,22,12,22],[15,0,16,3],[12,9,12,12],[9,0,10,3],[9,7,9,27]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Global Configuration Options",null,null,null,null,"Room or Zone Number",null,"CONFIGURATION"]
[null,null,null,null,null,null,null,"Beam Model","Number of Beams in Zone","Coil Length","Access Blank","Return Exhaust","Air Diffuser","Slimline Coupling","Border Style Tegular/Flush or Exposed","Beam",null,"Nozzle",null,"Air Inlet","Discharge Grille or Diffuser","Intake Grille","Dampers (Shipped Loose)","2 or 4 Pipe Coil","Coil Circuit","Condensate Sensor (fitted)","Lint Screen","Additional Notes"]
["Chilled Beam Face",null,null,null,null,null,null,null,null,null,"ACBL Series Only",null,null,null,null,"Length","Width","Size","Code","Size"]
[null,null,null,null,null,null,null,null,null,"(max combined length cannot exceed 10 ft). Each option adds 12\" to overall beam length.",null,null,null,"ACBL-HE Only",null,"ft (nom)","in (nom)",null,null,"in (nom)",null,"ACBL/R"]
["Paint Color",null,null,"B12 White"]
["Pattern Controller (model specific)",null,null,"No",null,{"$f":"IF('Run Selections'!$F15=\"\",\"\",'Run Selections'!$F15)","v":""},null,{"$f":"'Run Selections'!T15","v":"Select Model"},{"$f":"'Run Selections'!L15","v":""},{"$f":"'Run Selections'!W15","v":4},"N/A","N/A","N/A","N/A","N/A",{"$f":"IF(H15=\"Select Model\",\"\",combineACBLLength(J15,K15,L15,M15,N15))","v":""},{"$f":"IF(H15=\"Select Model\",\"\",combineACBWidth('Run Selections'!X15,O15,H15))","v":""},{"$f":" 'Run Selections'!BD15","v":0},{"$f":"'Run Selections'!AI15","v":""},{"$f":"'Run Selections'!AB15","v":5},"None","N/A",null,{"$f":"'Run Selections'!U15","v":2},{"$f":"'Run Selections'!V15","v":""},null,"None (Std)"]
["Chilled Beam Plenum",null,null,null,null,{"$f":"IF('Run Selections'!$F16=\"\",\"\",'Run Selections'!$F16)","v":""},null,{"$f":"'Run Selections'!T16","v":"Select Model"},{"$f":"'Run Selections'!L16","v":""},{"$f":"'Run Selections'!W16","v":4},null,null,null,null,null,{"$f":"IF(H16=\"Select Model\",\"\",combineACBLLength(J16,K16,L16,M16,N16))","v":""},{"$f":"IF(H16=\"Select Model\",\"\",combineACBWidth('Run Selections'!X16,O16,H16))","v":""},{"$f":" 'Run Selections'!BD16","v":0},{"$f":"'Run Selections'!AI16","v":""},{"$f":"'Run Selections'!AB16","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U16","v":2},{"$f":"'Run Selections'!V16","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F17=\"\",\"\",'Run Selections'!$F17)","v":""},null,{"$f":"'Run Selections'!T17","v":"Select Model"},{"$f":"'Run Selections'!L17","v":""},{"$f":"'Run Selections'!W17","v":4},null,null,null,null,null,{"$f":"IF(H17=\"Select Model\",\"\",combineACBLLength(J17,K17,L17,M17,N17))","v":""},{"$f":"IF(H17=\"Select Model\",\"\",combineACBWidth('Run Selections'!X17,O17,H17))","v":""},{"$f":" 'Run Selections'!BD17","v":0},{"$f":"'Run Selections'!AI17","v":""},{"$f":"'Run Selections'!AB17","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U17","v":2},{"$f":"'Run Selections'!V17","v":""}]
["Galv (std) or Painted",null,null,"Galv (std)",null,{"$f":"IF('Run Selections'!$F18=\"\",\"\",'Run Selections'!$F18)","v":""},null,{"$f":"'Run Selections'!T18","v":"Select Model"},{"$f":"'Run Selections'!L18","v":""},{"$f":"'Run Selections'!W18","v":4},null,null,null,null,null,{"$f":"IF(H18=\"Select Model\",\"\",combineACBLLength(J18,K18,L18,M18,N18))","v":""},{"$f":"IF(H18=\"Select Model\",\"\",combineACBWidth('Run Selections'!X18,O18,H18))","v":""},{"$f":" 'Run Selections'!BD18","v":0},{"$f":"'Run Selections'!AI18","v":""},{"$f":"'Run Selections'!AB18","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U18","v":2},{"$f":"'Run Selections'!V18","v":""}]
["Insulation",null,null,"None",null,{"$f":"IF('Run Selections'!$F19=\"\",\"\",'Run Selections'!$F19)","v":""},null,{"$f":"'Run Selections'!T19","v":"Select Model"},{"$f":"'Run Selections'!L19","v":""},{"$f":"'Run Selections'!W19","v":4},null,null,null,null,null,{"$f":"IF(H19=\"Select Model\",\"\",combineACBLLength(J19,K19,L19,M19,N19))","v":""},{"$f":"IF(H19=\"Select Model\",\"\",combineACBWidth('Run Selections'!X19,O19,H19))","v":""},{"$f":" 'Run Selections'!BD19","v":0},{"$f":"'Run Selections'!AI19","v":""},{"$f":"'Run Selections'!AB19","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U19","v":2},{"$f":"'Run Selections'!V19","v":""}]
["Chilled Beam Coil",null,null,null,null,{"$f":"IF('Run Selections'!$F20=\"\",\"\",'Run Selections'!$F20)","v":""},null,{"$f":"'Run Selections'!T20","v":"Select Model"},{"$f":"'Run Selections'!L20","v":""},{"$f":"'Run Selections'!W20","v":4},null,null,null,null,null,{"$f":"IF(H20=\"Select Model\",\"\",combineACBLLength(J20,K20,L20,M20,N20))","v":""},{"$f":"IF(H20=\"Select Model\",\"\",combineACBWidth('Run Selections'!X20,O20,H20))","v":""},{"$f":" 'Run Selections'!BD20","v":0},{"$f":"'Run Selections'!AI20","v":""},{"$f":"'Run Selections'!AB20","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U20","v":2},{"$f":"'Run Selections'!V20","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F21=\"\",\"\",'Run Selections'!$F21)","v":""},null,{"$f":"'Run Selections'!T21","v":"Select Model"},{"$f":"'Run Selections'!L21","v":""},{"$f":"'Run Selections'!W21","v":4},null,null,null,null,null,{"$f":"IF(H21=\"Select Model\",\"\",combineACBLLength(J21,K21,L21,M21,N21))","v":""},{"$f":"IF(H21=\"Select Model\",\"\",combineACBWidth('Run Selections'!X21,O21,H21))","v":""},{"$f":" 'Run Selections'!BD21","v":0},{"$f":"'Run Selections'!AI21","v":""},{"$f":"'Run Selections'!AB21","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U21","v":2},{"$f":"'Run Selections'!V21","v":""}]
["Drain & Vent (if applicable)",null,null,"DV",null,{"$f":"IF('Run Selections'!$F22=\"\",\"\",'Run Selections'!$F22)","v":""},null,{"$f":"'Run Selections'!T22","v":"Select Model"},{"$f":"'Run Selections'!L22","v":""},{"$f":"'Run Selections'!W22","v":4},null,null,null,null,null,{"$f":"IF(H22=\"Select Model\",\"\",combineACBLLength(J22,K22,L22,M22,N22))","v":""},{"$f":"IF(H22=\"Select Model\",\"\",combineACBWidth('Run Selections'!X22,O22,H22))","v":""},{"$f":" 'Run Selections'!BD22","v":0},{"$f":"'Run Selections'!AI22","v":""},{"$f":"'Run Selections'!AB22","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U22","v":2},{"$f":"'Run Selections'!V22","v":""}]
["Painted Coil, B17 Black",null,null,"None",null,{"$f":"IF('Run Selections'!$F23=\"\",\"\",'Run Selections'!$F23)","v":""},null,{"$f":"'Run Selections'!T23","v":"Select Model"},{"$f":"'Run Selections'!L23","v":""},{"$f":"'Run Selections'!W23","v":4},null,null,null,null,null,{"$f":"IF(H23=\"Select Model\",\"\",combineACBLLength(J23,K23,L23,M23,N23))","v":""},{"$f":"IF(H23=\"Select Model\",\"\",combineACBWidth('Run Selections'!X23,O23,H23))","v":""},{"$f":" 'Run Selections'!BD23","v":0},{"$f":"'Run Selections'!AI23","v":""},{"$f":"'Run Selections'!AB23","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U23","v":2},{"$f":"'Run Selections'!V23","v":""}]
["Drain Pan? (model specific)",null,null,"No",null,{"$f":"IF('Run Selections'!$F24=\"\",\"\",'Run Selections'!$F24)","v":""},null,{"$f":"'Run Selections'!T24","v":"Select Model"},{"$f":"'Run Selections'!L24","v":""},{"$f":"'Run Selections'!W24","v":4},null,null,null,null,null,{"$f":"IF(H24=\"Select Model\",\"\",combineACBLLength(J24,K24,L24,M24,N24))","v":""},{"$f":"IF(H24=\"Select Model\",\"\",combineACBWidth('Run Selections'!X24,O24,H24))","v":""},{"$f":" 'Run Selections'!BD24","v":0},{"$f":"'Run Selections'!AI24","v":""},{"$f":"'Run Selections'!AB24","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U24","v":2},{"$f":"'Run Selections'!V24","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F25=\"\",\"\",'Run Selections'!$F25)","v":""},null,{"$f":"'Run Selections'!T25","v":"Select Model"},{"$f":"'Run Selections'!L25","v":""},{"$f":"'Run Selections'!W25","v":4},null,null,null,null,null,{"$f":"IF(H25=\"Select Model\",\"\",combineACBLLength(J25,K25,L25,M25,N25))","v":""},{"$f":"IF(H25=\"Select Model\",\"\",combineACBWidth('Run Selections'!X25,O25,H25))","v":""},{"$f":" 'Run Selections'!BD25","v":0},{"$f":"'Run Selections'!AI25","v":""},{"$f":"'Run Selections'!AB25","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U25","v":2},{"$f":"'Run Selections'!V25","v":""}]
["Sweat (Std) or NPT fittings",null,null,"1/2in Sweat (std)",null,{"$f":"IF('Run Selections'!$F26=\"\",\"\",'Run Selections'!$F26)","v":""},null,{"$f":"'Run Selections'!T26","v":"Select Model"},{"$f":"'Run Selections'!L26","v":""},{"$f":"'Run Selections'!W26","v":4.33},null,null,null,null,null,{"$f":"IF(H26=\"Select Model\",\"\",combineACBLLength(J26,K26,L26,M26,N26))","v":""},{"$f":"IF(H26=\"Select Model\",\"\",combineACBWidth('Run Selections'!X26,O26,H26))","v":""},{"$f":" 'Run Selections'!BD26","v":0},{"$f":"'Run Selections'!AI26","v":""},{"$f":"'Run Selections'!AB26","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U26","v":2},{"$f":"'Run Selections'!V26","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F27=\"\",\"\",'Run Selections'!$F27)","v":""},null,{"$f":"'Run Selections'!T27","v":"Select Model"},{"$f":"'Run Selections'!L27","v":""},{"$f":"'Run Selections'!W27","v":4},null,null,null,null,null,{"$f":"IF(H27=\"Select Model\",\"\",combineACBLLength(J27,K27,L27,M27,N27))","v":""},{"$f":"IF(H27=\"Select Model\",\"\",combineACBWidth('Run Selections'!X27,O27,H27))","v":""},{"$f":" 'Run Selections'!BD27","v":0},{"$f":"'Run Selections'!AI27","v":""},{"$f":"'Run Selections'!AB27","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U27","v":2},{"$f":"'Run Selections'!V27","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F28=\"\",\"\",'Run Selections'!$F28)","v":""},null,{"$f":"'Run Selections'!T28","v":"Select Model"},{"$f":"'Run Selections'!L28","v":""},{"$f":"'Run Selections'!W28","v":4},null,null,null,null,null,{"$f":"IF(H28=\"Select Model\",\"\",combineACBLLength(J28,K28,L28,M28,N28))","v":""},{"$f":"IF(H28=\"Select Model\",\"\",combineACBWidth('Run Selections'!X28,O28,H28))","v":""},{"$f":" 'Run Selections'!BD28","v":0},{"$f":"'Run Selections'!AI28","v":""},{"$f":"'Run Selections'!AB28","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U28","v":2},{"$f":"'Run Selections'!V28","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F29=\"\",\"\",'Run Selections'!$F29)","v":""},null,{"$f":"'Run Selections'!T29","v":"Select Model"},{"$f":"'Run Selections'!L29","v":""},{"$f":"'Run Selections'!W29","v":4},null,null,null,null,null,{"$f":"IF(H29=\"Select Model\",\"\",combineACBLLength(J29,K29,L29,M29,N29))","v":""},{"$f":"IF(H29=\"Select Model\",\"\",combineACBWidth('Run Selections'!X29,O29,H29))","v":""},{"$f":" 'Run Selections'!BD29","v":0},{"$f":"'Run Selections'!AI29","v":""},{"$f":"'Run Selections'!AB29","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U29","v":2},{"$f":"'Run Selections'!V29","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F30=\"\",\"\",'Run Selections'!$F30)","v":""},null,{"$f":"'Run Selections'!T30","v":"Select Model"},{"$f":"'Run Selections'!L30","v":""},{"$f":"'Run Selections'!W30","v":4},null,null,null,null,null,{"$f":"IF(H30=\"Select Model\",\"\",combineACBLLength(J30,K30,L30,M30,N30))","v":""},{"$f":"IF(H30=\"Select Model\",\"\",combineACBWidth('Run Selections'!X30,O30,H30))","v":""},{"$f":" 'Run Selections'!BD30","v":0},{"$f":"'Run Selections'!AI30","v":""},{"$f":"'Run Selections'!AB30","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U30","v":2},{"$f":"'Run Selections'!V30","v":""}]
["Packaging",null,null,null,null,{"$f":"IF('Run Selections'!$F31=\"\",\"\",'Run Selections'!$F31)","v":""},null,{"$f":"'Run Selections'!T31","v":"Select Model"},{"$f":"'Run Selections'!L31","v":""},{"$f":"'Run Selections'!W31","v":4},null,null,null,null,null,{"$f":"IF(H31=\"Select Model\",\"\",combineACBLLength(J31,K31,L31,M31,N31))","v":""},{"$f":"IF(H31=\"Select Model\",\"\",combineACBWidth('Run Selections'!X31,O31,H31))","v":""},{"$f":" 'Run Selections'!BD31","v":0},{"$f":"'Run Selections'!AI31","v":""},{"$f":"'Run Selections'!AB31","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U31","v":2},{"$f":"'Run Selections'!V31","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F32=\"\",\"\",'Run Selections'!$F32)","v":""},null,{"$f":"'Run Selections'!T32","v":"Select Model"},{"$f":"'Run Selections'!L32","v":""},{"$f":"'Run Selections'!W32","v":4},null,null,null,null,null,{"$f":"IF(H32=\"Select Model\",\"\",combineACBLLength(J32,K32,L32,M32,N32))","v":""},{"$f":"IF(H32=\"Select Model\",\"\",combineACBWidth('Run Selections'!X32,O32,H32))","v":""},{"$f":" 'Run Selections'!BD32","v":0},{"$f":"'Run Selections'!AI32","v":""},{"$f":"'Run Selections'!AB32","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U32","v":2},{"$f":"'Run Selections'!V32","v":""}]
["Protective Film",null,null,"Yes PF",null,{"$f":"IF('Run Selections'!$F33=\"\",\"\",'Run Selections'!$F33)","v":""},null,{"$f":"'Run Selections'!T33","v":"Select Model"},{"$f":"'Run Selections'!L33","v":""},{"$f":"'Run Selections'!W33","v":4},null,null,null,null,null,{"$f":"IF(H33=\"Select Model\",\"\",combineACBLLength(J33,K33,L33,M33,N33))","v":""},{"$f":"IF(H33=\"Select Model\",\"\",combineACBWidth('Run Selections'!X33,O33,H33))","v":""},{"$f":" 'Run Selections'!BD33","v":0},{"$f":"'Run Selections'!AI33","v":""},{"$f":"'Run Selections'!AB33","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U33","v":2},{"$f":"'Run Selections'!V33","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F34=\"\",\"\",'Run Selections'!$F34)","v":""},null,{"$f":"'Run Selections'!T34","v":"Select Model"},{"$f":"'Run Selections'!L34","v":""},{"$f":"'Run Selections'!W34","v":4},null,null,null,null,null,{"$f":"IF(H34=\"Select Model\",\"\",combineACBLLength(J34,K34,L34,M34,N34))","v":""},{"$f":"IF(H34=\"Select Model\",\"\",combineACBWidth('Run Selections'!X34,O34,H34))","v":""},{"$f":" 'Run Selections'!BD34","v":0},{"$f":"'Run Selections'!AI34","v":""},{"$f":"'Run Selections'!AB34","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U34","v":2},{"$f":"'Run Selections'!V34","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F35=\"\",\"\",'Run Selections'!$F35)","v":""},null,{"$f":"'Run Selections'!T35","v":"Select Model"},{"$f":"'Run Selections'!L35","v":""},{"$f":"'Run Selections'!W35","v":4},null,null,null,null,null,{"$f":"IF(H35=\"Select Model\",\"\",combineACBLLength(J35,K35,L35,M35,N35))","v":""},{"$f":"IF(H35=\"Select Model\",\"\",combineACBWidth('Run Selections'!X35,O35,H35))","v":""},{"$f":" 'Run Selections'!BD35","v":0},{"$f":"'Run Selections'!AI35","v":""},{"$f":"'Run Selections'!AB35","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U35","v":2},{"$f":"'Run Selections'!V35","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F36=\"\",\"\",'Run Selections'!$F36)","v":""},null,{"$f":"'Run Selections'!T36","v":"Select Model"},{"$f":"'Run Selections'!L36","v":""},{"$f":"'Run Selections'!W36","v":4},null,null,null,null,null,{"$f":"IF(H36=\"Select Model\",\"\",combineACBLLength(J36,K36,L36,M36,N36))","v":""},{"$f":"IF(H36=\"Select Model\",\"\",combineACBWidth('Run Selections'!X36,O36,H36))","v":""},{"$f":" 'Run Selections'!BD36","v":0},{"$f":"'Run Selections'!AI36","v":""},{"$f":"'Run Selections'!AB36","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U36","v":2},{"$f":"'Run Selections'!V36","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F37=\"\",\"\",'Run Selections'!$F37)","v":""},null,{"$f":"'Run Selections'!T37","v":"Select Model"},{"$f":"'Run Selections'!L37","v":""},{"$f":"'Run Selections'!W37","v":4},null,null,null,null,null,{"$f":"IF(H37=\"Select Model\",\"\",combineACBLLength(J37,K37,L37,M37,N37))","v":""},{"$f":"IF(H37=\"Select Model\",\"\",combineACBWidth('Run Selections'!X37,O37,H37))","v":""},{"$f":" 'Run Selections'!BD37","v":0},{"$f":"'Run Selections'!AI37","v":""},{"$f":"'Run Selections'!AB37","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U37","v":2},{"$f":"'Run Selections'!V37","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F38=\"\",\"\",'Run Selections'!$F38)","v":""},null,{"$f":"'Run Selections'!T38","v":"Select Model"},{"$f":"'Run Selections'!L38","v":""},{"$f":"'Run Selections'!W38","v":4},null,null,null,null,null,{"$f":"IF(H38=\"Select Model\",\"\",combineACBLLength(J38,K38,L38,M38,N38))","v":""},{"$f":"IF(H38=\"Select Model\",\"\",combineACBWidth('Run Selections'!X38,O38,H38))","v":""},{"$f":" 'Run Selections'!BD38","v":0},{"$f":"'Run Selections'!AI38","v":""},{"$f":"'Run Selections'!AB38","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U38","v":2},{"$f":"'Run Selections'!V38","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F39=\"\",\"\",'Run Selections'!$F39)","v":""},null,{"$f":"'Run Selections'!T39","v":"Select Model"},{"$f":"'Run Selections'!L39","v":""},{"$f":"'Run Selections'!W39","v":4},null,null,null,null,null,{"$f":"IF(H39=\"Select Model\",\"\",combineACBLLength(J39,K39,L39,M39,N39))","v":""},{"$f":"IF(H39=\"Select Model\",\"\",combineACBWidth('Run Selections'!X39,O39,H39))","v":""},{"$f":" 'Run Selections'!BD39","v":0},{"$f":"'Run Selections'!AI39","v":""},{"$f":"'Run Selections'!AB39","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U39","v":2},{"$f":"'Run Selections'!V39","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F40=\"\",\"\",'Run Selections'!$F40)","v":""},null,{"$f":"'Run Selections'!T40","v":"Select Model"},{"$f":"'Run Selections'!L40","v":""},{"$f":"'Run Selections'!W40","v":4},null,null,null,null,null,{"$f":"IF(H40=\"Select Model\",\"\",combineACBLLength(J40,K40,L40,M40,N40))","v":""},{"$f":"IF(H40=\"Select Model\",\"\",combineACBWidth('Run Selections'!X40,O40,H40))","v":""},{"$f":" 'Run Selections'!BD40","v":0},{"$f":"'Run Selections'!AI40","v":""},{"$f":"'Run Selections'!AB40","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U40","v":2},{"$f":"'Run Selections'!V40","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F41=\"\",\"\",'Run Selections'!$F41)","v":""},null,{"$f":"'Run Selections'!T41","v":"Select Model"},{"$f":"'Run Selections'!L41","v":""},{"$f":"'Run Selections'!W41","v":4},null,null,null,null,null,{"$f":"IF(H41=\"Select Model\",\"\",combineACBLLength(J41,K41,L41,M41,N41))","v":""},{"$f":"IF(H41=\"Select Model\",\"\",combineACBWidth('Run Selections'!X41,O41,H41))","v":""},{"$f":" 'Run Selections'!BD41","v":0},{"$f":"'Run Selections'!AI41","v":""},{"$f":"'Run Selections'!AB41","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U41","v":2},{"$f":"'Run Selections'!V41","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F42=\"\",\"\",'Run Selections'!$F42)","v":""},null,{"$f":"'Run Selections'!T42","v":"Select Model"},{"$f":"'Run Selections'!L42","v":""},{"$f":"'Run Selections'!W42","v":4},null,null,null,null,null,{"$f":"IF(H42=\"Select Model\",\"\",combineACBLLength(J42,K42,L42,M42,N42))","v":""},{"$f":"IF(H42=\"Select Model\",\"\",combineACBWidth('Run Selections'!X42,O42,H42))","v":""},{"$f":" 'Run Selections'!BD42","v":0},{"$f":"'Run Selections'!AI42","v":""},{"$f":"'Run Selections'!AB42","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U42","v":2},{"$f":"'Run Selections'!V42","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F43=\"\",\"\",'Run Selections'!$F43)","v":""},null,{"$f":"'Run Selections'!T43","v":"Select Model"},{"$f":"'Run Selections'!L43","v":""},{"$f":"'Run Selections'!W43","v":4},null,null,null,null,null,{"$f":"IF(H43=\"Select Model\",\"\",combineACBLLength(J43,K43,L43,M43,N43))","v":""},{"$f":"IF(H43=\"Select Model\",\"\",combineACBWidth('Run Selections'!X43,O43,H43))","v":""},{"$f":" 'Run Selections'!BD43","v":0},{"$f":"'Run Selections'!AI43","v":""},{"$f":"'Run Selections'!AB43","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U43","v":2},{"$f":"'Run Selections'!V43","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F44=\"\",\"\",'Run Selections'!$F44)","v":""},null,{"$f":"'Run Selections'!T44","v":"Select Model"},{"$f":"'Run Selections'!L44","v":""},{"$f":"'Run Selections'!W44","v":4},null,null,null,null,null,{"$f":"IF(H44=\"Select Model\",\"\",combineACBLLength(J44,K44,L44,M44,N44))","v":""},{"$f":"IF(H44=\"Select Model\",\"\",combineACBWidth('Run Selections'!X44,O44,H44))","v":""},{"$f":" 'Run Selections'!BD44","v":0},{"$f":"'Run Selections'!AI44","v":""},{"$f":"'Run Selections'!AB44","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U44","v":2},{"$f":"'Run Selections'!V44","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F45=\"\",\"\",'Run Selections'!$F45)","v":""},null,{"$f":"'Run Selections'!T45","v":"Select Model"},{"$f":"'Run Selections'!L45","v":""},{"$f":"'Run Selections'!W45","v":4},null,null,null,null,null,{"$f":"IF(H45=\"Select Model\",\"\",combineACBLLength(J45,K45,L45,M45,N45))","v":""},{"$f":"IF(H45=\"Select Model\",\"\",combineACBWidth('Run Selections'!X45,O45,H45))","v":""},{"$f":" 'Run Selections'!BD45","v":0},{"$f":"'Run Selections'!AI45","v":""},{"$f":"'Run Selections'!AB45","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U45","v":2},{"$f":"'Run Selections'!V45","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F46=\"\",\"\",'Run Selections'!$F46)","v":""},null,{"$f":"'Run Selections'!T46","v":"Select Model"},{"$f":"'Run Selections'!L46","v":""},{"$f":"'Run Selections'!W46","v":4},null,null,null,null,null,{"$f":"IF(H46=\"Select Model\",\"\",combineACBLLength(J46,K46,L46,M46,N46))","v":""},{"$f":"IF(H46=\"Select Model\",\"\",combineACBWidth('Run Selections'!X46,O46,H46))","v":""},{"$f":" 'Run Selections'!BD46","v":0},{"$f":"'Run Selections'!AI46","v":""},{"$f":"'Run Selections'!AB46","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U46","v":2},{"$f":"'Run Selections'!V46","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F47=\"\",\"\",'Run Selections'!$F47)","v":""},null,{"$f":"'Run Selections'!T47","v":"Select Model"},{"$f":"'Run Selections'!L47","v":""},{"$f":"'Run Selections'!W47","v":4},null,null,null,null,null,{"$f":"IF(H47=\"Select Model\",\"\",combineACBLLength(J47,K47,L47,M47,N47))","v":""},{"$f":"IF(H47=\"Select Model\",\"\",combineACBWidth('Run Selections'!X47,O47,H47))","v":""},{"$f":" 'Run Selections'!BD47","v":0},{"$f":"'Run Selections'!AI47","v":""},{"$f":"'Run Selections'!AB47","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U47","v":2},{"$f":"'Run Selections'!V47","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F48=\"\",\"\",'Run Selections'!$F48)","v":""},null,{"$f":"'Run Selections'!T48","v":"Select Model"},{"$f":"'Run Selections'!L48","v":""},{"$f":"'Run Selections'!W48","v":4},null,null,null,null,null,{"$f":"IF(H48=\"Select Model\",\"\",combineACBLLength(J48,K48,L48,M48,N48))","v":""},{"$f":"IF(H48=\"Select Model\",\"\",combineACBWidth('Run Selections'!X48,O48,H48))","v":""},{"$f":" 'Run Selections'!BD48","v":0},{"$f":"'Run Selections'!AI48","v":""},{"$f":"'Run Selections'!AB48","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U48","v":2},{"$f":"'Run Selections'!V48","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F49=\"\",\"\",'Run Selections'!$F49)","v":""},null,{"$f":"'Run Selections'!T49","v":"Select Model"},{"$f":"'Run Selections'!L49","v":""},{"$f":"'Run Selections'!W49","v":4},null,null,null,null,null,{"$f":"IF(H49=\"Select Model\",\"\",combineACBLLength(J49,K49,L49,M49,N49))","v":""},{"$f":"IF(H49=\"Select Model\",\"\",combineACBWidth('Run Selections'!X49,O49,H49))","v":""},{"$f":" 'Run Selections'!BD49","v":0},{"$f":"'Run Selections'!AI49","v":""},{"$f":"'Run Selections'!AB49","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U49","v":2},{"$f":"'Run Selections'!V49","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F50=\"\",\"\",'Run Selections'!$F50)","v":""},null,{"$f":"'Run Selections'!T50","v":"Select Model"},{"$f":"'Run Selections'!L50","v":""},{"$f":"'Run Selections'!W50","v":4},null,null,null,null,null,{"$f":"IF(H50=\"Select Model\",\"\",combineACBLLength(J50,K50,L50,M50,N50))","v":""},{"$f":"IF(H50=\"Select Model\",\"\",combineACBWidth('Run Selections'!X50,O50,H50))","v":""},{"$f":" 'Run Selections'!BD50","v":0},{"$f":"'Run Selections'!AI50","v":""},{"$f":"'Run Selections'!AB50","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U50","v":2},{"$f":"'Run Selections'!V50","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F51=\"\",\"\",'Run Selections'!$F51)","v":""},null,{"$f":"'Run Selections'!T51","v":"Select Model"},{"$f":"'Run Selections'!L51","v":""},{"$f":"'Run Selections'!W51","v":4},null,null,null,null,null,{"$f":"IF(H51=\"Select Model\",\"\",combineACBLLength(J51,K51,L51,M51,N51))","v":""},{"$f":"IF(H51=\"Select Model\",\"\",combineACBWidth('Run Selections'!X51,O51,H51))","v":""},{"$f":" 'Run Selections'!BD51","v":0},{"$f":"'Run Selections'!AI51","v":""},{"$f":"'Run Selections'!AB51","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U51","v":2},{"$f":"'Run Selections'!V51","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F52=\"\",\"\",'Run Selections'!$F52)","v":""},null,{"$f":"'Run Selections'!T52","v":"Select Model"},{"$f":"'Run Selections'!L52","v":""},{"$f":"'Run Selections'!W52","v":4},null,null,null,null,null,{"$f":"IF(H52=\"Select Model\",\"\",combineACBLLength(J52,K52,L52,M52,N52))","v":""},{"$f":"IF(H52=\"Select Model\",\"\",combineACBWidth('Run Selections'!X52,O52,H52))","v":""},{"$f":" 'Run Selections'!BD52","v":0},{"$f":"'Run Selections'!AI52","v":""},{"$f":"'Run Selections'!AB52","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U52","v":2},{"$f":"'Run Selections'!V52","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F53=\"\",\"\",'Run Selections'!$F53)","v":""},null,{"$f":"'Run Selections'!T53","v":"Select Model"},{"$f":"'Run Selections'!L53","v":""},{"$f":"'Run Selections'!W53","v":4},null,null,null,null,null,{"$f":"IF(H53=\"Select Model\",\"\",combineACBLLength(J53,K53,L53,M53,N53))","v":""},{"$f":"IF(H53=\"Select Model\",\"\",combineACBWidth('Run Selections'!X53,O53,H53))","v":""},{"$f":" 'Run Selections'!BD53","v":0},{"$f":"'Run Selections'!AI53","v":""},{"$f":"'Run Selections'!AB53","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U53","v":2},{"$f":"'Run Selections'!V53","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F54=\"\",\"\",'Run Selections'!$F54)","v":""},null,{"$f":"'Run Selections'!T54","v":"Select Model"},{"$f":"'Run Selections'!L54","v":""},{"$f":"'Run Selections'!W54","v":4},null,null,null,null,null,{"$f":"IF(H54=\"Select Model\",\"\",combineACBLLength(J54,K54,L54,M54,N54))","v":""},{"$f":"IF(H54=\"Select Model\",\"\",combineACBWidth('Run Selections'!X54,O54,H54))","v":""},{"$f":" 'Run Selections'!BD54","v":0},{"$f":"'Run Selections'!AI54","v":""},{"$f":"'Run Selections'!AB54","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U54","v":2},{"$f":"'Run Selections'!V54","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F55=\"\",\"\",'Run Selections'!$F55)","v":""},null,{"$f":"'Run Selections'!T55","v":"Select Model"},{"$f":"'Run Selections'!L55","v":""},{"$f":"'Run Selections'!W55","v":4},null,null,null,null,null,{"$f":"IF(H55=\"Select Model\",\"\",combineACBLLength(J55,K55,L55,M55,N55))","v":""},{"$f":"IF(H55=\"Select Model\",\"\",combineACBWidth('Run Selections'!X55,O55,H55))","v":""},{"$f":" 'Run Selections'!BD55","v":0},{"$f":"'Run Selections'!AI55","v":""},{"$f":"'Run Selections'!AB55","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U55","v":2},{"$f":"'Run Selections'!V55","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F56=\"\",\"\",'Run Selections'!$F56)","v":""},null,{"$f":"'Run Selections'!T56","v":"Select Model"},{"$f":"'Run Selections'!L56","v":""},{"$f":"'Run Selections'!W56","v":4},null,null,null,null,null,{"$f":"IF(H56=\"Select Model\",\"\",combineACBLLength(J56,K56,L56,M56,N56))","v":""},{"$f":"IF(H56=\"Select Model\",\"\",combineACBWidth('Run Selections'!X56,O56,H56))","v":""},{"$f":" 'Run Selections'!BD56","v":0},{"$f":"'Run Selections'!AI56","v":""},{"$f":"'Run Selections'!AB56","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U56","v":2},{"$f":"'Run Selections'!V56","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F57=\"\",\"\",'Run Selections'!$F57)","v":""},null,{"$f":"'Run Selections'!T57","v":"Select Model"},{"$f":"'Run Selections'!L57","v":""},{"$f":"'Run Selections'!W57","v":4},null,null,null,null,null,{"$f":"IF(H57=\"Select Model\",\"\",combineACBLLength(J57,K57,L57,M57,N57))","v":""},{"$f":"IF(H57=\"Select Model\",\"\",combineACBWidth('Run Selections'!X57,O57,H57))","v":""},{"$f":" 'Run Selections'!BD57","v":0},{"$f":"'Run Selections'!AI57","v":""},{"$f":"'Run Selections'!AB57","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U57","v":2},{"$f":"'Run Selections'!V57","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F58=\"\",\"\",'Run Selections'!$F58)","v":""},null,{"$f":"'Run Selections'!T58","v":"Select Model"},{"$f":"'Run Selections'!L58","v":""},{"$f":"'Run Selections'!W58","v":4},null,null,null,null,null,{"$f":"IF(H58=\"Select Model\",\"\",combineACBLLength(J58,K58,L58,M58,N58))","v":""},{"$f":"IF(H58=\"Select Model\",\"\",combineACBWidth('Run Selections'!X58,O58,H58))","v":""},{"$f":" 'Run Selections'!BD58","v":0},{"$f":"'Run Selections'!AI58","v":""},{"$f":"'Run Selections'!AB58","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U58","v":2},{"$f":"'Run Selections'!V58","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F59=\"\",\"\",'Run Selections'!$F59)","v":""},null,{"$f":"'Run Selections'!T59","v":"Select Model"},{"$f":"'Run Selections'!L59","v":""},{"$f":"'Run Selections'!W59","v":4},null,null,null,null,null,{"$f":"IF(H59=\"Select Model\",\"\",combineACBLLength(J59,K59,L59,M59,N59))","v":""},{"$f":"IF(H59=\"Select Model\",\"\",combineACBWidth('Run Selections'!X59,O59,H59))","v":""},{"$f":" 'Run Selections'!BD59","v":0},{"$f":"'Run Selections'!AI59","v":""},{"$f":"'Run Selections'!AB59","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U59","v":2},{"$f":"'Run Selections'!V59","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F60=\"\",\"\",'Run Selections'!$F60)","v":""},null,{"$f":"'Run Selections'!T60","v":"Select Model"},{"$f":"'Run Selections'!L60","v":""},{"$f":"'Run Selections'!W60","v":4},null,null,null,null,null,{"$f":"IF(H60=\"Select Model\",\"\",combineACBLLength(J60,K60,L60,M60,N60))","v":""},{"$f":"IF(H60=\"Select Model\",\"\",combineACBWidth('Run Selections'!X60,O60,H60))","v":""},{"$f":" 'Run Selections'!BD60","v":0},{"$f":"'Run Selections'!AI60","v":""},{"$f":"'Run Selections'!AB60","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U60","v":2},{"$f":"'Run Selections'!V60","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F61=\"\",\"\",'Run Selections'!$F61)","v":""},null,{"$f":"'Run Selections'!T61","v":"Select Model"},{"$f":"'Run Selections'!L61","v":""},{"$f":"'Run Selections'!W61","v":4},null,null,null,null,null,{"$f":"IF(H61=\"Select Model\",\"\",combineACBLLength(J61,K61,L61,M61,N61))","v":""},{"$f":"IF(H61=\"Select Model\",\"\",combineACBWidth('Run Selections'!X61,O61,H61))","v":""},{"$f":" 'Run Selections'!BD61","v":0},{"$f":"'Run Selections'!AI61","v":""},{"$f":"'Run Selections'!AB61","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U61","v":2},{"$f":"'Run Selections'!V61","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F62=\"\",\"\",'Run Selections'!$F62)","v":""},null,{"$f":"'Run Selections'!T62","v":"Select Model"},{"$f":"'Run Selections'!L62","v":""},{"$f":"'Run Selections'!W62","v":4},null,null,null,null,null,{"$f":"IF(H62=\"Select Model\",\"\",combineACBLLength(J62,K62,L62,M62,N62))","v":""},{"$f":"IF(H62=\"Select Model\",\"\",combineACBWidth('Run Selections'!X62,O62,H62))","v":""},{"$f":" 'Run Selections'!BD62","v":0},{"$f":"'Run Selections'!AI62","v":""},{"$f":"'Run Selections'!AB62","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U62","v":2},{"$f":"'Run Selections'!V62","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F63=\"\",\"\",'Run Selections'!$F63)","v":""},null,{"$f":"'Run Selections'!T63","v":"Select Model"},{"$f":"'Run Selections'!L63","v":""},{"$f":"'Run Selections'!W63","v":4},null,null,null,null,null,{"$f":"IF(H63=\"Select Model\",\"\",combineACBLLength(J63,K63,L63,M63,N63))","v":""},{"$f":"IF(H63=\"Select Model\",\"\",combineACBWidth('Run Selections'!X63,O63,H63))","v":""},{"$f":" 'Run Selections'!BD63","v":0},{"$f":"'Run Selections'!AI63","v":""},{"$f":"'Run Selections'!AB63","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U63","v":2},{"$f":"'Run Selections'!V63","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F64=\"\",\"\",'Run Selections'!$F64)","v":""},null,{"$f":"'Run Selections'!T64","v":"Select Model"},{"$f":"'Run Selections'!L64","v":""},{"$f":"'Run Selections'!W64","v":4},null,null,null,null,null,{"$f":"IF(H64=\"Select Model\",\"\",combineACBLLength(J64,K64,L64,M64,N64))","v":""},{"$f":"IF(H64=\"Select Model\",\"\",combineACBWidth('Run Selections'!X64,O64,H64))","v":""},{"$f":" 'Run Selections'!BD64","v":0},{"$f":"'Run Selections'!AI64","v":""},{"$f":"'Run Selections'!AB64","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U64","v":2},{"$f":"'Run Selections'!V64","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F65=\"\",\"\",'Run Selections'!$F65)","v":""},null,{"$f":"'Run Selections'!T65","v":"Select Model"},{"$f":"'Run Selections'!L65","v":""},{"$f":"'Run Selections'!W65","v":4},null,null,null,null,null,{"$f":"IF(H65=\"Select Model\",\"\",combineACBLLength(J65,K65,L65,M65,N65))","v":""},{"$f":"IF(H65=\"Select Model\",\"\",combineACBWidth('Run Selections'!X65,O65,H65))","v":""},{"$f":" 'Run Selections'!BD65","v":0},{"$f":"'Run Selections'!AI65","v":""},{"$f":"'Run Selections'!AB65","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U65","v":2},{"$f":"'Run Selections'!V65","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F66=\"\",\"\",'Run Selections'!$F66)","v":""},null,{"$f":"'Run Selections'!T66","v":"Select Model"},{"$f":"'Run Selections'!L66","v":""},{"$f":"'Run Selections'!W66","v":4},null,null,null,null,null,{"$f":"IF(H66=\"Select Model\",\"\",combineACBLLength(J66,K66,L66,M66,N66))","v":""},{"$f":"IF(H66=\"Select Model\",\"\",combineACBWidth('Run Selections'!X66,O66,H66))","v":""},{"$f":" 'Run Selections'!BD66","v":0},{"$f":"'Run Selections'!AI66","v":""},{"$f":"'Run Selections'!AB66","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U66","v":2},{"$f":"'Run Selections'!V66","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F67=\"\",\"\",'Run Selections'!$F67)","v":""},null,{"$f":"'Run Selections'!T67","v":"Select Model"},{"$f":"'Run Selections'!L67","v":""},{"$f":"'Run Selections'!W67","v":4},null,null,null,null,null,{"$f":"IF(H67=\"Select Model\",\"\",combineACBLLength(J67,K67,L67,M67,N67))","v":""},{"$f":"IF(H67=\"Select Model\",\"\",combineACBWidth('Run Selections'!X67,O67,H67))","v":""},{"$f":" 'Run Selections'!BD67","v":0},{"$f":"'Run Selections'!AI67","v":""},{"$f":"'Run Selections'!AB67","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U67","v":2},{"$f":"'Run Selections'!V67","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F68=\"\",\"\",'Run Selections'!$F68)","v":""},null,{"$f":"'Run Selections'!T68","v":"Select Model"},{"$f":"'Run Selections'!L68","v":""},{"$f":"'Run Selections'!W68","v":4},null,null,null,null,null,{"$f":"IF(H68=\"Select Model\",\"\",combineACBLLength(J68,K68,L68,M68,N68))","v":""},{"$f":"IF(H68=\"Select Model\",\"\",combineACBWidth('Run Selections'!X68,O68,H68))","v":""},{"$f":" 'Run Selections'!BD68","v":0},{"$f":"'Run Selections'!AI68","v":""},{"$f":"'Run Selections'!AB68","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U68","v":2},{"$f":"'Run Selections'!V68","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F69=\"\",\"\",'Run Selections'!$F69)","v":""},null,{"$f":"'Run Selections'!T69","v":"Select Model"},{"$f":"'Run Selections'!L69","v":""},{"$f":"'Run Selections'!W69","v":4},null,null,null,null,null,{"$f":"IF(H69=\"Select Model\",\"\",combineACBLLength(J69,K69,L69,M69,N69))","v":""},{"$f":"IF(H69=\"Select Model\",\"\",combineACBWidth('Run Selections'!X69,O69,H69))","v":""},{"$f":" 'Run Selections'!BD69","v":0},{"$f":"'Run Selections'!AI69","v":""},{"$f":"'Run Selections'!AB69","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U69","v":2},{"$f":"'Run Selections'!V69","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F70=\"\",\"\",'Run Selections'!$F70)","v":""},null,{"$f":"'Run Selections'!T70","v":"Select Model"},{"$f":"'Run Selections'!L70","v":""},{"$f":"'Run Selections'!W70","v":4},null,null,null,null,null,{"$f":"IF(H70=\"Select Model\",\"\",combineACBLLength(J70,K70,L70,M70,N70))","v":""},{"$f":"IF(H70=\"Select Model\",\"\",combineACBWidth('Run Selections'!X70,O70,H70))","v":""},{"$f":" 'Run Selections'!BD70","v":0},{"$f":"'Run Selections'!AI70","v":""},{"$f":"'Run Selections'!AB70","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U70","v":2},{"$f":"'Run Selections'!V70","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F71=\"\",\"\",'Run Selections'!$F71)","v":""},null,{"$f":"'Run Selections'!T71","v":"Select Model"},{"$f":"'Run Selections'!L71","v":""},{"$f":"'Run Selections'!W71","v":4},null,null,null,null,null,{"$f":"IF(H71=\"Select Model\",\"\",combineACBLLength(J71,K71,L71,M71,N71))","v":""},{"$f":"IF(H71=\"Select Model\",\"\",combineACBWidth('Run Selections'!X71,O71,H71))","v":""},{"$f":" 'Run Selections'!BD71","v":0},{"$f":"'Run Selections'!AI71","v":""},{"$f":"'Run Selections'!AB71","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U71","v":2},{"$f":"'Run Selections'!V71","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F72=\"\",\"\",'Run Selections'!$F72)","v":""},null,{"$f":"'Run Selections'!T72","v":"Select Model"},{"$f":"'Run Selections'!L72","v":""},{"$f":"'Run Selections'!W72","v":4},null,null,null,null,null,{"$f":"IF(H72=\"Select Model\",\"\",combineACBLLength(J72,K72,L72,M72,N72))","v":""},{"$f":"IF(H72=\"Select Model\",\"\",combineACBWidth('Run Selections'!X72,O72,H72))","v":""},{"$f":" 'Run Selections'!BD72","v":0},{"$f":"'Run Selections'!AI72","v":""},{"$f":"'Run Selections'!AB72","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U72","v":2},{"$f":"'Run Selections'!V72","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F73=\"\",\"\",'Run Selections'!$F73)","v":""},null,{"$f":"'Run Selections'!T73","v":"Select Model"},{"$f":"'Run Selections'!L73","v":""},{"$f":"'Run Selections'!W73","v":4},null,null,null,null,null,{"$f":"IF(H73=\"Select Model\",\"\",combineACBLLength(J73,K73,L73,M73,N73))","v":""},{"$f":"IF(H73=\"Select Model\",\"\",combineACBWidth('Run Selections'!X73,O73,H73))","v":""},{"$f":" 'Run Selections'!BD73","v":0},{"$f":"'Run Selections'!AI73","v":""},{"$f":"'Run Selections'!AB73","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U73","v":2},{"$f":"'Run Selections'!V73","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F74=\"\",\"\",'Run Selections'!$F74)","v":""},null,{"$f":"'Run Selections'!T74","v":"Select Model"},{"$f":"'Run Selections'!L74","v":""},{"$f":"'Run Selections'!W74","v":4},null,null,null,null,null,{"$f":"IF(H74=\"Select Model\",\"\",combineACBLLength(J74,K74,L74,M74,N74))","v":""},{"$f":"IF(H74=\"Select Model\",\"\",combineACBWidth('Run Selections'!X74,O74,H74))","v":""},{"$f":" 'Run Selections'!BD74","v":0},{"$f":"'Run Selections'!AI74","v":""},{"$f":"'Run Selections'!AB74","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U74","v":2},{"$f":"'Run Selections'!V74","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F75=\"\",\"\",'Run Selections'!$F75)","v":""},null,{"$f":"'Run Selections'!T75","v":"Select Model"},{"$f":"'Run Selections'!L75","v":""},{"$f":"'Run Selections'!W75","v":4},null,null,null,null,null,{"$f":"IF(H75=\"Select Model\",\"\",combineACBLLength(J75,K75,L75,M75,N75))","v":""},{"$f":"IF(H75=\"Select Model\",\"\",combineACBWidth('Run Selections'!X75,O75,H75))","v":""},{"$f":" 'Run Selections'!BD75","v":0},{"$f":"'Run Selections'!AI75","v":""},{"$f":"'Run Selections'!AB75","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U75","v":2},{"$f":"'Run Selections'!V75","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F76=\"\",\"\",'Run Selections'!$F76)","v":""},null,{"$f":"'Run Selections'!T76","v":"Select Model"},{"$f":"'Run Selections'!L76","v":""},{"$f":"'Run Selections'!W76","v":4},null,null,null,null,null,{"$f":"IF(H76=\"Select Model\",\"\",combineACBLLength(J76,K76,L76,M76,N76))","v":""},{"$f":"IF(H76=\"Select Model\",\"\",combineACBWidth('Run Selections'!X76,O76,H76))","v":""},{"$f":" 'Run Selections'!BD76","v":0},{"$f":"'Run Selections'!AI76","v":""},{"$f":"'Run Selections'!AB76","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U76","v":2},{"$f":"'Run Selections'!V76","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F77=\"\",\"\",'Run Selections'!$F77)","v":""},null,{"$f":"'Run Selections'!T77","v":"Select Model"},{"$f":"'Run Selections'!L77","v":""},{"$f":"'Run Selections'!W77","v":4},null,null,null,null,null,{"$f":"IF(H77=\"Select Model\",\"\",combineACBLLength(J77,K77,L77,M77,N77))","v":""},{"$f":"IF(H77=\"Select Model\",\"\",combineACBWidth('Run Selections'!X77,O77,H77))","v":""},{"$f":" 'Run Selections'!BD77","v":0},{"$f":"'Run Selections'!AI77","v":""},{"$f":"'Run Selections'!AB77","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U77","v":2},{"$f":"'Run Selections'!V77","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F78=\"\",\"\",'Run Selections'!$F78)","v":""},null,{"$f":"'Run Selections'!T78","v":"Select Model"},{"$f":"'Run Selections'!L78","v":""},{"$f":"'Run Selections'!W78","v":4},null,null,null,null,null,{"$f":"IF(H78=\"Select Model\",\"\",combineACBLLength(J78,K78,L78,M78,N78))","v":""},{"$f":"IF(H78=\"Select Model\",\"\",combineACBWidth('Run Selections'!X78,O78,H78))","v":""},{"$f":" 'Run Selections'!BD78","v":0},{"$f":"'Run Selections'!AI78","v":""},{"$f":"'Run Selections'!AB78","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U78","v":2},{"$f":"'Run Selections'!V78","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F79=\"\",\"\",'Run Selections'!$F79)","v":""},null,{"$f":"'Run Selections'!T79","v":"Select Model"},{"$f":"'Run Selections'!L79","v":""},{"$f":"'Run Selections'!W79","v":4},null,null,null,null,null,{"$f":"IF(H79=\"Select Model\",\"\",combineACBLLength(J79,K79,L79,M79,N79))","v":""},{"$f":"IF(H79=\"Select Model\",\"\",combineACBWidth('Run Selections'!X79,O79,H79))","v":""},{"$f":" 'Run Selections'!BD79","v":0},{"$f":"'Run Selections'!AI79","v":""},{"$f":"'Run Selections'!AB79","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U79","v":2},{"$f":"'Run Selections'!V79","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F80=\"\",\"\",'Run Selections'!$F80)","v":""},null,{"$f":"'Run Selections'!T80","v":"Select Model"},{"$f":"'Run Selections'!L80","v":""},{"$f":"'Run Selections'!W80","v":4},null,null,null,null,null,{"$f":"IF(H80=\"Select Model\",\"\",combineACBLLength(J80,K80,L80,M80,N80))","v":""},{"$f":"IF(H80=\"Select Model\",\"\",combineACBWidth('Run Selections'!X80,O80,H80))","v":""},{"$f":" 'Run Selections'!BD80","v":0},{"$f":"'Run Selections'!AI80","v":""},{"$f":"'Run Selections'!AB80","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U80","v":2},{"$f":"'Run Selections'!V80","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F81=\"\",\"\",'Run Selections'!$F81)","v":""},null,{"$f":"'Run Selections'!T81","v":"Select Model"},{"$f":"'Run Selections'!L81","v":""},{"$f":"'Run Selections'!W81","v":4},null,null,null,null,null,{"$f":"IF(H81=\"Select Model\",\"\",combineACBLLength(J81,K81,L81,M81,N81))","v":""},{"$f":"IF(H81=\"Select Model\",\"\",combineACBWidth('Run Selections'!X81,O81,H81))","v":""},{"$f":" 'Run Selections'!BD81","v":0},{"$f":"'Run Selections'!AI81","v":""},{"$f":"'Run Selections'!AB81","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U81","v":2},{"$f":"'Run Selections'!V81","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F82=\"\",\"\",'Run Selections'!$F82)","v":""},null,{"$f":"'Run Selections'!T82","v":"Select Model"},{"$f":"'Run Selections'!L82","v":""},{"$f":"'Run Selections'!W82","v":4},null,null,null,null,null,{"$f":"IF(H82=\"Select Model\",\"\",combineACBLLength(J82,K82,L82,M82,N82))","v":""},{"$f":"IF(H82=\"Select Model\",\"\",combineACBWidth('Run Selections'!X82,O82,H82))","v":""},{"$f":" 'Run Selections'!BD82","v":0},{"$f":"'Run Selections'!AI82","v":""},{"$f":"'Run Selections'!AB82","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U82","v":2},{"$f":"'Run Selections'!V82","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F83=\"\",\"\",'Run Selections'!$F83)","v":""},null,{"$f":"'Run Selections'!T83","v":"Select Model"},{"$f":"'Run Selections'!L83","v":""},{"$f":"'Run Selections'!W83","v":4},null,null,null,null,null,{"$f":"IF(H83=\"Select Model\",\"\",combineACBLLength(J83,K83,L83,M83,N83))","v":""},{"$f":"IF(H83=\"Select Model\",\"\",combineACBWidth('Run Selections'!X83,O83,H83))","v":""},{"$f":" 'Run Selections'!BD83","v":0},{"$f":"'Run Selections'!AI83","v":""},{"$f":"'Run Selections'!AB83","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U83","v":2},{"$f":"'Run Selections'!V83","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F84=\"\",\"\",'Run Selections'!$F84)","v":""},null,{"$f":"'Run Selections'!T84","v":"Select Model"},{"$f":"'Run Selections'!L84","v":""},{"$f":"'Run Selections'!W84","v":4},null,null,null,null,null,{"$f":"IF(H84=\"Select Model\",\"\",combineACBLLength(J84,K84,L84,M84,N84))","v":""},{"$f":"IF(H84=\"Select Model\",\"\",combineACBWidth('Run Selections'!X84,O84,H84))","v":""},{"$f":" 'Run Selections'!BD84","v":0},{"$f":"'Run Selections'!AI84","v":""},{"$f":"'Run Selections'!AB84","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U84","v":2},{"$f":"'Run Selections'!V84","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F85=\"\",\"\",'Run Selections'!$F85)","v":""},null,{"$f":"'Run Selections'!T85","v":"Select Model"},{"$f":"'Run Selections'!L85","v":""},{"$f":"'Run Selections'!W85","v":4},null,null,null,null,null,{"$f":"IF(H85=\"Select Model\",\"\",combineACBLLength(J85,K85,L85,M85,N85))","v":""},{"$f":"IF(H85=\"Select Model\",\"\",combineACBWidth('Run Selections'!X85,O85,H85))","v":""},{"$f":" 'Run Selections'!BD85","v":0},{"$f":"'Run Selections'!AI85","v":""},{"$f":"'Run Selections'!AB85","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U85","v":2},{"$f":"'Run Selections'!V85","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F86=\"\",\"\",'Run Selections'!$F86)","v":""},null,{"$f":"'Run Selections'!T86","v":"Select Model"},{"$f":"'Run Selections'!L86","v":""},{"$f":"'Run Selections'!W86","v":4},null,null,null,null,null,{"$f":"IF(H86=\"Select Model\",\"\",combineACBLLength(J86,K86,L86,M86,N86))","v":""},{"$f":"IF(H86=\"Select Model\",\"\",combineACBWidth('Run Selections'!X86,O86,H86))","v":""},{"$f":" 'Run Selections'!BD86","v":0},{"$f":"'Run Selections'!AI86","v":""},{"$f":"'Run Selections'!AB86","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U86","v":2},{"$f":"'Run Selections'!V86","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F87=\"\",\"\",'Run Selections'!$F87)","v":""},null,{"$f":"'Run Selections'!T87","v":"Select Model"},{"$f":"'Run Selections'!L87","v":""},{"$f":"'Run Selections'!W87","v":4},null,null,null,null,null,{"$f":"IF(H87=\"Select Model\",\"\",combineACBLLength(J87,K87,L87,M87,N87))","v":""},{"$f":"IF(H87=\"Select Model\",\"\",combineACBWidth('Run Selections'!X87,O87,H87))","v":""},{"$f":" 'Run Selections'!BD87","v":0},{"$f":"'Run Selections'!AI87","v":""},{"$f":"'Run Selections'!AB87","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U87","v":2},{"$f":"'Run Selections'!V87","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F88=\"\",\"\",'Run Selections'!$F88)","v":""},null,{"$f":"'Run Selections'!T88","v":"Select Model"},{"$f":"'Run Selections'!L88","v":""},{"$f":"'Run Selections'!W88","v":4},null,null,null,null,null,{"$f":"IF(H88=\"Select Model\",\"\",combineACBLLength(J88,K88,L88,M88,N88))","v":""},{"$f":"IF(H88=\"Select Model\",\"\",combineACBWidth('Run Selections'!X88,O88,H88))","v":""},{"$f":" 'Run Selections'!BD88","v":0},{"$f":"'Run Selections'!AI88","v":""},{"$f":"'Run Selections'!AB88","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U88","v":2},{"$f":"'Run Selections'!V88","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F89=\"\",\"\",'Run Selections'!$F89)","v":""},null,{"$f":"'Run Selections'!T89","v":"Select Model"},{"$f":"'Run Selections'!L89","v":""},{"$f":"'Run Selections'!W89","v":4},null,null,null,null,null,{"$f":"IF(H89=\"Select Model\",\"\",combineACBLLength(J89,K89,L89,M89,N89))","v":""},{"$f":"IF(H89=\"Select Model\",\"\",combineACBWidth('Run Selections'!X89,O89,H89))","v":""},{"$f":" 'Run Selections'!BD89","v":0},{"$f":"'Run Selections'!AI89","v":""},{"$f":"'Run Selections'!AB89","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U89","v":2},{"$f":"'Run Selections'!V89","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F90=\"\",\"\",'Run Selections'!$F90)","v":""},null,{"$f":"'Run Selections'!T90","v":"Select Model"},{"$f":"'Run Selections'!L90","v":""},{"$f":"'Run Selections'!W90","v":4},null,null,null,null,null,{"$f":"IF(H90=\"Select Model\",\"\",combineACBLLength(J90,K90,L90,M90,N90))","v":""},{"$f":"IF(H90=\"Select Model\",\"\",combineACBWidth('Run Selections'!X90,O90,H90))","v":""},{"$f":" 'Run Selections'!BD90","v":0},{"$f":"'Run Selections'!AI90","v":""},{"$f":"'Run Selections'!AB90","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U90","v":2},{"$f":"'Run Selections'!V90","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F91=\"\",\"\",'Run Selections'!$F91)","v":""},null,{"$f":"'Run Selections'!T91","v":"Select Model"},{"$f":"'Run Selections'!L91","v":""},{"$f":"'Run Selections'!W91","v":4},null,null,null,null,null,{"$f":"IF(H91=\"Select Model\",\"\",combineACBLLength(J91,K91,L91,M91,N91))","v":""},{"$f":"IF(H91=\"Select Model\",\"\",combineACBWidth('Run Selections'!X91,O91,H91))","v":""},{"$f":" 'Run Selections'!BD91","v":0},{"$f":"'Run Selections'!AI91","v":""},{"$f":"'Run Selections'!AB91","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U91","v":2},{"$f":"'Run Selections'!V91","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F92=\"\",\"\",'Run Selections'!$F92)","v":""},null,{"$f":"'Run Selections'!T92","v":"Select Model"},{"$f":"'Run Selections'!L92","v":""},{"$f":"'Run Selections'!W92","v":4},null,null,null,null,null,{"$f":"IF(H92=\"Select Model\",\"\",combineACBLLength(J92,K92,L92,M92,N92))","v":""},{"$f":"IF(H92=\"Select Model\",\"\",combineACBWidth('Run Selections'!X92,O92,H92))","v":""},{"$f":" 'Run Selections'!BD92","v":0},{"$f":"'Run Selections'!AI92","v":""},{"$f":"'Run Selections'!AB92","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U92","v":2},{"$f":"'Run Selections'!V92","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F93=\"\",\"\",'Run Selections'!$F93)","v":""},null,{"$f":"'Run Selections'!T93","v":"Select Model"},{"$f":"'Run Selections'!L93","v":""},{"$f":"'Run Selections'!W93","v":4},null,null,null,null,null,{"$f":"IF(H93=\"Select Model\",\"\",combineACBLLength(J93,K93,L93,M93,N93))","v":""},{"$f":"IF(H93=\"Select Model\",\"\",combineACBWidth('Run Selections'!X93,O93,H93))","v":""},{"$f":" 'Run Selections'!BD93","v":0},{"$f":"'Run Selections'!AI93","v":""},{"$f":"'Run Selections'!AB93","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U93","v":2},{"$f":"'Run Selections'!V93","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F94=\"\",\"\",'Run Selections'!$F94)","v":""},null,{"$f":"'Run Selections'!T94","v":"Select Model"},{"$f":"'Run Selections'!L94","v":""},{"$f":"'Run Selections'!W94","v":4},null,null,null,null,null,{"$f":"IF(H94=\"Select Model\",\"\",combineACBLLength(J94,K94,L94,M94,N94))","v":""},{"$f":"IF(H94=\"Select Model\",\"\",combineACBWidth('Run Selections'!X94,O94,H94))","v":""},{"$f":" 'Run Selections'!BD94","v":0},{"$f":"'Run Selections'!AI94","v":""},{"$f":"'Run Selections'!AB94","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U94","v":2},{"$f":"'Run Selections'!V94","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F95=\"\",\"\",'Run Selections'!$F95)","v":""},null,{"$f":"'Run Selections'!T95","v":"Select Model"},{"$f":"'Run Selections'!L95","v":""},{"$f":"'Run Selections'!W95","v":4},null,null,null,null,null,{"$f":"IF(H95=\"Select Model\",\"\",combineACBLLength(J95,K95,L95,M95,N95))","v":""},{"$f":"IF(H95=\"Select Model\",\"\",combineACBWidth('Run Selections'!X95,O95,H95))","v":""},{"$f":" 'Run Selections'!BD95","v":0},{"$f":"'Run Selections'!AI95","v":""},{"$f":"'Run Selections'!AB95","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U95","v":2},{"$f":"'Run Selections'!V95","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F96=\"\",\"\",'Run Selections'!$F96)","v":""},null,{"$f":"'Run Selections'!T96","v":"Select Model"},{"$f":"'Run Selections'!L96","v":""},{"$f":"'Run Selections'!W96","v":4},null,null,null,null,null,{"$f":"IF(H96=\"Select Model\",\"\",combineACBLLength(J96,K96,L96,M96,N96))","v":""},{"$f":"IF(H96=\"Select Model\",\"\",combineACBWidth('Run Selections'!X96,O96,H96))","v":""},{"$f":" 'Run Selections'!BD96","v":0},{"$f":"'Run Selections'!AI96","v":""},{"$f":"'Run Selections'!AB96","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U96","v":2},{"$f":"'Run Selections'!V96","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F97=\"\",\"\",'Run Selections'!$F97)","v":""},null,{"$f":"'Run Selections'!T97","v":"Select Model"},{"$f":"'Run Selections'!L97","v":""},{"$f":"'Run Selections'!W97","v":4},null,null,null,null,null,{"$f":"IF(H97=\"Select Model\",\"\",combineACBLLength(J97,K97,L97,M97,N97))","v":""},{"$f":"IF(H97=\"Select Model\",\"\",combineACBWidth('Run Selections'!X97,O97,H97))","v":""},{"$f":" 'Run Selections'!BD97","v":0},{"$f":"'Run Selections'!AI97","v":""},{"$f":"'Run Selections'!AB97","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U97","v":2},{"$f":"'Run Selections'!V97","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F98=\"\",\"\",'Run Selections'!$F98)","v":""},null,{"$f":"'Run Selections'!T98","v":"Select Model"},{"$f":"'Run Selections'!L98","v":""},{"$f":"'Run Selections'!W98","v":4},null,null,null,null,null,{"$f":"IF(H98=\"Select Model\",\"\",combineACBLLength(J98,K98,L98,M98,N98))","v":""},{"$f":"IF(H98=\"Select Model\",\"\",combineACBWidth('Run Selections'!X98,O98,H98))","v":""},{"$f":" 'Run Selections'!BD98","v":0},{"$f":"'Run Selections'!AI98","v":""},{"$f":"'Run Selections'!AB98","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U98","v":2},{"$f":"'Run Selections'!V98","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F99=\"\",\"\",'Run Selections'!$F99)","v":""},null,{"$f":"'Run Selections'!T99","v":"Select Model"},{"$f":"'Run Selections'!L99","v":""},{"$f":"'Run Selections'!W99","v":4},null,null,null,null,null,{"$f":"IF(H99=\"Select Model\",\"\",combineACBLLength(J99,K99,L99,M99,N99))","v":""},{"$f":"IF(H99=\"Select Model\",\"\",combineACBWidth('Run Selections'!X99,O99,H99))","v":""},{"$f":" 'Run Selections'!BD99","v":0},{"$f":"'Run Selections'!AI99","v":""},{"$f":"'Run Selections'!AB99","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U99","v":2},{"$f":"'Run Selections'!V99","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F100=\"\",\"\",'Run Selections'!$F100)","v":""},null,{"$f":"'Run Selections'!T100","v":"Select Model"},{"$f":"'Run Selections'!L100","v":""},{"$f":"'Run Selections'!W100","v":4},null,null,null,null,null,{"$f":"IF(H100=\"Select Model\",\"\",combineACBLLength(J100,K100,L100,M100,N100))","v":""},{"$f":"IF(H100=\"Select Model\",\"\",combineACBWidth('Run Selections'!X100,O100,H100))","v":""},{"$f":" 'Run Selections'!BD100","v":0},{"$f":"'Run Selections'!AI100","v":""},{"$f":"'Run Selections'!AB100","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U100","v":2},{"$f":"'Run Selections'!V100","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F101=\"\",\"\",'Run Selections'!$F101)","v":""},null,{"$f":"'Run Selections'!T101","v":"Select Model"},{"$f":"'Run Selections'!L101","v":""},{"$f":"'Run Selections'!W101","v":4},null,null,null,null,null,{"$f":"IF(H101=\"Select Model\",\"\",combineACBLLength(J101,K101,L101,M101,N101))","v":""},{"$f":"IF(H101=\"Select Model\",\"\",combineACBWidth('Run Selections'!X101,O101,H101))","v":""},{"$f":" 'Run Selections'!BD101","v":0},{"$f":"'Run Selections'!AI101","v":""},{"$f":"'Run Selections'!AB101","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U101","v":2},{"$f":"'Run Selections'!V101","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F102=\"\",\"\",'Run Selections'!$F102)","v":""},null,{"$f":"'Run Selections'!T102","v":"Select Model"},{"$f":"'Run Selections'!L102","v":""},{"$f":"'Run Selections'!W102","v":4},null,null,null,null,null,{"$f":"IF(H102=\"Select Model\",\"\",combineACBLLength(J102,K102,L102,M102,N102))","v":""},{"$f":"IF(H102=\"Select Model\",\"\",combineACBWidth('Run Selections'!X102,O102,H102))","v":""},{"$f":" 'Run Selections'!BD102","v":0},{"$f":"'Run Selections'!AI102","v":""},{"$f":"'Run Selections'!AB102","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U102","v":2},{"$f":"'Run Selections'!V102","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F103=\"\",\"\",'Run Selections'!$F103)","v":""},null,{"$f":"'Run Selections'!T103","v":"Select Model"},{"$f":"'Run Selections'!L103","v":""},{"$f":"'Run Selections'!W103","v":4},null,null,null,null,null,{"$f":"IF(H103=\"Select Model\",\"\",combineACBLLength(J103,K103,L103,M103,N103))","v":""},{"$f":"IF(H103=\"Select Model\",\"\",combineACBWidth('Run Selections'!X103,O103,H103))","v":""},{"$f":" 'Run Selections'!BD103","v":0},{"$f":"'Run Selections'!AI103","v":""},{"$f":"'Run Selections'!AB103","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U103","v":2},{"$f":"'Run Selections'!V103","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F104=\"\",\"\",'Run Selections'!$F104)","v":""},null,{"$f":"'Run Selections'!T104","v":"Select Model"},{"$f":"'Run Selections'!L104","v":""},{"$f":"'Run Selections'!W104","v":4},null,null,null,null,null,{"$f":"IF(H104=\"Select Model\",\"\",combineACBLLength(J104,K104,L104,M104,N104))","v":""},{"$f":"IF(H104=\"Select Model\",\"\",combineACBWidth('Run Selections'!X104,O104,H104))","v":""},{"$f":" 'Run Selections'!BD104","v":0},{"$f":"'Run Selections'!AI104","v":""},{"$f":"'Run Selections'!AB104","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U104","v":2},{"$f":"'Run Selections'!V104","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F105=\"\",\"\",'Run Selections'!$F105)","v":""},null,{"$f":"'Run Selections'!T105","v":"Select Model"},{"$f":"'Run Selections'!L105","v":""},{"$f":"'Run Selections'!W105","v":4},null,null,null,null,null,{"$f":"IF(H105=\"Select Model\",\"\",combineACBLLength(J105,K105,L105,M105,N105))","v":""},{"$f":"IF(H105=\"Select Model\",\"\",combineACBWidth('Run Selections'!X105,O105,H105))","v":""},{"$f":" 'Run Selections'!BD105","v":0},{"$f":"'Run Selections'!AI105","v":""},{"$f":"'Run Selections'!AB105","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U105","v":2},{"$f":"'Run Selections'!V105","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F106=\"\",\"\",'Run Selections'!$F106)","v":""},null,{"$f":"'Run Selections'!T106","v":"Select Model"},{"$f":"'Run Selections'!L106","v":""},{"$f":"'Run Selections'!W106","v":4},null,null,null,null,null,{"$f":"IF(H106=\"Select Model\",\"\",combineACBLLength(J106,K106,L106,M106,N106))","v":""},{"$f":"IF(H106=\"Select Model\",\"\",combineACBWidth('Run Selections'!X106,O106,H106))","v":""},{"$f":" 'Run Selections'!BD106","v":0},{"$f":"'Run Selections'!AI106","v":""},{"$f":"'Run Selections'!AB106","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U106","v":2},{"$f":"'Run Selections'!V106","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F107=\"\",\"\",'Run Selections'!$F107)","v":""},null,{"$f":"'Run Selections'!T107","v":"Select Model"},{"$f":"'Run Selections'!L107","v":""},{"$f":"'Run Selections'!W107","v":4},null,null,null,null,null,{"$f":"IF(H107=\"Select Model\",\"\",combineACBLLength(J107,K107,L107,M107,N107))","v":""},{"$f":"IF(H107=\"Select Model\",\"\",combineACBWidth('Run Selections'!X107,O107,H107))","v":""},{"$f":" 'Run Selections'!BD107","v":0},{"$f":"'Run Selections'!AI107","v":""},{"$f":"'Run Selections'!AB107","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U107","v":2},{"$f":"'Run Selections'!V107","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F108=\"\",\"\",'Run Selections'!$F108)","v":""},null,{"$f":"'Run Selections'!T108","v":"Select Model"},{"$f":"'Run Selections'!L108","v":""},{"$f":"'Run Selections'!W108","v":4},null,null,null,null,null,{"$f":"IF(H108=\"Select Model\",\"\",combineACBLLength(J108,K108,L108,M108,N108))","v":""},{"$f":"IF(H108=\"Select Model\",\"\",combineACBWidth('Run Selections'!X108,O108,H108))","v":""},{"$f":" 'Run Selections'!BD108","v":0},{"$f":"'Run Selections'!AI108","v":""},{"$f":"'Run Selections'!AB108","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U108","v":2},{"$f":"'Run Selections'!V108","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F109=\"\",\"\",'Run Selections'!$F109)","v":""},null,{"$f":"'Run Selections'!T109","v":"Select Model"},{"$f":"'Run Selections'!L109","v":""},{"$f":"'Run Selections'!W109","v":4},null,null,null,null,null,{"$f":"IF(H109=\"Select Model\",\"\",combineACBLLength(J109,K109,L109,M109,N109))","v":""},{"$f":"IF(H109=\"Select Model\",\"\",combineACBWidth('Run Selections'!X109,O109,H109))","v":""},{"$f":" 'Run Selections'!BD109","v":0},{"$f":"'Run Selections'!AI109","v":""},{"$f":"'Run Selections'!AB109","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U109","v":2},{"$f":"'Run Selections'!V109","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F110=\"\",\"\",'Run Selections'!$F110)","v":""},null,{"$f":"'Run Selections'!T110","v":"Select Model"},{"$f":"'Run Selections'!L110","v":""},{"$f":"'Run Selections'!W110","v":4},null,null,null,null,null,{"$f":"IF(H110=\"Select Model\",\"\",combineACBLLength(J110,K110,L110,M110,N110))","v":""},{"$f":"IF(H110=\"Select Model\",\"\",combineACBWidth('Run Selections'!X110,O110,H110))","v":""},{"$f":" 'Run Selections'!BD110","v":0},{"$f":"'Run Selections'!AI110","v":""},{"$f":"'Run Selections'!AB110","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U110","v":2},{"$f":"'Run Selections'!V110","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F111=\"\",\"\",'Run Selections'!$F111)","v":""},null,{"$f":"'Run Selections'!T111","v":"Select Model"},{"$f":"'Run Selections'!L111","v":""},{"$f":"'Run Selections'!W111","v":4},null,null,null,null,null,{"$f":"IF(H111=\"Select Model\",\"\",combineACBLLength(J111,K111,L111,M111,N111))","v":""},{"$f":"IF(H111=\"Select Model\",\"\",combineACBWidth('Run Selections'!X111,O111,H111))","v":""},{"$f":" 'Run Selections'!BD111","v":0},{"$f":"'Run Selections'!AI111","v":""},{"$f":"'Run Selections'!AB111","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U111","v":2},{"$f":"'Run Selections'!V111","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F112=\"\",\"\",'Run Selections'!$F112)","v":""},null,{"$f":"'Run Selections'!T112","v":"Select Model"},{"$f":"'Run Selections'!L112","v":""},{"$f":"'Run Selections'!W112","v":4},null,null,null,null,null,{"$f":"IF(H112=\"Select Model\",\"\",combineACBLLength(J112,K112,L112,M112,N112))","v":""},{"$f":"IF(H112=\"Select Model\",\"\",combineACBWidth('Run Selections'!X112,O112,H112))","v":""},{"$f":" 'Run Selections'!BD112","v":0},{"$f":"'Run Selections'!AI112","v":""},{"$f":"'Run Selections'!AB112","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U112","v":2},{"$f":"'Run Selections'!V112","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F113=\"\",\"\",'Run Selections'!$F113)","v":""},null,{"$f":"'Run Selections'!T113","v":"Select Model"},{"$f":"'Run Selections'!L113","v":""},{"$f":"'Run Selections'!W113","v":4},null,null,null,null,null,{"$f":"IF(H113=\"Select Model\",\"\",combineACBLLength(J113,K113,L113,M113,N113))","v":""},{"$f":"IF(H113=\"Select Model\",\"\",combineACBWidth('Run Selections'!X113,O113,H113))","v":""},{"$f":" 'Run Selections'!BD113","v":0},{"$f":"'Run Selections'!AI113","v":""},{"$f":"'Run Selections'!AB113","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U113","v":2},{"$f":"'Run Selections'!V113","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F114=\"\",\"\",'Run Selections'!$F114)","v":""},null,{"$f":"'Run Selections'!T114","v":"Select Model"},{"$f":"'Run Selections'!L114","v":""},{"$f":"'Run Selections'!W114","v":4},null,null,null,null,null,{"$f":"IF(H114=\"Select Model\",\"\",combineACBLLength(J114,K114,L114,M114,N114))","v":""},{"$f":"IF(H114=\"Select Model\",\"\",combineACBWidth('Run Selections'!X114,O114,H114))","v":""},{"$f":" 'Run Selections'!BD114","v":0},{"$f":"'Run Selections'!AI114","v":""},{"$f":"'Run Selections'!AB114","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U114","v":2},{"$f":"'Run Selections'!V114","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F115=\"\",\"\",'Run Selections'!$F115)","v":""},null,{"$f":"'Run Selections'!T115","v":"Select Model"},{"$f":"'Run Selections'!L115","v":""},{"$f":"'Run Selections'!W115","v":4},null,null,null,null,null,{"$f":"IF(H115=\"Select Model\",\"\",combineACBLLength(J115,K115,L115,M115,N115))","v":""},{"$f":"IF(H115=\"Select Model\",\"\",combineACBWidth('Run Selections'!X115,O115,H115))","v":""},{"$f":" 'Run Selections'!BD115","v":0},{"$f":"'Run Selections'!AI115","v":""},{"$f":"'Run Selections'!AB115","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U115","v":2},{"$f":"'Run Selections'!V115","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F116=\"\",\"\",'Run Selections'!$F116)","v":""},null,{"$f":"'Run Selections'!T116","v":"Select Model"},{"$f":"'Run Selections'!L116","v":""},{"$f":"'Run Selections'!W116","v":4},null,null,null,null,null,{"$f":"IF(H116=\"Select Model\",\"\",combineACBLLength(J116,K116,L116,M116,N116))","v":""},{"$f":"IF(H116=\"Select Model\",\"\",combineACBWidth('Run Selections'!X116,O116,H116))","v":""},{"$f":" 'Run Selections'!BD116","v":0},{"$f":"'Run Selections'!AI116","v":""},{"$f":"'Run Selections'!AB116","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U116","v":2},{"$f":"'Run Selections'!V116","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F117=\"\",\"\",'Run Selections'!$F117)","v":""},null,{"$f":"'Run Selections'!T117","v":"Select Model"},{"$f":"'Run Selections'!L117","v":""},{"$f":"'Run Selections'!W117","v":4},null,null,null,null,null,{"$f":"IF(H117=\"Select Model\",\"\",combineACBLLength(J117,K117,L117,M117,N117))","v":""},{"$f":"IF(H117=\"Select Model\",\"\",combineACBWidth('Run Selections'!X117,O117,H117))","v":""},{"$f":" 'Run Selections'!BD117","v":0},{"$f":"'Run Selections'!AI117","v":""},{"$f":"'Run Selections'!AB117","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U117","v":2},{"$f":"'Run Selections'!V117","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F118=\"\",\"\",'Run Selections'!$F118)","v":""},null,{"$f":"'Run Selections'!T118","v":"Select Model"},{"$f":"'Run Selections'!L118","v":""},{"$f":"'Run Selections'!W118","v":4},null,null,null,null,null,{"$f":"IF(H118=\"Select Model\",\"\",combineACBLLength(J118,K118,L118,M118,N118))","v":""},{"$f":"IF(H118=\"Select Model\",\"\",combineACBWidth('Run Selections'!X118,O118,H118))","v":""},{"$f":" 'Run Selections'!BD118","v":0},{"$f":"'Run Selections'!AI118","v":""},{"$f":"'Run Selections'!AB118","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U118","v":2},{"$f":"'Run Selections'!V118","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F119=\"\",\"\",'Run Selections'!$F119)","v":""},null,{"$f":"'Run Selections'!T119","v":"Select Model"},{"$f":"'Run Selections'!L119","v":""},{"$f":"'Run Selections'!W119","v":4},null,null,null,null,null,{"$f":"IF(H119=\"Select Model\",\"\",combineACBLLength(J119,K119,L119,M119,N119))","v":""},{"$f":"IF(H119=\"Select Model\",\"\",combineACBWidth('Run Selections'!X119,O119,H119))","v":""},{"$f":" 'Run Selections'!BD119","v":0},{"$f":"'Run Selections'!AI119","v":""},{"$f":"'Run Selections'!AB119","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U119","v":2},{"$f":"'Run Selections'!V119","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F120=\"\",\"\",'Run Selections'!$F120)","v":""},null,{"$f":"'Run Selections'!T120","v":"Select Model"},{"$f":"'Run Selections'!L120","v":""},{"$f":"'Run Selections'!W120","v":4},null,null,null,null,null,{"$f":"IF(H120=\"Select Model\",\"\",combineACBLLength(J120,K120,L120,M120,N120))","v":""},{"$f":"IF(H120=\"Select Model\",\"\",combineACBWidth('Run Selections'!X120,O120,H120))","v":""},{"$f":" 'Run Selections'!BD120","v":0},{"$f":"'Run Selections'!AI120","v":""},{"$f":"'Run Selections'!AB120","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U120","v":2},{"$f":"'Run Selections'!V120","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F121=\"\",\"\",'Run Selections'!$F121)","v":""},null,{"$f":"'Run Selections'!T121","v":"Select Model"},{"$f":"'Run Selections'!L121","v":""},{"$f":"'Run Selections'!W121","v":4},null,null,null,null,null,{"$f":"IF(H121=\"Select Model\",\"\",combineACBLLength(J121,K121,L121,M121,N121))","v":""},{"$f":"IF(H121=\"Select Model\",\"\",combineACBWidth('Run Selections'!X121,O121,H121))","v":""},{"$f":" 'Run Selections'!BD121","v":0},{"$f":"'Run Selections'!AI121","v":""},{"$f":"'Run Selections'!AB121","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U121","v":2},{"$f":"'Run Selections'!V121","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F122=\"\",\"\",'Run Selections'!$F122)","v":""},null,{"$f":"'Run Selections'!T122","v":"Select Model"},{"$f":"'Run Selections'!L122","v":""},{"$f":"'Run Selections'!W122","v":4},null,null,null,null,null,{"$f":"IF(H122=\"Select Model\",\"\",combineACBLLength(J122,K122,L122,M122,N122))","v":""},{"$f":"IF(H122=\"Select Model\",\"\",combineACBWidth('Run Selections'!X122,O122,H122))","v":""},{"$f":" 'Run Selections'!BD122","v":0},{"$f":"'Run Selections'!AI122","v":""},{"$f":"'Run Selections'!AB122","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U122","v":2},{"$f":"'Run Selections'!V122","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F123=\"\",\"\",'Run Selections'!$F123)","v":""},null,{"$f":"'Run Selections'!T123","v":"Select Model"},{"$f":"'Run Selections'!L123","v":""},{"$f":"'Run Selections'!W123","v":4},null,null,null,null,null,{"$f":"IF(H123=\"Select Model\",\"\",combineACBLLength(J123,K123,L123,M123,N123))","v":""},{"$f":"IF(H123=\"Select Model\",\"\",combineACBWidth('Run Selections'!X123,O123,H123))","v":""},{"$f":" 'Run Selections'!BD123","v":0},{"$f":"'Run Selections'!AI123","v":""},{"$f":"'Run Selections'!AB123","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U123","v":2},{"$f":"'Run Selections'!V123","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F124=\"\",\"\",'Run Selections'!$F124)","v":""},null,{"$f":"'Run Selections'!T124","v":"Select Model"},{"$f":"'Run Selections'!L124","v":""},{"$f":"'Run Selections'!W124","v":4},null,null,null,null,null,{"$f":"IF(H124=\"Select Model\",\"\",combineACBLLength(J124,K124,L124,M124,N124))","v":""},{"$f":"IF(H124=\"Select Model\",\"\",combineACBWidth('Run Selections'!X124,O124,H124))","v":""},{"$f":" 'Run Selections'!BD124","v":0},{"$f":"'Run Selections'!AI124","v":""},{"$f":"'Run Selections'!AB124","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U124","v":2},{"$f":"'Run Selections'!V124","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F125=\"\",\"\",'Run Selections'!$F125)","v":""},null,{"$f":"'Run Selections'!T125","v":"Select Model"},{"$f":"'Run Selections'!L125","v":""},{"$f":"'Run Selections'!W125","v":4},null,null,null,null,null,{"$f":"IF(H125=\"Select Model\",\"\",combineACBLLength(J125,K125,L125,M125,N125))","v":""},{"$f":"IF(H125=\"Select Model\",\"\",combineACBWidth('Run Selections'!X125,O125,H125))","v":""},{"$f":" 'Run Selections'!BD125","v":0},{"$f":"'Run Selections'!AI125","v":""},{"$f":"'Run Selections'!AB125","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U125","v":2},{"$f":"'Run Selections'!V125","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F126=\"\",\"\",'Run Selections'!$F126)","v":""},null,{"$f":"'Run Selections'!T126","v":"Select Model"},{"$f":"'Run Selections'!L126","v":""},{"$f":"'Run Selections'!W126","v":4},null,null,null,null,null,{"$f":"IF(H126=\"Select Model\",\"\",combineACBLLength(J126,K126,L126,M126,N126))","v":""},{"$f":"IF(H126=\"Select Model\",\"\",combineACBWidth('Run Selections'!X126,O126,H126))","v":""},{"$f":" 'Run Selections'!BD126","v":0},{"$f":"'Run Selections'!AI126","v":""},{"$f":"'Run Selections'!AB126","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U126","v":2},{"$f":"'Run Selections'!V126","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F127=\"\",\"\",'Run Selections'!$F127)","v":""},null,{"$f":"'Run Selections'!T127","v":"Select Model"},{"$f":"'Run Selections'!L127","v":""},{"$f":"'Run Selections'!W127","v":4},null,null,null,null,null,{"$f":"IF(H127=\"Select Model\",\"\",combineACBLLength(J127,K127,L127,M127,N127))","v":""},{"$f":"IF(H127=\"Select Model\",\"\",combineACBWidth('Run Selections'!X127,O127,H127))","v":""},{"$f":" 'Run Selections'!BD127","v":0},{"$f":"'Run Selections'!AI127","v":""},{"$f":"'Run Selections'!AB127","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U127","v":2},{"$f":"'Run Selections'!V127","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F128=\"\",\"\",'Run Selections'!$F128)","v":""},null,{"$f":"'Run Selections'!T128","v":"Select Model"},{"$f":"'Run Selections'!L128","v":""},{"$f":"'Run Selections'!W128","v":4},null,null,null,null,null,{"$f":"IF(H128=\"Select Model\",\"\",combineACBLLength(J128,K128,L128,M128,N128))","v":""},{"$f":"IF(H128=\"Select Model\",\"\",combineACBWidth('Run Selections'!X128,O128,H128))","v":""},{"$f":" 'Run Selections'!BD128","v":0},{"$f":"'Run Selections'!AI128","v":""},{"$f":"'Run Selections'!AB128","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U128","v":2},{"$f":"'Run Selections'!V128","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F129=\"\",\"\",'Run Selections'!$F129)","v":""},null,{"$f":"'Run Selections'!T129","v":"Select Model"},{"$f":"'Run Selections'!L129","v":""},{"$f":"'Run Selections'!W129","v":4},null,null,null,null,null,{"$f":"IF(H129=\"Select Model\",\"\",combineACBLLength(J129,K129,L129,M129,N129))","v":""},{"$f":"IF(H129=\"Select Model\",\"\",combineACBWidth('Run Selections'!X129,O129,H129))","v":""},{"$f":" 'Run Selections'!BD129","v":0},{"$f":"'Run Selections'!AI129","v":""},{"$f":"'Run Selections'!AB129","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U129","v":2},{"$f":"'Run Selections'!V129","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F130=\"\",\"\",'Run Selections'!$F130)","v":""},null,{"$f":"'Run Selections'!T130","v":"Select Model"},{"$f":"'Run Selections'!L130","v":""},{"$f":"'Run Selections'!W130","v":4},null,null,null,null,null,{"$f":"IF(H130=\"Select Model\",\"\",combineACBLLength(J130,K130,L130,M130,N130))","v":""},{"$f":"IF(H130=\"Select Model\",\"\",combineACBWidth('Run Selections'!X130,O130,H130))","v":""},{"$f":" 'Run Selections'!BD130","v":0},{"$f":"'Run Selections'!AI130","v":""},{"$f":"'Run Selections'!AB130","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U130","v":2},{"$f":"'Run Selections'!V130","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F131=\"\",\"\",'Run Selections'!$F131)","v":""},null,{"$f":"'Run Selections'!T131","v":"Select Model"},{"$f":"'Run Selections'!L131","v":""},{"$f":"'Run Selections'!W131","v":4},null,null,null,null,null,{"$f":"IF(H131=\"Select Model\",\"\",combineACBLLength(J131,K131,L131,M131,N131))","v":""},{"$f":"IF(H131=\"Select Model\",\"\",combineACBWidth('Run Selections'!X131,O131,H131))","v":""},{"$f":" 'Run Selections'!BD131","v":0},{"$f":"'Run Selections'!AI131","v":""},{"$f":"'Run Selections'!AB131","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U131","v":2},{"$f":"'Run Selections'!V131","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F132=\"\",\"\",'Run Selections'!$F132)","v":""},null,{"$f":"'Run Selections'!T132","v":"Select Model"},{"$f":"'Run Selections'!L132","v":""},{"$f":"'Run Selections'!W132","v":4},null,null,null,null,null,{"$f":"IF(H132=\"Select Model\",\"\",combineACBLLength(J132,K132,L132,M132,N132))","v":""},{"$f":"IF(H132=\"Select Model\",\"\",combineACBWidth('Run Selections'!X132,O132,H132))","v":""},{"$f":" 'Run Selections'!BD132","v":0},{"$f":"'Run Selections'!AI132","v":""},{"$f":"'Run Selections'!AB132","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U132","v":2},{"$f":"'Run Selections'!V132","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F133=\"\",\"\",'Run Selections'!$F133)","v":""},null,{"$f":"'Run Selections'!T133","v":"Select Model"},{"$f":"'Run Selections'!L133","v":""},{"$f":"'Run Selections'!W133","v":4},null,null,null,null,null,{"$f":"IF(H133=\"Select Model\",\"\",combineACBLLength(J133,K133,L133,M133,N133))","v":""},{"$f":"IF(H133=\"Select Model\",\"\",combineACBWidth('Run Selections'!X133,O133,H133))","v":""},{"$f":" 'Run Selections'!BD133","v":0},{"$f":"'Run Selections'!AI133","v":""},{"$f":"'Run Selections'!AB133","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U133","v":2},{"$f":"'Run Selections'!V133","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F134=\"\",\"\",'Run Selections'!$F134)","v":""},null,{"$f":"'Run Selections'!T134","v":"Select Model"},{"$f":"'Run Selections'!L134","v":""},{"$f":"'Run Selections'!W134","v":4},null,null,null,null,null,{"$f":"IF(H134=\"Select Model\",\"\",combineACBLLength(J134,K134,L134,M134,N134))","v":""},{"$f":"IF(H134=\"Select Model\",\"\",combineACBWidth('Run Selections'!X134,O134,H134))","v":""},{"$f":" 'Run Selections'!BD134","v":0},{"$f":"'Run Selections'!AI134","v":""},{"$f":"'Run Selections'!AB134","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U134","v":2},{"$f":"'Run Selections'!V134","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F135=\"\",\"\",'Run Selections'!$F135)","v":""},null,{"$f":"'Run Selections'!T135","v":"Select Model"},{"$f":"'Run Selections'!L135","v":""},{"$f":"'Run Selections'!W135","v":4},null,null,null,null,null,{"$f":"IF(H135=\"Select Model\",\"\",combineACBLLength(J135,K135,L135,M135,N135))","v":""},{"$f":"IF(H135=\"Select Model\",\"\",combineACBWidth('Run Selections'!X135,O135,H135))","v":""},{"$f":" 'Run Selections'!BD135","v":0},{"$f":"'Run Selections'!AI135","v":""},{"$f":"'Run Selections'!AB135","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U135","v":2},{"$f":"'Run Selections'!V135","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F136=\"\",\"\",'Run Selections'!$F136)","v":""},null,{"$f":"'Run Selections'!T136","v":"Select Model"},{"$f":"'Run Selections'!L136","v":""},{"$f":"'Run Selections'!W136","v":4},null,null,null,null,null,{"$f":"IF(H136=\"Select Model\",\"\",combineACBLLength(J136,K136,L136,M136,N136))","v":""},{"$f":"IF(H136=\"Select Model\",\"\",combineACBWidth('Run Selections'!X136,O136,H136))","v":""},{"$f":" 'Run Selections'!BD136","v":0},{"$f":"'Run Selections'!AI136","v":""},{"$f":"'Run Selections'!AB136","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U136","v":2},{"$f":"'Run Selections'!V136","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F137=\"\",\"\",'Run Selections'!$F137)","v":""},null,{"$f":"'Run Selections'!T137","v":"Select Model"},{"$f":"'Run Selections'!L137","v":""},{"$f":"'Run Selections'!W137","v":4},null,null,null,null,null,{"$f":"IF(H137=\"Select Model\",\"\",combineACBLLength(J137,K137,L137,M137,N137))","v":""},{"$f":"IF(H137=\"Select Model\",\"\",combineACBWidth('Run Selections'!X137,O137,H137))","v":""},{"$f":" 'Run Selections'!BD137","v":0},{"$f":"'Run Selections'!AI137","v":""},{"$f":"'Run Selections'!AB137","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U137","v":2},{"$f":"'Run Selections'!V137","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F138=\"\",\"\",'Run Selections'!$F138)","v":""},null,{"$f":"'Run Selections'!T138","v":"Select Model"},{"$f":"'Run Selections'!L138","v":""},{"$f":"'Run Selections'!W138","v":4},null,null,null,null,null,{"$f":"IF(H138=\"Select Model\",\"\",combineACBLLength(J138,K138,L138,M138,N138))","v":""},{"$f":"IF(H138=\"Select Model\",\"\",combineACBWidth('Run Selections'!X138,O138,H138))","v":""},{"$f":" 'Run Selections'!BD138","v":0},{"$f":"'Run Selections'!AI138","v":""},{"$f":"'Run Selections'!AB138","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U138","v":2},{"$f":"'Run Selections'!V138","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F139=\"\",\"\",'Run Selections'!$F139)","v":""},null,{"$f":"'Run Selections'!T139","v":"Select Model"},{"$f":"'Run Selections'!L139","v":""},{"$f":"'Run Selections'!W139","v":4},null,null,null,null,null,{"$f":"IF(H139=\"Select Model\",\"\",combineACBLLength(J139,K139,L139,M139,N139))","v":""},{"$f":"IF(H139=\"Select Model\",\"\",combineACBWidth('Run Selections'!X139,O139,H139))","v":""},{"$f":" 'Run Selections'!BD139","v":0},{"$f":"'Run Selections'!AI139","v":""},{"$f":"'Run Selections'!AB139","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U139","v":2},{"$f":"'Run Selections'!V139","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F140=\"\",\"\",'Run Selections'!$F140)","v":""},null,{"$f":"'Run Selections'!T140","v":"Select Model"},{"$f":"'Run Selections'!L140","v":""},{"$f":"'Run Selections'!W140","v":4},null,null,null,null,null,{"$f":"IF(H140=\"Select Model\",\"\",combineACBLLength(J140,K140,L140,M140,N140))","v":""},{"$f":"IF(H140=\"Select Model\",\"\",combineACBWidth('Run Selections'!X140,O140,H140))","v":""},{"$f":" 'Run Selections'!BD140","v":0},{"$f":"'Run Selections'!AI140","v":""},{"$f":"'Run Selections'!AB140","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U140","v":2},{"$f":"'Run Selections'!V140","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F141=\"\",\"\",'Run Selections'!$F141)","v":""},null,{"$f":"'Run Selections'!T141","v":"Select Model"},{"$f":"'Run Selections'!L141","v":""},{"$f":"'Run Selections'!W141","v":4},null,null,null,null,null,{"$f":"IF(H141=\"Select Model\",\"\",combineACBLLength(J141,K141,L141,M141,N141))","v":""},{"$f":"IF(H141=\"Select Model\",\"\",combineACBWidth('Run Selections'!X141,O141,H141))","v":""},{"$f":" 'Run Selections'!BD141","v":0},{"$f":"'Run Selections'!AI141","v":""},{"$f":"'Run Selections'!AB141","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U141","v":2},{"$f":"'Run Selections'!V141","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F142=\"\",\"\",'Run Selections'!$F142)","v":""},null,{"$f":"'Run Selections'!T142","v":"Select Model"},{"$f":"'Run Selections'!L142","v":""},{"$f":"'Run Selections'!W142","v":4},null,null,null,null,null,{"$f":"IF(H142=\"Select Model\",\"\",combineACBLLength(J142,K142,L142,M142,N142))","v":""},{"$f":"IF(H142=\"Select Model\",\"\",combineACBWidth('Run Selections'!X142,O142,H142))","v":""},{"$f":" 'Run Selections'!BD142","v":0},{"$f":"'Run Selections'!AI142","v":""},{"$f":"'Run Selections'!AB142","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U142","v":2},{"$f":"'Run Selections'!V142","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F143=\"\",\"\",'Run Selections'!$F143)","v":""},null,{"$f":"'Run Selections'!T143","v":"Select Model"},{"$f":"'Run Selections'!L143","v":""},{"$f":"'Run Selections'!W143","v":4},null,null,null,null,null,{"$f":"IF(H143=\"Select Model\",\"\",combineACBLLength(J143,K143,L143,M143,N143))","v":""},{"$f":"IF(H143=\"Select Model\",\"\",combineACBWidth('Run Selections'!X143,O143,H143))","v":""},{"$f":" 'Run Selections'!BD143","v":0},{"$f":"'Run Selections'!AI143","v":""},{"$f":"'Run Selections'!AB143","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U143","v":2},{"$f":"'Run Selections'!V143","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F144=\"\",\"\",'Run Selections'!$F144)","v":""},null,{"$f":"'Run Selections'!T144","v":"Select Model"},{"$f":"'Run Selections'!L144","v":""},{"$f":"'Run Selections'!W144","v":4},null,null,null,null,null,{"$f":"IF(H144=\"Select Model\",\"\",combineACBLLength(J144,K144,L144,M144,N144))","v":""},{"$f":"IF(H144=\"Select Model\",\"\",combineACBWidth('Run Selections'!X144,O144,H144))","v":""},{"$f":" 'Run Selections'!BD144","v":0},{"$f":"'Run Selections'!AI144","v":""},{"$f":"'Run Selections'!AB144","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U144","v":2},{"$f":"'Run Selections'!V144","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F145=\"\",\"\",'Run Selections'!$F145)","v":""},null,{"$f":"'Run Selections'!T145","v":"Select Model"},{"$f":"'Run Selections'!L145","v":""},{"$f":"'Run Selections'!W145","v":4},null,null,null,null,null,{"$f":"IF(H145=\"Select Model\",\"\",combineACBLLength(J145,K145,L145,M145,N145))","v":""},{"$f":"IF(H145=\"Select Model\",\"\",combineACBWidth('Run Selections'!X145,O145,H145))","v":""},{"$f":" 'Run Selections'!BD145","v":0},{"$f":"'Run Selections'!AI145","v":""},{"$f":"'Run Selections'!AB145","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U145","v":2},{"$f":"'Run Selections'!V145","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F146=\"\",\"\",'Run Selections'!$F146)","v":""},null,{"$f":"'Run Selections'!T146","v":"Select Model"},{"$f":"'Run Selections'!L146","v":""},{"$f":"'Run Selections'!W146","v":4},null,null,null,null,null,{"$f":"IF(H146=\"Select Model\",\"\",combineACBLLength(J146,K146,L146,M146,N146))","v":""},{"$f":"IF(H146=\"Select Model\",\"\",combineACBWidth('Run Selections'!X146,O146,H146))","v":""},{"$f":" 'Run Selections'!BD146","v":0},{"$f":"'Run Selections'!AI146","v":""},{"$f":"'Run Selections'!AB146","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U146","v":2},{"$f":"'Run Selections'!V146","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F147=\"\",\"\",'Run Selections'!$F147)","v":""},null,{"$f":"'Run Selections'!T147","v":"Select Model"},{"$f":"'Run Selections'!L147","v":""},{"$f":"'Run Selections'!W147","v":4},null,null,null,null,null,{"$f":"IF(H147=\"Select Model\",\"\",combineACBLLength(J147,K147,L147,M147,N147))","v":""},{"$f":"IF(H147=\"Select Model\",\"\",combineACBWidth('Run Selections'!X147,O147,H147))","v":""},{"$f":" 'Run Selections'!BD147","v":0},{"$f":"'Run Selections'!AI147","v":""},{"$f":"'Run Selections'!AB147","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U147","v":2},{"$f":"'Run Selections'!V147","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F148=\"\",\"\",'Run Selections'!$F148)","v":""},null,{"$f":"'Run Selections'!T148","v":"Select Model"},{"$f":"'Run Selections'!L148","v":""},{"$f":"'Run Selections'!W148","v":4},null,null,null,null,null,{"$f":"IF(H148=\"Select Model\",\"\",combineACBLLength(J148,K148,L148,M148,N148))","v":""},{"$f":"IF(H148=\"Select Model\",\"\",combineACBWidth('Run Selections'!X148,O148,H148))","v":""},{"$f":" 'Run Selections'!BD148","v":0},{"$f":"'Run Selections'!AI148","v":""},{"$f":"'Run Selections'!AB148","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U148","v":2},{"$f":"'Run Selections'!V148","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F149=\"\",\"\",'Run Selections'!$F149)","v":""},null,{"$f":"'Run Selections'!T149","v":"Select Model"},{"$f":"'Run Selections'!L149","v":""},{"$f":"'Run Selections'!W149","v":4},null,null,null,null,null,{"$f":"IF(H149=\"Select Model\",\"\",combineACBLLength(J149,K149,L149,M149,N149))","v":""},{"$f":"IF(H149=\"Select Model\",\"\",combineACBWidth('Run Selections'!X149,O149,H149))","v":""},{"$f":" 'Run Selections'!BD149","v":0},{"$f":"'Run Selections'!AI149","v":""},{"$f":"'Run Selections'!AB149","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U149","v":2},{"$f":"'Run Selections'!V149","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F150=\"\",\"\",'Run Selections'!$F150)","v":""},null,{"$f":"'Run Selections'!T150","v":"Select Model"},{"$f":"'Run Selections'!L150","v":""},{"$f":"'Run Selections'!W150","v":4},null,null,null,null,null,{"$f":"IF(H150=\"Select Model\",\"\",combineACBLLength(J150,K150,L150,M150,N150))","v":""},{"$f":"IF(H150=\"Select Model\",\"\",combineACBWidth('Run Selections'!X150,O150,H150))","v":""},{"$f":" 'Run Selections'!BD150","v":0},{"$f":"'Run Selections'!AI150","v":""},{"$f":"'Run Selections'!AB150","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U150","v":2},{"$f":"'Run Selections'!V150","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F151=\"\",\"\",'Run Selections'!$F151)","v":""},null,{"$f":"'Run Selections'!T151","v":"Select Model"},{"$f":"'Run Selections'!L151","v":""},{"$f":"'Run Selections'!W151","v":4},null,null,null,null,null,{"$f":"IF(H151=\"Select Model\",\"\",combineACBLLength(J151,K151,L151,M151,N151))","v":""},{"$f":"IF(H151=\"Select Model\",\"\",combineACBWidth('Run Selections'!X151,O151,H151))","v":""},{"$f":" 'Run Selections'!BD151","v":0},{"$f":"'Run Selections'!AI151","v":""},{"$f":"'Run Selections'!AB151","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U151","v":2},{"$f":"'Run Selections'!V151","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F152=\"\",\"\",'Run Selections'!$F152)","v":""},null,{"$f":"'Run Selections'!T152","v":"Select Model"},{"$f":"'Run Selections'!L152","v":""},{"$f":"'Run Selections'!W152","v":4},null,null,null,null,null,{"$f":"IF(H152=\"Select Model\",\"\",combineACBLLength(J152,K152,L152,M152,N152))","v":""},{"$f":"IF(H152=\"Select Model\",\"\",combineACBWidth('Run Selections'!X152,O152,H152))","v":""},{"$f":" 'Run Selections'!BD152","v":0},{"$f":"'Run Selections'!AI152","v":""},{"$f":"'Run Selections'!AB152","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U152","v":2},{"$f":"'Run Selections'!V152","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F153=\"\",\"\",'Run Selections'!$F153)","v":""},null,{"$f":"'Run Selections'!T153","v":"Select Model"},{"$f":"'Run Selections'!L153","v":""},{"$f":"'Run Selections'!W153","v":4},null,null,null,null,null,{"$f":"IF(H153=\"Select Model\",\"\",combineACBLLength(J153,K153,L153,M153,N153))","v":""},{"$f":"IF(H153=\"Select Model\",\"\",combineACBWidth('Run Selections'!X153,O153,H153))","v":""},{"$f":" 'Run Selections'!BD153","v":0},{"$f":"'Run Selections'!AI153","v":""},{"$f":"'Run Selections'!AB153","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U153","v":2},{"$f":"'Run Selections'!V153","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F154=\"\",\"\",'Run Selections'!$F154)","v":""},null,{"$f":"'Run Selections'!T154","v":"Select Model"},{"$f":"'Run Selections'!L154","v":""},{"$f":"'Run Selections'!W154","v":4},null,null,null,null,null,{"$f":"IF(H154=\"Select Model\",\"\",combineACBLLength(J154,K154,L154,M154,N154))","v":""},{"$f":"IF(H154=\"Select Model\",\"\",combineACBWidth('Run Selections'!X154,O154,H154))","v":""},{"$f":" 'Run Selections'!BD154","v":0},{"$f":"'Run Selections'!AI154","v":""},{"$f":"'Run Selections'!AB154","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U154","v":2},{"$f":"'Run Selections'!V154","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F155=\"\",\"\",'Run Selections'!$F155)","v":""},null,{"$f":"'Run Selections'!T155","v":"Select Model"},{"$f":"'Run Selections'!L155","v":""},{"$f":"'Run Selections'!W155","v":4},null,null,null,null,null,{"$f":"IF(H155=\"Select Model\",\"\",combineACBLLength(J155,K155,L155,M155,N155))","v":""},{"$f":"IF(H155=\"Select Model\",\"\",combineACBWidth('Run Selections'!X155,O155,H155))","v":""},{"$f":" 'Run Selections'!BD155","v":0},{"$f":"'Run Selections'!AI155","v":""},{"$f":"'Run Selections'!AB155","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U155","v":2},{"$f":"'Run Selections'!V155","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F156=\"\",\"\",'Run Selections'!$F156)","v":""},null,{"$f":"'Run Selections'!T156","v":"Select Model"},{"$f":"'Run Selections'!L156","v":""},{"$f":"'Run Selections'!W156","v":4},null,null,null,null,null,{"$f":"IF(H156=\"Select Model\",\"\",combineACBLLength(J156,K156,L156,M156,N156))","v":""},{"$f":"IF(H156=\"Select Model\",\"\",combineACBWidth('Run Selections'!X156,O156,H156))","v":""},{"$f":" 'Run Selections'!BD156","v":0},{"$f":"'Run Selections'!AI156","v":""},{"$f":"'Run Selections'!AB156","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U156","v":2},{"$f":"'Run Selections'!V156","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F157=\"\",\"\",'Run Selections'!$F157)","v":""},null,{"$f":"'Run Selections'!T157","v":"Select Model"},{"$f":"'Run Selections'!L157","v":""},{"$f":"'Run Selections'!W157","v":4},null,null,null,null,null,{"$f":"IF(H157=\"Select Model\",\"\",combineACBLLength(J157,K157,L157,M157,N157))","v":""},{"$f":"IF(H157=\"Select Model\",\"\",combineACBWidth('Run Selections'!X157,O157,H157))","v":""},{"$f":" 'Run Selections'!BD157","v":0},{"$f":"'Run Selections'!AI157","v":""},{"$f":"'Run Selections'!AB157","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U157","v":2},{"$f":"'Run Selections'!V157","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F158=\"\",\"\",'Run Selections'!$F158)","v":""},null,{"$f":"'Run Selections'!T158","v":"Select Model"},{"$f":"'Run Selections'!L158","v":""},{"$f":"'Run Selections'!W158","v":4},null,null,null,null,null,{"$f":"IF(H158=\"Select Model\",\"\",combineACBLLength(J158,K158,L158,M158,N158))","v":""},{"$f":"IF(H158=\"Select Model\",\"\",combineACBWidth('Run Selections'!X158,O158,H158))","v":""},{"$f":" 'Run Selections'!BD158","v":0},{"$f":"'Run Selections'!AI158","v":""},{"$f":"'Run Selections'!AB158","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U158","v":2},{"$f":"'Run Selections'!V158","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F159=\"\",\"\",'Run Selections'!$F159)","v":""},null,{"$f":"'Run Selections'!T159","v":"Select Model"},{"$f":"'Run Selections'!L159","v":""},{"$f":"'Run Selections'!W159","v":4},null,null,null,null,null,{"$f":"IF(H159=\"Select Model\",\"\",combineACBLLength(J159,K159,L159,M159,N159))","v":""},{"$f":"IF(H159=\"Select Model\",\"\",combineACBWidth('Run Selections'!X159,O159,H159))","v":""},{"$f":" 'Run Selections'!BD159","v":0},{"$f":"'Run Selections'!AI159","v":""},{"$f":"'Run Selections'!AB159","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U159","v":2},{"$f":"'Run Selections'!V159","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F160=\"\",\"\",'Run Selections'!$F160)","v":""},null,{"$f":"'Run Selections'!T160","v":"Select Model"},{"$f":"'Run Selections'!L160","v":""},{"$f":"'Run Selections'!W160","v":4},null,null,null,null,null,{"$f":"IF(H160=\"Select Model\",\"\",combineACBLLength(J160,K160,L160,M160,N160))","v":""},{"$f":"IF(H160=\"Select Model\",\"\",combineACBWidth('Run Selections'!X160,O160,H160))","v":""},{"$f":" 'Run Selections'!BD160","v":0},{"$f":"'Run Selections'!AI160","v":""},{"$f":"'Run Selections'!AB160","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U160","v":2},{"$f":"'Run Selections'!V160","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F161=\"\",\"\",'Run Selections'!$F161)","v":""},null,{"$f":"'Run Selections'!T161","v":"Select Model"},{"$f":"'Run Selections'!L161","v":""},{"$f":"'Run Selections'!W161","v":4},null,null,null,null,null,{"$f":"IF(H161=\"Select Model\",\"\",combineACBLLength(J161,K161,L161,M161,N161))","v":""},{"$f":"IF(H161=\"Select Model\",\"\",combineACBWidth('Run Selections'!X161,O161,H161))","v":""},{"$f":" 'Run Selections'!BD161","v":0},{"$f":"'Run Selections'!AI161","v":""},{"$f":"'Run Selections'!AB161","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U161","v":2},{"$f":"'Run Selections'!V161","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F162=\"\",\"\",'Run Selections'!$F162)","v":""},null,{"$f":"'Run Selections'!T162","v":"Select Model"},{"$f":"'Run Selections'!L162","v":""},{"$f":"'Run Selections'!W162","v":4},null,null,null,null,null,{"$f":"IF(H162=\"Select Model\",\"\",combineACBLLength(J162,K162,L162,M162,N162))","v":""},{"$f":"IF(H162=\"Select Model\",\"\",combineACBWidth('Run Selections'!X162,O162,H162))","v":""},{"$f":" 'Run Selections'!BD162","v":0},{"$f":"'Run Selections'!AI162","v":""},{"$f":"'Run Selections'!AB162","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U162","v":2},{"$f":"'Run Selections'!V162","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F163=\"\",\"\",'Run Selections'!$F163)","v":""},null,{"$f":"'Run Selections'!T163","v":"Select Model"},{"$f":"'Run Selections'!L163","v":""},{"$f":"'Run Selections'!W163","v":4},null,null,null,null,null,{"$f":"IF(H163=\"Select Model\",\"\",combineACBLLength(J163,K163,L163,M163,N163))","v":""},{"$f":"IF(H163=\"Select Model\",\"\",combineACBWidth('Run Selections'!X163,O163,H163))","v":""},{"$f":" 'Run Selections'!BD163","v":0},{"$f":"'Run Selections'!AI163","v":""},{"$f":"'Run Selections'!AB163","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U163","v":2},{"$f":"'Run Selections'!V163","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F164=\"\",\"\",'Run Selections'!$F164)","v":""},null,{"$f":"'Run Selections'!T164","v":"Select Model"},{"$f":"'Run Selections'!L164","v":""},{"$f":"'Run Selections'!W164","v":4},null,null,null,null,null,{"$f":"IF(H164=\"Select Model\",\"\",combineACBLLength(J164,K164,L164,M164,N164))","v":""},{"$f":"IF(H164=\"Select Model\",\"\",combineACBWidth('Run Selections'!X164,O164,H164))","v":""},{"$f":" 'Run Selections'!BD164","v":0},{"$f":"'Run Selections'!AI164","v":""},{"$f":"'Run Selections'!AB164","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U164","v":2},{"$f":"'Run Selections'!V164","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F165=\"\",\"\",'Run Selections'!$F165)","v":""},null,{"$f":"'Run Selections'!T165","v":"Select Model"},{"$f":"'Run Selections'!L165","v":""},{"$f":"'Run Selections'!W165","v":4},null,null,null,null,null,{"$f":"IF(H165=\"Select Model\",\"\",combineACBLLength(J165,K165,L165,M165,N165))","v":""},{"$f":"IF(H165=\"Select Model\",\"\",combineACBWidth('Run Selections'!X165,O165,H165))","v":""},{"$f":" 'Run Selections'!BD165","v":0},{"$f":"'Run Selections'!AI165","v":""},{"$f":"'Run Selections'!AB165","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U165","v":2},{"$f":"'Run Selections'!V165","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F166=\"\",\"\",'Run Selections'!$F166)","v":""},null,{"$f":"'Run Selections'!T166","v":"Select Model"},{"$f":"'Run Selections'!L166","v":""},{"$f":"'Run Selections'!W166","v":4},null,null,null,null,null,{"$f":"IF(H166=\"Select Model\",\"\",combineACBLLength(J166,K166,L166,M166,N166))","v":""},{"$f":"IF(H166=\"Select Model\",\"\",combineACBWidth('Run Selections'!X166,O166,H166))","v":""},{"$f":" 'Run Selections'!BD166","v":0},{"$f":"'Run Selections'!AI166","v":""},{"$f":"'Run Selections'!AB166","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U166","v":2},{"$f":"'Run Selections'!V166","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F167=\"\",\"\",'Run Selections'!$F167)","v":""},null,{"$f":"'Run Selections'!T167","v":"Select Model"},{"$f":"'Run Selections'!L167","v":""},{"$f":"'Run Selections'!W167","v":4},null,null,null,null,null,{"$f":"IF(H167=\"Select Model\",\"\",combineACBLLength(J167,K167,L167,M167,N167))","v":""},{"$f":"IF(H167=\"Select Model\",\"\",combineACBWidth('Run Selections'!X167,O167,H167))","v":""},{"$f":" 'Run Selections'!BD167","v":0},{"$f":"'Run Selections'!AI167","v":""},{"$f":"'Run Selections'!AB167","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U167","v":2},{"$f":"'Run Selections'!V167","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F168=\"\",\"\",'Run Selections'!$F168)","v":""},null,{"$f":"'Run Selections'!T168","v":"Select Model"},{"$f":"'Run Selections'!L168","v":""},{"$f":"'Run Selections'!W168","v":4},null,null,null,null,null,{"$f":"IF(H168=\"Select Model\",\"\",combineACBLLength(J168,K168,L168,M168,N168))","v":""},{"$f":"IF(H168=\"Select Model\",\"\",combineACBWidth('Run Selections'!X168,O168,H168))","v":""},{"$f":" 'Run Selections'!BD168","v":0},{"$f":"'Run Selections'!AI168","v":""},{"$f":"'Run Selections'!AB168","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U168","v":2},{"$f":"'Run Selections'!V168","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F169=\"\",\"\",'Run Selections'!$F169)","v":""},null,{"$f":"'Run Selections'!T169","v":"Select Model"},{"$f":"'Run Selections'!L169","v":""},{"$f":"'Run Selections'!W169","v":4},null,null,null,null,null,{"$f":"IF(H169=\"Select Model\",\"\",combineACBLLength(J169,K169,L169,M169,N169))","v":""},{"$f":"IF(H169=\"Select Model\",\"\",combineACBWidth('Run Selections'!X169,O169,H169))","v":""},{"$f":" 'Run Selections'!BD169","v":0},{"$f":"'Run Selections'!AI169","v":""},{"$f":"'Run Selections'!AB169","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U169","v":2},{"$f":"'Run Selections'!V169","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F170=\"\",\"\",'Run Selections'!$F170)","v":""},null,{"$f":"'Run Selections'!T170","v":"Select Model"},{"$f":"'Run Selections'!L170","v":""},{"$f":"'Run Selections'!W170","v":4},null,null,null,null,null,{"$f":"IF(H170=\"Select Model\",\"\",combineACBLLength(J170,K170,L170,M170,N170))","v":""},{"$f":"IF(H170=\"Select Model\",\"\",combineACBWidth('Run Selections'!X170,O170,H170))","v":""},{"$f":" 'Run Selections'!BD170","v":0},{"$f":"'Run Selections'!AI170","v":""},{"$f":"'Run Selections'!AB170","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U170","v":2},{"$f":"'Run Selections'!V170","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F171=\"\",\"\",'Run Selections'!$F171)","v":""},null,{"$f":"'Run Selections'!T171","v":"Select Model"},{"$f":"'Run Selections'!L171","v":""},{"$f":"'Run Selections'!W171","v":4},null,null,null,null,null,{"$f":"IF(H171=\"Select Model\",\"\",combineACBLLength(J171,K171,L171,M171,N171))","v":""},{"$f":"IF(H171=\"Select Model\",\"\",combineACBWidth('Run Selections'!X171,O171,H171))","v":""},{"$f":" 'Run Selections'!BD171","v":0},{"$f":"'Run Selections'!AI171","v":""},{"$f":"'Run Selections'!AB171","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U171","v":2},{"$f":"'Run Selections'!V171","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F172=\"\",\"\",'Run Selections'!$F172)","v":""},null,{"$f":"'Run Selections'!T172","v":"Select Model"},{"$f":"'Run Selections'!L172","v":""},{"$f":"'Run Selections'!W172","v":4},null,null,null,null,null,{"$f":"IF(H172=\"Select Model\",\"\",combineACBLLength(J172,K172,L172,M172,N172))","v":""},{"$f":"IF(H172=\"Select Model\",\"\",combineACBWidth('Run Selections'!X172,O172,H172))","v":""},{"$f":" 'Run Selections'!BD172","v":0},{"$f":"'Run Selections'!AI172","v":""},{"$f":"'Run Selections'!AB172","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U172","v":2},{"$f":"'Run Selections'!V172","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F173=\"\",\"\",'Run Selections'!$F173)","v":""},null,{"$f":"'Run Selections'!T173","v":"Select Model"},{"$f":"'Run Selections'!L173","v":""},{"$f":"'Run Selections'!W173","v":4},null,null,null,null,null,{"$f":"IF(H173=\"Select Model\",\"\",combineACBLLength(J173,K173,L173,M173,N173))","v":""},{"$f":"IF(H173=\"Select Model\",\"\",combineACBWidth('Run Selections'!X173,O173,H173))","v":""},{"$f":" 'Run Selections'!BD173","v":0},{"$f":"'Run Selections'!AI173","v":""},{"$f":"'Run Selections'!AB173","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U173","v":2},{"$f":"'Run Selections'!V173","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F174=\"\",\"\",'Run Selections'!$F174)","v":""},null,{"$f":"'Run Selections'!T174","v":"Select Model"},{"$f":"'Run Selections'!L174","v":""},{"$f":"'Run Selections'!W174","v":4},null,null,null,null,null,{"$f":"IF(H174=\"Select Model\",\"\",combineACBLLength(J174,K174,L174,M174,N174))","v":""},{"$f":"IF(H174=\"Select Model\",\"\",combineACBWidth('Run Selections'!X174,O174,H174))","v":""},{"$f":" 'Run Selections'!BD174","v":0},{"$f":"'Run Selections'!AI174","v":""},{"$f":"'Run Selections'!AB174","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U174","v":2},{"$f":"'Run Selections'!V174","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F175=\"\",\"\",'Run Selections'!$F175)","v":""},null,{"$f":"'Run Selections'!T175","v":"Select Model"},{"$f":"'Run Selections'!L175","v":""},{"$f":"'Run Selections'!W175","v":4},null,null,null,null,null,{"$f":"IF(H175=\"Select Model\",\"\",combineACBLLength(J175,K175,L175,M175,N175))","v":""},{"$f":"IF(H175=\"Select Model\",\"\",combineACBWidth('Run Selections'!X175,O175,H175))","v":""},{"$f":" 'Run Selections'!BD175","v":0},{"$f":"'Run Selections'!AI175","v":""},{"$f":"'Run Selections'!AB175","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U175","v":2},{"$f":"'Run Selections'!V175","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F176=\"\",\"\",'Run Selections'!$F176)","v":""},null,{"$f":"'Run Selections'!T176","v":"Select Model"},{"$f":"'Run Selections'!L176","v":""},{"$f":"'Run Selections'!W176","v":4},null,null,null,null,null,{"$f":"IF(H176=\"Select Model\",\"\",combineACBLLength(J176,K176,L176,M176,N176))","v":""},{"$f":"IF(H176=\"Select Model\",\"\",combineACBWidth('Run Selections'!X176,O176,H176))","v":""},{"$f":" 'Run Selections'!BD176","v":0},{"$f":"'Run Selections'!AI176","v":""},{"$f":"'Run Selections'!AB176","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U176","v":2},{"$f":"'Run Selections'!V176","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F177=\"\",\"\",'Run Selections'!$F177)","v":""},null,{"$f":"'Run Selections'!T177","v":"Select Model"},{"$f":"'Run Selections'!L177","v":""},{"$f":"'Run Selections'!W177","v":4},null,null,null,null,null,{"$f":"IF(H177=\"Select Model\",\"\",combineACBLLength(J177,K177,L177,M177,N177))","v":""},{"$f":"IF(H177=\"Select Model\",\"\",combineACBWidth('Run Selections'!X177,O177,H177))","v":""},{"$f":" 'Run Selections'!BD177","v":0},{"$f":"'Run Selections'!AI177","v":""},{"$f":"'Run Selections'!AB177","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U177","v":2},{"$f":"'Run Selections'!V177","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F178=\"\",\"\",'Run Selections'!$F178)","v":""},null,{"$f":"'Run Selections'!T178","v":"Select Model"},{"$f":"'Run Selections'!L178","v":""},{"$f":"'Run Selections'!W178","v":4},null,null,null,null,null,{"$f":"IF(H178=\"Select Model\",\"\",combineACBLLength(J178,K178,L178,M178,N178))","v":""},{"$f":"IF(H178=\"Select Model\",\"\",combineACBWidth('Run Selections'!X178,O178,H178))","v":""},{"$f":" 'Run Selections'!BD178","v":0},{"$f":"'Run Selections'!AI178","v":""},{"$f":"'Run Selections'!AB178","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U178","v":2},{"$f":"'Run Selections'!V178","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F179=\"\",\"\",'Run Selections'!$F179)","v":""},null,{"$f":"'Run Selections'!T179","v":"Select Model"},{"$f":"'Run Selections'!L179","v":""},{"$f":"'Run Selections'!W179","v":4},null,null,null,null,null,{"$f":"IF(H179=\"Select Model\",\"\",combineACBLLength(J179,K179,L179,M179,N179))","v":""},{"$f":"IF(H179=\"Select Model\",\"\",combineACBWidth('Run Selections'!X179,O179,H179))","v":""},{"$f":" 'Run Selections'!BD179","v":0},{"$f":"'Run Selections'!AI179","v":""},{"$f":"'Run Selections'!AB179","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U179","v":2},{"$f":"'Run Selections'!V179","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F180=\"\",\"\",'Run Selections'!$F180)","v":""},null,{"$f":"'Run Selections'!T180","v":"Select Model"},{"$f":"'Run Selections'!L180","v":""},{"$f":"'Run Selections'!W180","v":4},null,null,null,null,null,{"$f":"IF(H180=\"Select Model\",\"\",combineACBLLength(J180,K180,L180,M180,N180))","v":""},{"$f":"IF(H180=\"Select Model\",\"\",combineACBWidth('Run Selections'!X180,O180,H180))","v":""},{"$f":" 'Run Selections'!BD180","v":0},{"$f":"'Run Selections'!AI180","v":""},{"$f":"'Run Selections'!AB180","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U180","v":2},{"$f":"'Run Selections'!V180","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F181=\"\",\"\",'Run Selections'!$F181)","v":""},null,{"$f":"'Run Selections'!T181","v":"Select Model"},{"$f":"'Run Selections'!L181","v":""},{"$f":"'Run Selections'!W181","v":4},null,null,null,null,null,{"$f":"IF(H181=\"Select Model\",\"\",combineACBLLength(J181,K181,L181,M181,N181))","v":""},{"$f":"IF(H181=\"Select Model\",\"\",combineACBWidth('Run Selections'!X181,O181,H181))","v":""},{"$f":" 'Run Selections'!BD181","v":0},{"$f":"'Run Selections'!AI181","v":""},{"$f":"'Run Selections'!AB181","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U181","v":2},{"$f":"'Run Selections'!V181","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F182=\"\",\"\",'Run Selections'!$F182)","v":""},null,{"$f":"'Run Selections'!T182","v":"Select Model"},{"$f":"'Run Selections'!L182","v":""},{"$f":"'Run Selections'!W182","v":4},null,null,null,null,null,{"$f":"IF(H182=\"Select Model\",\"\",combineACBLLength(J182,K182,L182,M182,N182))","v":""},{"$f":"IF(H182=\"Select Model\",\"\",combineACBWidth('Run Selections'!X182,O182,H182))","v":""},{"$f":" 'Run Selections'!BD182","v":0},{"$f":"'Run Selections'!AI182","v":""},{"$f":"'Run Selections'!AB182","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U182","v":2},{"$f":"'Run Selections'!V182","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F183=\"\",\"\",'Run Selections'!$F183)","v":""},null,{"$f":"'Run Selections'!T183","v":"Select Model"},{"$f":"'Run Selections'!L183","v":""},{"$f":"'Run Selections'!W183","v":4},null,null,null,null,null,{"$f":"IF(H183=\"Select Model\",\"\",combineACBLLength(J183,K183,L183,M183,N183))","v":""},{"$f":"IF(H183=\"Select Model\",\"\",combineACBWidth('Run Selections'!X183,O183,H183))","v":""},{"$f":" 'Run Selections'!BD183","v":0},{"$f":"'Run Selections'!AI183","v":""},{"$f":"'Run Selections'!AB183","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U183","v":2},{"$f":"'Run Selections'!V183","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F184=\"\",\"\",'Run Selections'!$F184)","v":""},null,{"$f":"'Run Selections'!T184","v":"Select Model"},{"$f":"'Run Selections'!L184","v":""},{"$f":"'Run Selections'!W184","v":4},null,null,null,null,null,{"$f":"IF(H184=\"Select Model\",\"\",combineACBLLength(J184,K184,L184,M184,N184))","v":""},{"$f":"IF(H184=\"Select Model\",\"\",combineACBWidth('Run Selections'!X184,O184,H184))","v":""},{"$f":" 'Run Selections'!BD184","v":0},{"$f":"'Run Selections'!AI184","v":""},{"$f":"'Run Selections'!AB184","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U184","v":2},{"$f":"'Run Selections'!V184","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F185=\"\",\"\",'Run Selections'!$F185)","v":""},null,{"$f":"'Run Selections'!T185","v":"Select Model"},{"$f":"'Run Selections'!L185","v":""},{"$f":"'Run Selections'!W185","v":4},null,null,null,null,null,{"$f":"IF(H185=\"Select Model\",\"\",combineACBLLength(J185,K185,L185,M185,N185))","v":""},{"$f":"IF(H185=\"Select Model\",\"\",combineACBWidth('Run Selections'!X185,O185,H185))","v":""},{"$f":" 'Run Selections'!BD185","v":0},{"$f":"'Run Selections'!AI185","v":""},{"$f":"'Run Selections'!AB185","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U185","v":2},{"$f":"'Run Selections'!V185","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F186=\"\",\"\",'Run Selections'!$F186)","v":""},null,{"$f":"'Run Selections'!T186","v":"Select Model"},{"$f":"'Run Selections'!L186","v":""},{"$f":"'Run Selections'!W186","v":4},null,null,null,null,null,{"$f":"IF(H186=\"Select Model\",\"\",combineACBLLength(J186,K186,L186,M186,N186))","v":""},{"$f":"IF(H186=\"Select Model\",\"\",combineACBWidth('Run Selections'!X186,O186,H186))","v":""},{"$f":" 'Run Selections'!BD186","v":0},{"$f":"'Run Selections'!AI186","v":""},{"$f":"'Run Selections'!AB186","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U186","v":2},{"$f":"'Run Selections'!V186","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F187=\"\",\"\",'Run Selections'!$F187)","v":""},null,{"$f":"'Run Selections'!T187","v":"Select Model"},{"$f":"'Run Selections'!L187","v":""},{"$f":"'Run Selections'!W187","v":4},null,null,null,null,null,{"$f":"IF(H187=\"Select Model\",\"\",combineACBLLength(J187,K187,L187,M187,N187))","v":""},{"$f":"IF(H187=\"Select Model\",\"\",combineACBWidth('Run Selections'!X187,O187,H187))","v":""},{"$f":" 'Run Selections'!BD187","v":0},{"$f":"'Run Selections'!AI187","v":""},{"$f":"'Run Selections'!AB187","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U187","v":2},{"$f":"'Run Selections'!V187","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F188=\"\",\"\",'Run Selections'!$F188)","v":""},null,{"$f":"'Run Selections'!T188","v":"Select Model"},{"$f":"'Run Selections'!L188","v":""},{"$f":"'Run Selections'!W188","v":4},null,null,null,null,null,{"$f":"IF(H188=\"Select Model\",\"\",combineACBLLength(J188,K188,L188,M188,N188))","v":""},{"$f":"IF(H188=\"Select Model\",\"\",combineACBWidth('Run Selections'!X188,O188,H188))","v":""},{"$f":" 'Run Selections'!BD188","v":0},{"$f":"'Run Selections'!AI188","v":""},{"$f":"'Run Selections'!AB188","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U188","v":2},{"$f":"'Run Selections'!V188","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F189=\"\",\"\",'Run Selections'!$F189)","v":""},null,{"$f":"'Run Selections'!T189","v":"Select Model"},{"$f":"'Run Selections'!L189","v":""},{"$f":"'Run Selections'!W189","v":4},null,null,null,null,null,{"$f":"IF(H189=\"Select Model\",\"\",combineACBLLength(J189,K189,L189,M189,N189))","v":""},{"$f":"IF(H189=\"Select Model\",\"\",combineACBWidth('Run Selections'!X189,O189,H189))","v":""},{"$f":" 'Run Selections'!BD189","v":0},{"$f":"'Run Selections'!AI189","v":""},{"$f":"'Run Selections'!AB189","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U189","v":2},{"$f":"'Run Selections'!V189","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F190=\"\",\"\",'Run Selections'!$F190)","v":""},null,{"$f":"'Run Selections'!T190","v":"Select Model"},{"$f":"'Run Selections'!L190","v":""},{"$f":"'Run Selections'!W190","v":4},null,null,null,null,null,{"$f":"IF(H190=\"Select Model\",\"\",combineACBLLength(J190,K190,L190,M190,N190))","v":""},{"$f":"IF(H190=\"Select Model\",\"\",combineACBWidth('Run Selections'!X190,O190,H190))","v":""},{"$f":" 'Run Selections'!BD190","v":0},{"$f":"'Run Selections'!AI190","v":""},{"$f":"'Run Selections'!AB190","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U190","v":2},{"$f":"'Run Selections'!V190","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F191=\"\",\"\",'Run Selections'!$F191)","v":""},null,{"$f":"'Run Selections'!T191","v":"Select Model"},{"$f":"'Run Selections'!L191","v":""},{"$f":"'Run Selections'!W191","v":4},null,null,null,null,null,{"$f":"IF(H191=\"Select Model\",\"\",combineACBLLength(J191,K191,L191,M191,N191))","v":""},{"$f":"IF(H191=\"Select Model\",\"\",combineACBWidth('Run Selections'!X191,O191,H191))","v":""},{"$f":" 'Run Selections'!BD191","v":0},{"$f":"'Run Selections'!AI191","v":""},{"$f":"'Run Selections'!AB191","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U191","v":2},{"$f":"'Run Selections'!V191","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F192=\"\",\"\",'Run Selections'!$F192)","v":""},null,{"$f":"'Run Selections'!T192","v":"Select Model"},{"$f":"'Run Selections'!L192","v":""},{"$f":"'Run Selections'!W192","v":4},null,null,null,null,null,{"$f":"IF(H192=\"Select Model\",\"\",combineACBLLength(J192,K192,L192,M192,N192))","v":""},{"$f":"IF(H192=\"Select Model\",\"\",combineACBWidth('Run Selections'!X192,O192,H192))","v":""},{"$f":" 'Run Selections'!BD192","v":0},{"$f":"'Run Selections'!AI192","v":""},{"$f":"'Run Selections'!AB192","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U192","v":2},{"$f":"'Run Selections'!V192","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F193=\"\",\"\",'Run Selections'!$F193)","v":""},null,{"$f":"'Run Selections'!T193","v":"Select Model"},{"$f":"'Run Selections'!L193","v":""},{"$f":"'Run Selections'!W193","v":4},null,null,null,null,null,{"$f":"IF(H193=\"Select Model\",\"\",combineACBLLength(J193,K193,L193,M193,N193))","v":""},{"$f":"IF(H193=\"Select Model\",\"\",combineACBWidth('Run Selections'!X193,O193,H193))","v":""},{"$f":" 'Run Selections'!BD193","v":0},{"$f":"'Run Selections'!AI193","v":""},{"$f":"'Run Selections'!AB193","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U193","v":2},{"$f":"'Run Selections'!V193","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F194=\"\",\"\",'Run Selections'!$F194)","v":""},null,{"$f":"'Run Selections'!T194","v":"Select Model"},{"$f":"'Run Selections'!L194","v":""},{"$f":"'Run Selections'!W194","v":4},null,null,null,null,null,{"$f":"IF(H194=\"Select Model\",\"\",combineACBLLength(J194,K194,L194,M194,N194))","v":""},{"$f":"IF(H194=\"Select Model\",\"\",combineACBWidth('Run Selections'!X194,O194,H194))","v":""},{"$f":" 'Run Selections'!BD194","v":0},{"$f":"'Run Selections'!AI194","v":""},{"$f":"'Run Selections'!AB194","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U194","v":2},{"$f":"'Run Selections'!V194","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F195=\"\",\"\",'Run Selections'!$F195)","v":""},null,{"$f":"'Run Selections'!T195","v":"Select Model"},{"$f":"'Run Selections'!L195","v":""},{"$f":"'Run Selections'!W195","v":4},null,null,null,null,null,{"$f":"IF(H195=\"Select Model\",\"\",combineACBLLength(J195,K195,L195,M195,N195))","v":""},{"$f":"IF(H195=\"Select Model\",\"\",combineACBWidth('Run Selections'!X195,O195,H195))","v":""},{"$f":" 'Run Selections'!BD195","v":0},{"$f":"'Run Selections'!AI195","v":""},{"$f":"'Run Selections'!AB195","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U195","v":2},{"$f":"'Run Selections'!V195","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F196=\"\",\"\",'Run Selections'!$F196)","v":""},null,{"$f":"'Run Selections'!T196","v":"Select Model"},{"$f":"'Run Selections'!L196","v":""},{"$f":"'Run Selections'!W196","v":4},null,null,null,null,null,{"$f":"IF(H196=\"Select Model\",\"\",combineACBLLength(J196,K196,L196,M196,N196))","v":""},{"$f":"IF(H196=\"Select Model\",\"\",combineACBWidth('Run Selections'!X196,O196,H196))","v":""},{"$f":" 'Run Selections'!BD196","v":0},{"$f":"'Run Selections'!AI196","v":""},{"$f":"'Run Selections'!AB196","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U196","v":2},{"$f":"'Run Selections'!V196","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F197=\"\",\"\",'Run Selections'!$F197)","v":""},null,{"$f":"'Run Selections'!T197","v":"Select Model"},{"$f":"'Run Selections'!L197","v":""},{"$f":"'Run Selections'!W197","v":4},null,null,null,null,null,{"$f":"IF(H197=\"Select Model\",\"\",combineACBLLength(J197,K197,L197,M197,N197))","v":""},{"$f":"IF(H197=\"Select Model\",\"\",combineACBWidth('Run Selections'!X197,O197,H197))","v":""},{"$f":" 'Run Selections'!BD197","v":0},{"$f":"'Run Selections'!AI197","v":""},{"$f":"'Run Selections'!AB197","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U197","v":2},{"$f":"'Run Selections'!V197","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F198=\"\",\"\",'Run Selections'!$F198)","v":""},null,{"$f":"'Run Selections'!T198","v":"Select Model"},{"$f":"'Run Selections'!L198","v":""},{"$f":"'Run Selections'!W198","v":4},null,null,null,null,null,{"$f":"IF(H198=\"Select Model\",\"\",combineACBLLength(J198,K198,L198,M198,N198))","v":""},{"$f":"IF(H198=\"Select Model\",\"\",combineACBWidth('Run Selections'!X198,O198,H198))","v":""},{"$f":" 'Run Selections'!BD198","v":0},{"$f":"'Run Selections'!AI198","v":""},{"$f":"'Run Selections'!AB198","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U198","v":2},{"$f":"'Run Selections'!V198","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F199=\"\",\"\",'Run Selections'!$F199)","v":""},null,{"$f":"'Run Selections'!T199","v":"Select Model"},{"$f":"'Run Selections'!L199","v":""},{"$f":"'Run Selections'!W199","v":4},null,null,null,null,null,{"$f":"IF(H199=\"Select Model\",\"\",combineACBLLength(J199,K199,L199,M199,N199))","v":""},{"$f":"IF(H199=\"Select Model\",\"\",combineACBWidth('Run Selections'!X199,O199,H199))","v":""},{"$f":" 'Run Selections'!BD199","v":0},{"$f":"'Run Selections'!AI199","v":""},{"$f":"'Run Selections'!AB199","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U199","v":2},{"$f":"'Run Selections'!V199","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F200=\"\",\"\",'Run Selections'!$F200)","v":""},null,{"$f":"'Run Selections'!T200","v":"Select Model"},{"$f":"'Run Selections'!L200","v":""},{"$f":"'Run Selections'!W200","v":4},null,null,null,null,null,{"$f":"IF(H200=\"Select Model\",\"\",combineACBLLength(J200,K200,L200,M200,N200))","v":""},{"$f":"IF(H200=\"Select Model\",\"\",combineACBWidth('Run Selections'!X200,O200,H200))","v":""},{"$f":" 'Run Selections'!BD200","v":0},{"$f":"'Run Selections'!AI200","v":""},{"$f":"'Run Selections'!AB200","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U200","v":2},{"$f":"'Run Selections'!V200","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F201=\"\",\"\",'Run Selections'!$F201)","v":""},null,{"$f":"'Run Selections'!T201","v":"Select Model"},{"$f":"'Run Selections'!L201","v":""},{"$f":"'Run Selections'!W201","v":4},null,null,null,null,null,{"$f":"IF(H201=\"Select Model\",\"\",combineACBLLength(J201,K201,L201,M201,N201))","v":""},{"$f":"IF(H201=\"Select Model\",\"\",combineACBWidth('Run Selections'!X201,O201,H201))","v":""},{"$f":" 'Run Selections'!BD201","v":0},{"$f":"'Run Selections'!AI201","v":""},{"$f":"'Run Selections'!AB201","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U201","v":2},{"$f":"'Run Selections'!V201","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F202=\"\",\"\",'Run Selections'!$F202)","v":""},null,{"$f":"'Run Selections'!T202","v":"Select Model"},{"$f":"'Run Selections'!L202","v":""},{"$f":"'Run Selections'!W202","v":4},null,null,null,null,null,{"$f":"IF(H202=\"Select Model\",\"\",combineACBLLength(J202,K202,L202,M202,N202))","v":""},{"$f":"IF(H202=\"Select Model\",\"\",combineACBWidth('Run Selections'!X202,O202,H202))","v":""},{"$f":" 'Run Selections'!BD202","v":0},{"$f":"'Run Selections'!AI202","v":""},{"$f":"'Run Selections'!AB202","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U202","v":2},{"$f":"'Run Selections'!V202","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F203=\"\",\"\",'Run Selections'!$F203)","v":""},null,{"$f":"'Run Selections'!T203","v":"Select Model"},{"$f":"'Run Selections'!L203","v":""},{"$f":"'Run Selections'!W203","v":4},null,null,null,null,null,{"$f":"IF(H203=\"Select Model\",\"\",combineACBLLength(J203,K203,L203,M203,N203))","v":""},{"$f":"IF(H203=\"Select Model\",\"\",combineACBWidth('Run Selections'!X203,O203,H203))","v":""},{"$f":" 'Run Selections'!BD203","v":0},{"$f":"'Run Selections'!AI203","v":""},{"$f":"'Run Selections'!AB203","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U203","v":2},{"$f":"'Run Selections'!V203","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F204=\"\",\"\",'Run Selections'!$F204)","v":""},null,{"$f":"'Run Selections'!T204","v":"Select Model"},{"$f":"'Run Selections'!L204","v":""},{"$f":"'Run Selections'!W204","v":4},null,null,null,null,null,{"$f":"IF(H204=\"Select Model\",\"\",combineACBLLength(J204,K204,L204,M204,N204))","v":""},{"$f":"IF(H204=\"Select Model\",\"\",combineACBWidth('Run Selections'!X204,O204,H204))","v":""},{"$f":" 'Run Selections'!BD204","v":0},{"$f":"'Run Selections'!AI204","v":""},{"$f":"'Run Selections'!AB204","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U204","v":2},{"$f":"'Run Selections'!V204","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F205=\"\",\"\",'Run Selections'!$F205)","v":""},null,{"$f":"'Run Selections'!T205","v":"Select Model"},{"$f":"'Run Selections'!L205","v":""},{"$f":"'Run Selections'!W205","v":4},null,null,null,null,null,{"$f":"IF(H205=\"Select Model\",\"\",combineACBLLength(J205,K205,L205,M205,N205))","v":""},{"$f":"IF(H205=\"Select Model\",\"\",combineACBWidth('Run Selections'!X205,O205,H205))","v":""},{"$f":" 'Run Selections'!BD205","v":0},{"$f":"'Run Selections'!AI205","v":""},{"$f":"'Run Selections'!AB205","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U205","v":2},{"$f":"'Run Selections'!V205","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F206=\"\",\"\",'Run Selections'!$F206)","v":""},null,{"$f":"'Run Selections'!T206","v":"Select Model"},{"$f":"'Run Selections'!L206","v":""},{"$f":"'Run Selections'!W206","v":4},null,null,null,null,null,{"$f":"IF(H206=\"Select Model\",\"\",combineACBLLength(J206,K206,L206,M206,N206))","v":""},{"$f":"IF(H206=\"Select Model\",\"\",combineACBWidth('Run Selections'!X206,O206,H206))","v":""},{"$f":" 'Run Selections'!BD206","v":0},{"$f":"'Run Selections'!AI206","v":""},{"$f":"'Run Selections'!AB206","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U206","v":2},{"$f":"'Run Selections'!V206","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F207=\"\",\"\",'Run Selections'!$F207)","v":""},null,{"$f":"'Run Selections'!T207","v":"Select Model"},{"$f":"'Run Selections'!L207","v":""},{"$f":"'Run Selections'!W207","v":4},null,null,null,null,null,{"$f":"IF(H207=\"Select Model\",\"\",combineACBLLength(J207,K207,L207,M207,N207))","v":""},{"$f":"IF(H207=\"Select Model\",\"\",combineACBWidth('Run Selections'!X207,O207,H207))","v":""},{"$f":" 'Run Selections'!BD207","v":0},{"$f":"'Run Selections'!AI207","v":""},{"$f":"'Run Selections'!AB207","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U207","v":2},{"$f":"'Run Selections'!V207","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F208=\"\",\"\",'Run Selections'!$F208)","v":""},null,{"$f":"'Run Selections'!T208","v":"Select Model"},{"$f":"'Run Selections'!L208","v":""},{"$f":"'Run Selections'!W208","v":4},null,null,null,null,null,{"$f":"IF(H208=\"Select Model\",\"\",combineACBLLength(J208,K208,L208,M208,N208))","v":""},{"$f":"IF(H208=\"Select Model\",\"\",combineACBWidth('Run Selections'!X208,O208,H208))","v":""},{"$f":" 'Run Selections'!BD208","v":0},{"$f":"'Run Selections'!AI208","v":""},{"$f":"'Run Selections'!AB208","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U208","v":2},{"$f":"'Run Selections'!V208","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F209=\"\",\"\",'Run Selections'!$F209)","v":""},null,{"$f":"'Run Selections'!T209","v":"Select Model"},{"$f":"'Run Selections'!L209","v":""},{"$f":"'Run Selections'!W209","v":4},null,null,null,null,null,{"$f":"IF(H209=\"Select Model\",\"\",combineACBLLength(J209,K209,L209,M209,N209))","v":""},{"$f":"IF(H209=\"Select Model\",\"\",combineACBWidth('Run Selections'!X209,O209,H209))","v":""},{"$f":" 'Run Selections'!BD209","v":0},{"$f":"'Run Selections'!AI209","v":""},{"$f":"'Run Selections'!AB209","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U209","v":2},{"$f":"'Run Selections'!V209","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F210=\"\",\"\",'Run Selections'!$F210)","v":""},null,{"$f":"'Run Selections'!T210","v":"Select Model"},{"$f":"'Run Selections'!L210","v":""},{"$f":"'Run Selections'!W210","v":4},null,null,null,null,null,{"$f":"IF(H210=\"Select Model\",\"\",combineACBLLength(J210,K210,L210,M210,N210))","v":""},{"$f":"IF(H210=\"Select Model\",\"\",combineACBWidth('Run Selections'!X210,O210,H210))","v":""},{"$f":" 'Run Selections'!BD210","v":0},{"$f":"'Run Selections'!AI210","v":""},{"$f":"'Run Selections'!AB210","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U210","v":2},{"$f":"'Run Selections'!V210","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F211=\"\",\"\",'Run Selections'!$F211)","v":""},null,{"$f":"'Run Selections'!T211","v":"Select Model"},{"$f":"'Run Selections'!L211","v":""},{"$f":"'Run Selections'!W211","v":4},null,null,null,null,null,{"$f":"IF(H211=\"Select Model\",\"\",combineACBLLength(J211,K211,L211,M211,N211))","v":""},{"$f":"IF(H211=\"Select Model\",\"\",combineACBWidth('Run Selections'!X211,O211,H211))","v":""},{"$f":" 'Run Selections'!BD211","v":0},{"$f":"'Run Selections'!AI211","v":""},{"$f":"'Run Selections'!AB211","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U211","v":2},{"$f":"'Run Selections'!V211","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F212=\"\",\"\",'Run Selections'!$F212)","v":""},null,{"$f":"'Run Selections'!T212","v":"Select Model"},{"$f":"'Run Selections'!L212","v":""},{"$f":"'Run Selections'!W212","v":4},null,null,null,null,null,{"$f":"IF(H212=\"Select Model\",\"\",combineACBLLength(J212,K212,L212,M212,N212))","v":""},{"$f":"IF(H212=\"Select Model\",\"\",combineACBWidth('Run Selections'!X212,O212,H212))","v":""},{"$f":" 'Run Selections'!BD212","v":0},{"$f":"'Run Selections'!AI212","v":""},{"$f":"'Run Selections'!AB212","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U212","v":2},{"$f":"'Run Selections'!V212","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F213=\"\",\"\",'Run Selections'!$F213)","v":""},null,{"$f":"'Run Selections'!T213","v":"Select Model"},{"$f":"'Run Selections'!L213","v":""},{"$f":"'Run Selections'!W213","v":4},null,null,null,null,null,{"$f":"IF(H213=\"Select Model\",\"\",combineACBLLength(J213,K213,L213,M213,N213))","v":""},{"$f":"IF(H213=\"Select Model\",\"\",combineACBWidth('Run Selections'!X213,O213,H213))","v":""},{"$f":" 'Run Selections'!BD213","v":0},{"$f":"'Run Selections'!AI213","v":""},{"$f":"'Run Selections'!AB213","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U213","v":2},{"$f":"'Run Selections'!V213","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F214=\"\",\"\",'Run Selections'!$F214)","v":""},null,{"$f":"'Run Selections'!T214","v":"Select Model"},{"$f":"'Run Selections'!L214","v":""},{"$f":"'Run Selections'!W214","v":4},null,null,null,null,null,{"$f":"IF(H214=\"Select Model\",\"\",combineACBLLength(J214,K214,L214,M214,N214))","v":""},{"$f":"IF(H214=\"Select Model\",\"\",combineACBWidth('Run Selections'!X214,O214,H214))","v":""},{"$f":" 'Run Selections'!BD214","v":0},{"$f":"'Run Selections'!AI214","v":""},{"$f":"'Run Selections'!AB214","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U214","v":2},{"$f":"'Run Selections'!V214","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F215=\"\",\"\",'Run Selections'!$F215)","v":""},null,{"$f":"'Run Selections'!T215","v":"Select Model"},{"$f":"'Run Selections'!L215","v":""},{"$f":"'Run Selections'!W215","v":4},null,null,null,null,null,{"$f":"IF(H215=\"Select Model\",\"\",combineACBLLength(J215,K215,L215,M215,N215))","v":""},{"$f":"IF(H215=\"Select Model\",\"\",combineACBWidth('Run Selections'!X215,O215,H215))","v":""},{"$f":" 'Run Selections'!BD215","v":0},{"$f":"'Run Selections'!AI215","v":""},{"$f":"'Run Selections'!AB215","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U215","v":2},{"$f":"'Run Selections'!V215","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F216=\"\",\"\",'Run Selections'!$F216)","v":""},null,{"$f":"'Run Selections'!T216","v":"Select Model"},{"$f":"'Run Selections'!L216","v":""},{"$f":"'Run Selections'!W216","v":4},null,null,null,null,null,{"$f":"IF(H216=\"Select Model\",\"\",combineACBLLength(J216,K216,L216,M216,N216))","v":""},{"$f":"IF(H216=\"Select Model\",\"\",combineACBWidth('Run Selections'!X216,O216,H216))","v":""},{"$f":" 'Run Selections'!BD216","v":0},{"$f":"'Run Selections'!AI216","v":""},{"$f":"'Run Selections'!AB216","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U216","v":2},{"$f":"'Run Selections'!V216","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F217=\"\",\"\",'Run Selections'!$F217)","v":""},null,{"$f":"'Run Selections'!T217","v":"Select Model"},{"$f":"'Run Selections'!L217","v":""},{"$f":"'Run Selections'!W217","v":4},null,null,null,null,null,{"$f":"IF(H217=\"Select Model\",\"\",combineACBLLength(J217,K217,L217,M217,N217))","v":""},{"$f":"IF(H217=\"Select Model\",\"\",combineACBWidth('Run Selections'!X217,O217,H217))","v":""},{"$f":" 'Run Selections'!BD217","v":0},{"$f":"'Run Selections'!AI217","v":""},{"$f":"'Run Selections'!AB217","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U217","v":2},{"$f":"'Run Selections'!V217","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F218=\"\",\"\",'Run Selections'!$F218)","v":""},null,{"$f":"'Run Selections'!T218","v":"Select Model"},{"$f":"'Run Selections'!L218","v":""},{"$f":"'Run Selections'!W218","v":4},null,null,null,null,null,{"$f":"IF(H218=\"Select Model\",\"\",combineACBLLength(J218,K218,L218,M218,N218))","v":""},{"$f":"IF(H218=\"Select Model\",\"\",combineACBWidth('Run Selections'!X218,O218,H218))","v":""},{"$f":" 'Run Selections'!BD218","v":0},{"$f":"'Run Selections'!AI218","v":""},{"$f":"'Run Selections'!AB218","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U218","v":2},{"$f":"'Run Selections'!V218","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F219=\"\",\"\",'Run Selections'!$F219)","v":""},null,{"$f":"'Run Selections'!T219","v":"Select Model"},{"$f":"'Run Selections'!L219","v":""},{"$f":"'Run Selections'!W219","v":4},null,null,null,null,null,{"$f":"IF(H219=\"Select Model\",\"\",combineACBLLength(J219,K219,L219,M219,N219))","v":""},{"$f":"IF(H219=\"Select Model\",\"\",combineACBWidth('Run Selections'!X219,O219,H219))","v":""},{"$f":" 'Run Selections'!BD219","v":0},{"$f":"'Run Selections'!AI219","v":""},{"$f":"'Run Selections'!AB219","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U219","v":2},{"$f":"'Run Selections'!V219","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F220=\"\",\"\",'Run Selections'!$F220)","v":""},null,{"$f":"'Run Selections'!T220","v":"Select Model"},{"$f":"'Run Selections'!L220","v":""},{"$f":"'Run Selections'!W220","v":4},null,null,null,null,null,{"$f":"IF(H220=\"Select Model\",\"\",combineACBLLength(J220,K220,L220,M220,N220))","v":""},{"$f":"IF(H220=\"Select Model\",\"\",combineACBWidth('Run Selections'!X220,O220,H220))","v":""},{"$f":" 'Run Selections'!BD220","v":0},{"$f":"'Run Selections'!AI220","v":""},{"$f":"'Run Selections'!AB220","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U220","v":2},{"$f":"'Run Selections'!V220","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F221=\"\",\"\",'Run Selections'!$F221)","v":""},null,{"$f":"'Run Selections'!T221","v":"Select Model"},{"$f":"'Run Selections'!L221","v":""},{"$f":"'Run Selections'!W221","v":4},null,null,null,null,null,{"$f":"IF(H221=\"Select Model\",\"\",combineACBLLength(J221,K221,L221,M221,N221))","v":""},{"$f":"IF(H221=\"Select Model\",\"\",combineACBWidth('Run Selections'!X221,O221,H221))","v":""},{"$f":" 'Run Selections'!BD221","v":0},{"$f":"'Run Selections'!AI221","v":""},{"$f":"'Run Selections'!AB221","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U221","v":2},{"$f":"'Run Selections'!V221","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F222=\"\",\"\",'Run Selections'!$F222)","v":""},null,{"$f":"'Run Selections'!T222","v":"Select Model"},{"$f":"'Run Selections'!L222","v":""},{"$f":"'Run Selections'!W222","v":4},null,null,null,null,null,{"$f":"IF(H222=\"Select Model\",\"\",combineACBLLength(J222,K222,L222,M222,N222))","v":""},{"$f":"IF(H222=\"Select Model\",\"\",combineACBWidth('Run Selections'!X222,O222,H222))","v":""},{"$f":" 'Run Selections'!BD222","v":0},{"$f":"'Run Selections'!AI222","v":""},{"$f":"'Run Selections'!AB222","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U222","v":2},{"$f":"'Run Selections'!V222","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F223=\"\",\"\",'Run Selections'!$F223)","v":""},null,{"$f":"'Run Selections'!T223","v":"Select Model"},{"$f":"'Run Selections'!L223","v":""},{"$f":"'Run Selections'!W223","v":4},null,null,null,null,null,{"$f":"IF(H223=\"Select Model\",\"\",combineACBLLength(J223,K223,L223,M223,N223))","v":""},{"$f":"IF(H223=\"Select Model\",\"\",combineACBWidth('Run Selections'!X223,O223,H223))","v":""},{"$f":" 'Run Selections'!BD223","v":0},{"$f":"'Run Selections'!AI223","v":""},{"$f":"'Run Selections'!AB223","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U223","v":2},{"$f":"'Run Selections'!V223","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F224=\"\",\"\",'Run Selections'!$F224)","v":""},null,{"$f":"'Run Selections'!T224","v":"Select Model"},{"$f":"'Run Selections'!L224","v":""},{"$f":"'Run Selections'!W224","v":4},null,null,null,null,null,{"$f":"IF(H224=\"Select Model\",\"\",combineACBLLength(J224,K224,L224,M224,N224))","v":""},{"$f":"IF(H224=\"Select Model\",\"\",combineACBWidth('Run Selections'!X224,O224,H224))","v":""},{"$f":" 'Run Selections'!BD224","v":0},{"$f":"'Run Selections'!AI224","v":""},{"$f":"'Run Selections'!AB224","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U224","v":2},{"$f":"'Run Selections'!V224","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F225=\"\",\"\",'Run Selections'!$F225)","v":""},null,{"$f":"'Run Selections'!T225","v":"Select Model"},{"$f":"'Run Selections'!L225","v":""},{"$f":"'Run Selections'!W225","v":4},null,null,null,null,null,{"$f":"IF(H225=\"Select Model\",\"\",combineACBLLength(J225,K225,L225,M225,N225))","v":""},{"$f":"IF(H225=\"Select Model\",\"\",combineACBWidth('Run Selections'!X225,O225,H225))","v":""},{"$f":" 'Run Selections'!BD225","v":0},{"$f":"'Run Selections'!AI225","v":""},{"$f":"'Run Selections'!AB225","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U225","v":2},{"$f":"'Run Selections'!V225","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F226=\"\",\"\",'Run Selections'!$F226)","v":""},null,{"$f":"'Run Selections'!T226","v":"Select Model"},{"$f":"'Run Selections'!L226","v":""},{"$f":"'Run Selections'!W226","v":4},null,null,null,null,null,{"$f":"IF(H226=\"Select Model\",\"\",combineACBLLength(J226,K226,L226,M226,N226))","v":""},{"$f":"IF(H226=\"Select Model\",\"\",combineACBWidth('Run Selections'!X226,O226,H226))","v":""},{"$f":" 'Run Selections'!BD226","v":0},{"$f":"'Run Selections'!AI226","v":""},{"$f":"'Run Selections'!AB226","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U226","v":2},{"$f":"'Run Selections'!V226","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F227=\"\",\"\",'Run Selections'!$F227)","v":""},null,{"$f":"'Run Selections'!T227","v":"Select Model"},{"$f":"'Run Selections'!L227","v":""},{"$f":"'Run Selections'!W227","v":4},null,null,null,null,null,{"$f":"IF(H227=\"Select Model\",\"\",combineACBLLength(J227,K227,L227,M227,N227))","v":""},{"$f":"IF(H227=\"Select Model\",\"\",combineACBWidth('Run Selections'!X227,O227,H227))","v":""},{"$f":" 'Run Selections'!BD227","v":0},{"$f":"'Run Selections'!AI227","v":""},{"$f":"'Run Selections'!AB227","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U227","v":2},{"$f":"'Run Selections'!V227","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F228=\"\",\"\",'Run Selections'!$F228)","v":""},null,{"$f":"'Run Selections'!T228","v":"Select Model"},{"$f":"'Run Selections'!L228","v":""},{"$f":"'Run Selections'!W228","v":4},null,null,null,null,null,{"$f":"IF(H228=\"Select Model\",\"\",combineACBLLength(J228,K228,L228,M228,N228))","v":""},{"$f":"IF(H228=\"Select Model\",\"\",combineACBWidth('Run Selections'!X228,O228,H228))","v":""},{"$f":" 'Run Selections'!BD228","v":0},{"$f":"'Run Selections'!AI228","v":""},{"$f":"'Run Selections'!AB228","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U228","v":2},{"$f":"'Run Selections'!V228","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F229=\"\",\"\",'Run Selections'!$F229)","v":""},null,{"$f":"'Run Selections'!T229","v":"Select Model"},{"$f":"'Run Selections'!L229","v":""},{"$f":"'Run Selections'!W229","v":4},null,null,null,null,null,{"$f":"IF(H229=\"Select Model\",\"\",combineACBLLength(J229,K229,L229,M229,N229))","v":""},{"$f":"IF(H229=\"Select Model\",\"\",combineACBWidth('Run Selections'!X229,O229,H229))","v":""},{"$f":" 'Run Selections'!BD229","v":0},{"$f":"'Run Selections'!AI229","v":""},{"$f":"'Run Selections'!AB229","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U229","v":2},{"$f":"'Run Selections'!V229","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F230=\"\",\"\",'Run Selections'!$F230)","v":""},null,{"$f":"'Run Selections'!T230","v":"Select Model"},{"$f":"'Run Selections'!L230","v":""},{"$f":"'Run Selections'!W230","v":4},null,null,null,null,null,{"$f":"IF(H230=\"Select Model\",\"\",combineACBLLength(J230,K230,L230,M230,N230))","v":""},{"$f":"IF(H230=\"Select Model\",\"\",combineACBWidth('Run Selections'!X230,O230,H230))","v":""},{"$f":" 'Run Selections'!BD230","v":0},{"$f":"'Run Selections'!AI230","v":""},{"$f":"'Run Selections'!AB230","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U230","v":2},{"$f":"'Run Selections'!V230","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F231=\"\",\"\",'Run Selections'!$F231)","v":""},null,{"$f":"'Run Selections'!T231","v":"Select Model"},{"$f":"'Run Selections'!L231","v":""},{"$f":"'Run Selections'!W231","v":4},null,null,null,null,null,{"$f":"IF(H231=\"Select Model\",\"\",combineACBLLength(J231,K231,L231,M231,N231))","v":""},{"$f":"IF(H231=\"Select Model\",\"\",combineACBWidth('Run Selections'!X231,O231,H231))","v":""},{"$f":" 'Run Selections'!BD231","v":0},{"$f":"'Run Selections'!AI231","v":""},{"$f":"'Run Selections'!AB231","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U231","v":2},{"$f":"'Run Selections'!V231","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F232=\"\",\"\",'Run Selections'!$F232)","v":""},null,{"$f":"'Run Selections'!T232","v":"Select Model"},{"$f":"'Run Selections'!L232","v":""},{"$f":"'Run Selections'!W232","v":4},null,null,null,null,null,{"$f":"IF(H232=\"Select Model\",\"\",combineACBLLength(J232,K232,L232,M232,N232))","v":""},{"$f":"IF(H232=\"Select Model\",\"\",combineACBWidth('Run Selections'!X232,O232,H232))","v":""},{"$f":" 'Run Selections'!BD232","v":0},{"$f":"'Run Selections'!AI232","v":""},{"$f":"'Run Selections'!AB232","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U232","v":2},{"$f":"'Run Selections'!V232","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F233=\"\",\"\",'Run Selections'!$F233)","v":""},null,{"$f":"'Run Selections'!T233","v":"Select Model"},{"$f":"'Run Selections'!L233","v":""},{"$f":"'Run Selections'!W233","v":4},null,null,null,null,null,{"$f":"IF(H233=\"Select Model\",\"\",combineACBLLength(J233,K233,L233,M233,N233))","v":""},{"$f":"IF(H233=\"Select Model\",\"\",combineACBWidth('Run Selections'!X233,O233,H233))","v":""},{"$f":" 'Run Selections'!BD233","v":0},{"$f":"'Run Selections'!AI233","v":""},{"$f":"'Run Selections'!AB233","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U233","v":2},{"$f":"'Run Selections'!V233","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F234=\"\",\"\",'Run Selections'!$F234)","v":""},null,{"$f":"'Run Selections'!T234","v":"Select Model"},{"$f":"'Run Selections'!L234","v":""},{"$f":"'Run Selections'!W234","v":4},null,null,null,null,null,{"$f":"IF(H234=\"Select Model\",\"\",combineACBLLength(J234,K234,L234,M234,N234))","v":""},{"$f":"IF(H234=\"Select Model\",\"\",combineACBWidth('Run Selections'!X234,O234,H234))","v":""},{"$f":" 'Run Selections'!BD234","v":0},{"$f":"'Run Selections'!AI234","v":""},{"$f":"'Run Selections'!AB234","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U234","v":2},{"$f":"'Run Selections'!V234","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F235=\"\",\"\",'Run Selections'!$F235)","v":""},null,{"$f":"'Run Selections'!T235","v":"Select Model"},{"$f":"'Run Selections'!L235","v":""},{"$f":"'Run Selections'!W235","v":4},null,null,null,null,null,{"$f":"IF(H235=\"Select Model\",\"\",combineACBLLength(J235,K235,L235,M235,N235))","v":""},{"$f":"IF(H235=\"Select Model\",\"\",combineACBWidth('Run Selections'!X235,O235,H235))","v":""},{"$f":" 'Run Selections'!BD235","v":0},{"$f":"'Run Selections'!AI235","v":""},{"$f":"'Run Selections'!AB235","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U235","v":2},{"$f":"'Run Selections'!V235","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F236=\"\",\"\",'Run Selections'!$F236)","v":""},null,{"$f":"'Run Selections'!T236","v":"Select Model"},{"$f":"'Run Selections'!L236","v":""},{"$f":"'Run Selections'!W236","v":4},null,null,null,null,null,{"$f":"IF(H236=\"Select Model\",\"\",combineACBLLength(J236,K236,L236,M236,N236))","v":""},{"$f":"IF(H236=\"Select Model\",\"\",combineACBWidth('Run Selections'!X236,O236,H236))","v":""},{"$f":" 'Run Selections'!BD236","v":0},{"$f":"'Run Selections'!AI236","v":""},{"$f":"'Run Selections'!AB236","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U236","v":2},{"$f":"'Run Selections'!V236","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F237=\"\",\"\",'Run Selections'!$F237)","v":""},null,{"$f":"'Run Selections'!T237","v":"Select Model"},{"$f":"'Run Selections'!L237","v":""},{"$f":"'Run Selections'!W237","v":4},null,null,null,null,null,{"$f":"IF(H237=\"Select Model\",\"\",combineACBLLength(J237,K237,L237,M237,N237))","v":""},{"$f":"IF(H237=\"Select Model\",\"\",combineACBWidth('Run Selections'!X237,O237,H237))","v":""},{"$f":" 'Run Selections'!BD237","v":0},{"$f":"'Run Selections'!AI237","v":""},{"$f":"'Run Selections'!AB237","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U237","v":2},{"$f":"'Run Selections'!V237","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F238=\"\",\"\",'Run Selections'!$F238)","v":""},null,{"$f":"'Run Selections'!T238","v":"Select Model"},{"$f":"'Run Selections'!L238","v":""},{"$f":"'Run Selections'!W238","v":4},null,null,null,null,null,{"$f":"IF(H238=\"Select Model\",\"\",combineACBLLength(J238,K238,L238,M238,N238))","v":""},{"$f":"IF(H238=\"Select Model\",\"\",combineACBWidth('Run Selections'!X238,O238,H238))","v":""},{"$f":" 'Run Selections'!BD238","v":0},{"$f":"'Run Selections'!AI238","v":""},{"$f":"'Run Selections'!AB238","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U238","v":2},{"$f":"'Run Selections'!V238","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F239=\"\",\"\",'Run Selections'!$F239)","v":""},null,{"$f":"'Run Selections'!T239","v":"Select Model"},{"$f":"'Run Selections'!L239","v":""},{"$f":"'Run Selections'!W239","v":4},null,null,null,null,null,{"$f":"IF(H239=\"Select Model\",\"\",combineACBLLength(J239,K239,L239,M239,N239))","v":""},{"$f":"IF(H239=\"Select Model\",\"\",combineACBWidth('Run Selections'!X239,O239,H239))","v":""},{"$f":" 'Run Selections'!BD239","v":0},{"$f":"'Run Selections'!AI239","v":""},{"$f":"'Run Selections'!AB239","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U239","v":2},{"$f":"'Run Selections'!V239","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F240=\"\",\"\",'Run Selections'!$F240)","v":""},null,{"$f":"'Run Selections'!T240","v":"Select Model"},{"$f":"'Run Selections'!L240","v":""},{"$f":"'Run Selections'!W240","v":4},null,null,null,null,null,{"$f":"IF(H240=\"Select Model\",\"\",combineACBLLength(J240,K240,L240,M240,N240))","v":""},{"$f":"IF(H240=\"Select Model\",\"\",combineACBWidth('Run Selections'!X240,O240,H240))","v":""},{"$f":" 'Run Selections'!BD240","v":0},{"$f":"'Run Selections'!AI240","v":""},{"$f":"'Run Selections'!AB240","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U240","v":2},{"$f":"'Run Selections'!V240","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F241=\"\",\"\",'Run Selections'!$F241)","v":""},null,{"$f":"'Run Selections'!T241","v":"Select Model"},{"$f":"'Run Selections'!L241","v":""},{"$f":"'Run Selections'!W241","v":4},null,null,null,null,null,{"$f":"IF(H241=\"Select Model\",\"\",combineACBLLength(J241,K241,L241,M241,N241))","v":""},{"$f":"IF(H241=\"Select Model\",\"\",combineACBWidth('Run Selections'!X241,O241,H241))","v":""},{"$f":" 'Run Selections'!BD241","v":0},{"$f":"'Run Selections'!AI241","v":""},{"$f":"'Run Selections'!AB241","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U241","v":2},{"$f":"'Run Selections'!V241","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F242=\"\",\"\",'Run Selections'!$F242)","v":""},null,{"$f":"'Run Selections'!T242","v":"Select Model"},{"$f":"'Run Selections'!L242","v":""},{"$f":"'Run Selections'!W242","v":4},null,null,null,null,null,{"$f":"IF(H242=\"Select Model\",\"\",combineACBLLength(J242,K242,L242,M242,N242))","v":""},{"$f":"IF(H242=\"Select Model\",\"\",combineACBWidth('Run Selections'!X242,O242,H242))","v":""},{"$f":" 'Run Selections'!BD242","v":0},{"$f":"'Run Selections'!AI242","v":""},{"$f":"'Run Selections'!AB242","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U242","v":2},{"$f":"'Run Selections'!V242","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F243=\"\",\"\",'Run Selections'!$F243)","v":""},null,{"$f":"'Run Selections'!T243","v":"Select Model"},{"$f":"'Run Selections'!L243","v":""},{"$f":"'Run Selections'!W243","v":4},null,null,null,null,null,{"$f":"IF(H243=\"Select Model\",\"\",combineACBLLength(J243,K243,L243,M243,N243))","v":""},{"$f":"IF(H243=\"Select Model\",\"\",combineACBWidth('Run Selections'!X243,O243,H243))","v":""},{"$f":" 'Run Selections'!BD243","v":0},{"$f":"'Run Selections'!AI243","v":""},{"$f":"'Run Selections'!AB243","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U243","v":2},{"$f":"'Run Selections'!V243","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F244=\"\",\"\",'Run Selections'!$F244)","v":""},null,{"$f":"'Run Selections'!T244","v":"Select Model"},{"$f":"'Run Selections'!L244","v":""},{"$f":"'Run Selections'!W244","v":4},null,null,null,null,null,{"$f":"IF(H244=\"Select Model\",\"\",combineACBLLength(J244,K244,L244,M244,N244))","v":""},{"$f":"IF(H244=\"Select Model\",\"\",combineACBWidth('Run Selections'!X244,O244,H244))","v":""},{"$f":" 'Run Selections'!BD244","v":0},{"$f":"'Run Selections'!AI244","v":""},{"$f":"'Run Selections'!AB244","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U244","v":2},{"$f":"'Run Selections'!V244","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F245=\"\",\"\",'Run Selections'!$F245)","v":""},null,{"$f":"'Run Selections'!T245","v":"Select Model"},{"$f":"'Run Selections'!L245","v":""},{"$f":"'Run Selections'!W245","v":4},null,null,null,null,null,{"$f":"IF(H245=\"Select Model\",\"\",combineACBLLength(J245,K245,L245,M245,N245))","v":""},{"$f":"IF(H245=\"Select Model\",\"\",combineACBWidth('Run Selections'!X245,O245,H245))","v":""},{"$f":" 'Run Selections'!BD245","v":0},{"$f":"'Run Selections'!AI245","v":""},{"$f":"'Run Selections'!AB245","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U245","v":2},{"$f":"'Run Selections'!V245","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F246=\"\",\"\",'Run Selections'!$F246)","v":""},null,{"$f":"'Run Selections'!T246","v":"Select Model"},{"$f":"'Run Selections'!L246","v":""},{"$f":"'Run Selections'!W246","v":4},null,null,null,null,null,{"$f":"IF(H246=\"Select Model\",\"\",combineACBLLength(J246,K246,L246,M246,N246))","v":""},{"$f":"IF(H246=\"Select Model\",\"\",combineACBWidth('Run Selections'!X246,O246,H246))","v":""},{"$f":" 'Run Selections'!BD246","v":0},{"$f":"'Run Selections'!AI246","v":""},{"$f":"'Run Selections'!AB246","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U246","v":2},{"$f":"'Run Selections'!V246","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F247=\"\",\"\",'Run Selections'!$F247)","v":""},null,{"$f":"'Run Selections'!T247","v":"Select Model"},{"$f":"'Run Selections'!L247","v":""},{"$f":"'Run Selections'!W247","v":4},null,null,null,null,null,{"$f":"IF(H247=\"Select Model\",\"\",combineACBLLength(J247,K247,L247,M247,N247))","v":""},{"$f":"IF(H247=\"Select Model\",\"\",combineACBWidth('Run Selections'!X247,O247,H247))","v":""},{"$f":" 'Run Selections'!BD247","v":0},{"$f":"'Run Selections'!AI247","v":""},{"$f":"'Run Selections'!AB247","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U247","v":2},{"$f":"'Run Selections'!V247","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F248=\"\",\"\",'Run Selections'!$F248)","v":""},null,{"$f":"'Run Selections'!T248","v":"Select Model"},{"$f":"'Run Selections'!L248","v":""},{"$f":"'Run Selections'!W248","v":4},null,null,null,null,null,{"$f":"IF(H248=\"Select Model\",\"\",combineACBLLength(J248,K248,L248,M248,N248))","v":""},{"$f":"IF(H248=\"Select Model\",\"\",combineACBWidth('Run Selections'!X248,O248,H248))","v":""},{"$f":" 'Run Selections'!BD248","v":0},{"$f":"'Run Selections'!AI248","v":""},{"$f":"'Run Selections'!AB248","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U248","v":2},{"$f":"'Run Selections'!V248","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F249=\"\",\"\",'Run Selections'!$F249)","v":""},null,{"$f":"'Run Selections'!T249","v":"Select Model"},{"$f":"'Run Selections'!L249","v":""},{"$f":"'Run Selections'!W249","v":4},null,null,null,null,null,{"$f":"IF(H249=\"Select Model\",\"\",combineACBLLength(J249,K249,L249,M249,N249))","v":""},{"$f":"IF(H249=\"Select Model\",\"\",combineACBWidth('Run Selections'!X249,O249,H249))","v":""},{"$f":" 'Run Selections'!BD249","v":0},{"$f":"'Run Selections'!AI249","v":""},{"$f":"'Run Selections'!AB249","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U249","v":2},{"$f":"'Run Selections'!V249","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F250=\"\",\"\",'Run Selections'!$F250)","v":""},null,{"$f":"'Run Selections'!T250","v":"Select Model"},{"$f":"'Run Selections'!L250","v":""},{"$f":"'Run Selections'!W250","v":4},null,null,null,null,null,{"$f":"IF(H250=\"Select Model\",\"\",combineACBLLength(J250,K250,L250,M250,N250))","v":""},{"$f":"IF(H250=\"Select Model\",\"\",combineACBWidth('Run Selections'!X250,O250,H250))","v":""},{"$f":" 'Run Selections'!BD250","v":0},{"$f":"'Run Selections'!AI250","v":""},{"$f":"'Run Selections'!AB250","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U250","v":2},{"$f":"'Run Selections'!V250","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F251=\"\",\"\",'Run Selections'!$F251)","v":""},null,{"$f":"'Run Selections'!T251","v":"Select Model"},{"$f":"'Run Selections'!L251","v":""},{"$f":"'Run Selections'!W251","v":4},null,null,null,null,null,{"$f":"IF(H251=\"Select Model\",\"\",combineACBLLength(J251,K251,L251,M251,N251))","v":""},{"$f":"IF(H251=\"Select Model\",\"\",combineACBWidth('Run Selections'!X251,O251,H251))","v":""},{"$f":" 'Run Selections'!BD251","v":0},{"$f":"'Run Selections'!AI251","v":""},{"$f":"'Run Selections'!AB251","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U251","v":2},{"$f":"'Run Selections'!V251","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F252=\"\",\"\",'Run Selections'!$F252)","v":""},null,{"$f":"'Run Selections'!T252","v":"Select Model"},{"$f":"'Run Selections'!L252","v":""},{"$f":"'Run Selections'!W252","v":4},null,null,null,null,null,{"$f":"IF(H252=\"Select Model\",\"\",combineACBLLength(J252,K252,L252,M252,N252))","v":""},{"$f":"IF(H252=\"Select Model\",\"\",combineACBWidth('Run Selections'!X252,O252,H252))","v":""},{"$f":" 'Run Selections'!BD252","v":0},{"$f":"'Run Selections'!AI252","v":""},{"$f":"'Run Selections'!AB252","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U252","v":2},{"$f":"'Run Selections'!V252","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F253=\"\",\"\",'Run Selections'!$F253)","v":""},null,{"$f":"'Run Selections'!T253","v":"Select Model"},{"$f":"'Run Selections'!L253","v":""},{"$f":"'Run Selections'!W253","v":4},null,null,null,null,null,{"$f":"IF(H253=\"Select Model\",\"\",combineACBLLength(J253,K253,L253,M253,N253))","v":""},{"$f":"IF(H253=\"Select Model\",\"\",combineACBWidth('Run Selections'!X253,O253,H253))","v":""},{"$f":" 'Run Selections'!BD253","v":0},{"$f":"'Run Selections'!AI253","v":""},{"$f":"'Run Selections'!AB253","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U253","v":2},{"$f":"'Run Selections'!V253","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F254=\"\",\"\",'Run Selections'!$F254)","v":""},null,{"$f":"'Run Selections'!T254","v":"Select Model"},{"$f":"'Run Selections'!L254","v":""},{"$f":"'Run Selections'!W254","v":4},null,null,null,null,null,{"$f":"IF(H254=\"Select Model\",\"\",combineACBLLength(J254,K254,L254,M254,N254))","v":""},{"$f":"IF(H254=\"Select Model\",\"\",combineACBWidth('Run Selections'!X254,O254,H254))","v":""},{"$f":" 'Run Selections'!BD254","v":0},{"$f":"'Run Selections'!AI254","v":""},{"$f":"'Run Selections'!AB254","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U254","v":2},{"$f":"'Run Selections'!V254","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F255=\"\",\"\",'Run Selections'!$F255)","v":""},null,{"$f":"'Run Selections'!T255","v":"Select Model"},{"$f":"'Run Selections'!L255","v":""},{"$f":"'Run Selections'!W255","v":4},null,null,null,null,null,{"$f":"IF(H255=\"Select Model\",\"\",combineACBLLength(J255,K255,L255,M255,N255))","v":""},{"$f":"IF(H255=\"Select Model\",\"\",combineACBWidth('Run Selections'!X255,O255,H255))","v":""},{"$f":" 'Run Selections'!BD255","v":0},{"$f":"'Run Selections'!AI255","v":""},{"$f":"'Run Selections'!AB255","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U255","v":2},{"$f":"'Run Selections'!V255","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F256=\"\",\"\",'Run Selections'!$F256)","v":""},null,{"$f":"'Run Selections'!T256","v":"Select Model"},{"$f":"'Run Selections'!L256","v":""},{"$f":"'Run Selections'!W256","v":4},null,null,null,null,null,{"$f":"IF(H256=\"Select Model\",\"\",combineACBLLength(J256,K256,L256,M256,N256))","v":""},{"$f":"IF(H256=\"Select Model\",\"\",combineACBWidth('Run Selections'!X256,O256,H256))","v":""},{"$f":" 'Run Selections'!BD256","v":0},{"$f":"'Run Selections'!AI256","v":""},{"$f":"'Run Selections'!AB256","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U256","v":2},{"$f":"'Run Selections'!V256","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F257=\"\",\"\",'Run Selections'!$F257)","v":""},null,{"$f":"'Run Selections'!T257","v":"Select Model"},{"$f":"'Run Selections'!L257","v":""},{"$f":"'Run Selections'!W257","v":4},null,null,null,null,null,{"$f":"IF(H257=\"Select Model\",\"\",combineACBLLength(J257,K257,L257,M257,N257))","v":""},{"$f":"IF(H257=\"Select Model\",\"\",combineACBWidth('Run Selections'!X257,O257,H257))","v":""},{"$f":" 'Run Selections'!BD257","v":0},{"$f":"'Run Selections'!AI257","v":""},{"$f":"'Run Selections'!AB257","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U257","v":2},{"$f":"'Run Selections'!V257","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F258=\"\",\"\",'Run Selections'!$F258)","v":""},null,{"$f":"'Run Selections'!T258","v":"Select Model"},{"$f":"'Run Selections'!L258","v":""},{"$f":"'Run Selections'!W258","v":4},null,null,null,null,null,{"$f":"IF(H258=\"Select Model\",\"\",combineACBLLength(J258,K258,L258,M258,N258))","v":""},{"$f":"IF(H258=\"Select Model\",\"\",combineACBWidth('Run Selections'!X258,O258,H258))","v":""},{"$f":" 'Run Selections'!BD258","v":0},{"$f":"'Run Selections'!AI258","v":""},{"$f":"'Run Selections'!AB258","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U258","v":2},{"$f":"'Run Selections'!V258","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F259=\"\",\"\",'Run Selections'!$F259)","v":""},null,{"$f":"'Run Selections'!T259","v":"Select Model"},{"$f":"'Run Selections'!L259","v":""},{"$f":"'Run Selections'!W259","v":4},null,null,null,null,null,{"$f":"IF(H259=\"Select Model\",\"\",combineACBLLength(J259,K259,L259,M259,N259))","v":""},{"$f":"IF(H259=\"Select Model\",\"\",combineACBWidth('Run Selections'!X259,O259,H259))","v":""},{"$f":" 'Run Selections'!BD259","v":0},{"$f":"'Run Selections'!AI259","v":""},{"$f":"'Run Selections'!AB259","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U259","v":2},{"$f":"'Run Selections'!V259","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F260=\"\",\"\",'Run Selections'!$F260)","v":""},null,{"$f":"'Run Selections'!T260","v":"Select Model"},{"$f":"'Run Selections'!L260","v":""},{"$f":"'Run Selections'!W260","v":4},null,null,null,null,null,{"$f":"IF(H260=\"Select Model\",\"\",combineACBLLength(J260,K260,L260,M260,N260))","v":""},{"$f":"IF(H260=\"Select Model\",\"\",combineACBWidth('Run Selections'!X260,O260,H260))","v":""},{"$f":" 'Run Selections'!BD260","v":0},{"$f":"'Run Selections'!AI260","v":""},{"$f":"'Run Selections'!AB260","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U260","v":2},{"$f":"'Run Selections'!V260","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F261=\"\",\"\",'Run Selections'!$F261)","v":""},null,{"$f":"'Run Selections'!T261","v":"Select Model"},{"$f":"'Run Selections'!L261","v":""},{"$f":"'Run Selections'!W261","v":4},null,null,null,null,null,{"$f":"IF(H261=\"Select Model\",\"\",combineACBLLength(J261,K261,L261,M261,N261))","v":""},{"$f":"IF(H261=\"Select Model\",\"\",combineACBWidth('Run Selections'!X261,O261,H261))","v":""},{"$f":" 'Run Selections'!BD261","v":0},{"$f":"'Run Selections'!AI261","v":""},{"$f":"'Run Selections'!AB261","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U261","v":2},{"$f":"'Run Selections'!V261","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F262=\"\",\"\",'Run Selections'!$F262)","v":""},null,{"$f":"'Run Selections'!T262","v":"Select Model"},{"$f":"'Run Selections'!L262","v":""},{"$f":"'Run Selections'!W262","v":4},null,null,null,null,null,{"$f":"IF(H262=\"Select Model\",\"\",combineACBLLength(J262,K262,L262,M262,N262))","v":""},{"$f":"IF(H262=\"Select Model\",\"\",combineACBWidth('Run Selections'!X262,O262,H262))","v":""},{"$f":" 'Run Selections'!BD262","v":0},{"$f":"'Run Selections'!AI262","v":""},{"$f":"'Run Selections'!AB262","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U262","v":2},{"$f":"'Run Selections'!V262","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F263=\"\",\"\",'Run Selections'!$F263)","v":""},null,{"$f":"'Run Selections'!T263","v":"Select Model"},{"$f":"'Run Selections'!L263","v":""},{"$f":"'Run Selections'!W263","v":4},null,null,null,null,null,{"$f":"IF(H263=\"Select Model\",\"\",combineACBLLength(J263,K263,L263,M263,N263))","v":""},{"$f":"IF(H263=\"Select Model\",\"\",combineACBWidth('Run Selections'!X263,O263,H263))","v":""},{"$f":" 'Run Selections'!BD263","v":0},{"$f":"'Run Selections'!AI263","v":""},{"$f":"'Run Selections'!AB263","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U263","v":2},{"$f":"'Run Selections'!V263","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F264=\"\",\"\",'Run Selections'!$F264)","v":""},null,{"$f":"'Run Selections'!T264","v":"Select Model"},{"$f":"'Run Selections'!L264","v":""},{"$f":"'Run Selections'!W264","v":4},null,null,null,null,null,{"$f":"IF(H264=\"Select Model\",\"\",combineACBLLength(J264,K264,L264,M264,N264))","v":""},{"$f":"IF(H264=\"Select Model\",\"\",combineACBWidth('Run Selections'!X264,O264,H264))","v":""},{"$f":" 'Run Selections'!BD264","v":0},{"$f":"'Run Selections'!AI264","v":""},{"$f":"'Run Selections'!AB264","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U264","v":2},{"$f":"'Run Selections'!V264","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F265=\"\",\"\",'Run Selections'!$F265)","v":""},null,{"$f":"'Run Selections'!T265","v":"Select Model"},{"$f":"'Run Selections'!L265","v":""},{"$f":"'Run Selections'!W265","v":4},null,null,null,null,null,{"$f":"IF(H265=\"Select Model\",\"\",combineACBLLength(J265,K265,L265,M265,N265))","v":""},{"$f":"IF(H265=\"Select Model\",\"\",combineACBWidth('Run Selections'!X265,O265,H265))","v":""},{"$f":" 'Run Selections'!BD265","v":0},{"$f":"'Run Selections'!AI265","v":""},{"$f":"'Run Selections'!AB265","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U265","v":2},{"$f":"'Run Selections'!V265","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F266=\"\",\"\",'Run Selections'!$F266)","v":""},null,{"$f":"'Run Selections'!T266","v":"Select Model"},{"$f":"'Run Selections'!L266","v":""},{"$f":"'Run Selections'!W266","v":4},null,null,null,null,null,{"$f":"IF(H266=\"Select Model\",\"\",combineACBLLength(J266,K266,L266,M266,N266))","v":""},{"$f":"IF(H266=\"Select Model\",\"\",combineACBWidth('Run Selections'!X266,O266,H266))","v":""},{"$f":" 'Run Selections'!BD266","v":0},{"$f":"'Run Selections'!AI266","v":""},{"$f":"'Run Selections'!AB266","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U266","v":2},{"$f":"'Run Selections'!V266","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F267=\"\",\"\",'Run Selections'!$F267)","v":""},null,{"$f":"'Run Selections'!T267","v":"Select Model"},{"$f":"'Run Selections'!L267","v":""},{"$f":"'Run Selections'!W267","v":4},null,null,null,null,null,{"$f":"IF(H267=\"Select Model\",\"\",combineACBLLength(J267,K267,L267,M267,N267))","v":""},{"$f":"IF(H267=\"Select Model\",\"\",combineACBWidth('Run Selections'!X267,O267,H267))","v":""},{"$f":" 'Run Selections'!BD267","v":0},{"$f":"'Run Selections'!AI267","v":""},{"$f":"'Run Selections'!AB267","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U267","v":2},{"$f":"'Run Selections'!V267","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F268=\"\",\"\",'Run Selections'!$F268)","v":""},null,{"$f":"'Run Selections'!T268","v":"Select Model"},{"$f":"'Run Selections'!L268","v":""},{"$f":"'Run Selections'!W268","v":4},null,null,null,null,null,{"$f":"IF(H268=\"Select Model\",\"\",combineACBLLength(J268,K268,L268,M268,N268))","v":""},{"$f":"IF(H268=\"Select Model\",\"\",combineACBWidth('Run Selections'!X268,O268,H268))","v":""},{"$f":" 'Run Selections'!BD268","v":0},{"$f":"'Run Selections'!AI268","v":""},{"$f":"'Run Selections'!AB268","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U268","v":2},{"$f":"'Run Selections'!V268","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F269=\"\",\"\",'Run Selections'!$F269)","v":""},null,{"$f":"'Run Selections'!T269","v":"Select Model"},{"$f":"'Run Selections'!L269","v":""},{"$f":"'Run Selections'!W269","v":4},null,null,null,null,null,{"$f":"IF(H269=\"Select Model\",\"\",combineACBLLength(J269,K269,L269,M269,N269))","v":""},{"$f":"IF(H269=\"Select Model\",\"\",combineACBWidth('Run Selections'!X269,O269,H269))","v":""},{"$f":" 'Run Selections'!BD269","v":0},{"$f":"'Run Selections'!AI269","v":""},{"$f":"'Run Selections'!AB269","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U269","v":2},{"$f":"'Run Selections'!V269","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F270=\"\",\"\",'Run Selections'!$F270)","v":""},null,{"$f":"'Run Selections'!T270","v":"Select Model"},{"$f":"'Run Selections'!L270","v":""},{"$f":"'Run Selections'!W270","v":4},null,null,null,null,null,{"$f":"IF(H270=\"Select Model\",\"\",combineACBLLength(J270,K270,L270,M270,N270))","v":""},{"$f":"IF(H270=\"Select Model\",\"\",combineACBWidth('Run Selections'!X270,O270,H270))","v":""},{"$f":" 'Run Selections'!BD270","v":0},{"$f":"'Run Selections'!AI270","v":""},{"$f":"'Run Selections'!AB270","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U270","v":2},{"$f":"'Run Selections'!V270","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F271=\"\",\"\",'Run Selections'!$F271)","v":""},null,{"$f":"'Run Selections'!T271","v":"Select Model"},{"$f":"'Run Selections'!L271","v":""},{"$f":"'Run Selections'!W271","v":4},null,null,null,null,null,{"$f":"IF(H271=\"Select Model\",\"\",combineACBLLength(J271,K271,L271,M271,N271))","v":""},{"$f":"IF(H271=\"Select Model\",\"\",combineACBWidth('Run Selections'!X271,O271,H271))","v":""},{"$f":" 'Run Selections'!BD271","v":0},{"$f":"'Run Selections'!AI271","v":""},{"$f":"'Run Selections'!AB271","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U271","v":2},{"$f":"'Run Selections'!V271","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F272=\"\",\"\",'Run Selections'!$F272)","v":""},null,{"$f":"'Run Selections'!T272","v":"Select Model"},{"$f":"'Run Selections'!L272","v":""},{"$f":"'Run Selections'!W272","v":4},null,null,null,null,null,{"$f":"IF(H272=\"Select Model\",\"\",combineACBLLength(J272,K272,L272,M272,N272))","v":""},{"$f":"IF(H272=\"Select Model\",\"\",combineACBWidth('Run Selections'!X272,O272,H272))","v":""},{"$f":" 'Run Selections'!BD272","v":0},{"$f":"'Run Selections'!AI272","v":""},{"$f":"'Run Selections'!AB272","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U272","v":2},{"$f":"'Run Selections'!V272","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F273=\"\",\"\",'Run Selections'!$F273)","v":""},null,{"$f":"'Run Selections'!T273","v":"Select Model"},{"$f":"'Run Selections'!L273","v":""},{"$f":"'Run Selections'!W273","v":4},null,null,null,null,null,{"$f":"IF(H273=\"Select Model\",\"\",combineACBLLength(J273,K273,L273,M273,N273))","v":""},{"$f":"IF(H273=\"Select Model\",\"\",combineACBWidth('Run Selections'!X273,O273,H273))","v":""},{"$f":" 'Run Selections'!BD273","v":0},{"$f":"'Run Selections'!AI273","v":""},{"$f":"'Run Selections'!AB273","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U273","v":2},{"$f":"'Run Selections'!V273","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F274=\"\",\"\",'Run Selections'!$F274)","v":""},null,{"$f":"'Run Selections'!T274","v":"Select Model"},{"$f":"'Run Selections'!L274","v":""},{"$f":"'Run Selections'!W274","v":4},null,null,null,null,null,{"$f":"IF(H274=\"Select Model\",\"\",combineACBLLength(J274,K274,L274,M274,N274))","v":""},{"$f":"IF(H274=\"Select Model\",\"\",combineACBWidth('Run Selections'!X274,O274,H274))","v":""},{"$f":" 'Run Selections'!BD274","v":0},{"$f":"'Run Selections'!AI274","v":""},{"$f":"'Run Selections'!AB274","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U274","v":2},{"$f":"'Run Selections'!V274","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F275=\"\",\"\",'Run Selections'!$F275)","v":""},null,{"$f":"'Run Selections'!T275","v":"Select Model"},{"$f":"'Run Selections'!L275","v":""},{"$f":"'Run Selections'!W275","v":4},null,null,null,null,null,{"$f":"IF(H275=\"Select Model\",\"\",combineACBLLength(J275,K275,L275,M275,N275))","v":""},{"$f":"IF(H275=\"Select Model\",\"\",combineACBWidth('Run Selections'!X275,O275,H275))","v":""},{"$f":" 'Run Selections'!BD275","v":0},{"$f":"'Run Selections'!AI275","v":""},{"$f":"'Run Selections'!AB275","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U275","v":2},{"$f":"'Run Selections'!V275","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F276=\"\",\"\",'Run Selections'!$F276)","v":""},null,{"$f":"'Run Selections'!T276","v":"Select Model"},{"$f":"'Run Selections'!L276","v":""},{"$f":"'Run Selections'!W276","v":4},null,null,null,null,null,{"$f":"IF(H276=\"Select Model\",\"\",combineACBLLength(J276,K276,L276,M276,N276))","v":""},{"$f":"IF(H276=\"Select Model\",\"\",combineACBWidth('Run Selections'!X276,O276,H276))","v":""},{"$f":" 'Run Selections'!BD276","v":0},{"$f":"'Run Selections'!AI276","v":""},{"$f":"'Run Selections'!AB276","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U276","v":2},{"$f":"'Run Selections'!V276","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F277=\"\",\"\",'Run Selections'!$F277)","v":""},null,{"$f":"'Run Selections'!T277","v":"Select Model"},{"$f":"'Run Selections'!L277","v":""},{"$f":"'Run Selections'!W277","v":4},null,null,null,null,null,{"$f":"IF(H277=\"Select Model\",\"\",combineACBLLength(J277,K277,L277,M277,N277))","v":""},{"$f":"IF(H277=\"Select Model\",\"\",combineACBWidth('Run Selections'!X277,O277,H277))","v":""},{"$f":" 'Run Selections'!BD277","v":0},{"$f":"'Run Selections'!AI277","v":""},{"$f":"'Run Selections'!AB277","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U277","v":2},{"$f":"'Run Selections'!V277","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F278=\"\",\"\",'Run Selections'!$F278)","v":""},null,{"$f":"'Run Selections'!T278","v":"Select Model"},{"$f":"'Run Selections'!L278","v":""},{"$f":"'Run Selections'!W278","v":4},null,null,null,null,null,{"$f":"IF(H278=\"Select Model\",\"\",combineACBLLength(J278,K278,L278,M278,N278))","v":""},{"$f":"IF(H278=\"Select Model\",\"\",combineACBWidth('Run Selections'!X278,O278,H278))","v":""},{"$f":" 'Run Selections'!BD278","v":0},{"$f":"'Run Selections'!AI278","v":""},{"$f":"'Run Selections'!AB278","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U278","v":2},{"$f":"'Run Selections'!V278","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F279=\"\",\"\",'Run Selections'!$F279)","v":""},null,{"$f":"'Run Selections'!T279","v":"Select Model"},{"$f":"'Run Selections'!L279","v":""},{"$f":"'Run Selections'!W279","v":4},null,null,null,null,null,{"$f":"IF(H279=\"Select Model\",\"\",combineACBLLength(J279,K279,L279,M279,N279))","v":""},{"$f":"IF(H279=\"Select Model\",\"\",combineACBWidth('Run Selections'!X279,O279,H279))","v":""},{"$f":" 'Run Selections'!BD279","v":0},{"$f":"'Run Selections'!AI279","v":""},{"$f":"'Run Selections'!AB279","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U279","v":2},{"$f":"'Run Selections'!V279","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F280=\"\",\"\",'Run Selections'!$F280)","v":""},null,{"$f":"'Run Selections'!T280","v":"Select Model"},{"$f":"'Run Selections'!L280","v":""},{"$f":"'Run Selections'!W280","v":4},null,null,null,null,null,{"$f":"IF(H280=\"Select Model\",\"\",combineACBLLength(J280,K280,L280,M280,N280))","v":""},{"$f":"IF(H280=\"Select Model\",\"\",combineACBWidth('Run Selections'!X280,O280,H280))","v":""},{"$f":" 'Run Selections'!BD280","v":0},{"$f":"'Run Selections'!AI280","v":""},{"$f":"'Run Selections'!AB280","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U280","v":2},{"$f":"'Run Selections'!V280","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F281=\"\",\"\",'Run Selections'!$F281)","v":""},null,{"$f":"'Run Selections'!T281","v":"Select Model"},{"$f":"'Run Selections'!L281","v":""},{"$f":"'Run Selections'!W281","v":4},null,null,null,null,null,{"$f":"IF(H281=\"Select Model\",\"\",combineACBLLength(J281,K281,L281,M281,N281))","v":""},{"$f":"IF(H281=\"Select Model\",\"\",combineACBWidth('Run Selections'!X281,O281,H281))","v":""},{"$f":" 'Run Selections'!BD281","v":0},{"$f":"'Run Selections'!AI281","v":""},{"$f":"'Run Selections'!AB281","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U281","v":2},{"$f":"'Run Selections'!V281","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F282=\"\",\"\",'Run Selections'!$F282)","v":""},null,{"$f":"'Run Selections'!T282","v":"Select Model"},{"$f":"'Run Selections'!L282","v":""},{"$f":"'Run Selections'!W282","v":4},null,null,null,null,null,{"$f":"IF(H282=\"Select Model\",\"\",combineACBLLength(J282,K282,L282,M282,N282))","v":""},{"$f":"IF(H282=\"Select Model\",\"\",combineACBWidth('Run Selections'!X282,O282,H282))","v":""},{"$f":" 'Run Selections'!BD282","v":0},{"$f":"'Run Selections'!AI282","v":""},{"$f":"'Run Selections'!AB282","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U282","v":2},{"$f":"'Run Selections'!V282","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F283=\"\",\"\",'Run Selections'!$F283)","v":""},null,{"$f":"'Run Selections'!T283","v":"Select Model"},{"$f":"'Run Selections'!L283","v":""},{"$f":"'Run Selections'!W283","v":4},null,null,null,null,null,{"$f":"IF(H283=\"Select Model\",\"\",combineACBLLength(J283,K283,L283,M283,N283))","v":""},{"$f":"IF(H283=\"Select Model\",\"\",combineACBWidth('Run Selections'!X283,O283,H283))","v":""},{"$f":" 'Run Selections'!BD283","v":0},{"$f":"'Run Selections'!AI283","v":""},{"$f":"'Run Selections'!AB283","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U283","v":2},{"$f":"'Run Selections'!V283","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F284=\"\",\"\",'Run Selections'!$F284)","v":""},null,{"$f":"'Run Selections'!T284","v":"Select Model"},{"$f":"'Run Selections'!L284","v":""},{"$f":"'Run Selections'!W284","v":4},null,null,null,null,null,{"$f":"IF(H284=\"Select Model\",\"\",combineACBLLength(J284,K284,L284,M284,N284))","v":""},{"$f":"IF(H284=\"Select Model\",\"\",combineACBWidth('Run Selections'!X284,O284,H284))","v":""},{"$f":" 'Run Selections'!BD284","v":0},{"$f":"'Run Selections'!AI284","v":""},{"$f":"'Run Selections'!AB284","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U284","v":2},{"$f":"'Run Selections'!V284","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F285=\"\",\"\",'Run Selections'!$F285)","v":""},null,{"$f":"'Run Selections'!T285","v":"Select Model"},{"$f":"'Run Selections'!L285","v":""},{"$f":"'Run Selections'!W285","v":4},null,null,null,null,null,{"$f":"IF(H285=\"Select Model\",\"\",combineACBLLength(J285,K285,L285,M285,N285))","v":""},{"$f":"IF(H285=\"Select Model\",\"\",combineACBWidth('Run Selections'!X285,O285,H285))","v":""},{"$f":" 'Run Selections'!BD285","v":0},{"$f":"'Run Selections'!AI285","v":""},{"$f":"'Run Selections'!AB285","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U285","v":2},{"$f":"'Run Selections'!V285","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F286=\"\",\"\",'Run Selections'!$F286)","v":""},null,{"$f":"'Run Selections'!T286","v":"Select Model"},{"$f":"'Run Selections'!L286","v":""},{"$f":"'Run Selections'!W286","v":4},null,null,null,null,null,{"$f":"IF(H286=\"Select Model\",\"\",combineACBLLength(J286,K286,L286,M286,N286))","v":""},{"$f":"IF(H286=\"Select Model\",\"\",combineACBWidth('Run Selections'!X286,O286,H286))","v":""},{"$f":" 'Run Selections'!BD286","v":0},{"$f":"'Run Selections'!AI286","v":""},{"$f":"'Run Selections'!AB286","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U286","v":2},{"$f":"'Run Selections'!V286","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F287=\"\",\"\",'Run Selections'!$F287)","v":""},null,{"$f":"'Run Selections'!T287","v":"Select Model"},{"$f":"'Run Selections'!L287","v":""},{"$f":"'Run Selections'!W287","v":4},null,null,null,null,null,{"$f":"IF(H287=\"Select Model\",\"\",combineACBLLength(J287,K287,L287,M287,N287))","v":""},{"$f":"IF(H287=\"Select Model\",\"\",combineACBWidth('Run Selections'!X287,O287,H287))","v":""},{"$f":" 'Run Selections'!BD287","v":0},{"$f":"'Run Selections'!AI287","v":""},{"$f":"'Run Selections'!AB287","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U287","v":2},{"$f":"'Run Selections'!V287","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F288=\"\",\"\",'Run Selections'!$F288)","v":""},null,{"$f":"'Run Selections'!T288","v":"Select Model"},{"$f":"'Run Selections'!L288","v":""},{"$f":"'Run Selections'!W288","v":4},null,null,null,null,null,{"$f":"IF(H288=\"Select Model\",\"\",combineACBLLength(J288,K288,L288,M288,N288))","v":""},{"$f":"IF(H288=\"Select Model\",\"\",combineACBWidth('Run Selections'!X288,O288,H288))","v":""},{"$f":" 'Run Selections'!BD288","v":0},{"$f":"'Run Selections'!AI288","v":""},{"$f":"'Run Selections'!AB288","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U288","v":2},{"$f":"'Run Selections'!V288","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F289=\"\",\"\",'Run Selections'!$F289)","v":""},null,{"$f":"'Run Selections'!T289","v":"Select Model"},{"$f":"'Run Selections'!L289","v":""},{"$f":"'Run Selections'!W289","v":4},null,null,null,null,null,{"$f":"IF(H289=\"Select Model\",\"\",combineACBLLength(J289,K289,L289,M289,N289))","v":""},{"$f":"IF(H289=\"Select Model\",\"\",combineACBWidth('Run Selections'!X289,O289,H289))","v":""},{"$f":" 'Run Selections'!BD289","v":0},{"$f":"'Run Selections'!AI289","v":""},{"$f":"'Run Selections'!AB289","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U289","v":2},{"$f":"'Run Selections'!V289","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F290=\"\",\"\",'Run Selections'!$F290)","v":""},null,{"$f":"'Run Selections'!T290","v":"Select Model"},{"$f":"'Run Selections'!L290","v":""},{"$f":"'Run Selections'!W290","v":4},null,null,null,null,null,{"$f":"IF(H290=\"Select Model\",\"\",combineACBLLength(J290,K290,L290,M290,N290))","v":""},{"$f":"IF(H290=\"Select Model\",\"\",combineACBWidth('Run Selections'!X290,O290,H290))","v":""},{"$f":" 'Run Selections'!BD290","v":0},{"$f":"'Run Selections'!AI290","v":""},{"$f":"'Run Selections'!AB290","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U290","v":2},{"$f":"'Run Selections'!V290","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F291=\"\",\"\",'Run Selections'!$F291)","v":""},null,{"$f":"'Run Selections'!T291","v":"Select Model"},{"$f":"'Run Selections'!L291","v":""},{"$f":"'Run Selections'!W291","v":4},null,null,null,null,null,{"$f":"IF(H291=\"Select Model\",\"\",combineACBLLength(J291,K291,L291,M291,N291))","v":""},{"$f":"IF(H291=\"Select Model\",\"\",combineACBWidth('Run Selections'!X291,O291,H291))","v":""},{"$f":" 'Run Selections'!BD291","v":0},{"$f":"'Run Selections'!AI291","v":""},{"$f":"'Run Selections'!AB291","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U291","v":2},{"$f":"'Run Selections'!V291","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F292=\"\",\"\",'Run Selections'!$F292)","v":""},null,{"$f":"'Run Selections'!T292","v":"Select Model"},{"$f":"'Run Selections'!L292","v":""},{"$f":"'Run Selections'!W292","v":4},null,null,null,null,null,{"$f":"IF(H292=\"Select Model\",\"\",combineACBLLength(J292,K292,L292,M292,N292))","v":""},{"$f":"IF(H292=\"Select Model\",\"\",combineACBWidth('Run Selections'!X292,O292,H292))","v":""},{"$f":" 'Run Selections'!BD292","v":0},{"$f":"'Run Selections'!AI292","v":""},{"$f":"'Run Selections'!AB292","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U292","v":2},{"$f":"'Run Selections'!V292","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F293=\"\",\"\",'Run Selections'!$F293)","v":""},null,{"$f":"'Run Selections'!T293","v":"Select Model"},{"$f":"'Run Selections'!L293","v":""},{"$f":"'Run Selections'!W293","v":4},null,null,null,null,null,{"$f":"IF(H293=\"Select Model\",\"\",combineACBLLength(J293,K293,L293,M293,N293))","v":""},{"$f":"IF(H293=\"Select Model\",\"\",combineACBWidth('Run Selections'!X293,O293,H293))","v":""},{"$f":" 'Run Selections'!BD293","v":0},{"$f":"'Run Selections'!AI293","v":""},{"$f":"'Run Selections'!AB293","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U293","v":2},{"$f":"'Run Selections'!V293","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F294=\"\",\"\",'Run Selections'!$F294)","v":""},null,{"$f":"'Run Selections'!T294","v":"Select Model"},{"$f":"'Run Selections'!L294","v":""},{"$f":"'Run Selections'!W294","v":4},null,null,null,null,null,{"$f":"IF(H294=\"Select Model\",\"\",combineACBLLength(J294,K294,L294,M294,N294))","v":""},{"$f":"IF(H294=\"Select Model\",\"\",combineACBWidth('Run Selections'!X294,O294,H294))","v":""},{"$f":" 'Run Selections'!BD294","v":0},{"$f":"'Run Selections'!AI294","v":""},{"$f":"'Run Selections'!AB294","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U294","v":2},{"$f":"'Run Selections'!V294","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F295=\"\",\"\",'Run Selections'!$F295)","v":""},null,{"$f":"'Run Selections'!T295","v":"Select Model"},{"$f":"'Run Selections'!L295","v":""},{"$f":"'Run Selections'!W295","v":4},null,null,null,null,null,{"$f":"IF(H295=\"Select Model\",\"\",combineACBLLength(J295,K295,L295,M295,N295))","v":""},{"$f":"IF(H295=\"Select Model\",\"\",combineACBWidth('Run Selections'!X295,O295,H295))","v":""},{"$f":" 'Run Selections'!BD295","v":0},{"$f":"'Run Selections'!AI295","v":""},{"$f":"'Run Selections'!AB295","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U295","v":2},{"$f":"'Run Selections'!V295","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F296=\"\",\"\",'Run Selections'!$F296)","v":""},null,{"$f":"'Run Selections'!T296","v":"Select Model"},{"$f":"'Run Selections'!L296","v":""},{"$f":"'Run Selections'!W296","v":4},null,null,null,null,null,{"$f":"IF(H296=\"Select Model\",\"\",combineACBLLength(J296,K296,L296,M296,N296))","v":""},{"$f":"IF(H296=\"Select Model\",\"\",combineACBWidth('Run Selections'!X296,O296,H296))","v":""},{"$f":" 'Run Selections'!BD296","v":0},{"$f":"'Run Selections'!AI296","v":""},{"$f":"'Run Selections'!AB296","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U296","v":2},{"$f":"'Run Selections'!V296","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F297=\"\",\"\",'Run Selections'!$F297)","v":""},null,{"$f":"'Run Selections'!T297","v":"Select Model"},{"$f":"'Run Selections'!L297","v":""},{"$f":"'Run Selections'!W297","v":4},null,null,null,null,null,{"$f":"IF(H297=\"Select Model\",\"\",combineACBLLength(J297,K297,L297,M297,N297))","v":""},{"$f":"IF(H297=\"Select Model\",\"\",combineACBWidth('Run Selections'!X297,O297,H297))","v":""},{"$f":" 'Run Selections'!BD297","v":0},{"$f":"'Run Selections'!AI297","v":""},{"$f":"'Run Selections'!AB297","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U297","v":2},{"$f":"'Run Selections'!V297","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F298=\"\",\"\",'Run Selections'!$F298)","v":""},null,{"$f":"'Run Selections'!T298","v":"Select Model"},{"$f":"'Run Selections'!L298","v":""},{"$f":"'Run Selections'!W298","v":4},null,null,null,null,null,{"$f":"IF(H298=\"Select Model\",\"\",combineACBLLength(J298,K298,L298,M298,N298))","v":""},{"$f":"IF(H298=\"Select Model\",\"\",combineACBWidth('Run Selections'!X298,O298,H298))","v":""},{"$f":" 'Run Selections'!BD298","v":0},{"$f":"'Run Selections'!AI298","v":""},{"$f":"'Run Selections'!AB298","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U298","v":2},{"$f":"'Run Selections'!V298","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F299=\"\",\"\",'Run Selections'!$F299)","v":""},null,{"$f":"'Run Selections'!T299","v":"Select Model"},{"$f":"'Run Selections'!L299","v":""},{"$f":"'Run Selections'!W299","v":4},null,null,null,null,null,{"$f":"IF(H299=\"Select Model\",\"\",combineACBLLength(J299,K299,L299,M299,N299))","v":""},{"$f":"IF(H299=\"Select Model\",\"\",combineACBWidth('Run Selections'!X299,O299,H299))","v":""},{"$f":" 'Run Selections'!BD299","v":0},{"$f":"'Run Selections'!AI299","v":""},{"$f":"'Run Selections'!AB299","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U299","v":2},{"$f":"'Run Selections'!V299","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F300=\"\",\"\",'Run Selections'!$F300)","v":""},null,{"$f":"'Run Selections'!T300","v":"Select Model"},{"$f":"'Run Selections'!L300","v":""},{"$f":"'Run Selections'!W300","v":4},null,null,null,null,null,{"$f":"IF(H300=\"Select Model\",\"\",combineACBLLength(J300,K300,L300,M300,N300))","v":""},{"$f":"IF(H300=\"Select Model\",\"\",combineACBWidth('Run Selections'!X300,O300,H300))","v":""},{"$f":" 'Run Selections'!BD300","v":0},{"$f":"'Run Selections'!AI300","v":""},{"$f":"'Run Selections'!AB300","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U300","v":2},{"$f":"'Run Selections'!V300","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F301=\"\",\"\",'Run Selections'!$F301)","v":""},null,{"$f":"'Run Selections'!T301","v":"Select Model"},{"$f":"'Run Selections'!L301","v":""},{"$f":"'Run Selections'!W301","v":4},null,null,null,null,null,{"$f":"IF(H301=\"Select Model\",\"\",combineACBLLength(J301,K301,L301,M301,N301))","v":""},{"$f":"IF(H301=\"Select Model\",\"\",combineACBWidth('Run Selections'!X301,O301,H301))","v":""},{"$f":" 'Run Selections'!BD301","v":0},{"$f":"'Run Selections'!AI301","v":""},{"$f":"'Run Selections'!AB301","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U301","v":2},{"$f":"'Run Selections'!V301","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F302=\"\",\"\",'Run Selections'!$F302)","v":""},null,{"$f":"'Run Selections'!T302","v":"Select Model"},{"$f":"'Run Selections'!L302","v":""},{"$f":"'Run Selections'!W302","v":4},null,null,null,null,null,{"$f":"IF(H302=\"Select Model\",\"\",combineACBLLength(J302,K302,L302,M302,N302))","v":""},{"$f":"IF(H302=\"Select Model\",\"\",combineACBWidth('Run Selections'!X302,O302,H302))","v":""},{"$f":" 'Run Selections'!BD302","v":0},{"$f":"'Run Selections'!AI302","v":""},{"$f":"'Run Selections'!AB302","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U302","v":2},{"$f":"'Run Selections'!V302","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F303=\"\",\"\",'Run Selections'!$F303)","v":""},null,{"$f":"'Run Selections'!T303","v":"Select Model"},{"$f":"'Run Selections'!L303","v":""},{"$f":"'Run Selections'!W303","v":4},null,null,null,null,null,{"$f":"IF(H303=\"Select Model\",\"\",combineACBLLength(J303,K303,L303,M303,N303))","v":""},{"$f":"IF(H303=\"Select Model\",\"\",combineACBWidth('Run Selections'!X303,O303,H303))","v":""},{"$f":" 'Run Selections'!BD303","v":0},{"$f":"'Run Selections'!AI303","v":""},{"$f":"'Run Selections'!AB303","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U303","v":2},{"$f":"'Run Selections'!V303","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F304=\"\",\"\",'Run Selections'!$F304)","v":""},null,{"$f":"'Run Selections'!T304","v":"Select Model"},{"$f":"'Run Selections'!L304","v":""},{"$f":"'Run Selections'!W304","v":4},null,null,null,null,null,{"$f":"IF(H304=\"Select Model\",\"\",combineACBLLength(J304,K304,L304,M304,N304))","v":""},{"$f":"IF(H304=\"Select Model\",\"\",combineACBWidth('Run Selections'!X304,O304,H304))","v":""},{"$f":" 'Run Selections'!BD304","v":0},{"$f":"'Run Selections'!AI304","v":""},{"$f":"'Run Selections'!AB304","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U304","v":2},{"$f":"'Run Selections'!V304","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F305=\"\",\"\",'Run Selections'!$F305)","v":""},null,{"$f":"'Run Selections'!T305","v":"Select Model"},{"$f":"'Run Selections'!L305","v":""},{"$f":"'Run Selections'!W305","v":4},null,null,null,null,null,{"$f":"IF(H305=\"Select Model\",\"\",combineACBLLength(J305,K305,L305,M305,N305))","v":""},{"$f":"IF(H305=\"Select Model\",\"\",combineACBWidth('Run Selections'!X305,O305,H305))","v":""},{"$f":" 'Run Selections'!BD305","v":0},{"$f":"'Run Selections'!AI305","v":""},{"$f":"'Run Selections'!AB305","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U305","v":2},{"$f":"'Run Selections'!V305","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F306=\"\",\"\",'Run Selections'!$F306)","v":""},null,{"$f":"'Run Selections'!T306","v":"Select Model"},{"$f":"'Run Selections'!L306","v":""},{"$f":"'Run Selections'!W306","v":4},null,null,null,null,null,{"$f":"IF(H306=\"Select Model\",\"\",combineACBLLength(J306,K306,L306,M306,N306))","v":""},{"$f":"IF(H306=\"Select Model\",\"\",combineACBWidth('Run Selections'!X306,O306,H306))","v":""},{"$f":" 'Run Selections'!BD306","v":0},{"$f":"'Run Selections'!AI306","v":""},{"$f":"'Run Selections'!AB306","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U306","v":2},{"$f":"'Run Selections'!V306","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F307=\"\",\"\",'Run Selections'!$F307)","v":""},null,{"$f":"'Run Selections'!T307","v":"Select Model"},{"$f":"'Run Selections'!L307","v":""},{"$f":"'Run Selections'!W307","v":4},null,null,null,null,null,{"$f":"IF(H307=\"Select Model\",\"\",combineACBLLength(J307,K307,L307,M307,N307))","v":""},{"$f":"IF(H307=\"Select Model\",\"\",combineACBWidth('Run Selections'!X307,O307,H307))","v":""},{"$f":" 'Run Selections'!BD307","v":0},{"$f":"'Run Selections'!AI307","v":""},{"$f":"'Run Selections'!AB307","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U307","v":2},{"$f":"'Run Selections'!V307","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F308=\"\",\"\",'Run Selections'!$F308)","v":""},null,{"$f":"'Run Selections'!T308","v":"Select Model"},{"$f":"'Run Selections'!L308","v":""},{"$f":"'Run Selections'!W308","v":4},null,null,null,null,null,{"$f":"IF(H308=\"Select Model\",\"\",combineACBLLength(J308,K308,L308,M308,N308))","v":""},{"$f":"IF(H308=\"Select Model\",\"\",combineACBWidth('Run Selections'!X308,O308,H308))","v":""},{"$f":" 'Run Selections'!BD308","v":0},{"$f":"'Run Selections'!AI308","v":""},{"$f":"'Run Selections'!AB308","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U308","v":2},{"$f":"'Run Selections'!V308","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F309=\"\",\"\",'Run Selections'!$F309)","v":""},null,{"$f":"'Run Selections'!T309","v":"Select Model"},{"$f":"'Run Selections'!L309","v":""},{"$f":"'Run Selections'!W309","v":4},null,null,null,null,null,{"$f":"IF(H309=\"Select Model\",\"\",combineACBLLength(J309,K309,L309,M309,N309))","v":""},{"$f":"IF(H309=\"Select Model\",\"\",combineACBWidth('Run Selections'!X309,O309,H309))","v":""},{"$f":" 'Run Selections'!BD309","v":0},{"$f":"'Run Selections'!AI309","v":""},{"$f":"'Run Selections'!AB309","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U309","v":2},{"$f":"'Run Selections'!V309","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F310=\"\",\"\",'Run Selections'!$F310)","v":""},null,{"$f":"'Run Selections'!T310","v":"Select Model"},{"$f":"'Run Selections'!L310","v":""},{"$f":"'Run Selections'!W310","v":4},null,null,null,null,null,{"$f":"IF(H310=\"Select Model\",\"\",combineACBLLength(J310,K310,L310,M310,N310))","v":""},{"$f":"IF(H310=\"Select Model\",\"\",combineACBWidth('Run Selections'!X310,O310,H310))","v":""},{"$f":" 'Run Selections'!BD310","v":0},{"$f":"'Run Selections'!AI310","v":""},{"$f":"'Run Selections'!AB310","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U310","v":2},{"$f":"'Run Selections'!V310","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F311=\"\",\"\",'Run Selections'!$F311)","v":""},null,{"$f":"'Run Selections'!T311","v":"Select Model"},{"$f":"'Run Selections'!L311","v":""},{"$f":"'Run Selections'!W311","v":4},null,null,null,null,null,{"$f":"IF(H311=\"Select Model\",\"\",combineACBLLength(J311,K311,L311,M311,N311))","v":""},{"$f":"IF(H311=\"Select Model\",\"\",combineACBWidth('Run Selections'!X311,O311,H311))","v":""},{"$f":" 'Run Selections'!BD311","v":0},{"$f":"'Run Selections'!AI311","v":""},{"$f":"'Run Selections'!AB311","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U311","v":2},{"$f":"'Run Selections'!V311","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F312=\"\",\"\",'Run Selections'!$F312)","v":""},null,{"$f":"'Run Selections'!T312","v":"Select Model"},{"$f":"'Run Selections'!L312","v":""},{"$f":"'Run Selections'!W312","v":4},null,null,null,null,null,{"$f":"IF(H312=\"Select Model\",\"\",combineACBLLength(J312,K312,L312,M312,N312))","v":""},{"$f":"IF(H312=\"Select Model\",\"\",combineACBWidth('Run Selections'!X312,O312,H312))","v":""},{"$f":" 'Run Selections'!BD312","v":0},{"$f":"'Run Selections'!AI312","v":""},{"$f":"'Run Selections'!AB312","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U312","v":2},{"$f":"'Run Selections'!V312","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F313=\"\",\"\",'Run Selections'!$F313)","v":""},null,{"$f":"'Run Selections'!T313","v":"Select Model"},{"$f":"'Run Selections'!L313","v":""},{"$f":"'Run Selections'!W313","v":4},null,null,null,null,null,{"$f":"IF(H313=\"Select Model\",\"\",combineACBLLength(J313,K313,L313,M313,N313))","v":""},{"$f":"IF(H313=\"Select Model\",\"\",combineACBWidth('Run Selections'!X313,O313,H313))","v":""},{"$f":" 'Run Selections'!BD313","v":0},{"$f":"'Run Selections'!AI313","v":""},{"$f":"'Run Selections'!AB313","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U313","v":2},{"$f":"'Run Selections'!V313","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F314=\"\",\"\",'Run Selections'!$F314)","v":""},null,{"$f":"'Run Selections'!T314","v":"Select Model"},{"$f":"'Run Selections'!L314","v":""},{"$f":"'Run Selections'!W314","v":4},null,null,null,null,null,{"$f":"IF(H314=\"Select Model\",\"\",combineACBLLength(J314,K314,L314,M314,N314))","v":""},{"$f":"IF(H314=\"Select Model\",\"\",combineACBWidth('Run Selections'!X314,O314,H314))","v":""},{"$f":" 'Run Selections'!BD314","v":0},{"$f":"'Run Selections'!AI314","v":""},{"$f":"'Run Selections'!AB314","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U314","v":2},{"$f":"'Run Selections'!V314","v":""}]
[null,null,null,null,null,{"$f":"IF('Run Selections'!$F315=\"\",\"\",'Run Selections'!$F315)","v":""},null,{"$f":"'Run Selections'!T315","v":"Select Model"},{"$f":"'Run Selections'!L315","v":""},{"$f":"'Run Selections'!W315","v":4},null,null,null,null,null,{"$f":"IF(H315=\"Select Model\",\"\",combineACBLLength(J315,K315,L315,M315,N315))","v":""},{"$f":"IF(H315=\"Select Model\",\"\",combineACBWidth('Run Selections'!X315,O315,H315))","v":""},{"$f":" 'Run Selections'!BD315","v":0},{"$f":"'Run Selections'!AI315","v":""},{"$f":"'Run Selections'!AB315","v":5},null,"Perf Face",null,{"$f":"'Run Selections'!U315","v":2},{"$f":"'Run Selections'!V315","v":""}]

{"sheet":"ListSheet","index":8,"n_rows":68,"n_cols":44,"rows_kept":68,"cut":false,"hidden":true,"merged":[[4,17,4,25],[4,28,4,39],[4,6,4,14],[4,42,4,43]]}
["NOTE: DO NOT PROTECT THIS SHEET!",null,"William Last Updated ","2023-07-09"]
["Lists for Internal Use Only",null,"Spreadsheet Version:","23.1.8.1","Last Update","2023-08-17T14:31:02"]
["2015-11-03",null,"Server Version:","23.1.6.1","Today",{"$f":"TODAY()","v":"2023-09-06"}]
[null,null,null,"Update was unsuccessful.  Please try again later."]
["Fluid Type",null,"Zone/Room Selection Options","Piping",null,"Unit Type","Lengths (ft)",null,null,null,null,null,null,null,null,null,"Unit Type","Available Nozzles",null,null,null,null,null,null,null,null,null,"Unit Type","Availble Duct Connections",null,null,null,null,null,null,null,null,null,null,null,null,"Unit Type","Availble Piping Types"]
["Water",null,"Default",2,null,"Select Model",null,null,null,null,null,null,null,null,null,null,"Select Model",10,20,30,35,40,50,60,70,80,null,"Select Model",null,null,null,null,null,null,null,null,null,null,null,null,null,"Select Model"]
["Ethylene Glycol",null,"Locked",4,null,"ACBL12_1W",2,3,4,5,6,7,8,9,10,null,"ACBL24_1W",10,20,30,35,40,50,60,70,80,null,"ACBL24_1W",5,"6E","8E",null,null,null,null,null,null,null,null,null,null,"ACBL24_1W",2,4]
["Propylene Glycol",null,"VAV",null,null,"ACBL12_2W",2,3,4,5,6,7,null,null,null,null,"ACBL24_2W",10,20,30,35,40,50,60,70,80,null,"ACBL24_2W",5,"6E","8E",null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",2,4]
["Glycol Percentage",null,"Inlet Locations","Nozzle",null,"ACBL24_1W",2,3,4,5,6,7,8,9,10,null,"ACBL12_1W",20,30,40,50,60,70,80,null,null,null,"ACBL12_2W",5,6,8,"6E","8E",null,null,null,null,null,null,null,null,"ACBL12_2W",2,4]
[0,null,"Side",101,null,"ACBL24_2W",2,3,4,5,6,7,8,9,10,null,"ACBL12_2W",20,30,40,50,60,70,80,null,null,null,"ACBL12_1W",5,6,8,"6E","8E",null,null,null,null,null,null,null,null,"ACBL12_1W",2,4]
[5,null,"Top",201,null,"ACBC_1W",3,4,5,6,7,null,null,null,null,null,"ACBM",20,30,40,50,60,70,null,null,null,null,"ACBM",3,4,null,null,null,null,null,null,null,null,null,null,null,"ACBM",2,4]
[10,null,"End",301,null,"ACBC_2W",3,4,5,6,7,null,null,null,null,null,"ACBR",10,20,30,40,50,60,null,null,null,null,"ACBR","3B","4A","4B","4C","4D","4E","5eC","5eD","5eE","6eC","6eD","6eE",null,"ACBR",2,4]
[15,null,"Inlet Sizes",309,null,"ACBM",2,4,null,null,null,null,null,null,null,null,"LIU2",10,20,30,35,40,50,60,70,80,null,"ACBC_1W","6E","8E",null,null,null,null,null,null,null,null,null,null,null,"ACBC_1W",2,4]
[20,null,3,401,null,"ACBR",2,3,4,5,6,7,8,null,null,null,"ACBC",50,70,483,null,null,null,null,null,null,null,"ACBC_2W","6E","8E",null,null,null,null,null,null,null,null,null,null,null,"PCBL",2]
[25,null,4,405,null,"PCBL",2,3,4,5,6,7,8,9,10,null,"RIU_FB",10,20,30,40,50,60,null,null,null,null,"PCBL",null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU",2,4]
[30,null,5,406,null,"LIU24_2W",2,3,4,5,6,7,8,9,10,null,"RIU_TB",10,20,30,40,50,60,null,null,null,null,"LIU24_2W",5,6,8,"5T","6T","8T","10T",null,null,null,null,null,null,"ACBC_2W",4]
[35,null,6,412,null,"RIU_FB",2,2.67,3.33,4.33,5.33,6.33,7.3440000000000003,null,null,null,"RIU_LB",10,20,30,40,50,60,null,null,null,null,"RIU_FB",3,4,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB",2,4]
[40,null,8,416,null,"RIU_TB",2,2.67,3.33,4.33,5.33,6.33,7.3440000000000003,null,null,null,"ACBR_LP",10,20,30,40,50,60,null,null,null,null,"RIU_TB",3,4,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB",2,4]
[45,null,"5E",483,null,"RIU_LB",2,2.67,3.33,4.33,5.33,6.33,7.3440000000000003,null,null,null,"ACBL24",10,20,30,35,40,50,60,70,80,null,"RIU_LB","3E","4E",null,null,null,null,null,null,null,null,null,null,null,"RIU_LB",2,4]
[50,null,"6E",501,null,null,2,2.67,3.33,4.33,5.33,6.33,7.3440000000000003,null,null,null,"ACBL12",20,30,40,50,60,70,80,null,null,null,"ACBR_LP","3E","4E","6E",null,null,null,null,null,null,null,null,null,null,"ACBR_LP",2,4]
[55,null,"8E",503,null,"ACBC",3,4,5,6,7,null,null,null,null,null,"ACBM",20,30,40,50,60,70,null,null,null,null,"ACBL",5,"6E","8E",null,null,null,null,null,null,null,null,null,null,"ACBL24_1W",2,4]
[60,null,"Inlet Sizes",504,null,"ACBL",2,3,4,5,6,7,8,9,10,null,"ACBR",10,20,30,40,50,60,null,null,null,null,"ACBM",5,6,8,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",2,4]
[null,null,"5 - Side",506,null,"ACBM",2,4,null,null,null,null,null,null,null,null,"ACBC_1W",50,70,null,null,null,null,null,null,null,null,"ACBR","3B","4A","4B","4C","4D","4E","5eC","5eD","5eE","6eC","6eD","6eE",null,"ACBL12_2W",2,4]
[null,null,"5 - Top",510,null,"ACBR",2,3,4,5,6,7,8,null,null,null,"ACBC_2W",50,null,null,null,null,null,null,null,null,null,"ACBC","6E","8E",null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W",2,4]
[null,null,"6 - Side",601,null,"PCBL",2,3,4,5,6,7,8,9,10,null,"PCBL",null,null,null,null,null,null,null,null,null,null,"PCBL",null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM",2,4]
[null,null,"6 - Top",603,null,"LIU2",2,3,4,5,6,7,8,null,null,null,"LIU2",10,20,30,35,40,50,60,70,80,null,"LIU2",5,6,8,"5T","6T","8T","10T",null,null,null,null,null,null,"ACBR",2,4]
[null,null,"8 - Side",604,null,"RIU_",2,2.67,3.33,4.33,5.33,6.33,7.3440000000000003,null,null,null,"RIU_",10,20,30,40,50,60,null,null,null,null,"RIU_",3,4,"3E","4E",null,null,null,null,null,null,null,null,null,"ACBC_1W",2,4]
[null,null,"8 - Top",605,null,"ACBR_LP",2,2.67,3.33,4.33,5.33,6.33,7.3440000000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","3E","4E","6E",null,null,null,null,null,null,null,null,null,null,"ACBC_2W",4]
[null,null,null,607,null,"ACBH",2,3,4,5,6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PCBL",2]
["Sound",null,null,608,null,"ACBV",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU",2,4]
["NC Level",20,25,26,27,28,29,30,35,40,45,50,55,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB",2,4]
["Room Attenuation",20,15,10,9,8,7,6,5,4,3,2,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB",2,4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB",2,4]
["Configuration",null,null,null,null,null,null,null,null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP",2,4]
[]
["Condensate Pipe","No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL-R","ACBL 24\" and ACBS"]
["Coil","None","Black",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,20,30,35,40,50,60,70,80]
["Hoses","No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CI","DM","DL","DF","EJ","EF","FG","FD","FA"]
["Isolation Valves","No","Yes",null,null,null,null,"Lint Screen","None (Std)","Yes LS"]
["Protective Film","No","Yes PF",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL 12\""]
["Insulation","None","Internal","External","Int & Ext",null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,30,40,50,60,70,80]
["Paint Color","B12 White","SPL Special",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AA","BA","CA","DE","DA","EA","FA"]
["Air Plenum","Galv (std)","Painted"]
["Vent & Drain","NODV","DV",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM"]
["Fittings","1/2in Sweat (std)","1/2in Female NPT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,30,40,50,60,70]
["Pattern Controller","No","Yes PC",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AA","BA","CA","DA","EA","FA"]
[]
["Lint Screen","None (Std)","Yes LS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC"]
["Orientation","Left Hand","Right Hand",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,30,40,50,60,70,80,90]
["Inlet Location","Side","Top",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CD","DJ","DF","EJ","EF","EC","EA","FB"]
["ACBR","Perf Face","LV1","AS-1/AS-2","SDS","JS 210"]
["ACBL Grille","Perf Face","Bar Grille"]
["ACBC Grille","Perf Face","TL Louver"]
["ACBM Grille","Perf Face","Bar Grille"]
[]
["VFR Options","VFR4","VFR5","VFR6","VFR8","None (Std)"]
["VFR Ranges","10-60","35-105","75-175","125-295"]
["Inlet Damper","None","MQ Manual","VAV Actuated","None (Std)","Yes -Damper","Yes -VFR"]
["Inlet Damper","None","MQ4","MQ5","MQ6","MQ8","VAV4","VAV5","VAV6","VAV8","VFR4-10","VFR4-20","VFR4-25","VFR4-30","VFR4-35","VFR4-45","VFR4-50","VFR4-60","VFR5-35","VFR5-50","VFR5-60","VFR5-75","VFR5-90","VFR5-105","VFR6-75","VFR6-90","VFR6-105","VFR6-125","VFR6-140","VFR6-160","VFR6-175","VFR8-125","VFR8-140","VFR8-160","VFR8-175","VFR8-205","VFR8-235","VFR8-265","VFR8-295"]
[]
["Condensate Pipe","No","Yes"]
[]
["Air Diffuser","None (Std)","ADS12A 12in","ADS12VAV-A 12in","ADS24A 24in","ADS24VAV-A 24in","ADS12B 12in","ADS12VAV-B 12in","ADS24B 24in","ADS24VAV-B 24in","ADS12T 12in","ADS12VAV-T 12in","ADS24T 24in","ADS24VAV-T 24in"]
["Slim Line Coupling ACBL-HE only","None (Std)","SLIM-1","SLIM-2","SLIM-MID"]
["Access Blank Seection","None (Std)","ABS12 12in"]
["Return Exhaust","None (Std)","RET12 12in"]
[]
["ACBR Available Inlet Damper","None","MQ4","MQ5","MQ6","VAV4","VAV5","VAV6","VFR4-10","VFR4-20","VFR4-25","VFR4-30","VFR4-35","VFR4-45","VFR4-50","VFR4-60","VFR5-35","VFR5-50","VFR5-60","VFR5-75","VFR5-90","VFR5-105","VFR6-75","VFR6-90","VFR6-105"]

{"sheet":"Lookup Tables","index":9,"n_rows":621,"n_cols":301,"rows_kept":281,"cut":true,"hidden":true,"merged":[[9,215,9,216],[9,217,9,220],[9,211,9,214],[9,207,9,210],[9,175,9,178],[9,179,9,182],[9,183,9,187],[9,188,9,192],[9,193,9,194],[9,195,9,206]],"bounds":{"rows_first":125,"rows_last":31,"rows_between":125,"halvings":4}}
[null,"Description:",null,null,null,null,"Legend:"]
[null,"This worksheet contains a number of lookup tables that are leveraged by the VBA code and the spreadsheet.",null,null,null,null,"Test Data"]
[null,"To facilitate future maintenance, each table is defined as a Table in Excel.",null,null,null,null,"Extrapolation"]
[null,"Each table stacked horizontally."]
[null,"In this way, you can easily insert table rows or table columns without impacting any other tables"]
[]
[null,"Here is a current list of all of the tables, with hyperlinks for easy access:"]
[]
[null,"Lookup Tables",null,null,null,null,"Induction Ratios",null,null,null,null,null,null,null,null,null,null,null,null,"Throw Constants",null,null,null,null,null,null,null,null,null,null,"Nozzle Codes",null,null,null,null,null,null,null,null,null,null,"Model Descriptions",null,null,"Model Widths",null,null,"Available Lengths",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Available Nozzles",null,null,null,null,null,null,null,null,null,null,"Available Duct Connections",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Inlet Duct Area",null,null,"Sound Data",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nozzles Per Beam",null,null,null,null,null,null,null,null,null,null,null,"Nozzles Diameters",null,null,null,null,null,null,null,null,null,null,"Number Of Coil Passes",null,null,null,null,"Coil Water Pressure Drop",null,null,null,null,null,null,null,"Performance Constants",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"New Performance Constants",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A-Weighting",null,null,null,null,null,null,null,null,null,null,null,null,"Log Sound",null,null,null,null,null,null,null,null,null,null,null,"Inlet Location Factors",null,null,null,null,null,null,null,null,null,null,null,null,"Nozzle Data",null,null,null,null,null,null,null,"Reference Values",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Conversion Ratios"]
[null,null,null,null,null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,null,null,null,null,null,null,null,null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,null,null,null,null,null,null,null,null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,null,null,null,null,null,null,null,null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,null,null,null,null,null,null,null,null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,null,null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,null,null,null,null,null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,"F1",null,null,null,"F2",null,null,null,"F3",null,null,null,null,"F4",null,null,null,null,"Airflow",null,"Correlation Constants - Induction Ratio",null,null,null,null,null,null,null,null,null,null,null,"Correlation Constants - WPD",null,null,null,"Adjacent Zone",null,null,null,"Throw Constants",null,"Total Capacity Constants",null,null,null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,null,null,null,null,null,null,null,null,null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,null,null,null,null,null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"HYPERLINK(\"#LookupTables\", \"Back to Lookup Tables\")","v":"Back to Lookup Tables"}]
[null,"Table Name","Last Updated","Updated By","Hyperlink",null,"Key","Length","Derate","10","20","30","35","40","50","60","70","80",null,"Key","a","b","c","d","e","f","g","h","Power",null,"Key","10","20","30","35","40","50","60","70","80",null,"Key","Description",null,"Key","Width",null,"Key","2","2.67","3","3.33","4","4.33","5","5.33","6","6.33","7","7.344","8","9","10",null,"Key","10","20","30","35","40","50","60","70","80",null,"Key","3","3E","3B","4","4A","4B","4C","4D","4E","5","5eC","5eD","5eE","5E","5T","6eC","6eD","6eE","6","6E","6T","8","8E","8ET","8T","10T",null,"Key","AD",null,"Key","Length","InletDiameter","slotWidth","numberSlots","a","b","c","d","logVel","logSlotVel","logSlotArea","logADAN0","logCalcTPVP","intercept",null,"Key","Length","10","20","30","35","40","50","60","70","80",null,"Key","10","20","30","35","40","50","60","70","80",null,"Key","operatingType","coilPipe","numberPasses",null,"Key","a","b","c","d","e","f",null,"Key","coilType","nozzles","OperatingMode","Derate","Length","k","a","b","c","alpha","beta","InductionRatioDerate","r",null,"Key","Test Length","b1","b2","b3","b4","b5","b6","b7","b8","b9","b10","b11","b12","b13","b14","b15","b16","b17","b18","b19","b20","b21-Cool","b22-Cool","b23-Cool","b24-Cool","b25-Cool","b26-Cool","b21-Heat","b22-Heat","b23-Heat","b24-Heat","b25-Heat","b26-Heat","b27","b28","b29","b30","b31_60","b32_60","b31_40","b32_40","b33","b34","b35","b36","b37","b38",null,"Model","Category","63","125","250","500","1000","2000","4000","8000","NC","dBA",null,"Model","Variable","Column1","63","125","250","500","1000","2000","4000","8000",null,"Model","Nozzle ","Inlet","Code","63","125","250","500","1000","2000","4000","8000",null,"Model","Code","Length [ft]","Nozzle Size","Nozzle Diameter [in]","Total Nozzles","Bottom Nozzles",null,"Model","AI [cm2]","Pipe Diameter [in]","Pipe Area [m2]","Flow Exponent","Circuit Exponent","Water Density [kg/m3]","Max Norm Airflow","Max Norm Capacity","pREF [in WG]","uREF [m/s]","Refrence Length [ft]","Max Induced Velocity [FPM]","TPVP constant 1","TPVP constant 2","TPVP constant 3","Max Distance [ft]","Max CFM","Npu2[m/s]","(L/D)u2","WPDREF [ft H2O]","Circuit Coefficient",null,"F > R","C > K","K > R","pascal -> in.h20","Watts -> BTU","l/s -> CFM","meter -> ft","L/s-m -> cfm/ft","W/m -> Btu/hr ft","GPM -> kg/hr"]
[null,"Induction Ratios","2016-08-24","Steven Schroeder",{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to Induction Ratios"},null,"ACBM",2,1,3.7,3.2,null,2.8,1.8,1.5,1.5,1.5,1.2,null,"ACBL12_1W",9.3799999999999994E-2,-0.20860000000000001,4.4949999999999997E-2,-6.7799999999999999E-2,1.4999999999999999E-2,2.5000000000000001E-2,0.16669999999999999,-1.3899999999999999E-2,-1,null,"ACBC_1W",null,null,null,null,null,405,null,504,null,null,"ACBL12_1W","Ceiling mounted 12” wide 1-way discharge linear beam",null,"ACBL12_1W",12,null,"ACBL12_1W",2,null,3,null,4,null,5,null,6,null,7,null,8,9,10,null,"ACBL12_1W",null,20,30,null,40,50,60,70,80,null,"ACBL12_1W",null,null,null,null,null,null,null,null,null,"5",null,null,null,null,null,null,null,null,null,"6E",null,null,"8E",null,null,null,null,"3B","0.049",null,"ACBL12_1W",null,null,1.875,1,0,1.1903999999999999,2.6000999999999999,-6.0079000000000002,-28.326699999999999,81.777469999999994,12.93412,-77.606999999999999,22.74437,-70.582499999999996,null,"ACBL12_2W",2,null,32,32,null,32,24,32,32,32,null,"ACBL12_1W",null,0.125,0.16,null,0.188,0.25,0.25,0.3,0.35,null,"ACBL12_1W","cooling",2,10,null,"cooling|2P1C",0.81451711189999998,1.0687757040000001,1.003191612,0.1052948346,0.7807993969,1.8102732109999999,null,"ACBC","4P1C",20,"cooling",0,7.3,6.097002570006798,0.64617580138468744,0.96180153927094336,4.5202387620426512E-2,3.7482812306102402,1.5393799567659041,0,2.54,null,"ACBR",4,1.536814976E-2,9.665436292E-3,0.59540213939999997,0,0.18414388579999999,-9.2147542400000004E-2,0.9727358841,0.10366683190000001,3.9041584789999998E-3,-8.5861843240000006E-3,2.9701423670000001E-3,3.6364718390000002E-3,-3.0483351759999998E-3,5.1005627749999997E-2,-2.9793614389999998E-3,7.1941820879999993E-2,3.120796478E-2,-4.9063723390000001E-2,0.74176013090000004,-3.5867859750000002E-2,-0.55349999999999999,2.1739999999999999,1.2204999999999999,-0.13669999999999999,0.97670000000000001,null,null,null,null,null,null,null,0.4248060796,0.87175385419999996,0.12895133049999999,1.106880826,null,null,null,null,null,null,null,null,null,null,null,"ACBR","A-Weighting",-26.2,-16.100000000000001,-8.6,-3.2,0,1.2,1,-1.1000000000000001,{"$f":"IF(MAX((1.285450062*(HR12-10)-31.62762022),(1.181332986*(HS12-10)-18.53553762),(1.087868418*(HT12-10)-8.44850425),(1.042347753*(HU12-10)-3.10271421),(0.9981412639*(HV12-10)+0.9107806691),(0.9812108559*(HW12-10)+3.006263048))<0,\"\",ROUND(MAX((1.285450062*(HR12-10)-31.62762022),(1.181332986*(HS12-10)-18.53553762),(1.087868418*(HT12-10)-8.44850425),(1.042347753*(HU12-10)-3.10271421),(0.9981412639*(HV12-10)+0.9107806691),(0.9812108559*(HW12-10)+3.006263048)),1))","v":""},{"$f":"10*LOG(10^((HR12+HR$46)/10)+10^((HS12+HS$46)/10)+10^((HT12+HT$46)/10)+10^((HU12+HU$46)/10)+10^((HV12+HV$46)/10)+10^((HW12+HW$46)/10))","v":6.2514752753391667},null,"ACBR","log Inlet Vel",1,36.588039559538061,94.914445937067711,111.98564131148562,131.28410588546942,171.72612171649294,149.53311694825226,155.63761440930847,97.782166037515395,null,null,null,null,1,2,3,4,5,6,7,8,9,null,"ACBR",{"$f":"CONCATENATE(JD12,\"-\",JC12)","v":"10-2"},2,10,0.25,16,0,null,"ACBC_1W",126.67686977437442,0.5,1.2667686977437442E-4,0.2,0.08,999.1,2.5,19,1,1,5,100,1.2474000000000001,-0.25869999999999999,1.0074000000000001,30,500,64,5000,60,100,null,459.67,273.14999999999998,1.8,4.0146307871549653E-3,3.4151790000000002,2.1188799999999999,3.28084,0.645834625,1.0400207739,227.12]
[null,"Throw Constants","2016-09-16","Steven Schroeder",{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to Throw Constants"},null,"ACBM",4,1,4.2,3.3,null,2.8,2.2999999999999998,1.2,1.2,1.2,1.3,null,"ACBL12_2W",6.5000000000000002E-2,1.23,-0.115,4.37,-0.42499999999999999,9.5167000000000002,0.20349999999999999,-0.18559999999999999,1,null,"ACBC_2W",null,null,null,null,null,483,null,null,null,null,"ACBL12_2W","Ceiling mounted 12” wide 2-way discharge linear beam",null,"ACBL12_2W",12,null,"ACBL12_2W",2,null,3,null,4,null,5,null,6,null,7,null,8,9,10,null,"ACBL12_2W",null,20,30,null,40,50,60,70,80,null,"ACBL12_2W",null,null,null,null,null,null,null,null,null,"5",null,null,null,null,null,null,null,null,null,"6E",null,null,"8E",null,null,null,null,"3E",4.9000000000000002E-2,null,"ACBL12_2W",null,null,1,2,0,1.4481999999999999,-1.3542000000000001,3.8085,30.714139899999999,29.913256499999999,6.0630829999999998,-76.021559100000005,48.894012400000001,-153.5925958,null,"ACBL12_2W",3,null,56,56,null,56,40,56,56,56,null,"ACBL12_2W",null,0.125,0.16,null,0.188,0.25,0.25,0.3,0.35,null,"ACBL12_1W","heating",2,10,null,"cooling|4P1C",0.81451711189999998,1.0687757040000001,1.003191612,0.1052948346,0.7807993969,1.8102732109999999,null,"ACBC","4P2C",20,"cooling",-0.03,7.3,6.097002570006798,0.64617580138468744,0.96180153927094336,4.5202387620426512E-2,3.7482812306102402,1.5393799567659041,0,2.54,null,"ACBL24_1W",6,1.529657957E-2,2.0017889850000001E-2,0.77705604029999997,0,9.9445756910000002E-2,-8.6456731810000007E-2,1.1057241980000001,-0.1208122226,-1.387913751E-3,2.4904954919999999E-3,-1.9942687039999998E-3,-1.4960098799999999E-3,5.295928771E-4,5.9394997230000003E-2,1.9484306010000001E-2,8.9585821479999994E-2,3.8395004769999998E-2,-5.187640818E-2,0.72182239640000001,-2.0360502490000001E-2,-0.31030000000000002,1.3577999999999999,1.0819000000000001,0,1,null,null,null,null,null,null,null,0.47950702499999998,0.87963997559999996,0.1076378157,0.99729185090000005,null,null,null,null,null,null,null,null,null,null,null,"ACBC_1W","A-Weighting",-26.2,-16.100000000000001,-8.6,-3.2,0,1.2,1,-1.1000000000000001,null,6.2514752753391667,null,"ACBR","log slot vel",2,-28.556285510118013,-61.352604620638779,-61.775782903013223,-61.418174791369822,-79.411938715610603,-60.314072416923196,-65.533911692043731,-45.544828294480219,null,"ACBR",10,"3B",{"$f":"CONCATENATE(IN13,\"_\",IO13,\"_\",IP13)","v":"ACBR_10_3B"},0,0,0,0,0,0,0,0,null,"ACBR","20-2",2,20,0.3,16,0,null,"ACBC_2W",126.67686977437442,0.5,1.2667686977437442E-4,0.2,0.08,999.1,2.5,19,1,1,5,100,1.3186,-0.36919999999999997,1.0702,30,500,64,5000,60,100]
[null,"Nozzle Codes",null,null,{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to Nozzle Codes"},null,"ACBL-R2",null,1,5.7,5.3,4.9000000000000004,4.5,3.6,3.3,3.3,3.3,2.7,null,"ACBL24_2W",-7.4999999999999997E-2,1.85,2.5000000000000001E-2,2.9159999999999999,0,5.9,0.33300000000000002,0,1,null,"ACBL12_1W",null,101,201,null,301,405,401,501,601,null,"ACBL24_2W","Ceiling mounted 24” wide 2-way discharge linear beam",null,"ACBM",24,null,"ACBL24_2W",2,null,3,null,4,null,5,null,6,null,7,null,8,9,10,null,"ACBL24_2W",10,20,30,35,40,50,60,70,80,null,"ACBL24_2W",null,null,null,null,null,null,null,null,null,"5",null,null,null,null,null,null,null,null,null,"6E",null,null,"8E",null,null,null,null,"4A",8.6999999999999994E-2,null,"ACBL24_2W",null,null,1.625,2,0,1.3064,0.43280000000000002,2.0487000000000002,18.8061979172771,41.309035003793802,5.3829433622629201,-47.002352311214999,32.622143971047201,-148.56963549520501,null,"ACBL12_2W",4,null,80,80,null,80,56,80,80,80,null,"ACBL24_2W",0.188,0.25,0.25,0.25,0.3,0.3,0.35,0.35,0.35,null,"ACBL12_1W","cooling",4,6,null,"heating|2P1C",0.81451711189999998,1.0687757040000001,1.003191612,0.1052948346,0.7807993969,1.8102732109999999,null,"ACBC","2P1C",20,"heating",0.05,7.3,6.097002570006798,0.64617580138468744,0.96180153927094336,4.5202387620426512E-2,3.7482812306102402,1.5393799567659041,0,2.54,null,"ACBL24_2W",6,1.7158144560000001E-2,1.6809030209999999E-2,0.88777851100000005,-0.37612801820000002,-1.9020155800000001E-2,0.1167500788,1.1128259869999999,-4.148904665E-2,5.0417280959999999E-4,-1.267421382E-4,1.495399794E-3,1.3819004189999999E-4,-2.0105743929999999E-3,5.6361004540000002E-2,6.1481806119999998E-3,8.8660449089999996E-2,3.9174972609999997E-2,-3.2843108760000003E-2,0.70009235999999997,-2.4498595920000001E-2,-0.59840000000000004,2.1465999999999998,1.1963999999999999,0,1,null,null,null,null,null,null,null,0.47950702499999998,0.87963997559999996,0.1076378157,0.99729185090000005,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W","A-Weighting",-26.2,-16.100000000000001,-8.6,-3.2,0,1.2,1,-1.1000000000000001,null,6.2514752753391667,null,"ACBR","log slot area",3,-13.109957428285611,-36.880572589199453,-52.814392305463642,-53.226639446675762,-55.595259450646836,-37.676317959417354,-36.697063500949945,-30.413560533868658,null,"ACBR",10,"4B",{"$f":"CONCATENATE(IN14,\"_\",IO14,\"_\",IP14)","v":"ACBR_10_4B"},0,0,0,0,0,0,0,0,null,"ACBR","30-2",2,30,0.35,14,0,null,"ACBR",126.67686977437442,0.5,1.2667686977437442E-4,0.2,0.08,999.1,2.5,19,1,1,4,100,1.3355999999999999,0.16950000000000001,1.5313000000000001,null,null,64,5000,60,100]
[null,"Model Descriptions",null,null,{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to Model Descriptions"},null,"ACBL-R1",null,1,null,null,null,4.5,3.5,3.3,3.3,3.3,3,null,"ACBL24_1W",-0.79169999999999996,10.227,-0.7167,11.867000000000001,-0.75,15,0.23233300000000001,0,1,null,"ACBL12_2W",null,101,201,null,301,405,401,501,601,null,"ACBL24_1W","Ceiling mounted 24” wide 1-way discharge linear beam",null,"ACBL24_2W",24,null,"ACBL24_1W",2,null,3,null,4,null,5,null,6,null,7,null,8,9,10,null,"ACBL24_1W",10,20,30,35,40,50,60,70,80,null,"ACBL24_1W",null,null,null,null,null,null,null,null,null,"5",null,null,null,null,null,null,null,null,null,"6E",null,null,"8E",null,null,null,null,"4B",8.6999999999999994E-2,null,"ACBL24_1W",null,null,1.625,1,0,1.2718,1.952,-6.1214000000000004,57.382609537127202,7.8309791292514896,-2.0547049395492398,82.486585810217903,-17.833078214218901,-188.31779785312301,null,"ACBL12_2W",5,null,104,104,null,104,76,104,104,104,null,"ACBL24_1W",0.188,0.25,0.25,0.25,0.3,0.3,0.35,0.35,0.35,null,"ACBL12_1W","heating",4,4,null,"heating|4P1C",0.81451711189999998,1.0687757040000001,1.003191612,0.1052948346,0.7807993969,1.8102732109999999,null,"ACBC","2P2C",20,"heating",0,7.3,6.097002570006798,0.64617580138468744,0.96180153927094336,4.5202387620426512E-2,3.7482812306102402,1.5393799567659041,0,2.54,null,"ACBC_1W",5,1.3614267689999999E-2,-4.5699773989999999E-3,2.2403652269999998,0,-0.39924623180000002,-9.2271585249999996E-2,1.184817384,-1.3693974940000001E-2,2.3548303539999999E-3,1.694765205E-3,-7.7435014419999998E-3,2.8569275260000001E-3,1.636761831E-3,3.3470910290000003E-2,1.5168899160000001E-2,4.2862211650000002E-2,1.2213021960000001E-2,-2.5780522980000001E-2,0.72430100180000001,1.321209634E-2,-0.28810000000000002,1.0972999999999999,1.1315999999999999,-0.36330000000000001,1.4027000000000001,null,null,null,null,null,null,null,0.39025843100000002,0.92831523090000001,7.965430876E-2,0.46637564520000002,0.73027733957160079,-8.9036240327667326E-2,0.86197010551943809,4.6346697107444823E-2,null,null,null,null,null,null,null,"ACBL24_1W","A-Weighting",-26.2,-16.100000000000001,-8.6,-3.2,0,1.2,1,-1.1000000000000001,{"$f":"IF(MAX((1.285450062*(HR15-10)-31.62762022),(1.181332986*(HS15-10)-18.53553762),(1.087868418*(HT15-10)-8.44850425),(1.042347753*(HU15-10)-3.10271421),(0.9981412639*(HV15-10)+0.9107806691),(0.9812108559*(HW15-10)+3.006263048))<0,\"\",ROUND(MAX((1.285450062*(HR15-10)-31.62762022),(1.181332986*(HS15-10)-18.53553762),(1.087868418*(HT15-10)-8.44850425),(1.042347753*(HU15-10)-3.10271421),(0.9981412639*(HV15-10)+0.9107806691),(0.9812108559*(HW15-10)+3.006263048)),1))","v":""},6.2514752753391667,null,"ACBR","log Ainlet/ Anozzle",4,41.895215764174552,39.41279956117755,71.935827614414194,89.952252115818311,79.644594328996916,41.873897945796685,118.02532620216105,133.07602880187255,null,"ACBR",10,"4C","ACBR_10_4C",-0.8,-1.3,0.4,1.6,1,0.2,-0.5,0.6,null,"ACBR","40-2",2,40,0.35,16,0,null,"ACBL24_1W",126.67686977437442,0.5,1.2667686977437442E-4,0.2,0.08,999.1,2.5,19,1,1,5,100,1.3188,0.54769999999999996,-0.82150000000000001,30,500,64,5000,60,100]
[null,"Model Widths",null,null,{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to Model Widths"},null,"ACBR",null,1,3.8,3.8,null,3.4,3.2,2.7,2.7,2.7,null,null,"ACBM",0,1.3,0.23,2.2400000000000002,0.375,5,0.1585,0.27400000000000002,1,null,"ACBL24_1W",309,416,412,406,510,506,607,604,601,null,"ACBM","Ceiling mounted 24” wide 4-way discharge modular beam",null,"ACBL24_1W",24,null,"ACBM",2,null,null,null,4,null,null,null,null,null,null,null,null,null,null,null,"ACBM",null,20,30,null,40,50,60,70,null,null,"ACBM",null,null,null,null,null,null,null,null,null,"5",null,null,null,null,null,null,null,null,"6",null,null,"8",null,null,null,null,null,"4C",8.6999999999999994E-2,null,"ACBC",null,null,1,1,0,0,0,1,62.088128009999998,null,null,16.081012309999998,null,-167.6514138,null,"ACBL12_2W",6,null,128,128,null,128,92,128,128,128,null,"ACBM",null,0.125,0.16,null,0.188,0.25,0.3,0.35,null,null,"ACBL12_2W","cooling",2,10,null,"cooling|2P2C",0.81451711189999998,1.0687757040000001,1.003191612,5.6099827919999998E-2,0.58116618769999995,1.8915960629999999,null,"ACBC","4P1C",20,"heating",0,7.3,4.8732431713296727,0.59012331657813288,0.96516036663475502,7.5242376065686664E-2,3.7482812306102402,1.5393799567659041,0,2.54,null,"ACBC_2W",5,5.4819017860000003E-3,0,1.1694521680000001,0,0.1857372598,0,1.4062883420000001,0,1.176492734E-3,-2.6166491129999997E-4,0,1.419156854E-3,0,4.4576256170000002E-2,0,5.5054596589999998E-2,0,-6.7943117669999997E-2,0.70470704039999998,2.2693552589999999E-2,6.9450000000000003,-8.8683999999999994,1.1839999999999999,-5.3319999999999999,6.57,null,-1.84,4.1900000000000004,1.2070000000000001,-0.41899999999999998,1.9550000000000001,null,0.41639671979999998,0.924534462,2.8350843279999999E-2,0.37767533759999999,0.26056832315365458,8.0417292488173753E-2,0.4785190607886548,0.13383931014661432,null,null,null,null,null,null,null,"ACBL24_2W","A-Weighting",-26.2,-16.100000000000001,-8.6,-3.2,0,1.2,1,-1.1000000000000001,"",6.2514752753391667,null,"ACBR","log calculated TPVP",5,-14.282501620979044,-5.405979777927044,-30.301570072707666,-32.613128079557775,-9.0589962832365032,14.692003490986405,-19.992997948502836,-47.583643872492601,null,"ACBR",10,"4D","ACBR_10_4D",-0.5,-1,-0.3,-0.1,0,0.2,-0.7,0.1,null,"ACBR","50-2",2,50,0.35,20,0,null,"ACBL24_2W",126.67686977437442,0.5,1.2667686977437442E-4,0.2,0.08,999.1,2.5,19,1,1,5,100,1.3988,0.72450000000000003,-0.55900000000000005,30,500,64,5000,60,100]
[null,"Available Lengths","2016-09-15","Steven Schroeder",{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to Available Lengths"},null,"ACBC_1W",null,1,2.54,2.34,null,2.06,2,1.76,1.76,1.76,1.52,null,"LIU24_2W",0,2.6749999999999998,0,5.125,0,8.6999999999999993,0,2.4703541666666666,1,null,"ACBL24_2W",309,416,412,406,510,506,607,604,601,null,"ACBC_2W","Floor mounted 30” tall x 13.5” deep 2-way displacement beam",null,"ACBR",9,null,"ACBR",2,null,3,null,4,null,5,null,6,null,7,null,8,null,null,null,"ACBR",10,20,30,null,40,50,60,null,null,null,"ACBC_1W",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6E",null,null,"8E",null,null,null,null,"4D",8.6999999999999994E-2,null,"ACBM",2,5,3.5399999999999996,1,0,1.3581000000000001,1.72E-2,1E-4,16.105889220000002,46.582941230000003,0,-13705.84209,6862.888809,-1063.298481,null,"ACBL12_2W",7,null,152,152,null,152,108,152,152,152,null,"ACBR",0.25,0.3,0.35,null,0.35,0.35,0.35,null,null,null,"ACBL12_2W","heating",2,10,null,"cooling|4P2C",0.81451711189999998,1.0687757040000001,1.003191612,5.6099827919999998E-2,0.58116618769999995,1.8915960629999999,null,"ACBC","4P2C",20,"heating",0,7.3,4.8732431713296727,0.59012331657813288,0.96516036663475502,7.5242376065686664E-2,3.7482812306102402,1.5393799567659041,0,2.54,null,"ACBL12_1W",6,8.971999451E-4,3.1800820289999997E-2,-0.6923087067,0,12.6400337,-11.47243823,1.086939799,-0.2553609516,-2.4413722790000002E-2,2.2320436320000001E-2,-1.212338282E-2,3.8148478580000002E-3,1.0829399119999999E-2,0.25912243140000002,-0.1161800625,2.73341309E-2,4.1893815530000003E-2,3.9693096499999999E-3,0.68485688089999996,2.48867056E-2,-0.31777376959999998,1.794922879,0.94154843389999998,-0.2816533839,1.4657623049999999,null,null,null,null,null,null,null,0.31360820700000003,0.83949681470000004,0.45487818499999999,1.0493849930000001,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","A-Weighting",-26.2,-16.100000000000001,-8.6,-3.2,0,1.2,1,-1.1000000000000001,"",6.2514752753391667,null,"ACBR","log Inlet Area",6,20.095508701920796,59.013756862120687,84.018189636123452,85.219436424191514,92.830380248057523,69.483331808031593,68.204642934094494,47.622361086830715,null,"ACBR",10,"4E","ACBR_10_4E",-1.6,-2,-7.8,-10.9,-8.1,-4.8,-5.3,-3.2,null,"ACBR","60-2",2,60,0.35,24,0,null,"ACBL12_1W",126.67686977437442,0.5,1.2667686977437442E-4,0.2,0.08,999.1,2.5,19,1,1,5,100,1.3548,-1.0652999999999999,4.7759,30,500,64,5000,60,100]
[null,"Available Nozzles","2016-09-15","Steven Schroeder",{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to Available Nozzles"},null,"ACBC_2W",null,1,2.54,2.34,null,2.06,2,1.76,1.76,1.76,1.52,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM",null,101,201,null,301,401,501,601,null,null,"ACBC_1W","Floor mounted 30” tall x 13.5” deep 1-way displacement beam",null,"ACBC_1W",13.5,null,"ACBC_2W",null,null,3,null,4,null,5,null,6,null,7,null,null,null,null,null,"ACBC_1W",null,null,null,null,null,50,null,70,null,null,"ACBC_2W",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6E",null,null,"8E",null,null,null,null,"4E",8.6999999999999994E-2,null,"ACBM",2,6,3.5399999999999996,1,0,1.3581000000000001,1.72E-2,1E-4,16.105889220000002,46.582941230000003,0,-13705.84209,6862.888809,-1063.298481,null,"ACBL12_2W",8,null,176,176,null,176,128,176,176,176,null,"ACBC_1W",null,null,null,null,null,0.25,null,0.3,null,null,"ACBL12_2W","cooling",4,6,null,"heating|2P2C",0.81451711189999998,1.0687757040000001,1.003191612,5.6099827919999998E-2,0.58116618769999995,1.8915960629999999,null,"ACBC","4P1C",30,"cooling",0,7.3,4.7496921590000003,0.67868702299999994,1.004689355,4.2982425999999997E-2,0.91471000000000002,1.8573,0,2.34,null,"ACBL12_2W",6,1.161363579E-2,1.6293179089999998E-2,0.20670672349999999,0.20670672349999999,0.1194849639,3.0909367149999999E-2,0.88844449299999995,5.1143862810000003E-2,-4.9067807449999995E-4,2.334043348E-4,2.1886287429999998E-3,2.7081551190000002E-4,-1.6174203170000001E-3,-0.44838443360000002,0.49521511540000002,5.0292137549999998E-2,3.10811496E-2,-1.007013516E-2,0.65926347910000005,3.96952759E-2,-0.52932346060000002,2.1420300380000001,0.98082661380000002,0,1,null,null,null,null,null,null,null,0.4604207468,0.87431877499999999,0.13001674690000001,0.99249836459999996,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","A-Weighting",-26.2,-16.100000000000001,-8.6,-3.2,0,1.2,1,-1.1000000000000001,"",6.2514752753391667,null,"ACBR","intercept",7,26.924797272480461,-42.819205000398114,-46.616608139118142,-109.16556944266499,-205.46145244594186,-227.41771579869248,-234.26241972473451,-104.85385123506779,null,"ACBR",10,"5eC","ACBR_10_5eC",-0.7,-0.7,-3.5,-4.0999999999999996,-3.1,-2.2000000000000002,-3.3,-1.5,null,"ACBR","10-3",3,10,0.25,24,0,null,"ACBL12_2W",126.67686977437442,0.5,1.2667686977437442E-4,0.2,0.08,999.1,2.5,19,1,1,5,100,1.407,-0.64970000000000006,1.9728000000000001,30,500,64,5000,60,100]
[null,"Available Duct Connections","2016-09-15","Steven Schroeder",{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to Available Duct Connections"},null,"ACBL24_1W",null,1,5.16,4.8899999999999997,4.7300000000000004,4.54,4.13,3.65,3.65,3.65,3.09,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR",406,506,608,null,605,603,601,null,null,null,"PCBL","Passive Beam. Ceiling mounted 24” wide 2-way discharge linear beam.  ",null,"ACBC_2W",13.5,null,"ACBC_1W",null,null,3,null,4,null,5,null,6,null,7,null,null,null,null,null,"ACBC_2W",null,null,null,null,null,50,null,null,null,null,"ACBR",null,null,"3B",null,"4A","4B","4C","4D","4E",null,"5eC","5eD","5eE",null,null,"6eC","6ed","6eE",null,null,null,null,null,null,null,null,null,"5eC",0.14299999999999999,null,"ACBM",2,8,3.5399999999999996,1,0,1.3581000000000001,1.72E-2,1E-4,16.105889220000002,46.582941230000003,0,-13705.84209,6862.888809,-1063.298481,null,"ACBL12_2W",9,null,200,200,null,200,144,200,200,200,null,"ACBC_2W",null,null,null,null,null,0.25,null,null,null,null,"ACBL12_2W","heating",4,4,null,"heating|4P2C",0.81451711189999998,1.0687757040000001,1.003191612,0.1052948346,0.7807993969,1.8102732109999999,null,"ACBC","4P2C",30,"cooling",-0.06,7.3,4.7496921590000003,0.67868702299999994,1.004689355,4.2982425999999997E-2,0.91471000000000002,1.8573,0,2.34,null,"ACBM",4,1.7158144560000001E-2,1.6809030209999999E-2,0.88777851100000005,-0.37612801820000002,-1.9020155800000001E-2,0.1167500788,1.1128259869999999,-4.148904665E-2,5.0417280959999999E-4,-1.267421382E-4,1.495399794E-3,1.3819004189999999E-4,-2.0105743929999999E-3,5.6361004540000002E-2,6.1481806119999998E-3,8.8660449089999996E-2,3.9174972609999997E-2,-3.2843108760000003E-2,0.70009235999999997,-2.4498595920000001E-2,-2.4920742410000001,8.9640442369999995,1.198532149,-0.6513894348,2.8730768109999998,null,null,null,null,null,null,null,0.47950702499999998,0.87963997559999996,0.1076378157,0.99729185090000005,null,null,null,null,null,null,null,null,null,null,null,"ACBM","A-Weighting",-26.2,-16.100000000000001,-8.6,-3.2,0,1.2,1,-1.1000000000000001,"",6.2514752753391667,null,"ACBR","r^2",8,0.2323836436768274,0.91624227772712197,0.93296909780216664,0.92920871411339345,0.94450630345666853,0.9478811333509336,0.92893108972636684,0.66187325223140414,null,"ACBR",10,"5eD","ACBR_10_5eD",0,0,0,0,0,0,0,0,null,"ACBR","20-3",3,20,0.3,24,0,null,"ACBM",126.67686977437442,0.5,1.2667686977437442E-4,0.2,0.08,999.1,2.5,19,1,1,5,100,1.2474000000000001,0.25869999999999999,1.0074000000000001,30,500,64,5000,60,100]
[null,"Inlet Duct Area","2016-06-03","Steven Schroeder",{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to Inlet Duct Area"},null,"ACBL24_2W",null,1,5.05,4.37,4.07,3.79,3.32,2.96,2.96,2.96,2.7,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",309,416,412,406,510,506,607,604,601,null,"LIU24_2W","Ceiling mounted 24” wide 2-way discharge linear beam with 2 sloped coils and a drain pan",null,"PCBL",24,null,"PCBL",2,null,3,null,4,null,5,null,6,null,7,null,8,9,10,null,"PCBL",null,null,null,null,null,null,null,null,null,null,"PCBL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5eD",0.14299999999999999,null,"ACBM",4,5,2.73,1,0,1.3581000000000001,1.72E-2,1E-4,96.509152589999999,-38.129330699999997,0,-10519.575940000001,5284.4019289999997,-887.13754100000006,null,"ACBL12_2W",10,null,224,224,null,224,160,224,224,224,null,"PCBL",0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,0.1,null,"ACBL24_2W","cooling",2,16,null,"ACBM",0.81451711189999998,1.0687757040000001,1.003191612,0.2436714743,0.63078793529999999,1.845070735,null,"ACBC","2P1C",30,"heating",0,7.3,4.7496921590000003,0.67868702299999994,1.004689355,4.2982425999999997E-2,0.91471000000000002,1.8573,0,2.34,null,"PCBL",6,0.43133329860396419,1.2499803843933965,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"All","AHRI 880-2011 Min. Significant - LW",44.4,36,29,26,22,19,17,14.8,9.9,{"$f":"10*LOG(10^((HR20+HR$46)/10)+10^((HS20+HS$46)/10)+10^((HT20+HT$46)/10)+10^((HU20+HU$46)/10)+10^((HV20+HV$46)/10)+10^((HW20+HW$46)/10))","v":37.373157530603592},null,"ACBC_1W","log Inlet Vel",9,260.98750656535714,-1619.1850721331525,-1493.7483196636458,-1220.2215834320989,-1353.8456074455414,-1521.280229437242,-2003.1703120333516,-168.88051855020171,null,"ACBR",10,"5eE","ACBR_10_5eE",-1.2,-0.8,-4.5999999999999996,-6.5,-4.3,-2.8,-3.5,-0.9,null,"ACBR","30-3",3,30,0.35,20,0,null,"LIU24_2W",126.67686977437442,0.5,1.2999999999999999E-4,0.2,0.08,999.1,2.5,19,1,1,6,100,1.2998000000000001,2E-14,1,30,500,64,5000,60,100]
[null,"Sound Data","2016-06-03","Steven Schroeder",{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to Sound Data"},null,"ACBL12_1W",null,1,null,null,null,3.3,3.2,2.4,2.4,2.4,2.2000000000000002,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB",406,506,608,null,605,603,601,null,null,null,"RIU_FB","10.8\" D x 11.5\" H - Retrofit Induction unit. 1-way discharge ",null,"LIU24_2W",24,null,"LIU24_2W",2,null,3,null,4,null,5,null,6,null,7,null,8,null,null,null,"LIU24_2W",10,20,30,35,40,50,60,70,80,null,"LIU24_2W",null,null,null,null,null,null,null,null,null,"5",null,null,null,null,"5T",null,null,null,"6",null,"6T","8",null,null,"8T","10T",null,"5eE",0.14299999999999999,null,"ACBM",4,6,2.73,1,0,1.3581000000000001,1.72E-2,1E-4,93.294418429999993,-35.709181340000001,0,-9719.9621389999993,4882.5999430000002,-818.33844199999999,null,"ACBL12_1W",2,null,16,16,null,16,12,16,16,16,null,"LIU24_2W",0.1875,0.25,0.25,0.25,0.3,0.3,0.35,0.35,0.35,null,"ACBL24_2W","heating",2,16,null,null,null,null,null,null,null,null,null,"ACBC","2P2C",30,"heating",0,7.3,4.7496921590000003,0.67868702299999994,1.004689355,4.2982425999999997E-2,0.91471000000000002,1.8573,0,2.34,null,"LIU24_2W",6,2.525858684E-2,2.8122072830000001E-2,0,0,0,0,1.009602463,-7.1045935239999997E-2,0,0,0,-1.026958215E-4,-2.4502330479999998E-3,0,0,8.9144198630000004E-2,5.6137945609999997E-2,-1.7672059510000001E-2,0.71330000000000005,0,-0.52717582529999996,1.7862114120000001,1.158704183,0,1,null,null,null,null,null,null,null,0.31360820700000003,0.83949681470000004,0.45487818499999999,1.0493849930000001,null,null,null,null,-0.18086831370815601,0.73166913734043604,0.27510781049999999,-1.75687965E-3,-2.4487134319999999E-2,0.71453753789999996,null,"LIU24_2W","A-Weighting",-26.2,-16.100000000000001,-8.6,-3.2,0,1.2,1,-1.1000000000000001,"",{"$f":"10*LOG(10^((HR21+HR$46)/10)+10^((HS21+HS$46)/10)+10^((HT21+HT$46)/10)+10^((HU21+HU$46)/10)+10^((HV21+HV$46)/10)+10^((HW21+HW$46)/10))","v":6.2514752753391667},null,"ACBC_1W","log slot vel",10,-1496.5617811973511,317.82256080488304,688.86322178626506,732.29105062148369,1004.2196170676293,456.26763981590017,443.16110703987175,-1149.7590513131202,null,"ACBR",10,"6eC","ACBR_10_6eC",-0.1,-0.4,-3.2,-4.7,-3.3,-2.4,-3.6,-1.2,null,"ACBR","40-3",3,40,0.35,26,0,null,"RIU_FB",81.073196655599602,0.5,1.2667686977437442E-4,0.2,0.08,999.1,2.5,19,1,1,3.33,100,1.256,-5.3999999999999999E-2,0.66,30,500,64,5000,60,100]
[null,"Nozzles Per Beam","2016-09-15","Steven Schroeder",{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to Nozzles Per Beam"},null,"ACBL12_2W",null,1,3.6,2.9,null,2.6,2.2000000000000002,2.1,2.1,2.1,1.5,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB",406,506,608,null,605,603,601,null,null,null,"RIU_TB","7\" D x 17\" H - Retrofit Induction unit. 1-way discharge ",null,"RIU_FB",10.8,null,"RIU_FB",2,2.67,null,3.33,null,4.33,null,5.33,null,6.33,null,7.3440000000000003,null,null,null,null,"RIU_FB",10,20,30,null,40,50,60,null,null,null,"RIU_FB","3",null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6eC",0.16400000000000001,null,"ACBM",4,8,2.73,1,0,1.3581000000000001,1.72E-2,1E-4,67.631624479999999,-8.3675625060000005,0,-4117.619737,2075.9728700000001,-426.6523828,null,"ACBL12_1W",3,null,28,28,null,28,20,28,28,28,null,"RIU_FB",0.25,0.3,0.35,null,0.35,0.35,0.35,null,null,null,"ACBL24_2W","cooling",4,12,null,null,null,null,null,null,null,null,null,"ACBC","4P1C",30,"heating",0,7.3,4.6726090850000004,0.590323775,0.98099430300000001,6.4770559000000005E-2,0.91471000000000002,1.8573,0,2.34,null,"RIU_FB",3.33,1.3205E-2,1.0191E-2,1.008051,0,7.6985999999999999E-2,-7.4529999999999999E-2,1.1122920000000001,0.29064299999999998,1.4970000000000001E-3,-2.3369999999999998E-2,-4.4200000000000003E-3,9.4280000000000006E-3,5.7169999999999999E-3,0.14185200000000001,3.2927999999999999E-2,0.159137,4.8828999999999997E-2,-0.19306999999999999,0.70060699999999998,2.5166000000000001E-2,-0.46490999999999999,2.1522480000000002,1.073197,0.12984899999999999,1.2140679999999999,null,null,null,null,null,null,null,0.482267,0.95121999999999995,0.11314,0.88423600000000002,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","A-Weighting",-26.2,-16.100000000000001,-8.6,-3.2,0,1.2,1,-1.1000000000000001,"",{"$f":"10*LOG(10^((HR22+HR$46)/10)+10^((HS22+HS$46)/10)+10^((HT22+HT$46)/10)+10^((HU22+HU$46)/10)+10^((HV22+HV$46)/10)+10^((HW22+HW$46)/10))","v":6.2514752753391667},null,"ACBC_1W","log slot area",11,-128.61866372191756,828.39565737233409,777.53785701481172,645.84778768004435,716.65974754042918,799.77527887912925,1040.747310998298,114.41745147464331,null,"ACBR",10,"6eD","ACBR_10_6eD",0,0,0,0,0,0,0,0,null,"ACBR","50-3",3,50,0.35,30,0,null,"RIU_TB",81.073196655599631,0.5,1.2667686977437442E-4,0.2,0.08,999.1,2.5,19,1,1,3.33,100,1.256,-5.3999999999999999E-2,0.66,30,500,64,5000,60,100]
[null,"Nozzle Diameters","2016-09-15","Steven Schroeder",{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to Nozzle Diameters"},null,"PCBL",null,1,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB",406,506,608,null,605,603,601,null,null,null,"RIU_LB","8.8\" D x 11.5\" H - Retrofit Induction unit. 1-way discharge ",null,"RIU_TB",7,null,"RIU_TB",2,2.67,null,3.33,null,4.33,null,5.33,null,6.33,null,7.3440000000000003,null,null,null,null,"RIU_TB",10,20,30,null,40,50,60,null,null,null,"RIU_TB","3",null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6eD",0.16400000000000001,null,"PCBL",null,null,1,1,0,0,0,0,0,0,0,0,0,0,null,"ACBL12_1W",4,null,40,40,null,40,28,40,40,40,null,"RIU_TB",0.25,0.3,0.35,null,0.35,0.35,0.35,null,null,null,"ACBL24_2W","heating",4,4,null,null,null,null,null,null,null,null,null,"ACBC","4P2C",30,"heating",0.05,7.3,4.6726090850000004,0.590323775,0.98099430300000001,6.4770559000000005E-2,0.91471000000000002,1.8573,0,2.34,null,"RIU_TB",3.33,1.3205E-2,1.0191E-2,1.008051,0,7.6985999999999999E-2,-7.4529999999999999E-2,1.1122920000000001,0.29064299999999998,1.4970000000000001E-3,-2.3369999999999998E-2,-4.4200000000000003E-3,9.4280000000000006E-3,5.7169999999999999E-3,0.14185200000000001,3.2927999999999999E-2,0.159137,4.8828999999999997E-2,-0.19306999999999999,0.70060699999999998,2.5166000000000001E-2,-0.46490999999999999,2.1522480000000002,1.073197,0.12984899999999999,1.2140679999999999,null,null,null,null,null,null,null,0.482267,0.95121999999999995,0.11314,0.88423600000000002,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","A-Weighting",-26.2,-16.100000000000001,-8.6,-3.2,0,1.2,1,-1.1000000000000001,"",6.2514752753391667,null,"ACBC_1W","log Ainlet/ Anozzle",12,0,0,0,0,0,0,0,0,null,"ACBR",10,"6eE","ACBR_10_6eE",-0.5,-0.3,-3.7,-4.4000000000000004,-3,-1.9,-2.8,-0.8,null,"ACBR","60-3",3,60,0.35,36,0,null,"RIU_LB",81.073196655599631,0.5,1.2667686977437442E-4,0.2,0.08,999.1,2.5,19,1,1,3.33,100,1.256,-5.3999999999999999E-2,0.66,30,500,64,5000,60,100]
[null,"Number Of Coil Passes","2016-09-15","Steven Schroeder",{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to Number Of Coil Passes"},null,"LIU24_2W",null,1,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP",406,506,608,null,605,603,601,null,null,null,"ACBR_LP","8.8\" D x 11.5\" H - Retrofit Induction unit. 1-way discharge ",null,"RIU_LB",8.8000000000000007,null,"RIU_LB",2,2.67,null,3.33,null,4.33,null,5.33,null,6.33,null,7.3440000000000003,null,null,null,null,"RIU_LB",10,20,30,null,40,50,60,null,null,null,"RIU_LB",null,"3E",null,null,null,null,null,null,"4E",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6eE",0.16400000000000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W",5,null,52,52,null,52,38,52,52,52,null,"RIU_LB",0.25,0.3,0.35,null,0.35,0.35,0.35,null,null,null,"ACBL24_1W","cooling",2,16,null,null,null,null,null,null,null,null,null,"ACBC","4P1C",40,"cooling",0,7.3,3.2256091152397421,0.7628658201342321,0.99346880637190782,5.9947113698384985E-2,0.89362446951179353,1.7638655105941077,0,2.06,null,"RIU_LB",3.33,1.3205E-2,1.0191E-2,1.008051,0,7.6985999999999999E-2,-7.4529999999999999E-2,1.1122920000000001,0.29064299999999998,1.4970000000000001E-3,-2.3369999999999998E-2,-4.4200000000000003E-3,9.4280000000000006E-3,5.7169999999999999E-3,0.14185200000000001,3.2927999999999999E-2,0.159137,4.8828999999999997E-2,-0.19306999999999999,0.70060699999999998,2.5166000000000001E-2,-0.46490999999999999,2.1522480000000002,1.073197,0.12984899999999999,1.2140679999999999,null,null,null,null,null,null,null,0.482267,0.95121999999999995,0.11314,0.88423600000000002,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","A-Weighting",-26.2,-16.100000000000001,-8.6,-3.2,0,1.2,1,-1.1000000000000001,"",6.2514752753391667,null,"ACBC_1W","log calculated TPVP",13,-618.60390165401157,-666.48342059105903,-425.66863372081207,-273.76201061015877,-204.23140547940542,-559.71845243190057,-803.15034696273119,-681.63605367088348,null,"ACBR",20,"3B","ACBR_20_3B",0,0,0,0,0,0,0,0,null,"ACBR","10-4",4,10,0.25,32,0,null,"ACBR_LP",81.073196655599602,0.5,1.2667686977437442E-4,0.2,0.08,999.1,2.5,19,1,1,3.33,100,1.256,-5.3999999999999999E-2,0.66,30,500,64,5000,60,100]
[null,"Coil Water Pressure Drop","2016-06-06","Steven Schroeder",{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to Coil Water Pressure Drop"},null,"RIU_FB",null,1,4.2955077781361535,3.6462094095916582,null,null,3.279806658718901,2.7187297312016185,2.5405474990721024,2.222149804379645,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP",8.8000000000000007,null,"ACBR_LP",2,2.67,null,3.33,null,4.33,null,5.33,null,6.33,null,7.3440000000000003,null,null,null,null,"ACBR_LP",10,20,30,null,40,50,60,null,null,null,"ACBR_LP",null,"3E",null,null,null,null,null,null,"4E",null,null,null,null,null,null,null,null,null,null,"6E",null,null,null,null,null,null,null,"3",4.9000000000000002E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W",6,null,64,64,null,64,46,64,64,64,null,"ACBR_LP",0.25,0.3,0.35,null,0.35,0.35,0.35,null,null,null,"ACBL24_1W","heating",2,16,null,null,null,null,null,null,null,null,null,"ACBC","4P2C",40,"cooling",-0.06,7.3,3.2256091152397421,0.7628658201342321,0.99346880637190782,5.9947113698384985E-2,0.89362446951179353,1.7638655105941077,0,2.06,null,"ACBR_LP",3.33,1.3205E-2,1.0191E-2,1.008051,0,7.6985999999999999E-2,-7.4529999999999999E-2,1.1122920000000001,0.29064299999999998,1.4970000000000001E-3,-2.3369999999999998E-2,-4.4200000000000003E-3,9.4280000000000006E-3,5.7169999999999999E-3,0.14185200000000001,3.2927999999999999E-2,0.159137,4.8828999999999997E-2,-0.19306999999999999,0.70060699999999998,2.5166000000000001E-2,-0.46490999999999999,2.1522480000000002,1.073197,0.12984899999999999,1.2140679999999999,null,null,null,null,null,null,null,0.482267,0.95121999999999995,0.11314,0.88423600000000002,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","A-Weighting",-26.2,-16.100000000000001,-8.6,-3.2,0,1.2,1,-1.1000000000000001,"",6.2514752753391667,null,"ACBC_1W","log Inlet Area",14,-8.0979128128951228,-7.1887266831888041,-23.055474174802011,-43.87685871006245,-38.646122486572395,-31.698916110072599,-17.606801478139239,-42.675306303455514,null,"ACBR",20,"4B","ACBR_20_4B",0,0,0,0,0,0,0,0,null,"ACBR","20-4",4,20,0.3,32,0]
[null,"Performance Constants","2016-09-15","Steven Schroeder",{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to Performance Constants"},null,"RIU_TB",null,1,4.2955077781361535,3.6462094095916582,null,null,3.279806658718901,2.7187297312016185,2.5405474990721024,2.222149804379645,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4",8.6999999999999994E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W",7,null,76,76,null,76,54,76,76,76,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","cooling",4,12,null,null,null,null,null,null,null,null,null,"ACBC","2P1C",40,"heating",0,7.3,3.2256091152397421,0.7628658201342321,0.99346880637190782,5.9947113698384985E-2,0.89362446951179353,1.7638655105941077,0,2.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_1W","intercept",15,-1697.5870883504545,6096.0385307868692,5888.5671962548322,4980.2567827588509,5599.3809291347598,5882.7640923403087,7577.9962126562605,133.37713376460584,null,"ACBR",20,"4C","ACBR_20_4C",-1.3,-2,-4,-2.6,-1.6,-1.9,-3.9,-2.6,null,"ACBR","30-4",4,30,0.35,28,0]
[null,"New Performance Constants","2018-10-01","Elijah Smith",{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to New Performance Constants"},null,"RIU_LB",null,1,4.2955077781361535,3.6462094095916582,null,null,3.279806658718901,2.7187297312016185,2.5405474990721024,2.222149804379645,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5",0.13600000000000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W",8,null,88,88,null,88,64,88,88,88,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","heating",4,4,null,null,null,null,null,null,null,null,null,"ACBC","2P2C",40,"heating",0,7.3,3.2256091152397421,0.7628658201342321,0.99346880637190782,5.9947113698384985E-2,0.89362446951179353,1.7638655105941077,0,2.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_1W","r^2",16,0.57375260037486764,0.90734297958807375,0.98989621137538408,0.98994408448700788,0.98371428821859153,0.97380065896040724,0.96010628902431883,0.89574953307092275,null,"ACBR",20,"4D","ACBR_20_4D",-0.5,-3.8,-4.5999999999999996,-3.6,-2.1,-1.4,-3.2,-4,null,"ACBR","40-4",4,40,0.35,34,0]
[null,"A_Weighting","2018-10-01","Elijah Smith",{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to A_Weighting"},null,"ACBR_LP",null,1,4.2955077781361535,3.6462094095916582,null,null,3.279806658718901,2.7187297312016185,2.5405474990721024,2.222149804379645,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5E",0.111,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W",9,null,100,100,null,100,72,100,100,100,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR","cooling",2,16,null,null,null,null,null,null,null,null,null,"ACBC","4P1C",40,"heating",0,7.3,3.5065644395949489,0.65657123811247176,0.98726946002844929,6.7434649461362031E-2,0.89362446951179353,1.7638655105941077,0,2.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W","log inlet vel",17,-774.4605551624478,-432.68984662598911,-338.41081627123054,-344.77062323112523,-318.31608951087691,-195.03013199736344,-13.228743852760683,256.76006920806782,null,"ACBR",20,"4E","ACBR_20_4E",-1.6,-2,-7.8,-10.9,-8.1,-4.8,-5.3,-3.2,null,"ACBR","50-4",4,50,0.35,40,0]
[null,"Log Sound","2018-10-01","Elijah Smith",{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to Log Sound"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6",0.19600000000000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W",10,null,112,112,null,112,80,112,112,112,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR","heating",2,16,null,null,null,null,null,null,null,null,null,"ACBC","4P2C",40,"heating",0.06,7.3,3.5065644395949489,0.65657123811247176,0.98726946002844929,6.7434649461362031E-2,0.89362446951179353,1.7638655105941077,0,2.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W","log nozzle area",18,0,0,0,0,0,0,0,0,null,"ACBR",20,"5eC","ACBR_20_5eC",-0.7,-0.7,-3.5,-4.0999999999999996,-3.1,-2.2000000000000002,-3.3,-1.5,null,"ACBR","60-4",4,60,0.35,48,0]
[null,"Inlet Location Factors","2018-10-01","Elijah Smith",{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to Inlet Location Factors"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6E",0.17100000000000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",2,18,14,16,22,18,22,20,24,32,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR","cooling",4,12,null,null,null,null,null,null,null,null,null,"ACBC","4P1C",50,"cooling",0,7.3,3.0803558726862641,0.75993880949929782,1.0013235004419103,6.9579845535146345E-2,0.70140779250079677,1.7580044850242893,0,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W","log SP",19,389.24896388466686,236.44913817555693,197.10132689804774,200.84803209320134,192.71056863174749,138.22242837458396,44.993521678528886,-104.03387034250716,null,"ACBR",20,"5eD","ACBR_20_5eD",0,0,0,0,0,0,0,0,null,"ACBR","10-5",5,10,0.25,40,0]
[null,"Nozzle Data","2018-10-01","Elijah Smith",{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to Nozzle Data"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8",0.34899999999999998,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",3,30,22,28,38,30,38,34,42,56,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR","heating",4,4,null,null,null,null,null,null,null,null,null,"ACBC","4P2C",50,"cooling",-0.1,7.3,3.0803558726862641,0.75993880949929782,1.0013235004419103,6.9579845535146345E-2,0.70140779250079677,1.7580044850242893,0,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W","log AD/AN",20,0,0,0,0,0,0,0,0,null,"ACBR",20,"5eE","ACBR_20_5eE",-1.2,-0.8,-4.5999999999999996,-6.5,-4.3,-2.8,-3.5,-0.9,null,"ACBR","20-5",5,20,0.3,40,0]
[null,"Reference Values","2018-10-01","Elijah Smith",{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to Reference Values"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"`",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8E",0.254,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",4,44,32,38,54,42,54,48,60,80,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_1W","cooling",2,8,null,null,null,null,null,null,null,null,null,"ACBC","2P1C",50,"heating",0,7.3,3.0803558726862641,0.75993880949929782,1.0013235004419103,6.9579845535146345E-2,0.70140779250079677,1.7580044850242893,0,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W","log TP/VP",21,-400.99695518841236,-228.81877752283987,-179.72910657191753,-181.65702476106134,-169.15188880826923,-106.701801351931,-12.194378198668872,129.1179011726077,null,"ACBR",20,"6eC","ACBR_20_6eC",-0.1,-0.4,-3.2,-4.7,-3.3,-2.4,-3.6,-1.2,null,"ACBR","30-5",5,30,0.35,34,0]
[null,"Conversion Ratios","2018-10-01","Elijah Smith",{"$f":"HYPERLINK(CONCATENATE(\"#\",SUBSTITUTE(LookupTables[[#This Row],[Table Name]],\" \",\"\")), CONCATENATE(\"Link to \",LookupTables[[#This Row],[Table Name]]))","v":"Link to Conversion Ratios"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5T",0.13600000000000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",5,56,42,50,66,56,70,64,78,104,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_1W","heating",2,8,null,null,null,null,null,null,null,null,null,"ACBC","2P2C",50,"heating",0,7.3,3.0803558726862641,0.75993880949929782,1.0013235004419103,6.9579845535146345E-2,0.70140779250079677,1.7580044850242893,0,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W","log # of nozzles",22,0,0,0,0,0,0,0,0,null,"ACBR",20,"6eD","ACBR_20_6eD",0,0,0,0,0,0,0,0,null,"ACBR","40-5",5,40,0.35,42,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6T",0.19600000000000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",6,70,52,62,82,68,86,78,96,128,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_1W","cooling",4,12,null,null,null,null,null,null,null,null,null,"ACBC","4P1C",50,"heating",0,7.3,2.6791729301721063,0.66391118745543432,1.0472150488370877,9.1844196366672529E-2,0.70140779250079677,1.7580044850242893,0,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W","Intercept",23,2866.5148471564953,1622.7221533387881,1278.4861779532062,1302.1990291177244,1207.0193089304773,757.59442488413083,91.960211106948435,-893.97210191575766,null,"ACBR",20,"6eE","ACBR_20_6eE",-0.5,-0.3,-3.7,-4.4000000000000004,-3,-1.9,-2.8,-0.8,null,"ACBR","50-5",5,50,0.35,50,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"8T",0.34899999999999998,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",7,82,62,72,98,80,102,92,114,152,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_1W","heating",4,4,null,null,null,null,null,null,null,null,null,"ACBC","4P2C",50,"heating",7.0000000000000007E-2,7.3,2.6791729301721063,0.66391118745543432,1.0472150488370877,9.1844196366672529E-2,0.70140779250079677,1.7580044850242893,0,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W","r²",24,0.73252552433974749,0.96000330804681233,0.99592646288112963,0.99410379901267754,0.99210759251379732,0.98994509779603634,0.97533816098248327,0.87902397205760652,null,"ACBR",30,"3B","ACBR_30_3B",0,0,0,0,0,0,0,0,null,"ACBR","60-5",5,60,0.35,60,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10T",0.54500000000000004,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",8,96,70,84,114,94,118,106,134,176,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W","cooling",4,6,null,null,null,null,null,null,null,null,null,"ACBC","4P1C",60,"cooling",0,7.3,3.0734312629468401,0.75665684146709566,1.0518301977181677,2.5730968899201005E-2,0.45845939209473796,1.7497254197165204,0,1.76,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","log slot vel",25,5.8185533158805365,19.863275038851082,44.820834090189138,45.960434003660211,35.630090241291001,26.498399792831986,17.782812440806374,19.067031619761952,null,"ACBR",30,"4B","ACBR_30_4B",0,0,0,0,0,0,0,0,null,"ACBR","10-6",6,10,0.25,48,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",9,108,80,96,130,106,134,122,152,200,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W","heating",4,6,null,null,null,null,null,null,null,null,null,"ACBC","4P2C",60,"cooling",-0.08,7.3,3.0734312629468401,0.75665684146709566,1.0518301977181677,2.5730968899201005E-2,0.45845939209473796,1.7497254197165204,0,1.76,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","log slot area",26,8.1204052319919278,-9.597172911511139,2.8395849471008683,-15.073970905232905,-24.150821971606849,-13.641557763240394,-8.45845051514498,-38.671781476115285,null,"ACBR",30,"4C","ACBR_30_4C",0.25,2.65,3.5,4.7,5.85,4.9000000000000004,1.75,-0.19999999999999996,null,"ACBR","20-6",6,20,0.3,48,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",10,122,90,108,146,118,150,136,170,224,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","cooling",2,16,null,null,null,null,null,null,null,null,null,"ACBC","2P1C",60,"heating",0,7.3,3.0734312629468401,0.75665684146709566,1.0518301977181677,2.5730968899201005E-2,0.45845939209473796,1.7497254197165204,0,1.76,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","log Ainlet/ Anozzle",27,6.5974670543800036,826.56969445116408,501.96807769033484,152.12997378067936,89.546436543253066,516.41925207490556,56.401815808927253,-369.75456527723469,null,"ACBR",30,"4D","ACBR_30_4D",0.55000000000000004,2.9,3.2,3.5,4.0999999999999996,4.2,1.6,0.25,null,"ACBR","30-6",6,30,0.35,42,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W",2,9,7,8,11,9,11,10,12,16,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","heating",2,16,null,null,null,null,null,null,null,null,null,"ACBC","2P2C",60,"heating",0,7.3,3.0734312629468401,0.75665684146709566,1.0518301977181677,2.5730968899201005E-2,0.45845939209473796,1.7497254197165204,0,1.76,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","log calculated TPVP",28,-3.3370566588928758,-417.51046807107906,-251.646408903246,-76.236487248691873,-46.525520979523158,-263.85115810861231,-30.180561355763359,187.4246272071625,null,"ACBR",30,"4E","ACBR_30_4E",-2.5,-3.7,-5.6,-6.9,-7.7,-6.7,1.4,4,null,"ACBR","40-6",6,40,0.35,50,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W",3,15,11,14,19,15,19,17,21,28,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","cooling",4,16,null,null,null,null,null,null,null,null,null,"ACBC","4P1C",60,"heating",0,7.3,2.4019931051509755,0.68565453172569879,1.0200092093093411,8.2316950533224353E-2,0.45845939209473796,1.7497254197165204,0,1.76,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","log Nozzle Vel",29,174.38629967892612,-602.52346566325173,-608.37632823089803,-1237.6289773272201,-1315.6963717842987,-851.68190106533052,-511.59790788930701,-1483.4030235359714,null,"ACBR",30,"5eC","ACBR_30_5eC",-0.7,-0.7,-3.5,-4.0999999999999996,-3.1,-2.2000000000000002,-3.3,-1.5,null,"ACBR","50-6",6,50,0.35,60,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W",4,22,16,19,27,21,27,24,30,40,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","heating",4,8,null,null,null,null,null,null,null,null,null,"ACBC","4P2C",60,"heating",7.0000000000000007E-2,7.3,2.4019931051509755,0.68565453172569879,1.0200092093093411,8.2316950533224353E-2,0.45845939209473796,1.7497254197165204,0,1.76,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","log SP",30,-85.141282659223975,303.22210515255443,298.877411360172,615.80137457976605,666.36205909064336,446.58601602890474,282.91120115396626,755.39931681309758,null,"ACBR",30,"5eD","ACBR_30_5eD",0,0,0,0,0,0,0,0,null,"ACBR","60-6",6,60,0.35,72,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W",5,28,21,25,33,28,35,32,39,52,null,null,null,null,null,null,null,null,null,null,null,null,"PCBL","cooling",2,12,null,null,null,null,null,null,null,null,null,"ACBC","4P1C",70,"cooling",0,7.3,2.272210469,0.77998774599999998,1.032413977,4.9319505999999999E-2,0.17398,1.91073,0,1.52,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","log no of nozz/ft",31,-0.74536437582086446,4.6128076538648628,11.916336926128462,5.8085845845616442,7.7797717374299777,3.2148107156258496,3.9034118717781716,0.83376743180776158,null,"ACBR",30,"5eE","ACBR_30_5eE",-1.2,-0.8,-4.5999999999999996,-6.5,-4.3,-2.8,-3.5,-0.9,null,"ACBR","10-7",7,10,0.25,56,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W",6,35,26,31,41,34,43,39,48,64,null,null,null,null,null,null,null,null,null,null,null,null,"PCBL","cooling",4,12,null,null,null,null,null,null,null,null,null,"ACBC","4P2C",70,"cooling",-7.0000000000000007E-2,7.3,2.272210469,0.77998774599999998,1.032413977,4.9319505999999999E-2,0.17398,1.91073,0,1.52,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","Intercept",32,-581.45272339627923,2176.2706214111922,2093.1129099730597,4295.1109138491247,4594.3686641591885,3015.99692670901,1795.4038450928649,5192.3582487759932,null,"ACBR",30,"6eC","ACBR_30_6eC",-0.5,0.2,2.6,2.9,0.5,-2.2000000000000002,2.1,5.6,null,"ACBR","20-7",7,20,0.3,56,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W",7,41,31,36,49,40,51,46,57,76,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","cooling",2,20,null,null,null,null,null,null,null,null,null,"ACBC","2P1C",70,"heating",0,7.3,2.272210469,0.77998774599999998,1.032413977,4.9319505999999999E-2,0.17398,1.91073,0,1.52,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","r^2",33,0.46943103764844052,0.81940233247477745,0.9053282864680503,0.90176670230728562,0.92616084746223526,0.92383890903343591,0.92741819778497092,0.75327361954056116,null,"ACBR",30,"6eD","ACBR_30_6eD",0,0,0,0,0,0,0,0,null,"ACBR","30-7",7,30,0.35,48,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W",8,48,35,42,57,47,59,53,67,88,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","heating",2,20,null,null,null,null,null,null,null,null,null,"ACBC","2P2C",70,"heating",0,7.3,2.272210469,0.77998774599999998,1.032413977,4.9319505999999999E-2,0.17398,1.91073,0,1.52,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","log slot vel",34,5.858702645643671,28.103691384729593,48.55670929887436,52.9347093900654,53.622237692638947,37.77032164506798,21.654852067356376,11.555819552028531,null,"ACBR",30,"6eE","ACBR_30_6eE",-0.7,-0.5,1.5,1.4,-0.8,-3,2.4,5.4,null,"ACBR","40-7",7,40,0.35,60,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W",9,54,40,48,65,53,67,61,76,100,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","cooling",4,14,null,null,null,null,null,null,null,null,null,"ACBC","4P1C",70,"heating",0,7.3,2.467831168,0.67004910299999998,1.0066897669999999,7.4180053999999995E-2,0.17398,1.91073,0,1.52,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","log slot area",35,-3.1695567151222108,16.178051403507954,1.914155212940406,-9.8720768778609855,-10.805638564993536,-12.679742982245193,-20.220995443965759,-41.509098614017873,null,"ACBR",40,"3B","ACBR_40_3B",0,0,0,0,0,0,0,0,null,"ACBR","50-7",7,50,0.35,70,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W",10,61,45,54,73,59,75,68,85,112,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","heating",4,6,null,null,null,null,null,null,null,null,null,"ACBC","4P2C",70,"heating",0.06,7.3,2.467831168,0.67004910299999998,1.0066897669999999,7.4180053999999995E-2,0.17398,1.91073,0,1.52,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","log Ainlet/ Anozzle",36,321.77633646736098,485.34615215875453,284.11627733738953,37.050306541762495,-68.856353913696339,84.398818882638878,190.74494177172537,164.73920153623658,null,"ACBR",40,"4B","ACBR_40_4B",0,0,0,0,0,0,0,0,null,"ACBR","60-7",7,60,0.35,84,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM",2,null,64,64,null,64,64,64,64,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","cooling",2,16,null,null,null,null,null,null,null,null,null,"ACBC","4P1C",80,"cooling",0,7.3,2.2903737738860772,0.69750119547793821,1.0653582365223337,5.9636832522870713E-2,0.29617311576777983,1.6530677080861371,0,1.28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","log calculated TPVP",37,-165.94025805618202,-251.42016136316576,-147.17604324533241,-19.548101073239152,34.291008094735702,-47.325399664910698,-100.63620909509585,-85.487547408750714,null,"ACBR",40,"4C","ACBR_40_4C",0.25,2.65,3.5,4.7,5.85,4.9000000000000004,1.75,-0.19999999999999996,null,"ACBR","10-8",8,10,0.25,64,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM",4,null,112,112,null,112,112,112,112,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","heating",2,16,null,null,null,null,null,null,null,null,null,"ACBC","4P2C",80,"cooling",-0.04,7.3,2.2903737738860772,0.69750119547793821,1.0653582365223337,5.9636832522870713E-2,0.29617311576777983,1.6530677080861371,0,1.28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","log Nozzle Vel",38,-179.08212149144751,11.836304214365565,-614.19510006255859,-925.00504026909152,-838.33176465065981,-633.0454458040092,-564.70307563822462,-1050.4917223911568,null,"ACBR",40,"4D","ACBR_40_4D",0.55000000000000004,2.9,3.2,3.5,4.0999999999999996,4.2,1.6,0.25,null,"ACBR","20-8",8,20,0.3,64,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR",2,16,16,14,null,16,20,24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","cooling",4,12,null,null,null,null,null,null,null,null,null,"ACBC","2P1C",80,"heating",0.05,7.3,2.2903737738860772,0.69750119547793821,1.0653582365223337,5.9636832522870713E-2,0.29617311576777983,1.6530677080861371,0,1.28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","log Nozzle size",39,91.244120348268822,-5.9414997377130367,301.83377042844864,457.44146568821844,419.37654583616359,329.86711878297444,305.33660545067278,542.76497923509237,null,"ACBR",40,"4E","ACBR_40_4E",-2.5,-3.7,-5.6,-6.9,-7.7,-6.7,1.4,4,null,"ACBR","30-8",8,30,0.35,56,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR",3,24,24,20,null,26,30,36,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","heating",4,4,null,null,null,null,null,null,null,null,null,"ACBC","2P2C",80,"heating",0.06,7.3,2.2903737738860772,0.69750119547793821,1.0653582365223337,5.9636832522870713E-2,0.29617311576777983,1.6530677080861371,0,1.28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","log no of nozz/ft",40,4.5762479450186104,11.434650502935639,15.521448027590891,15.364447833141256,18.277076526347468,26.344549713892402,37.016023952630711,27.875159419955498,null,"ACBR",40,"5eC","ACBR_40_5eC",-0.7,-0.7,-3.5,-4.0999999999999996,-3.1,-2.2000000000000002,-3.3,-1.5,null,"ACBR","40-8",8,40,0.35,68,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR",4,32,32,28,null,34,40,48,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","cooling",2,16,null,null,null,null,null,null,null,null,null,"ACBC","4P1C",80,"heating",0,7.3,2.6868133694074037,0.59247546727531231,1.0428095848891554,7.1102490708863805E-2,0.29617311576777983,1.6530677080861371,0,1.28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","Intercept",41,697.90072781305491,-31.281836658887173,2094.3059164307265,3152.4842370440756,2830.3969088169747,2158.3947018476429,1956.3450181766596,3701.1360586861956,null,"ACBR",40,"5eD","ACBR_40_5eD",0,0,0,0,0,0,0,0,null,"ACBR","50-8",8,50,0.35,80,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR",5,40,40,34,null,42,50,60,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","heating",2,16,null,null,null,null,null,null,null,null,null,"ACBC","4P2C",80,"heating",0.05,7.3,2.6868133694074037,0.59247546727531231,1.0428095848891554,7.1102490708863805E-2,0.29617311576777983,1.6530677080861371,0,1.28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","r^2",42,0.66550082275834233,0.82933083016891762,0.94028584410976324,0.94298855517383251,0.95646939249178076,0.96342664455897331,0.93770013902721638,0.78802018942251828,null,"ACBR",40,"5eE","ACBR_40_5eE",-1.2,-0.8,-4.5999999999999996,-6.5,-4.3,-2.8,-3.5,-0.9,null,"ACBR","60-8",8,60,0.35,96,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR",6,48,48,42,null,50,60,72,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","cooling",4,12,null,null,null,null,null,null,null,null,null,"ACBC_1W","FTH",0,"heating",0,3,0.76360010599972705,3.6506486728727409E-2,1.6102821516629802,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","log slot vel",43,2.9921141177023887,35.914867436781229,59.864043866496168,64.567645708456482,71.654579764764577,64.40842596573394,36.327151323226005,9.942808379102507,null,"ACBR",40,"6eC","ACBR_40_6eC",-0.5,0.2,2.6,2.9,0.5,-2.2000000000000002,2.1,5.6,null,"ACBC_2W",{"$f":"CONCATENATE(JD54,\"-\",JC54)","v":"50-3"},3,50,0.25,76,33]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR",7,56,56,48,null,60,70,84,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","heating",4,4,null,null,null,null,null,null,null,null,null,"ACBC_1W","2P1C",20,"cooling",0,7.3,6.097002570006798,0.64617580138468744,0.96180153927094336,4.5202387620426512E-2,3.7482812306102402,1.5393799567659041,0,2.54,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","log slot area",44,1.6191340370105551,-2.9396258010167076,-3.9634217800067608,12.072871626185373,44.473273488193634,35.250710390407804,9.0369918521272758,-6.6071851404317439,null,"ACBR",40,"6eD","ACBR_40_6eD",0,0,0,0,0,0,0,0,null,"ACBC_2W",{"$f":"CONCATENATE(JD55,\"-\",JC55)","v":"50-4"},4,50,0.25,110,47]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR",8,64,64,56,null,68,80,96,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","cooling",2,16,null,null,null,null,null,null,null,null,null,"ACBC_1W","2P1C",30,"cooling",0,7.3,4.7496921590000003,0.67868702299999994,1.004689355,4.2982425999999997E-2,0.91471000000000002,1.8573,0,2.34,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","log Ainlet/ Anozzle",45,6.4522894081997642,-25.386956166084797,-42.650366540224766,-40.708083502691153,-43.292029987656214,-20.463774681081716,-25.125725468715352,-17.548237656876093,null,"ACBR",40,"6eE","ACBR_40_6eE",-0.7,-0.5,1.5,1.4,-0.8,-3,2.4,5.4,null,"ACBC_2W","50-5",5,50,0.25,144,61]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_1W",3,null,null,null,null,null,39,null,43,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","heating",2,16,null,null,null,null,null,null,null,null,null,"ACBC_1W","2P1C",40,"cooling",0,7.3,3.2256091152397421,0.7628658201342321,0.99346880637190782,5.9947113698384985E-2,0.89362446951179353,1.7638655105941077,0,2.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","log calculated TPVP",46,-2.9954273879654285,13.537837307422416,22.466151364700814,21.709321051667668,25.135163486477815,13.129179622527262,13.807564286880329,8.17443912678225,null,"ACBR",50,"3B","ACBR_50_3B",0,0,0,0,0,0,0,0,null,"ACBC_2W","50-6",6,50,0.25,178,75]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_1W",4,null,null,null,null,null,59,null,63,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","cooling",4,12,null,null,null,null,null,null,null,null,null,"ACBC_1W","2P1C",50,"cooling",0,7.3,3.0803558726862641,0.75993880949929782,1.0013235004419103,6.9579845535146345E-2,0.70140779250079677,1.7580044850242893,0,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","log Nozzle Vel",47,60.671357198496622,213.2117232240484,203.46991878898032,-203.99338501697648,-1113.6329693367684,-965.90691474842413,-235.25646702520817,164.65413912941321,null,"ACBR",50,"4B","ACBR_50_4B",0,0,0,0,0,0,0,0,null,"ACBC_2W","50-7",7,50,0.25,212,89]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_1W",5,null,null,null,null,null,75,null,79,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","heating",4,4,null,null,null,null,null,null,null,null,null,"ACBC_1W","2P1C",60,"cooling",0,7.3,3.0734312629468401,0.75665684146709566,1.0518301977181677,2.5730968899201005E-2,0.45845939209473796,1.7497254197165204,0,1.76,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","log Nozzle size",48,-29.906464715696409,-106.69103979251111,-105.69350837194376,100.41281529656489,558.6341028886668,491.3509347955158,135.42833481368254,-63.61974292959561,null,"ACBR",50,"4C","ACBR_50_4C",0.25,2.65,3.5,4.7,5.85,4.9000000000000004,1.75,-0.19999999999999996,null,"ACBC_1W","50-3",3,50,0.25,39,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_1W",6,null,null,null,null,null,91,null,99,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","cooling",2,16,null,null,null,null,null,null,null,null,null,"ACBC_1W","2P1C",70,"cooling",0,7.3,2.272210469,0.77998774599999998,1.032413977,4.9319505999999999E-2,0.17398,1.91073,0,1.52,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","log no of nozz/ft",49,-2.9546662829999959,-11.267387974013246,-24.54206604439668,-31.329231303846786,-26.353039831216883,-18.502852313345578,0.76909132641294797,-2.5895594713943564,null,"ACBR",50,"4D","ACBR_50_4D",0.55000000000000004,2.9,3.2,3.5,4.0999999999999996,4.2,1.6,0.25,null,"ACBC_1W","50-4",4,50,0.25,59,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_1W",7,null,null,null,null,null,107,null,115,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","heating",2,16,null,null,null,null,null,null,null,null,null,"ACBC_1W","2P1C",80,"cooling",0.05,7.3,2.2903737738860772,0.69750119547793821,1.0653582365223337,5.9636832522870713E-2,0.29617311576777983,1.6530677080861371,0,1.28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","Intercept",50,-169.90699175110839,-813.62359904705579,-836.02355223056293,612.00334198812584,3821.1043682921818,3306.6280172101333,760.86555940400558,-583.31504074175336,null,"ACBR",50,"4E","ACBR_50_4E",-2.5,-3.7,-5.6,-6.9,-7.7,-6.7,1.4,4,null,"ACBC_1W","50-5",5,50,0.25,75,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W",3,null,null,null,null,null,76,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","cooling",4,12,null,null,null,null,null,null,null,null,null,"ACBC_2W","2P2C",20,"cooling",0,7.3,6.097002570006798,0.64617580138468744,0.96180153927094336,4.5202387620426512E-2,3.7482812306102402,1.5393799567659041,0,2.54,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","r^2",51,0.75890787761551892,0.92535604687957629,0.97529410210527767,0.9801317911709696,0.97805172399515805,0.9769270583732228,0.95841628093874398,0.87708089703447378,null,"ACBR",50,"5eC","ACBR_50_5eC",-0.7,-0.7,-3.5,-4.0999999999999996,-3.1,-2.2000000000000002,-3.3,-1.5,null,"ACBC_1W","50-6",6,50,0.25,91,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W",4,null,null,null,null,null,110,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","heating",4,4,null,null,null,null,null,null,null,null,null,"ACBC_2W","2P2C",30,"cooling",0,7.3,4.7496921590000003,0.67868702299999994,1.004689355,4.2982425999999997E-2,0.91471000000000002,1.8573,0,2.34,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","log slot vel",52,3.5990354372969691,23.656751438834824,48.749416454395103,54.014482148874087,48.818165263357336,35.086359017834781,18.115997954528268,6.3318305195265259,null,"ACBR",50,"5eD","ACBR_50_5eD",0,0,0,0,0,0,0,0,null,"ACBC_1W","50-7",7,50,0.25,107,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W",5,null,null,null,null,null,144,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W","2P2C",40,"cooling",0,7.3,3.2256091152397421,0.7628658201342321,0.99346880637190782,5.9947113698384985E-2,0.89362446951179353,1.7638655105941077,0,2.06,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","log slot area",53,31.336728396510328,19.013760464544223,6.4972948793685523,2.9092600893234697,-30.596671781199753,-24.197154159637126,-3.9485548265806831,-4.360492423758858,null,"ACBR",50,"5eE","ACBR_50_5eE",-1.2,-0.8,-4.5999999999999996,-6.5,-4.3,-2.8,-3.5,-0.9,null,"ACBC_1W","70-3",3,70,0.3,43,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W",6,null,null,null,null,null,178,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W","2P2C",50,"cooling",0,7.3,3.0803558726862641,0.75993880949929782,1.0013235004419103,6.9579845535146345E-2,0.70140779250079677,1.7580044850242893,0,2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","log Ainlet/ Anozzle",54,-7.5592505478386727,-69.472881261998808,-110.24932693793434,-114.25214318191856,-92.788843948318387,-81.843420374653832,-78.300293454507681,-68.285547876810952,null,"ACBR",50,"6eC","ACBR_50_6eC",-0.5,0.2,2.6,2.9,0.5,-2.2000000000000002,2.1,5.6,null,"ACBC_1W","70-4",4,70,0.3,63,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W",7,null,null,null,null,null,212,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W","2P2C",60,"cooling",0,7.3,3.0734312629468401,0.75665684146709566,1.0518301977181677,2.5730968899201005E-2,0.45845939209473796,1.7497254197165204,0,1.76,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","log calculated TPVP",55,3.6995797053195427,31.779972055190179,50.030556071503561,50.256197544253354,37.563475948729391,35.914139609875711,37.051263016682277,31.5919430539013,null,"ACBR",50,"6eD","ACBR_50_6eD",0,0,0,0,0,0,0,0,null,"ACBC_1W","70-5",5,70,0.3,79,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PCBL",1,1,1,1,1,1,1,1,1,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W","2P2C",70,"cooling",0,7.3,2.272210469,0.77998774599999998,1.032413977,4.9319505999999999E-2,0.17398,1.91073,0,1.52,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","log Nozzle Vel",56,-518.09510812747806,-349.61060567037271,-117.07092049942257,-54.614577843132764,560.22642108686034,423.74050838842481,33.421302742581588,-52.435495234863303,null,"ACBR",50,"6eE","ACBR_50_6eE",-0.7,-0.5,1.5,1.4,-0.8,-3,2.4,5.4,null,"ACBC_1W","70-6",6,70,0.3,99,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",2,18,14,16,22,18,22,20,24,32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBC_2W","2P2C",80,"cooling",0.06,7.3,2.2903737738860772,0.69750119547793821,1.0653582365223337,5.9636832522870713E-2,0.29617311576777983,1.6530677080861371,0,1.28,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","log Nozzle size",57,259.15975280549077,177.18313238451032,58.872952359170462,32.926877565480879,-264.62817569905741,-191.9312584419539,2.7644733192783217,44.802013065004964,null,"ACBR",60,"3B","ACBR_60_3B",0,0,0,0,0,0,0,0,null,"ACBC_1W","70-7",7,70,0.3,115,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",3,30,22,28,38,30,38,34,42,56,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","2P1C",40,"cooling",0,8,4.3222639999999997,0.79511864899999996,1.018220831,5.9720500000000003E-2,2.161616,1.926425743,0,3.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","log no of nozz/ft",58,-0.81308441871485981,-3.33041482010657,-4.8631588590982036,-13.532088421456164,-15.522218010509567,-6.869208835652568,9.1786695673417409,11.784666965111368,null,"ACBR",60,"4B","ACBR_60_4B",0,0,0,0,0,0,0,0,null,"ACBL24_1W",{"$f":"CONCATENATE(JD69,\"-\",JC69)","v":"10-2"},2,10,0.188,18,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",4,44,32,38,54,42,54,48,60,80,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","2P2C",40,"cooling",0,8,4.3222639999999997,0.79511864899999996,1.018220831,5.9720500000000003E-2,2.161616,1.926425743,0,3.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","Intercept",59,1880.6751323275219,1220.8026986597281,330.65351011316523,110.92165505064121,-2053.0726224162777,-1552.0033198954827,-150.05292939709216,183.51268398795435,null,"ACBR",60,"4C","ACBR_60_4C",0.25,2.65,3.5,4.7,5.85,4.9000000000000004,1.75,-0.19999999999999996,null,"ACBL24_1W","20-2",2,20,0.25,14,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",5,56,42,50,66,56,70,64,78,104,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","4P1C",40,"cooling",0,8,4.3222639999999997,0.79511864899999996,1.018220831,5.9720500000000003E-2,2.161616,1.926425743,0,3.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","r^2",60,0.69326565544351271,0.92032592325269258,0.95363408382876147,0.94850254439916104,0.94758264275523041,0.93621971226056167,0.87632155228723663,0.8700907975415797,null,"ACBR",60,"4D","ACBR_60_4D",0.55000000000000004,2.9,3.2,3.5,4.0999999999999996,4.2,1.6,0.25,null,"ACBL24_1W","30-2",2,30,0.25,16,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",6,70,52,62,82,68,86,78,96,128,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","4P2C",40,"cooling",0.06,8,4.3222639999999997,0.79511864899999996,1.018220831,5.9720500000000003E-2,2.161616,1.926425743,0,3.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","log slot vel",61,-0.6358546387974171,18.326084721593627,37.132703841301812,44.606432271129023,49.814548094586264,42.322437565340607,24.422391252207174,16.419704820759975,null,"ACBR",60,"4E","ACBR_60_4E",-2.5,-3.7,-5.6,-6.9,-7.7,-6.7,1.4,4,null,"ACBL24_1W","35-2",2,35,0.25,22,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",7,82,62,72,98,80,102,92,114,152,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","2P1C",40,"heating",0,8,4.3222639999999997,0.79511864899999996,1.018220831,5.9720500000000003E-2,2.161616,1.926425743,0,3.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","log slot area",62,-0.46247623968465884,1.4734843395647481,3.918873622776609,7.4926429958441574,9.3357971723889968,9.4275272941672288,8.1496529709445102,5.2741648194780311,null,"ACBR",60,"5eC","ACBR_60_5eC",-0.7,-0.7,-3.5,-4.0999999999999996,-3.1,-2.2000000000000002,-3.3,-1.5,null,"ACBL24_1W","40-2",2,40,0.3,18,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",8,96,70,84,114,94,118,106,134,176,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","2P2C",40,"heating",0,8,4.3222639999999997,0.79511864899999996,1.018220831,5.9720500000000003E-2,2.161616,1.926425743,0,3.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","log Ainlet/ Anozzle",63,14.849053475554369,-75.856459498245371,-157.23121374659871,-156.11661974518432,-143.86429795343395,-158.10991908549471,-140.75010636927189,-89.441787172517536,null,"ACBR",60,"5eD","ACBR_60_5eD",0,0,0,0,0,0,0,0,null,"ACBL24_1W","50-2",2,50,0.3,22,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB",2,15,15,13,null,17,19,23,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","4P1C",40,"heating",0,8,4.3222639999999997,0.79511864899999996,1.018220831,5.9720500000000003E-2,2.161616,1.926425743,0,3.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","log calculated TPVP",64,-8.5241044647278557,36.106673656887118,78.063738246331781,77.467873248477574,71.663553113343468,79.734939395730791,72.199837030427133,47.035993816116772,null,"ACBR",60,"5eE","ACBR_60_5eE",-1.2,-0.8,-4.5999999999999996,-6.5,-4.3,-2.8,-3.5,-0.9,null,"ACBL24_1W","60-2",2,60,0.35,20,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB",2.67,21,21,18,null,22,26,31,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","4P2C",40,"heating",0.06,8,3.6954379999999998,0.77705599999999997,1.037695,7.2144E-2,2.161616,1.926425743,0,3.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","log Nozzle Vel",65,null,null,null,null,null,null,null,null,null,"ACBR",60,"6eC","ACBR_60_6eC",-0.5,0.2,2.6,2.9,0.5,-2.2000000000000002,2.1,5.6,null,"ACBL24_1W","70-2",2,70,0.35,24,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB",3.33,26,26,23,null,28,33,39,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","2P1C",50,"cooling",0,8,3.6252469999999999,0.79863327799999995,1.027807922,6.3346100000000002E-2,1.2951760000000001,1.9291176919999999,0,3.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","log Nozzle size",66,0.79283772526720409,3.0414050908306387,3.8894650618648545,4.7223176667017137,6.7220193452497439,12.089160664564574,16.167565050427974,12.404877276066092,null,"ACBR",60,"6eD","ACBR_60_6eD",0,0,0,0,0,0,0,0,null,"ACBL24_1W","80-2",2,80,0.35,32,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB",4.33,34,34,30,null,37,43,51,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","2P2C",50,"cooling",0,8,3.6252469999999999,0.79863327799999995,1.027807922,6.3346100000000002E-2,1.2951760000000001,1.9291176919999999,0,3.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","log no of nozz/ft",67,null,null,null,null,null,null,null,null,null,"ACBR",60,"6eE",{"$f":"CONCATENATE(IN78,\"_\",IO78,\"_\",IP78)","v":"ACBR_60_6eE"},-0.7,-0.5,1.5,1.4,-0.8,-3,2.4,5.4,null,"ACBL24_1W","10-3",3,10,0.188,30,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB",5.33,42,42,37,null,45,53,63,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","4P1C",50,"cooling",0,8,3.6252469999999999,0.79863327799999995,1.027807922,6.3346100000000002E-2,1.2951760000000001,1.9291176919999999,0,3.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","Intercept",68,59.206112713991949,5.0584176732852759,-34.034118257104367,-48.923476434727853,-62.206901356735784,-56.624299608660898,-27.809042811787442,-10.690552578049854,null,"ACBC_1W",50,"6E","ACBC_1W_50_6E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","20-3",3,20,0.25,22,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB",6.33,50,50,44,null,54,63,75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","4P2C",50,"cooling",0.1,8,3.6252469999999999,0.79863327799999995,1.027807922,6.3346100000000002E-2,1.2951760000000001,1.9291176919999999,0,3.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","r^2",69,0.21671849028002374,0.8180340672248454,0.93857739551546115,0.96074559415942473,0.98250020642224434,0.9427867825752958,0.9005156731820454,0.83057865730924707,null,"ACBC_1W",70,"6E","ACBC_1W_70_6E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","30-3",3,30,0.25,28,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB",7.3440000000000003,58,58,51,null,62,73,87,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","2P1C",50,"heating",0,8,3.6252469999999999,0.79863327799999995,1.027807922,6.3346100000000002E-2,1.2951760000000001,1.9291176919999999,0,3.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","log slot vel",70,0,24.535392752782101,48.693555436368477,55.609090483823195,56.338436473493061,47.072659349366482,27.017571730806822,0,null,"ACBC_1W",50,"8E","ACBC_1W_50_8E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","35-3",3,35,0.25,38,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB",2,15,15,13,null,17,19,23,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","2P2C",50,"heating",0,8,3.6252469999999999,0.79863327799999995,1.027807922,6.3346100000000002E-2,1.2951760000000001,1.9291176919999999,0,3.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","log slot area",71,0,0,0,0,0,0,0,0,null,"ACBC_1W",70,"8E","ACBC_1W_70_8E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","40-3",3,40,0.3,30,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB",2.67,21,21,18,null,22,26,31,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","4P1C",50,"heating",0,8,3.6252469999999999,0.79863327799999995,1.027807922,6.3346100000000002E-2,1.2951760000000001,1.9291176919999999,0,3.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","log Ainlet/ Anozzle",72,0,-198.58352197318027,-117.27258573851945,-36.259476409344266,-4.7243647728535905,-52.391782523221522,-135.99766283867663,0,null,"ACBC_2W",50,"6E","ACBC_2W_50_6E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","50-3",3,50,0.3,38,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB",3.33,26,26,23,null,28,33,39,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","4P2C",50,"heating",7.0000000000000007E-2,8,3.1822140000000001,0.75856800000000002,1.0419,8.2841999999999999E-2,1.2951760000000001,1.9291176919999999,0,3.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","log calculated TPVP",73,0,99.573829495205501,57.118429699754344,15.393338912945415,-0.55499625324025137,24.128271335247074,67.210503047419394,0,null,"ACBC_2W",50,"8E","ACBC_2W_50_8E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","60-3",3,60,0.35,34,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB",4.33,34,34,30,null,37,43,51,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","2P1C",60,"cooling",0,8,3.3069199999999999,0.75389939100000003,1.037337341,7.0709800000000003E-2,0.57175399999999998,2.0161067560000001,0,2.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","log Nozzle Vel",74,0,0,0,0,0,0,0,0,null,"ACBL24_1W",10,5,"ACBL24_1W_10_5",0,0,0,0,0,0,0,0,null,"ACBL24_1W","70-3",3,70,0.35,42,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB",5.33,42,42,37,null,45,53,63,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","2P2C",60,"cooling",0,8,3.3069199999999999,0.75389939100000003,1.037337341,7.0709800000000003E-2,0.57175399999999998,2.0161067560000001,0,2.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","log Nozzle size",75,0,1.3267787501004822,-7.0538862240441995,-7.7971724207193542,-1.3095773108955413,11.645413614149842,16.794506072328875,0,null,"ACBL24_1W",10,"6E","ACBL24_1W_10_6E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","80-3",3,80,0.35,56,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB",6.33,50,50,44,null,54,63,75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","4P1C",60,"cooling",0,8,3.3069199999999999,0.75389939100000003,1.037337341,7.0709800000000003E-2,0.57175399999999998,2.0161067560000001,0,2.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","log no of nozz/ft",76,0,4.0307540707134111,0.51608052353649181,-1.8297641658928703,-1.0102192775966323,8.1918887515006436,12.852008951332339,0,null,"ACBL24_1W",10,"8E","ACBL24_1W_10_8E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","10-4",4,10,0.188,44,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB",7.3440000000000003,58,58,51,null,62,73,87,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","4P2C",60,"cooling",0.08,8,3.3069199999999999,0.75389939100000003,1.037337341,7.0709800000000003E-2,0.57175399999999998,2.0161067560000001,0,2.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","Intercept",77,0,-43.351418998206874,-93.722488712745175,-100.65998539672388,-101.26520560810512,-95.540033213621626,-58.945055246696249,0,null,"ACBL24_1W",10,"5T","ACBL24_1W_10_5T",0,0,0,0,0,0,0,0,null,"ACBL24_1W","20-4",4,20,0.25,32,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB",2,15,15,13,null,17,19,23,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","2P1C",60,"heating",0,8,3.3069199999999999,0.75389939100000003,1.037337341,7.0709800000000003E-2,0.57175399999999998,2.0161067560000001,0,2.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","r^2",78,0,0.87259218527172244,0.97472368005637178,0.97907394983051865,0.97754024554210694,0.97937138175862326,0.93732275057875214,0,null,"ACBL24_1W",10,"6ET","ACBL24_1W_10_6ET",0,0,0,0,0,0,0,0,null,"ACBL24_1W","30-4",4,30,0.25,38,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB",2.67,21,21,18,null,22,26,31,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","2P2C",60,"heating",0,8,3.3069199999999999,0.75389939100000003,1.037337341,7.0709800000000003E-2,0.57175399999999998,2.0161067560000001,0,2.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","log slot vel",79,-4.5700459682098513,25.496360535387819,37.087921140039533,28.145181974622176,18.537918896468963,19.153990623865827,14.010909149662695,-5.9215302744275462,null,"ACBL24_1W",10,"8ET","ACBL24_1W_10_8ET",0,0,0,0,0,0,0,0,null,"ACBL24_1W","35-4",4,35,0.25,54,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB",3.33,26,26,23,null,28,33,39,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","4P1C",60,"heating",0,8,3.3069199999999999,0.75389939100000003,1.037337341,7.0709800000000003E-2,0.57175399999999998,2.0161067560000001,0,2.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","log slot area",80,43.447866214959433,20.931109856107231,-13.07710850585077,-36.766878533294594,-27.82460233237385,-7.3811728883787344,2.2661796013065709,-11.773628250112374,null,"ACBL24_1W",20,5,"ACBL24_1W_20_5",0,0,0,0,0,0,0,0,null,"ACBL24_1W","40-4",4,40,0.3,42,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB",4.33,34,34,30,null,37,43,51,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","4P2C",60,"heating",7.0000000000000007E-2,8,2.363696,0.76662200000000003,1.0165569999999999,0.116553,0.57175399999999998,2.0161067560000001,0,2.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","log Ainlet/ Anozzle",81,268.57946754059742,-21.76185593417912,24.245836991148362,43.273815504586416,-92.848946835846533,-298.40499890984375,-187.13304185862279,-36.144976959929089,null,"ACBL24_1W",20,"6E","ACBL24_1W_20_6E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","50-4",4,50,0.3,54,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB",5.33,42,42,37,null,45,53,63,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","2P1C",70,"cooling",0,8,3.2094749999999999,0.74920599600000004,0.95908603400000003,7.2235999999999995E-2,0.28942299999999999,1.9924449820000001,0,2.2000000000000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","log calculated TPVP",82,-142.77090217398586,9.1467482695643145,-17.537366954833583,-32.635454798380024,38.820211841944378,150.02033189364775,94.760955175571226,13.236275442918531,null,"ACBL24_1W",20,"8E","ACBL24_1W_20_8E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","60-4",4,60,0.35,48,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB",6.33,50,50,44,null,54,63,75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","2P2C",70,"cooling",0,8,3.2094749999999999,0.74920599600000004,0.95908603400000003,7.2235999999999995E-2,0.28942299999999999,1.9924449820000001,0,2.2000000000000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","log Nozzle Vel",83,-806.68269756462223,-262.33969678014643,380.31038326455433,751.91085792195383,597.01880781424711,271.7631497057925,34.145157819800303,119.20795491486345,null,"ACBL24_1W",20,"5T","ACBL24_1W_20_5T",0,0,0,0,0,0,0,0,null,"ACBL24_1W","70-4",4,70,0.35,60,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB",7.3440000000000003,58,58,51,null,62,73,87,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","4P1C",70,"cooling",0,8,3.2094749999999999,0.74920599600000004,0.95908603400000003,7.2235999999999995E-2,0.28942299999999999,1.9924449820000001,0,2.2000000000000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","log SP",84,413.66071371239531,135.01926121404529,-182.85047827416514,-358.10892094886009,-276.15045281912722,-110.77155530796493,11.139177901898867,-22.752036908610002,null,"ACBL24_1W",20,"6ET","ACBL24_1W_20_6ET",0,0,0,0,0,0,0,0,null,"ACBL24_1W","80-4",4,80,0.35,80,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP",2,15,15,13,null,17,19,23,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","4P2C",70,"cooling",7.0000000000000007E-2,8,3.2094749999999999,0.74920599600000004,0.95908603400000003,7.2235999999999995E-2,0.28942299999999999,1.9924449820000001,0,2.2000000000000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","log no of nozz/ft",85,13.904520403337761,-4.837068498072445,-4.8406456090189582,-8.8124041063243634,-2.3870465080584959,5.5464412113927013,8.5330345816283177,5.0579025158000297,null,"ACBL24_1W",20,"8ET","ACBL24_1W_20_8ET",0,0,0,0,0,0,0,0,null,"ACBL24_1W","10-5",5,10,0.188,56,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP",2.67,21,21,18,null,22,26,31,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","2P1C",70,"heating",0,8,3.2094749999999999,0.74920599600000004,0.95908603400000003,7.2235999999999995E-2,0.28942299999999999,1.9924449820000001,0,2.2000000000000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","Intercept",86,2934.5565438056919,912.50779934022989,-1391.3208416374182,-2676.8921585179978,-2122.8145399908485,-1003.1945384528917,-145.89312063830229,-379.94645297357994,null,"ACBL24_1W",30,5,"ACBL24_1W_30_5",0,0,0,0,0,0,0,0,null,"ACBL24_1W","20-5",5,20,0.25,42,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP",3.33,26,26,23,null,28,33,39,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","2P2C",70,"heating",0,8,3.2094749999999999,0.74920599600000004,0.95908603400000003,7.2235999999999995E-2,0.28942299999999999,1.9924449820000001,0,2.2000000000000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","r^2",87,0.87751667840487202,0.85366218986052078,0.94280167382634872,0.96652303973599696,0.96657555774763315,0.98854333796273619,0.98810150866891366,0.94494221750143981,null,"ACBL24_1W",30,"6E","ACBL24_1W_30_6E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","30-5",5,30,0.25,50,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP",4.33,34,34,30,null,37,43,51,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","4P1C",70,"heating",0,8,3.2094749999999999,0.74920599600000004,0.95908603400000003,7.2235999999999995E-2,0.28942299999999999,1.9924449820000001,0,2.2000000000000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","log slot vel",88,-4.5700459682098513,25.496360535387819,37.087921140039533,28.145181974622176,18.537918896468963,19.153990623865827,14.010909149662695,-5.9215302744275462,null,"ACBL24_1W",30,"8E","ACBL24_1W_30_8E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","35-5",5,35,0.25,66,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP",5.33,42,42,37,null,45,53,63,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","4P2C",70,"heating",0.06,8,2.8868100000000001,0.693716,1.0156959999999999,8.6057999999999996E-2,0.28942299999999999,1.9924449820000001,0,2.2000000000000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","log slot area",89,43.447866214959433,20.931109856107231,-13.07710850585077,-36.766878533294594,-27.82460233237385,-7.3811728883787344,2.2661796013065709,-11.773628250112374,null,"ACBL24_1W",30,"5T","ACBL24_1W_30_5T",0,0,0,0,0,0,0,0,null,"ACBL24_1W","40-5",5,40,0.3,56,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP",6.33,50,50,44,null,54,63,75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","2P1C",80,"cooling",0.05,8,2.2719900000000002,0.69573907099999999,1.0345319719999999,0.10219789999999999,0.112937,2.0791757550000001,0,1.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","log Ainlet/ Anozzle",90,268.57946754059742,-21.76185593417912,24.245836991148362,43.273815504586416,-92.848946835846533,-298.40499890984375,-187.13304185862279,-36.144976959929089,null,"ACBL24_1W",30,"6ET","ACBL24_1W_30_6ET",0,0,0,0,0,0,0,0,null,"ACBL24_1W",{"$f":"CONCATENATE(JD101,\"-\",JC101)","v":"50-5"},5,50,0.3,70,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP",7.3440000000000003,58,58,51,null,62,73,87,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","2P2C",80,"cooling",0.06,8,2.2719900000000002,0.69573907099999999,1.0345319719999999,0.10219789999999999,0.112937,2.0791757550000001,0,1.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","log calculated TPVP",91,-142.77090217398586,9.1467482695643145,-17.537366954833583,-32.635454798380024,38.820211841944378,150.02033189364775,94.760955175571226,13.236275442918531,null,"ACBL24_1W",30,"8ET","ACBL24_1W_30_8ET",0,0,0,0,0,0,0,0,null,"ACBL24_1W","60-5",5,60,0.35,64,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","4P1C",80,"cooling",0,8,2.2719900000000002,0.69573907099999999,1.0345319719999999,0.10219789999999999,0.112937,2.0791757550000001,0,1.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","log Nozzle Vel",92,-806.68269756462223,-262.33969678014643,380.31038326455433,751.91085792195383,597.01880781424711,271.7631497057925,34.145157819800303,119.20795491486345,null,"ACBL24_1W",40,5,"ACBL24_1W_40_5",0,0,0,0,0,0,0,0,null,"ACBL24_1W","70-5",5,70,0.35,78,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","4P2C",80,"cooling",0.04,8,2.2719900000000002,0.69573907099999999,1.0345319719999999,0.10219789999999999,0.112937,2.0791757550000001,0,1.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","log SP",93,413.66071371239531,135.01926121404529,-182.85047827416514,-358.10892094886009,-276.15045281912722,-110.77155530796493,11.139177901898867,-22.752036908610002,null,"ACBL24_1W",40,"6E","ACBL24_1W_40_6E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","80-5",5,80,0.35,104,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","2P1C",80,"heating",0.05,8,2.2719900000000002,0.69573907099999999,1.0345319719999999,0.10219789999999999,0.112937,2.0791757550000001,0,1.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","log no of nozz/ft",94,13.904520403337761,-4.837068498072445,-4.8406456090189582,-8.8124041063243634,-2.3870465080584959,5.5464412113927013,8.5330345816283177,5.0579025158000297,null,"ACBL24_1W",40,"8E","ACBL24_1W_40_8E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","10-6",6,10,0.188,70,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","2P2C",80,"heating",0.06,8,2.2719900000000002,0.69573907099999999,1.0345319719999999,0.10219789999999999,0.112937,2.0791757550000001,0,1.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","Intercept",95,2934.5565438056919,912.50779934022989,-1391.3208416374182,-2676.8921585179978,-2122.8145399908485,-1003.1945384528917,-145.89312063830229,-379.94645297357994,null,"ACBL24_1W",40,"5T","ACBL24_1W_40_5T",0,0,0,0,0,0,0,0,null,"ACBL24_1W","20-6",6,20,0.25,52,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","4P1C",80,"heating",0,8,2.2719900000000002,0.69573907099999999,1.0345319719999999,0.10219789999999999,0.112937,2.0791757550000001,0,1.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","r^2",96,0.87751667840487202,0.85366218986052078,0.94280167382634872,0.96652303973599696,0.96657555774763315,0.98854333796273619,0.98810150866891366,0.94494221750143981,null,"ACBL24_1W",40,"6ET","ACBL24_1W_40_6ET",0,0,0,0,0,0,0,0,null,"ACBL24_1W","30-6",6,30,0.25,62,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W","4P2C",80,"heating",0.05,8,2.1650809999999998,0.67016200000000004,0.99895400000000001,0.12565899999999999,0.112937,2.0791757550000001,0,1.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","log slot vel",97,-4.5700459682098513,25.496360535387819,37.087921140039533,28.145181974622176,18.537918896468963,19.153990623865827,14.010909149662695,-5.9215302744275462,null,"ACBL24_1W",40,"8ET","ACBL24_1W_40_8ET",0,0,0,0,0,0,0,0,null,"ACBL24_1W","35-6",6,35,0.25,82,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","2P1C",20,"cooling",0,8,3.4884437620000002,0.856208423,1.0432428,8.7156999999999998E-2,3.233746,1.8893589669999999,0,3.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","log slot area",98,43.447866214959433,20.931109856107231,-13.07710850585077,-36.766878533294594,-27.82460233237385,-7.3811728883787344,2.2661796013065709,-11.773628250112374,null,"ACBL24_1W",50,5,"ACBL24_1W_50_5",0,0,0,0,0,0,0,0,null,"ACBL24_1W","40-6",6,40,0.3,68,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","2P2C",20,"cooling",0,8,3.4884437620000002,0.856208423,1.0432428,8.7156999999999998E-2,3.233746,1.8893589669999999,0,3.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","log Ainlet/ Anozzle",99,268.57946754059742,-21.76185593417912,24.245836991148362,43.273815504586416,-92.848946835846533,-298.40499890984375,-187.13304185862279,-36.144976959929089,null,"ACBL24_1W",50,"6E","ACBL24_1W_50_6E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","50-6",6,50,0.3,86,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","4P1C",20,"cooling",0,8,3.4884437620000002,0.856208423,1.0432428,8.7156999999999998E-2,3.233746,1.8893589669999999,0,3.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","log calculated TPVP",100,-142.77090217398586,9.1467482695643145,-17.537366954833583,-32.635454798380024,38.820211841944378,150.02033189364775,94.760955175571226,13.236275442918531,null,"ACBL24_1W",50,"8E","ACBL24_1W_50_8E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","60-6",6,60,0.35,78,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","4P2C",20,"cooling",0.03,8,3.4884437620000002,0.856208423,1.0432428,8.7156999999999998E-2,3.233746,1.8893589669999999,0,3.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","log Nozzle Vel",101,-806.68269756462223,-262.33969678014643,380.31038326455433,751.91085792195383,597.01880781424711,271.7631497057925,34.145157819800303,119.20795491486345,null,"ACBL24_1W",50,"5T","ACBL24_1W_50_5T",0,0,0,0,0,0,0,0,null,"ACBL24_1W","70-6",6,70,0.35,96,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","2P1C",20,"heating",0.05,8,3.4884437620000002,0.856208423,1.0432428,8.7156999999999998E-2,3.233746,1.8893589669999999,0,3.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","log SP",102,413.66071371239531,135.01926121404529,-182.85047827416514,-358.10892094886009,-276.15045281912722,-110.77155530796493,11.139177901898867,-22.752036908610002,null,"ACBL24_1W",50,"6ET","ACBL24_1W_50_6ET",0,0,0,0,0,0,0,0,null,"ACBL24_1W","80-6",6,80,0.35,128,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","2P2C",20,"heating",0,8,3.4884437620000002,0.856208423,1.0432428,8.7156999999999998E-2,3.233746,1.8893589669999999,0,3.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","log no of nozz/ft",103,13.904520403337761,-4.837068498072445,-4.8406456090189582,-8.8124041063243634,-2.3870465080584959,5.5464412113927013,8.5330345816283177,5.0579025158000297,null,"ACBL24_1W",50,"8ET","ACBL24_1W_50_8ET",0,0,0,0,0,0,0,0,null,"ACBL24_1W","10-7",7,10,0.188,82,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","4P1C",20,"heating",0,8,3.4884437620000002,0.856208423,1.0432428,8.7156999999999998E-2,3.233746,1.8893589669999999,0,3.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","Intercept",104,2934.5565438056919,912.50779934022989,-1391.3208416374182,-2676.8921585179978,-2122.8145399908485,-1003.1945384528917,-145.89312063830229,-379.94645297357994,null,"ACBL24_1W",60,5,"ACBL24_1W_60_5",0,0,0,0,0,0,0,0,null,"ACBL24_1W","20-7",7,20,0.25,62,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","4P2C",20,"heating",0,8,3.0539550000000002,0.81813800000000003,1.0383230000000001,0.112271,3.233746,1.8893589669999999,0,3.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","r^2",105,0.87751667840487202,0.85366218986052078,0.94280167382634872,0.96652303973599696,0.96657555774763315,0.98854333796273619,0.98810150866891366,0.94494221750143981,null,"ACBL24_1W",60,"6E","ACBL24_1W_60_6E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","30-7",7,30,0.25,72,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","2P1C",30,"cooling",0,8,4.0949064929999999,0.69239486699999997,0.9966235,0.101658,1.489852,1.850369363,0,2.9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","log slot vel",106,-4.5700459682098513,25.496360535387819,37.087921140039533,28.145181974622176,18.537918896468963,19.153990623865827,14.010909149662695,-5.9215302744275462,null,"ACBL24_1W",60,"8E","ACBL24_1W_60_8E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","35-7",7,35,0.25,98,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","2P2C",30,"cooling",0,8,4.0949064929999999,0.69239486699999997,0.9966235,0.101658,1.489852,1.850369363,0,2.9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","log slot area",107,43.447866214959433,20.931109856107231,-13.07710850585077,-36.766878533294594,-27.82460233237385,-7.3811728883787344,2.2661796013065709,-11.773628250112374,null,"ACBL24_1W",60,"5T","ACBL24_1W_60_5T",0,0,0,0,0,0,0,0,null,"ACBL24_1W","40-7",7,40,0.3,80,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","4P1C",30,"cooling",0,8,4.0949064929999999,0.69239486699999997,0.9966235,0.101658,1.489852,1.850369363,0,2.9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","log Ainlet/ Anozzle",108,268.57946754059742,-21.76185593417912,24.245836991148362,43.273815504586416,-92.848946835846533,-298.40499890984375,-187.13304185862279,-36.144976959929089,null,"ACBL24_1W",60,"6ET","ACBL24_1W_60_6ET",0,0,0,0,0,0,0,0,null,"ACBL24_1W","50-7",7,50,0.3,102,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","4P2C",30,"cooling",0.06,8,4.0949064929999999,0.69239486699999997,0.9966235,0.101658,1.489852,1.850369363,0,2.9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","log calculated TPVP",109,-142.77090217398586,9.1467482695643145,-17.537366954833583,-32.635454798380024,38.820211841944378,150.02033189364775,94.760955175571226,13.236275442918531,null,"ACBL24_1W",60,"8ET","ACBL24_1W_60_8ET",0,0,0,0,0,0,0,0,null,"ACBL24_1W","60-7",7,60,0.35,92,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","2P1C",30,"heating",0,8,4.0949064929999999,0.69239486699999997,0.9966235,0.101658,1.489852,1.850369363,0,2.9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","log Nozzle Vel",110,-806.68269756462223,-262.33969678014643,380.31038326455433,751.91085792195383,597.01880781424711,271.7631497057925,34.145157819800303,119.20795491486345,null,"ACBL24_1W",70,5,"ACBL24_1W_70_5",0,0,0,0,0,0,0,0,null,"ACBL24_1W","70-7",7,70,0.35,114,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","2P2C",30,"heating",0,8,4.0949064929999999,0.69239486699999997,0.9966235,0.101658,1.489852,1.850369363,0,2.9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","log SP",111,413.66071371239531,135.01926121404529,-182.85047827416514,-358.10892094886009,-276.15045281912722,-110.77155530796493,11.139177901898867,-22.752036908610002,null,"ACBL24_1W",70,"6E","ACBL24_1W_70_6E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","80-7",7,80,0.35,152,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","4P1C",30,"heating",0,8,4.0949064929999999,0.69239486699999997,0.9966235,0.101658,1.489852,1.850369363,0,2.9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","log no of nozz/ft",112,13.904520403337761,-4.837068498072445,-4.8406456090189582,-8.8124041063243634,-2.3870465080584959,5.5464412113927013,8.5330345816283177,5.0579025158000297,null,"ACBL24_1W",70,"8E","ACBL24_1W_70_8E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","10-8",8,10,0.188,96,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","4P2C",30,"heating",0.05,8,3.8124630000000002,0.64947900000000003,0.99526000000000003,0.12063699999999999,1.489852,1.850369363,0,2.9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","Intercept",113,2934.5565438056919,912.50779934022989,-1391.3208416374182,-2676.8921585179978,-2122.8145399908485,-1003.1945384528917,-145.89312063830229,-379.94645297357994,null,"ACBL24_1W",70,"5T","ACBL24_1W_70_5T",0,0,0,0,0,0,0,0,null,"ACBL24_1W","20-8",8,20,0.25,70,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","2P1C",40,"cooling",0,8,3.5327782779999999,0.69801435000000001,1.0180096999999999,9.7125000000000003E-2,0.65582499999999999,1.9070284319999999,0,2.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","r^2",114,0.87751667840487202,0.85366218986052078,0.94280167382634872,0.96652303973599696,0.96657555774763315,0.98854333796273619,0.98810150866891366,0.94494221750143981,null,"ACBL24_1W",70,"6ET","ACBL24_1W_70_6ET",0,0,0,0,0,0,0,0,null,"ACBL24_1W","30-8",8,30,0.25,84,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","2P2C",40,"cooling",0,8,3.5327782779999999,0.69801435000000001,1.0180096999999999,9.7125000000000003E-2,0.65582499999999999,1.9070284319999999,0,2.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W",70,"8ET","ACBL24_1W_70_8ET",0,0,0,0,0,0,0,0,null,"ACBL24_1W","35-8",8,35,0.25,114,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","4P1C",40,"heating",0,8,3.5327782779999999,0.69801435000000001,1.0180096999999999,9.7125000000000003E-2,0.65582499999999999,1.9070284319999999,0,2.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W",80,"6ET","ACBL24_1W_80_6ET",0,0,0,0,0,0,0,0,null,"ACBL24_1W","80-8",8,80,0.35,176,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","4P2C",50,"cooling",0.1,8,3.300552384,0.68446441099999999,0.99999610000000005,9.5064999999999997E-2,0.54455299999999995,1.83322505,0,2.2000000000000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",10,"5T","ACBL24_2W_10_5T",0,0,0,0,0,0,0,0,null,"ACBL24_1W","40-9",9,40,0.3,106,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","4P1C",50,"heating",0,8,3.300552384,0.68446441099999999,0.99999610000000005,9.5064999999999997E-2,0.54455299999999995,1.83322505,0,2.2000000000000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",20,5,"ACBL24_2W_20_5",0,0,0,0,0,0,0,0,null,"ACBL24_1W","70-9",9,70,0.35,152,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","2P1C",60,"cooling",0,8,3.4198933610000002,0.63771499499999995,0.99238020000000005,0.107901,0.23932300000000001,1.8862544969999999,0,2.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",20,"8E","ACBL24_2W_20_8E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","10-10",10,10,0.188,122,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","2P2C",60,"heating",0,8,3.4198933610000002,0.63771499499999995,0.99238020000000005,0.107901,0.23932300000000001,1.8862544969999999,0,2.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",30,"6E","ACBL24_2W_30_6E",0,0,0,0,0,0,0,0,null,"ACBL24_1W","50-10",10,50,0.3,150,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","4P1C",70,"cooling",0,8,3.5413219460000001,0.58455728699999998,0.98024509999999998,0.11493,9.7983000000000001E-2,1.947122845,0,1.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",35,5,"ACBL24_2W_35_5",0,0,0,0,0,0,0,0,null,"ACBL24_2W","20-2",2,20,0.25,14,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","4P2C",70,"cooling",7.0000000000000007E-2,8,3.5413219460000001,0.58455728699999998,0.98024509999999998,0.11493,9.7983000000000001E-2,1.947122845,0,1.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",35,"6E","ACBL24_2W_35_6E",0,0,0,0,0,0,0,0,null,"ACBL24_2W","30-2",2,30,0.25,16,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","4P2C",70,"heating",0.06,8,2.7829030000000001,0.55779699999999999,0.96786899999999998,0.16008500000000001,9.7983000000000001E-2,1.947122845,0,1.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",35,"8ET","ACBL24_2W_35_8ET",0,0,0,0,0,0,0,0,null,"ACBL24_2W","60-2",2,60,0.35,20,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","2P1C",80,"heating",0.05,8,2.4811665550000002,0.65962189999999998,0.98432339999999996,9.3441999999999997E-2,2.9430999999999999E-2,2.0802738060000001,0,1.1499999999999999,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",40,"6ET","ACBL24_2W_40_6ET",0,0,0,0,0,0,0,0,null,"ACBL24_2W","30-3",3,30,0.25,28,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W","4P2C",80,"heating",0.05,8,2.6904379999999999,0.52350200000000002,1.020014,0.14341699999999999,2.9430999999999999E-2,2.0802738060000001,0,1.1499999999999999,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",50,"6E","ACBL24_2W_50_6E",0,0,0,0,0,0,0,0,null,"ACBL24_2W","50-3",3,50,0.3,38,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","2P2C",10,"cooling",0,6,7.3478000000000003,0.93259999999999998,1.0519000000000001,3.1199999999999999E-2,8.3463100000000008,1.9170199999999999,0,5.3673960000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",50,"5T","ACBL24_2W_50_5T",0,0,0,0,0,0,0,0,null,"ACBL24_2W","70-3",3,70,0.35,42,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","4P1C",10,"heating",0,6,6.5293999999999999,0.69120000000000004,1.004,0.1048,8.3463100000000008,1.9170199999999999,0,5.3673960000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",60,"8E","ACBL24_2W_60_8E",0,0,0,0,0,0,0,0,null,"ACBL24_2W","35-4",4,35,0.25,54,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","4P2C",20,"cooling",0,6,6.4545500000000002,0.87387000000000004,1.0313600000000001,5.0099999999999999E-2,3.9763299999999999,1.9928999999999999,0,5.1630024772248584,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",70,"6E","ACBL24_2W_70_6E",0,0,0,0,0,0,0,0,null,"ACBL24_2W","80-4",4,80,0.35,80,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","2P2C",20,"heating",0,6,6.64663,0.90827000000000002,1.03474,3.8460000000000001E-2,3.9763299999999999,1.9928999999999999,0,5.1630024772248584,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",70,"5T","ACBL24_2W_70_5T",0,0,0,0,0,0,0,0,null,"ACBL24_2W","20-5",5,20,0.25,42,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","2P1C",30,"cooling",0,6,6.5200500000000003,0.88270999999999999,1.0079199999999999,4.904E-2,2.8882699999999999,1.9890600000000001,0,4.888776,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",80,5,"ACBL24_2W_80_5",0,0,0,0,0,0,0,0,null,"ACBL24_2W","40-5",5,40,0.3,56,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","2P2C",30,"heating",0,6,6.3474700000000004,0.88183,1.0335099999999999,4.2029999999999998E-2,2.8882699999999999,1.9890600000000001,0,4.888776,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W",80,"8ET","ACBL24_2W_80_8ET",0,0,0,0,0,0,0,0,null,"ACBL24_2W","10-6",6,10,0.188,70,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","2P2C",35,"cooling",0,6,5.6821999999999999,0.85563999999999996,1.0317400000000001,4.7289999999999999E-2,1.6325799999999999,1.98749,0,4.7253710000000009,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W",10,"5T","ACBL12_1W_10_5T",0,0,0,0,0,0,0,0,null,"ACBL24_2W","40-6",6,40,0.3,68,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","4P1C",35,"heating",0,6,5.6708744691297239,0.64647759839183139,0.99595029107017086,0.1027194988080649,1.6325799999999999,1.98749,0,4.7253710000000009,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W",20,"8E","ACBL12_1W_20_8E",0,0,0,0,0,0,0,0,null,"ACBL24_2W","10-7",7,10,0.188,82,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","4P2C",35,"heating",0,6,6.2889600000000003,0.61004999999999998,0.97438000000000002,9.4210000000000002E-2,1.6325799999999999,1.98749,0,4.7253710000000009,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W",20,"5T","ACBL12_1W_20_5T",0,0,0,0,0,0,0,0,null,"ACBL24_2W","20-7",7,20,0.25,62,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","2P1C",40,"heating",0,4,5.3334999999999999,0.871,0.99990000000000001,5.2400000000000002E-2,1.0085299999999999,2.0486599999999999,0,4.5441413732582561,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W",30,"8E","ACBL12_1W_30_8E",0,0,0,0,0,0,0,0,null,"ACBL24_2W","60-7",7,60,0.35,92,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","4P2C",40,"heating",0,6,5.5933999999999999,0.60619999999999996,0.98670000000000002,0.1037,1.0085299999999999,2.0486599999999999,0,4.5441413732582561,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W",30,"8ET","ACBL12_1W_30_8ET",0,0,0,0,0,0,0,0,null,"ACBL24_2W","10-8",8,10,0.188,96,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","2P2C",50,"heating",0,6,4.7087500000000002,0.83848,1.02982,5.2920000000000002E-2,0.64419000000000004,2.0407000000000002,0,4.1301560000000004,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W",40,"8ET","ACBL12_1W_40_8ET",0,0,0,0,0,0,0,0,null,"ACBL24_2W","60-8",8,60,0.35,106,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","4P1C",50,"heating",0,6,4.9977,0.59850000000000003,0.98899999999999999,0.122,0.64419000000000004,2.0407000000000002,0,4.1301560000000004,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W",50,5,"ACBL12_1W_50_5",0,0,0,0,0,0,0,0,null,"ACBL24_2W","70-8",8,70,0.35,134,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","4P2C",60,"cooling",0,6,4.0859100000000002,0.79610999999999998,1.05531,6.343E-2,0.42393999999999998,2.0230800000000002,0,3.6458460000000006,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W",50,"8ET","ACBL12_1W_50_8ET",0,0,0,0,0,0,0,0,null,"ACBL24_2W","35-9",9,35,0.25,130,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","4P2C",60,"heating",0,6,5.1522800000000002,0.58301999999999998,0.98477000000000003,9.7799999999999998E-2,0.42393999999999998,2.0230800000000002,0,3.6458460000000006,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W",60,"5T","ACBL12_1W_60_5T",0,0,0,0,0,0,0,0,null,"ACBL24_2W","70-9",9,70,0.35,152,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","2P1C",70,"heating",0,6,3.6957800000000001,0.83504,1.0120400000000001,6.5989999999999993E-2,0.34792000000000001,1.9648600000000001,0,3.0905550916819045,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W",70,"8E","ACBL12_1W_70_8E",0,0,0,0,0,0,0,0,null,"ACBL24_2W","35-10",10,35,0.25,146,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","2P2C",70,"heating",0,6,4.2128800000000002,0.79384999999999994,1.0282800000000001,5.7549999999999997E-2,0.34792000000000001,1.9648600000000001,0,3.0905550916819045,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W",70,"5T","ACBL12_1W_70_5T",0,0,0,0,0,0,0,0,null,"ACBL24_2W","40-10",10,40,0.3,118,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","4P2C",80,"cooling",0,6,3.3536000000000001,0.76,1.0704,7.0499999999999993E-2,0.21,1.94878,0,2.4672260000000006,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_1W",80,"5T","ACBL12_1W_80_5T",0,0,0,0,0,0,0,0,null,"ACBM","30-2",2,30,0.16,64,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_1W","4P1C",80,"heating",0,6,3.66,0.6149,1.0115000000000001,0.10580000000000001,0.21,1.94878,0,2.4672260000000006,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W",20,5,"ACBL12_2W_20_5",0,0,0,0,0,0,0,0,null,"ACBM","60-2",2,60,0.3,64,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","4P2C",10,"cooling",0,6,4.1230000000000002,0.96599999999999997,1.0362,6.9599999999999995E-2,2.2897579532236279,1.902581502342191,0,5.8351170000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W",20,"8ET","ACBL12_2W_20_8ET",0,0,0,0,0,0,0,0,null,"ACBM","50-4",4,50,0.25,112,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","2P1C",10,"heating",0,6,5.2895354954228342,0.93015769552691496,1.015589457439515,6.2175996861110347E-2,2.2897579532236279,1.902581502342191,0,5.8351170000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W",30,5,"ACBL12_2W_30_5",0,0,0,0,0,0,0,0,null,"ACBM","60-4",4,60,0.3,112,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","2P2C",20,"cooling",0,6,4.9390200000000002,0.93132999999999999,1.0302199999999999,4.224E-2,1.2149057861379946,1.953035075340368,0,5.0486425530167613,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W",30,"8ET","ACBL12_2W_30_8ET",0,0,0,0,0,0,0,0,null,"LIU24_2W","35-2",2,35,0.25,22,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","2P2C",20,"heating",0,6,4.9390200000000002,0.93132999999999999,1.0302199999999999,4.224E-2,1.2149057861379946,1.953035075340368,0,5.0486425530167613,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W",40,"5T","ACBL12_2W_40_5T",0,0,0,0,0,0,0,0,null,"LIU24_2W","70-2",2,70,0.35,24,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","4P1C",30,"cooling",0,6,4.0126118705126315,0.85474076995478609,1.035090985050215,9.2968595197129522E-2,0.87139191555771811,1.9315233318194709,0,4.368017,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W",50,"8E","ACBL12_2W_50_8E",0,0,0,0,0,0,0,0,null,"LIU24_2W","35-3",3,35,0.25,38,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","2P2C",30,"heating",0,6,4.6768799999999997,0.8992,1.0313600000000001,4.7419999999999997E-2,0.87139191555771811,1.9315233318194709,0,4.368017,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W",50,"8ET","ACBL12_2W_50_8ET",0,0,0,0,0,0,0,0,null,"LIU24_2W","60-3",3,60,0.35,34,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","4P2C",30,"heating",0,6,5.2587999999999999,0.61795999999999995,0.97890999999999995,0.11117,0.87139191555771811,1.9315233318194709,0,4.368017,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W",60,"6E","ACBL12_2W_60_6E",0,0,0,0,0,0,0,0,null,"LIU24_2W","80-3",3,80,0.35,56,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","2P1C",35,"heating",0,6,5.1204655139294113,0.773844420719487,1.0180560120687074,8.1012098571163801E-2,0.7531925598239404,1.8292035627683361,0,4.067367,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W",70,5,"ACBL12_2W_70_5",0,0,0,0,0,0,0,0,null,"LIU24_2W","40-4",4,40,0.3,42,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","2P2C",40,"cooling",0,6,4.6936999999999998,0.81179999999999997,1.0129999999999999,5.74E-2,0.47815348738143149,1.8495971103882154,0,3.7930638214042567,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W",70,"8ET",{"$f":"CONCATENATE(IN270,\"_\",IO270,\"_\",IP270)","v":"ACBL12_2W_70_8ET"},0,0,0,0,0,0,0,0,null,"LIU24_2W","10-5",5,10,0.188,56,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","4P1C",40,"cooling",0,6,4.9000473767808908,0.70328700287172163,1.0197301287031342,0.10843629019005371,0.47815348738143149,1.8495971103882154,0,3.7930638214042567,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W",80,5,"ACBL12_2W_80_5",0,0,0,0,0,0,0,0,null,"LIU24_2W","20-5",5,20,0.25,42,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","4P1C",40,"heating",0,6,5.5759352760158736,0.5109140414590837,1.0137152325510541,0.12911479361523923,0.47815348738143149,1.8495971103882154,0,3.7930638214042567,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL12_2W",80,"6ET","ACBL12_2W_80_6ET",0,0,0,0,0,0,0,0,null,"LIU24_2W","50-5",5,50,0.3,70,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","4P2C",50,"cooling",0,6,4.0967399999999996,0.74626999999999999,1.0427999999999999,7.5770000000000004E-2,0.32892130750673021,1.8360692602535555,0,3.3241170000000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM",30,"5T","ACBM_30_5T",null,null,null,null,null,null,null,null,null,"LIU24_2W","20-6",6,20,0.25,52,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","4P2C",50,"heating",0,6,4.8685600000000004,0.53081,0.97789000000000004,0.13081999999999999,0.32892130750673021,1.8360692602535555,0,3.3241170000000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM",40,"6T","ACBM_40_6T",null,null,null,null,null,null,null,null,null,"LIU24_2W","50-6",6,50,0.3,86,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","2P1C",60,"cooling",0,6,4.1153071480202037,0.72868693180977873,1.0202612095812595,9.0814357187386688E-2,0.16443739560310769,1.9123161515678218,0,2.9608669999999995,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM",40,"8T","ACBM_40_8T",null,null,null,null,null,null,null,null,null,"LIU24_2W","60-6",6,60,0.35,78,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","2P2C",60,"heating",0,6,3.6115300000000001,0.79932000000000003,1.0348999999999999,6.3549999999999995E-2,0.16443739560310769,1.9123161515678218,0,2.9608669999999995,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM",60,"6T","ACBM_60_6T",null,null,null,null,null,null,null,null,null,"LIU24_2W","30-7",7,30,0.25,72,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","4P1C",70,"cooling",0,6,3.8364187564726588,0.68163108574876341,1.0302701440242945,0.11096164693151411,0.11632799613580581,1.9069294072602954,0,2.7030936388126676,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",10,5,"LIU24_2W_10_5",0,0,0,0,0,0,0,0,null,"LIU24_2W","70-7",7,70,0.35,114,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","2P1C",70,"heating",0,6,3.9350913386865636,0.71323941358870091,1.0207538475999776,9.3004093254599726E-2,0.11632799613580581,1.9069294072602954,0,2.7030936388126676,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",10,8,"LIU24_2W_10_8",0,0,0,0,0,0,0,0,null,"LIU24_2W","10-8",8,10,0.188,96,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","4P2C",70,"heating",0,6,4.39405,0.50736999999999999,0.97738999999999998,0.14052000000000001,0.11632799613580581,1.9069294072602954,0,2.7030936388126676,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",10,"8T","LIU24_2W_10_8T",0,-0.9,-2.1,-1.7,-1.4,-1.2,-1.3,0,null,"LIU24_2W","35-8",8,35,0.25,114,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBL24_2W","2P1C",80,"heating",0,6,3.4963708062486569,0.70690857072487667,1.0220699606238486,9.4468496911810487E-2,7.3929485675477732E-2,1.8927583654320854,0,2.551766999999999,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",20,"6T","LIU24_2W_20_6T",0,-0.2,-3.4,-2.6,-1.2,0.1,-0.5,0,null,"LIU24_2W","80-8",8,80,0.35,176,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","2P2C",20,"cooling",0,4,4.2448236646952244,0.89506068282256102,1.0170877780339935,6.8271915447100706E-2,2.2722269164965256,1.8203064889529088,0,4.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",30,"5T","LIU24_2W_30_5T",0,0,-3,-2.5,-1,0,0,0,null,"LIU24_2W","40-9",9,40,0.3,106,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","2P2C",20,"heating",0.05,4,4.2448236646952244,0.89506068282256102,1.0170877780339935,6.8271915447100706E-2,2.2722269164965256,1.8203064889529088,0,4.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",35,6,"LIU24_2W_35_6",0,0,0,0,0,0,0,0,null,"LIU24_2W","80-9",9,80,0.35,200,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","4P2C",20,"heating",0,2,2.8099432456917843,0.85913545611724262,1.0619902213489603,0.1121129576986666,2.0669563511035864,1.7322085335052795,0,3.7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",35,8,"LIU24_2W_35_8",0,0,0,0,0,0,0,0,null,"LIU24_2W","10-10",10,10,0.188,122,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","4P2C",30,"cooling",0,4,3.8565990755149238,0.83203649806552593,1.019396950526732,7.020409844043396E-2,0.920847873097971,1.8321672216250515,0,3.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",40,6,"LIU24_2W_40_6",0,0,0,0,0,0,0,0,null,"LIU24_2W","50-10",10,50,0.3,150,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","4P2C",30,"heating",0,2,3.7275280197678611,0.82197433727582148,1.0148138172898278,6.7202878564951773E-2,0.82051620684319604,1.7812237704431988,0,3.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",40,"6T","LIU24_2W_40_6T",0,-0.2,-3.4,-2.6,-1.2,0.1,-0.5,0,null,"LIU24_2W","80-10",10,80,0.35,224,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","2P2C",40,"heating",0,2,3.8188037933182262,0.72537009668722185,1.0104897251932445,8.8208521021810191E-2,6.0511000770223082E-2,2.3029999009194686,0,2.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",50,"6T","LIU24_2W_50_6T",0,-0.2,-3.4,-2.6,-1.2,0.1,-0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","2P2C",40,"heating",0,4,4.2218662414129149,0.7395721475014333,1.0018322204037711,8.2112454106472277E-2,0.38434799577173573,1.8696038733016778,0,2.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",50,"8T","LIU24_2W_50_8T",0,-0.9,-2.1,-1.7,-1.4,-1.2,-1.3,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","4P2C",50,"cooling",0,2,3.5580537683322642,0.68603693721599235,1.0070672977805624,9.219650235422272E-2,0.14575258023241405,1.8278018862104786,0,1.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",60,"6T","LIU24_2W_60_6T",0,-0.2,-3.4,-2.6,-1.2,0.1,-0.5,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","4P2C",50,"heating",0,2,3.5580537683322642,0.68603693721599235,1.0070672977805624,9.219650235422272E-2,0.14575258023241405,1.8278018862104786,0,1.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",70,8,"LIU24_2W_70_8",0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","4P2C",60,"cooling",0,4,2.2160883961940048,0.78994415257540851,1.014730409938212,6.9606858519212264E-2,6.5961640958322493E-2,1.8677125277227133,0,1.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",80,6,"LIU24_2W_80_6",0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","2P2C",60,"heating",0,2,2.5195579125241858,0.72161283115551544,1.0127583063070835,9.4282343593629123E-2,5.1304641372310403E-2,1.9018861623191501,0,1.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",80,8,"LIU24_2W_80_8",0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","4P2C",70,"cooling",0,2,2.7271967572909332,0.73362345049799482,0.95336474531006621,6.6331584576885511E-2,1.0077834838650605E-2,2.1010285136192604,0,1.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",30,"10T","LIU24_2W_30_10T",0,-1.7,-2.6,-2.2000000000000002,-2.5,-2.5,-1.8,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBM","2P2C",70,"heating",0,4,2.2955779941098466,0.78392960202530115,0.97367658343091401,6.4491073945682098E-2,2.072535768266549E-2,2.0246391819486171,0,1.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W",50,"10T","LIU24_2W_50_10T",0,-1.7,-2.6,-2.2000000000000002,-2.5,-2.5,-1.8,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","4P1C",10,"heating",0,6,5.3180773703623414,0.68781952295744819,1.0067238498142861,0.10853819992019048,2.2897579532236279,1.902581502342191,0,4.9013726352478804,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB",10,3.33,"RIU_FB_10_3.33",-0.12450000000000028,-2.7873000000000001,-1.0820000000000001,-2.0967999999999996,-3.5878000000000005,-0.49099999999999999,-0.49099999999999999,-2.3027999999999995]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","4P2C",10,"heating",0,6,4.547678951883908,0.76741077989460138,1.009852958289801,8.3067682714707283E-2,1.8490235856448791,1.9565320553152776,0,4.9013726352478804,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB",10,5.33,"RIU_FB_10_5.33",-1.4245000000000001,-0.40730000000000022,0.11799999999999988,-1.6799999999999038E-2,-0.90779999999999994,0.10899999999999999,0.10899999999999999,-0.6227999999999998]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","2P1C",20,"heating",0,6,5.2176635590456142,0.86156177844505155,1.0160419723342169,7.2052660947244968E-2,1.2149057861379946,1.953035075340368,0,4.55,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB",20,7.3440000000000003,"RIU_FB_20_7.344",-2.7336,1.9893599999999996,1.3263999999999996,2.0777600000000014,1.7909600000000001,0.71319999999999983,0.71319999999999983,1.0689600000000006]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","2P1C",20,"cooling",0,6,5.2176635590456142,0.86156177844505155,1.0160419723342169,7.2052660947244968E-2,1.2149057861379946,1.953035075340368,0,4.55,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB",30,7.3440000000000003,"RIU_FB_30_7.344",4.6049600000000002,15.581760000000001,17.172879999999999,19.245760000000004,15.37552,10.565280000000001,10.222480000000001,11.720959999999998]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","2P2C",30,"heating",0,6,2.7469999999999999,0.93409999999999993,1.0488,9.0999999999999998E-2,0.80970000000000031,1.9433,0,4.368017,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB",50,2.67,"RIU_FB_50_2.67",-0.25230000000000008,-0.19060000000000077,-0.62709999999999866,1.0461999999999998,0.82189999999999941,-0.3525999999999998,-0.82139999999999969,0.40059999999999985]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","2P1C",30,"cooling",0,6,5.0476438741556215,0.82670922585047024,1.0170539174666613,7.6553971135702004E-2,0.87139191555771811,1.9315233318194709,0,4.368017,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB",50,7.3440000000000003,"RIU_FB_50_7.344",1.1966399999999999,12.990080000000003,12.787280000000003,14.41384,12.83408,10.023680000000002,6.5635200000000014,5.9159199999999998]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","4P1C",30,"cooling",0,6,4.0126118705126315,0.85474076995478609,1.035090985050215,9.2968595197129522E-2,0.87139191555771811,1.9315233318194709,0,4.368017,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB",60,3.33,"RIU_FB_60_3.33",0.21970000000000001,2.3557000000000006,1.0465999999999998,2.0324000000000009,2.0122,1.0521000000000003,0.4986000000000006,1.3146999999999993]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","4P2C",35,"heating",0,6,4.4146000000000001,0.67301493957276226,0.99472579961317542,9.845000000000001E-2,0.4936086143442468,1.9152500000000001,0,4.067367,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB",10,5.33,"RIU_TB_10_5.33",-1.4245000000000001,-0.40730000000000022,0.11799999999999988,-1.6799999999999038E-2,-0.90779999999999994,0.10899999999999999,0.10899999999999999,-0.6227999999999998]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","2P1C",40,"heating",0,6,5.4532731018248422,0.71673964106289134,1.0171479393353196,8.7936621709911678E-2,0.47815348738143149,1.8495971103882154,0,3.2610521092625002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB",20,7.3440000000000003,"RIU_TB_20_7.344",-2.7336,1.9893599999999996,1.3263999999999996,2.0777600000000014,1.7909600000000001,0.71319999999999983,0.71319999999999983,1.0689600000000006]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","4P1C",40,"heating",0,6,5.5759352760158736,0.5109140414590837,1.0137152325510541,0.12911479361523923,0.47815348738143149,1.8495971103882154,0,3.2610521092625002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB",30,3.33,"RIU_TB_30_3.33",0.22970000000000024,2.3757000000000001,1.0366,2.0257000000000005,2.0089000000000006,1.0521000000000003,0.50860000000000039,1.3246999999999991]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","2P2C",40,"cooling",0,6,3.2164000000000001,0.82810000000000006,1.0135000000000001,9.3799999999999994E-2,0.3707999999999998,1.9044000000000001,0,3.2610521092625002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB",40,2.67,"RIU_TB_40_2.67",-0.21420000000000006,-0.49509999999999987,-2.9900000000000482E-2,2.1727999999999996,1.4133999999999998,-0.28960000000000008,-0.70020000000000016,0.77049999999999996]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","4P1C",50,"heating",0,6,4.7704106378325344,0.51089063974090831,1.0028918324840346,0.14892973593767114,0.32892130750673021,1.8360692602535555,0,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB",50,3.33,"RIU_TB_50_3.33",-4.7700000000000076E-2,1.6705999999999994,1.267100000000001,2.9337999999999997,2.5180999999999996,1.1126000000000005,0.22140000000000004,1.1793999999999998]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","4P2C",50,"cooling",0,6,2.7915000000000001,0.78080000000000005,1.0191467379083534,0.10925768403496422,0.22969283687559228,1.9085000000000001,0,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB",60,5.33,"RIU_TB_60_5.33",2.3997000000000002,8.9357000000000024,9.0865999999999971,10.5924,8.6921999999999997,5.7921000000000014,5.3386000000000005,6.494699999999999]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","4P1C",60,"heating",0,6,4.2337252879439511,0.52435960868968456,1.0224637849976359,0.14139907600437487,0.16443739560310769,1.9123161515678218,0,2.5793829276231501,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB",10,3.33,"RIU_LB_10_3.33",-0.12450000000000028,-2.7873000000000001,-1.0820000000000001,-2.0967999999999996,-3.5878000000000005,-0.49099999999999999,-0.49099999999999999,-2.3027999999999995]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","2P1C",60,"cooling",0,6,4.1153071480202037,0.72868693180977873,1.0202612095812595,9.0814357187386688E-2,0.16443739560310769,1.9123161515678218,0,2.5793829276231501,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB",10,7.3440000000000003,"RIU_LB_10_7.344",-2.7336,1.9893599999999996,1.3263999999999996,2.0777600000000014,1.7909600000000001,0.71319999999999983,0.71319999999999983,1.0689600000000006]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","2P2C",70,"heating",0,6,2.1756000000000002,0.83630000000000004,1.018,9.74E-2,0.10200000000000004,1.913,0,2.35,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB",30,2.67,"RIU_LB_30_2.67",-0.48969999999999958,0.20429999999999993,-1.6166000000000018,-0.80569999999999986,-0.18890000000000029,-0.51209999999999933,-1.0886000000000005,-0.38470000000000049]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","4P2C",70,"heating",0,6,3.8020999999999994,0.62310834257244618,0.98044867746908837,0.10790000000000001,8.2826074771338826E-2,1.9205000000000001,0,2.35,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB",30,5.33,"RIU_LB_30_5.33",2.4097000000000004,8.955700000000002,9.0765999999999973,10.605700000000001,8.6688999999999989,5.7921000000000014,5.3486000000000002,6.5046999999999988]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","4P1C",70,"cooling",0,6,3.8364187564726588,0.68163108574876341,1.0302701440242945,0.11096164693151411,0.11632799613580581,1.9069294072602954,0,2.35,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB",40,3.33,"RIU_LB_40_3.33",-0.38580000000000003,1.1351000000000013,1.309899999999999,3.3872,2.7466000000000004,1.1096000000000004,-7.9800000000000093E-2,0.86949999999999994]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LIU24_2W","4P2C",80,"heating",0,6,3.2232975281327274,0.62201716017035658,0.98006641042962894,0.11045420777221195,5.2848605293414744E-2,1.9511881846395511,0,2.0785275864688009,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB",50,5.33,"RIU_LB_50_5.33",0.57230000000000003,7.3106,7.0071000000000012,8.6538000000000004,7.6581000000000001,5.5526000000000009,3.3814000000000002,3.5393999999999997]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","2P1C","10","cooling",0,3.33,2.5949625000000003,0.71675,1.0096499999999999,0.17454999999999998,1.0451000000000001,1.8435000000000001,0,4.2955077781361535,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB",60,7.3440000000000003,"RIU_LB_60_7.344",4.5949600000000004,15.561760000000001,17.182879999999997,19.212320000000005,15.418960000000002,10.565280000000001,10.212480000000003,11.71096]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","2P1C","50","cooling",0,3.33,2.3996500000000003,0.80089999999999995,0.95930000000000004,0.14685000000000001,0.21534999999999999,1.9656500000000001,0,2.5405474990721024,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP",10,7.3440000000000003,"ACBR_LP_10_7.344",-2.7336,1.9893599999999996,1.3263999999999996,2.0777600000000014,1.7909600000000001,0.71319999999999983,0.71319999999999983,1.0689600000000006]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","2P1C","60","cooling",0,3.33,2.8062,0.75669999999999993,0.90490000000000004,0.14080000000000001,0.16679999999999998,1.9337000000000002,0,2.222149804379645,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP",20,2.67,"ACBR_LP_20_2.67",0.30449999999999999,-3.5727000000000002,-1.4780000000000002,-2.7831999999999995,-4.4722000000000008,-0.68900000000000006,-0.68900000000000006,-2.8571999999999997]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","2P1C","50","heating",0,3.33,2.3996500000000003,0.80089999999999995,0.95930000000000004,0.14685000000000001,0.21534999999999999,1.9656500000000001,0,2.5405474990721024,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP",30,3.33,"ACBR_LP_30_3.33",0.22970000000000024,2.3757000000000001,1.0366,2.0257000000000005,2.0089000000000006,1.0521000000000003,0.50860000000000039,1.3246999999999991]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","2P2C","20","cooling",0,3.33,2.1591999999999998,0.81569999999999998,1.0661999999999998,0.16260000000000002,0.7619999999999999,1.9015000000000002,0,3.6462094095916582,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP",40,2.67,"ACBR_LP_40_2.67",-0.21420000000000006,-0.49509999999999987,-2.9900000000000482E-2,2.1727999999999996,1.4133999999999998,-0.28960000000000008,-0.70020000000000016,0.77049999999999996]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","2P2C","20","heating",0,3.33,2.1591999999999998,0.81569999999999998,1.0661999999999998,0.16260000000000002,0.7619999999999999,1.9015000000000002,0,3.6462094095916582,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP",50,5.33,"ACBR_LP_50_5.33",0.57230000000000003,7.3106,7.0071000000000012,8.6538000000000004,7.6581000000000001,5.5526000000000009,3.3814000000000002,3.5393999999999997]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","2P2C","30","heating",0,3.33,1.8019499999999999,0.81595000000000006,1.06355,0.18080000000000002,0.55089999999999995,1.9131500000000001,0,3.279806658718901,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP",50,7.3440000000000003,"ACBR_LP_50_7.344",1.1966399999999999,12.990080000000003,12.787280000000003,14.41384,12.83408,10.023680000000002,6.5635200000000014,5.9159199999999998]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","4P1C","20","cooling",0,3.33,2.457031391271463,0.78387398955983578,1.0099550944000919,0.17604761918059322,0.78794177785591468,1.8898593686999265,0,3.6462094095916582]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","4P1C","60","cooling",0,3.33,3.1296070346103191,0.72459611353607145,0.92978762573637497,0.12667355807032349,0.17919746119384117,1.9134252196949866,0,2.222149804379645]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","4P1C","50","heating",0,3.33,3.2056873004038913,0.56460145590539312,0.91350305655730013,0.18965651180849208,0.27532664015612418,1.8958451773097236,0,2.5405474990721024]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","4P1C","60","heating",0,3.33,3.6138449982390033,0.55440297873821398,0.92288037354184582,0.15267388867893864,0.17919746119384117,1.9134252196949866,0,2.222149804379645]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","4P2C","40","cooling",0,3.33,1.4169,0.8266,1.0191999999999999,0.20269999999999999,0.30899999999999994,1.9467999999999999,0,2.7187297312016185]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_FB","4P2C","30","heating",0,3.33,4.0894500000000003,0.53120000000000001,0.94299999999999995,0.18595,0.44154999999999994,1.9683499999999998,0,3.279806658718901]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","2P1C","20","cooling",0,3.33,2.9056000000000002,0.75950000000000006,1.0109999999999999,0.16729999999999998,0.78470000000000006,1.8949,0,3.6462094095916582]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","2P1C","30","cooling",0,3.33,2.4493999999999998,0.80225000000000002,1.0123500000000001,0.16005,0.52429999999999999,1.9462999999999999,0,3.279806658718901]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","2P1C","20","heating",0,3.33,2.9056000000000002,0.75950000000000006,1.0109999999999999,0.16729999999999998,0.78470000000000006,1.8949,0,3.6462094095916582]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","2P1C","60","heating",0,3.33,2.8062,0.75669999999999993,0.90490000000000004,0.14080000000000001,0.16679999999999998,1.9337000000000002,0,2.222149804379645]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","2P2C","50","cooling",0,3.33,1.3892500000000001,0.8,1.02485,0.20370000000000002,0.26109999999999994,1.91455,0,2.5405474990721024]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","2P2C","60","cooling",0,3.33,1.3338000000000001,0.78369999999999995,0.98869999999999991,0.20830000000000001,0.18239999999999995,1.9041999999999999,0,2.222149804379645]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","2P2C","40","heating",0,3.33,1.4446999999999999,0.81620000000000004,1.0609,0.19900000000000001,0.33979999999999988,1.9248000000000001,0,2.7187297312016185]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","4P1C","30","cooling",0,3.33,2.8102288604773236,0.72763475036526837,0.94982838102882539,0.19351165651688929,0.49262346094289033,1.9229285701145435,0,3.279806658718901]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","4P1C","20","heating",0,3.33,4.138516601221605,0.5272431067836385,0.97617120086335596,0.17987864925886607,0.78794177785591468,1.8898593686999265,0,3.6462094095916582]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","4P1C","40","heating",0,3.33,3.5140502325419884,0.5938864627627829,0.97517705726139903,0.15089321043612972,0.36807553486059136,1.8863863294357037,0,2.7187297312016185]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","4P2C","10","cooling",0,3.33,1.9635000000000002,0.69025000000000003,1.06585,0.24349999999999999,0.70665,2.01145,0,4.2955077781361535]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","4P2C","60","cooling",0,3.33,1.4164000000000001,0.73750000000000004,0.97830000000000006,0.22389999999999999,0.16830000000000001,1.9353,0,2.222149804379645]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_TB","4P2C","50","heating",0,3.33,3.6620500000000002,0.55025000000000002,0.9326000000000001,0.16935,0.23865,1.9410499999999999,0,2.5405474990721024]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","2P1C","20","cooling",0,3.33,2.9056000000000002,0.75950000000000006,1.0109999999999999,0.16729999999999998,0.78470000000000006,1.8949,0,3.6462094095916582]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","2P1C","40","cooling",0,3.33,1.9932000000000001,0.84500000000000008,1.0137,0.15279999999999999,0.26390000000000002,1.9977,0,2.7187297312016185]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","2P1C","30","heating",0,3.33,2.4493999999999998,0.80225000000000002,1.0123500000000001,0.16005,0.52429999999999999,1.9462999999999999,0,3.279806658718901]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","2P1C","60","heating",0,3.33,2.8062,0.75669999999999993,0.90490000000000004,0.14080000000000001,0.16679999999999998,1.9337000000000002,0,2.222149804379645]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","2P2C","20","cooling",0,3.33,2.1591999999999998,0.81569999999999998,1.0661999999999998,0.16260000000000002,0.7619999999999999,1.9015000000000002,0,3.6462094095916582]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","2P2C","10","heating",0,3.33,2.5164499999999999,0.81545000000000001,1.0688499999999999,0.1444,0.97309999999999985,1.88985,0,4.2955077781361535]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","2P2C","60","heating",0,3.33,1.3338000000000001,0.78369999999999995,0.98869999999999991,0.20830000000000001,0.18239999999999995,1.9041999999999999,0,2.222149804379645]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","4P1C","40","cooling",0,3.33,2.4732697134292163,0.78787697372002075,0.99278777245578309,0.14971324544273937,0.36807553486059136,1.8863863294357037,0,2.7187297312016185]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","4P1C","50","cooling",0,3.33,2.1118580146768826,0.78938326955320648,0.96048688695280693,0.16722624011084156,0.27532664015612418,1.8958451773097236,0,2.5405474990721024]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","4P1C","40","heating",0,3.33,3.5140502325419884,0.5938864627627829,0.97517705726139903,0.15089321043612972,0.36807553486059136,1.8863863294357037,0,2.7187297312016185]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","4P2C","10","cooling",0,3.33,1.9635000000000002,0.69025000000000003,1.06585,0.24349999999999999,0.70665,2.01145,0,4.2955077781361535]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","4P2C","10","heating",0,3.33,5.2413500000000006,0.46260000000000001,0.88700000000000001,0.21685000000000001,0.70665,2.01145,0,4.2955077781361535]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RIU_LB","4P2C","20","heating",0,3.33,4.6654,0.49690000000000001,0.91500000000000004,0.2014,0.57409999999999994,1.9899,0,3.6462094095916582]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","2P1C","10","cooling",0,3.33,2.5949625000000003,0.71675,1.0096499999999999,0.17454999999999998,1.0451000000000001,1.8435000000000001,0,4.2955077781361535]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","2P1C","60","cooling",0,3.33,2.8062,0.75669999999999993,0.90490000000000004,0.14080000000000001,0.16679999999999998,1.9337000000000002,0,2.222149804379645]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","2P1C","40","heating",0,3.33,1.9932000000000001,0.84500000000000008,1.0137,0.15279999999999999,0.26390000000000002,1.9977,0,2.7187297312016185]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","2P1C","50","heating",0,3.33,2.3996500000000003,0.80089999999999995,0.95930000000000004,0.14685000000000001,0.21534999999999999,1.9656500000000001,0,2.5405474990721024]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","2P2C","40","cooling",0,3.33,1.4446999999999999,0.81620000000000004,1.0609,0.19900000000000001,0.33979999999999988,1.9248000000000001,0,2.7187297312016185]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","2P2C","10","heating",0,3.33,2.5164499999999999,0.81545000000000001,1.0688499999999999,0.1444,0.97309999999999985,1.88985,0,4.2955077781361535]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","2P2C","20","heating",0,3.33,2.1591999999999998,0.81569999999999998,1.0661999999999998,0.16260000000000002,0.7619999999999999,1.9015000000000002,0,3.6462094095916582]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","2P2C","30","heating",0,3.33,1.8019499999999999,0.81595000000000006,1.06355,0.18080000000000002,0.55089999999999995,1.9131500000000001,0,3.279806658718901]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","2P2C","40","heating",0,3.33,1.4446999999999999,0.81620000000000004,1.0609,0.19900000000000001,0.33979999999999988,1.9248000000000001,0,2.7187297312016185]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","2P2C","50","heating",0,3.33,1.3892500000000001,0.8,1.02485,0.20370000000000002,0.26109999999999994,1.91455,0,2.5405474990721024]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","2P2C","60","heating",0,3.33,1.3338000000000001,0.78369999999999995,0.98869999999999991,0.20830000000000001,0.18239999999999995,1.9041999999999999,0,2.222149804379645]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P1C","10","cooling",0,3.33,2.1209807678253227,1.0404757698636466,0.92566563124586165,0.13093320636912978,1.4670986032302269,1.9191969723552433,0,4.2955077781361535]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P1C","20","cooling",0,3.33,2.457031391271463,0.78387398955983578,1.0099550944000919,0.17604761918059322,0.78794177785591468,1.8898593686999265,0,3.6462094095916582]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P1C","30","cooling",0,3.33,2.8102288604773236,0.72763475036526837,0.94982838102882539,0.19351165651688929,0.49262346094289033,1.9229285701145435,0,3.279806658718901]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P1C","40","cooling",0,3.33,2.4732697134292163,0.78787697372002075,0.99278777245578309,0.14971324544273937,0.36807553486059136,1.8863863294357037,0,2.7187297312016185]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P1C","50","cooling",0,3.33,2.1118580146768826,0.78938326955320648,0.96048688695280693,0.16722624011084156,0.27532664015612418,1.8958451773097236,0,2.5405474990721024]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P1C","60","cooling",0,3.33,3.1296070346103191,0.72459611353607145,0.92978762573637497,0.12667355807032349,0.17919746119384117,1.9134252196949866,0,2.222149804379645]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P1C","10","heating",0,3.33,2.2632913404615129,0.84517869183162408,0.90176565647424445,0.17222136470614724,1.4670986032302269,1.9191969723552433,0,4.2955077781361535]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P1C","20","heating",0,3.33,4.138516601221605,0.5272431067836385,0.97617120086335596,0.17987864925886607,0.78794177785591468,1.8898593686999265,0,3.6462094095916582]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P1C","30","heating",0,3.33,3.995033606550912,0.522033089867735,0.93839463793771716,0.19570852588972812,0.49262346094289033,1.9229285701145435,0,3.279806658718901]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P1C","40","heating",0,3.33,3.5140502325419884,0.5938864627627829,0.97517705726139903,0.15089321043612972,0.36807553486059136,1.8863863294357037,0,2.7187297312016185]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P1C","50","heating",0,3.33,3.2056873004038913,0.56460145590539312,0.91350305655730013,0.18965651180849208,0.27532664015612418,1.8958451773097236,0,2.5405474990721024]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P1C","60","heating",0,3.33,3.6138449982390033,0.55440297873821398,0.92288037354184582,0.15267388867893864,0.17919746119384117,1.9134252196949866,0,2.222149804379645]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P2C","10","cooling",0,3.33,1.9635000000000002,0.69025000000000003,1.06585,0.24349999999999999,0.70665,2.01145,0,4.2955077781361535]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P2C","20","cooling",0,3.33,1.7813000000000001,0.73570000000000002,1.0503,0.22989999999999999,0.57409999999999994,1.9899,0,3.6462094095916582]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P2C","30","cooling",0,3.33,1.5991000000000002,0.78115000000000001,1.0347499999999998,0.21629999999999999,0.44154999999999994,1.9683499999999998,0,3.279806658718901]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P2C","40","cooling",0,3.33,1.4169,0.8266,1.0191999999999999,0.20269999999999999,0.30899999999999994,1.9467999999999999,0,2.7187297312016185]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P2C","50","cooling",0,3.33,1.4166000000000001,0.78200000000000003,0.99870000000000003,0.21325,0.23865,1.9410499999999999,0,2.5405474990721024]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P2C","60","cooling",0,3.33,1.4164000000000001,0.73750000000000004,0.97830000000000006,0.22389999999999999,0.16830000000000001,1.9353,0,2.222149804379645]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P2C","10","heating",0,3.33,5.2413500000000006,0.46260000000000001,0.88700000000000001,0.21685000000000001,0.70665,2.01145,0,4.2955077781361535]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P2C","20","heating",0,3.33,4.6654,0.49690000000000001,0.91500000000000004,0.2014,0.57409999999999994,1.9899,0,3.6462094095916582]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P2C","30","heating",0,3.33,4.0894500000000003,0.53120000000000001,0.94299999999999995,0.18595,0.44154999999999994,1.9683499999999998,0,3.279806658718901]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P2C","40","heating",0,3.33,3.5135000000000005,0.5655,0.97099999999999997,0.17050000000000001,0.30899999999999994,1.9467999999999999,0,2.7187297312016185]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P2C","50","heating",0,3.33,3.6620500000000002,0.55025000000000002,0.9326000000000001,0.16935,0.23865,1.9410499999999999,0,2.5405474990721024]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ACBR_LP","4P2C","60","heating",0,3.33,3.8106,0.53499999999999992,0.89420000000000011,0.16829999999999998,0.16830000000000001,1.9353,0,2.222149804379645]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PCBL","2P1C",null,"cooling ",null,8,17.696878806375835,1.3060022235208978E-2,1.4404879191074722,0,0,0,0,2.6]